(footprint "SLO1365H" (version 20210126) (generator pcbnew) (layer "F.Cu")
  (tedit 605A7250)
  (fp_text reference "REF**" (at 0 -5 unlocked) (layer "F.SilkS"))
  (fp_text value "SLO1365H" (at -3.5 -7.5 unlocked) (layer "F.Fab"))
  (fp_text user "${REFERENCE}" (at 0 -5 unlocked) (layer "F.Fab"))
  (pad "1" smd rect (at -4.375 0) (size 5.35 4.5) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "2" smd rect (at 4.375 0) (size 5.35 4.5) (layers "F.Cu" "F.Paste" "F.Mask"))
)
