(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "/D.N")
  (net 2 "/D.P")
  (footprint "Connector_JST:JST_ZE_S02B-ZESK-2D_1x02_P1.50mm_Horizontal" (layer "F.Cu")
    (tedit 5B775643)
    (at 148.775 98.775)
    (descr "JST ZE series connector, S02B-ZESK-2D (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator")
    (tags "connector JST ZE top entry")
    (property "Sheetfile" "test.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 0.75 -2.08) (layer "F.SilkS"))
    (fp_text value "Conn_01x02_Female" (at 0.75 8.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.75 3.45) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 3.05 1.85) (size 1.15 1.15) (drill 1.15) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at -1.55 1.85) (size 1.15 1.15) (drill 1.15) (layers *.Cu *.Mask))
    (pad "1" thru_hole roundrect locked (at 0 0) (size 1.4 1.75) (drill 0.75) (layers *.Cu *.Mask) (roundrect_rratio 0.178571)
      (net 2 "/D.P") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 1.5 3.7) (size 1.4 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 1 "/D.N") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_ZE_S02B-ZESK-2D_1x02_P1.50mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_JST:JST_ZE_S02B-ZESK-2D_1x02_P1.50mm_Horizontal" (layer "F.Cu")
    (tedit 5B775643)
    (at 148.775 139.325)
    (descr "JST ZE series connector, S02B-ZESK-2D (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator")
    (tags "connector JST ZE top entry")
    (property "Sheetfile" "test.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 0.75 -2.08) (layer "F.SilkS"))
    (fp_text value "Conn_01x02_Female" (at 0.75 8.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.75 3.45) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 3.05 1.85) (size 1.15 1.15) (drill 1.15) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at -1.55 1.85) (size 1.15 1.15) (drill 1.15) (layers *.Cu *.Mask))
    (pad "1" thru_hole roundrect locked (at 0 0) (size 1.4 1.75) (drill 0.75) (layers *.Cu *.Mask) (roundrect_rratio 0.178571)
      (net 2 "/D.P") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 1.5 3.7) (size 1.4 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 1 "/D.N") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_ZE_S02B-ZESK-2D_1x02_P1.50mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
)
