(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (aux_axis_origin 80 150)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "GND")
  (net 3 "VCC")
  (net 4 "Net-(C3-Pad1)")
  (net 5 "Net-(C7-Pad2)")
  (net 6 "+12V")
  (net 7 "Net-(C8-Pad1)")
  (net 8 "/+25V")
  (net 9 "Net-(D1-Pad2)")
  (net 10 "Net-(D2-Pad2)")
  (net 11 "/Vpp")
  (net 12 "Net-(D4-Pad1)")
  (net 13 "Net-(D5-Pad1)")
  (net 14 "/B_D5")
  (net 15 "/B_D6")
  (net 16 "/B_D3")
  (net 17 "/B_D4")
  (net 18 "/B_A2")
  (net 19 "/B_A4")
  (net 20 "/B_A5")
  (net 21 "/B_A6")
  (net 22 "/\\WAIT")
  (net 23 "/\\BUSRQ")
  (net 24 "/\\BAI")
  (net 25 "/B_A19")
  (net 26 "-12V")
  (net 27 "/B_A30")
  (net 28 "/\\BAO")
  (net 29 "/B_A14")
  (net 30 "/\\M1")
  (net 31 "/B_A22")
  (net 32 "/B_A23")
  (net 33 "/\\IQ1")
  (net 34 "/VBAT")
  (net 35 "/\\IQ2")
  (net 36 "/\\RFSH")
  (net 37 "/B_A13")
  (net 38 "/B_A9")
  (net 39 "/\\BUSAK")
  (net 40 "/B_D0")
  (net 41 "/B_D7")
  (net 42 "/B_D2")
  (net 43 "/B_A0")
  (net 44 "/B_A3")
  (net 45 "/B_A1")
  (net 46 "/B_A8")
  (net 47 "/B_A7")
  (net 48 "/B_A16")
  (net 49 "/\\IEI")
  (net 50 "/B_A17")
  (net 51 "/B_A18")
  (net 52 "/B_D1")
  (net 53 "/B_A31")
  (net 54 "/\\IEO")
  (net 55 "/B_A11")
  (net 56 "/B_A10")
  (net 57 "/B_A21")
  (net 58 "/\\NMI")
  (net 59 "/\\INT")
  (net 60 "/\\WR")
  (net 61 "/B_A20")
  (net 62 "/\\HALT")
  (net 63 "/\\RESOUT")
  (net 64 "/B_A12")
  (net 65 "/B_A15")
  (net 66 "/\\CLK")
  (net 67 "/\\MREQ")
  (net 68 "/\\RESET")
  (net 69 "/VccE")
  (net 70 "/EA12")
  (net 71 "/nPGM")
  (net 72 "/EA7")
  (net 73 "/EA13")
  (net 74 "/EA6")
  (net 75 "/EA8")
  (net 76 "/EA5")
  (net 77 "/EA9")
  (net 78 "/EA4")
  (net 79 "/EA11")
  (net 80 "/EA3")
  (net 81 "/nOE")
  (net 82 "/EA2")
  (net 83 "/EA10")
  (net 84 "/EA1")
  (net 85 "/nCE")
  (net 86 "/EA0")
  (net 87 "/ED7")
  (net 88 "/ED0")
  (net 89 "/ED6")
  (net 90 "/ED1")
  (net 91 "/ED5")
  (net 92 "/ED2")
  (net 93 "/ED4")
  (net 94 "/ED3")
  (net 95 "Net-(K1-Pad6)")
  (net 96 "Net-(K2-Pad6)")
  (net 97 "Net-(L1-Pad1)")
  (net 98 "Net-(L1-Pad2)")
  (net 99 "Net-(Q1-Pad2)")
  (net 100 "Net-(Q2-Pad2)")
  (net 101 "Net-(Q3-Pad2)")
  (net 102 "Net-(Q4-Pad2)")
  (net 103 "Net-(Q5-Pad2)")
  (net 104 "Net-(R1-Pad2)")
  (net 105 "Net-(R2-Pad2)")
  (net 106 "Net-(R3-Pad2)")
  (net 107 "Net-(R4-Pad2)")
  (net 108 "Net-(R6-Pad1)")
  (net 109 "Net-(R7-Pad2)")
  (net 110 "Net-(R11-Pad2)")
  (net 111 "Net-(R13-Pad2)")
  (net 112 "Net-(R15-Pad2)")
  (net 113 "Net-(R17-Pad2)")
  (net 114 "Net-(U1-Pad19)")
  (net 115 "Net-(U1-Pad18)")
  (net 116 "Net-(U1-Pad17)")
  (net 117 "Net-(U1-Pad16)")
  (net 118 "Net-(U1-Pad15)")
  (net 119 "Net-(U1-Pad14)")
  (net 120 "Net-(U1-Pad13)")
  (net 121 "Net-(U1-Pad12)")
  (net 122 "Net-(U1-Pad11)")
  (net 123 "Net-(U1-Pad1)")
  (net 124 "Net-(U2-Pad4)")
  (net 125 "Net-(U2-Pad5)")
  (net 126 "Net-(U2-Pad6)")
  (net 127 "Net-(U2-Pad7)")
  (net 128 "Net-(U3-Pad2)")
  (net 129 "Net-(U3-Pad3)")
  (net 130 "Net-(U3-Pad5)")
  (net 131 "Net-(U3-Pad6)")
  (net 132 "Net-(U4-Pad4)")
  (net 133 "Net-(U5-Pad1)")
  (net 134 "Net-(U5-Pad11)")
  (net 135 "Net-(U5-Pad12)")
  (net 136 "Net-(U5-Pad13)")
  (net 137 "Net-(U5-Pad14)")
  (net 138 "Net-(U5-Pad6)")
  (net 139 "Net-(U5-Pad7)")
  (net 140 "Net-(U5-Pad19)")
  (net 141 "Net-(U6-Pad21)")
  (net 142 "Net-(U6-Pad22)")
  (net 143 "Net-(U6-Pad23)")
  (net 144 "Net-(U6-Pad24)")
  (net 145 "Net-(U6-Pad26)")
  (net 146 "/paEA11")
  (net 147 "/paEA13")
  (net 148 "/paEA14")
  (net 149 "/paEA15")
  (net 150 "Net-(U6-Pad16)")
  (net 151 "Net-(U6-Pad17)")
  (net 152 "Net-(U6-Pad18)")
  (net 153 "Net-(U7-Pad18)")
  (net 154 "Net-(U7-Pad17)")
  (net 155 "Net-(U7-Pad16)")
  (net 156 "/pbEA22")
  (net 157 "/pbEA21")
  (net 158 "/pbEA20")
  (net 159 "/pbEA19")
  (net 160 "/pbEA18")
  (net 161 "/pbEA17")
  (net 162 "/pbEA16")
  (net 163 "Net-(U7-Pad24)")
  (net 164 "Net-(U7-Pad23)")
  (net 165 "Net-(U7-Pad22)")
  (net 166 "Net-(U7-Pad21)")
  (net 167 "Net-(U9-Pad9)")
  (net 168 "Net-(U9-Pad8)")
  (net 169 "Net-(U11-Pad9)")
  (net 170 "Net-(U11-Pad11)")
  (net 171 "Net-(U11-Pad12)")
  (net 172 "Net-(J3-Pad4)")
  (net 173 "Net-(J3-Pad1)")
  (net 174 "Net-(J3-Pad3)")
  (net 175 "Net-(K2-Pad1)")
  (net 176 "/nM1")
  (net 177 "/nIORQ")
  (net 178 "/nRD")
  (net 179 "/nCLK")
  (net 180 "+15V")
  (net 181 "Net-(J2-Pad1)")
  (footprint "Capacitor_THT:C_Rect_L7.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 137.16 60.96 -90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2.5mm Capacitor")
    (attr through_hole)
    (fp_text reference "C1" (at 2.5 -2.5 -90) (layer "F.SilkS"))
    (fp_text value "100p" (at 2.5 2.5 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 -90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad "2" thru_hole circle locked (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_Tantal_D4.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 154.94 60.96 -90)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (attr through_hole)
    (fp_text reference "C2" (at 2.5 -3.5 90) (layer "F.SilkS"))
    (fp_text value "47u" (at 2.5 3.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "VCC"))
    (pad "2" thru_hole circle locked (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitors_THT.3dshapes/CP_Radial_D12.5mm_P7.50mm.step"
      (offset (xyz 0 0 0))
      (scale (xyz 0.65 0.65 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 137.16 71.755 -90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2.5mm Capacitor")
    (attr through_hole)
    (fp_text reference "C3" (at 2.5 -2.5 -90) (layer "F.SilkS"))
    (fp_text value "1n" (at 2.5 2.5 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 -90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad "2" thru_hole circle locked (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 114.3 113.17 180)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2.5mm Capacitor")
    (attr through_hole)
    (fp_text reference "C11" (at 2.5 -2.5) (layer "F.SilkS"))
    (fp_text value "100n" (at 2.5 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "VCC"))
    (pad "2" thru_hole circle locked (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 129.54 146.05 90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2.5mm Capacitor")
    (attr through_hole)
    (fp_text reference "C12" (at 2.5 -2.5 90) (layer "F.SilkS"))
    (fp_text value "100n" (at 2.5 2.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.01 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "VCC"))
    (pad "2" thru_hole circle locked (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 129.54 110.49 180)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2.5mm Capacitor")
    (attr through_hole)
    (fp_text reference "C14" (at 2.5 -2.5) (layer "F.SilkS"))
    (fp_text value "100n" (at 2.5 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "VCC"))
    (pad "2" thru_hole circle locked (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 124.46 92.71)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2.5mm Capacitor")
    (attr through_hole)
    (fp_text reference "C15" (at 2.5 -2.5) (layer "F.SilkS"))
    (fp_text value "100n" (at 2.5 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "VCC"))
    (pad "2" thru_hole circle locked (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50CD5)
    (at 229.87 73.66 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (attr through_hole)
    (fp_text reference "D1" (at 3.81 -2.12 90) (layer "F.SilkS"))
    (fp_text value "ZPD3.9" (at 3.81 2.12 90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.8 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 4.11 0 90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.8 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "/+25V"))
    (pad "2" thru_hole oval locked (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(D1-Pad2)"))
    (model "${KICAD6_3DMODEL_DIR}/Diodes_THT.3dshapes/D_5W_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50CD5)
    (at 237.49 105.41 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (attr through_hole)
    (fp_text reference "D2" (at 3.81 -2.12 90) (layer "F.SilkS"))
    (fp_text value "ZPD13" (at 3.81 2.12 90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.8 90) (layer "F.SilkS"))
    (fp_text user "K" (at 0 -1.8 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 4.11 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "/+25V"))
    (pad "2" thru_hole oval locked (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(D2-Pad2)"))
    (model "${KICAD6_3DMODEL_DIR}/Diodes_THT.3dshapes/D_5W_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50CD5)
    (at 231.14 144.78 180)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (attr through_hole)
    (fp_text reference "D3" (at 3.81 -2.12) (layer "F.SilkS"))
    (fp_text value "1N4148" (at 3.81 2.12) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.8) (layer "F.SilkS"))
    (fp_text user "K" (at 0 -1.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 4.11 0) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "/Vpp"))
    (pad "2" thru_hole oval locked (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 69 "/VccE"))
    (model "${KICAD6_3DMODEL_DIR}/Diodes_THT.3dshapes/D_5W_P10.16mm_Horizontal_glas.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50CD5)
    (at 237.49 133.35 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (attr through_hole)
    (fp_text reference "D4" (at 3.81 -2.12 90) (layer "F.SilkS"))
    (fp_text value "1N4148" (at 3.81 2.12 90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.8 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 4.11 0 90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.8 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(D4-Pad1)"))
    (pad "2" thru_hole oval locked (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 69 "/VccE"))
    (model "${KICAD6_3DMODEL_DIR}/Diodes_THT.3dshapes/D_5W_P10.16mm_Horizontal_glas.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50CD5)
    (at 215.9 71.12)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (attr through_hole)
    (fp_text reference "D5" (at 3.81 -2.12) (layer "F.SilkS"))
    (fp_text value "1N4148" (at 3.81 2.12) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.8) (layer "F.SilkS"))
    (fp_text user "K" (at 0 -1.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 4.11 0.068999) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(D5-Pad1)"))
    (pad "2" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 69 "/VccE"))
    (model "${KICAD6_3DMODEL_DIR}/Diodes_THT.3dshapes/D_5W_P10.16mm_Horizontal_glas.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_DIN:DIN41612_C_2x32_Male_Horizontal_THT" (layer "F.Cu")
    (tedit 5EAFCB7F)
    (at 85.09 139.7 90)
    (descr "DIN41612 connector, type C, Horizontal, 3 rows 32 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf")
    (tags "DIN 41612 IEC 60603 C")
    (attr through_hole)
    (fp_text reference "J1" (at -5.08 1 90) (layer "F.SilkS"))
    (fp_text value "DIN41612_02x32_AC" (at 39.37 7.62 90) (layer "F.Fab"))
    (fp_text user "Board edge" (at 39.37 -7.3 90) (layer "Cmts.User"))
    (fp_text user "${REFERENCE}" (at 39.6365 -3.217 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at -5.08 -2.54 90) (size 2.85 2.85) (drill 2.85) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 83.82 -2.54 90) (size 2.85 2.85) (drill 2.85) (layers *.Cu *.Mask))
    (pad "a1" thru_hole roundrect locked (at 0 0 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.16129)
      (net 3 "VCC"))
    (pad "a2" thru_hole circle locked (at 2.54 0 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 14 "/B_D5"))
    (pad "a3" thru_hole circle locked (at 5.08 0 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 15 "/B_D6"))
    (pad "a4" thru_hole circle locked (at 7.62 0 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 16 "/B_D3"))
    (pad "a5" thru_hole circle locked (at 10.16 0 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 17 "/B_D4"))
    (pad "a6" thru_hole circle locked (at 12.7 0 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 18 "/B_A2"))
    (pad "a7" thru_hole circle locked (at 15.24 0 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 19 "/B_A4"))
    (pad "a8" thru_hole circle locked (at 17.78 0 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 20 "/B_A5"))
    (pad "a9" thru_hole circle locked (at 20.32 0 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 21 "/B_A6"))
    (pad "a10" thru_hole circle locked (at 22.86 0 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 22 "/\\WAIT"))
    (pad "a11" thru_hole circle locked (at 25.4 0 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 23 "/\\BUSRQ"))
    (pad "a12" thru_hole circle locked (at 27.94 0 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 24 "/\\BAI"))
    (pad "a13" thru_hole circle locked (at 30.48 0 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 6 "+12V"))
    (pad "a14" thru_hole circle locked (at 33.02 0 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 25 "/B_A19"))
    (pad "a15" thru_hole circle locked (at 35.56 0 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 26 "-12V"))
    (pad "a16" thru_hole circle locked (at 38.1 0 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 27 "/B_A30"))
    (pad "a17" thru_hole circle locked (at 40.64 0 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 28 "/\\BAO"))
    (pad "a18" thru_hole circle locked (at 43.18 0 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 29 "/B_A14"))
    (pad "a19" thru_hole circle locked (at 45.72 0 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 180 "+15V"))
    (pad "a20" thru_hole circle locked (at 48.26 0 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 176 "/nM1"))
    (pad "a21" thru_hole circle locked (at 50.8 0 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 31 "/B_A22"))
    (pad "a22" thru_hole circle locked (at 53.34 0 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 32 "/B_A23"))
    (pad "a23" thru_hole circle locked (at 55.88 0 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 33 "/\\IQ1"))
    (pad "a24" thru_hole circle locked (at 58.42 0 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 34 "/VBAT"))
    (pad "a25" thru_hole circle locked (at 60.96 0 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 33 "/\\IQ1"))
    (pad "a26" thru_hole circle locked (at 63.5 0 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 35 "/\\IQ2"))
    (pad "a27" thru_hole circle locked (at 66.04 0 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 177 "/nIORQ"))
    (pad "a28" thru_hole circle locked (at 68.58 0 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 36 "/\\RFSH"))
    (pad "a29" thru_hole circle locked (at 71.12 0 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 37 "/B_A13"))
    (pad "a30" thru_hole circle locked (at 73.66 0 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 38 "/B_A9"))
    (pad "a31" thru_hole circle locked (at 76.2 0 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 39 "/\\BUSAK"))
    (pad "a32" thru_hole circle locked (at 78.74 0 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (pad "c1" thru_hole circle locked (at 0 5.08 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 3 "VCC"))
    (pad "c2" thru_hole circle locked (at 2.54 5.08 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 40 "/B_D0"))
    (pad "c3" thru_hole circle locked (at 5.08 5.08 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 41 "/B_D7"))
    (pad "c4" thru_hole circle locked (at 7.62 5.08 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 42 "/B_D2"))
    (pad "c5" thru_hole circle locked (at 10.16 5.08 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 43 "/B_A0"))
    (pad "c6" thru_hole circle locked (at 12.7 5.08 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 44 "/B_A3"))
    (pad "c7" thru_hole circle locked (at 15.24 5.08 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 45 "/B_A1"))
    (pad "c8" thru_hole circle locked (at 17.78 5.08 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 46 "/B_A8"))
    (pad "c9" thru_hole circle locked (at 20.32 5.08 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 47 "/B_A7"))
    (pad "c10" thru_hole circle locked (at 22.86 5.08 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 48 "/B_A16"))
    (pad "c11" thru_hole circle locked (at 25.4 5.08 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 49 "/\\IEI"))
    (pad "c12" thru_hole circle locked (at 27.94 5.08 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 50 "/B_A17"))
    (pad "c13" thru_hole circle locked (at 30.48 5.08 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 51 "/B_A18"))
    (pad "c14" thru_hole circle locked (at 33.02 5.08 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 52 "/B_D1"))
    (pad "c15" thru_hole circle locked (at 35.56 5.08 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 53 "/B_A31"))
    (pad "c16" thru_hole circle locked (at 38.1 5.08 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 54 "/\\IEO"))
    (pad "c17" thru_hole circle locked (at 40.64 5.08 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 55 "/B_A11"))
    (pad "c18" thru_hole circle locked (at 43.18 5.08 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 56 "/B_A10"))
    (pad "c19" thru_hole circle locked (at 45.72 5.08 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 57 "/B_A21"))
    (pad "c20" thru_hole circle locked (at 48.26 5.08 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 58 "/\\NMI"))
    (pad "c21" thru_hole circle locked (at 50.8 5.08 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 59 "/\\INT"))
    (pad "c22" thru_hole circle locked (at 53.34 5.08 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 60 "/\\WR"))
    (pad "c23" thru_hole circle locked (at 55.88 5.08 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 61 "/B_A20"))
    (pad "c24" thru_hole circle locked (at 58.42 5.08 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 178 "/nRD"))
    (pad "c25" thru_hole circle locked (at 60.96 5.08 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 62 "/\\HALT"))
    (pad "c26" thru_hole circle locked (at 63.5 5.08 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 63 "/\\RESOUT"))
    (pad "c27" thru_hole circle locked (at 66.04 5.08 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 64 "/B_A12"))
    (pad "c28" thru_hole circle locked (at 68.58 5.08 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 65 "/B_A15"))
    (pad "c29" thru_hole circle locked (at 71.12 5.08 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 179 "/nCLK"))
    (pad "c30" thru_hole circle locked (at 73.66 5.08 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 67 "/\\MREQ"))
    (pad "c31" thru_hole circle locked (at 76.2 5.08 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 68 "/\\RESET"))
    (pad "c32" thru_hole circle locked (at 78.74 5.08 90) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (model "${KICAD6_3DMODEL_DIR}//3D-Spezial/walter/conn_din41612/DIN64_M_90.wrl"
      (offset (xyz 39.5 -2.6 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (footprint "Relay_THT:Relay_StandexMeder_DIP_LowProfile" (layer "F.Cu")
    (tedit 5A54BF5F)
    (at 218.44 67.31 90)
    (descr "package for Standex Meder DIP reed relay series, see https://standexelectronics.com/wp-content/uploads/datasheet_reed_relay_DIP.pdf")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil reed relay")
    (attr through_hole)
    (fp_text reference "K1" (at 3.81 -3.39 90) (layer "F.SilkS"))
    (fp_text value "DIPxx-1Axx-12xD" (at 3.81 18.63 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.815 7.62 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 "Net-(C8-Pad1)"))
    (pad "2" thru_hole circle locked (at 0 2.54 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 "VCC"))
    (pad "6" thru_hole circle locked (at 0 12.8 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 95 "Net-(K1-Pad6)"))
    (pad "7" thru_hole circle locked (at 0 15.24 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 69 "/VccE"))
    (pad "8" thru_hole circle locked (at 7.62 15.24 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 69 "/VccE"))
    (pad "9" thru_hole circle locked (at 7.62 12.8 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
    (pad "13" thru_hole circle locked (at 7.62 2.54 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 "VCC"))
    (pad "14" thru_hole circle locked (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 "Net-(C8-Pad1)"))
    (model "${KICAD6_3DMODEL_DIR}/Relay_THT.3dshapes/Relay_StandexMeder_DIP_LowProfile.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Relay_THT:Relay_StandexMeder_DIP_LowProfile" (layer "F.Cu")
    (tedit 5A54BF5F)
    (at 203.2 123.19)
    (descr "package for Standex Meder DIP reed relay series, see https://standexelectronics.com/wp-content/uploads/datasheet_reed_relay_DIP.pdf")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil reed relay")
    (attr through_hole)
    (fp_text reference "K2" (at 3.81 -3.39) (layer "F.SilkS"))
    (fp_text value "DIPxx-1Axx-12xD" (at 3.81 18.63) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.815 7.62) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 175 "Net-(K2-Pad1)"))
    (pad "2" thru_hole circle locked (at 0 2.54) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 "VCC"))
    (pad "6" thru_hole circle locked (at 0 12.8) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 96 "Net-(K2-Pad6)"))
    (pad "7" thru_hole circle locked (at 0 15.24) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 69 "/VccE"))
    (pad "8" thru_hole circle locked (at 7.62 15.24) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 69 "/VccE"))
    (pad "9" thru_hole circle locked (at 7.62 12.8) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
    (pad "13" thru_hole circle locked (at 7.62 2.54) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 "VCC"))
    (pad "14" thru_hole circle locked (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 175 "Net-(K2-Pad1)"))
    (model "${KICAD6_3DMODEL_DIR}/Relay_THT.3dshapes/Relay_StandexMeder_DIP_LowProfile.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-92" (layer "F.Cu")
    (tedit 5A279852)
    (at 234.95 102.87)
    (descr "TO-92 leads molded, narrow, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (attr through_hole)
    (fp_text reference "Q1" (at 1.27 -3.56) (layer "F.SilkS"))
    (fp_text value "BC558" (at 1.27 2.79) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 0) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 79 "/EA11"))
    (pad "2" thru_hole circle locked (at 1.27 -1.27) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 99 "Net-(Q1-Pad2)"))
    (pad "3" thru_hole circle locked (at 2.54 0) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 8 "/+25V"))
    (model "${KICAD6_3DMODEL_DIR}/TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Narrow.wrl"
      (offset (xyz 1.3 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-92" (layer "F.Cu")
    (tedit 5A279852)
    (at 234.95 88.9)
    (descr "TO-92 leads molded, narrow, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (attr through_hole)
    (fp_text reference "Q2" (at 1.27 -3.56) (layer "F.SilkS"))
    (fp_text value "BC558" (at 1.27 2.79) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 0) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 81 "/nOE"))
    (pad "2" thru_hole circle locked (at 1.27 -1.27) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 100 "Net-(Q2-Pad2)"))
    (pad "3" thru_hole circle locked (at 2.54 0) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 8 "/+25V"))
    (model "${KICAD6_3DMODEL_DIR}/TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Narrow.wrl"
      (offset (xyz 1.3 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-92" (layer "F.Cu")
    (tedit 5A279852)
    (at 227.33 71.12)
    (descr "TO-92 leads molded, narrow, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (attr through_hole)
    (fp_text reference "Q3" (at 1.27 -3.56) (layer "F.SilkS"))
    (fp_text value "BC558" (at 1.27 2.79) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 0) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 81 "/nOE"))
    (pad "2" thru_hole circle locked (at 1.27 -1.27) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 101 "Net-(Q3-Pad2)"))
    (pad "3" thru_hole circle locked (at 2.54 0) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 9 "Net-(D1-Pad2)"))
    (model "${KICAD6_3DMODEL_DIR}/TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Narrow.wrl"
      (offset (xyz 1.3 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 94.107 109.855)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (attr through_hole)
    (fp_text reference "R1" (at 3.81 -2.37) (layer "F.SilkS"))
    (fp_text value "1k" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "VCC"))
    (pad "2" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 104 "Net-(R1-Pad2)"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial/1_braun.wrl"
      (offset (xyz 2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial/0_schwarz.wrl"
      (offset (xyz 2.75 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial/2_rot.wrl"
      (offset (xyz 3.5 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial/5_gold.wrl"
      (offset (xyz 5 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 93.98 104.775)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (attr through_hole)
    (fp_text reference "R2" (at 3.81 -2.37) (layer "F.SilkS"))
    (fp_text value "1k" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "VCC"))
    (pad "2" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 105 "Net-(R2-Pad2)"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial/1_braun.wrl"
      (offset (xyz 2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial/0_schwarz.wrl"
      (offset (xyz 2.75 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial/2_rot.wrl"
      (offset (xyz 3.5 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial/5_gold.wrl"
      (offset (xyz 5 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 93.98 92.075)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (attr through_hole)
    (fp_text reference "R4" (at 3.81 -2.37) (layer "F.SilkS"))
    (fp_text value "1k" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "VCC"))
    (pad "2" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 107 "Net-(R4-Pad2)"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial/1_braun.wrl"
      (offset (xyz 2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial/0_schwarz.wrl"
      (offset (xyz 2.75 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial/2_rot.wrl"
      (offset (xyz 3.5 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial/5_gold.wrl"
      (offset (xyz 5 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 133.35 60.96 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (attr through_hole)
    (fp_text reference "R5" (at 3.81 -2.37) (layer "F.SilkS"))
    (fp_text value "1" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 98 "Net-(L1-Pad2)"))
    (pad "2" thru_hole oval locked (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "VCC"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/1_braun.wrl"
      (offset (xyz 2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/0_schwarz.wrl"
      (offset (xyz 2.75 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/5_gold.wrl"
      (offset (xyz 3.5 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/5_gold.wrl"
      (offset (xyz 5 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 152.4 76.2)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (attr through_hole)
    (fp_text reference "R6" (at 3.81 -2.37) (layer "F.SilkS"))
    (fp_text value "33k" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 108 "Net-(R6-Pad1)"))
    (pad "2" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//3_orange.wrl"
      (offset (xyz 2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//3_orange.wrl"
      (offset (xyz 2.75 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//3_orange.wrl"
      (offset (xyz 3.5 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//5_gold.wrl"
      (offset (xyz 5 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Potentiometer_THT:Potentiometer_ACP_CA9-V10_Vertical" (layer "F.Cu")
    (tedit 5A3D4994)
    (at 163.83 68.58 -90)
    (descr "Potentiometer, vertical, ACP CA9-V10, http://www.acptechnologies.com/wp-content/uploads/2017/05/02-ACP-CA9-CE9.pdf")
    (tags "Potentiometer vertical ACP CA9-V10")
    (attr through_hole)
    (fp_text reference "R7" (at 5 -8.65 90) (layer "F.SilkS"))
    (fp_text value "1k" (at 5 3.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1 -2.5) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 270) (size 2.34 2.34) (drill 1.3) (layers *.Cu *.Mask)
      (net 108 "Net-(R6-Pad1)"))
    (pad "2" thru_hole circle locked (at 10 -2.5 270) (size 2.34 2.34) (drill 1.3) (layers *.Cu *.Mask)
      (net 109 "Net-(R7-Pad2)"))
    (pad "3" thru_hole circle locked (at 0 -5 270) (size 2.34 2.34) (drill 1.3) (layers *.Cu *.Mask))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometers.3dshapes/Potentiometer_Trimmer_ACP_CA14v_Horizontal_Px15.0mm_Py10.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.26 0.2 0.2))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 152.4 73.66)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (attr through_hole)
    (fp_text reference "R8" (at 3.81 -2.37) (layer "F.SilkS"))
    (fp_text value "1k" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 4.067999 0.049999) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (pad "2" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 109 "Net-(R7-Pad2)"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//1_braun.wrl"
      (offset (xyz 2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//0_schwarz.wrl"
      (offset (xyz 2.75 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//2_rot.wrl"
      (offset (xyz 3.5 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//5_gold.wrl"
      (offset (xyz 5 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 152.4 78.74)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (attr through_hole)
    (fp_text reference "R9" (at 3.81 -2.37) (layer "F.SilkS"))
    (fp_text value "4.7" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "/+25V"))
    (pad "2" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//4_gelb.wrl"
      (offset (xyz 2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//7_lila.wrl"
      (offset (xyz 2.75 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//5_gold.wrl"
      (offset (xyz 3.5 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//5_gold.wrl"
      (offset (xyz 5 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 232.41 105.41 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (attr through_hole)
    (fp_text reference "R10" (at 3.81 -2.37 90) (layer "F.SilkS"))
    (fp_text value "1k" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "/+25V"))
    (pad "2" thru_hole oval locked (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 99 "Net-(Q1-Pad2)"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//1_braun.wrl"
      (offset (xyz 2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//0_schwarz.wrl"
      (offset (xyz 2.75 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//2_rot.wrl"
      (offset (xyz 3.5 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//5_gold.wrl"
      (offset (xyz 5 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 228.6 97.79 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (attr through_hole)
    (fp_text reference "R11" (at 3.81 -2.37 90) (layer "F.SilkS"))
    (fp_text value "10k" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 99 "Net-(Q1-Pad2)"))
    (pad "2" thru_hole oval locked (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 110 "Net-(R11-Pad2)"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//1_braun.wrl"
      (offset (xyz 2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//0_schwarz.wrl"
      (offset (xyz 2.75 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//3_orange.wrl"
      (offset (xyz 3.5 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//5_gold.wrl"
      (offset (xyz 5 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 232.41 91.44 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (attr through_hole)
    (fp_text reference "R12" (at 3.81 -2.37 90) (layer "F.SilkS"))
    (fp_text value "1k" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "/+25V"))
    (pad "2" thru_hole oval locked (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 100 "Net-(Q2-Pad2)"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//1_braun.wrl"
      (offset (xyz 2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//0_schwarz.wrl"
      (offset (xyz 2.756 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//2_rot.wrl"
      (offset (xyz 3.5 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//5_gold.wrl"
      (offset (xyz 5 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 228.6 83.82 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (attr through_hole)
    (fp_text reference "R13" (at 3.81 -2.37 90) (layer "F.SilkS"))
    (fp_text value "10k" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 100 "Net-(Q2-Pad2)"))
    (pad "2" thru_hole oval locked (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 111 "Net-(R13-Pad2)"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//1_braun.wrl"
      (offset (xyz 2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//0_schwarz.wrl"
      (offset (xyz 2.75 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//3_orange.wrl"
      (offset (xyz 3.5 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//5_gold.wrl"
      (offset (xyz 5 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 237.49 78.74 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (attr through_hole)
    (fp_text reference "R14" (at 3.81 -2.37 90) (layer "F.SilkS"))
    (fp_text value "1k" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(D1-Pad2)"))
    (pad "2" thru_hole oval locked (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 101 "Net-(Q3-Pad2)"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//1_braun.wrl"
      (offset (xyz 2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//0_schwarz.wrl"
      (offset (xyz 2.75 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//2_rot.wrl"
      (offset (xyz 3.5 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//5_gold.wrl"
      (offset (xyz 5 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 233.68 71.12 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (attr through_hole)
    (fp_text reference "R15" (at 3.81 -2.37 90) (layer "F.SilkS"))
    (fp_text value "10k" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 101 "Net-(Q3-Pad2)"))
    (pad "2" thru_hole oval locked (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 112 "Net-(R15-Pad2)"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//1_braun.wrl"
      (offset (xyz 2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//0_schwarz.wrl"
      (offset (xyz 2.75 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//3_orange.wrl"
      (offset (xyz 3.5 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//5_gold.wrl"
      (offset (xyz 5 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 232.41 119.38 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (attr through_hole)
    (fp_text reference "R16" (at 3.81 -2.37 90) (layer "F.SilkS"))
    (fp_text value "1k" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(D1-Pad2)"))
    (pad "2" thru_hole oval locked (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 102 "Net-(Q4-Pad2)"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//1_Braun.wrl"
      (offset (xyz 2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//0_schwarz.wrl"
      (offset (xyz 2.75 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//5_gold.wrl"
      (offset (xyz 5 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//2_rot.wrl"
      (offset (xyz 3.5 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 228.6 111.76 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (attr through_hole)
    (fp_text reference "R17" (at 3.81 -2.37 90) (layer "F.SilkS"))
    (fp_text value "10k" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 102 "Net-(Q4-Pad2)"))
    (pad "2" thru_hole oval locked (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 113 "Net-(R17-Pad2)"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//1_Braun.wrl"
      (offset (xyz 2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//0_schwarz.wrl"
      (offset (xyz 2.75 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//3_orange.wrl"
      (offset (xyz 3.5 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//5_gold.wrl"
      (offset (xyz 5 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 232.41 133.35 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (attr through_hole)
    (fp_text reference "R18" (at 3.81 -2.37 90) (layer "F.SilkS"))
    (fp_text value "1k" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.8735 0.0635 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(D2-Pad2)"))
    (pad "2" thru_hole oval locked (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 103 "Net-(Q5-Pad2)"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//1_Braun.wrl"
      (offset (xyz 2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//0_schwarz.wrl"
      (offset (xyz 2.75 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//2_rot.wrl"
      (offset (xyz 3.5 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//5_gold.wrl"
      (offset (xyz 5 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 233.68 137.16 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (attr through_hole)
    (fp_text reference "R20" (at 3.81 -2.37) (layer "F.SilkS"))
    (fp_text value "100k" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "/Vpp"))
    (pad "2" thru_hole oval locked (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//1_braun.wrl"
      (offset (xyz 2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//0_schwarz.wrl"
      (offset (xyz 2.75 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//4_gelb.wrl"
      (offset (xyz 3.5 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//5_gold.wrl"
      (offset (xyz 5 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 198.12 119.38 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (attr through_hole)
    (fp_text reference "R21" (at 3.81 -2.37 90) (layer "F.SilkS"))
    (fp_text value "100k" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (pad "2" thru_hole oval locked (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 79 "/EA11"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//1_braun.wrl"
      (offset (xyz 2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//0_schwarz.wrl"
      (offset (xyz 2.75 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//4_gelb.wrl"
      (offset (xyz 3.5 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//5_gold.wrl"
      (offset (xyz 5 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 215.9 76.2)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (attr through_hole)
    (fp_text reference "R22" (at 3.81 -2.37) (layer "F.SilkS"))
    (fp_text value "100k" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (pad "2" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 81 "/nOE"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//1_braun.wrl"
      (offset (xyz 2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//0_schwarz.wrl"
      (offset (xyz 2.75 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//4_gelb.wrl"
      (offset (xyz 3.5 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//5_gold.wrl"
      (offset (xyz 5 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 226.06 140.97)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (attr through_hole)
    (fp_text reference "R23" (at 3.81 -2.37) (layer "F.SilkS"))
    (fp_text value "2.2k" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 79 "/EA11"))
    (pad "2" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(D4-Pad1)"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//0_schwarz.wrl"
      (offset (xyz 2.75 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//1_Braun.wrl"
      (offset (xyz 2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//2_rot.wrl"
      (offset (xyz 3.5 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//5_gold.wrl"
      (offset (xyz 5 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 223.52 73.66 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (attr through_hole)
    (fp_text reference "R24" (at 3.81 -2.37) (layer "F.SilkS"))
    (fp_text value "2.2k" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 81 "/nOE"))
    (pad "2" thru_hole oval locked (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(D5-Pad1)"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//2_rot.wrl"
      (offset (xyz 2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//2_rot.wrl"
      (offset (xyz 2.75 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//2_rot.wrl"
      (offset (xyz 3.5 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//5_gold.wrl"
      (offset (xyz 5 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Potentiometer_THT:Potentiometer_ACP_CA9-V10_Vertical" (layer "F.Cu")
    (tedit 5A3D4994)
    (at 187.96 80.01 -90)
    (descr "Potentiometer, vertical, ACP CA9-V10, http://www.acptechnologies.com/wp-content/uploads/2017/05/02-ACP-CA9-CE9.pdf")
    (tags "Potentiometer vertical ACP CA9-V10")
    (attr through_hole)
    (fp_text reference "R25" (at 5 -8.65 90) (layer "F.SilkS"))
    (fp_text value "1k" (at 5 3.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1 -2.5) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 270) (size 2.34 2.34) (drill 1.3) (layers *.Cu *.Mask)
      (net 5 "Net-(C7-Pad2)"))
    (pad "2" thru_hole circle locked (at 10 -2.5 270) (size 2.34 2.34) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (pad "3" thru_hole circle locked (at 0 -5 270) (size 2.34 2.34) (drill 1.3) (layers *.Cu *.Mask))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometers.3dshapes/Potentiometer_Trimmer_ACP_CA14v_Horizontal_Px15.0mm_Py10.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.26 0.2 0.2))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 198.12 123.19 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (attr through_hole)
    (fp_text reference "R26" (at 3.81 -2.37 90) (layer "F.SilkS"))
    (fp_text value "1k" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (pad "2" thru_hole oval locked (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 175 "Net-(K2-Pad1)"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/0_schwarz.wrl"
      (offset (xyz 2.75 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/1_Braun.wrl"
      (offset (xyz 2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/2_rot.wrl"
      (offset (xyz 3.5 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/5_gold.wrl"
      (offset (xyz 5 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-20_W7.62mm_LongPads" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 106.67 116.84)
    (descr "20-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads")
    (attr through_hole)
    (fp_text reference "U1" (at 3.81 -2.33) (layer "F.SilkS"))
    (fp_text value "74LS245" (at 3.81 25.19) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 4.054999 11.493499) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 123 "Net-(U1-Pad1)"))
    (pad "2" thru_hole oval locked (at 0 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "/B_D7"))
    (pad "3" thru_hole oval locked (at 0 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "/B_D6"))
    (pad "4" thru_hole oval locked (at 0 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "/B_D5"))
    (pad "5" thru_hole oval locked (at 0 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "/B_D4"))
    (pad "6" thru_hole oval locked (at 0 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "/B_D3"))
    (pad "7" thru_hole oval locked (at 0 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "/B_D2"))
    (pad "8" thru_hole oval locked (at 0 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 "/B_D1"))
    (pad "9" thru_hole oval locked (at 0 20.32) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "/B_D0"))
    (pad "10" thru_hole oval locked (at 0 22.86) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (pad "11" thru_hole oval locked (at 7.62 22.86) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 122 "Net-(U1-Pad11)"))
    (pad "12" thru_hole oval locked (at 7.62 20.32) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 121 "Net-(U1-Pad12)"))
    (pad "13" thru_hole oval locked (at 7.62 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 120 "Net-(U1-Pad13)"))
    (pad "14" thru_hole oval locked (at 7.62 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 119 "Net-(U1-Pad14)"))
    (pad "15" thru_hole oval locked (at 7.62 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 118 "Net-(U1-Pad15)"))
    (pad "16" thru_hole oval locked (at 7.62 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 117 "Net-(U1-Pad16)"))
    (pad "17" thru_hole oval locked (at 7.62 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 116 "Net-(U1-Pad17)"))
    (pad "18" thru_hole oval locked (at 7.62 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 115 "Net-(U1-Pad18)"))
    (pad "19" thru_hole oval locked (at 7.62 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 114 "Net-(U1-Pad19)"))
    (pad "20" thru_hole oval locked (at 7.62 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "VCC"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-20_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-16_W7.62mm" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 123.19 115.57)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (attr through_hole)
    (fp_text reference "U2" (at 3.81 -2.33) (layer "F.SilkS"))
    (fp_text value "74LS139" (at 3.81 20.11) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 8.89) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 114 "Net-(U1-Pad19)"))
    (pad "2" thru_hole oval locked (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "/B_A2"))
    (pad "3" thru_hole oval locked (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "/B_A3"))
    (pad "4" thru_hole oval locked (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 124 "Net-(U2-Pad4)"))
    (pad "5" thru_hole oval locked (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 125 "Net-(U2-Pad5)"))
    (pad "6" thru_hole oval locked (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 126 "Net-(U2-Pad6)"))
    (pad "7" thru_hole oval locked (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 127 "Net-(U2-Pad7)"))
    (pad "8" thru_hole oval locked (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (pad "9" thru_hole oval locked (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "10" thru_hole oval locked (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "11" thru_hole oval locked (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "12" thru_hole oval locked (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "13" thru_hole oval locked (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "14" thru_hole oval locked (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "15" thru_hole oval locked (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "16" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "VCC"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-16_W7.62mm_Socket" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 106.67 90.31)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (attr through_hole)
    (fp_text reference "U3" (at 3.81 -2.33) (layer "F.SilkS"))
    (fp_text value "74LS85" (at 3.81 20.11) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 8.89) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 107 "Net-(R4-Pad2)"))
    (pad "2" thru_hole oval locked (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 128 "Net-(U3-Pad2)"))
    (pad "3" thru_hole oval locked (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 129 "Net-(U3-Pad3)"))
    (pad "4" thru_hole oval locked (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (pad "5" thru_hole oval locked (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 130 "Net-(U3-Pad5)"))
    (pad "6" thru_hole oval locked (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 131 "Net-(U3-Pad6)"))
    (pad "7" thru_hole oval locked (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (pad "8" thru_hole oval locked (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (pad "9" thru_hole oval locked (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 104 "Net-(R1-Pad2)"))
    (pad "10" thru_hole oval locked (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "/B_A4"))
    (pad "11" thru_hole oval locked (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 105 "Net-(R2-Pad2)"))
    (pad "12" thru_hole oval locked (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "/B_A5"))
    (pad "13" thru_hole oval locked (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "/B_A6"))
    (pad "14" thru_hole oval locked (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 106 "Net-(R3-Pad2)"))
    (pad "15" thru_hole oval locked (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "/B_A7"))
    (pad "16" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "VCC"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-16_W7.62mm_Socket.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl"
      (offset (xyz 0 0 3.3528))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-14_W7.62mm" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 123.19 72.39)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (attr through_hole)
    (fp_text reference "U4" (at 3.81 -2.33) (layer "F.SilkS"))
    (fp_text value "74LS00" (at 3.81 17.57) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 7.62) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 131 "Net-(U3-Pad6)"))
    (pad "2" thru_hole oval locked (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 131 "Net-(U3-Pad6)"))
    (pad "3" thru_hole oval locked (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 114 "Net-(U1-Pad19)"))
    (pad "4" thru_hole oval locked (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 132 "Net-(U4-Pad4)"))
    (pad "5" thru_hole oval locked (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 132 "Net-(U4-Pad4)"))
    (pad "6" thru_hole oval locked (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 129 "Net-(U3-Pad3)"))
    (pad "7" thru_hole oval locked (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (pad "8" thru_hole oval locked (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "9" thru_hole oval locked (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "10" thru_hole oval locked (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "11" thru_hole oval locked (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "12" thru_hole oval locked (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "13" thru_hole oval locked (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "14" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "VCC"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-14_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-20_W7.62mm_LongPads" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 106.67 57.29)
    (descr "20-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads")
    (attr through_hole)
    (fp_text reference "U5" (at 3.81 -2.33) (layer "F.SilkS"))
    (fp_text value "74LS245" (at 3.81 25.19) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 11.43) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 133 "Net-(U5-Pad1)"))
    (pad "2" thru_hole oval locked (at 0 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 176 "/nM1"))
    (pad "3" thru_hole oval locked (at 0 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 177 "/nIORQ"))
    (pad "4" thru_hole oval locked (at 0 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 179 "/nCLK"))
    (pad "5" thru_hole oval locked (at 0 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 178 "/nRD"))
    (pad "6" thru_hole oval locked (at 0 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 138 "Net-(U5-Pad6)"))
    (pad "7" thru_hole oval locked (at 0 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 139 "Net-(U5-Pad7)"))
    (pad "8" thru_hole oval locked (at 0 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "/B_A0"))
    (pad "9" thru_hole oval locked (at 0 20.32) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 "/B_A1"))
    (pad "10" thru_hole oval locked (at 0 22.86) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (pad "11" thru_hole oval locked (at 7.62 22.86) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 134 "Net-(U5-Pad11)"))
    (pad "12" thru_hole oval locked (at 7.62 20.32) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 135 "Net-(U5-Pad12)"))
    (pad "13" thru_hole oval locked (at 7.62 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 136 "Net-(U5-Pad13)"))
    (pad "14" thru_hole oval locked (at 7.62 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 137 "Net-(U5-Pad14)"))
    (pad "15" thru_hole oval locked (at 7.62 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 123 "Net-(U1-Pad1)"))
    (pad "16" thru_hole oval locked (at 7.62 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 66 "/\\CLK"))
    (pad "17" thru_hole oval locked (at 7.62 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 132 "Net-(U4-Pad4)"))
    (pad "18" thru_hole oval locked (at 7.62 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "/\\M1"))
    (pad "19" thru_hole oval locked (at 7.62 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 140 "Net-(U5-Pad19)"))
    (pad "20" thru_hole oval locked (at 7.62 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "VCC"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-20_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-40_W15.24mm" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 144.78 135.89 90)
    (descr "40-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil")
    (attr through_hole)
    (fp_text reference "U6" (at 7.62 -2.33 90) (layer "F.SilkS"))
    (fp_text value "Z8420" (at 7.62 50.59 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.62 24.13 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 120 "Net-(U1-Pad13)"))
    (pad "2" thru_hole oval locked (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 115 "Net-(U1-Pad18)"))
    (pad "3" thru_hole oval locked (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 116 "Net-(U1-Pad17)"))
    (pad "4" thru_hole oval locked (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 126 "Net-(U2-Pad6)"))
    (pad "5" thru_hole oval locked (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 134 "Net-(U5-Pad11)"))
    (pad "6" thru_hole oval locked (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 135 "Net-(U5-Pad12)"))
    (pad "7" thru_hole oval locked (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 72 "/EA7"))
    (pad "8" thru_hole oval locked (at 0 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 74 "/EA6"))
    (pad "9" thru_hole oval locked (at 0 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 76 "/EA5"))
    (pad "10" thru_hole oval locked (at 0 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 78 "/EA4"))
    (pad "11" thru_hole oval locked (at 0 25.4 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (pad "12" thru_hole oval locked (at 0 27.94 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 80 "/EA3"))
    (pad "13" thru_hole oval locked (at 0 30.48 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 82 "/EA2"))
    (pad "14" thru_hole oval locked (at 0 33.02 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 84 "/EA1"))
    (pad "15" thru_hole oval locked (at 0 35.56 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 86 "/EA0"))
    (pad "16" thru_hole oval locked (at 0 38.1 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 150 "Net-(U6-Pad16)"))
    (pad "17" thru_hole oval locked (at 0 40.64 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 151 "Net-(U6-Pad17)"))
    (pad "18" thru_hole oval locked (at 0 43.18 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 152 "Net-(U6-Pad18)"))
    (pad "19" thru_hole oval locked (at 0 45.72 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 122 "Net-(U1-Pad11)"))
    (pad "20" thru_hole oval locked (at 0 48.26 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 121 "Net-(U1-Pad12)"))
    (pad "21" thru_hole oval locked (at 15.24 48.26 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 141 "Net-(U6-Pad21)"))
    (pad "22" thru_hole oval locked (at 15.24 45.72 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 142 "Net-(U6-Pad22)"))
    (pad "23" thru_hole oval locked (at 15.24 43.18 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 143 "Net-(U6-Pad23)"))
    (pad "24" thru_hole oval locked (at 15.24 40.64 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 144 "Net-(U6-Pad24)"))
    (pad "25" thru_hole oval locked (at 15.24 38.1 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 66 "/\\CLK"))
    (pad "26" thru_hole oval locked (at 15.24 35.56 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 145 "Net-(U6-Pad26)"))
    (pad "27" thru_hole oval locked (at 15.24 33.02 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 75 "/EA8"))
    (pad "28" thru_hole oval locked (at 15.24 30.48 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 77 "/EA9"))
    (pad "29" thru_hole oval locked (at 15.24 27.94 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 83 "/EA10"))
    (pad "30" thru_hole oval locked (at 15.24 25.4 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 146 "/paEA11"))
    (pad "31" thru_hole oval locked (at 15.24 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 70 "/EA12"))
    (pad "32" thru_hole oval locked (at 15.24 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 147 "/paEA13"))
    (pad "33" thru_hole oval locked (at 15.24 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 148 "/paEA14"))
    (pad "34" thru_hole oval locked (at 15.24 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 149 "/paEA15"))
    (pad "35" thru_hole oval locked (at 15.24 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 123 "Net-(U1-Pad1)"))
    (pad "36" thru_hole oval locked (at 15.24 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 132 "Net-(U4-Pad4)"))
    (pad "37" thru_hole oval locked (at 15.24 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "/\\M1"))
    (pad "38" thru_hole oval locked (at 15.24 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 117 "Net-(U1-Pad16)"))
    (pad "39" thru_hole oval locked (at 15.24 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 118 "Net-(U1-Pad15)"))
    (pad "40" thru_hole oval locked (at 15.24 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 119 "Net-(U1-Pad14)"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-40_W15.24mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-40_W15.24mm" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 144.78 113.03 90)
    (descr "40-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil")
    (attr through_hole)
    (fp_text reference "U7" (at 7.62 -2.33 90) (layer "F.SilkS"))
    (fp_text value "Z8420" (at 7.62 50.59 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.62 24.13 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 120 "Net-(U1-Pad13)"))
    (pad "2" thru_hole oval locked (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 115 "Net-(U1-Pad18)"))
    (pad "3" thru_hole oval locked (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 116 "Net-(U1-Pad17)"))
    (pad "4" thru_hole oval locked (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 127 "Net-(U2-Pad7)"))
    (pad "5" thru_hole oval locked (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 135 "Net-(U5-Pad12)"))
    (pad "6" thru_hole oval locked (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 134 "Net-(U5-Pad11)"))
    (pad "7" thru_hole oval locked (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 87 "/ED7"))
    (pad "8" thru_hole oval locked (at 0 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 89 "/ED6"))
    (pad "9" thru_hole oval locked (at 0 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 91 "/ED5"))
    (pad "10" thru_hole oval locked (at 0 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 93 "/ED4"))
    (pad "11" thru_hole oval locked (at 0 25.4 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (pad "12" thru_hole oval locked (at 0 27.94 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 94 "/ED3"))
    (pad "13" thru_hole oval locked (at 0 30.48 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 92 "/ED2"))
    (pad "14" thru_hole oval locked (at 0 33.02 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 90 "/ED1"))
    (pad "15" thru_hole oval locked (at 0 35.56 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 88 "/ED0"))
    (pad "16" thru_hole oval locked (at 0 38.1 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 155 "Net-(U7-Pad16)"))
    (pad "17" thru_hole oval locked (at 0 40.64 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 154 "Net-(U7-Pad17)"))
    (pad "18" thru_hole oval locked (at 0 43.18 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 153 "Net-(U7-Pad18)"))
    (pad "19" thru_hole oval locked (at 0 45.72 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 122 "Net-(U1-Pad11)"))
    (pad "20" thru_hole oval locked (at 0 48.26 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 121 "Net-(U1-Pad12)"))
    (pad "21" thru_hole oval locked (at 15.24 48.26 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 166 "Net-(U7-Pad21)"))
    (pad "22" thru_hole oval locked (at 15.24 45.72 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 165 "Net-(U7-Pad22)"))
    (pad "23" thru_hole oval locked (at 15.24 43.18 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 164 "Net-(U7-Pad23)"))
    (pad "24" thru_hole oval locked (at 15.24 40.64 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 163 "Net-(U7-Pad24)"))
    (pad "25" thru_hole oval locked (at 15.24 38.1 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 66 "/\\CLK"))
    (pad "26" thru_hole oval locked (at 15.24 35.56 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "VCC"))
    (pad "27" thru_hole oval locked (at 15.24 33.02 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 162 "/pbEA16"))
    (pad "28" thru_hole oval locked (at 15.24 30.48 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 161 "/pbEA17"))
    (pad "29" thru_hole oval locked (at 15.24 27.94 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 160 "/pbEA18"))
    (pad "30" thru_hole oval locked (at 15.24 25.4 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 159 "/pbEA19"))
    (pad "31" thru_hole oval locked (at 15.24 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 158 "/pbEA20"))
    (pad "32" thru_hole oval locked (at 15.24 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 157 "/pbEA21"))
    (pad "33" thru_hole oval locked (at 15.24 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 156 "/pbEA22"))
    (pad "34" thru_hole oval locked (at 15.24 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 85 "/nCE"))
    (pad "35" thru_hole oval locked (at 15.24 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 123 "Net-(U1-Pad1)"))
    (pad "36" thru_hole oval locked (at 15.24 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 132 "Net-(U4-Pad4)"))
    (pad "37" thru_hole oval locked (at 15.24 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "/\\M1"))
    (pad "38" thru_hole oval locked (at 15.24 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 117 "Net-(U1-Pad16)"))
    (pad "39" thru_hole oval locked (at 15.24 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 118 "Net-(U1-Pad15)"))
    (pad "40" thru_hole oval locked (at 15.24 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 119 "Net-(U1-Pad14)"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-40_W15.24mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-14_W7.62mm" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 203.2 73.66)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (attr through_hole)
    (fp_text reference "U8" (at 3.81 -2.33) (layer "F.SilkS"))
    (fp_text value "74LS07" (at 3.81 17.57) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 7.62) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 156 "/pbEA22"))
    (pad "2" thru_hole oval locked (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 71 "/nPGM"))
    (pad "3" thru_hole oval locked (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 158 "/pbEA20"))
    (pad "4" thru_hole oval locked (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 95 "Net-(K1-Pad6)"))
    (pad "5" thru_hole oval locked (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 160 "/pbEA18"))
    (pad "6" thru_hole oval locked (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 112 "Net-(R15-Pad2)"))
    (pad "7" thru_hole oval locked (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (pad "8" thru_hole oval locked (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 111 "Net-(R13-Pad2)"))
    (pad "9" thru_hole oval locked (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 161 "/pbEA17"))
    (pad "10" thru_hole oval locked (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 113 "Net-(R17-Pad2)"))
    (pad "11" thru_hole oval locked (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 159 "/pbEA19"))
    (pad "12" thru_hole oval locked (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 81 "/nOE"))
    (pad "13" thru_hole oval locked (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 157 "/pbEA21"))
    (pad "14" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "VCC"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-14_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-14_W7.62mm" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 203.2 100.33)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (attr through_hole)
    (fp_text reference "U9" (at 3.81 -2.33) (layer "F.SilkS"))
    (fp_text value "74LS07" (at 3.81 17.57) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 7.62) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 162 "/pbEA16"))
    (pad "2" thru_hole oval locked (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 110 "Net-(R11-Pad2)"))
    (pad "3" thru_hole oval locked (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 147 "/paEA13"))
    (pad "4" thru_hole oval locked (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 "Net-(K2-Pad6)"))
    (pad "5" thru_hole oval locked (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 148 "/paEA14"))
    (pad "6" thru_hole oval locked (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 173 "Net-(J3-Pad1)"))
    (pad "7" thru_hole oval locked (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (pad "8" thru_hole oval locked (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 168 "Net-(U9-Pad8)"))
    (pad "9" thru_hole oval locked (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 167 "Net-(U9-Pad9)"))
    (pad "10" thru_hole oval locked (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 79 "/EA11"))
    (pad "11" thru_hole oval locked (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 146 "/paEA11"))
    (pad "12" thru_hole oval locked (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C7-Pad2)"))
    (pad "13" thru_hole oval locked (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 149 "/paEA15"))
    (pad "14" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "VCC"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-14_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-92" (layer "F.Cu")
    (tedit 5A279852)
    (at 234.95 116.84)
    (descr "TO-92 leads molded, narrow, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (attr through_hole)
    (fp_text reference "Q4" (at 1.27 -3.56) (layer "F.SilkS"))
    (fp_text value "BC558" (at 1.27 2.79) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 0) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 11 "/Vpp"))
    (pad "2" thru_hole circle locked (at 1.27 -1.27) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 102 "Net-(Q4-Pad2)"))
    (pad "3" thru_hole circle locked (at 2.54 0) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 9 "Net-(D1-Pad2)"))
    (model "${KICAD6_3DMODEL_DIR}/TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Narrow.wrl"
      (offset (xyz 1.3 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-92" (layer "F.Cu")
    (tedit 5A279852)
    (at 234.95 130.81)
    (descr "TO-92 leads molded, narrow, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (attr through_hole)
    (fp_text reference "Q5" (at 1.27 -3.56) (layer "F.SilkS"))
    (fp_text value "BC558" (at 1.27 2.79) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 0) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 11 "/Vpp"))
    (pad "2" thru_hole circle locked (at 1.27 -1.27) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 103 "Net-(Q5-Pad2)"))
    (pad "3" thru_hole circle locked (at 2.54 0) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 10 "Net-(D2-Pad2)"))
    (model "${KICAD6_3DMODEL_DIR}/TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Narrow.wrl"
      (offset (xyz 1.3 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (footprint "Package_DIP:DIP-14_W7.62mm" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 142.24 60.96)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (attr through_hole)
    (fp_text reference "U11" (at 3.81 -2.33) (layer "F.SilkS"))
    (fp_text value "TL497" (at 3.81 17.57) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 7.62) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 108 "Net-(R6-Pad1)"))
    (pad "2" thru_hole oval locked (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (pad "3" thru_hole oval locked (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad "4" thru_hole oval locked (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (pad "5" thru_hole oval locked (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (pad "6" thru_hole oval locked (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad "7" thru_hole oval locked (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 97 "Net-(L1-Pad1)"))
    (pad "8" thru_hole oval locked (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (pad "9" thru_hole oval locked (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 169 "Net-(U11-Pad9)"))
    (pad "10" thru_hole oval locked (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 97 "Net-(L1-Pad1)"))
    (pad "11" thru_hole oval locked (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 170 "Net-(U11-Pad11)"))
    (pad "12" thru_hole oval locked (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 171 "Net-(U11-Pad12)"))
    (pad "13" thru_hole oval locked (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 98 "Net-(L1-Pad2)"))
    (pad "14" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "VCC"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-14_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 228.6 125.73 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (attr through_hole)
    (fp_text reference "R19" (at 3.81 -2.37 90) (layer "F.SilkS"))
    (fp_text value "10k" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 103 "Net-(Q5-Pad2)"))
    (pad "2" thru_hole oval locked (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 172 "Net-(J3-Pad4)"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//1_Braun.wrl"
      (offset (xyz 2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//0_schwarz.wrl"
      (offset (xyz 2.75 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//3_orange.wrl"
      (offset (xyz 3.5 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//5_gold.wrl"
      (offset (xyz 5 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 93.98 97.155)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (attr through_hole)
    (fp_text reference "R3" (at 3.81 -2.37) (layer "F.SilkS"))
    (fp_text value "1k" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.683 0.127) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "VCC"))
    (pad "2" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 106 "Net-(R3-Pad2)"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial/1_braun.wrl"
      (offset (xyz 2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial/0_schwarz.wrl"
      (offset (xyz 2.75 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial/2_rot.wrl"
      (offset (xyz 3.5 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial/5_gold.wrl"
      (offset (xyz 5 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 114.3 85.23 180)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2.5mm Capacitor")
    (attr through_hole)
    (fp_text reference "C10" (at 2.5 -2.5) (layer "F.SilkS"))
    (fp_text value "100n" (at 2.5 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "VCC"))
    (pad "2" thru_hole circle locked (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 170.18 146.05 90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2.5mm Capacitor")
    (attr through_hole)
    (fp_text reference "C16" (at 2.5 -2.5 90) (layer "F.SilkS"))
    (fp_text value "100n" (at 2.5 2.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "VCC"))
    (pad "2" thru_hole circle locked (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 218.44 120.65)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2.5mm Capacitor")
    (attr through_hole)
    (fp_text reference "C13" (at 2.5 -2.5) (layer "F.SilkS"))
    (fp_text value "100n" (at 2.5 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "VCC"))
    (pad "2" thru_hole circle locked (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-8_W7.62mm" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 123.19 97.79)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (attr through_hole)
    (fp_text reference "SW1" (at 3.81 -2.33) (layer "F.SilkS"))
    (fp_text value "SW_DIP_x04" (at 3.81 9.95) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 3.81) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 107 "Net-(R4-Pad2)"))
    (pad "2" thru_hole oval locked (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 106 "Net-(R3-Pad2)"))
    (pad "3" thru_hole oval locked (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 105 "Net-(R2-Pad2)"))
    (pad "4" thru_hole oval locked (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 104 "Net-(R1-Pad2)"))
    (pad "5" thru_hole oval locked (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (pad "6" thru_hole oval locked (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (pad "7" thru_hole oval locked (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (pad "8" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (model "${KICAD6_3DMODEL_DIR}/3D-Spezial/walter/switch/dip_4-300.wrl"
      (offset (xyz 3.9 -3.9 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 224.79 133.35 180)
    (descr "Through hole straight pin header, 2x02, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x02 2.54mm double row")
    (attr through_hole)
    (fp_text reference "J3" (at 1.27 -2.33) (layer "F.SilkS"))
    (fp_text value "Conn_02x02_Counter_Clockwise_MountingPin" (at 1.27 4.87) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 1.27 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 173 "Net-(J3-Pad1)"))
    (pad "2" thru_hole oval locked (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 173 "Net-(J3-Pad1)"))
    (pad "3" thru_hole oval locked (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 174 "Net-(J3-Pad3)"))
    (pad "4" thru_hole oval locked (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 172 "Net-(J3-Pad4)"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}/Pin_Headers.3dshapes/Jumper_2-Fusion002.wrl"
      (offset (xyz 3.5 -3.25 3.5))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 -90))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 204.47 93.98)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2.5mm Capacitor")
    (attr through_hole)
    (fp_text reference "C17" (at 2.5 -2.5) (layer "F.SilkS"))
    (fp_text value "100n" (at 2.5 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 69 "/VccE"))
    (pad "2" thru_hole circle locked (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 203.2 69.85)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (attr through_hole)
    (fp_text reference "R27" (at 3.81 -2.37) (layer "F.SilkS"))
    (fp_text value "1k" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.638999 -0.128001) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 71 "/nPGM"))
    (pad "2" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 69 "/VccE"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//2_rot.wrl"
      (offset (xyz 2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//2_rot.wrl"
      (offset (xyz 2.75 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//2_rot.wrl"
      (offset (xyz 3.5 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}3D-Spezial//5_gold.wrl"
      (offset (xyz 5 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 198.12 78.74 -90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (attr through_hole)
    (fp_text reference "C6" (at 2.5 -2.5 90) (layer "F.SilkS"))
    (fp_text value "10u" (at 2.5 2.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "+12V"))
    (pad "2" thru_hole circle locked (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitors_THT.3dshapes/CP_Radial_D12.5mm_P7.50mm.step"
      (offset (xyz 0 0 0))
      (scale (xyz 0.65 0.65 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 182.88 78.74 -90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (attr through_hole)
    (fp_text reference "C9" (at 2.5 -2.5 90) (layer "F.SilkS"))
    (fp_text value "10u" (at 2.5 2.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C8-Pad1)"))
    (pad "2" thru_hole circle locked (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitors_THT.3dshapes/CP_Radial_D12.5mm_P7.50mm.step"
      (offset (xyz 0 0 0))
      (scale (xyz 0.65 0.65 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-92Flat" (layer "F.Cu")
    (tedit 5C2D433B)
    (at 187.96 73.66)
    (descr "TO-92Flat package, often used for hall sensors, drill 0.75mm (see e.g. http://www.ti.com/lit/ds/symlink/drv5023.pdf)")
    (tags "to-92Flat hall sensor")
    (attr through_hole)
    (fp_text reference "U10" (at 1.27 -1.45) (layer "F.SilkS"))
    (fp_text value "LM78L05ACZ" (at 1.25 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 0.2) (layer "F.Fab"))
    (pad "1" thru_hole roundrect locked (at 0 0) (size 1.05 1.3) (drill 0.75) (layers *.Cu *.Mask) (roundrect_rratio 0.238)
      (net 7 "Net-(C8-Pad1)"))
    (pad "2" thru_hole oval locked (at 1.27 0) (size 1.05 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 5 "Net-(C7-Pad2)"))
    (pad "3" thru_hole oval locked (at 2.54 0) (size 1.05 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 6 "+12V"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92Flat.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 184.15 76.2)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2.5mm Capacitor")
    (attr through_hole)
    (fp_text reference "C8" (at 2.5 -2.5) (layer "F.SilkS"))
    (fp_text value "C" (at 2.5 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C8-Pad1)"))
    (pad "2" thru_hole circle locked (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C7-Pad2)"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 191.77 76.2)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2.5mm Capacitor")
    (attr through_hole)
    (fp_text reference "C7" (at 2.5 -2.5) (layer "F.SilkS"))
    (fp_text value "C" (at 2.5 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "+12V"))
    (pad "2" thru_hole circle locked (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C7-Pad2)"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "D:/Program Files/KiCad/share/kicad/packages3d/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W2.5mm_P5.00mm.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_Tantal_D4.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 95.25 142.24)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (attr through_hole)
    (fp_text reference "C18" (at 2.5 -3.5) (layer "F.SilkS"))
    (fp_text value "10u" (at 2.5 3.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "VCC"))
    (pad "2" thru_hole circle locked (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitors_THT.3dshapes/CP_Radial_D12.5mm_P7.50mm.step"
      (offset (xyz 0 0 0))
      (scale (xyz 0.65 0.65 0.65))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x15_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 222.25 78.74)
    (descr "Through hole straight pin header, 2x15, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x15 2.54mm double row")
    (attr through_hole)
    (fp_text reference "J2" (at 1.27 -2.33) (layer "F.SilkS"))
    (fp_text value "CONN-100MIL-M-2x15" (at 1.27 37.89) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 17.78 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 181 "Net-(J2-Pad1)"))
    (pad "2" thru_hole oval locked (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "VCC"))
    (pad "3" thru_hole oval locked (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "/Vpp"))
    (pad "4" thru_hole oval locked (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 "/VccE"))
    (pad "5" thru_hole oval locked (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 70 "/EA12"))
    (pad "6" thru_hole oval locked (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 71 "/nPGM"))
    (pad "7" thru_hole oval locked (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 72 "/EA7"))
    (pad "8" thru_hole oval locked (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 73 "/EA13"))
    (pad "9" thru_hole oval locked (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 "/EA6"))
    (pad "10" thru_hole oval locked (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 75 "/EA8"))
    (pad "11" thru_hole oval locked (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 76 "/EA5"))
    (pad "12" thru_hole oval locked (at 2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 77 "/EA9"))
    (pad "13" thru_hole oval locked (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 78 "/EA4"))
    (pad "14" thru_hole oval locked (at 2.54 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 79 "/EA11"))
    (pad "15" thru_hole oval locked (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 80 "/EA3"))
    (pad "16" thru_hole oval locked (at 2.54 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 "/nOE"))
    (pad "17" thru_hole oval locked (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 82 "/EA2"))
    (pad "18" thru_hole oval locked (at 2.54 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 83 "/EA10"))
    (pad "19" thru_hole oval locked (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 84 "/EA1"))
    (pad "20" thru_hole oval locked (at 2.54 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 85 "/nCE"))
    (pad "21" thru_hole oval locked (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 86 "/EA0"))
    (pad "22" thru_hole oval locked (at 2.54 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 87 "/ED7"))
    (pad "23" thru_hole oval locked (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 88 "/ED0"))
    (pad "24" thru_hole oval locked (at 2.54 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 89 "/ED6"))
    (pad "25" thru_hole oval locked (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 90 "/ED1"))
    (pad "26" thru_hole oval locked (at 2.54 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 91 "/ED5"))
    (pad "27" thru_hole oval locked (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 92 "/ED2"))
    (pad "28" thru_hole oval locked (at 2.54 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 93 "/ED4"))
    (pad "29" thru_hole oval locked (at 0 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (pad "30" thru_hole oval locked (at 2.54 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 94 "/ED3"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x15_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Axial_L25.0mm_D10.0mm_P30.00mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50EF2)
    (at 144.78 86.36)
    (descr "CP, Axial series, Axial, Horizontal, pin pitch=30mm, , length*diameter=25*10mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/28325/021asm.pdf")
    (tags "CP Axial series Axial Horizontal pin pitch 30mm  length 25mm diameter 10mm Electrolytic Capacitor")
    (attr through_hole)
    (fp_text reference "C4" (at 15 -6.12) (layer "F.SilkS"))
    (fp_text value "220u" (at 15 6.12) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 15 0) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad "2" thru_hole oval locked (at 30 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Axial_L25.0mm_D10.0mm_P30.00mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Axial_L25.0mm_D10.0mm_P30.00mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50EF2)
    (at 177.8 63.5)
    (descr "CP, Axial series, Axial, Horizontal, pin pitch=30mm, , length*diameter=25*10mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/28325/021asm.pdf")
    (tags "CP Axial series Axial Horizontal pin pitch 30mm  length 25mm diameter 10mm Electrolytic Capacitor")
    (attr through_hole)
    (fp_text reference "C5" (at 15 -6.12) (layer "F.SilkS"))
    (fp_text value "220u" (at 15 6.12) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 15 0) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 "/+25V"))
    (pad "2" thru_hole oval locked (at 30 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Axial_L25.0mm_D10.0mm_P30.00mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_THT:L_Toroid_Horizontal_D4.1mm_P8.00mm_Diameter4-5mm_Amidon-T16" (layer "F.Cu")
    (tedit 5AE59B06)
    (at 161.29 63.5)
    (descr "L_Toroid, Horizontal series, Radial, pin pitch=8.00mm, , diameter=4.064mm, Diameter4-5mm, Amidon-T16")
    (tags "L_Toroid Horizontal series Radial pin pitch 8.00mm  diameter 4.064mm Diameter4-5mm Amidon-T16")
    (attr through_hole)
    (fp_text reference "L1" (at 4 -3.282) (layer "F.SilkS"))
    (fp_text value "47u" (at 4 3.282) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 4 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 97 "Net-(L1-Pad1)"))
    (pad "2" thru_hole circle locked (at 8 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 98 "Net-(L1-Pad2)"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_THT.3dshapes/L_Toroid_Horizontal_D4.1mm_P8.00mm_Diameter4-5mm_Amidon-T16.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}Inductors_THT.3dshapes/L_Axial_L11.0mm_D4.5mm_P15.24mm_Horizontal_Fastron_MECC.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.2 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}/Schalenkerne/c61035-a0010-c062_P18_without_hole.stp"
      (offset (xyz 3.81 0 0.508))
      (scale (xyz 0.6 0.5 0.6))
      (rotate (xyz -90 0 90))
    )
    (model "${KICAD6_3DMODEL_DIR}/Schalenkerne/c61035-a0010-c062_P18_without_hole.stp"
      (offset (xyz 3.8354 0 5.8166))
      (scale (xyz 0.6 0.5 0.6))
      (rotate (xyz 90 0 90))
    )
  )
  (gr_line (start 80 50) (end 240 50) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 80 150) (end 80 50) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 240 150) (end 80 150) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 240 50) (end 240 150) (layer "Edge.Cuts") (width 0.15))
  (gr_text "Prommer-80" (at 226.695 54.61) (layer "F.Cu"))
  (gr_text "202110203AAU001\n" (at 205.105 54.61) (layer "F.Cu"))
  (gr_text "202110203AAU001" (at 205.105 54.61) (layer "B.Cu"))
  (gr_text "Prommer-80\n" (at 226.695 54.61) (layer "B.Cu"))
  (zone (net 3) (net_name "VCC") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 240.03 149.86)
        (xy 80.01 149.86)
        (xy 80.01 50.165)
        (xy 240.03 50.165)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 240.03 149.86)
        (xy 80.01 149.86)
        (xy 80.01 50.165)
        (xy 240.03 50.165)
      )
    )
  )
)
