(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.69)
  )
  (paper "A4")
  (title_block
    (title "Yupstick")
    (date "2022-10-22")
    (rev "1.0")
    (company "Stefan Frings")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen") (color "White"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (color "#3A043CB3") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.6) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (color "#3A043CB3") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen") (color "White"))
      (copper_finish "HAL lead-free")
      (dielectric_constraints no)
      (edge_connector bevelled)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber/")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(C2-Pad2)")
  (net 4 "VBUS")
  (net 5 "/Reset")
  (net 6 "Net-(C5-Pad1)")
  (net 7 "VDD")
  (net 8 "Net-(H1-Pad1)")
  (net 9 "Net-(H2-Pad1)")
  (net 10 "Net-(H3-Pad1)")
  (net 11 "Net-(H4-Pad1)")
  (net 12 "Net-(H5-Pad1)")
  (net 13 "/PA12")
  (net 14 "/PA11")
  (net 15 "/PB15")
  (net 16 "/PB0")
  (net 17 "/PB14")
  (net 18 "/PB1")
  (net 19 "/PB13")
  (net 20 "/PB2")
  (net 21 "/PB12")
  (net 22 "/PB3")
  (net 23 "/PB11")
  (net 24 "/PB4")
  (net 25 "/PB10")
  (net 26 "/PB5")
  (net 27 "/PB9")
  (net 28 "/PB6")
  (net 29 "/PB8")
  (net 30 "/PB7")
  (net 31 "Net-(LS1-Pad2)")
  (net 32 "/PA5")
  (net 33 "/Boot0")
  (net 34 "/PC13")
  (net 35 "/PA4")
  (net 36 "/PA6")
  (net 37 "/PA7")
  (net 38 "/PA8")
  (net 39 "/PA9")
  (net 40 "/PA10")
  (net 41 "/PA13")
  (net 42 "/PA14")
  (net 43 "/PA15")
  (net 44 "/PA0")
  (net 45 "/PA1")
  (net 46 "/PA2")
  (net 47 "/PA3")
  (net 48 "unconnected-(U2-Pad5)")
  (net 49 "unconnected-(U2-Pad6)")
  (net 50 "Net-(R11-Pad2)")
  (net 51 "Net-(R12-Pad2)")
  (net 52 "Net-(R13-Pad2)")
  (net 53 "Net-(R14-Pad2)")
  (net 54 "Net-(D1-Pad2)")
  (net 55 "Net-(D2-Pad2)")
  (net 56 "Net-(D2-Pad3)")
  (net 57 "Net-(D3-Pad2)")
  (net 58 "Net-(D3-Pad3)")
  (net 59 "Net-(D4-Pad2)")
  (net 60 "Net-(D4-Pad3)")
  (net 61 "Net-(D5-Pad2)")
  (net 62 "Net-(D5-Pad3)")
  (net 63 "/Bat")
  (net 64 "Net-(R21-Pad2)")
  (footprint "Button_Switch_THT:SW_PUSH_6mm_H5mm" (layer "F.Cu")
    (tedit 5A02FE31)
    (at 175.11 78.74)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=5mm")
    (tags "tact sw push 6mm")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW2" (at 3.39 2.26 180) (layer "F.SilkS"))
    (fp_text value "Reset" (at 3.14 6.51) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.25 2.25) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 "/Reset") (pinfunction "2") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 "/Reset") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 126.625 84.455 -90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at 0.045 8.625 180) (layer "F.SilkS"))
    (fp_text value "SWD" (at 0.045 -3.875 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 8.375) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "/PA13") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "/PA14") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 167 87.5 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R22" (at 0 -1.75 180) (layer "F.SilkS"))
    (fp_text value "1kΩ" (at -3 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "Net-(R21-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "/PC13") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_Pad_Via" (layer "F.Cu")
    (tedit 56DDBCCA)
    (at 121 108)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0 4.2) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 "Net-(H1-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 "Net-(H1-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 "Net-(H1-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 "Net-(H1-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 8 "Net-(H1-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 "Net-(H1-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 "Net-(H1-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 "Net-(H1-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 "Net-(H1-Pad1)") (pinfunction "1") (pintype "input"))
  )
  (footprint "Package_TO_SOT_SMD:SOT-89-3" (layer "F.Cu")
    (tedit 5C33D6E8)
    (at 120.03 76.2 -90)
    (descr "SOT-89-3, http://ww1.microchip.com/downloads/en/DeviceDoc/3L_SOT-89_MB_C04-029C.pdf")
    (tags "SOT-89-3")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at -1.7 3.53 180) (layer "F.SilkS"))
    (fp_text value "MCP1700T-3002 or HT7830-A" (at 9.55 19.53 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.5 0) (layer "F.Fab"))
    (pad "1" smd rect (at -1.65 -1.5 270) (size 1.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "2" smd custom (at -1.5625 0 270) (size 1.475 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "VBUS") (pinfunction "VI") (pintype "power_in") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 3.8625 0.8665)
            (xy 0.7375 0.8665)
            (xy 0.7375 -0.8665)
            (xy 3.8625 -0.8665)
          ) (width 0) (fill yes))
      ))
    (pad "3" smd rect (at -1.65 1.5 270) (size 1.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(C5-Pad1)") (pinfunction "VO") (pintype "power_out"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-89-3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 121.25 80 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 2.9 0) (layer "F.SilkS"))
    (fp_text value "10kΩ" (at 0 -1.27) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "/Boot0") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 162 103.5 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R19" (at -2.25 -0.75 90) (layer "F.SilkS"))
    (fp_text value "1kΩ" (at 0 -1.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 47 "/PA3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(H4-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 141.5 98 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R8" (at 2.5 0.105 90) (layer "F.SilkS"))
    (fp_text value "1kΩ" (at 3 0 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 60 "Net-(D4-Pad3)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 126.5 98 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R5" (at 2.5 0 90) (layer "F.SilkS"))
    (fp_text value "1kΩ" (at 3 0 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 57 "Net-(D3-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 158 103.5 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R14" (at 2.25 -0.75 90) (layer "F.SilkS"))
    (fp_text value "1kΩ" (at 0 -1.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "VDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 53 "Net-(R14-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_Pad_Via" (layer "F.Cu")
    (tedit 56DDBCCA)
    (at 180 103)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H6" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0 4.2) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "1") (pintype "input"))
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 149 83.2 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C7" (at 2.3 -0.2) (layer "F.SilkS"))
    (fp_text value "100nF" (at -0.2 1.3 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "VDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_Pad_Via" (layer "F.Cu")
    (tedit 56DDBCCA)
    (at 134 108)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 -4.417944) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0 4.2) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 9 "Net-(H2-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 9 "Net-(H2-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 9 "Net-(H2-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 9 "Net-(H2-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 9 "Net-(H2-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 9 "Net-(H2-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 9 "Net-(H2-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 9 "Net-(H2-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 9 "Net-(H2-Pad1)") (pinfunction "1") (pintype "input"))
  )
  (footprint "Button_Switch_THT:SW_PUSH_6mm_H5mm" (layer "F.Cu")
    (tedit 5A02FE31)
    (at 118.75 101.25 90)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=5mm")
    (tags "tact sw push 6mm")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW3" (at 3.25 2.25 90) (layer "F.SilkS"))
    (fp_text value "PA0 Btn" (at -0.635 2.25 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.25 2.25 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 50 "Net-(R11-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole circle (at 6.5 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 50 "Net-(R11-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 6.5 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 44 "/PA0") (pinfunction "2") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 44 "/PA0") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 163 85.5 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at 0.056661 -1.64) (layer "F.SilkS"))
    (fp_text value "1kΩ" (at -0.495 -1.64) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "VDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 54 "Net-(D1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 136 103.5 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R17" (at -2.25 -0.75 90) (layer "F.SilkS"))
    (fp_text value "1kΩ" (at 0 -1.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "/PA1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(H2-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_Pad_Via" (layer "F.Cu")
    (tedit 56DDBCCA)
    (at 147 108)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0 4.2) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 10 "Net-(H3-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 10 "Net-(H3-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 10 "Net-(H3-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 10 "Net-(H3-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 10 "Net-(H3-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 10 "Net-(H3-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 10 "Net-(H3-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 10 "Net-(H3-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 10 "Net-(H3-Pad1)") (pinfunction "1") (pintype "input"))
  )
  (footprint "Package_QFP:LQFP-48_7x7mm_P0.5mm" (layer "F.Cu")
    (tedit 5D9F72AF)
    (at 142.24 85 180)
    (descr "LQFP, 48 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/ltc2358-16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "LQFP QFP")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U2" (at 4.74 4.59) (layer "F.SilkS"))
    (fp_text value "STM32L072CBT6" (at 1.74 4.59) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -4.1625 -2.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "VDD") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd roundrect (at -4.1625 -2.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "/PC13") (pinfunction "PC13") (pintype "bidirectional"))
    (pad "3" smd roundrect (at -4.1625 -1.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(C1-Pad2)") (pinfunction "PC14") (pintype "bidirectional"))
    (pad "4" smd roundrect (at -4.1625 -1.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(C2-Pad2)") (pinfunction "PC15") (pintype "bidirectional"))
    (pad "5" smd roundrect (at -4.1625 -0.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "unconnected-(U2-Pad5)") (pinfunction "PH0") (pintype "input+no_connect"))
    (pad "6" smd roundrect (at -4.1625 -0.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 49 "unconnected-(U2-Pad6)") (pinfunction "PH1") (pintype "input+no_connect"))
    (pad "7" smd roundrect (at -4.1625 0.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/Reset") (pinfunction "NRST") (pintype "input"))
    (pad "8" smd roundrect (at -4.1625 0.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "VSSA") (pintype "power_in"))
    (pad "9" smd roundrect (at -4.1625 1.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "VDD") (pinfunction "VDDA") (pintype "power_in"))
    (pad "10" smd roundrect (at -4.1625 1.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "/PA0") (pinfunction "PA0") (pintype "bidirectional"))
    (pad "11" smd roundrect (at -4.1625 2.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "/PA1") (pinfunction "PA1") (pintype "bidirectional"))
    (pad "12" smd roundrect (at -4.1625 2.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "/PA2") (pinfunction "PA2") (pintype "bidirectional"))
    (pad "13" smd roundrect (at -2.75 4.1625 180) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 47 "/PA3") (pinfunction "PA3") (pintype "bidirectional"))
    (pad "14" smd roundrect (at -2.25 4.1625 180) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "/PA4") (pinfunction "PA4") (pintype "bidirectional"))
    (pad "15" smd roundrect (at -1.75 4.1625 180) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/PA5") (pinfunction "PA5") (pintype "bidirectional"))
    (pad "16" smd roundrect (at -1.25 4.1625 180) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "/PA6") (pinfunction "PA6") (pintype "bidirectional"))
    (pad "17" smd roundrect (at -0.75 4.1625 180) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "/PA7") (pinfunction "PA7") (pintype "bidirectional"))
    (pad "18" smd roundrect (at -0.25 4.1625 180) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "/PB0") (pinfunction "PB0") (pintype "bidirectional"))
    (pad "19" smd roundrect (at 0.25 4.1625 180) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "/PB1") (pinfunction "PB1") (pintype "bidirectional"))
    (pad "20" smd roundrect (at 0.75 4.1625 180) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "/PB2") (pinfunction "PB2") (pintype "bidirectional"))
    (pad "21" smd roundrect (at 1.25 4.1625 180) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "/PB10") (pinfunction "PB10") (pintype "bidirectional"))
    (pad "22" smd roundrect (at 1.75 4.1625 180) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "/PB11") (pinfunction "PB11") (pintype "bidirectional"))
    (pad "23" smd roundrect (at 2.25 4.1625 180) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "24" smd roundrect (at 2.75 4.1625 180) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "VDD") (pinfunction "VDD") (pintype "power_in"))
    (pad "25" smd roundrect (at 4.1625 2.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "/PB12") (pinfunction "PB12") (pintype "bidirectional"))
    (pad "26" smd roundrect (at 4.1625 2.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "/PB13") (pinfunction "PB13") (pintype "bidirectional"))
    (pad "27" smd roundrect (at 4.1625 1.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "/PB14") (pinfunction "PB14") (pintype "bidirectional"))
    (pad "28" smd roundrect (at 4.1625 1.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "/PB15") (pinfunction "PB15") (pintype "bidirectional"))
    (pad "29" smd roundrect (at 4.1625 0.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "/PA8") (pinfunction "PA8") (pintype "bidirectional"))
    (pad "30" smd roundrect (at 4.1625 0.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "/PA9") (pinfunction "PA9") (pintype "bidirectional"))
    (pad "31" smd roundrect (at 4.1625 -0.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "/PA10") (pinfunction "PA10") (pintype "bidirectional"))
    (pad "32" smd roundrect (at 4.1625 -0.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "/PA11") (pinfunction "PA11") (pintype "bidirectional"))
    (pad "33" smd roundrect (at 4.1625 -1.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "/PA12") (pinfunction "PA12") (pintype "bidirectional"))
    (pad "34" smd roundrect (at 4.1625 -1.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "/PA13") (pinfunction "PA13") (pintype "bidirectional"))
    (pad "35" smd roundrect (at 4.1625 -2.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "36" smd roundrect (at 4.1625 -2.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "VBUS") (pinfunction "VDD_USB") (pintype "power_in"))
    (pad "37" smd roundrect (at 2.75 -4.1625 180) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "/PA14") (pinfunction "PA14") (pintype "bidirectional"))
    (pad "38" smd roundrect (at 2.25 -4.1625 180) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "/PA15") (pinfunction "PA15") (pintype "bidirectional"))
    (pad "39" smd roundrect (at 1.75 -4.1625 180) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/PB3") (pinfunction "PB3") (pintype "bidirectional"))
    (pad "40" smd roundrect (at 1.25 -4.1625 180) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "/PB4") (pinfunction "PB4") (pintype "bidirectional"))
    (pad "41" smd roundrect (at 0.75 -4.1625 180) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "/PB5") (pinfunction "PB5") (pintype "bidirectional"))
    (pad "42" smd roundrect (at 0.25 -4.1625 180) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "/PB6") (pinfunction "PB6") (pintype "bidirectional"))
    (pad "43" smd roundrect (at -0.25 -4.1625 180) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "/PB7") (pinfunction "PB7") (pintype "bidirectional"))
    (pad "44" smd roundrect (at -0.75 -4.1625 180) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "/Boot0") (pinfunction "BOOT0") (pintype "input"))
    (pad "45" smd roundrect (at -1.25 -4.1625 180) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "/PB8") (pinfunction "PB8") (pintype "bidirectional"))
    (pad "46" smd roundrect (at -1.75 -4.1625 180) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "/PB9") (pinfunction "PB9") (pintype "bidirectional"))
    (pad "47" smd roundrect (at -2.25 -4.1625 180) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "48" smd roundrect (at -2.75 -4.1625 180) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "VDD") (pinfunction "VDD") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_QFP.3dshapes/LQFP-48_7x7mm_P0.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_Kingbright_APHBM2012_2x1.25mm" (layer "F.Cu")
    (tedit 6145EE54)
    (at 166.5 93.5)
    (descr "Dual LED SMD https://www.kingbrightusa.com/KCpack.asp?txtPack=APHBM2012")
    (tags "LED Kingbright APHM2012")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D2" (at 0 -2.5 180) (layer "F.SilkS"))
    (fp_text value "LED red/green" (at -5.715 0.37 180) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.15 -2.5 180) (layer "F.Fab"))
    (pad "1" smd rect (at -0.475 -0.9 90) (size 1.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "/PA8") (pinfunction "A1") (pintype "input"))
    (pad "2" smd rect (at -0.475 0.9 90) (size 1.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 55 "Net-(D2-Pad2)") (pinfunction "K1") (pintype "input"))
    (pad "3" smd rect (at 0.475 0.9 90) (size 1.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "Net-(D2-Pad3)") (pinfunction "K2") (pintype "input"))
    (pad "4" smd rect (at 0.475 -0.9 90) (size 1.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "/PA9") (pinfunction "A2") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_Kingbright_APHBM2012_2x1.25mm.wrl" hide
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric_Castellated.wrl"
      (offset (xyz -0.4 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric_Castellated.wrl"
      (offset (xyz 0.4 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x10_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 147.325 73.665 90)
    (descr "Through hole straight pin header, 2x10, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x10 2.54mm double row")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at -0.335 -3.325 180) (layer "F.SilkS"))
    (fp_text value "Extension 2.54mm" (at 0.005 12.06 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 11.43 180) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "/PB15") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "/PB0") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "/PB14") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "/PB1") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "/PB13") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "/PB2") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "/PB12") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "/PB3") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "/PB11") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "/PB4") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "/PB10") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "/PB5") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "/PA7") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval (at 2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "/PB6") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "/PA6") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole oval (at 2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "/PB7") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole oval (at 2.54 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "VDD") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" thru_hole oval (at 2.54 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "VDD") (pinfunction "Pin_20") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x10_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_THT:SW_PUSH_6mm_H5mm" (layer "F.Cu")
    (tedit 5A02FE31)
    (at 130.81 79.375 180)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=5mm")
    (tags "tact sw push 6mm")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW1" (at 3.31 2.375) (layer "F.SilkS"))
    (fp_text value "Boot0" (at 3.25 -1.905) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.25 2.25) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 6.5 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 33 "/Boot0") (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole circle (at 0 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 33 "/Boot0") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 6.5 4.5 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 7 "VDD") (pinfunction "2") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 4.5 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 7 "VDD") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 126.38 71.12 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "JP1" (at -0.38 -2.88) (layer "F.SilkS"))
    (fp_text value "Power src" (at 1.905 2.525 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.62 2.12) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(C5-Pad1)") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "VDD") (pinfunction "C") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 "/Bat") (pinfunction "B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 178.435 76.2 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C4" (at 2.54 0) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/Reset") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 146.4 91 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C8" (at 0.5 -1.85) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 -1.6 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "VDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 120 70.5 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C3" (at 0.5 1.75 270) (layer "F.SilkS"))
    (fp_text value "10µF" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "VBUS") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 174 101 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R15" (at 3 0) (layer "F.SilkS"))
    (fp_text value "1kΩ" (at -2.86 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "Net-(LS1-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "/PA4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 139.5 98 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R7" (at 2.5 0 90) (layer "F.SilkS"))
    (fp_text value "1kΩ" (at 3 0 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "Net-(D4-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 128.5 98 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R6" (at 2.5 0 90) (layer "F.SilkS"))
    (fp_text value "1kΩ" (at 3 0 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "Net-(D3-Pad3)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 135.75 71)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C6" (at 0.25 1.75) (layer "F.SilkS"))
    (fp_text value "10µF" (at 3.71 0.38) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 63 "/Bat") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 135.5 88.5 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C10" (at -0.5 -2.5) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 -1.6 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "VBUS") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 159 85.5)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D1" (at -0.381 1.778) (layer "F.SilkS"))
    (fp_text value "LED yellow" (at -1.504 1.64) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "/PC13") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 54 "Net-(D1-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Buzzer_Beeper:MagneticBuzzer_ProSignal_ABT-410-RC" (layer "F.Cu")
    (tedit 5A030281)
    (at 174.25 93)
    (descr "Buzzer, Elektromagnetic Beeper, Summer, 1,5V-DC,")
    (tags "Pro Signal ABT-410-RC ")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "LS1" (at -3.75 3.5 180) (layer "F.SilkS"))
    (fp_text value "Piezo" (at 3.5 2.25) (layer "F.Fab"))
    (fp_text user "+" (at 0 -1.8) (layer "F.SilkS"))
    (fp_text user "+" (at 0 -1.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.25 -3.735) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 7 "VDD") (pinfunction "1") (pintype "input"))
    (pad "2" thru_hole circle (at 6.5 0) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(LS1-Pad2)") (pinfunction "2") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Buzzer_Beeper.3dshapes/MagneticBuzzer_ProSignal_ABT-410-RC.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_Pad_Via" (layer "F.Cu")
    (tedit 56DDBCCA)
    (at 160 108)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0 4.2) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 11 "Net-(H4-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 11 "Net-(H4-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 11 "Net-(H4-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 11 "Net-(H4-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 11 "Net-(H4-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 11 "Net-(H4-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 11 "Net-(H4-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 11 "Net-(H4-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 11 "Net-(H4-Pad1)") (pinfunction "1") (pintype "input"))
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 153.505959 83.185)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at 0.994041 1.315) (layer "F.SilkS"))
    (fp_text value "4,3pF" (at -0.005959 1.315) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(C2-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D5.0mm_Clear" (layer "F.Cu")
    (tedit 5A6C9BC0)
    (at 171.5 80.5 180)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Q1" (at -0.5 -4 180) (layer "F.SilkS"))
    (fp_text value "PT331C" (at 1.27 -4 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 1.75) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 "VDD") (pinfunction "C") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 32 "/PA5") (pinfunction "E") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm_Clear.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Crystal:Crystal_C38-LF_D3.0mm_L8.0mm_Horizontal" (layer "F.Cu")
    (tedit 5A0FD1B2)
    (at 155.575 83.18 90)
    (descr "Crystal THT C38-LF 8.0mm length 3.0mm diameter")
    (tags "['C38-LF']")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Y1" (at 0.98 6.625 180) (layer "F.SilkS"))
    (fp_text value "32,768kHz" (at 3.68 6.175 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 6.5 180) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 1.9 0 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Crystal_C38-LF_D3.0mm_L8.0mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 118.25 70.5 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C5" (at 0.5 -1.5 270) (layer "F.SilkS"))
    (fp_text value "2.2µF" (at 0.25 -1.6 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(C5-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_THT:SW_PUSH_6mm_H5mm" (layer "F.Cu")
    (tedit 5A02FE31)
    (at 131.75 101.25 90)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=5mm")
    (tags "tact sw push 6mm")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW4" (at 3.25 2.25 270) (layer "F.SilkS"))
    (fp_text value "PA1 Btn" (at -0.625 2.25 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.25 2.25 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 51 "Net-(R12-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole circle (at 6.5 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 51 "Net-(R12-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 45 "/PA1") (pinfunction "2") (pintype "passive"))
    (pad "2" thru_hole circle (at 6.5 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 45 "/PA1") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 132 103.5 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R12" (at 2.25 -0.75 90) (layer "F.SilkS"))
    (fp_text value "1kΩ" (at 0 -1.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -4.43) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "VDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "Net-(R12-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_THT:SW_PUSH_6mm_H5mm" (layer "F.Cu")
    (tedit 5A02FE31)
    (at 144.78 101.25 90)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=5mm")
    (tags "tact sw push 6mm")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW5" (at 3.25 2.25 270) (layer "F.SilkS"))
    (fp_text value "PA2 Btn" (at -0.485 2.25 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.25 2.25 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 52 "Net-(R13-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole circle (at 6.5 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 52 "Net-(R13-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 46 "/PA2") (pinfunction "2") (pintype "passive"))
    (pad "2" thru_hole circle (at 6.5 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 46 "/PA2") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 165.5 98 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at 2.5 0 90) (layer "F.SilkS"))
    (fp_text value "1kΩ" (at 2.5 0 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 55 "Net-(D2-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 167 85.5)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R21" (at 0.75 -1.5 180) (layer "F.SilkS"))
    (fp_text value "1kΩ" (at 3 0.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/PA5") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "Net-(R21-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 153.515 81.28)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 0.985 -1.28) (layer "F.SilkS"))
    (fp_text value "4,3pF" (at -0.015 -1.28) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(C1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 123 103.5 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R16" (at -2.25 -0.75 90) (layer "F.SilkS"))
    (fp_text value "1kΩ" (at 0 -1.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "/PA0") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(H1-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_Kingbright_APHBM2012_2x1.25mm" (layer "F.Cu")
    (tedit 6145EE54)
    (at 127.5 93.5)
    (descr "Dual LED SMD https://www.kingbrightusa.com/KCpack.asp?txtPack=APHBM2012")
    (tags "LED Kingbright APHM2012")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D3" (at 0.03 -2.555 180) (layer "F.SilkS"))
    (fp_text value "LED red/green" (at -6.35 -0.445 180) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.15 -2.5 180) (layer "F.Fab"))
    (pad "1" smd rect (at -0.475 -0.9 90) (size 1.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "/PA10") (pinfunction "A1") (pintype "input"))
    (pad "2" smd rect (at -0.475 0.9 90) (size 1.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 57 "Net-(D3-Pad2)") (pinfunction "K1") (pintype "input"))
    (pad "3" smd rect (at 0.475 0.9 90) (size 1.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 58 "Net-(D3-Pad3)") (pinfunction "K2") (pintype "input"))
    (pad "4" smd rect (at 0.475 -0.9 90) (size 1.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "/PA13") (pinfunction "A2") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_Kingbright_APHBM2012_2x1.25mm.wrl" hide
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric_Castellated.wrl"
      (offset (xyz -0.4 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric_Castellated.wrl"
      (offset (xyz 0.4 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "LED_SMD:LED_Kingbright_APHBM2012_2x1.25mm" (layer "F.Cu")
    (tedit 6145EE54)
    (at 140.5 93.5)
    (descr "Dual LED SMD https://www.kingbrightusa.com/KCpack.asp?txtPack=APHBM2012")
    (tags "LED Kingbright APHM2012")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D4" (at -0.01 -2.345 180) (layer "F.SilkS"))
    (fp_text value "LED red/green" (at -6.19 0 180) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.15 -2.5 180) (layer "F.Fab"))
    (pad "1" smd rect (at -0.475 -0.9 90) (size 1.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "/PA14") (pinfunction "A1") (pintype "input"))
    (pad "2" smd rect (at -0.475 0.9 90) (size 1.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 59 "Net-(D4-Pad2)") (pinfunction "K1") (pintype "input"))
    (pad "3" smd rect (at 0.475 0.9 90) (size 1.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "Net-(D4-Pad3)") (pinfunction "K2") (pintype "input"))
    (pad "4" smd rect (at 0.475 -0.9 90) (size 1.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "/PA15") (pinfunction "A2") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_Kingbright_APHBM2012_2x1.25mm.wrl" hide
      (offset (xyz 0.4 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric_Castellated.wrl"
      (offset (xyz 0.4 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric_Castellated.wrl"
      (offset (xyz -0.4 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 145 103.5 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R13" (at 2.25 -0.75 90) (layer "F.SilkS"))
    (fp_text value "1kΩ" (at 0 -1.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "VDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 52 "Net-(R13-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 149 103.5 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R18" (at -2.25 -0.75 90) (layer "F.SilkS"))
    (fp_text value "1kΩ" (at 0 -1.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "/PA2") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(H3-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_Kingbright_APHBM2012_2x1.25mm" (layer "F.Cu")
    (tedit 6145EE54)
    (at 153.5 93.5)
    (descr "Dual LED SMD https://www.kingbrightusa.com/KCpack.asp?txtPack=APHBM2012")
    (tags "LED Kingbright APHM2012")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D5" (at 0.13 -2.445) (layer "F.SilkS"))
    (fp_text value "LED red/green" (at -6.35 0) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.15 -2.5) (layer "F.Fab"))
    (pad "1" smd rect (at -0.475 -0.9 90) (size 1.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "/PB8") (pinfunction "A1") (pintype "input"))
    (pad "2" smd rect (at -0.475 0.9 90) (size 1.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "Net-(D5-Pad2)") (pinfunction "K1") (pintype "input"))
    (pad "3" smd rect (at 0.475 0.9 90) (size 1.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "Net-(D5-Pad3)") (pinfunction "K2") (pintype "input"))
    (pad "4" smd rect (at 0.475 -0.9 90) (size 1.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "/PB9") (pinfunction "A2") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_Kingbright_APHBM2012_2x1.25mm.wrl" hide
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric_Castellated.wrl"
      (offset (xyz -0.4 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric_Castellated.wrl"
      (offset (xyz 0.4 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 167.5 98 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R4" (at 2.5 0 90) (layer "F.SilkS"))
    (fp_text value "1kΩ" (at 2.5 0 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 56 "Net-(D2-Pad3)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 154.5 98 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R10" (at 3 0 90) (layer "F.SilkS"))
    (fp_text value "1kΩ" (at 2.5 0 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "Net-(D5-Pad3)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 119 103.5 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R11" (at 2.25 -0.75 90) (layer "F.SilkS"))
    (fp_text value "1kΩ" (at 0 -1.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "VDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 50 "Net-(R11-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 152.5 98 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R9" (at 2.5 -0.1 90) (layer "F.SilkS"))
    (fp_text value "1kΩ" (at 2.5 -0.1 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "Net-(D5-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 174 103)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R20" (at -3 0) (layer "F.SilkS"))
    (fp_text value "1kΩ" (at 2.86 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "/PA4") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(H5-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 138.9 78.2)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C9" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0.1 -1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "VDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_Pad_Via" (layer "F.Cu")
    (tedit 56DDBCCA)
    (at 173 108)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H5" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0 4.2) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 12 "Net-(H5-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 12 "Net-(H5-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 12 "Net-(H5-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 12 "Net-(H5-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 12 "Net-(H5-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 12 "Net-(H5-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 12 "Net-(H5-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 12 "Net-(H5-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 12 "Net-(H5-Pad1)") (pinfunction "1") (pintype "input"))
  )
  (footprint "Button_Switch_THT:SW_PUSH_6mm_H5mm" (layer "F.Cu")
    (tedit 5A02FE31)
    (at 157.75 101.25 90)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=5mm")
    (tags "tact sw push 6mm")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW6" (at 3.25 2.25 270) (layer "F.SilkS"))
    (fp_text value "PA3 Btn" (at -0.635 2.595 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.25 2.25 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 6.5 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 53 "Net-(R14-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole circle (at 0 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 53 "Net-(R14-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 6.5 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 47 "/PA3") (pinfunction "2") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 47 "/PA3") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library:USB A Plug PCB" (layer "F.Cu")
    (tedit 542BB0AF)
    (at 103 76 -90)
    (descr "USB A Plug on PCB")
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "J1" (at -1.07 -9.76) (layer "F.SilkS"))
    (fp_text value "USB-A" (at 0 -5.785 -90) (layer "F.Fab"))
    (fp_text user "5V" (at 4 -9.76 unlocked) (layer "F.SilkS"))
    (fp_text user "USB" (at 1.27 -9.525 unlocked) (layer "F.SilkS"))
    (fp_text user "GND" (at -4 -9.76 unlocked) (layer "F.SilkS"))
    (fp_text user "D-" (at 1.27 -7.874 unlocked) (layer "Dwgs.User"))
    (fp_text user "D+" (at -1.27 -7.874 unlocked) (layer "Dwgs.User"))
    (pad "1" connect rect (at 3.81 -4.9 270) (size 1.9 8) (layers "F.Cu" "F.Mask")
      (net 4 "VBUS") (pinfunction "VBUS") (pintype "power_in"))
    (pad "2" connect rect (at 1.3 -5.45 270) (size 2 6.9) (layers "F.Cu" "F.Mask")
      (net 14 "/PA11") (pinfunction "D-") (pintype "bidirectional"))
    (pad "3" connect rect (at -1.3 -5.45 270) (size 2 6.9) (layers "F.Cu" "F.Mask")
      (net 13 "/PA12") (pinfunction "D+") (pintype "bidirectional"))
    (pad "4" connect rect (at -3.81 -4.9 270) (size 1.9 8) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints not_allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 103 82)
          (xy 103 70)
          (xy 114 70)
          (xy 114 82)
        )
      )
    )
  )
  (footprint "Library:2x LR44 or coin cell holder" (layer "B.Cu")
    (tedit 5C12D246)
    (at 167.75 88.264148)
    (property "Sheetfile" "Datei: yupstick.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "BT1" (at -3.05 -0.02) (layer "B.SilkS"))
    (fp_text value "3V Battery" (at -11 -9.764148) (layer "B.SilkS"))
    (fp_text user "+" (at -16.5 -0.014148 180 unlocked) (layer "B.SilkS"))
    (fp_text user "-" (at 13.95 -2.764148 180 unlocked) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at -3.05 -0.02) (layer "B.Fab"))
    (pad "1" smd rect (at -10.55 0.03) (size 7 4.1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 63 "/Bat") (pinfunction "+") (pintype "passive"))
    (pad "2" smd rect (at 8.95 0.03) (size 13 4.1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "-") (pintype "passive"))
  )
  (gr_line (start 115 70) (end 103 70) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 115 112) (end 184 112) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 184 67.5) (end 115 67.5) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 103 70) (end 103 82) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 184 112) (end 184 67.5) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 115 67.5) (end 115 70) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 115 112) (end 115 82) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 103 82) (end 115 82) (layer "Edge.Cuts") (width 0.1))
  (gr_text "PB8,9" (at 156.5 92.25) (layer "F.SilkS"))
  (gr_text "B2" (at 152.4 68.75) (layer "F.SilkS"))
  (gr_text "GND" (at 182 107.5) (layer "F.SilkS"))
  (gr_text "1" (at 149.25 87.25) (layer "F.SilkS"))
  (gr_text "B12" (at 154.94 76.2) (layer "F.SilkS"))
  (gr_text "Power src" (at 136 68.75) (layer "F.SilkS"))
  (gr_text "USB" (at 126.647066 68.75) (layer "F.SilkS"))
  (gr_text "GND" (at 120 86.7) (layer "F.SilkS"))
  (gr_text "A7" (at 162.547348 76.1921) (layer "F.SilkS"))
  (gr_text "3V" (at 170.18 76.2) (layer "F.SilkS"))
  (gr_text "PA1" (at 139.065 110) (layer "F.SilkS"))
  (gr_text "PA4" (at 178 110) (layer "F.SilkS"))
  (gr_text "B1" (at 149.86 68.75) (layer "F.SilkS"))
  (gr_text "Sensor" (at 171.75 86) (layer "F.SilkS"))
  (gr_text "B7" (at 165.1 68.75) (layer "F.SilkS"))
  (gr_text "B6" (at 162.56 68.75) (layer "F.SilkS"))
  (gr_text "3V" (at 170.18 68.75) (layer "F.SilkS"))
  (gr_text "PA0" (at 126 110) (layer "F.SilkS"))
  (gr_text "PA14,15" (at 144 93) (layer "F.SilkS"))
  (gr_text "B15" (at 147.32 76.2) (layer "F.SilkS"))
  (gr_text "B0" (at 147.32 68.75) (layer "F.SilkS"))
  (gr_text "B14" (at 149.86 76.2) (layer "F.SilkS"))
  (gr_text "B13" (at 152.455169 76.1921) (layer "F.SilkS"))
  (gr_text "B10" (at 160.018394 76.1921) (layer "F.SilkS"))
  (gr_text "GND" (at 167.64 76.2) (layer "F.SilkS"))
  (gr_text "SWDIO" (at 127.7 86.7) (layer "F.SilkS"))
  (gr_text "GND" (at 167.64 68.75) (layer "F.SilkS"))
  (gr_text "B4" (at 157.48 68.75) (layer "F.SilkS"))
  (gr_text "PA3" (at 165 110) (layer "F.SilkS"))
  (gr_text "Boot0" (at 127.5 81.455113) (layer "F.SilkS"))
  (gr_text "STM32L072C" (at 145.5 78.5) (layer "F.SilkS"))
  (gr_text "PA8,9" (at 169.25 92.25) (layer "F.SilkS"))
  (gr_text "A6" (at 165.1 76.2) (layer "F.SilkS"))
  (gr_text "B11" (at 157.48 76.2) (layer "F.SilkS"))
  (gr_text "B3" (at 154.94 68.75) (layer "F.SilkS"))
  (gr_text "PA10,13" (at 131 92.25) (layer "F.SilkS"))
  (gr_text "PA2" (at 152 110) (layer "F.SilkS"))
  (gr_text "Reset" (at 178.25 85.25) (layer "F.SilkS"))
  (gr_text "BATT" (at 130.986466 68.75) (layer "F.SilkS"))
  (gr_text "SWCLK" (at 123.6 86.7) (layer "F.SilkS"))
  (gr_text "YupStick" (at 177.75 69.75) (layer "F.SilkS"))
  (gr_text "B5" (at 160 68.75) (layer "F.SilkS"))
  (zone (net 0) (net_name "") (layer "F.Cu") (name "GND") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 156.5 85.5)
        (xy 149.5 85.5)
        (xy 149.5 80.5)
        (xy 156.5 80.5)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layers F&B.Cu) (name "GND") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 186 114)
        (xy 101 114)
        (xy 101 66)
        (xy 186 66)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 146.5 92.25)
        (xy 144.5 92.25)
        (xy 144.5 90.5)
        (xy 146.5 90.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 137 89)
        (xy 131.75 89)
        (xy 131.75 87)
        (xy 137 87)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F&B.Cu) (name "Kante") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 183.995853 108.5)
        (xy 183.995956 112.225191)
        (xy 115.009703 112.232993)
        (xy 115.0096 109)
      )
    )
  )
)
