(kicad_sch (version 20211123) (generator eeschema)
  (paper "A4")
  (lib_symbols
    (symbol "Device:LED" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "D" (id 0) (at 0 2.54 0))
      (property "Value" "LED" (id 1) (at 0 -2.54 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "LED diode" (id 4) (at 0 0 0))
      (property "ki_description" "Light emitting diode" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "LED* LED_SMD:* LED_THT:*" (id 6) (at 0 0 0))
      (symbol "LED_0_1"
        (polyline
          (pts
            (xy -1.27 -1.27)
            (xy -1.27 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 0)
            (xy 1.27 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -1.27)
            (xy 1.27 1.27)
            (xy -1.27 0)
            (xy 1.27 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.048 -0.762)
            (xy -4.572 -2.286)
            (xy -3.81 -2.286)
            (xy -4.572 -2.286)
            (xy -4.572 -1.524)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.778 -0.762)
            (xy -3.302 -2.286)
            (xy -2.54 -2.286)
            (xy -3.302 -2.286)
            (xy -3.302 -1.524)
          )
          (fill (type none))
        )
      )
      (symbol "LED_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "K")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "A")
          (number "2")
        )
      )
    )
    (symbol "Device:R" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "R" (id 0) (at 2.032 0 90))
      (property "Value" "R" (id 1) (at 0 0 90))
      (property "Footprint" "" (id 2) (at -1.778 0 90))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "R res resistor" (id 4) (at 0 0 0))
      (property "ki_description" "Resistor" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "R_*" (id 6) (at 0 0 0))
      (symbol "R_0_1"
        (rectangle (start -1.016 -2.54) (end 1.016 2.54)
          (fill (type none))
        )
      )
      (symbol "R_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Diode:1N4001" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "D" (id 0) (at 0 2.54 0))
      (property "Value" "1N4001" (id 1) (at 0 -2.54 0))
      (property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal" (id 2) (at 0 -4.445 0))
      (property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf" (id 3) (at 0 0 0))
      (property "ki_keywords" "diode" (id 4) (at 0 0 0))
      (property "ki_description" "50V 1A General Purpose Rectifier Diode, DO-41" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "D*DO?41*" (id 6) (at 0 0 0))
      (symbol "1N4001_0_1"
        (polyline
          (pts
            (xy -1.27 1.27)
            (xy -1.27 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 0)
            (xy -1.27 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 1.27)
            (xy 1.27 -1.27)
            (xy -1.27 0)
            (xy 1.27 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "1N4001_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "K")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "A")
          (number "2")
        )
      )
    )
    (symbol "MCU_Microchip_ATmega:ATmega8A-A" (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -12.7 34.29 0))
      (property "Value" "ATmega8A-A" (id 1) (at 5.08 -34.29 0))
      (property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm" (id 2) (at 0 0 0))
      (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Microchip%208bit%20mcu%20AVR%20ATmega8A%20data%20sheet%2040001974A.pdf" (id 3) (at 0 0 0))
      (property "ki_keywords" "AVR 8bit Microcontroller MegaAVR" (id 4) (at 0 0 0))
      (property "ki_description" "16MHz, 8kB Flash, 1kB SRAM, 512B EEPROM, TQFP-32" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*" (id 6) (at 0 0 0))
      (symbol "ATmega8A-A_0_1"
        (rectangle (start -12.7 -33.02) (end 12.7 33.02)
          (fill (type background))
        )
      )
      (symbol "ATmega8A-A_1_1"
        (pin bidirectional line (at 15.24 -15.24 180) (length 2.54)
          (name "PD3")
          (number "1")
        )
        (pin bidirectional line (at 15.24 -22.86 180) (length 2.54)
          (name "PD6")
          (number "10")
        )
        (pin bidirectional line (at 15.24 -25.4 180) (length 2.54)
          (name "PD7")
          (number "11")
        )
        (pin bidirectional line (at 15.24 27.94 180) (length 2.54)
          (name "PB0")
          (number "12")
        )
        (pin bidirectional line (at 15.24 25.4 180) (length 2.54)
          (name "PB1")
          (number "13")
        )
        (pin bidirectional line (at 15.24 22.86 180) (length 2.54)
          (name "PB2")
          (number "14")
        )
        (pin bidirectional line (at 15.24 20.32 180) (length 2.54)
          (name "PB3")
          (number "15")
        )
        (pin bidirectional line (at 15.24 17.78 180) (length 2.54)
          (name "PB4")
          (number "16")
        )
        (pin bidirectional line (at 15.24 15.24 180) (length 2.54)
          (name "PB5")
          (number "17")
        )
        (pin power_in line (at 2.54 35.56 270) (length 2.54)
          (name "AVCC")
          (number "18")
        )
        (pin input line (at -15.24 7.62 0) (length 2.54)
          (name "ADC6")
          (number "19")
        )
        (pin bidirectional line (at 15.24 -17.78 180) (length 2.54)
          (name "PD4")
          (number "2")
        )
        (pin passive line (at -15.24 12.7 0) (length 2.54)
          (name "AREF")
          (number "20")
        )
        (pin power_in line (at 2.54 -35.56 90) (length 2.54)
          (name "AGND")
          (number "21")
        )
        (pin input line (at -15.24 5.08 0) (length 2.54)
          (name "ADC7")
          (number "22")
        )
        (pin bidirectional line (at 15.24 10.16 180) (length 2.54)
          (name "PC0")
          (number "23")
        )
        (pin bidirectional line (at 15.24 7.62 180) (length 2.54)
          (name "PC1")
          (number "24")
        )
        (pin bidirectional line (at 15.24 5.08 180) (length 2.54)
          (name "PC2")
          (number "25")
        )
        (pin bidirectional line (at 15.24 2.54 180) (length 2.54)
          (name "PC3")
          (number "26")
        )
        (pin bidirectional line (at 15.24 0 180) (length 2.54)
          (name "PC4")
          (number "27")
        )
        (pin bidirectional line (at 15.24 -2.54 180) (length 2.54)
          (name "PC5")
          (number "28")
        )
        (pin bidirectional line (at -15.24 27.94 0) (length 2.54)
          (name "PC6/~{RESET}")
          (number "29")
        )
        (pin power_in line (at 0 -35.56 90) (length 2.54)
          (name "GND")
          (number "3")
        )
        (pin bidirectional line (at 15.24 -7.62 180) (length 2.54)
          (name "PD0")
          (number "30")
        )
        (pin bidirectional line (at 15.24 -10.16 180) (length 2.54)
          (name "PD1")
          (number "31")
        )
        (pin bidirectional line (at 15.24 -12.7 180) (length 2.54)
          (name "PD2")
          (number "32")
        )
        (pin power_in line (at 0 35.56 270) (length 2.54)
          (name "VCC")
          (number "4")
        )
        (pin passive line (at 0 -35.56 90) (length 2.54) hide
          (name "GND")
          (number "5")
        )
        (pin passive line (at 0 35.56 270) (length 2.54) hide
          (name "VCC")
          (number "6")
        )
        (pin bidirectional line (at -15.24 22.86 0) (length 2.54)
          (name "PB6/XTAL1")
          (number "7")
        )
        (pin bidirectional line (at -15.24 17.78 0) (length 2.54)
          (name "PB7/XTAL2")
          (number "8")
        )
        (pin bidirectional line (at 15.24 -20.32 180) (length 2.54)
          (name "PD5")
          (number "9")
        )
      )
    )
    (symbol "MJE13003_1" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "Ansteuerung_Relais_Absaugung_ein" (id 0) (at 5.08 1.2701 0))
      (property "Value" "MJE13003_1" (id 1) (at 5.08 -1.2699 0))
      (property "Footprint" "Package_TO_SOT_THT:TO-126-3_Vertical" (id 2) (at 5.08 1.905 0))
      (property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/MJE13003-D.PDF" (id 3) (at 0 0 0))
      (property "ki_keywords" "Switching Power High Voltage NPN Transistor" (id 4) (at 0 0 0))
      (property "ki_description" "1.5A Ic, 400V Vce, Silicon Switching Power NPN Transistor, TO-225" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "TO?126*" (id 6) (at 0 0 0))
      (symbol "MJE13003_1_0_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0.635 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 -2.54)
            (xy 0.635 -0.635)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 2.54)
            (xy 0.635 0.635)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.635 1.905)
            (xy 0.635 -1.905)
            (xy 0.635 -1.905)
          )
          (fill (type outline))
        )
        (polyline
          (pts
            (xy 1.2446 -1.778)
            (xy 1.7526 -1.27)
            (xy 2.286 -2.286)
            (xy 1.2446 -1.778)
            (xy 1.2446 -1.778)
          )
          (fill (type outline))
        )
        (circle (center 1.27 0) (radius 2.8194)
          (fill (type none))
        )
      )
      (symbol "MJE13003_1_1_1"
        (pin passive line (at 2.54 5.08 270) (length 2.54)
          (name "C")
          (number "1")
        )
        (pin input line (at -5.08 0 0) (length 5.08)
          (name "B")
          (number "2")
        )
        (pin passive line (at 2.54 -5.08 90) (length 2.54)
          (name "E")
          (number "3")
        )
      )
    )
    (symbol "Relay:G5Q-1A" (in_bom yes) (on_board yes)
      (property "Reference" "K" (id 0) (at 8.89 3.81 0))
      (property "Value" "G5Q-1A" (id 1) (at 8.89 1.27 0))
      (property "Footprint" "Relay_THT:Relay_SPST_Omron-G5Q-1A" (id 2) (at 8.89 -1.27 0))
      (property "Datasheet" "https://www.omron.com/ecb/products/pdf/en-g5q.pdf" (id 3) (at 0 0 0))
      (property "ki_keywords" "Miniature Single Pole Relay" (id 4) (at 0 0 0))
      (property "ki_description" "Omron G5Q relay, Miniature Single Pole, SPST-NO, 10A" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Relay*SPST*Omron*G5Q*" (id 6) (at 0 0 0))
      (symbol "G5Q-1A_0_0"
        (polyline
          (pts
            (xy 5.08 5.08)
            (xy 5.08 2.54)
            (xy 4.445 3.175)
            (xy 5.08 3.81)
          )
          (fill (type none))
        )
      )
      (symbol "G5Q-1A_0_1"
        (rectangle (start -10.16 5.08) (end 7.62 -5.08)
          (fill (type background))
        )
        (rectangle (start -8.255 1.905) (end -1.905 -1.905)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -7.62 -1.905)
            (xy -2.54 1.905)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -5.08 -5.08)
            (xy -5.08 -1.905)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -5.08 5.08)
            (xy -5.08 1.905)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.905 0)
            (xy -1.27 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -0.635 0)
            (xy 0 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.635 0)
            (xy 1.27 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.905 0)
            (xy 2.54 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 3.175 0)
            (xy 3.81 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 5.08 -2.54)
            (xy 3.175 3.81)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 5.08 -2.54)
            (xy 5.08 -5.08)
          )
          (fill (type none))
        )
      )
      (symbol "G5Q-1A_1_1"
        (pin passive line (at -5.08 -7.62 90) (length 2.54)
          (name "~")
          (number "1")
        )
        (pin passive line (at 5.08 -7.62 90) (length 2.54)
          (name "~")
          (number "2")
        )
        (pin passive line (at 5.08 7.62 270) (length 2.54)
          (name "~")
          (number "3")
        )
        (pin passive line (at -5.08 7.62 270) (length 2.54)
          (name "~")
          (number "5")
        )
      )
    )
    (symbol "Transistor_BJT:MJE13003" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "Q" (id 0) (at 5.08 1.905 0))
      (property "Value" "MJE13003" (id 1) (at 5.08 0 0))
      (property "Footprint" "Package_TO_SOT_THT:TO-126-3_Vertical" (id 2) (at 5.08 -1.905 0))
      (property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/MJE13003-D.PDF" (id 3) (at 0 0 0))
      (property "ki_keywords" "Switching Power High Voltage NPN Transistor" (id 4) (at 0 0 0))
      (property "ki_description" "1.5A Ic, 400V Vce, Silicon Switching Power NPN Transistor, TO-225" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "TO?126*" (id 6) (at 0 0 0))
      (symbol "MJE13003_0_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0.635 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 -2.54)
            (xy 0.635 -0.635)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 2.54)
            (xy 0.635 0.635)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.635 1.905)
            (xy 0.635 -1.905)
            (xy 0.635 -1.905)
          )
          (fill (type outline))
        )
        (polyline
          (pts
            (xy 1.2446 -1.778)
            (xy 1.7526 -1.27)
            (xy 2.286 -2.286)
            (xy 1.2446 -1.778)
            (xy 1.2446 -1.778)
          )
          (fill (type outline))
        )
        (circle (center 1.27 0) (radius 2.8194)
          (fill (type none))
        )
      )
      (symbol "MJE13003_1_1"
        (pin input line (at -5.08 0 0) (length 5.08)
          (name "B")
          (number "1")
        )
        (pin passive line (at 2.54 5.08 270) (length 2.54)
          (name "C")
          (number "2")
        )
        (pin passive line (at 2.54 -5.08 90) (length 2.54)
          (name "E")
          (number "3")
        )
      )
    )
    (symbol "Valve:EABC80" (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at 5.08 6.35 0))
      (property "Value" "EABC80" (id 1) (at 7.62 -8.89 0))
      (property "Footprint" "Valve:Valve_Noval_P" (id 2) (at 4.318 -10.414 0))
      (property "Datasheet" "https://frank.pocnet.net/sheets/082/e/EABC80.pdf" (id 3) (at 0 0 0))
      (property "ki_locked" "" (id 4) (at 0 0 0))
      (property "ki_keywords" "diode triode valve" (id 5) (at 0 0 0))
      (property "ki_description" "triple diode triode" (id 6) (at 0 0 0))
      (property "ki_fp_filters" "VALVE*NOVAL*P*" (id 7) (at 0 0 0))
      (symbol "EABC80_0_1"
        (arc (start -5.08 -2.54) (mid 0 -7.62) (end 5.08 -2.54)
          (fill (type none))
        )
        (polyline
          (pts
            (xy 5.08 2.54)
            (xy 5.08 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -5.08 2.54)
            (xy -5.08 -2.54)
            (xy -5.08 -2.54)
          )
          (fill (type none))
        )
        (arc (start 5.08 2.54) (mid 0 7.62) (end -5.08 2.54)
          (fill (type none))
        )
      )
      (symbol "EABC80_1_0"
        (polyline
          (pts
            (xy -2.54 -5.08)
            (xy -2.54 -7.62)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 5.08)
            (xy 0 7.62)
          )
          (fill (type none))
        )
      )
      (symbol "EABC80_1_1"
        (polyline
          (pts
            (xy -2.54 5.08)
            (xy 2.54 5.08)
            (xy 2.54 5.08)
            (xy 2.54 5.08)
          )
          (fill (type none))
        )
        (arc (start 2.54 -5.08) (mid 0 -3.0968) (end -2.54 -5.08)
          (fill (type none))
        )
        (pin output line (at 0 10.16 270) (length 2.54)
          (name "A2")
          (number "2")
        )
        (pin input line (at -2.54 -10.16 90) (length 2.54)
          (name "K")
          (number "3")
        )
      )
      (symbol "EABC80_2_1"
        (polyline
          (pts
            (xy -2.54 -6.858)
            (xy -2.54 -5.842)
            (xy -2.54 -5.842)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 7.112)
            (xy -2.54 2.54)
            (xy -2.54 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 3.81)
            (xy 3.81 1.27)
            (xy 3.81 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 6.858)
            (xy 2.54 2.54)
            (xy 2.54 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.81 1.27)
            (xy -1.27 3.81)
            (xy -1.27 3.81)
            (xy -1.27 3.81)
          )
          (fill (type none))
        )
        (arc (start 2.54 -5.842) (mid 0 -3.8588) (end -2.54 -5.842)
          (fill (type none))
        )
        (pin input line (at -2.54 10.16 270) (length 3.81)
          (name "A1")
          (number "1")
        )
        (pin output line (at 2.54 10.16 270) (length 3.81)
          (name "A3")
          (number "6")
        )
        (pin input line (at -2.54 -10.16 90) (length 3.81)
          (name "K")
          (number "7")
        )
      )
      (symbol "EABC80_3_0"
        (polyline
          (pts
            (xy -5.08 0)
            (xy -3.175 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -5.08 2.54)
            (xy -5.08 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 -5.08)
            (xy -2.54 -7.62)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 5.08)
            (xy 0 7.62)
          )
          (fill (type none))
        )
      )
      (symbol "EABC80_3_1"
        (polyline
          (pts
            (xy -1.905 0)
            (xy -3.175 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -0.635 0)
            (xy 0.635 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.905 0)
            (xy 3.175 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 5.08)
            (xy 2.54 5.08)
            (xy 2.54 5.08)
          )
          (fill (type none))
        )
        (arc (start 2.54 -5.08) (mid 0 -3.0968) (end -2.54 -5.08)
          (fill (type none))
        )
        (pin input line (at -2.54 -10.16 90) (length 2.54)
          (name "K")
          (number "7")
        )
        (pin input line (at -7.62 0 0) (length 2.54)
          (name "G")
          (number "8")
        )
        (pin output line (at 0 10.16 270) (length 2.54)
          (name "A2")
          (number "9")
        )
      )
      (symbol "EABC80_4_1"
        (arc (start 2.54 -6.35) (mid 0 -5.1292) (end -2.54 -6.35)
          (fill (type none))
        )
        (pin input line (at -2.54 -8.89 90) (length 2.54)
          (name "F1")
          (number "4")
        )
        (pin input line (at 2.54 -8.89 90) (length 2.54)
          (name "F2")
          (number "5")
        )
      )
    )
  )
  (junction (at 211.455 99.06) (diameter 0) (color 0 0 0 0))
  (junction (at 105.41 142.24) (diameter 0) (color 0 0 0 0))
  (junction (at 256.54 117.475) (diameter 0) (color 0 0 0 0))
  (junction (at 71.12 61.595) (diameter 0) (color 0 0 0 0))
  (junction (at 64.135 59.055) (diameter 0) (color 0 0 0 0))
  (junction (at 210.82 117.475) (diameter 0) (color 0 0 0 0))
  (junction (at 171.45 64.135) (diameter 0) (color 0 0 0 0))
  (junction (at 172.085 81.28) (diameter 0) (color 0 0 0 0))
  (junction (at 172.085 99.06) (diameter 0) (color 0 0 0 0))
  (junction (at 264.16 24.765) (diameter 0) (color 0 0 0 0))
  (junction (at 256.54 64.135) (diameter 0) (color 0 0 0 0))
  (junction (at 203.835 90.17) (diameter 0) (color 0 0 0 0))
  (junction (at 172.085 117.475) (diameter 0) (color 0 0 0 0))
  (junction (at 71.12 24.765) (diameter 0) (color 0 0 0 0))
  (junction (at 85.09 112.395) (diameter 0) (color 0 0 0 0))
  (junction (at 211.455 64.135) (diameter 0) (color 0 0 0 0))
  (junction (at 182.88 154.305) (diameter 0) (color 0 0 0 0))
  (junction (at 203.2 126.365) (diameter 0) (color 0 0 0 0))
  (junction (at 105.41 24.765) (diameter 0) (color 0 0 0 0))
  (junction (at 78.105 24.765) (diameter 0) (color 0 0 0 0))
  (junction (at 256.54 99.06) (diameter 0) (color 0 0 0 0))
  (junction (at 260.35 18.415) (diameter 0) (color 0 0 0 0))
  (junction (at 125.73 24.765) (diameter 0) (color 0 0 0 0))
  (junction (at 256.54 81.28) (diameter 0) (color 0 0 0 0))
  (junction (at 203.835 107.95) (diameter 0) (color 0 0 0 0))
  (junction (at 64.135 24.765) (diameter 0) (color 0 0 0 0))
  (junction (at 115.57 24.765) (diameter 0) (color 0 0 0 0))
  (junction (at 211.455 67.945) (diameter 0) (color 0 0 0 0))
  (junction (at 211.455 81.28) (diameter 0) (color 0 0 0 0))
  (junction (at 210.82 121.285) (diameter 0) (color 0 0 0 0))
  (junction (at 135.255 24.765) (diameter 0) (color 0 0 0 0))
  (junction (at 256.54 21.59) (diameter 0) (color 0 0 0 0))
  (junction (at 211.455 102.87) (diameter 0) (color 0 0 0 0))
  (junction (at 203.835 73.025) (diameter 0) (color 0 0 0 0))
  (junction (at 182.88 132.08) (diameter 0) (color 0 0 0 0))
  (junction (at 85.09 24.765) (diameter 0) (color 0 0 0 0))
  (junction (at 207.645 132.08) (diameter 0) (color 0 0 0 0))
  (junction (at 78.105 93.98) (diameter 0) (color 0 0 0 0))
  (junction (at 211.455 85.09) (diameter 0) (color 0 0 0 0))
  (wire (pts (xy 213.995 107.95) (xy 203.835 107.95)))
  (wire (pts (xy 213.995 85.09) (xy 211.455 85.09)))
  (wire (pts (xy 256.54 132.08) (xy 256.54 117.475)))
  (wire (pts (xy 85.09 112.395) (xy 89.535 112.395)))
  (wire (pts (xy 182.88 132.08) (xy 182.88 138.43)))
  (wire (pts (xy 57.15 66.675) (xy 66.04 66.675)))
  (wire (pts (xy 105.41 161.925) (xy 105.41 156.845)))
  (wire (pts (xy 135.255 24.765) (xy 264.16 24.765)))
  (wire (pts (xy 105.41 142.24) (xy 105.41 146.685)))
  (wire (pts (xy 64.135 24.765) (xy 71.12 24.765)))
  (wire (pts (xy 256.54 99.06) (xy 256.54 117.475)))
  (wire (pts (xy 172.085 126.365) (xy 172.085 117.475)))
  (wire (pts (xy 96.52 76.2) (xy 118.11 76.2)))
  (wire (pts (xy 125.73 81.28) (xy 172.085 81.28)))
  (wire (pts (xy 213.995 73.025) (xy 203.835 73.025)))
  (wire (pts (xy 66.04 66.675) (xy 66.04 112.395)))
  (wire (pts (xy 135.255 64.135) (xy 171.45 64.135)))
  (wire (pts (xy 85.09 52.07) (xy 85.09 112.395)))
  (wire (pts (xy 182.88 132.08) (xy 207.645 132.08)))
  (wire (pts (xy 105.41 117.475) (xy 172.085 117.475)))
  (wire (pts (xy 153.035 142.24) (xy 153.035 154.305)))
  (wire (pts (xy 172.085 107.95) (xy 172.085 99.06)))
  (wire (pts (xy 57.15 69.215) (xy 63.5 69.215)))
  (wire (pts (xy 78.105 93.98) (xy 88.9 93.98)))
  (wire (pts (xy 71.12 52.07) (xy 71.12 61.595)))
  (wire (pts (xy 256.54 81.28) (xy 256.54 99.06)))
  (wire (pts (xy 182.88 154.305) (xy 207.645 154.305)))
  (wire (pts (xy 105.41 132.08) (xy 105.41 142.24)))
  (wire (pts (xy 71.12 44.45) (xy 71.12 24.765)))
  (wire (pts (xy 71.12 24.765) (xy 78.105 24.765)))
  (wire (pts (xy 125.73 24.765) (xy 135.255 24.765)))
  (wire (pts (xy 57.15 61.595) (xy 71.12 61.595)))
  (wire (pts (xy 97.155 112.395) (xy 97.79 112.395)))
  (wire (pts (xy 203.835 85.09) (xy 203.835 90.17)))
  (wire (pts (xy 211.455 99.06) (xy 256.54 99.06)))
  (wire (pts (xy 172.085 81.28) (xy 177.165 81.28)))
  (wire (pts (xy 105.41 24.765) (xy 115.57 24.765)))
  (wire (pts (xy 211.455 85.09) (xy 211.455 81.28)))
  (wire (pts (xy 201.93 117.475) (xy 210.82 117.475)))
  (wire (pts (xy 105.41 161.925) (xy 264.16 161.925)))
  (wire (pts (xy 32.385 18.415) (xy 260.35 18.415)))
  (wire (pts (xy 203.2 121.285) (xy 203.2 126.365)))
  (wire (pts (xy 210.82 117.475) (xy 256.54 117.475)))
  (wire (pts (xy 172.085 90.17) (xy 172.085 81.28)))
  (wire (pts (xy 207.645 150.495) (xy 207.645 154.305)))
  (wire (pts (xy 135.255 24.765) (xy 135.255 53.975)))
  (wire (pts (xy 200.66 81.28) (xy 211.455 81.28)))
  (wire (pts (xy 78.105 24.765) (xy 85.09 24.765)))
  (wire (pts (xy 88.265 151.765) (xy 97.79 151.765)))
  (wire (pts (xy 171.45 73.025) (xy 171.45 64.135)))
  (wire (pts (xy 207.645 132.08) (xy 207.645 135.255)))
  (wire (pts (xy 264.16 24.765) (xy 270.51 24.765)))
  (wire (pts (xy 78.105 24.765) (xy 78.105 44.45)))
  (wire (pts (xy 203.835 107.95) (xy 172.085 107.95)))
  (wire (pts (xy 142.875 132.08) (xy 182.88 132.08)))
  (wire (pts (xy 78.105 52.07) (xy 78.105 93.98)))
  (wire (pts (xy 171.45 64.135) (xy 177.165 64.135)))
  (wire (pts (xy 66.04 112.395) (xy 85.09 112.395)))
  (wire (pts (xy 210.82 121.285) (xy 210.82 117.475)))
  (wire (pts (xy 256.54 21.59) (xy 256.54 64.135)))
  (wire (pts (xy 203.835 67.945) (xy 203.835 73.025)))
  (wire (pts (xy 64.135 59.055) (xy 88.265 59.055)))
  (wire (pts (xy 213.995 121.285) (xy 210.82 121.285)))
  (wire (pts (xy 203.835 90.17) (xy 172.085 90.17)))
  (wire (pts (xy 260.35 18.415) (xy 270.51 18.415)))
  (wire (pts (xy 105.41 24.765) (xy 105.41 107.315)))
  (wire (pts (xy 96.52 93.98) (xy 107.95 93.98)))
  (wire (pts (xy 211.455 67.945) (xy 211.455 64.135)))
  (wire (pts (xy 199.39 64.135) (xy 211.455 64.135)))
  (wire (pts (xy 57.15 64.135) (xy 68.58 64.135)))
  (wire (pts (xy 203.2 126.365) (xy 172.085 126.365)))
  (wire (pts (xy 211.455 102.87) (xy 211.455 99.06)))
  (wire (pts (xy 115.57 24.765) (xy 125.73 24.765)))
  (wire (pts (xy 68.58 93.98) (xy 78.105 93.98)))
  (wire (pts (xy 125.73 24.765) (xy 125.73 71.12)))
  (wire (pts (xy 64.135 52.07) (xy 64.135 59.055)))
  (wire (pts (xy 217.805 150.495) (xy 217.805 154.94)))
  (wire (pts (xy 32.385 21.59) (xy 256.54 21.59)))
  (wire (pts (xy 186.69 117.475) (xy 194.31 117.475)))
  (wire (pts (xy 217.805 154.94) (xy 260.35 154.94)))
  (wire (pts (xy 68.58 64.135) (xy 68.58 93.98)))
  (wire (pts (xy 182.88 146.05) (xy 182.88 154.305)))
  (wire (pts (xy 213.995 67.945) (xy 211.455 67.945)))
  (wire (pts (xy 203.835 73.025) (xy 171.45 73.025)))
  (wire (pts (xy 115.57 99.06) (xy 172.085 99.06)))
  (wire (pts (xy 211.455 64.135) (xy 256.54 64.135)))
  (wire (pts (xy 172.085 117.475) (xy 179.07 117.475)))
  (wire (pts (xy 57.15 59.055) (xy 64.135 59.055)))
  (wire (pts (xy 172.085 99.06) (xy 177.8 99.06)))
  (wire (pts (xy 203.835 102.87) (xy 203.835 107.95)))
  (wire (pts (xy 256.54 64.135) (xy 256.54 81.28)))
  (wire (pts (xy 184.785 81.28) (xy 193.04 81.28)))
  (wire (pts (xy 213.995 126.365) (xy 203.2 126.365)))
  (wire (pts (xy 256.54 21.59) (xy 270.51 21.59)))
  (wire (pts (xy 115.57 24.765) (xy 115.57 88.9)))
  (wire (pts (xy 32.385 24.765) (xy 64.135 24.765)))
  (wire (pts (xy 71.12 76.2) (xy 88.9 76.2)))
  (wire (pts (xy 105.41 132.08) (xy 121.285 132.08)))
  (wire (pts (xy 71.12 61.595) (xy 71.12 76.2)))
  (wire (pts (xy 207.645 132.08) (xy 256.54 132.08)))
  (wire (pts (xy 105.41 142.24) (xy 153.035 142.24)))
  (wire (pts (xy 85.09 24.765) (xy 105.41 24.765)))
  (wire (pts (xy 153.035 154.305) (xy 182.88 154.305)))
  (wire (pts (xy 64.135 24.765) (xy 64.135 44.45)))
  (wire (pts (xy 213.995 102.87) (xy 211.455 102.87)))
  (wire (pts (xy 128.905 132.08) (xy 135.255 132.08)))
  (wire (pts (xy 264.16 24.765) (xy 264.16 161.925)))
  (wire (pts (xy 63.5 151.765) (xy 80.645 151.765)))
  (wire (pts (xy 85.09 24.765) (xy 85.09 44.45)))
  (wire (pts (xy 184.785 64.135) (xy 191.77 64.135)))
  (wire (pts (xy 185.42 99.06) (xy 193.04 99.06)))
  (wire (pts (xy 63.5 69.215) (xy 63.5 151.765)))
  (wire (pts (xy 260.35 154.94) (xy 260.35 18.415)))
  (wire (pts (xy 211.455 81.28) (xy 256.54 81.28)))
  (wire (pts (xy 95.885 59.055) (xy 127.635 59.055)))
  (wire (pts (xy 213.995 90.17) (xy 203.835 90.17)))
  (wire (pts (xy 200.66 99.06) (xy 211.455 99.06)))
  (global_label "+12V" (shape input) (at 32.385 21.59 180) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 24.8919 21.5106 0))
  )
  (global_label "gnd" (shape input) (at 32.385 24.765 180) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 26.5248 24.6856 0))
  )
  (global_label "+24V" (shape input) (at 32.385 18.415 180) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 24.8919 18.3356 0))
  )
  (symbol (lib_id "Device:LED") (at 196.85 81.28 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "Ventil_Zuziehhilfe_auf" (id 0) (at 200.025 78.105 0))
    (property "Value" "LED" (id 1) (at 196.85 78.105 0))
    (property "Footprint" "" (id 2) (at 196.85 81.28 0))
    (property "Datasheet" "~" (id 3) (at 196.85 81.28 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Transistor_BJT:MJE13003") (at 113.03 93.98 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "Ansteuerung_Ventil_Klappe_zu" (id 0) (at 118.11 92.7099 0))
    (property "Value" "MJ10012" (id 1) (at 118.11 95.2499 0))
    (property "Footprint" "Package_TO_SOT_THT:TO-126-3_Vertical" (id 2) (at 118.11 95.885 0))
    (property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/MJE13003-D.PDF" (id 3) (at 113.03 93.98 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
  (symbol (lib_id "Device:R") (at 181.61 99.06 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "470_Ohm" (id 0) (at 178.435 95.885 90))
    (property "Value" "R" (id 1) (at 181.61 99.06 90))
    (property "Footprint" "" (id 2) (at 181.61 97.282 90))
    (property "Datasheet" "~" (id 3) (at 181.61 99.06 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 182.88 117.475 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "470_Ohm" (id 0) (at 179.705 114.3 90))
    (property "Value" "R" (id 1) (at 182.88 117.475 90))
    (property "Footprint" "" (id 2) (at 182.88 115.697 90))
    (property "Datasheet" "~" (id 3) (at 182.88 117.475 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 85.09 48.26 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "47_KOhm" (id 0) (at 81.915 51.435 90))
    (property "Value" "R" (id 1) (at 85.09 48.26 90))
    (property "Footprint" "" (id 2) (at 83.312 48.26 90))
    (property "Datasheet" "~" (id 3) (at 85.09 48.26 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:LED") (at 195.58 64.135 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "Ventil_Zuziehhilfe_zu" (id 0) (at 198.755 60.96 0))
    (property "Value" "LED" (id 1) (at 195.58 60.96 0))
    (property "Footprint" "" (id 2) (at 195.58 64.135 0))
    (property "Datasheet" "~" (id 3) (at 195.58 64.135 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 93.345 112.395 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "470_Ohm" (id 0) (at 90.17 109.22 90))
    (property "Value" "R" (id 1) (at 93.345 112.395 90))
    (property "Footprint" "" (id 2) (at 93.345 110.617 90))
    (property "Datasheet" "~" (id 3) (at 93.345 112.395 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 92.71 93.98 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "470_Ohm" (id 0) (at 89.535 90.805 90))
    (property "Value" "R" (id 1) (at 92.71 93.98 90))
    (property "Footprint" "" (id 2) (at 92.71 92.202 90))
    (property "Datasheet" "~" (id 3) (at 92.71 93.98 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:LED") (at 196.85 99.06 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "Ventil_Klappe_zu" (id 0) (at 200.025 95.885 0))
    (property "Value" "LED" (id 1) (at 196.85 95.885 0))
    (property "Footprint" "" (id 2) (at 196.85 99.06 0))
    (property "Datasheet" "~" (id 3) (at 196.85 99.06 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Transistor_BJT:MJE13003") (at 132.715 59.055 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "Ansteuerung_Ventil_Zuziehhilfe_zu" (id 0) (at 137.795 57.785 0))
    (property "Value" "MJ10012" (id 1) (at 137.795 60.3249 0))
    (property "Footprint" "Package_TO_SOT_THT:TO-126-3_Vertical" (id 2) (at 137.795 60.96 0))
    (property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/MJE13003-D.PDF" (id 3) (at 132.715 59.055 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
  (symbol (lib_id "Device:LED") (at 139.065 132.08 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "Freigabe_Absaugung_ein" (id 0) (at 142.24 128.905 0))
    (property "Value" "LED" (id 1) (at 139.065 128.905 0))
    (property "Footprint" "" (id 2) (at 139.065 132.08 0))
    (property "Datasheet" "~" (id 3) (at 139.065 132.08 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Diode:1N4001") (at 182.88 142.24 90) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "D?" (id 0) (at 175.895 142.24 0))
    (property "Value" "1N4001" (id 1) (at 178.435 142.24 0))
    (property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal" (id 2) (at 187.325 142.24 0))
    (property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf" (id 3) (at 182.88 142.24 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 64.135 48.26 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "47_KOhm" (id 0) (at 60.96 51.435 90))
    (property "Value" "R" (id 1) (at 64.135 48.26 90))
    (property "Footprint" "" (id 2) (at 62.357 48.26 90))
    (property "Datasheet" "~" (id 3) (at 64.135 48.26 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 71.12 48.26 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "47_KOhm" (id 0) (at 67.945 51.435 90))
    (property "Value" "R" (id 1) (at 71.12 48.26 90))
    (property "Footprint" "" (id 2) (at 69.342 48.26 90))
    (property "Datasheet" "~" (id 3) (at 71.12 48.26 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Diode:1N4001") (at 207.645 102.87 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "D?" (id 0) (at 207.645 95.885 0))
    (property "Value" "1N4001" (id 1) (at 207.645 98.425 0))
    (property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal" (id 2) (at 207.645 107.315 0))
    (property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf" (id 3) (at 207.645 102.87 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Valve:EABC80") (at 222.885 123.825 270) (unit 4)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "Ventil_Klappe_auf" (id 0) (at 231.14 123.8249 90))
    (property "Value" "ventil" (id 1) (at 221.6151 130.175 0))
    (property "Footprint" "Valve:Valve_Noval_P" (id 2) (at 212.471 128.143 0))
    (property "Datasheet" "https://frank.pocnet.net/sheets/082/e/EABC80.pdf" (id 3) (at 222.885 123.825 0))
    (pin "2")
    (pin "3")
    (pin "1")
    (pin "6")
    (pin "7")
    (pin "7")
    (pin "8")
    (pin "9")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "Device:R") (at 125.095 132.08 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "2200_Ohm" (id 0) (at 121.92 128.905 90))
    (property "Value" "R" (id 1) (at 125.095 132.08 90))
    (property "Footprint" "" (id 2) (at 125.095 130.302 90))
    (property "Datasheet" "~" (id 3) (at 125.095 132.08 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Diode:1N4001") (at 207.01 121.285 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "D?" (id 0) (at 207.01 114.3 0))
    (property "Value" "1N4001" (id 1) (at 207.01 116.84 0))
    (property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal" (id 2) (at 207.01 125.73 0))
    (property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf" (id 3) (at 207.01 121.285 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Valve:EABC80") (at 222.885 70.485 270) (unit 4)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "Ventil_Zuziehhilfe_zu" (id 0) (at 231.14 70.4849 90))
    (property "Value" "ventil" (id 1) (at 221.6151 76.835 0))
    (property "Footprint" "Valve:Valve_Noval_P" (id 2) (at 212.471 74.803 0))
    (property "Datasheet" "https://frank.pocnet.net/sheets/082/e/EABC80.pdf" (id 3) (at 222.885 70.485 0))
    (pin "2")
    (pin "3")
    (pin "1")
    (pin "6")
    (pin "7")
    (pin "7")
    (pin "8")
    (pin "9")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "Device:R") (at 92.71 76.2 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "470_Ohm" (id 0) (at 89.535 73.025 90))
    (property "Value" "R" (id 1) (at 92.71 76.2 90))
    (property "Footprint" "" (id 2) (at 92.71 74.422 90))
    (property "Datasheet" "~" (id 3) (at 92.71 76.2 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Transistor_BJT:MJE13003") (at 123.19 76.2 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "Ansteuerung_Ventil_Zuziehhilfe_auf" (id 0) (at 128.27 74.93 0))
    (property "Value" "MJ10012" (id 1) (at 128.27 77.4699 0))
    (property "Footprint" "Package_TO_SOT_THT:TO-126-3_Vertical" (id 2) (at 128.27 78.105 0))
    (property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/MJE13003-D.PDF" (id 3) (at 123.19 76.2 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
  (symbol (lib_id "Device:R") (at 92.075 59.055 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "470_Ohm" (id 0) (at 88.9 55.88 90))
    (property "Value" "R" (id 1) (at 92.075 59.055 90))
    (property "Footprint" "" (id 2) (at 92.075 57.277 90))
    (property "Datasheet" "~" (id 3) (at 92.075 59.055 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Transistor_BJT:MJE13003") (at 102.87 112.395 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "Ansteuerung_Ventil_Klappe_auf" (id 0) (at 107.95 111.1249 0))
    (property "Value" "MJ10012" (id 1) (at 107.95 113.6649 0))
    (property "Footprint" "Package_TO_SOT_THT:TO-126-3_Vertical" (id 2) (at 107.95 114.3 0))
    (property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/MJE13003-D.PDF" (id 3) (at 102.87 112.395 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
  (symbol (lib_id "Device:LED") (at 198.12 117.475 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "Ventil_Klappe_auf" (id 0) (at 201.295 114.3 0))
    (property "Value" "LED" (id 1) (at 198.12 114.3 0))
    (property "Footprint" "" (id 2) (at 198.12 117.475 0))
    (property "Datasheet" "~" (id 3) (at 198.12 117.475 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 84.455 151.765 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "470_Ohm" (id 0) (at 81.28 148.59 90))
    (property "Value" "R" (id 1) (at 84.455 151.765 90))
    (property "Footprint" "" (id 2) (at 84.455 149.987 90))
    (property "Datasheet" "~" (id 3) (at 84.455 151.765 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Relay:G5Q-1A") (at 212.725 142.875 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "24V_Kontakt" (id 0) (at 222.885 147.955 90))
    (property "Value" "Relais 12V" (id 1) (at 200.66 147.955 90))
    (property "Footprint" "Relay_THT:Relay_SPST_Omron-G5Q-1A" (id 2) (at 221.615 144.145 0))
    (property "Datasheet" "https://www.omron.com/ecb/products/pdf/en-g5q.pdf" (id 3) (at 212.725 142.875 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "5")
  )
  (symbol (lib_id "MCU_Microchip_ATmega:ATmega8A-A") (at 41.91 69.215 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "U?" (id 0) (at 46.4694 31.115 0))
    (property "Value" "ATmega8A-A" (id 1) (at 46.4694 33.655 0))
    (property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm" (id 2) (at 41.91 69.215 0))
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Microchip%208bit%20mcu%20AVR%20ATmega8A%20data%20sheet%2040001974A.pdf" (id 3) (at 41.91 69.215 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "17")
    (pin "18")
    (pin "19")
    (pin "2")
    (pin "20")
    (pin "21")
    (pin "22")
    (pin "23")
    (pin "24")
    (pin "25")
    (pin "26")
    (pin "27")
    (pin "28")
    (pin "29")
    (pin "3")
    (pin "30")
    (pin "31")
    (pin "32")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
  )
  (symbol (lib_id "Diode:1N4001") (at 207.645 85.09 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "D?" (id 0) (at 207.645 78.105 0))
    (property "Value" "1N4001" (id 1) (at 207.645 80.645 0))
    (property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal" (id 2) (at 207.645 89.535 0))
    (property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf" (id 3) (at 207.645 85.09 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 180.975 81.28 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "470_Ohm" (id 0) (at 177.8 78.105 90))
    (property "Value" "R" (id 1) (at 180.975 81.28 90))
    (property "Footprint" "" (id 2) (at 180.975 79.502 90))
    (property "Datasheet" "~" (id 3) (at 180.975 81.28 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Valve:EABC80") (at 222.885 105.41 270) (unit 4)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "Ventil_Klappe_zu" (id 0) (at 231.14 105.4099 90))
    (property "Value" "ventil" (id 1) (at 221.6151 111.76 0))
    (property "Footprint" "Valve:Valve_Noval_P" (id 2) (at 212.471 109.728 0))
    (property "Datasheet" "https://frank.pocnet.net/sheets/082/e/EABC80.pdf" (id 3) (at 222.885 105.41 0))
    (pin "2")
    (pin "3")
    (pin "1")
    (pin "6")
    (pin "7")
    (pin "7")
    (pin "8")
    (pin "9")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_name "MJE13003_1") (lib_id "Transistor_BJT:MJE13003") (at 102.87 151.765 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "Ansteuerung_Relais_Absaugung_ein" (id 0) (at 107.95 150.4949 0))
    (property "Value" "BC546A" (id 1) (at 107.95 153.0349 0))
    (property "Footprint" "Package_TO_SOT_THT:TO-126-3_Vertical" (id 2) (at 107.95 149.86 0))
    (property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/MJE13003-D.PDF" (id 3) (at 102.87 151.765 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
  (symbol (lib_id "Valve:EABC80") (at 222.885 87.63 270) (unit 4)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "Ventil_Zuziehhilfe_auf" (id 0) (at 231.14 87.6299 90))
    (property "Value" "ventil" (id 1) (at 221.6151 93.98 0))
    (property "Footprint" "Valve:Valve_Noval_P" (id 2) (at 212.471 91.948 0))
    (property "Datasheet" "https://frank.pocnet.net/sheets/082/e/EABC80.pdf" (id 3) (at 222.885 87.63 0))
    (pin "2")
    (pin "3")
    (pin "1")
    (pin "6")
    (pin "7")
    (pin "7")
    (pin "8")
    (pin "9")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "Device:R") (at 78.105 48.26 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "47_KOhm" (id 0) (at 74.93 51.435 90))
    (property "Value" "R" (id 1) (at 78.105 48.26 90))
    (property "Footprint" "" (id 2) (at 76.327 48.26 90))
    (property "Datasheet" "~" (id 3) (at 78.105 48.26 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 180.975 64.135 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "470_Ohm" (id 0) (at 177.8 60.96 90))
    (property "Value" "R" (id 1) (at 180.975 64.135 90))
    (property "Footprint" "" (id 2) (at 180.975 62.357 90))
    (property "Datasheet" "~" (id 3) (at 180.975 64.135 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Diode:1N4001") (at 207.645 67.945 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "D?" (id 0) (at 207.645 60.96 0))
    (property "Value" "1N4001" (id 1) (at 207.645 63.5 0))
    (property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal" (id 2) (at 207.645 72.39 0))
    (property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf" (id 3) (at 207.645 67.945 0))
    (pin "1")
    (pin "2")
  )
  (sheet (at 35.56 128.905) (size 12.7 55.245) (fields_autoplaced)
    (fill (color 0 0 0 0.0000))
    (property "Sheet name" "Untitled Sheet" (id 0) (at 35.56 128.1934 0))
    (property "Sheet file" "untitled.kicad_sch" (id 1) (at 35.56 184.7346 0))
  )
  (sheet_instances
    (path (page "1"))
    (path (page "2"))
  )
  (symbol_instances
    (path
      (reference "24V_Kontakt") (unit 1) (value "Relais 12V") (footprint "Relay_THT:Relay_SPST_Omron-G5Q-1A")
    )
    (path
      (reference "47_KOhm") (unit 1) (value "R") (footprint "")
    )
    (path
      (reference "47_KOhm") (unit 1) (value "R") (footprint "")
    )
    (path
      (reference "47_KOhm") (unit 1) (value "R") (footprint "")
    )
    (path
      (reference "47_KOhm") (unit 1) (value "R") (footprint "")
    )
    (path
      (reference "470_Ohm") (unit 1) (value "R") (footprint "")
    )
    (path
      (reference "470_Ohm") (unit 1) (value "R") (footprint "")
    )
    (path
      (reference "470_Ohm") (unit 1) (value "R") (footprint "")
    )
    (path
      (reference "470_Ohm") (unit 1) (value "R") (footprint "")
    )
    (path
      (reference "470_Ohm") (unit 1) (value "R") (footprint "")
    )
    (path
      (reference "470_Ohm") (unit 1) (value "R") (footprint "")
    )
    (path
      (reference "470_Ohm") (unit 1) (value "R") (footprint "")
    )
    (path
      (reference "470_Ohm") (unit 1) (value "R") (footprint "")
    )
    (path
      (reference "470_Ohm") (unit 1) (value "R") (footprint "")
    )
    (path
      (reference "2200_Ohm") (unit 1) (value "R") (footprint "")
    )
    (path
      (reference "Ansteuerung_Relais_Absaugung_ein") (unit 1) (value "BC546A") (footprint "Package_TO_SOT_THT:TO-126-3_Vertical")
    )
    (path
      (reference "Ansteuerung_Ventil_Klappe_auf") (unit 1) (value "MJ10012") (footprint "Package_TO_SOT_THT:TO-126-3_Vertical")
    )
    (path
      (reference "Ansteuerung_Ventil_Klappe_zu") (unit 1) (value "MJ10012") (footprint "Package_TO_SOT_THT:TO-126-3_Vertical")
    )
    (path
      (reference "Ansteuerung_Ventil_Zuziehhilfe_auf") (unit 1) (value "MJ10012") (footprint "Package_TO_SOT_THT:TO-126-3_Vertical")
    )
    (path
      (reference "Ansteuerung_Ventil_Zuziehhilfe_zu") (unit 1) (value "MJ10012") (footprint "Package_TO_SOT_THT:TO-126-3_Vertical")
    )
    (path
      (reference "D?") (unit 1) (value "1N4001") (footprint "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal")
    )
    (path
      (reference "D?") (unit 1) (value "1N4001") (footprint "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal")
    )
    (path
      (reference "D?") (unit 1) (value "1N4001") (footprint "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal")
    )
    (path
      (reference "D?") (unit 1) (value "1N4001") (footprint "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal")
    )
    (path
      (reference "D?") (unit 1) (value "1N4001") (footprint "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal")
    )
    (path
      (reference "Freigabe_Absaugung_ein") (unit 1) (value "LED") (footprint "")
    )
    (path
      (reference "U?") (unit 1) (value "ATmega8A-A") (footprint "Package_QFP:TQFP-32_7x7mm_P0.8mm")
    )
    (path
      (reference "Ventil_Klappe_auf") (unit 1) (value "LED") (footprint "")
    )
    (path
      (reference "Ventil_Klappe_auf") (unit 4) (value "ventil") (footprint "Valve:Valve_Noval_P")
    )
    (path
      (reference "Ventil_Klappe_zu") (unit 1) (value "LED") (footprint "")
    )
    (path
      (reference "Ventil_Klappe_zu") (unit 4) (value "ventil") (footprint "Valve:Valve_Noval_P")
    )
    (path
      (reference "Ventil_Zuziehhilfe_auf") (unit 1) (value "LED") (footprint "")
    )
    (path
      (reference "Ventil_Zuziehhilfe_auf") (unit 4) (value "ventil") (footprint "Valve:Valve_Noval_P")
    )
    (path
      (reference "Ventil_Zuziehhilfe_zu") (unit 1) (value "LED") (footprint "")
    )
    (path
      (reference "Ventil_Zuziehhilfe_zu") (unit 4) (value "ventil") (footprint "Valve:Valve_Noval_P")
    )
  )
)
