(kicad_sch (version 20211123) (generator eeschema)
  (paper "A4")
  (lib_symbols
    (symbol "Device:CircuitBreaker_1P" (in_bom yes) (on_board yes)
      (property "Reference" "CB" (id 0) (at 1.905 0 0))
      (property "Value" "CircuitBreaker_1P" (id 1) (at 1.905 1.905 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "CB" (id 4) (at 0 0 0))
      (property "ki_description" "Single pole circuit breaker" (id 5) (at 0 0 0))
      (symbol "CircuitBreaker_1P_0_1"
        (polyline
          (pts
            (xy 0 -5.08)
            (xy 0 -3.81)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 -3.81)
            (xy -2.54 3.81)
          )
          (fill (type none))
        )
      )
      (symbol "CircuitBreaker_1P_1_1"
        (polyline
          (pts
            (xy -0.635 4.445)
            (xy 0.635 3.175)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 5.08)
            (xy 0 3.81)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.635 4.445)
            (xy -0.635 3.175)
          )
          (fill (type none))
        )
        (pin passive line (at 0 7.62 270) (length 2.54)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -7.62 90) (length 2.54)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:LED" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "D" (id 0) (at 0 2.54 0))
      (property "Value" "LED" (id 1) (at 0 -2.54 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "LED diode" (id 4) (at 0 0 0))
      (property "ki_description" "Light emitting diode" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "LED* LED_SMD:* LED_THT:*" (id 6) (at 0 0 0))
      (symbol "LED_0_1"
        (polyline
          (pts
            (xy -1.27 -1.27)
            (xy -1.27 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 0)
            (xy 1.27 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -1.27)
            (xy 1.27 1.27)
            (xy -1.27 0)
            (xy 1.27 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.048 -0.762)
            (xy -4.572 -2.286)
            (xy -3.81 -2.286)
            (xy -4.572 -2.286)
            (xy -4.572 -1.524)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.778 -0.762)
            (xy -3.302 -2.286)
            (xy -2.54 -2.286)
            (xy -3.302 -2.286)
            (xy -3.302 -1.524)
          )
          (fill (type none))
        )
      )
      (symbol "LED_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "K")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "A")
          (number "2")
        )
      )
    )
    (symbol "Device:R" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "R" (id 0) (at 2.032 0 90))
      (property "Value" "R" (id 1) (at 0 0 90))
      (property "Footprint" "" (id 2) (at -1.778 0 90))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "R res resistor" (id 4) (at 0 0 0))
      (property "ki_description" "Resistor" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "R_*" (id 6) (at 0 0 0))
      (symbol "R_0_1"
        (rectangle (start -1.016 -2.54) (end 1.016 2.54)
          (fill (type none))
        )
      )
      (symbol "R_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "MCU_Microchip_ATmega:ATmega8A-A" (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -12.7 34.29 0))
      (property "Value" "ATmega8A-A" (id 1) (at 5.08 -34.29 0))
      (property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm" (id 2) (at 0 0 0))
      (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Microchip%208bit%20mcu%20AVR%20ATmega8A%20data%20sheet%2040001974A.pdf" (id 3) (at 0 0 0))
      (property "ki_keywords" "AVR 8bit Microcontroller MegaAVR" (id 4) (at 0 0 0))
      (property "ki_description" "16MHz, 8kB Flash, 1kB SRAM, 512B EEPROM, TQFP-32" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*" (id 6) (at 0 0 0))
      (symbol "ATmega8A-A_0_1"
        (rectangle (start -12.7 -33.02) (end 12.7 33.02)
          (fill (type background))
        )
      )
      (symbol "ATmega8A-A_1_1"
        (pin bidirectional line (at 15.24 -15.24 180) (length 2.54)
          (name "PD3")
          (number "1")
        )
        (pin bidirectional line (at 15.24 -22.86 180) (length 2.54)
          (name "PD6")
          (number "10")
        )
        (pin bidirectional line (at 15.24 -25.4 180) (length 2.54)
          (name "PD7")
          (number "11")
        )
        (pin bidirectional line (at 15.24 27.94 180) (length 2.54)
          (name "PB0")
          (number "12")
        )
        (pin bidirectional line (at 15.24 25.4 180) (length 2.54)
          (name "PB1")
          (number "13")
        )
        (pin bidirectional line (at 15.24 22.86 180) (length 2.54)
          (name "PB2")
          (number "14")
        )
        (pin bidirectional line (at 15.24 20.32 180) (length 2.54)
          (name "PB3")
          (number "15")
        )
        (pin bidirectional line (at 15.24 17.78 180) (length 2.54)
          (name "PB4")
          (number "16")
        )
        (pin bidirectional line (at 15.24 15.24 180) (length 2.54)
          (name "PB5")
          (number "17")
        )
        (pin power_in line (at 2.54 35.56 270) (length 2.54)
          (name "AVCC")
          (number "18")
        )
        (pin input line (at -15.24 7.62 0) (length 2.54)
          (name "ADC6")
          (number "19")
        )
        (pin bidirectional line (at 15.24 -17.78 180) (length 2.54)
          (name "PD4")
          (number "2")
        )
        (pin passive line (at -15.24 12.7 0) (length 2.54)
          (name "AREF")
          (number "20")
        )
        (pin power_in line (at 2.54 -35.56 90) (length 2.54)
          (name "AGND")
          (number "21")
        )
        (pin input line (at -15.24 5.08 0) (length 2.54)
          (name "ADC7")
          (number "22")
        )
        (pin bidirectional line (at 15.24 10.16 180) (length 2.54)
          (name "PC0")
          (number "23")
        )
        (pin bidirectional line (at 15.24 7.62 180) (length 2.54)
          (name "PC1")
          (number "24")
        )
        (pin bidirectional line (at 15.24 5.08 180) (length 2.54)
          (name "PC2")
          (number "25")
        )
        (pin bidirectional line (at 15.24 2.54 180) (length 2.54)
          (name "PC3")
          (number "26")
        )
        (pin bidirectional line (at 15.24 0 180) (length 2.54)
          (name "PC4")
          (number "27")
        )
        (pin bidirectional line (at 15.24 -2.54 180) (length 2.54)
          (name "PC5")
          (number "28")
        )
        (pin bidirectional line (at -15.24 27.94 0) (length 2.54)
          (name "PC6/~{RESET}")
          (number "29")
        )
        (pin power_in line (at 0 -35.56 90) (length 2.54)
          (name "GND")
          (number "3")
        )
        (pin bidirectional line (at 15.24 -7.62 180) (length 2.54)
          (name "PD0")
          (number "30")
        )
        (pin bidirectional line (at 15.24 -10.16 180) (length 2.54)
          (name "PD1")
          (number "31")
        )
        (pin bidirectional line (at 15.24 -12.7 180) (length 2.54)
          (name "PD2")
          (number "32")
        )
        (pin power_in line (at 0 35.56 270) (length 2.54)
          (name "VCC")
          (number "4")
        )
        (pin passive line (at 0 -35.56 90) (length 2.54) hide
          (name "GND")
          (number "5")
        )
        (pin passive line (at 0 35.56 270) (length 2.54) hide
          (name "VCC")
          (number "6")
        )
        (pin bidirectional line (at -15.24 22.86 0) (length 2.54)
          (name "PB6/XTAL1")
          (number "7")
        )
        (pin bidirectional line (at -15.24 17.78 0) (length 2.54)
          (name "PB7/XTAL2")
          (number "8")
        )
        (pin bidirectional line (at 15.24 -20.32 180) (length 2.54)
          (name "PD5")
          (number "9")
        )
      )
    )
  )
  (junction (at 191.135 78.105) (diameter 0) (color 0 0 0 0))
  (junction (at 110.49 78.105) (diameter 0) (color 0 0 0 0))
  (junction (at 49.53 49.53) (diameter 0) (color 0 0 0 0))
  (junction (at 191.135 49.53) (diameter 0) (color 0 0 0 0))
  (junction (at 105.41 38.1) (diameter 0) (color 0 0 0 0))
  (junction (at 191.135 73.66) (diameter 0) (color 0 0 0 0))
  (junction (at 113.03 82.55) (diameter 0) (color 0 0 0 0))
  (junction (at 113.03 55.245) (diameter 0) (color 0 0 0 0))
  (junction (at 49.53 43.815) (diameter 0) (color 0 0 0 0))
  (junction (at 191.135 38.1) (diameter 0) (color 0 0 0 0))
  (junction (at 49.53 19.05) (diameter 0) (color 0 0 0 0))
  (junction (at 110.49 49.53) (diameter 0) (color 0 0 0 0))
  (junction (at 191.135 22.225) (diameter 0) (color 0 0 0 0))
  (junction (at 191.135 55.245) (diameter 0) (color 0 0 0 0))
  (junction (at 102.87 32.385) (diameter 0) (color 0 0 0 0))
  (junction (at 105.41 69.215) (diameter 0) (color 0 0 0 0))
  (junction (at 49.53 32.385) (diameter 0) (color 0 0 0 0))
  (junction (at 191.135 69.215) (diameter 0) (color 0 0 0 0))
  (junction (at 49.53 38.1) (diameter 0) (color 0 0 0 0))
  (junction (at 102.87 64.77) (diameter 0) (color 0 0 0 0))
  (junction (at 191.135 32.385) (diameter 0) (color 0 0 0 0))
  (junction (at 191.135 64.77) (diameter 0) (color 0 0 0 0))
  (junction (at 191.135 43.815) (diameter 0) (color 0 0 0 0))
  (junction (at 107.95 43.815) (diameter 0) (color 0 0 0 0))
  (junction (at 107.95 73.66) (diameter 0) (color 0 0 0 0))
  (wire (pts (xy 110.49 49.53) (xy 110.49 78.105)))
  (wire (pts (xy 99.06 85.09) (xy 102.87 85.09)))
  (wire (pts (xy 49.53 43.815) (xy 52.705 43.815)))
  (wire (pts (xy 130.175 73.66) (xy 158.75 73.66)))
  (wire (pts (xy 191.135 64.77) (xy 191.135 55.245)))
  (wire (pts (xy 68.58 32.385) (xy 102.87 32.385)))
  (wire (pts (xy 129.54 38.1) (xy 191.135 38.1)))
  (wire (pts (xy 107.95 73.66) (xy 122.555 73.66)))
  (wire (pts (xy 49.53 19.05) (xy 270.51 19.05)))
  (wire (pts (xy 129.54 43.815) (xy 191.135 43.815)))
  (wire (pts (xy 110.49 49.53) (xy 121.92 49.53)))
  (wire (pts (xy 113.03 55.245) (xy 121.92 55.245)))
  (wire (pts (xy 130.175 64.77) (xy 158.75 64.77)))
  (wire (pts (xy 166.37 78.105) (xy 191.135 78.105)))
  (wire (pts (xy 26.67 19.05) (xy 49.53 19.05)))
  (wire (pts (xy 105.41 69.215) (xy 105.41 87.63)))
  (wire (pts (xy 191.135 82.55) (xy 191.135 78.105)))
  (wire (pts (xy 191.135 78.105) (xy 191.135 73.66)))
  (wire (pts (xy 191.135 43.815) (xy 191.135 49.53)))
  (wire (pts (xy 49.53 38.1) (xy 52.705 38.1)))
  (wire (pts (xy 129.54 32.385) (xy 191.135 32.385)))
  (wire (pts (xy 49.53 32.385) (xy 49.53 38.1)))
  (wire (pts (xy 122.555 78.105) (xy 110.49 78.105)))
  (wire (pts (xy 53.34 32.385) (xy 49.53 32.385)))
  (wire (pts (xy 102.87 64.77) (xy 102.87 85.09)))
  (wire (pts (xy 130.175 78.105) (xy 158.75 78.105)))
  (wire (pts (xy 52.705 55.245) (xy 49.53 55.245)))
  (wire (pts (xy 52.705 49.53) (xy 49.53 49.53)))
  (wire (pts (xy 166.37 82.55) (xy 191.135 82.55)))
  (wire (pts (xy 130.175 69.215) (xy 158.75 69.215)))
  (wire (pts (xy 107.95 43.815) (xy 121.92 43.815)))
  (wire (pts (xy 113.03 82.55) (xy 113.03 95.25)))
  (wire (pts (xy 191.135 32.385) (xy 191.135 38.1)))
  (wire (pts (xy 166.37 64.77) (xy 191.135 64.77)))
  (wire (pts (xy 113.03 55.245) (xy 113.03 82.55)))
  (wire (pts (xy 99.06 92.71) (xy 110.49 92.71)))
  (wire (pts (xy 49.53 38.1) (xy 49.53 43.815)))
  (wire (pts (xy 110.49 78.105) (xy 110.49 92.71)))
  (wire (pts (xy 67.945 55.245) (xy 113.03 55.245)))
  (wire (pts (xy 158.75 82.55) (xy 130.175 82.55)))
  (wire (pts (xy 99.06 90.17) (xy 107.95 90.17)))
  (wire (pts (xy 191.135 22.225) (xy 270.51 22.225)))
  (wire (pts (xy 191.135 32.385) (xy 191.135 22.225)))
  (wire (pts (xy 26.67 22.225) (xy 191.135 22.225)))
  (wire (pts (xy 191.135 38.1) (xy 191.135 43.815)))
  (wire (pts (xy 105.41 38.1) (xy 105.41 69.215)))
  (wire (pts (xy 122.555 69.215) (xy 105.41 69.215)))
  (wire (pts (xy 129.54 49.53) (xy 191.135 49.53)))
  (wire (pts (xy 67.945 38.1) (xy 105.41 38.1)))
  (wire (pts (xy 107.95 73.66) (xy 107.95 43.815)))
  (wire (pts (xy 49.53 55.245) (xy 49.53 49.53)))
  (wire (pts (xy 122.555 64.77) (xy 102.87 64.77)))
  (wire (pts (xy 99.06 87.63) (xy 105.41 87.63)))
  (wire (pts (xy 49.53 49.53) (xy 49.53 43.815)))
  (wire (pts (xy 102.87 32.385) (xy 121.92 32.385)))
  (wire (pts (xy 49.53 19.05) (xy 49.53 32.385)))
  (wire (pts (xy 129.54 55.245) (xy 191.135 55.245)))
  (wire (pts (xy 67.945 43.815) (xy 107.95 43.815)))
  (wire (pts (xy 113.03 82.55) (xy 122.555 82.55)))
  (wire (pts (xy 107.95 73.66) (xy 107.95 90.17)))
  (wire (pts (xy 166.37 73.66) (xy 191.135 73.66)))
  (wire (pts (xy 113.03 95.25) (xy 99.06 95.25)))
  (wire (pts (xy 102.87 32.385) (xy 102.87 64.77)))
  (wire (pts (xy 166.37 69.215) (xy 191.135 69.215)))
  (wire (pts (xy 191.135 69.215) (xy 191.135 64.77)))
  (wire (pts (xy 191.135 49.53) (xy 191.135 55.245)))
  (wire (pts (xy 67.945 49.53) (xy 110.49 49.53)))
  (wire (pts (xy 105.41 38.1) (xy 121.92 38.1)))
  (wire (pts (xy 191.135 73.66) (xy 191.135 69.215)))
  (global_label "+5V" (shape input) (at 26.67 19.05 180) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 20.3864 18.9706 0))
  )
  (global_label "gnd" (shape input) (at 26.67 22.225 180) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 20.8098 22.1456 0))
  )
  (symbol (lib_id "Device:LED") (at 126.365 73.66 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "Klappe_zu" (id 0) (at 134.62 72.39 0))
    (property "Value" "LED" (id 1) (at 131.445 72.39 0))
    (property "Footprint" "" (id 2) (at 126.365 73.66 0))
    (property "Datasheet" "~" (id 3) (at 126.365 73.66 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 162.56 78.105 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "470_Ohm" (id 0) (at 169.545 76.835 90))
    (property "Value" "R" (id 1) (at 162.56 78.105 90))
    (property "Footprint" "" (id 2) (at 162.56 76.327 90))
    (property "Datasheet" "~" (id 3) (at 162.56 78.105 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:CircuitBreaker_1P") (at 60.325 43.815 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "CB?" (id 0) (at 89.535 42.545 90))
    (property "Value" "Endlage_Klappe_zu" (id 1) (at 69.215 42.545 90))
    (property "Footprint" "" (id 2) (at 60.325 43.815 0))
    (property "Datasheet" "~" (id 3) (at 60.325 43.815 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:CircuitBreaker_1P") (at 60.325 55.245 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "CB?" (id 0) (at 89.535 53.975 90))
    (property "Value" "Taster_Klappe_auf_zu" (id 1) (at 69.215 53.975 90))
    (property "Footprint" "" (id 2) (at 60.325 55.245 0))
    (property "Datasheet" "~" (id 3) (at 60.325 55.245 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 125.73 43.815 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "2400_Ohm" (id 0) (at 132.715 42.545 90))
    (property "Value" "R" (id 1) (at 125.73 43.815 90))
    (property "Footprint" "" (id 2) (at 125.73 42.037 90))
    (property "Datasheet" "~" (id 3) (at 125.73 43.815 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:LED") (at 126.365 64.77 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "Absaugung_ein" (id 0) (at 134.62 63.5 0))
    (property "Value" "LED" (id 1) (at 131.445 63.5 0))
    (property "Footprint" "" (id 2) (at 126.365 64.77 0))
    (property "Datasheet" "~" (id 3) (at 126.365 64.77 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:LED") (at 126.365 82.55 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "Taster_Klappe_auf_zu" (id 0) (at 134.62 81.28 0))
    (property "Value" "LED" (id 1) (at 131.445 81.28 0))
    (property "Footprint" "" (id 2) (at 126.365 82.55 0))
    (property "Datasheet" "~" (id 3) (at 126.365 82.55 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:LED") (at 126.365 78.105 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "Zuziehhilfe_auf" (id 0) (at 134.62 76.835 0))
    (property "Value" "LED" (id 1) (at 131.445 76.835 0))
    (property "Footprint" "" (id 2) (at 126.365 78.105 0))
    (property "Datasheet" "~" (id 3) (at 126.365 78.105 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 162.56 82.55 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "470_Ohm" (id 0) (at 169.545 81.28 90))
    (property "Value" "R" (id 1) (at 162.56 82.55 90))
    (property "Footprint" "" (id 2) (at 162.56 80.772 90))
    (property "Datasheet" "~" (id 3) (at 162.56 82.55 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 162.56 69.215 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "470_Ohm" (id 0) (at 169.545 67.945 90))
    (property "Value" "R" (id 1) (at 162.56 69.215 90))
    (property "Footprint" "" (id 2) (at 162.56 67.437 90))
    (property "Datasheet" "~" (id 3) (at 162.56 69.215 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:CircuitBreaker_1P") (at 60.96 32.385 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "keine?" (id 0) (at 90.17 31.115 90))
    (property "Value" "Schalter_Absaugung_ein" (id 1) (at 69.215 31.115 90))
    (property "Footprint" "" (id 2) (at 60.96 32.385 0))
    (property "Datasheet" "~" (id 3) (at 60.96 32.385 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 125.73 38.1 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "2400_Ohm" (id 0) (at 132.715 36.83 90))
    (property "Value" "R" (id 1) (at 125.73 38.1 90))
    (property "Footprint" "" (id 2) (at 125.73 36.322 90))
    (property "Datasheet" "~" (id 3) (at 125.73 38.1 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:LED") (at 126.365 69.215 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "Klappe_auf" (id 0) (at 134.62 67.945 0))
    (property "Value" "LED" (id 1) (at 131.445 67.945 0))
    (property "Footprint" "" (id 2) (at 126.365 69.215 0))
    (property "Datasheet" "~" (id 3) (at 126.365 69.215 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 162.56 73.66 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "470_Ohm" (id 0) (at 169.545 72.39 90))
    (property "Value" "R" (id 1) (at 162.56 73.66 90))
    (property "Footprint" "" (id 2) (at 162.56 71.882 90))
    (property "Datasheet" "~" (id 3) (at 162.56 73.66 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 162.56 64.77 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "470_Ohm" (id 0) (at 169.545 63.5 90))
    (property "Value" "R" (id 1) (at 162.56 64.77 90))
    (property "Footprint" "" (id 2) (at 162.56 62.992 90))
    (property "Datasheet" "~" (id 3) (at 162.56 64.77 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "MCU_Microchip_ATmega:ATmega8A-A") (at 83.82 110.49 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "U?" (id 0) (at 88.3794 72.39 0))
    (property "Value" "ATmega8A-A" (id 1) (at 88.3794 74.93 0))
    (property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm" (id 2) (at 83.82 110.49 0))
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Microchip%208bit%20mcu%20AVR%20ATmega8A%20data%20sheet%2040001974A.pdf" (id 3) (at 83.82 110.49 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "17")
    (pin "18")
    (pin "19")
    (pin "2")
    (pin "20")
    (pin "21")
    (pin "22")
    (pin "23")
    (pin "24")
    (pin "25")
    (pin "26")
    (pin "27")
    (pin "28")
    (pin "29")
    (pin "3")
    (pin "30")
    (pin "31")
    (pin "32")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
  )
  (symbol (lib_id "Device:R") (at 125.73 55.245 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "2400_Ohm" (id 0) (at 132.715 53.975 90))
    (property "Value" "R" (id 1) (at 125.73 55.245 90))
    (property "Footprint" "" (id 2) (at 125.73 53.467 90))
    (property "Datasheet" "~" (id 3) (at 125.73 55.245 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 125.73 49.53 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "2400_Ohm" (id 0) (at 132.715 48.26 90))
    (property "Value" "R" (id 1) (at 125.73 49.53 90))
    (property "Footprint" "" (id 2) (at 125.73 47.752 90))
    (property "Datasheet" "~" (id 3) (at 125.73 49.53 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:CircuitBreaker_1P") (at 60.325 38.1 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "keine" (id 0) (at 89.535 36.83 90))
    (property "Value" "Endlage_Klappe_auf" (id 1) (at 69.215 36.83 90))
    (property "Footprint" "" (id 2) (at 60.325 38.1 0))
    (property "Datasheet" "~" (id 3) (at 60.325 38.1 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:CircuitBreaker_1P") (at 60.325 49.53 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "CB?" (id 0) (at 89.535 48.26 90))
    (property "Value" "Endlage_Zuziehhilfe_auf" (id 1) (at 69.215 48.26 90))
    (property "Footprint" "" (id 2) (at 60.325 49.53 0))
    (property "Datasheet" "~" (id 3) (at 60.325 49.53 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 125.73 32.385 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "2400_Ohm" (id 0) (at 132.715 31.115 90))
    (property "Value" "R" (id 1) (at 125.73 32.385 90))
    (property "Footprint" "" (id 2) (at 125.73 30.607 90))
    (property "Datasheet" "~" (id 3) (at 125.73 32.385 0))
    (pin "1")
    (pin "2")
  )
  (sheet (at 20.955 135.255) (size 12.7 55.245) (fields_autoplaced)
    (fill (color 0 0 0 0.0000))
    (property "Sheet name" "Untitled Sheet" (id 0) (at 20.955 134.5434 0))
    (property "Sheet file" "untitled.kicad_sch" (id 1) (at 20.955 191.0846 0))
  )
  (sheet_instances
    (path (page "1"))
    (path (page "2"))
  )
  (symbol_instances
    (path
      (reference "470_Ohm") (unit 1) (value "R") (footprint "")
    )
    (path
      (reference "470_Ohm") (unit 1) (value "R") (footprint "")
    )
    (path
      (reference "470_Ohm") (unit 1) (value "R") (footprint "")
    )
    (path
      (reference "470_Ohm") (unit 1) (value "R") (footprint "")
    )
    (path
      (reference "470_Ohm") (unit 1) (value "R") (footprint "")
    )
    (path
      (reference "2400_Ohm") (unit 1) (value "R") (footprint "")
    )
    (path
      (reference "2400_Ohm") (unit 1) (value "R") (footprint "")
    )
    (path
      (reference "2400_Ohm") (unit 1) (value "R") (footprint "")
    )
    (path
      (reference "2400_Ohm") (unit 1) (value "R") (footprint "")
    )
    (path
      (reference "2400_Ohm") (unit 1) (value "R") (footprint "")
    )
    (path
      (reference "Absaugung_ein") (unit 1) (value "LED") (footprint "")
    )
    (path
      (reference "CB?") (unit 1) (value "Endlage_Klappe_zu") (footprint "")
    )
    (path
      (reference "CB?") (unit 1) (value "Taster_Klappe_auf_zu") (footprint "")
    )
    (path
      (reference "CB?") (unit 1) (value "Endlage_Zuziehhilfe_auf") (footprint "")
    )
    (path
      (reference "Klappe_auf") (unit 1) (value "LED") (footprint "")
    )
    (path
      (reference "Klappe_zu") (unit 1) (value "LED") (footprint "")
    )
    (path
      (reference "Taster_Klappe_auf_zu") (unit 1) (value "LED") (footprint "")
    )
    (path
      (reference "U?") (unit 1) (value "ATmega8A-A") (footprint "Package_QFP:TQFP-32_7x7mm_P0.8mm")
    )
    (path
      (reference "Zuziehhilfe_auf") (unit 1) (value "LED") (footprint "")
    )
    (path
      (reference "keine") (unit 1) (value "Endlage_Klappe_auf") (footprint "")
    )
    (path
      (reference "keine?") (unit 1) (value "Schalter_Absaugung_ein") (footprint "")
    )
  )
)
