(kicad_sch (version 20211123) (generator eeschema)
  (paper "A4")
  (lib_symbols
    (symbol "Connector_Generic:Conn_02x05_Top_Bottom" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at 1.27 7.62 0))
      (property "Value" "Conn_02x05_Top_Bottom" (id 1) (at 1.27 -7.62 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "connector" (id 4) (at 0 0 0))
      (property "ki_description" "Generic connector, double row, 02x05, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Connector*:*_2x??_*" (id 6) (at 0 0 0))
      (symbol "Conn_02x05_Top_Bottom_1_1"
        (rectangle (start -1.27 -4.953) (end 0 -5.207)
          (fill (type none))
        )
        (rectangle (start -1.27 -2.413) (end 0 -2.667)
          (fill (type none))
        )
        (rectangle (start -1.27 0.127) (end 0 -0.127)
          (fill (type none))
        )
        (rectangle (start -1.27 2.667) (end 0 2.413)
          (fill (type none))
        )
        (rectangle (start -1.27 5.207) (end 0 4.953)
          (fill (type none))
        )
        (rectangle (start -1.27 6.35) (end 3.81 -6.35)
          (fill (type background))
        )
        (rectangle (start 3.81 -4.953) (end 2.54 -5.207)
          (fill (type none))
        )
        (rectangle (start 3.81 -2.413) (end 2.54 -2.667)
          (fill (type none))
        )
        (rectangle (start 3.81 0.127) (end 2.54 -0.127)
          (fill (type none))
        )
        (rectangle (start 3.81 2.667) (end 2.54 2.413)
          (fill (type none))
        )
        (rectangle (start 3.81 5.207) (end 2.54 4.953)
          (fill (type none))
        )
        (pin passive line (at -5.08 5.08 0) (length 3.81)
          (name "Pin_1")
          (number "1")
        )
        (pin passive line (at 7.62 -5.08 180) (length 3.81)
          (name "Pin_10")
          (number "10")
        )
        (pin passive line (at -5.08 2.54 0) (length 3.81)
          (name "Pin_2")
          (number "2")
        )
        (pin passive line (at -5.08 0 0) (length 3.81)
          (name "Pin_3")
          (number "3")
        )
        (pin passive line (at -5.08 -2.54 0) (length 3.81)
          (name "Pin_4")
          (number "4")
        )
        (pin passive line (at -5.08 -5.08 0) (length 3.81)
          (name "Pin_5")
          (number "5")
        )
        (pin passive line (at 7.62 5.08 180) (length 3.81)
          (name "Pin_6")
          (number "6")
        )
        (pin passive line (at 7.62 2.54 180) (length 3.81)
          (name "Pin_7")
          (number "7")
        )
        (pin passive line (at 7.62 0 180) (length 3.81)
          (name "Pin_8")
          (number "8")
        )
        (pin passive line (at 7.62 -2.54 180) (length 3.81)
          (name "Pin_9")
          (number "9")
        )
      )
    )
    (symbol "Device:C" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.635 2.54 0))
      (property "Value" "C" (id 1) (at 0.635 -2.54 0))
      (property "Footprint" "" (id 2) (at 0.9652 -3.81 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "cap capacitor" (id 4) (at 0 0 0))
      (property "ki_description" "Unpolarized capacitor" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "C_*" (id 6) (at 0 0 0))
      (symbol "C_0_1"
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy 2.032 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762)
          )
          (fill (type none))
        )
      )
      (symbol "C_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 2.794)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:Fuse" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "F" (id 0) (at 2.032 0 90))
      (property "Value" "Fuse" (id 1) (at -1.905 0 90))
      (property "Footprint" "" (id 2) (at -1.778 0 90))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "fuse" (id 4) (at 0 0 0))
      (property "ki_description" "Fuse" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "*Fuse*" (id 6) (at 0 0 0))
      (symbol "Fuse_0_1"
        (rectangle (start -0.762 -2.54) (end 0.762 2.54)
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0 -2.54)
          )
          (fill (type none))
        )
      )
      (symbol "Fuse_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:LED" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "D" (id 0) (at 0 2.54 0))
      (property "Value" "LED" (id 1) (at 0 -2.54 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "LED diode" (id 4) (at 0 0 0))
      (property "ki_description" "Light emitting diode" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "LED* LED_SMD:* LED_THT:*" (id 6) (at 0 0 0))
      (symbol "LED_0_1"
        (polyline
          (pts
            (xy -1.27 -1.27)
            (xy -1.27 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 0)
            (xy 1.27 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -1.27)
            (xy 1.27 1.27)
            (xy -1.27 0)
            (xy 1.27 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.048 -0.762)
            (xy -4.572 -2.286)
            (xy -3.81 -2.286)
            (xy -4.572 -2.286)
            (xy -4.572 -1.524)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.778 -0.762)
            (xy -3.302 -2.286)
            (xy -2.54 -2.286)
            (xy -3.302 -2.286)
            (xy -3.302 -1.524)
          )
          (fill (type none))
        )
      )
      (symbol "LED_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "K")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "A")
          (number "2")
        )
      )
    )
    (symbol "Device:R" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "R" (id 0) (at 2.032 0 90))
      (property "Value" "R" (id 1) (at 0 0 90))
      (property "Footprint" "" (id 2) (at -1.778 0 90))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "R res resistor" (id 4) (at 0 0 0))
      (property "ki_description" "Resistor" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "R_*" (id 6) (at 0 0 0))
      (symbol "R_0_1"
        (rectangle (start -1.016 -2.54) (end 1.016 2.54)
          (fill (type none))
        )
      )
      (symbol "R_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "MCU_Microchip_ATmega:ATmega8A-A" (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -12.7 34.29 0))
      (property "Value" "ATmega8A-A" (id 1) (at 5.08 -34.29 0))
      (property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm" (id 2) (at 0 0 0))
      (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Microchip%208bit%20mcu%20AVR%20ATmega8A%20data%20sheet%2040001974A.pdf" (id 3) (at 0 0 0))
      (property "ki_keywords" "AVR 8bit Microcontroller MegaAVR" (id 4) (at 0 0 0))
      (property "ki_description" "16MHz, 8kB Flash, 1kB SRAM, 512B EEPROM, TQFP-32" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*" (id 6) (at 0 0 0))
      (symbol "ATmega8A-A_0_1"
        (rectangle (start -12.7 -33.02) (end 12.7 33.02)
          (fill (type background))
        )
      )
      (symbol "ATmega8A-A_1_1"
        (pin bidirectional line (at 15.24 -15.24 180) (length 2.54)
          (name "PD3")
          (number "1")
        )
        (pin bidirectional line (at 15.24 -22.86 180) (length 2.54)
          (name "PD6")
          (number "10")
        )
        (pin bidirectional line (at 15.24 -25.4 180) (length 2.54)
          (name "PD7")
          (number "11")
        )
        (pin bidirectional line (at 15.24 27.94 180) (length 2.54)
          (name "PB0")
          (number "12")
        )
        (pin bidirectional line (at 15.24 25.4 180) (length 2.54)
          (name "PB1")
          (number "13")
        )
        (pin bidirectional line (at 15.24 22.86 180) (length 2.54)
          (name "PB2")
          (number "14")
        )
        (pin bidirectional line (at 15.24 20.32 180) (length 2.54)
          (name "PB3")
          (number "15")
        )
        (pin bidirectional line (at 15.24 17.78 180) (length 2.54)
          (name "PB4")
          (number "16")
        )
        (pin bidirectional line (at 15.24 15.24 180) (length 2.54)
          (name "PB5")
          (number "17")
        )
        (pin power_in line (at 2.54 35.56 270) (length 2.54)
          (name "AVCC")
          (number "18")
        )
        (pin input line (at -15.24 7.62 0) (length 2.54)
          (name "ADC6")
          (number "19")
        )
        (pin bidirectional line (at 15.24 -17.78 180) (length 2.54)
          (name "PD4")
          (number "2")
        )
        (pin passive line (at -15.24 12.7 0) (length 2.54)
          (name "AREF")
          (number "20")
        )
        (pin power_in line (at 2.54 -35.56 90) (length 2.54)
          (name "AGND")
          (number "21")
        )
        (pin input line (at -15.24 5.08 0) (length 2.54)
          (name "ADC7")
          (number "22")
        )
        (pin bidirectional line (at 15.24 10.16 180) (length 2.54)
          (name "PC0")
          (number "23")
        )
        (pin bidirectional line (at 15.24 7.62 180) (length 2.54)
          (name "PC1")
          (number "24")
        )
        (pin bidirectional line (at 15.24 5.08 180) (length 2.54)
          (name "PC2")
          (number "25")
        )
        (pin bidirectional line (at 15.24 2.54 180) (length 2.54)
          (name "PC3")
          (number "26")
        )
        (pin bidirectional line (at 15.24 0 180) (length 2.54)
          (name "PC4")
          (number "27")
        )
        (pin bidirectional line (at 15.24 -2.54 180) (length 2.54)
          (name "PC5")
          (number "28")
        )
        (pin bidirectional line (at -15.24 27.94 0) (length 2.54)
          (name "PC6/~{RESET}")
          (number "29")
        )
        (pin power_in line (at 0 -35.56 90) (length 2.54)
          (name "GND")
          (number "3")
        )
        (pin bidirectional line (at 15.24 -7.62 180) (length 2.54)
          (name "PD0")
          (number "30")
        )
        (pin bidirectional line (at 15.24 -10.16 180) (length 2.54)
          (name "PD1")
          (number "31")
        )
        (pin bidirectional line (at 15.24 -12.7 180) (length 2.54)
          (name "PD2")
          (number "32")
        )
        (pin power_in line (at 0 35.56 270) (length 2.54)
          (name "VCC")
          (number "4")
        )
        (pin passive line (at 0 -35.56 90) (length 2.54) hide
          (name "GND")
          (number "5")
        )
        (pin passive line (at 0 35.56 270) (length 2.54) hide
          (name "VCC")
          (number "6")
        )
        (pin bidirectional line (at -15.24 22.86 0) (length 2.54)
          (name "PB6/XTAL1")
          (number "7")
        )
        (pin bidirectional line (at -15.24 17.78 0) (length 2.54)
          (name "PB7/XTAL2")
          (number "8")
        )
        (pin bidirectional line (at 15.24 -20.32 180) (length 2.54)
          (name "PD5")
          (number "9")
        )
      )
    )
    (symbol "Motor:Fan" (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "M" (id 0) (at 2.54 5.08 0))
      (property "Value" "Fan" (id 1) (at 2.54 -2.54 0))
      (property "Footprint" "" (id 2) (at 0 0.254 0))
      (property "Datasheet" "~" (id 3) (at 0 0.254 0))
      (property "ki_keywords" "Fan Motor" (id 4) (at 0 0 0))
      (property "ki_description" "Fan" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "PinHeader*P2.54mm* TerminalBlock*" (id 6) (at 0 0 0))
      (symbol "Fan_0_1"
        (arc (start -2.54 -0.508) (mid 0.0028 0.9121) (end 0 3.81)
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 -5.08)
            (xy 0 -4.572)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 -2.2352)
            (xy 0 -2.6416)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 4.2672)
            (xy 0 4.6228)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 4.572)
            (xy 0 5.08)
          )
          (fill (type none))
        )
        (circle (center 0 1.016) (radius 3.2512)
          (fill (type none))
        )
        (arc (start 0 3.81) (mid 0.053 0.921) (end 2.54 -0.508)
          (fill (type none))
        )
        (arc (start 2.54 -0.508) (mid 0 1.0618) (end -2.54 -0.508)
          (fill (type none))
        )
      )
      (symbol "Fan_1_1"
        (pin passive line (at 0 7.62 270) (length 2.54)
          (name "+")
          (number "1")
        )
        (pin passive line (at 0 -5.08 90) (length 2.54)
          (name "-")
          (number "2")
        )
      )
    )
    (symbol "Regulator_Linear:LM7805_TO220" (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -3.81 3.175 0))
      (property "Value" "LM7805_TO220" (id 1) (at 0 3.175 0))
      (property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical" (id 2) (at 0 5.715 0))
      (property "Datasheet" "https://www.onsemi.cn/PowerSolutions/document/MC7800-D.PDF" (id 3) (at 0 -1.27 0))
      (property "ki_keywords" "Voltage Regulator 1A Positive" (id 4) (at 0 0 0))
      (property "ki_description" "Positive 1A 35V Linear Regulator, Fixed Output 5V, TO-220" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "TO?220*" (id 6) (at 0 0 0))
      (symbol "LM7805_TO220_0_1"
        (rectangle (start -5.08 1.905) (end 5.08 -5.08)
          (fill (type background))
        )
      )
      (symbol "LM7805_TO220_1_1"
        (pin power_in line (at -7.62 0 0) (length 2.54)
          (name "VI")
          (number "1")
        )
        (pin power_in line (at 0 -7.62 90) (length 2.54)
          (name "GND")
          (number "2")
        )
        (pin power_out line (at 7.62 0 180) (length 2.54)
          (name "VO")
          (number "3")
        )
      )
    )
    (symbol "Regulator_Linear:LM7812_TO220" (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -3.81 3.175 0))
      (property "Value" "LM7812_TO220" (id 1) (at 0 3.175 0))
      (property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical" (id 2) (at 0 5.715 0))
      (property "Datasheet" "https://www.onsemi.cn/PowerSolutions/document/MC7800-D.PDF" (id 3) (at 0 -1.27 0))
      (property "ki_keywords" "Voltage Regulator 1A Positive" (id 4) (at 0 0 0))
      (property "ki_description" "Positive 1A 35V Linear Regulator, Fixed Output 12V, TO-220" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "TO?220*" (id 6) (at 0 0 0))
      (symbol "LM7812_TO220_0_1"
        (rectangle (start -5.08 1.905) (end 5.08 -5.08)
          (fill (type background))
        )
      )
      (symbol "LM7812_TO220_1_1"
        (pin power_in line (at -7.62 0 0) (length 2.54)
          (name "VI")
          (number "1")
        )
        (pin power_in line (at 0 -7.62 90) (length 2.54)
          (name "GND")
          (number "2")
        )
        (pin power_out line (at 7.62 0 180) (length 2.54)
          (name "VO")
          (number "3")
        )
      )
    )
    (symbol "Switch:SW_DPST_x2" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "SW" (id 0) (at 0 3.175 0))
      (property "Value" "SW_DPST_x2" (id 1) (at 0 -2.54 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "switch lever" (id 4) (at 0 0 0))
      (property "ki_description" "Single Pole Single Throw (SPST) switch, separate symbol" (id 5) (at 0 0 0))
      (symbol "SW_DPST_x2_0_0"
        (circle (center -2.032 0) (radius 0.508)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.524 0.254)
            (xy 1.524 1.778)
          )
          (fill (type none))
        )
        (circle (center 2.032 0) (radius 0.508)
          (fill (type none))
        )
      )
      (symbol "SW_DPST_x2_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "A")
          (number "1")
        )
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "B")
          (number "2")
        )
      )
      (symbol "SW_DPST_x2_2_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "A")
          (number "3")
        )
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "B")
          (number "4")
        )
      )
    )
  )
  (junction (at 114.935 145.415) (diameter 0) (color 0 0 0 0))
  (junction (at 53.34 54.61) (diameter 0) (color 0 0 0 0))
  (junction (at 34.29 19.05) (diameter 0) (color 0 0 0 0))
  (junction (at 137.16 145.415) (diameter 0) (color 0 0 0 0))
  (junction (at 74.93 145.415) (diameter 0) (color 0 0 0 0))
  (junction (at 155.575 54.61) (diameter 0) (color 0 0 0 0))
  (junction (at 53.34 19.05) (diameter 0) (color 0 0 0 0))
  (junction (at 207.645 54.61) (diameter 0) (color 0 0 0 0))
  (junction (at 160.655 145.415) (diameter 0) (color 0 0 0 0))
  (junction (at 97.155 145.415) (diameter 0) (color 0 0 0 0))
  (junction (at 205.105 54.61) (diameter 0) (color 0 0 0 0))
  (junction (at 114.935 54.61) (diameter 0) (color 0 0 0 0))
  (junction (at 34.29 145.415) (diameter 0) (color 0 0 0 0))
  (junction (at 74.93 66.675) (diameter 0) (color 0 0 0 0))
  (junction (at 137.16 66.675) (diameter 0) (color 0 0 0 0))
  (junction (at 89.535 54.61) (diameter 0) (color 0 0 0 0))
  (junction (at 179.705 54.61) (diameter 0) (color 0 0 0 0))
  (junction (at 97.155 54.61) (diameter 0) (color 0 0 0 0))
  (junction (at 160.655 54.61) (diameter 0) (color 0 0 0 0))
  (junction (at 53.34 145.415) (diameter 0) (color 0 0 0 0))
  (wire (pts (xy 82.55 54.61) (xy 89.535 54.61)))
  (wire (pts (xy 160.655 104.775) (xy 160.655 145.415)))
  (wire (pts (xy 53.34 19.05) (xy 270.51 19.05)))
  (wire (pts (xy 207.645 54.61) (xy 205.105 54.61)))
  (wire (pts (xy 89.535 54.61) (xy 97.155 54.61)))
  (wire (pts (xy 224.155 44.45) (xy 243.205 44.45)))
  (wire (pts (xy 185.42 59.69) (xy 185.42 73.66)))
  (wire (pts (xy 34.29 19.05) (xy 53.34 19.05)))
  (wire (pts (xy 53.34 74.295) (xy 53.34 97.79)))
  (wire (pts (xy 234.95 59.69) (xy 185.42 59.69)))
  (wire (pts (xy 53.34 36.195) (xy 53.34 42.545)))
  (wire (pts (xy 97.155 54.61) (xy 114.935 54.61)))
  (wire (pts (xy 160.655 34.29) (xy 160.655 54.61)))
  (wire (pts (xy 179.705 88.9) (xy 179.705 54.61)))
  (wire (pts (xy 144.78 54.61) (xy 155.575 54.61)))
  (wire (pts (xy 224.155 46.99) (xy 240.03 46.99)))
  (wire (pts (xy 160.655 75.565) (xy 160.655 97.155)))
  (wire (pts (xy 74.93 66.675) (xy 74.93 145.415)))
  (wire (pts (xy 34.29 71.12) (xy 34.29 145.415)))
  (wire (pts (xy 53.34 54.61) (xy 67.31 54.61)))
  (wire (pts (xy 220.345 81.28) (xy 237.49 81.28)))
  (wire (pts (xy 74.93 145.415) (xy 97.155 145.415)))
  (wire (pts (xy 137.16 66.675) (xy 137.16 145.415)))
  (wire (pts (xy 185.42 73.66) (xy 189.865 73.66)))
  (wire (pts (xy 151.765 66.675) (xy 155.575 66.675)))
  (wire (pts (xy 224.155 49.53) (xy 234.95 49.53)))
  (wire (pts (xy 53.34 105.41) (xy 53.34 145.415)))
  (wire (pts (xy 34.29 145.415) (xy 53.34 145.415)))
  (wire (pts (xy 97.155 54.61) (xy 97.155 67.945)))
  (wire (pts (xy 97.155 75.565) (xy 97.155 97.155)))
  (wire (pts (xy 85.725 66.675) (xy 89.535 66.675)))
  (wire (pts (xy 89.535 66.675) (xy 89.535 54.61)))
  (wire (pts (xy 179.705 54.61) (xy 205.105 54.61)))
  (wire (pts (xy 172.085 34.29) (xy 160.655 34.29)))
  (wire (pts (xy 74.93 66.675) (xy 74.93 62.23)))
  (wire (pts (xy 160.655 145.415) (xy 205.105 145.415)))
  (wire (pts (xy 26.67 19.05) (xy 34.29 19.05)))
  (wire (pts (xy 26.67 145.415) (xy 34.29 145.415)))
  (wire (pts (xy 160.655 54.61) (xy 179.705 54.61)))
  (wire (pts (xy 234.95 49.53) (xy 234.95 59.69)))
  (wire (pts (xy 155.575 66.675) (xy 155.575 54.61)))
  (wire (pts (xy 224.155 54.61) (xy 237.49 54.61)))
  (wire (pts (xy 220.345 83.82) (xy 243.205 83.82)))
  (wire (pts (xy 114.935 145.415) (xy 137.16 145.415)))
  (wire (pts (xy 114.935 76.2) (xy 114.935 94.615)))
  (wire (pts (xy 155.575 54.61) (xy 160.655 54.61)))
  (wire (pts (xy 237.49 54.61) (xy 237.49 81.28)))
  (wire (pts (xy 97.155 104.775) (xy 97.155 145.415)))
  (wire (pts (xy 53.34 50.165) (xy 53.34 54.61)))
  (wire (pts (xy 114.935 54.61) (xy 129.54 54.61)))
  (wire (pts (xy 97.155 34.29) (xy 114.3 34.29)))
  (wire (pts (xy 114.935 54.61) (xy 114.935 68.58)))
  (wire (pts (xy 240.03 46.99) (xy 240.03 86.36)))
  (wire (pts (xy 189.865 88.9) (xy 179.705 88.9)))
  (wire (pts (xy 74.93 66.675) (xy 78.105 66.675)))
  (wire (pts (xy 137.16 62.23) (xy 137.16 66.675)))
  (wire (pts (xy 97.155 34.29) (xy 97.155 54.61)))
  (wire (pts (xy 205.105 145.415) (xy 205.105 137.16)))
  (wire (pts (xy 97.155 145.415) (xy 114.935 145.415)))
  (wire (pts (xy 137.16 145.415) (xy 160.655 145.415)))
  (wire (pts (xy 220.345 86.36) (xy 240.03 86.36)))
  (wire (pts (xy 53.34 54.61) (xy 53.34 66.675)))
  (wire (pts (xy 160.655 54.61) (xy 160.655 67.945)))
  (wire (pts (xy 205.105 54.61) (xy 205.105 66.04)))
  (wire (pts (xy 53.34 19.05) (xy 53.34 26.035)))
  (wire (pts (xy 34.29 19.05) (xy 34.29 63.5)))
  (wire (pts (xy 53.34 145.415) (xy 74.93 145.415)))
  (wire (pts (xy 211.455 54.61) (xy 207.645 54.61)))
  (wire (pts (xy 243.205 44.45) (xy 243.205 83.82)))
  (wire (pts (xy 114.935 107.315) (xy 114.935 145.415)))
  (wire (pts (xy 207.645 54.61) (xy 207.645 66.04)))
  (wire (pts (xy 137.16 66.675) (xy 144.145 66.675)))
  (global_label "+24V" (shape input) (at 26.67 19.05 180) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 19.1769 18.9706 0))
  )
  (global_label "V_out_12V" (shape input) (at 114.3 34.29 0) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 126.2683 34.2106 0))
  )
  (global_label "V_out_5V" (shape input) (at 172.085 34.29 0) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 182.8438 34.2106 0))
  )
  (global_label "gnd" (shape input) (at 26.67 145.415 180) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 20.8098 145.3356 0))
  )
  (symbol (lib_id "Device:R") (at 53.34 70.485 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "2200_Ohm" (id 0) (at 56.515 75.565 90))
    (property "Value" "R" (id 1) (at 55.88 71.7549 0))
    (property "Footprint" "" (id 2) (at 51.562 70.485 90))
    (property "Datasheet" "~" (id 3) (at 53.34 70.485 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:LED") (at 97.155 100.965 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "D?" (id 0) (at 90.17 102.5525 0))
    (property "Value" "Kontroll LED 12V" (id 1) (at 100.965 97.79 0))
    (property "Footprint" "" (id 2) (at 97.155 100.965 0))
    (property "Datasheet" "~" (id 3) (at 97.155 100.965 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Connector_Generic:Conn_02x05_Top_Bottom") (at 216.535 49.53 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "Stecker" (id 0) (at 217.805 38.1 0))
    (property "Value" "Codierung" (id 1) (at 217.805 40.64 0))
    (property "Footprint" "" (id 2) (at 216.535 49.53 0))
    (property "Datasheet" "~" (id 3) (at 216.535 49.53 0))
    (pin "1")
    (pin "10")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
  )
  (symbol (lib_id "Motor:Fan") (at 114.935 102.235 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "LM7812CT" (id 0) (at 123.19 97.79 90))
    (property "Value" "Lüfter für" (id 1) (at 120.65 97.79 90))
    (property "Footprint" "" (id 2) (at 114.935 101.981 0))
    (property "Datasheet" "~" (id 3) (at 114.935 101.981 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:Fuse") (at 53.34 46.355 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "F?" (id 0) (at 55.88 45.0849 0))
    (property "Value" "Fuse 2A" (id 1) (at 55.88 46.3549 0))
    (property "Footprint" "" (id 2) (at 51.562 46.355 90))
    (property "Datasheet" "~" (id 3) (at 53.34 46.355 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 114.935 72.39 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "100_Ohm" (id 0) (at 118.745 67.945 90))
    (property "Value" "R" (id 1) (at 117.475 73.6599 0))
    (property "Footprint" "" (id 2) (at 113.157 72.39 90))
    (property "Datasheet" "~" (id 3) (at 114.935 72.39 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Regulator_Linear:LM7805_TO220") (at 137.16 54.61 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U?" (id 0) (at 137.16 46.99 0))
    (property "Value" "LM7805CV_TO220" (id 1) (at 137.16 49.53 0))
    (property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical" (id 2) (at 137.16 48.895 0))
    (property "Datasheet" "https://www.onsemi.cn/PowerSolutions/document/MC7800-D.PDF" (id 3) (at 137.16 55.88 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
  (symbol (lib_id "Device:C") (at 34.29 67.31 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "25V_2200uF" (id 0) (at 39.37 62.23 90))
    (property "Value" "C" (id 1) (at 38.1 68.5799 0))
    (property "Footprint" "" (id 2) (at 35.2552 71.12 0))
    (property "Datasheet" "~" (id 3) (at 34.29 67.31 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Switch:SW_DPST_x2") (at 53.34 31.115 90) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "SW?" (id 0) (at 46.355 31.115 0))
    (property "Value" "Schalter on/off" (id 1) (at 54.61 31.1149 90))
    (property "Footprint" "" (id 2) (at 53.34 31.115 0))
    (property "Datasheet" "~" (id 3) (at 53.34 31.115 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
  )
  (symbol (lib_id "Device:LED") (at 160.655 100.965 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "D?" (id 0) (at 154.305 102.5525 0))
    (property "Value" "Kontroll LED 5V" (id 1) (at 164.465 99.06 0))
    (property "Footprint" "" (id 2) (at 160.655 100.965 0))
    (property "Datasheet" "~" (id 3) (at 160.655 100.965 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:LED") (at 53.34 101.6 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "D?" (id 0) (at 46.355 103.1875 0))
    (property "Value" "Kontroll LED Spannung" (id 1) (at 57.15 95.885 0))
    (property "Footprint" "" (id 2) (at 53.34 101.6 0))
    (property "Datasheet" "~" (id 3) (at 53.34 101.6 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 81.915 66.675 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "25V_33uF" (id 0) (at 77.47 70.485 90))
    (property "Value" "C" (id 1) (at 83.1849 62.865 0))
    (property "Footprint" "" (id 2) (at 85.725 65.7098 0))
    (property "Datasheet" "~" (id 3) (at 81.915 66.675 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 97.155 71.755 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "910_Ohm" (id 0) (at 100.965 76.2 90))
    (property "Value" "R" (id 1) (at 99.695 73.0249 0))
    (property "Footprint" "" (id 2) (at 95.377 71.755 90))
    (property "Datasheet" "~" (id 3) (at 97.155 71.755 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "MCU_Microchip_ATmega:ATmega8A-A") (at 205.105 101.6 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "U?" (id 0) (at 209.6644 63.5 0))
    (property "Value" "ATmega8A-A" (id 1) (at 209.6644 66.04 0))
    (property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm" (id 2) (at 205.105 101.6 0))
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Microchip%208bit%20mcu%20AVR%20ATmega8A%20data%20sheet%2040001974A.pdf" (id 3) (at 205.105 101.6 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "17")
    (pin "18")
    (pin "19")
    (pin "2")
    (pin "20")
    (pin "21")
    (pin "22")
    (pin "23")
    (pin "24")
    (pin "25")
    (pin "26")
    (pin "27")
    (pin "28")
    (pin "29")
    (pin "3")
    (pin "30")
    (pin "31")
    (pin "32")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
  )
  (symbol (lib_id "Device:R") (at 160.655 71.755 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "470_Ohm" (id 0) (at 163.83 76.2 90))
    (property "Value" "R" (id 1) (at 163.195 73.0249 0))
    (property "Footprint" "" (id 2) (at 158.877 71.755 90))
    (property "Datasheet" "~" (id 3) (at 160.655 71.755 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Regulator_Linear:LM7812_TO220") (at 74.93 54.61 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U?" (id 0) (at 74.93 46.99 0))
    (property "Value" "LM7812CT_TO220" (id 1) (at 74.93 49.53 0))
    (property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical" (id 2) (at 74.93 48.895 0))
    (property "Datasheet" "https://www.onsemi.cn/PowerSolutions/document/MC7800-D.PDF" (id 3) (at 74.93 55.88 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
  (symbol (lib_id "Device:C") (at 147.955 66.675 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "25V_33uF" (id 0) (at 143.51 70.485 90))
    (property "Value" "C" (id 1) (at 149.2249 62.865 0))
    (property "Footprint" "" (id 2) (at 151.765 65.7098 0))
    (property "Datasheet" "~" (id 3) (at 147.955 66.675 0))
    (pin "1")
    (pin "2")
  )
  (sheet (at 252.73 105.41) (size 12.7 55.245) (fields_autoplaced)
    (fill (color 0 0 0 0.0000))
    (property "Sheet name" "Untitled Sheet" (id 0) (at 252.73 104.6984 0))
    (property "Sheet file" "untitled.kicad_sch" (id 1) (at 252.73 161.2396 0))
  )
  (sheet_instances
    (path (page "1"))
    (path (page "2"))
  )
  (symbol_instances
    (path
      (reference "25V_33uF") (unit 1) (value "C") (footprint "")
    )
    (path
      (reference "25V_33uF") (unit 1) (value "C") (footprint "")
    )
    (path
      (reference "25V_2200uF") (unit 1) (value "C") (footprint "")
    )
    (path
      (reference "100_Ohm") (unit 1) (value "R") (footprint "")
    )
    (path
      (reference "470_Ohm") (unit 1) (value "R") (footprint "")
    )
    (path
      (reference "910_Ohm") (unit 1) (value "R") (footprint "")
    )
    (path
      (reference "2200_Ohm") (unit 1) (value "R") (footprint "")
    )
    (path
      (reference "D?") (unit 1) (value "Kontroll LED 12V") (footprint "")
    )
    (path
      (reference "D?") (unit 1) (value "Kontroll LED 5V") (footprint "")
    )
    (path
      (reference "D?") (unit 1) (value "Kontroll LED Spannung") (footprint "")
    )
    (path
      (reference "F?") (unit 1) (value "Fuse 2A") (footprint "")
    )
    (path
      (reference "LM7812CT") (unit 1) (value "Lüfter für") (footprint "")
    )
    (path
      (reference "SW?") (unit 1) (value "Schalter on/off") (footprint "")
    )
    (path
      (reference "Stecker") (unit 1) (value "Codierung") (footprint "")
    )
    (path
      (reference "U?") (unit 1) (value "LM7805CV_TO220") (footprint "Package_TO_SOT_THT:TO-220-3_Vertical")
    )
    (path
      (reference "U?") (unit 1) (value "ATmega8A-A") (footprint "Package_QFP:TQFP-32_7x7mm_P0.8mm")
    )
    (path
      (reference "U?") (unit 1) (value "LM7812CT_TO220") (footprint "Package_TO_SOT_THT:TO-220-3_Vertical")
    )
  )
)
