(kicad_sch (version 20211123) (generator eeschema)
  (paper "A4")
  (lib_symbols
    (symbol "74xx:74LS132" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at 0 1.27 0))
      (property "Value" "74LS132" (id 1) (at 0 -1.27 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS132" (id 3) (at 0 0 0))
      (property "ki_locked" "" (id 4) (at 0 0 0))
      (property "ki_keywords" "TTL Nand2" (id 5) (at 0 0 0))
      (property "ki_description" "Quad 2-input NAND Schmitt trigger" (id 6) (at 0 0 0))
      (property "ki_fp_filters" "DIP*W7.62mm*" (id 7) (at 0 0 0))
      (symbol "74LS132_1_0"
        (polyline
          (pts
            (xy -0.635 -1.27)
            (xy -0.635 1.27)
            (xy 0.635 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -0.635 -1.27)
            (xy -0.635 1.27)
            (xy 0.635 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 -1.27)
            (xy 0.635 -1.27)
            (xy 0.635 1.27)
            (xy 1.27 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 -1.27)
            (xy 0.635 -1.27)
            (xy 0.635 1.27)
            (xy 1.27 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "74LS132_1_1"
        (arc (start 0 -3.81) (mid 3.81 0) (end 0 3.81)
          (fill (type background))
        )
        (polyline
          (pts
            (xy 0 3.81)
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 0 -3.81)
          )
          (fill (type background))
        )
        (pin input line (at -7.62 2.54 0) (length 3.81)
          (name "~")
          (number "1")
        )
        (pin input line (at -7.62 -2.54 0) (length 3.81)
          (name "~")
          (number "2")
        )
        (pin output inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "3")
        )
      )
      (symbol "74LS132_1_2"
        (arc (start -3.81 -3.81) (mid -2.589 0) (end -3.81 3.81)
          (fill (type none))
        )
        (arc (start -0.6096 -3.81) (mid 2.1842 -2.5851) (end 3.81 0)
          (fill (type background))
        )
        (polyline
          (pts
            (xy -3.81 -3.81)
            (xy -0.635 -3.81)
          )
          (fill (type background))
        )
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -0.635 3.81)
          )
          (fill (type background))
        )
        (polyline
          (pts
            (xy -0.635 3.81)
            (xy -3.81 3.81)
            (xy -3.81 3.81)
            (xy -3.556 3.4036)
            (xy -3.0226 2.2606)
            (xy -2.6924 1.0414)
            (xy -2.6162 -0.254)
            (xy -2.7686 -1.4986)
            (xy -3.175 -2.7178)
            (xy -3.81 -3.81)
            (xy -3.81 -3.81)
            (xy -0.635 -3.81)
          )
          (fill (type background))
        )
        (arc (start 3.81 0) (mid 2.1915 2.5936) (end -0.6096 3.81)
          (fill (type background))
        )
        (pin input inverted (at -7.62 2.54 0) (length 4.318)
          (name "~")
          (number "1")
        )
        (pin input inverted (at -7.62 -2.54 0) (length 4.318)
          (name "~")
          (number "2")
        )
        (pin output line (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "3")
        )
      )
      (symbol "74LS132_2_0"
        (polyline
          (pts
            (xy -0.635 -1.27)
            (xy -0.635 1.27)
            (xy 0.635 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -0.635 -1.27)
            (xy -0.635 1.27)
            (xy 0.635 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 -1.27)
            (xy 0.635 -1.27)
            (xy 0.635 1.27)
            (xy 1.27 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 -1.27)
            (xy 0.635 -1.27)
            (xy 0.635 1.27)
            (xy 1.27 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "74LS132_2_1"
        (arc (start 0 -3.81) (mid 3.81 0) (end 0 3.81)
          (fill (type background))
        )
        (polyline
          (pts
            (xy 0 3.81)
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 0 -3.81)
          )
          (fill (type background))
        )
        (pin input line (at -7.62 2.54 0) (length 3.81)
          (name "~")
          (number "4")
        )
        (pin input line (at -7.62 -2.54 0) (length 3.81)
          (name "~")
          (number "5")
        )
        (pin output inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "6")
        )
      )
      (symbol "74LS132_2_2"
        (arc (start -3.81 -3.81) (mid -2.589 0) (end -3.81 3.81)
          (fill (type none))
        )
        (arc (start -0.6096 -3.81) (mid 2.1842 -2.5851) (end 3.81 0)
          (fill (type background))
        )
        (polyline
          (pts
            (xy -3.81 -3.81)
            (xy -0.635 -3.81)
          )
          (fill (type background))
        )
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -0.635 3.81)
          )
          (fill (type background))
        )
        (polyline
          (pts
            (xy -0.635 3.81)
            (xy -3.81 3.81)
            (xy -3.81 3.81)
            (xy -3.556 3.4036)
            (xy -3.0226 2.2606)
            (xy -2.6924 1.0414)
            (xy -2.6162 -0.254)
            (xy -2.7686 -1.4986)
            (xy -3.175 -2.7178)
            (xy -3.81 -3.81)
            (xy -3.81 -3.81)
            (xy -0.635 -3.81)
          )
          (fill (type background))
        )
        (arc (start 3.81 0) (mid 2.1915 2.5936) (end -0.6096 3.81)
          (fill (type background))
        )
        (pin input inverted (at -7.62 2.54 0) (length 4.318)
          (name "~")
          (number "4")
        )
        (pin input inverted (at -7.62 -2.54 0) (length 4.318)
          (name "~")
          (number "5")
        )
        (pin output line (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "6")
        )
      )
      (symbol "74LS132_3_0"
        (polyline
          (pts
            (xy -0.635 -1.27)
            (xy -0.635 1.27)
            (xy 0.635 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -0.635 -1.27)
            (xy -0.635 1.27)
            (xy 0.635 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 -1.27)
            (xy 0.635 -1.27)
            (xy 0.635 1.27)
            (xy 1.27 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 -1.27)
            (xy 0.635 -1.27)
            (xy 0.635 1.27)
            (xy 1.27 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "74LS132_3_1"
        (arc (start 0 -3.81) (mid 3.81 0) (end 0 3.81)
          (fill (type background))
        )
        (polyline
          (pts
            (xy 0 3.81)
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 0 -3.81)
          )
          (fill (type background))
        )
        (pin input line (at -7.62 -2.54 0) (length 3.81)
          (name "~")
          (number "10")
        )
        (pin output inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "8")
        )
        (pin input line (at -7.62 2.54 0) (length 3.81)
          (name "~")
          (number "9")
        )
      )
      (symbol "74LS132_3_2"
        (arc (start -3.81 -3.81) (mid -2.589 0) (end -3.81 3.81)
          (fill (type none))
        )
        (arc (start -0.6096 -3.81) (mid 2.1842 -2.5851) (end 3.81 0)
          (fill (type background))
        )
        (polyline
          (pts
            (xy -3.81 -3.81)
            (xy -0.635 -3.81)
          )
          (fill (type background))
        )
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -0.635 3.81)
          )
          (fill (type background))
        )
        (polyline
          (pts
            (xy -0.635 3.81)
            (xy -3.81 3.81)
            (xy -3.81 3.81)
            (xy -3.556 3.4036)
            (xy -3.0226 2.2606)
            (xy -2.6924 1.0414)
            (xy -2.6162 -0.254)
            (xy -2.7686 -1.4986)
            (xy -3.175 -2.7178)
            (xy -3.81 -3.81)
            (xy -3.81 -3.81)
            (xy -0.635 -3.81)
          )
          (fill (type background))
        )
        (arc (start 3.81 0) (mid 2.1915 2.5936) (end -0.6096 3.81)
          (fill (type background))
        )
        (pin input inverted (at -7.62 -2.54 0) (length 4.318)
          (name "~")
          (number "10")
        )
        (pin output line (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "8")
        )
        (pin input inverted (at -7.62 2.54 0) (length 4.318)
          (name "~")
          (number "9")
        )
      )
      (symbol "74LS132_4_0"
        (polyline
          (pts
            (xy -0.635 -1.27)
            (xy -0.635 1.27)
            (xy 0.635 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -0.635 -1.27)
            (xy -0.635 1.27)
            (xy 0.635 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 -1.27)
            (xy 0.635 -1.27)
            (xy 0.635 1.27)
            (xy 1.27 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 -1.27)
            (xy 0.635 -1.27)
            (xy 0.635 1.27)
            (xy 1.27 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "74LS132_4_1"
        (arc (start 0 -3.81) (mid 3.81 0) (end 0 3.81)
          (fill (type background))
        )
        (polyline
          (pts
            (xy 0 3.81)
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 0 -3.81)
          )
          (fill (type background))
        )
        (pin output inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "11")
        )
        (pin input line (at -7.62 2.54 0) (length 3.81)
          (name "~")
          (number "12")
        )
        (pin input line (at -7.62 -2.54 0) (length 3.81)
          (name "~")
          (number "13")
        )
      )
      (symbol "74LS132_4_2"
        (arc (start -3.81 -3.81) (mid -2.589 0) (end -3.81 3.81)
          (fill (type none))
        )
        (arc (start -0.6096 -3.81) (mid 2.1842 -2.5851) (end 3.81 0)
          (fill (type background))
        )
        (polyline
          (pts
            (xy -3.81 -3.81)
            (xy -0.635 -3.81)
          )
          (fill (type background))
        )
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -0.635 3.81)
          )
          (fill (type background))
        )
        (polyline
          (pts
            (xy -0.635 3.81)
            (xy -3.81 3.81)
            (xy -3.81 3.81)
            (xy -3.556 3.4036)
            (xy -3.0226 2.2606)
            (xy -2.6924 1.0414)
            (xy -2.6162 -0.254)
            (xy -2.7686 -1.4986)
            (xy -3.175 -2.7178)
            (xy -3.81 -3.81)
            (xy -3.81 -3.81)
            (xy -0.635 -3.81)
          )
          (fill (type background))
        )
        (arc (start 3.81 0) (mid 2.1915 2.5936) (end -0.6096 3.81)
          (fill (type background))
        )
        (pin output line (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "11")
        )
        (pin input inverted (at -7.62 2.54 0) (length 4.318)
          (name "~")
          (number "12")
        )
        (pin input inverted (at -7.62 -2.54 0) (length 4.318)
          (name "~")
          (number "13")
        )
      )
      (symbol "74LS132_5_0"
        (pin power_in line (at 0 12.7 270) (length 5.08)
          (name "VCC")
          (number "14")
        )
        (pin power_in line (at 0 -12.7 90) (length 5.08)
          (name "GND")
          (number "7")
        )
      )
      (symbol "74LS132_5_1"
        (rectangle (start -5.08 7.62) (end 5.08 -7.62)
          (fill (type background))
        )
      )
    )
    (symbol "Device:C" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.635 2.54 0))
      (property "Value" "C" (id 1) (at 0.635 -2.54 0))
      (property "Footprint" "" (id 2) (at 0.9652 -3.81 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "cap capacitor" (id 4) (at 0 0 0))
      (property "ki_description" "Unpolarized capacitor" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "C_*" (id 6) (at 0 0 0))
      (symbol "C_0_1"
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy 2.032 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762)
          )
          (fill (type none))
        )
      )
      (symbol "C_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 2.794)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:R" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "R" (id 0) (at 2.032 0 90))
      (property "Value" "R" (id 1) (at 0 0 90))
      (property "Footprint" "" (id 2) (at -1.778 0 90))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "R res resistor" (id 4) (at 0 0 0))
      (property "ki_description" "Resistor" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "R_*" (id 6) (at 0 0 0))
      (symbol "R_0_1"
        (rectangle (start -1.016 -2.54) (end 1.016 2.54)
          (fill (type none))
        )
      )
      (symbol "R_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "power:VDD" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -3.81 0))
      (property "Value" "VDD" (id 1) (at 0 3.81 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "global power" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"VDD\"" (id 5) (at 0 0 0))
      (symbol "VDD_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "VDD_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "VDD")
          (number "1")
        )
      )
    )
  )
  (junction (at 113.03 60.96) (diameter 0) (color 0 0 0 0))
  (junction (at 88.9 80.01) (diameter 0) (color 0 0 0 0))
  (junction (at 88.9 58.42) (diameter 0) (color 0 0 0 0))
  (junction (at 63.5 58.42) (diameter 0) (color 0 0 0 0))
  (wire (pts (xy 88.9 78.74) (xy 88.9 80.01)))
  (wire (pts (xy 86.36 80.01) (xy 88.9 80.01)))
  (wire (pts (xy 111.76 67.31) (xy 111.76 77.47)))
  (wire (pts (xy 59.69 80.01) (xy 78.74 80.01)))
  (wire (pts (xy 96.52 63.5) (xy 96.52 67.31)))
  (wire (pts (xy 88.9 80.01) (xy 96.52 80.01)))
  (wire (pts (xy 111.76 60.96) (xy 113.03 60.96)))
  (wire (pts (xy 59.69 58.42) (xy 63.5 58.42)))
  (wire (pts (xy 86.36 58.42) (xy 88.9 58.42)))
  (wire (pts (xy 113.03 60.96) (xy 113.03 69.85)))
  (wire (pts (xy 96.52 67.31) (xy 111.76 67.31)))
  (wire (pts (xy 113.03 60.96) (xy 120.65 60.96)))
  (wire (pts (xy 113.03 69.85) (xy 96.52 69.85)))
  (wire (pts (xy 88.9 57.15) (xy 88.9 58.42)))
  (wire (pts (xy 63.5 58.42) (xy 63.5 60.96)))
  (wire (pts (xy 63.5 55.88) (xy 63.5 58.42)))
  (wire (pts (xy 88.9 58.42) (xy 96.52 58.42)))
  (wire (pts (xy 96.52 69.85) (xy 96.52 74.93)))
  (global_label "L=Aus" (shape input) (at 59.69 80.01 180) (fields_autoplaced)
    (property "Referenzen zwischen Schaltplänen" "${INTERSHEET_REFS}" (id 0) (at 51.4107 79.9306 0))
  )
  (global_label "Ausgang" (shape output) (at 120.65 60.96 0) (fields_autoplaced)
    (property "Referenzen zwischen Schaltplänen" "${INTERSHEET_REFS}" (id 0) (at 130.925 61.0394 0))
  )
  (global_label "H=Ein" (shape input) (at 59.69 58.42 180) (fields_autoplaced)
    (property "Referenzen zwischen Schaltplänen" "${INTERSHEET_REFS}" (id 0) (at 51.4712 58.3406 0))
  )
  (symbol (lib_id "power:VDD") (at 88.9 49.53 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR01" (id 0) (at 88.9 53.34 0))
    (property "Value" "VDD" (id 1) (at 88.9 44.45 0))
    (property "Footprint" "" (id 2) (at 88.9 49.53 0))
    (property "Datasheet" "" (id 3) (at 88.9 49.53 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 88.9 74.93 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R2" (id 0) (at 91.44 73.6599 0))
    (property "Value" "R" (id 1) (at 91.44 76.1999 0))
    (property "Footprint" "" (id 2) (at 87.122 74.93 90))
    (property "Datasheet" "~" (id 3) (at 88.9 74.93 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 82.55 58.42 90) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "C1" (id 0) (at 82.55 50.8 90))
    (property "Value" "C" (id 1) (at 82.55 53.34 90))
    (property "Footprint" "" (id 2) (at 86.36 57.4548 0))
    (property "Datasheet" "~" (id 3) (at 82.55 58.42 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "74xx:74LS132") (at 104.14 60.96 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "U2" (id 0) (at 104.14 52.07 0))
    (property "Value" "74LS132" (id 1) (at 104.14 54.61 0))
    (property "Footprint" "" (id 2) (at 104.14 60.96 0))
    (property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS132" (id 3) (at 104.14 60.96 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "10")
    (pin "8")
    (pin "9")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "7")
  )
  (symbol (lib_id "power:VDD") (at 88.9 71.12 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR02" (id 0) (at 88.9 74.93 0))
    (property "Value" "VDD" (id 1) (at 88.9 66.04 0))
    (property "Footprint" "" (id 2) (at 88.9 71.12 0))
    (property "Datasheet" "" (id 3) (at 88.9 71.12 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 88.9 53.34 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R1" (id 0) (at 91.44 52.0699 0))
    (property "Value" "R" (id 1) (at 91.44 54.6099 0))
    (property "Footprint" "" (id 2) (at 87.122 53.34 90))
    (property "Datasheet" "~" (id 3) (at 88.9 53.34 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 82.55 80.01 90) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "C2" (id 0) (at 82.55 72.39 90))
    (property "Value" "C" (id 1) (at 82.55 74.93 90))
    (property "Footprint" "" (id 2) (at 86.36 79.0448 0))
    (property "Datasheet" "~" (id 3) (at 82.55 80.01 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "74xx:74LS132") (at 71.12 58.42 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "U1" (id 0) (at 71.12 49.53 0))
    (property "Value" "74LS132" (id 1) (at 71.12 52.07 0))
    (property "Footprint" "" (id 2) (at 71.12 58.42 0))
    (property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS132" (id 3) (at 71.12 58.42 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "10")
    (pin "8")
    (pin "9")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "7")
  )
  (symbol (lib_id "74xx:74LS132") (at 104.14 77.47 0) (unit 2)
    (in_bom yes) (on_board yes)
    (property "Reference" "U1" (id 0) (at 102.87 85.09 0))
    (property "Value" "74LS132" (id 1) (at 104.14 87.63 0))
    (property "Footprint" "" (id 2) (at 104.14 77.47 0))
    (property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS132" (id 3) (at 104.14 77.47 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "10")
    (pin "8")
    (pin "9")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "7")
  )
  (sheet_instances
    (path (page "1"))
  )
  (symbol_instances
    (path
      (reference "#PWR01") (unit 1) (value "VDD") (footprint "")
    )
    (path
      (reference "#PWR02") (unit 1) (value "VDD") (footprint "")
    )
    (path
      (reference "C1") (unit 1) (value "C") (footprint "")
    )
    (path
      (reference "C2") (unit 1) (value "C") (footprint "")
    )
    (path
      (reference "R1") (unit 1) (value "R") (footprint "")
    )
    (path
      (reference "R2") (unit 1) (value "R") (footprint "")
    )
    (path
      (reference "U1") (unit 1) (value "74LS132") (footprint "")
    )
    (path
      (reference "U1") (unit 2) (value "74LS132") (footprint "")
    )
    (path
      (reference "U2") (unit 1) (value "74LS132") (footprint "")
    )
  )
)
