(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Panel/")
    )
  )
  (net 0 "")
  (net 1 "Net-(BT1-Pad2)")
  (net 2 "Net-(C2-Pad1)")
  (net 3 "Net-(C1-Pad2)")
  (net 4 "Net-(C6-Pad1)")
  (net 5 "Net-(C7-Pad1)")
  (net 6 "Net-(C8-Pad1)")
  (net 7 "Net-(C9-Pad2)")
  (net 8 "Net-(C10-Pad2)")
  (net 9 "Net-(C12-Pad1)")
  (net 10 "Net-(C14-Pad1)")
  (net 11 "Net-(BT1-Pad1)")
  (net 12 "Net-(C25-Pad1)")
  (net 13 "Net-(C27-Pad1)")
  (net 14 "Net-(C28-Pad2)")
  (net 15 "Net-(C3-Pad1)")
  (net 16 "Net-(D3-Pad1)")
  (net 17 "Net-(D3-Pad2)")
  (net 18 "Net-(D4-Pad2)")
  (net 19 "Net-(D5-Pad2)")
  (net 20 "Net-(D6-Pad1)")
  (net 21 "Net-(D7-Pad2)")
  (net 22 "Net-(D8-Pad1)")
  (net 23 "Net-(F2-Pad1)")
  (net 24 "Net-(F3-Pad1)")
  (net 25 "Net-(J3-Pad1)")
  (net 26 "Net-(J3-Pad3)")
  (net 27 "Net-(J3-Pad4)")
  (net 28 "Net-(J14-Pad13)")
  (net 29 "Net-(J14-Pad14)")
  (net 30 "Net-(J14-Pad15)")
  (net 31 "Net-(J14-Pad16)")
  (net 32 "Net-(J14-Pad17)")
  (net 33 "Net-(J14-Pad19)")
  (net 34 "Net-(J14-Pad20)")
  (net 35 "Net-(J15-Pad1)")
  (net 36 "Net-(J15-Pad3)")
  (net 37 "Net-(J15-Pad4)")
  (net 38 "unconnected-(K1-Pad12)")
  (net 39 "unconnected-(K2-Pad12)")
  (net 40 "Net-(Q1-Pad2)")
  (net 41 "Net-(Q2-Pad2)")
  (net 42 "Net-(Q3-Pad2)")
  (net 43 "Net-(Q4-Pad2)")
  (net 44 "Net-(C11-Pad1)")
  (net 45 "Net-(J4-Pad2)")
  (net 46 "Net-(R8-Pad2)")
  (net 47 "Net-(J4-Pad4)")
  (net 48 "Net-(R18-Pad1)")
  (net 49 "Net-(J5-Pad3)")
  (net 50 "Net-(R20-Pad1)")
  (net 51 "Net-(R21-Pad1)")
  (net 52 "Net-(R22-Pad1)")
  (net 53 "Net-(R24-Pad1)")
  (net 54 "Net-(R25-Pad1)")
  (net 55 "Net-(J4-Pad6)")
  (net 56 "Net-(R26-Pad2)")
  (net 57 "Net-(R27-Pad1)")
  (net 58 "Net-(R27-Pad2)")
  (net 59 "Net-(R28-Pad1)")
  (net 60 "Net-(R29-Pad1)")
  (net 61 "Net-(R30-Pad1)")
  (net 62 "Net-(R31-Pad1)")
  (net 63 "Net-(R32-Pad1)")
  (net 64 "Net-(R33-Pad1)")
  (net 65 "Net-(R34-Pad1)")
  (net 66 "Net-(R35-Pad1)")
  (net 67 "Net-(R37-Pad1)")
  (net 68 "Net-(R38-Pad1)")
  (net 69 "Net-(R39-Pad1)")
  (net 70 "Net-(R41-Pad1)")
  (net 71 "Net-(R42-Pad1)")
  (net 72 "Net-(R43-Pad1)")
  (net 73 "Net-(R44-Pad1)")
  (net 74 "Net-(R45-Pad1)")
  (net 75 "Net-(R46-Pad1)")
  (net 76 "Net-(R47-Pad1)")
  (net 77 "Net-(R48-Pad1)")
  (net 78 "Net-(R49-Pad1)")
  (net 79 "Net-(R50-Pad1)")
  (net 80 "unconnected-(U1-Pad2)")
  (net 81 "unconnected-(U1-Pad3)")
  (net 82 "Net-(U6-Pad1)")
  (net 83 "Net-(U6-Pad2)")
  (net 84 "unconnected-(U6-Pad7)")
  (net 85 "Net-(C20-Pad1)")
  (net 86 "Net-(C31-Pad2)")
  (net 87 "Net-(D11-Pad1)")
  (net 88 "Net-(D11-Pad2)")
  (net 89 "Net-(R53-Pad1)")
  (net 90 "Net-(J12-Pad1)")
  (net 91 "Net-(J12-Pad2)")
  (net 92 "Net-(J12-Pad3)")
  (net 93 "Net-(J12-Pad4)")
  (net 94 "Net-(J12-Pad5)")
  (net 95 "Net-(J12-Pad6)")
  (net 96 "Net-(D12-Pad1)")
  (net 97 "Net-(C36-Pad1)")
  (net 98 "Net-(F4-Pad2)")
  (net 99 "unconnected-(K3-Pad12)")
  (net 100 "Net-(Q5-Pad2)")
  (net 101 "Net-(R52-Pad2)")
  (net 102 "Net-(R16-Pad2)")
  (net 103 "Net-(D9-Pad1)")
  (net 104 "Net-(D15-Pad2)")
  (net 105 "Net-(D16-Pad2)")
  (net 106 "Net-(R14-Pad2)")
  (net 107 "Net-(R24-Pad2)")
  (net 108 "Net-(R28-Pad2)")
  (net 109 "Net-(R31-Pad2)")
  (net 110 "Net-(R34-Pad2)")
  (net 111 "Net-(R38-Pad2)")
  (net 112 "Net-(R41-Pad2)")
  (net 113 "Net-(R54-Pad1)")
  (net 114 "Net-(RV1-Pad2)")
  (net 115 "unconnected-(U5-Pad7)")
  (net 116 "unconnected-(U5-Pad8)")
  (net 117 "unconnected-(U5-Pad9)")
  (net 118 "unconnected-(U5-Pad10)")
  (net 119 "Net-(J14-Pad18)")
  (net 120 "unconnected-(J12-Pad8)")
  (net 121 "Net-(D9-Pad2)")
  (net 122 "Net-(D10-Pad2)")
  (net 123 "unconnected-(J13-Pad8)")
  (net 124 "Net-(D13-Pad1)")
  (net 125 "Net-(J13-Pad6)")
  (net 126 "Net-(J13-Pad5)")
  (net 127 "Net-(J13-Pad4)")
  (net 128 "Net-(J13-Pad3)")
  (net 129 "Net-(J13-Pad2)")
  (net 130 "Net-(J13-Pad1)")
  (net 131 "Net-(D10-Pad1)")
  (net 132 "Net-(J12-Pad10)")
  (net 133 "Net-(D13-Pad2)")
  (net 134 "Net-(R55-Pad1)")
  (net 135 "Net-(J13-Pad9)")
  (footprint "Crystal:Crystal_HC49-4H_Vertical" (layer "F.Cu")
    (tedit 5A1AD3B7)
    (at 25.527 94.887 90)
    (descr "Crystal THT HC-49-4H http://5hertz.com/pdfs/04404_D.pdf")
    (tags "THT crystalHC-49-4H")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Y2" (at 2.44 -3.525 90) (layer "F.SilkS"))
    (fp_text value "Crystal" (at 2.44 3.525 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.44 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(C28-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 4.88 0 90) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(C27-Pad1)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Crystal_HC49-4H_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 44.069 61.722 180)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R33" (at 3.302 0 90) (layer "F.SilkS"))
    (fp_text value "SMD 1/4W 10k" (at 0 2.28) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 180) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 64 "Net-(R33-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 180) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 85 "Net-(C20-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50CD5)
    (at 99.441 55.88 180)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D7" (at 9.652 0.254 90) (layer "F.SilkS"))
    (fp_text value "1N4148" (at 3.81 2.12) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.032 90) (layer "F.SilkS"))
    (fp_text user "K" (at 0 -1.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 4.11 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(D3-Pad2)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(D7-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_THT:OMR B3F-4000" (layer "F.Cu")
    (tedit 5D160D14)
    (at 100.049 157.56)
    (descr "SW PUSH 12mm https://www.e-switch.com/system/asset/product_line/data_sheet/143/TL1100.pdf")
    (tags "tact sw push 12mm")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW3" (at 6.123 -4.525) (layer "F.SilkS"))
    (fp_text value "X10" (at 6.62 9.93) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 2.54) (layer "F.Fab"))
    (pad "1" thru_hole oval (at 12.5 5) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 125 "Net-(J13-Pad6)") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 5) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 125 "Net-(J13-Pad6)") (pinfunction "A") (pintype "passive"))
    (pad "3" thru_hole oval (at 12.5 0) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 128 "Net-(J13-Pad3)") (pinfunction "B") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 0) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 128 "Net-(J13-Pad3)") (pinfunction "B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH-12mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuseholder_Cylinder-5x20mm_Schurter_0031_8201_Horizontal_Open" (layer "F.Cu")
    (tedit 5D717D34)
    (at 154.051 41.021 180)
    (descr "Fuseholder horizontal open, 5x20mm, 500V, 16A, Schurter 0031.8201, https://us.schurter.com/bundles/snceschurter/epim/_ProdPool_/newDS/en/typ_OGN.pdf")
    (tags "Fuseholder horizontal open 5x20 Schurter 0031.8201")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "F3" (at 12.827 -5.969 180) (layer "F.SilkS"))
    (fp_text value "Fuse" (at 11.25 6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 11.25 4) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 11.25 0 180) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 0 0 180) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 24 "Net-(F3-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 22.5 0 180) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 44 "Net-(C11-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Fuse.3dshapes/Fuseholder_Cylinder-5x20mm_Schurter_0031_8201_Horizontal_Open.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 86.741 48.641 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C34" (at -0.127 2.032 -90) (layer "F.SilkS"))
    (fp_text value "100n 25V" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 3 "Net-(C1-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 1 "Net-(BT1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 45.974 55.779 90)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R37" (at 0 -2.413 90) (layer "F.SilkS"))
    (fp_text value "SMD 1/4W 10k" (at 0 2.28 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 90) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 67 "Net-(R37-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 90) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 85 "Net-(C20-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 25.761 100.33 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C28" (at 4.679 0 90) (layer "F.SilkS"))
    (fp_text value " " (at 1.25 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad2)") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(C28-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TerminalBlock_RND:TerminalBlock_RND_205-00001_1x02_P5.00mm_Horizontal" (layer "F.Cu")
    (tedit 5B294F8C)
    (at 165.981 80.986 90)
    (descr "terminal block RND 205-00001, 2 pins, pitch 5mm, size 10x9mm^2, drill diamater 1.3mm, pad diameter 2.5mm, see http://cdn-reichelt.de/documents/datenblatt/C151/RND_205-00001_DB_EN.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_RND")
    (tags "THT terminal block RND 205-00001 pitch 5mm size 10x9mm^2 drill 1.3mm pad 2.5mm")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J9" (at 2.5 -6.06 90) (layer "F.SilkS"))
    (fp_text value "DC 21V Out" (at 2.5 5.06 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 -6.06 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 10 "Net-(C14-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock_RND.3dshapes/TerminalBlock_RND_205-00001_1x02_P5.00mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_Power_L25.0mm_W6.4mm_P30.48mm" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 133.731 81.031 90)
    (descr "Resistor, Axial_Power series, Box, pin pitch=30.48mm, 5W, length*width*height=25*6.4*6.4mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf")
    (tags "Resistor Axial_Power series Box pin pitch 30.48mm 5W length 25mm width 6.4mm height 6.4mm")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R17" (at 15.24 -4.32 90) (layer "F.SilkS"))
    (fp_text value "18R 5W KH208-810B18R" (at 15.24 4.32 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 15.24 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 10 "Net-(C14-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 30.48 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 15 "Net-(C3-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_Power_L25.0mm_W6.4mm_P30.48mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 98.171 72.136 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C7" (at 0 -2.032 90) (layer "F.SilkS"))
    (fp_text value "22u 25V X5R-G1210 22" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 5 "Net-(C7-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 1 "Net-(BT1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 88.891 19.556 90)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D12" (at 0.127 -1.905 270) (layer "F.SilkS"))
    (fp_text value "OSO LYR976 Grün" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 96 "Net-(D12-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 87 "Net-(D11-Pad1)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_Power_L25.0mm_W6.4mm_P30.48mm" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 82.926 88.646)
    (descr "Resistor, Axial_Power series, Box, pin pitch=30.48mm, 5W, length*width*height=25*6.4*6.4mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf")
    (tags "Resistor Axial_Power series Box pin pitch 30.48mm 5W length 25mm width 6.4mm height 6.4mm")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R9" (at -2.281 0 90) (layer "F.SilkS"))
    (fp_text value "2R7 5W AXIAL 2,7" (at 15.24 4.32) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 15.24 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 85 "Net-(C20-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 30.48 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 104 "Net-(D15-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_Power_L25.0mm_W6.4mm_P30.48mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 53.721 112.522)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R24" (at 3.302 0.127 90) (layer "F.SilkS"))
    (fp_text value "SMD 1/4W 1k" (at 0 2.28) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.026 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 53 "Net-(R24-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 107 "Net-(R24-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 54.737 96.52 -90)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R25" (at 0 2.286 90) (layer "F.SilkS"))
    (fp_text value "SMD 1/4W 1k" (at 0 2.28 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -0.019 0.019 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 54 "Net-(R25-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 95 "Net-(J12-Pad6)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 81.661 36.576 180)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R10" (at 3.302 0 90) (layer "F.SilkS"))
    (fp_text value "SMD 1/4W 2k2" (at 0 2.28) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 180) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 41 "Net-(Q2-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 180) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 47 "Net-(J4-Pad4)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50CD5)
    (at 88.773 112.014 180)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D4" (at 9.652 0 90) (layer "F.SilkS"))
    (fp_text value "1N4148" (at 3.81 2.12) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.8) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 4.11 0) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.8) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(D3-Pad2)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(D4-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 29.337 83.058 90)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R51" (at -0.889 2.413 90) (layer "F.SilkS"))
    (fp_text value "SMD 1/4W 10k" (at 0 2.28 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 90) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 85 "Net-(C20-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 90) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 12 "Net-(C25-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_THT:OMR B3F-4000" (layer "F.Cu")
    (tedit 5D160D14)
    (at 127.989 129.62)
    (descr "SW PUSH 12mm https://www.e-switch.com/system/asset/product_line/data_sheet/143/TL1100.pdf")
    (tags "tact sw push 12mm")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW8" (at -3.402 -2.874) (layer "F.SilkS"))
    (fp_text value "Hoch" (at 6.62 9.93) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 2.54) (layer "F.Fab"))
    (pad "1" thru_hole oval (at 12.5 5) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 129 "Net-(J13-Pad2)") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 5) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 129 "Net-(J13-Pad2)") (pinfunction "A") (pintype "passive"))
    (pad "3" thru_hole oval (at 12.5 0) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 127 "Net-(J13-Pad4)") (pinfunction "B") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 0) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 127 "Net-(J13-Pad4)") (pinfunction "B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH-12mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TerminalBlock_RND:TerminalBlock_RND_205-00001_1x02_P5.00mm_Horizontal" (layer "F.Cu")
    (tedit 5B294F8C)
    (at 165.981 93.686 90)
    (descr "terminal block RND 205-00001, 2 pins, pitch 5mm, size 10x9mm^2, drill diamater 1.3mm, pad diameter 2.5mm, see http://cdn-reichelt.de/documents/datenblatt/C151/RND_205-00001_DB_EN.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_RND")
    (tags "THT terminal block RND 205-00001 pitch 5mm size 10x9mm^2 drill 1.3mm pad 2.5mm")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J8" (at 2.5 -6.06 90) (layer "F.SilkS"))
    (fp_text value "DC 21V Out" (at 2.5 5.06 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 -6.06 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 10 "Net-(C14-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock_RND.3dshapes/TerminalBlock_RND_205-00001_1x02_P5.00mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 83.82 25.146 -90)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R13" (at 0 2.413 -90) (layer "F.SilkS"))
    (fp_text value "SMD 1/4W 10k" (at 0 2.28 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 20 "Net-(D6-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 21 "Net-(D7-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-92_Inline" (layer "F.Cu")
    (tedit 5A1DD157)
    (at 89.281 44.196 90)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Q2" (at 1.27 -3.556 270) (layer "F.SilkS"))
    (fp_text value "BC337" (at 1.27 2.79 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 21 "Net-(D7-Pad2)") (pinfunction "C") (pintype "passive"))
    (pad "2" thru_hole oval (at 1.27 0 90) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 41 "Net-(Q2-Pad2)") (pinfunction "B") (pintype "input"))
    (pad "3" thru_hole oval (at 2.54 0 90) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad2)") (pinfunction "E") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_THT:OMR B3F-4000" (layer "F.Cu")
    (tedit 5D160D14)
    (at 138.149 143.59)
    (descr "SW PUSH 12mm https://www.e-switch.com/system/asset/product_line/data_sheet/143/TL1100.pdf")
    (tags "tact sw push 12mm")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW6" (at 6.08 -4.66) (layer "F.SilkS"))
    (fp_text value "Rechts" (at 6.62 9.93) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 2.54) (layer "F.Fab"))
    (pad "1" thru_hole oval (at 12.5 5) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 126 "Net-(J13-Pad5)") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 5) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 126 "Net-(J13-Pad5)") (pinfunction "A") (pintype "passive"))
    (pad "3" thru_hole oval (at 12.5 0) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 128 "Net-(J13-Pad3)") (pinfunction "B") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 0) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 128 "Net-(J13-Pad3)") (pinfunction "B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH-12mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 79 25 -90)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R6" (at 0 2.413 -90) (layer "F.SilkS"))
    (fp_text value "SMD 1/4W 10k" (at 0 2.28 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 16 "Net-(D3-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 18 "Net-(D4-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 156.083 128.27 90)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D9" (at 0 -1.65 90) (layer "F.SilkS"))
    (fp_text value "OSO LYR976 Rot" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 103 "Net-(D9-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 121 "Net-(D9-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 26.543 55.118 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C19" (at 0 -2.032 90) (layer "F.SilkS"))
    (fp_text value "100n 50V KEM X7R1206 1,0U" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 1 "Net-(BT1-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 11 "Net-(BT1-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_QFP:TQFP-44_10x10mm_P0.8mm" (layer "F.Cu")
    (tedit 5A02F146)
    (at 39.516 90.151)
    (descr "44-Lead Plastic Thin Quad Flatpack (PT) - 10x10x1.0 mm Body [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U8" (at -5.48 -7.45) (layer "F.SilkS"))
    (fp_text value "ATmega324A-A (TQFP)" (at 0 7.45) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -5.7 -4) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "Net-(J15-Pad4)") (pinfunction "MOSI_PB5") (pintype "bidirectional"))
    (pad "2" smd rect (at -5.7 -3.2) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "Net-(J15-Pad1)") (pinfunction "MISO_PB6") (pintype "bidirectional"))
    (pad "3" smd rect (at -5.7 -2.4) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "Net-(J15-Pad3)") (pinfunction "SCK_PB7") (pintype "bidirectional"))
    (pad "4" smd rect (at -5.7 -1.6) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "Net-(C25-Pad1)") (pinfunction "~{RESET}") (pintype "input"))
    (pad "5" smd rect (at -5.7 -0.8) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 85 "Net-(C20-Pad1)") (pinfunction "VCC") (pintype "power_in"))
    (pad "6" smd rect (at -5.7 0) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(BT1-Pad2)") (pinfunction "GND") (pintype "power_in"))
    (pad "7" smd rect (at -5.7 0.8) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "Net-(C27-Pad1)") (pinfunction "XTAL2") (pintype "output"))
    (pad "8" smd rect (at -5.7 1.6) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "Net-(C28-Pad2)") (pinfunction "XTAL1") (pintype "input"))
    (pad "9" smd rect (at -5.7 2.4) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 52 "Net-(R22-Pad1)") (pinfunction "PD0") (pintype "bidirectional"))
    (pad "10" smd rect (at -5.7 3.2) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 51 "Net-(R21-Pad1)") (pinfunction "PD1") (pintype "bidirectional"))
    (pad "11" smd rect (at -5.7 4) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "Net-(R26-Pad2)") (pinfunction "INT0_PD2") (pintype "bidirectional"))
    (pad "12" smd rect (at -4 5.7 90) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "Net-(R18-Pad1)") (pinfunction "INT1_PD3") (pintype "bidirectional"))
    (pad "13" smd rect (at -3.2 5.7 90) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "Net-(R31-Pad1)") (pinfunction "OC1B_PD4") (pintype "bidirectional"))
    (pad "14" smd rect (at -2.4 5.7 90) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 65 "Net-(R34-Pad1)") (pinfunction "OC1A_PD5") (pintype "bidirectional"))
    (pad "15" smd rect (at -1.6 5.7 90) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 68 "Net-(R38-Pad1)") (pinfunction "OC2B_PD6") (pintype "bidirectional"))
    (pad "16" smd rect (at -0.8 5.7 90) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "Net-(R41-Pad1)") (pinfunction "OC2A_PD7") (pintype "bidirectional"))
    (pad "17" smd rect (at 0 5.7 90) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 85 "Net-(C20-Pad1)") (pinfunction "VCC") (pintype "passive"))
    (pad "18" smd rect (at 0.8 5.7 90) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(BT1-Pad2)") (pinfunction "GND") (pintype "passive"))
    (pad "19" smd rect (at 1.6 5.7 90) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 71 "Net-(R42-Pad1)") (pinfunction "PC0") (pintype "bidirectional"))
    (pad "20" smd rect (at 2.4 5.7 90) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 69 "Net-(R39-Pad1)") (pinfunction "PC1") (pintype "bidirectional"))
    (pad "21" smd rect (at 3.2 5.7 90) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 66 "Net-(R35-Pad1)") (pinfunction "PC2") (pintype "bidirectional"))
    (pad "22" smd rect (at 4 5.7 90) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "Net-(R32-Pad1)") (pinfunction "PC3") (pintype "bidirectional"))
    (pad "23" smd rect (at 5.7 4) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "Net-(R29-Pad1)") (pinfunction "PC4") (pintype "bidirectional"))
    (pad "24" smd rect (at 5.7 3.2) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 54 "Net-(R25-Pad1)") (pinfunction "PC5") (pintype "bidirectional"))
    (pad "25" smd rect (at 5.7 2.4) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 134 "Net-(R55-Pad1)") (pinfunction "PC6") (pintype "bidirectional"))
    (pad "26" smd rect (at 5.7 1.6) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 50 "Net-(R20-Pad1)") (pinfunction "PC7") (pintype "bidirectional"))
    (pad "27" smd rect (at 5.7 0.8) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 85 "Net-(C20-Pad1)") (pinfunction "AVCC") (pintype "power_in"))
    (pad "28" smd rect (at 5.7 0) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(BT1-Pad2)") (pinfunction "GND") (pintype "passive"))
    (pad "29" smd rect (at 5.7 -0.8) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 101 "Net-(R52-Pad2)") (pinfunction "AREF") (pintype "passive"))
    (pad "30" smd rect (at 5.7 -1.6) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 58 "Net-(R27-Pad2)") (pinfunction "PA7") (pintype "bidirectional"))
    (pad "31" smd rect (at 5.7 -2.4) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 77 "Net-(R48-Pad1)") (pinfunction "PA6") (pintype "bidirectional"))
    (pad "32" smd rect (at 5.7 -3.2) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 78 "Net-(R49-Pad1)") (pinfunction "PA5") (pintype "bidirectional"))
    (pad "33" smd rect (at 5.7 -4) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 79 "Net-(R50-Pad1)") (pinfunction "PA4") (pintype "bidirectional"))
    (pad "34" smd rect (at 4 -5.7 90) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 72 "Net-(R43-Pad1)") (pinfunction "PA3") (pintype "bidirectional"))
    (pad "35" smd rect (at 3.2 -5.7 90) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 73 "Net-(R44-Pad1)") (pinfunction "PA2") (pintype "bidirectional"))
    (pad "36" smd rect (at 2.4 -5.7 90) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 74 "Net-(R45-Pad1)") (pinfunction "PA1") (pintype "bidirectional"))
    (pad "37" smd rect (at 1.6 -5.7 90) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 75 "Net-(R46-Pad1)") (pinfunction "PA0") (pintype "bidirectional"))
    (pad "38" smd rect (at 0.8 -5.7 90) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 85 "Net-(C20-Pad1)") (pinfunction "VCC") (pintype "passive"))
    (pad "39" smd rect (at 0 -5.7 90) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(BT1-Pad2)") (pinfunction "GND") (pintype "passive"))
    (pad "40" smd rect (at -0.8 -5.7 90) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "Net-(R30-Pad1)") (pinfunction "PB0") (pintype "bidirectional"))
    (pad "41" smd rect (at -1.6 -5.7 90) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 67 "Net-(R37-Pad1)") (pinfunction "PB1") (pintype "bidirectional"))
    (pad "42" smd rect (at -2.4 -5.7 90) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 53 "Net-(R24-Pad1)") (pinfunction "INT2_PB2") (pintype "bidirectional"))
    (pad "43" smd rect (at -3.2 -5.7 90) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 76 "Net-(R47-Pad1)") (pinfunction "OC0A_PB3") (pintype "bidirectional"))
    (pad "44" smd rect (at -4 -5.7 90) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 59 "Net-(R28-Pad1)") (pinfunction "OC0B_PB4") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Package_QFP.3dshapes/TQFP-44_10x10mm_P0.8mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 50.038 89.916 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C30" (at 0 -1.85 90) (layer "F.SilkS"))
    (fp_text value "100n 50V KEM X7R1206 1,0U" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 85 "Net-(C20-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 1 "Net-(BT1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 39.0275 79.991 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C24" (at 0 -2.051) (layer "F.SilkS"))
    (fp_text value "100n 50V KEM X7R1206 1,0U" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 180) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 85 "Net-(C20-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 180) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 1 "Net-(BT1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 79 19.556 90)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D3" (at -0.127 -1.905 270) (layer "F.SilkS"))
    (fp_text value "OSO LYR976 Grün" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 16 "Net-(D3-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 17 "Net-(D3-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D12.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF1)
    (at 150.241 101.129959 90)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=12.5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 12.5mm Electrolytic Capacitor")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C14" (at 2.5 -7.5 90) (layer "F.SilkS"))
    (fp_text value "ELKO 680/35 FK 1500/35 AM" (at 2.5 7.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 10 "Net-(C14-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D12.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 63.881 96.901 90)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R53" (at 0 2.667 90) (layer "F.SilkS"))
    (fp_text value "SMD 1/4W Variabel" (at 0 2.28 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 90) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 89 "Net-(R53-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 90) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 85 "Net-(C20-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 83.891 19.556 90)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D6" (at 0.127 -1.905 270) (layer "F.SilkS"))
    (fp_text value "OSO LYR976 Grün" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 20 "Net-(D6-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 17 "Net-(D3-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 29.972 107.95 90)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R26" (at -4.191 0.508 90) (layer "F.SilkS"))
    (fp_text value "SMD 1/4W 1k" (at 0 2.28 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 90) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 55 "Net-(J4-Pad6)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 90) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 56 "Net-(R26-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 113.8835 64.516 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C3" (at 0 1.9965 90) (layer "F.SilkS"))
    (fp_text value "10u 50V KEM X5R1210 10U" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 15 "Net-(C3-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 1 "Net-(BT1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 54.488 33.005 180)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J4" (at 5.085 2.779 90) (layer "F.SilkS"))
    (fp_text value "Humper Programmieren" (at 5.085 2.525 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 1.89 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J3-Pad3)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "Net-(J4-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J3-Pad1)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(J4-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J3-Pad4)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 "Net-(J4-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 88.773 25.146 -90)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R15" (at 0 2.413 -90) (layer "F.SilkS"))
    (fp_text value "SMD 1/4W 10k" (at 0 2.28 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 96 "Net-(D12-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 88 "Net-(D11-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 49.149 42.672 90)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R20" (at 0 2.54 90) (layer "F.SilkS"))
    (fp_text value "SMD 1/4W 1k" (at 0 2.28 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 90) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 50 "Net-(R20-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 90) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 43 "Net-(Q4-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 66.675 54.636 90)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R7" (at -1.498 -2.54 90) (layer "F.SilkS"))
    (fp_text value "SMD 1/4W 2k2" (at 0 2.28 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 90) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 40 "Net-(Q1-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 90) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 45 "Net-(J4-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TerminalBlock_RND:TerminalBlock_RND_205-00001_1x02_P5.00mm_Horizontal" (layer "F.Cu")
    (tedit 5B294F8C)
    (at 165.981 106.386 90)
    (descr "terminal block RND 205-00001, 2 pins, pitch 5mm, size 10x9mm^2, drill diamater 1.3mm, pad diameter 2.5mm, see http://cdn-reichelt.de/documents/datenblatt/C151/RND_205-00001_DB_EN.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_RND")
    (tags "THT terminal block RND 205-00001 pitch 5mm size 10x9mm^2 drill 1.3mm pad 2.5mm")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J7" (at 2.5 -6.06 90) (layer "F.SilkS"))
    (fp_text value "DC 21V Out" (at 2.5 5.06 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 -6.06 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 10 "Net-(C14-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock_RND.3dshapes/TerminalBlock_RND_205-00001_1x02_P5.00mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 86.741 54.991 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C11" (at 0.127 -2.032 270) (layer "F.SilkS"))
    (fp_text value "330n 50V" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 44 "Net-(C11-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 1 "Net-(BT1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 73.787 72.136 90)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "F1" (at 3.81 -2.667 90) (layer "F.SilkS"))
    (fp_text value "Fuse" (at 6.35 2.72 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(D3-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(C3-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector:FanPinHeader_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19DCDF)
    (at 37.891 19.691)
    (descr "3-pin CPU fan Through hole pin header, see http://www.formfactors.org/developer%5Cspecs%5Crev1_2_public.pdf")
    (tags "pin header 3-pin CPU fan")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J5" (at -2.712 -1.911 90) (layer "F.SilkS"))
    (fp_text value "Fan" (at 2.55 4.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.45 1.8) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 9 "Net-(C12-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 5.08 0 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 49 "Net-(J5-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector.3dshapes/FanPinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 68.834 25.1206 -90)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R56" (at 0.0254 2.3876 -90) (layer "F.SilkS"))
    (fp_text value "SMD 1/4W 2k2" (at 0 2.28 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 124 "Net-(D13-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 1 "Net-(BT1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_IDC:IDC-Header_2x05_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5EAC9A07)
    (at 129.154 121.965 90)
    (descr "Through hole IDC box header, 2x05, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0")
    (tags "Through hole vertical IDC box header THT 2x05 2.54mm double row")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J13" (at 1.27 -6.1 90) (layer "F.SilkS"))
    (fp_text value "In Tastenfeld" (at 1.27 16.26 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 5.08 180) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.1470588235)
      (net 130 "Net-(J13-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 129 "Net-(J13-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 128 "Net-(J13-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 127 "Net-(J13-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole circle (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 126 "Net-(J13-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 125 "Net-(J13-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole circle (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 121 "Net-(D9-Pad2)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole circle (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 123 "unconnected-(J13-Pad8)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole circle (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 135 "Net-(J13-Pad9)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole circle (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 122 "Net-(D10-Pad2)") (pinfunction "Pin_10") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_IDC.3dshapes/IDC-Header_2x05_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 48.133 101.6 -90)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R35" (at 0 -2.28 90) (layer "F.SilkS"))
    (fp_text value "SMD 1/4W 1k" (at 0 2.28 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 66 "Net-(R35-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 92 "Net-(J12-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-220-3_Vertical" (layer "F.Cu")
    (tedit 5AC8BA0D)
    (at 103.576 65.786 -90)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U3" (at 2.54 2.357 90) (layer "F.SilkS"))
    (fp_text value "LM78M05_TO220" (at 2.54 2.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -4.27 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 15 "Net-(C3-Pad1)") (pinfunction "VI") (pintype "power_in"))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad2)") (pinfunction "GND") (pintype "power_in"))
    (pad "3" thru_hole oval (at 5.08 0 270) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 "Net-(C7-Pad1)") (pinfunction "VO") (pintype "power_out"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 75.311 32.131 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C10" (at -3.175 0 180) (layer "F.SilkS"))
    (fp_text value "1µ 50V KEM X7R1206 1,0U" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 1 "Net-(BT1-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 8 "Net-(C10-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_IDC:IDC-Header_2x05_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5EAC9A07)
    (at 37.211 160.8995 90)
    (descr "Through hole IDC box header, 2x05, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0")
    (tags "Through hole vertical IDC box header THT 2x05 2.54mm double row")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J12" (at 1.2605 -6.604 90) (layer "F.SilkS"))
    (fp_text value "Out Tastenfeld" (at 1.27 16.26 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 5.08) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.1470588235)
      (net 90 "Net-(J12-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 91 "Net-(J12-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 92 "Net-(J12-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 93 "Net-(J12-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole circle (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 94 "Net-(J12-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 95 "Net-(J12-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole circle (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 133 "Net-(D13-Pad2)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole circle (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 120 "unconnected-(J12-Pad8)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole circle (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad2)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole circle (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 132 "Net-(J12-Pad10)") (pinfunction "Pin_10") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_IDC.3dshapes/IDC-Header_2x05_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuseholder_Cylinder-5x20mm_Schurter_0031_8201_Horizontal_Open" (layer "F.Cu")
    (tedit 5D717D34)
    (at 154.051 28.956 180)
    (descr "Fuseholder horizontal open, 5x20mm, 500V, 16A, Schurter 0031.8201, https://us.schurter.com/bundles/snceschurter/epim/_ProdPool_/newDS/en/typ_OGN.pdf")
    (tags "Fuseholder horizontal open 5x20 Schurter 0031.8201")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "F2" (at 12.573 5.842 180) (layer "F.SilkS"))
    (fp_text value "Fuse" (at 11.25 6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 11.25 4) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 11.25 0 180) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 0 0 180) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 23 "Net-(F2-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 22.5 0 180) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 44 "Net-(C11-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Fuse.3dshapes/Fuseholder_Cylinder-5x20mm_Schurter_0031_8201_Horizontal_Open.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 52.451 151.892)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R60" (at -3.556 -0.127 90) (layer "F.SilkS"))
    (fp_text value "SMD 1/4W 2k2" (at 4.064 0.762) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 132 "Net-(J12-Pad10)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 85 "Net-(C20-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 60.071 34.671 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at 1.524 2.413 90) (layer "F.SilkS"))
    (fp_text value "100n 50V KEM X7R1206 1,0U" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 180) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 2 "Net-(C2-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 180) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 1 "Net-(BT1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_THT:OMR B3F-4000" (layer "F.Cu")
    (tedit 5D160D14)
    (at 100.049 143.59)
    (descr "SW PUSH 12mm https://www.e-switch.com/system/asset/product_line/data_sheet/143/TL1100.pdf")
    (tags "tact sw push 12mm")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW2" (at 6.08 -4.525) (layer "F.SilkS"))
    (fp_text value "Start" (at 6.62 9.93) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 2.54) (layer "F.Fab"))
    (pad "1" thru_hole oval (at 12.5 5) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 125 "Net-(J13-Pad6)") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 5) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 125 "Net-(J13-Pad6)") (pinfunction "A") (pintype "passive"))
    (pad "3" thru_hole oval (at 12.5 0) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 129 "Net-(J13-Pad2)") (pinfunction "B") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 0) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 129 "Net-(J13-Pad2)") (pinfunction "B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH-12mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Display:RC1602A Ohne Seitenpads" (layer "F.Cu")
    (tedit 5A02FE80)
    (at 59.309 106.222 -90)
    (descr "http://www.raystar-optronics.com/down.php?ProID=18")
    (tags "LCD 16x2 Alphanumeric 16pin")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U5" (at -38.53 -3.41 90) (layer "F.SilkS"))
    (fp_text value "LCD-PM 2X16-6 E" (at -37.22 43.58 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.185 21.705 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 40.72 38 90) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -36.78 2 90) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -38.28 38 90) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 39.22 2 90) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad2)") (pinfunction "VSS") (pintype "power_in"))
    (pad "2" thru_hole oval (at 2.54 0 90) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 85 "Net-(C20-Pad1)") (pinfunction "VDD") (pintype "power_in"))
    (pad "3" thru_hole oval (at 5.08 0 90) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 114 "Net-(RV1-Pad2)") (pinfunction "VO") (pintype "power_in"))
    (pad "4" thru_hole oval (at 7.62 0 90) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 107 "Net-(R24-Pad2)") (pinfunction "RS") (pintype "input"))
    (pad "5" thru_hole oval (at 10.16 0 90) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 108 "Net-(R28-Pad2)") (pinfunction "R/W") (pintype "input"))
    (pad "6" thru_hole oval (at 12.7 0 90) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 106 "Net-(R14-Pad2)") (pinfunction "E") (pintype "input"))
    (pad "7" thru_hole oval (at 15.24 0 90) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 115 "unconnected-(U5-Pad7)") (pinfunction "DB0") (pintype "bidirectional"))
    (pad "8" thru_hole oval (at 17.78 0 90) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 116 "unconnected-(U5-Pad8)") (pinfunction "DB1") (pintype "bidirectional"))
    (pad "9" thru_hole oval (at 20.32 0 90) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 117 "unconnected-(U5-Pad9)") (pinfunction "DB2") (pintype "bidirectional"))
    (pad "10" thru_hole oval (at 22.86 0 90) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 118 "unconnected-(U5-Pad10)") (pinfunction "DB3") (pintype "bidirectional"))
    (pad "11" thru_hole oval (at 25.4 0 90) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 109 "Net-(R31-Pad2)") (pinfunction "DB4") (pintype "bidirectional"))
    (pad "12" thru_hole oval (at 27.94 0 90) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 110 "Net-(R34-Pad2)") (pinfunction "DB5") (pintype "bidirectional"))
    (pad "13" thru_hole oval (at 30.48508 0.00254 90) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 111 "Net-(R38-Pad2)") (pinfunction "DB6") (pintype "bidirectional"))
    (pad "14" thru_hole oval (at 33.02 0 90) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 112 "Net-(R41-Pad2)") (pinfunction "DB7") (pintype "bidirectional"))
    (pad "15" thru_hole oval (at -5.08 0 90) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 113 "Net-(R54-Pad1)") (pinfunction "A/VEE") (pintype "power_in"))
    (pad "16" thru_hole oval (at -2.53492 0.00254 90) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad2)") (pinfunction "K") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Display.3dshapes/RC1602A.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 36.703 101.473 -90)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R38" (at -3.175 -0.127 180) (layer "F.SilkS"))
    (fp_text value "SMD 1/4W 1k" (at 0 2.28 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 68 "Net-(R38-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 111 "Net-(R38-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 74 25 -90)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R8" (at 0 2.413 -90) (layer "F.SilkS"))
    (fp_text value "SMD 1/4W 10k" (at 0 2.28 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 19 "Net-(D5-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 46 "Net-(R8-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 45.339 80.518)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R44" (at 0 2.3368 180) (layer "F.SilkS"))
    (fp_text value "SMD 1/4W 1k" (at 0 2.28) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 73 "Net-(R44-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 32 "Net-(J14-Pad17)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 42.056 107.931 -90)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R42" (at 4.083 0.146 90) (layer "F.SilkS"))
    (fp_text value "SMD 1/4W 1k" (at 0 2.28 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 71 "Net-(R42-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 90 "Net-(J12-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_THT:OMR B3F-4000" (layer "F.Cu")
    (tedit 5D160D14)
    (at 117.829 143.59)
    (descr "SW PUSH 12mm https://www.e-switch.com/system/asset/product_line/data_sheet/143/TL1100.pdf")
    (tags "tact sw push 12mm")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW5" (at 6.08 -4.66) (layer "F.SilkS"))
    (fp_text value "Links" (at 6.62 9.93) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 2.54) (layer "F.Fab"))
    (pad "1" thru_hole oval (at 12.5 5) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 126 "Net-(J13-Pad5)") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 5) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 126 "Net-(J13-Pad5)") (pinfunction "A") (pintype "passive"))
    (pad "3" thru_hole oval (at 12.5 0) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 129 "Net-(J13-Pad2)") (pinfunction "B") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 0) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 129 "Net-(J13-Pad2)") (pinfunction "B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH-12mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 59.563 96.901 90)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R54" (at 0.254 -2.286 90) (layer "F.SilkS"))
    (fp_text value "SMD 1/4W 6R3" (at 0 2.28 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 90) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 113 "Net-(R54-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 90) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 89 "Net-(R53-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 49.149 96.52)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R32" (at 0 -2.28) (layer "F.SilkS"))
    (fp_text value "SMD 1/4W 1k" (at 0 2.28) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 63 "Net-(R32-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 93 "Net-(J12-Pad4)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 44.069 75.692 90)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R45" (at 0 2.413 90) (layer "F.SilkS"))
    (fp_text value "SMD 1/4W 1k" (at 0 2.28 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 90) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 74 "Net-(R45-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 90) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 30 "Net-(J14-Pad15)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 57.404 78.994 180)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R27" (at -0.0508 2.2352 180) (layer "F.SilkS"))
    (fp_text value "SMD 1/4W 1k" (at 0 2.28) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 180) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 57 "Net-(R27-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 180) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 58 "Net-(R27-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D12.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF1)
    (at 150.241 59.219959 90)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=12.5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 12.5mm Electrolytic Capacitor")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C17" (at 2.5 -7.5 90) (layer "F.SilkS"))
    (fp_text value "ELKO 680/35 RAD FC 680/35" (at 2.5 7.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 10 "Net-(C14-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D12.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 23.261 84.328)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C27" (at -2.306 -0.127 90) (layer "F.SilkS"))
    (fp_text value " " (at 1.25 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(C27-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D12.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF1)
    (at 150.241 87.159959 90)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=12.5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 12.5mm Electrolytic Capacitor")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C15" (at 2.5 -7.5 90) (layer "F.SilkS"))
    (fp_text value "ELKO 680/35 FK 1500/35 AM" (at 2.5 7.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 10 "Net-(C14-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D12.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 33.909 107.931 -90)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R34" (at 4.1846 0.0254 90) (layer "F.SilkS"))
    (fp_text value "SMD 1/4W 1k" (at 0 2.28 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.28 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 65 "Net-(R34-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 110 "Net-(R34-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 51.308 84.582)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R48" (at -3.0988 -0.1016 90) (layer "F.SilkS"))
    (fp_text value "SMD 1/4W 1k" (at 0 2.28) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 77 "Net-(R48-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 29 "Net-(J14-Pad14)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_1.27mm:PinHeader_2x03_P1.27mm_Vertical_SMD" (layer "F.Cu")
    (tedit 59FED6E3)
    (at 21.844 60.706)
    (descr "surface-mounted straight pin header, 2x03, 1.27mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x03 1.27mm double row")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J15" (at -5.08 -0.381 90) (layer "F.SilkS"))
    (fp_text value "ISP" (at 0 2.965) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.95 -1.27) (size 2.4 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "Net-(J15-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd rect (at 1.95 -1.27) (size 2.4 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 85 "Net-(C20-Pad1)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd rect (at -1.95 0) (size 2.4 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "Net-(J15-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd rect (at 1.95 0) (size 2.4 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "Net-(J15-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" smd rect (at -1.95 1.27) (size 2.4 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "Net-(C25-Pad1)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" smd rect (at 1.95 1.27) (size 2.4 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(BT1-Pad2)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x03_P1.27mm_Vertical_SMD.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TerminalBlock_RND:TerminalBlock_RND_205-00001_1x02_P5.00mm_Horizontal" (layer "F.Cu")
    (tedit 5B294F8C)
    (at 165.981 42.056 90)
    (descr "terminal block RND 205-00001, 2 pins, pitch 5mm, size 10x9mm^2, drill diamater 1.3mm, pad diameter 2.5mm, see http://cdn-reichelt.de/documents/datenblatt/C151/RND_205-00001_DB_EN.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_RND")
    (tags "THT terminal block RND 205-00001 pitch 5mm size 10x9mm^2 drill 1.3mm pad 2.5mm")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 2.5 -6.06 90) (layer "F.SilkS"))
    (fp_text value "DC 21V 2" (at 2.5 5.06 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 -6.06 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 24 "Net-(F3-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock_RND.3dshapes/TerminalBlock_RND_205-00001_1x02_P5.00mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 160.655 133.35 -90)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R40" (at 0 2.159 90) (layer "F.SilkS"))
    (fp_text value "SMD 1/4W 2k2" (at 0 2.28 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 131 "Net-(D10-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 135 "Net-(J13-Pad9)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-92_Inline" (layer "F.Cu")
    (tedit 5A1DD157)
    (at 80.666 51.181 -90)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U9" (at 1.143 2.815 -90) (layer "F.SilkS"))
    (fp_text value "LM78L05_TO92" (at 1.27 2.79 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 "Net-(C1-Pad2)") (pinfunction "VO") (pintype "power_out"))
    (pad "2" thru_hole oval (at 1.27 0 270) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad2)") (pinfunction "GND") (pintype "power_in"))
    (pad "3" thru_hole oval (at 2.54 0 270) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 44 "Net-(C11-Pad1)") (pinfunction "VI") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 53.467 89.916 90)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R52" (at 3.048 0.254 180) (layer "F.SilkS"))
    (fp_text value "100R 0W25 SMD 1/4W 100" (at 0 2.28 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 90) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 85 "Net-(C20-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 90) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 101 "Net-(R52-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D8.0mm_P3.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 86.995 139.066651 90)
    (descr "CP, Radial series, Radial, pin pitch=3.50mm, , diameter=8mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 3.50mm  diameter 8mm Electrolytic Capacitor")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C23" (at 2.160651 -5.461 270) (layer "F.SilkS"))
    (fp_text value "470U 10V RAD FC 470/10" (at 1.652651 5.334 270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.75 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 85 "Net-(C20-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 3.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D8.0mm_P3.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 50.419 53.086)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C32" (at -3.556 -1.524 90) (layer "F.SilkS"))
    (fp_text value "100n 50V KEM X7R1206 1,0U" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 1 "Net-(BT1-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 85 "Net-(C20-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TerminalBlock_RND:TerminalBlock_RND_205-00001_1x02_P5.00mm_Horizontal" (layer "F.Cu")
    (tedit 5B294F8C)
    (at 165.981 68.286 90)
    (descr "terminal block RND 205-00001, 2 pins, pitch 5mm, size 10x9mm^2, drill diamater 1.3mm, pad diameter 2.5mm, see http://cdn-reichelt.de/documents/datenblatt/C151/RND_205-00001_DB_EN.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_RND")
    (tags "THT terminal block RND 205-00001 pitch 5mm size 10x9mm^2 drill 1.3mm pad 2.5mm")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J10" (at 2.5 -6.06 90) (layer "F.SilkS"))
    (fp_text value "DC 21V Out" (at 2.5 5.06 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 -6.06 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 10 "Net-(C14-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock_RND.3dshapes/TerminalBlock_RND_205-00001_1x02_P5.00mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-220-3_Vertical" (layer "F.Cu")
    (tedit 5AC8BA0D)
    (at 119.2885 65.786 -90)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U2" (at 2.54 2.3215 90) (layer "F.SilkS"))
    (fp_text value "LM78M05_TO220" (at 2.54 2.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -4.27 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 15 "Net-(C3-Pad1)") (pinfunction "VI") (pintype "power_in"))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad2)") (pinfunction "GND") (pintype "power_in"))
    (pad "3" thru_hole oval (at 5.08 0 270) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 "Net-(C6-Pad1)") (pinfunction "VO") (pintype "power_out"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 96.901 18.796)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "F5" (at 3.81 -2.667) (layer "F.SilkS"))
    (fp_text value "Fuse" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 87 "Net-(D11-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "Net-(C11-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_1.27mm:PinHeader_2x03_P1.27mm_Vertical_SMD" (layer "F.Cu")
    (tedit 59FED6E3)
    (at 57.023 20.701 -90)
    (descr "surface-mounted straight pin header, 2x03, 1.27mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x03 1.27mm double row")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J3" (at 3.683 3.302 90) (layer "F.SilkS"))
    (fp_text value "ISP" (at 0 2.965 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -1.95 -1.27 270) (size 2.4 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "Net-(J3-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd rect (at 1.95 -1.27 270) (size 2.4 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(C1-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd rect (at -1.95 0 270) (size 2.4 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "Net-(J3-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd rect (at 1.95 0 270) (size 2.4 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "Net-(J3-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" smd rect (at -1.95 1.27 270) (size 2.4 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(C9-Pad2)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" smd rect (at 1.95 1.27 270) (size 2.4 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(BT1-Pad2)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x03_P1.27mm_Vertical_SMD.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_THT:OMR B3F-4000" (layer "F.Cu")
    (tedit 5D160D14)
    (at 100.049 129.62)
    (descr "SW PUSH 12mm https://www.e-switch.com/system/asset/product_line/data_sheet/143/TL1100.pdf")
    (tags "tact sw push 12mm")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW1" (at 6.08 -4.66) (layer "F.SilkS"))
    (fp_text value "Stop" (at 6.62 9.93) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 2.54) (layer "F.Fab"))
    (pad "1" thru_hole oval (at 12.5 5) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 125 "Net-(J13-Pad6)") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 5) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 125 "Net-(J13-Pad6)") (pinfunction "A") (pintype "passive"))
    (pad "3" thru_hole oval (at 12.5 0) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 130 "Net-(J13-Pad1)") (pinfunction "B") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 0) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 130 "Net-(J13-Pad1)") (pinfunction "B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH-12mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 160.655 128.27 90)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D10" (at 0 -1.65 90) (layer "F.SilkS"))
    (fp_text value "OSO LYR976 Rot" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 131 "Net-(D10-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 122 "Net-(D10-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-92_Inline" (layer "F.Cu")
    (tedit 5A1DD157)
    (at 81.259 105.918 90)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Q1" (at 1.27 -3.56 90) (layer "F.SilkS"))
    (fp_text value "BC337" (at 1.27 2.79 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 18 "Net-(D4-Pad2)") (pinfunction "C") (pintype "passive"))
    (pad "2" thru_hole oval (at 1.27 0 90) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 40 "Net-(Q1-Pad2)") (pinfunction "B") (pintype "input"))
    (pad "3" thru_hole oval (at 2.54 0 90) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad2)") (pinfunction "E") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TerminalBlock_RND:TerminalBlock_RND_205-00001_1x02_P5.00mm_Horizontal" (layer "F.Cu")
    (tedit 5B294F8C)
    (at 165.981 55.586 90)
    (descr "terminal block RND 205-00001, 2 pins, pitch 5mm, size 10x9mm^2, drill diamater 1.3mm, pad diameter 2.5mm, see http://cdn-reichelt.de/documents/datenblatt/C151/RND_205-00001_DB_EN.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_RND")
    (tags "THT terminal block RND 205-00001 pitch 5mm size 10x9mm^2 drill 1.3mm pad 2.5mm")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J11" (at 2.5 -6.06 90) (layer "F.SilkS"))
    (fp_text value "DC 21V Out" (at 2.5 5.06 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 -6.06 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 10 "Net-(C14-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock_RND.3dshapes/TerminalBlock_RND_205-00001_1x02_P5.00mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 113.8835 72.136 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C6" (at 0 -1.85 90) (layer "F.SilkS"))
    (fp_text value "22u 25V X5R-G1210 22" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 4 "Net-(C6-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 1 "Net-(BT1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:CP_Elec_6.3x7.7" (layer "F.Cu")
    (tedit 5BCA39D0)
    (at 60.071 51.308 180)
    (descr "SMD capacitor, aluminum electrolytic, Nichicon, 6.3x7.7mm")
    (tags "capacitor electrolytic")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C20" (at 4.826 2.794 90) (layer "F.SilkS"))
    (fp_text value "150µ 10V ECC ZJ100151MF6" (at 0 4.35) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.7 0 180) (size 3.5 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15625)
      (net 85 "Net-(C20-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.7 0 180) (size 3.5 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15625)
      (net 1 "Net-(BT1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_6.3x7.7.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 81.661 31.496 180)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R16" (at 3.302 0 90) (layer "F.SilkS"))
    (fp_text value "SMD 1/4W 2k2" (at 0 2.28) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 180) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 100 "Net-(Q5-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 180) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 102 "Net-(R16-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 77.851 117.348 180)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R59" (at 3.556 0 90) (layer "F.SilkS"))
    (fp_text value "SMD 1/4W 10k" (at 0 2.28) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 180) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 97 "Net-(C36-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 180) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 105 "Net-(D16-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 52.578 102.108 -90)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R29" (at 0 -2.54 90) (layer "F.SilkS"))
    (fp_text value "SMD 1/4W 1k" (at -0.254 2.032 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 60 "Net-(R29-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 94 "Net-(J12-Pad5)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 40.005 25.4)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C13" (at -3.302 0 90) (layer "F.SilkS"))
    (fp_text value "100n 50V KEM X7R1206 1,0U" (at -0.254 2.032) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 9 "Net-(C12-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 1 "Net-(BT1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_THT:SW_PUSH_6mm 1-4" (layer "F.Cu")
    (tedit 5A02FE31)
    (at 29.031 156.174 180)
    (descr "https://www.omron.com/ecb/products/pdf/en-b3f.pdf")
    (tags "tact sw push 6mm")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW10" (at 8.965 2.631 90) (layer "F.SilkS"))
    (fp_text value "reset" (at 3.75 6.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.25 2.25) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 12 "Net-(C25-Pad1)") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole circle (at 6.5 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 12 "Net-(C25-Pad1)") (pinfunction "A") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 4.5 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad2)") (pinfunction "B") (pintype "passive"))
    (pad "4" thru_hole circle (at 6.5 4.5 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad2)") (pinfunction "B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_THT:OMR B3F-4000" (layer "F.Cu")
    (tedit 5D160D14)
    (at 155.929 143.59)
    (descr "SW PUSH 12mm https://www.e-switch.com/system/asset/product_line/data_sheet/143/TL1100.pdf")
    (tags "tact sw push 12mm")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW7" (at 6.08 -4.66) (layer "F.SilkS"))
    (fp_text value "Zurück" (at 6.62 9.93) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 2.54) (layer "F.Fab"))
    (pad "1" thru_hole oval (at 12.5 5) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 127 "Net-(J13-Pad4)") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 5) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 127 "Net-(J13-Pad4)") (pinfunction "A") (pintype "passive"))
    (pad "3" thru_hole oval (at 12.5 0) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 130 "Net-(J13-Pad1)") (pinfunction "B") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 0) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 130 "Net-(J13-Pad1)") (pinfunction "B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH-12mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_THT:OMR B3F-4000" (layer "F.Cu")
    (tedit 5D160D14)
    (at 127.989 157.56)
    (descr "SW PUSH 12mm https://www.e-switch.com/system/asset/product_line/data_sheet/143/TL1100.pdf")
    (tags "tact sw push 12mm")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW9" (at 6.08 -4.66) (layer "F.SilkS"))
    (fp_text value "Runter" (at 6.62 9.93) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 2.54) (layer "F.Fab"))
    (pad "1" thru_hole oval (at 12.5 5) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 127 "Net-(J13-Pad4)") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 5) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 127 "Net-(J13-Pad4)") (pinfunction "A") (pintype "passive"))
    (pad "3" thru_hole oval (at 12.5 0) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 128 "Net-(J13-Pad3)") (pinfunction "B") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 0) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 128 "Net-(J13-Pad3)") (pinfunction "B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH-12mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 44.323 101.581 -90)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R39" (at -3.156 0 180) (layer "F.SilkS"))
    (fp_text value "SMD 1/4W 1k" (at 0 2.28 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 69 "Net-(R39-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 91 "Net-(J12-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 66.421 34.671)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C31" (at 3.302 0.127 90) (layer "F.SilkS"))
    (fp_text value "1µ 50V KEM X7R1206 1,0U" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 1 "Net-(BT1-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 86 "Net-(C31-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_THT:OMR B3F-4000" (layer "F.Cu")
    (tedit 5D160D14)
    (at 155.929 157.56)
    (descr "SW PUSH 12mm https://www.e-switch.com/system/asset/product_line/data_sheet/143/TL1100.pdf")
    (tags "tact sw push 12mm")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW4" (at 6.08 -4.525) (layer "F.SilkS"))
    (fp_text value "Ok" (at 6.62 9.93) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 2.54) (layer "F.Fab"))
    (pad "1" thru_hole oval (at 12.5 5) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 126 "Net-(J13-Pad5)") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 5) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 126 "Net-(J13-Pad5)") (pinfunction "A") (pintype "passive"))
    (pad "3" thru_hole oval (at 12.5 0) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 130 "Net-(J13-Pad1)") (pinfunction "B") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 0) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 130 "Net-(J13-Pad1)") (pinfunction "B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH-12mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 156.083 133.35 -90)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R36" (at 0 2.286 90) (layer "F.SilkS"))
    (fp_text value "SMD 1/4W 2k2" (at 0 2.28 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 103 "Net-(D9-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 135 "Net-(J13-Pad9)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 30.861 55.626 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C33" (at 1.778 -3.048 90) (layer "F.SilkS"))
    (fp_text value "100n 50V KEM X7R1206 1,0U" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 180) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 85 "Net-(C20-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 180) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 1 "Net-(BT1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 53.721 121.666 90)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R14" (at -0.127 2.54 90) (layer "F.SilkS"))
    (fp_text value "SMD 1/4W 10k" (at 0 2.28 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 90) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 1 "Net-(BT1-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 90) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 106 "Net-(R14-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 74.676 47.685888 -90)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C35" (at 1.082112 3.683 -90) (layer "F.SilkS"))
    (fp_text value "GA-A 10U 16V" (at 1 3.75 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C1-Pad2)") (pintype "passive"))
    (pad "2" thru_hole circle (at 2 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50CD5)
    (at 30.861 39.37 90)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D8" (at 5.08 -2.47 90) (layer "F.SilkS"))
    (fp_text value "1N4007" (at 5.08 2.47 90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 5.47 0 90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 22 "Net-(D8-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 "Net-(C12-Pad1)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 81.661 41.656 180)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R11" (at 3.302 0 90) (layer "F.SilkS"))
    (fp_text value "SMD 1/4W 15k" (at 0 2.28) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 180) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 10 "Net-(C14-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 180) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 8 "Net-(C10-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-92_Inline" (layer "F.Cu")
    (tedit 5A1DD157)
    (at 38.375 41.275 -90)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Q3" (at -0.635 2.942 90) (layer "F.SilkS"))
    (fp_text value "BC327" (at 1.27 2.79 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 22 "Net-(D8-Pad1)") (pinfunction "C") (pintype "passive"))
    (pad "2" thru_hole oval (at 1.27 0 270) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 42 "Net-(Q3-Pad2)") (pinfunction "B") (pintype "input"))
    (pad "3" thru_hole oval (at 2.54 0 270) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 10 "Net-(C14-Pad1)") (pinfunction "E") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 37.973 49.377 90)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R22" (at -0.153 2.794 90) (layer "F.SilkS"))
    (fp_text value "SMD 1/4W 10k" (at 0 2.28 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 90) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 52 "Net-(R22-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 90) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 85 "Net-(C20-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Relay_THT:Relay_SPDT_Finder_40.51" (layer "F.Cu")
    (tedit 5A5B3F25)
    (at 87.7335 100.1785)
    (descr "Relay DPDT Finder 40.51, Pitch 5mm/7.5mm, https://www.finder-relais.net/de/finder-relais-serie-40.pdf")
    (tags "Relay DPDT Finder 40.51 Pitch 5mm")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "K1" (at 25.4235 -4.1665 90) (layer "F.SilkS"))
    (fp_text value "FINDER-40.51" (at 12.192 11.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 12.065 3.81) (layer "F.Fab"))
    (pad "11" thru_hole circle (at 20 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 85 "Net-(C20-Pad1)") (pintype "passive"))
    (pad "12" thru_hole circle (at 15 7.5) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 38 "unconnected-(K1-Pad12)") (pintype "passive"))
    (pad "14" thru_hole circle (at 25 7.5) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 104 "Net-(D15-Pad2)") (pintype "passive"))
    (pad "A1" thru_hole rect (at 0 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 17 "Net-(D3-Pad2)") (pintype "passive"))
    (pad "A2" thru_hole circle (at 0 7.5) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 18 "Net-(D4-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Relay_THT.3dshapes/Relay_SPDT_Finder_40.51.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 32.131 50.546)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U6" (at 4.826 2.159 180) (layer "F.SilkS"))
    (fp_text value "DS1307Z RTC" (at 0 3.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 82 "Net-(U6-Pad1)") (pinfunction "X1") (pintype "input"))
    (pad "2" smd roundrect (at -2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 83 "Net-(U6-Pad2)") (pinfunction "X2") (pintype "input"))
    (pad "3" smd roundrect (at -2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(BT1-Pad1)") (pinfunction "VBAT") (pintype "power_in"))
    (pad "4" smd roundrect (at -2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(BT1-Pad2)") (pinfunction "GND") (pintype "power_in"))
    (pad "5" smd roundrect (at 2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "Net-(R21-Pad1)") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "6" smd roundrect (at 2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 52 "Net-(R22-Pad1)") (pinfunction "SCL") (pintype "input"))
    (pad "7" smd roundrect (at 2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 84 "unconnected-(U6-Pad7)") (pinfunction "SQW/OUT") (pintype "open_collector"))
    (pad "8" smd roundrect (at 2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 85 "Net-(C20-Pad1)") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_THT:L_Radial_D9.5mm_P5.00mm_Fastron_07HVP" (layer "F.Cu")
    (tedit 5AE59B06)
    (at 41.021 31.536 -90)
    (descr "Inductor, Radial series, Radial, pin pitch=5.00mm, , diameter=9.5mm, Fastron, 07HVP, http://www.fastrongroup.com/image-show/107/07HVP%2007HVP_T.pdf?type=Complete-DataSheet&productType=series")
    (tags "Inductor Radial series Radial pin pitch 5.00mm  diameter 9.5mm Fastron 07HVP")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "L1" (at 2.5 -6 90) (layer "F.SilkS"))
    (fp_text value "L-07HVP 820µ 0A53" (at 2.754 5.842 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 9 "Net-(C12-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 22 "Net-(D8-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_THT.3dshapes/L_Radial_D9.5mm_P5.00mm_Fastron_07HVP.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 33.909 79.375 90)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R47" (at 0.381 -2.413 90) (layer "F.SilkS"))
    (fp_text value "SMD 1/4W 1k" (at 0 2.28 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 90) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 76 "Net-(R47-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 90) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 119 "Net-(J14-Pad18)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 81.4985 72.136 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C8" (at 0 -1.85 90) (layer "F.SilkS"))
    (fp_text value "22u 25V X5R-G1210 22" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 6 "Net-(C8-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 1 "Net-(BT1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Potentiometer_THT:Potentiometer_ACP_CA9-H5_Horizontal" (layer "F.Cu")
    (tedit 5A3D4994)
    (at 63.54 139.257)
    (descr "Potentiometer, horizontal, ACP CA9-H5, http://www.acptechnologies.com/wp-content/uploads/2017/05/02-ACP-CA9-CE9.pdf")
    (tags "Potentiometer horizontal ACP CA9-H5")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "RV1" (at -0.294 -4.256 90) (layer "F.SilkS"))
    (fp_text value "76-40 10K" (at 0 8.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.548 1.713) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.34 2.34) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 2.5) (size 2.34 2.34) (drill 1.3) (layers *.Cu *.Mask)
      (net 114 "Net-(RV1-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 5) (size 2.34 2.34) (drill 1.3) (layers *.Cu *.Mask)
      (net 85 "Net-(C20-Pad1)") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_ACP_CA9-H5_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 33.02 101.981 -90)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R31" (at -3.175 -0.127 180) (layer "F.SilkS"))
    (fp_text value "SMD 1/4W 1k" (at 0 2.28 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 62 "Net-(R31-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 109 "Net-(R31-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Relay_THT:Relay_SPDT_Finder_40.61" (layer "F.Cu")
    (tedit 5A5B3E92)
    (at 96.6235 43.0285)
    (descr "Relay DPDT Finder 40.52, Pitch 5mm/7.5mm, https://www.finder-relais.net/de/finder-relais-serie-40.pdf")
    (tags "Relay DPDT Finder 40.52 Pitch 5mm")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "K2" (at 10 -3.6) (layer "F.SilkS"))
    (fp_text value "FINDER-40.51" (at 12.192 11.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 12.065 3.81) (layer "F.Fab"))
    (pad "11" thru_hole circle (at 20 7.5) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 15 "Net-(C3-Pad1)") (pintype "passive"))
    (pad "11" thru_hole circle (at 20 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 15 "Net-(C3-Pad1)") (pintype "passive"))
    (pad "12" thru_hole circle (at 15 7.5) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 39 "unconnected-(K2-Pad12)") (pintype "passive"))
    (pad "12" thru_hole circle (at 15 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 39 "unconnected-(K2-Pad12)") (pintype "passive"))
    (pad "14" thru_hole circle (at 25 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 10 "Net-(C14-Pad1)") (pintype "passive"))
    (pad "14" thru_hole circle (at 25 7.5) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 10 "Net-(C14-Pad1)") (pintype "passive"))
    (pad "A1" thru_hole rect (at 0 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 17 "Net-(D3-Pad2)") (pintype "passive"))
    (pad "A2" thru_hole circle (at 0 7.5) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 21 "Net-(D7-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Relay_THT.3dshapes/Relay_DPDT_Finder_40.52.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 63.246 41.021 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C9" (at -3.683 -0.127 -90) (layer "F.SilkS"))
    (fp_text value "100n 50V KEM X7R1206 1,0U" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 1 "Net-(BT1-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 7 "Net-(C9-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-92_Inline" (layer "F.Cu")
    (tedit 5A1DD157)
    (at 89.281 32.766 90)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Q5" (at 1.27 -3.81 270) (layer "F.SilkS"))
    (fp_text value "BC337" (at 1.27 2.79 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 88 "Net-(D11-Pad2)") (pinfunction "C") (pintype "passive"))
    (pad "2" thru_hole oval (at 1.27 0 90) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 100 "Net-(Q5-Pad2)") (pinfunction "B") (pintype "input"))
    (pad "3" thru_hole oval (at 2.54 0 90) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad2)") (pinfunction "E") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 81.4985 64.516 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C5" (at 0 -1.85 90) (layer "F.SilkS"))
    (fp_text value "10u 50V KEM X5R1210 10U" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 1 "Net-(BT1-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 15 "Net-(C3-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 73.533 125.73 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C36" (at 4.064 0 90) (layer "F.SilkS"))
    (fp_text value "100n 50V KEM X7R1206 1,0U" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 97 "Net-(C36-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 1 "Net-(BT1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 74.676 55.946113 90)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C18" (at 1 -3.75 90) (layer "F.SilkS"))
    (fp_text value "RAD FC 4,7U/50V" (at 1 3.75 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "Net-(C11-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 2 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 55.753 59.69 -90)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R30" (at 0 -2.54 90) (layer "F.SilkS"))
    (fp_text value "SMD 1/4W 10k" (at 0 2.28 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 61 "Net-(R30-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 85 "Net-(C20-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 69.596 41.021 90)
    (descr "SOIC, 14 Pin (JEDEC MS-012AB, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at -0.127 5.461 270) (layer "F.SilkS"))
    (fp_text value "ATtiny44-20SS" (at 0 5.28 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -3.81 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(C1-Pad2)") (pinfunction "VCC") (pintype "power_in"))
    (pad "2" smd roundrect (at -2.475 -2.54 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 80 "unconnected-(U1-Pad2)") (pinfunction "XTAL1/PB0") (pintype "bidirectional"))
    (pad "3" smd roundrect (at -2.475 -1.27 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 81 "unconnected-(U1-Pad3)") (pinfunction "XTAL2/PB1") (pintype "bidirectional"))
    (pad "4" smd roundrect (at -2.475 0 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(C9-Pad2)") (pinfunction "~{RESET}/PB3") (pintype "bidirectional"))
    (pad "5" smd roundrect (at -2.475 1.27 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "Net-(R8-Pad2)") (pinfunction "PB2") (pintype "bidirectional"))
    (pad "6" smd roundrect (at -2.475 2.54 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 57 "Net-(R27-Pad1)") (pinfunction "PA7") (pintype "bidirectional"))
    (pad "7" smd roundrect (at -2.475 3.81 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(J3-Pad4)") (pinfunction "MOSI_PA6") (pintype "bidirectional"))
    (pad "8" smd roundrect (at 2.475 3.81 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "Net-(J3-Pad1)") (pinfunction "MISO_ADC5_PA5") (pintype "bidirectional"))
    (pad "9" smd roundrect (at 2.475 2.54 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(J3-Pad3)") (pinfunction "SCK_ADC4_PA4") (pintype "bidirectional"))
    (pad "10" smd roundrect (at 2.475 1.27 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(C10-Pad2)") (pinfunction "ADC3_PA3") (pintype "bidirectional"))
    (pad "11" smd roundrect (at 2.475 0 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 102 "Net-(R16-Pad2)") (pinfunction "ADC2_PA2") (pintype "bidirectional"))
    (pad "12" smd roundrect (at 2.475 -1.27 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 86 "Net-(C31-Pad2)") (pinfunction "ADC1_PA1") (pintype "bidirectional"))
    (pad "13" smd roundrect (at 2.475 -2.54 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(C2-Pad1)") (pinfunction "AREF_ADC0_PA0") (pintype "bidirectional"))
    (pad "14" smd roundrect (at 2.475 -3.81 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(BT1-Pad2)") (pinfunction "GND") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 74 19.558 90)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D5" (at 0.125 -1.802 90) (layer "F.SilkS"))
    (fp_text value "OSO LYR976 Grün" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 1 "Net-(BT1-Pad2)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 19 "Net-(D5-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D8.0mm_P3.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 86.741 148.972651 90)
    (descr "CP, Radial series, Radial, pin pitch=3.50mm, , diameter=8mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 3.50mm  diameter 8mm Electrolytic Capacitor")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C22" (at -2.665349 -3.81 270) (layer "F.SilkS"))
    (fp_text value "470U 10V RAD FC 470/10" (at 1.398651 5.334 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.75 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 85 "Net-(C20-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 3.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D8.0mm_P3.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 57.15 89.89 90)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R55" (at 3.149 0.127 180) (layer "F.SilkS"))
    (fp_text value "SMD 1/4W 1k" (at 0 2.28 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 90) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 134 "Net-(R55-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 90) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 133 "Net-(D13-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Crystal:Crystal_C38-LF_D3.0mm_L8.0mm_Horizontal_1EP_style1" (layer "F.Cu")
    (tedit 5A0FD1B2)
    (at 26.731 50.716 180)
    (descr "Crystal THT C38-LF 8.0mm length 3.0mm diameter")
    (tags "['C38-LF']")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Y1" (at 4.252 0.17 90) (layer "F.SilkS"))
    (fp_text value "Crystal" (at 3.97 2.25 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.95 5.25) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 83 "Net-(U6-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 1.9 0 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 82 "Net-(U6-Pad1)") (pinfunction "2") (pintype "passive"))
    (pad "3" smd rect (at 0.95 7 180) (size 3 8) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Crystal_C38-LF_D3.0mm_L8.0mm_Horizontal_1EP_style1.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SC-80_HandSoldering" (layer "F.Cu")
    (tedit 58A57D7F)
    (at 70.739 125.222 90)
    (descr "JEITA SC-80")
    (tags "SC-80")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D16" (at -3.556 0 90) (layer "F.SilkS"))
    (fp_text value "SMD ZF 5,6" (at 0 1.6 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.5 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.1 0 90) (size 1.1 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 104 "Net-(D15-Pad2)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect (at 1.1 0 90) (size 1.1 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 105 "Net-(D16-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SC-80.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:CP_Elec_6.3x7.7" (layer "F.Cu")
    (tedit 5BCA39D0)
    (at 62.738 88.646 90)
    (descr "SMD capacitor, aluminum electrolytic, Nichicon, 6.3x7.7mm")
    (tags "capacitor electrolytic")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C21" (at 0 4.699 90) (layer "F.SilkS"))
    (fp_text value "150µ 10V ECC ZJ100151MF6" (at 0 4.35 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.7 0 90) (size 3.5 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15625)
      (net 85 "Net-(C20-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.7 0 90) (size 3.5 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15625)
      (net 1 "Net-(BT1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_6.3x7.7.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 98.171 64.516 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C4" (at 0 2.032 90) (layer "F.SilkS"))
    (fp_text value "10u 50V KEM X5R1210 10U" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 15 "Net-(C3-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 1 "Net-(BT1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 57.023 82.804)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R49" (at 3.3274 0 90) (layer "F.SilkS"))
    (fp_text value "SMD 1/4W 1k" (at 0 2.28) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.127 0.127) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 78 "Net-(R49-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 31 "Net-(J14-Pad16)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuseholder_Cylinder-5x20mm_Schurter_0031_8201_Horizontal_Open" (layer "F.Cu")
    (tedit 5D717D34)
    (at 122.301 108.966 90)
    (descr "Fuseholder horizontal open, 5x20mm, 500V, 16A, Schurter 0031.8201, https://us.schurter.com/bundles/snceschurter/epim/_ProdPool_/newDS/en/typ_OGN.pdf")
    (tags "Fuseholder horizontal open 5x20 Schurter 0031.8201")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "F4" (at 10.033 -5.842 90) (layer "F.SilkS"))
    (fp_text value "Fuse" (at 11.25 6 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 11.25 4 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 11.25 0 90) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 0 0 90) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 104 "Net-(D15-Pad2)") (pintype "passive"))
    (pad "2" thru_hole circle (at 22.5 0 90) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 98 "Net-(F4-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Fuse.3dshapes/Fuseholder_Cylinder-5x20mm_Schurter_0031_8201_Horizontal_Open.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:CP_Elec_6.3x5.9" (layer "F.Cu")
    (tedit 5BCA39D0)
    (at 31.891 22.606 -90)
    (descr "SMD capacitor, aluminum electrolytic, Panasonic C6, 6.3x5.9mm")
    (tags "capacitor electrolytic")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C12" (at -4.318 3.824 -90) (layer "F.SilkS"))
    (fp_text value "100µ 35V ECC ZA350101MF8" (at 0 4.35 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.8 0 270) (size 3.5 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15625)
      (net 9 "Net-(C12-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.8 0 270) (size 3.5 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15625)
      (net 1 "Net-(BT1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_6.3x5.9.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Relay_THT:Relay_SPDT_Finder_40.61" (layer "F.Cu")
    (tedit 5A5B3E92)
    (at 96.6235 23.9785)
    (descr "Relay DPDT Finder 40.52, Pitch 5mm/7.5mm, https://www.finder-relais.net/de/finder-relais-serie-40.pdf")
    (tags "Relay DPDT Finder 40.52 Pitch 5mm")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "K3" (at 10 -3.6) (layer "F.SilkS"))
    (fp_text value "FINDER-40.51" (at 12.192 11.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 12.065 3.81) (layer "F.Fab"))
    (pad "11" thru_hole circle (at 20 7.5) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 15 "Net-(C3-Pad1)") (pintype "passive"))
    (pad "11" thru_hole circle (at 20 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 15 "Net-(C3-Pad1)") (pintype "passive"))
    (pad "12" thru_hole circle (at 15 7.5) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 99 "unconnected-(K3-Pad12)") (pintype "passive"))
    (pad "12" thru_hole circle (at 15 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 99 "unconnected-(K3-Pad12)") (pintype "passive"))
    (pad "14" thru_hole circle (at 25 7.5) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 44 "Net-(C11-Pad1)") (pintype "passive"))
    (pad "14" thru_hole circle (at 25 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 44 "Net-(C11-Pad1)") (pintype "passive"))
    (pad "A1" thru_hole rect (at 0 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 87 "Net-(D11-Pad1)") (pintype "passive"))
    (pad "A2" thru_hole circle (at 0 7.5) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 88 "Net-(D11-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Relay_THT.3dshapes/Relay_DPDT_Finder_40.52.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 37.973 107.931 -90)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R41" (at 3.9306 -0.127 90) (layer "F.SilkS"))
    (fp_text value "SMD 1/4W 1k" (at 0 2.28 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 70 "Net-(R41-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 112 "Net-(R41-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 31.877 43.307)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R19" (at -3.175 0 90) (layer "F.SilkS"))
    (fp_text value "SMD 1/4W 22k" (at 0 2.28) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 10 "Net-(C14-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 42 "Net-(Q3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_IDC:IDC-Header_2x10_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5EAC9A07)
    (at 84.201 158.3785 -90)
    (descr "Through hole IDC box header, 2x10, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0")
    (tags "Through hole vertical IDC box header THT 2x10 2.54mm double row")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J14" (at 0.8795 29.464 90) (layer "F.SilkS"))
    (fp_text value "Data Out" (at 1.27 28.96 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 11.43) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.1470588235)
      (net 85 "Net-(C20-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 85 "Net-(C20-Pad1)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 85 "Net-(C20-Pad1)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 85 "Net-(C20-Pad1)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole circle (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 85 "Net-(C20-Pad1)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 85 "Net-(C20-Pad1)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole circle (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad2)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole circle (at 2.54 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad2)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole circle (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad2)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole circle (at 2.54 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad2)") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole circle (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad2)") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole circle (at 2.54 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad2)") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole circle (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J14-Pad13)") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole circle (at 2.54 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J14-Pad14)") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole circle (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J14-Pad15)") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole circle (at 2.54 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J14-Pad16)") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" thru_hole circle (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J14-Pad17)") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole circle (at 2.54 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 119 "Net-(J14-Pad18)") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" thru_hole circle (at 0 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J14-Pad19)") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" thru_hole circle (at 2.54 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(J14-Pad20)") (pinfunction "Pin_20") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_IDC.3dshapes/IDC-Header_2x10_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-220-3_Vertical" (layer "F.Cu")
    (tedit 5AC8BA0D)
    (at 78.796 127.762 90)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D15" (at 2.54 2.357 90) (layer "F.SilkS"))
    (fp_text value "FS 1610DH" (at 2.54 2.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -4.27 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad2)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 90) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 104 "Net-(D15-Pad2)") (pinfunction "A") (pintype "passive"))
    (pad "3" thru_hole oval (at 5.08 0 90) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 97 "Net-(C36-Pad1)") (pinfunction "G") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 53.721 116.332)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R28" (at 3.302 0 90) (layer "F.SilkS"))
    (fp_text value "SMD 1/4W 1k" (at 0 2.28) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 59 "Net-(R28-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 108 "Net-(R28-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Battery:KHZ 20PCB-V CR2032" (layer "F.Cu")
    (tedit 0)
    (at 30.7145 28.086 -90)
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "BT1" (at -0.4 11.5375 90 unlocked) (layer "F.SilkS"))
    (fp_text value "CR2032 KEYSTONE 1058" (at -0.3 13.0615 90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 7.5 -90 unlocked) (layer "F.Fab"))
    (pad "" thru_hole oval (at -5.2 8.9 270) (size 2.8 2.2) (drill 1.3) (layers *.Cu *.Mask))
    (pad "1" thru_hole oval (at 4.5 8.9 270) (size 2.8 2.2) (drill 1.3) (layers *.Cu *.Mask)
      (net 11 "Net-(BT1-Pad1)") (pinfunction "+") (pintype "passive"))
    (pad "2" thru_hole oval (at -0.5 5.5 270) (size 2.8 2.2) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad2)") (pinfunction "-") (pintype "passive"))
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 60.071 41.021 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at -3.683 -0.254 -90) (layer "F.SilkS"))
    (fp_text value "100n 50V KEM X7R1206 1,0U" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 1 "Net-(BT1-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 3 "Net-(C1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 113.8835 78.206 -90)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 0 -2.28 90) (layer "F.SilkS"))
    (fp_text value "SMD 1/4W 0R1" (at 0 2.28 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 4 "Net-(C6-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 98 "Net-(F4-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TerminalBlock_RND:TerminalBlock_RND_205-00001_1x02_P5.00mm_Horizontal" (layer "F.Cu")
    (tedit 5B294F8C)
    (at 165.989 28.956 90)
    (descr "terminal block RND 205-00001, 2 pins, pitch 5mm, size 10x9mm^2, drill diamater 1.3mm, pad diameter 2.5mm, see http://cdn-reichelt.de/documents/datenblatt/C151/RND_205-00001_DB_EN.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_RND")
    (tags "THT terminal block RND 205-00001 pitch 5mm size 10x9mm^2 drill 1.3mm pad 2.5mm")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 2.5 -6.06 90) (layer "F.SilkS"))
    (fp_text value "DC 21V 1" (at 2.5 5.06 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 -6.06 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 23 "Net-(F2-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock_RND.3dshapes/TerminalBlock_RND_205-00001_1x02_P5.00mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50CD5)
    (at 99.441 36.576 180)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D11" (at 9.652 0 90) (layer "F.SilkS"))
    (fp_text value "1N4148" (at 3.81 2.12) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.032 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.8) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 87 "Net-(D11-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 88 "Net-(D11-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_MELF_Handsoldering" (layer "F.Cu")
    (tedit 5905D89D)
    (at 140.97 19.812)
    (descr "Diode MELF Handsoldering")
    (tags "Diode MELF Handsoldering")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D1" (at -6.276 0 90) (layer "F.SilkS"))
    (fp_text value "SA265" (at 0 2.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.25) (layer "F.Fab"))
    (pad "1" smd rect (at -3.4 0) (size 3.5 2.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "Net-(C11-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect (at 3.4 0) (size 3.5 2.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(BT1-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MELF.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 40.259 75.692 90)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R46" (at 0 -2.28 90) (layer "F.SilkS"))
    (fp_text value "SMD 1/4W 1k" (at 0 2.28 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 90) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 75 "Net-(R46-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 90) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 28 "Net-(J14-Pad13)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 56.261 41.021 90)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R4" (at 3.683 0.254 270) (layer "F.SilkS"))
    (fp_text value "SMD 1/4W 10k" (at 0 2.28 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 90) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 3 "Net-(C1-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 90) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 7 "Net-(C9-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 68.891 19.556 90)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D13" (at 0.127 -1.651 270) (layer "F.SilkS"))
    (fp_text value "OSO LYR976 Grün" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 124 "Net-(D13-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 133 "Net-(D13-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 98.171 78.206 -90)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at 0.026 2.54 90) (layer "F.SilkS"))
    (fp_text value "SMD 1/4W 0R1" (at 0 2.28 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -0.088 -0.026 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 5 "Net-(C7-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 98 "Net-(F4-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 28.956 77.597 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C25" (at 0 -1.85 90) (layer "F.SilkS"))
    (fp_text value "100n 50V KEM X7R1206 1,0U" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 12 "Net-(C25-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 1 "Net-(BT1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 66.421 30.226)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R5" (at -3.302 0 90) (layer "F.SilkS"))
    (fp_text value "SMD 1/4W 1k" (at 0 2.28) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 85 "Net-(C20-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 86 "Net-(C31-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 72.009 32.131 90)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R12" (at 0.127 -2.286 270) (layer "F.SilkS"))
    (fp_text value "SMD 1/4W 3k3" (at 0 2.28 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -0.168 0.082 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 90) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 8 "Net-(C10-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 90) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 1 "Net-(BT1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 30.099 89.516 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C29" (at 0 -1.85 90) (layer "F.SilkS"))
    (fp_text value "100n 50V KEM X7R1206 1,0U" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 85 "Net-(C20-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 1 "Net-(BT1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-92_Inline" (layer "F.Cu")
    (tedit 5A1DD157)
    (at 45.191 43.815 90)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Q4" (at 5.207 1.672 90) (layer "F.SilkS"))
    (fp_text value "BC337" (at 1.27 2.79 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 42 "Net-(Q3-Pad2)") (pinfunction "C") (pintype "passive"))
    (pad "2" thru_hole oval (at 1.27 0 90) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 43 "Net-(Q4-Pad2)") (pinfunction "B") (pintype "input"))
    (pad "3" thru_hole oval (at 2.54 0 90) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad2)") (pinfunction "E") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 72.517 120.65)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R58" (at -1.778 -3.302 90) (layer "F.SilkS"))
    (fp_text value "SMD 1/4W 10k" (at 0 2.28) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 1 "Net-(BT1-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 105 "Net-(D16-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 40.64 100.838 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C26" (at 3.175 0 180) (layer "F.SilkS"))
    (fp_text value "100n 50V KEM X7R1206 1,0U" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 85 "Net-(C20-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 1 "Net-(BT1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 51.181 80.518)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R50" (at 0.889 -6.985) (layer "F.SilkS"))
    (fp_text value "SMD 1/4W 1k" (at 0 2.28) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0.121) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 79 "Net-(R50-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 34 "Net-(J14-Pad20)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 51.181 76.708)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R43" (at 0.889 -4.572) (layer "F.SilkS"))
    (fp_text value "SMD 1/4W 1k" (at 0 2.28) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 72 "Net-(R43-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 33 "Net-(J14-Pad19)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D12.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF1)
    (at 150.241 73.189959 90)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=12.5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 12.5mm Electrolytic Capacitor")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C16" (at 2.5 -7.5 90) (layer "F.SilkS"))
    (fp_text value "ELKO 680/35 FK 1500/35 AM" (at 2.5 7.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 10 "Net-(C14-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D12.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-220-3_Vertical" (layer "F.Cu")
    (tedit 5AC8BA0D)
    (at 86.9035 65.786 -90)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U4" (at 2.54 2.4485 90) (layer "F.SilkS"))
    (fp_text value "LM78M05_TO220" (at 2.54 2.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -4.27 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 15 "Net-(C3-Pad1)") (pinfunction "VI") (pintype "power_in"))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad2)") (pinfunction "GND") (pintype "power_in"))
    (pad "3" thru_hole oval (at 5.08 0 270) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 "Net-(C8-Pad1)") (pinfunction "VO") (pintype "power_out"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 36.322 55.245 180)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R21" (at -3.429 -0.127 90) (layer "F.SilkS"))
    (fp_text value "SMD 1/4W 10k" (at 0 2.28) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 180) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 51 "Net-(R21-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 180) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 85 "Net-(C20-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 81.4985 78.206 -90)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at 0 -2.28 90) (layer "F.SilkS"))
    (fp_text value "SMD 1/4W 0R1" (at 0 2.28 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 6 "Net-(C8-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 98 "Net-(F4-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 45.466 26.416 90)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R18" (at -0.254 2.413 270) (layer "F.SilkS"))
    (fp_text value "SMD 1/4W 1k" (at 1.778 2.667 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 90) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 48 "Net-(R18-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 90) (size 1.3 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 49 "Net-(J5-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 50.673 59.182 -90)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "Lauflicht_Steuerplatine.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U7" (at 4.826 2.032 90) (layer "F.SilkS"))
    (fp_text value "25A512-ISN 512kb" (at 0 3.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "Net-(R30-Pad1)") (pinfunction "~{CS}") (pintype "input"))
    (pad "2" smd roundrect (at -2.475 -0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "Net-(J15-Pad1)") (pinfunction "MISO") (pintype "tri_state"))
    (pad "3" smd roundrect (at -2.475 0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 67 "Net-(R37-Pad1)") (pinfunction "~{WP}") (pintype "input"))
    (pad "4" smd roundrect (at -2.475 1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(BT1-Pad2)") (pinfunction "GND") (pintype "power_in"))
    (pad "5" smd roundrect (at 2.475 1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "Net-(J15-Pad4)") (pinfunction "MOSI") (pintype "input"))
    (pad "6" smd roundrect (at 2.475 0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "Net-(J15-Pad3)") (pinfunction "SCK") (pintype "input"))
    (pad "7" smd roundrect (at 2.475 -0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "Net-(R33-Pad1)") (pinfunction "~{HOLD}") (pintype "input"))
    (pad "8" smd roundrect (at 2.475 -1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 85 "Net-(C20-Pad1)") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_circle (center 77.851 145.796) (end 79.851 148.296) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_circle (center 49.784 19.685) (end 51.784 22.185) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_circle (center 21.336 162.941) (end 23.336 165.441) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_circle (center 18.891 46.736) (end 20.891 49.236) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_circle (center 119.761 163.576) (end 121.761 166.076) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_circle (center 63.246 61.341) (end 65.246 63.841) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_circle (center 119.126 58.166) (end 121.126 60.666) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_circle (center 148.971 163.576) (end 150.971 166.076) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_circle (center 101.981 120.396) (end 103.981 122.896) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_circle (center 166.751 120.396) (end 168.751 122.896) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_circle (center 155.321 18.796) (end 157.321 21.296) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_circle (center 135.662562 108.966) (end 137.662562 111.466) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_rect (start 174.371 169.291) (end 14.351 14.605) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_text "Betrieb ______\nPause - - -\nStörung  . . ." (at 63.246 22.733 90) (layer "F.SilkS"))
  (gr_text "DC21V 1" (at 171.704 26.543 90) (layer "F.SilkS"))
  (gr_text "M2,5A" (at 116.332 94.615 90) (layer "F.SilkS"))
  (gr_text "Netz" (at 107.0864 35.306) (layer "F.SilkS"))
  (gr_text "Panel 2" (at 171.45 65.659 90) (layer "F.SilkS"))
  (gr_text "Panel 4" (at 171.45 91.44 90) (layer "F.SilkS"))
  (gr_text "5V" (at 78.994 16.891) (layer "F.SilkS"))
  (gr_text "M10A" (at 144.526 46.99) (layer "F.SilkS"))
  (gr_text "ISP PCPU" (at 60.325 20.955 90) (layer "F.SilkS"))
  (gr_text "M10A" (at 144.78 23.114) (layer "F.SilkS"))
  (gr_text "Netz" (at 88.646 16.891) (layer "F.SilkS"))
  (gr_text "Panel 3" (at 171.45 78.232 90) (layer "F.SilkS"))
  (gr_text "Panel 1\n" (at 171.45 52.959 90) (layer "F.SilkS"))
  (gr_text "M0,2A" (at 104.267 16.129) (layer "F.SilkS"))
  (gr_text "HCPU" (at 68.834 16.891) (layer "F.SilkS"))
  (gr_text "Panel 5" (at 171.45 104.14 90) (layer "F.SilkS"))
  (gr_text "DC21V 2" (at 171.577 39.878 90) (layer "F.SilkS"))
  (gr_text "ISP HCPU" (at 20.828 57.404) (layer "F.SilkS"))
  (gr_text "M0,2A" (at 71.12 64.77 90) (layer "F.SilkS"))
  (gr_text "20,00" (at 21.844 88.392 90) (layer "F.SilkS"))
  (gr_text "PCPU" (at 74.041 16.891) (layer "F.SilkS"))
  (gr_text "21V" (at 83.947 16.891) (layer "F.SilkS"))
  (zone (net 1) (net_name "Net-(BT1-Pad2)") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 27.889373 45.719495)
        (xy 30.429373 45.719495)
        (xy 64.719373 45.719495)
        (xy 72.39 45.72)
        (xy 72.339373 48.259495)
        (xy 72.339373 72.389495)
        (xy 76.2 77.469495)
        (xy 76.2 111.76)
        (xy 83.18502 118.749992)
        (xy 84.404373 150.494495)
        (xy 79.324373 155.574495)
        (xy 79.436244 156.415247)
        (xy 79.324184 167.65848)
        (xy 15.189373 167.639495)
        (xy 15.189373 16.509495)
        (xy 27.889373 16.509495)
      )
    )
  )
  (zone (net 135) (net_name "Net-(J13-Pad9)") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 172.72 167.64)
        (xy 96.52 167.64)
        (xy 96.52 115.57)
        (xy 172.72 115.57)
      )
    )
  )
)
