(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (aux_axis_origin 120 120)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (gr_arc (start 118.063805 113.63811) (mid 118.527172 113.730429) (end 118.706777 114.167434)
    (layer "Edge.Cuts"))
  (gr_arc (start 121.293223 114.167434) (mid 120 115.6) (end 118.706777 114.167434)
    (layer "Edge.Cuts"))
  (gr_arc (start 121.936195 113.63811) (mid 120 126.65) (end 118.063805 113.63811)
    (layer "Edge.Cuts"))
  (gr_arc (start 121.293223 114.167434) (mid 121.472829 113.730429) (end 121.936195 113.63811)
    (layer "Edge.Cuts"))
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 114.59 117.18)
        (xy 119.038823 118.37021)
        (xy 119.08 118.39)
        (xy 119.119004 118.423785)
        (xy 119.15 118.49)
        (xy 119.15 121.484901)
        (xy 119.14 121.54)
        (xy 119.119003 121.576215)
        (xy 119.08 121.61)
        (xy 119.05 121.63)
        (xy 114.59 122.82)
        (xy 114.51 122.83)
        (xy 114.44 122.82)
        (xy 114.36 122.8)
        (xy 114.28 122.75)
        (xy 114.21 122.69)
        (xy 114.17 122.63)
        (xy 114.147561 122.590165)
        (xy 113.95 122.09)
        (xy 113.8 121.59)
        (xy 113.69 121.07)
        (xy 113.62 120.53)
        (xy 113.6 120)
        (xy 113.62 119.48)
        (xy 113.69 118.93)
        (xy 113.8 118.41)
        (xy 113.95 117.92)
        (xy 114 117.78)
        (xy 114.147561 117.409835)
        (xy 114.19 117.33)
        (xy 114.27 117.25)
        (xy 114.340734 117.210876)
        (xy 114.42 117.18)
        (xy 114.49 117.17)
        (xy 114.55 117.17)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 125.41 122.83)
        (xy 120.961177 121.63979)
        (xy 120.92 121.62)
        (xy 120.880996 121.586215)
        (xy 120.85 121.52)
        (xy 120.85 118.525099)
        (xy 120.86 118.47)
        (xy 120.880997 118.433785)
        (xy 120.92 118.4)
        (xy 120.95 118.38)
        (xy 125.41 117.19)
        (xy 125.49 117.18)
        (xy 125.56 117.19)
        (xy 125.64 117.21)
        (xy 125.72 117.26)
        (xy 125.79 117.32)
        (xy 125.83 117.38)
        (xy 125.852439 117.419835)
        (xy 126.05 117.92)
        (xy 126.2 118.42)
        (xy 126.31 118.94)
        (xy 126.38 119.48)
        (xy 126.4 120.01)
        (xy 126.38 120.53)
        (xy 126.31 121.08)
        (xy 126.2 121.6)
        (xy 126.05 122.09)
        (xy 126 122.23)
        (xy 125.852439 122.600165)
        (xy 125.81 122.68)
        (xy 125.73 122.76)
        (xy 125.659266 122.799124)
        (xy 125.58 122.83)
        (xy 125.51 122.84)
        (xy 125.45 122.84)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 121.749571 114.261248)
        (xy 121.77 114.12)
        (xy 121.84 114.04)
        (xy 121.93 113.98)
        (xy 122.04 113.95)
        (xy 122.150292 113.972045)
        (xy 122.62 114.16)
        (xy 123.08 114.39)
        (xy 123.53 114.66)
        (xy 123.94214 114.958222)
        (xy 124.33 115.29)
        (xy 124.7 115.66)
        (xy 125.03 116.04)
        (xy 125.331376 116.459317)
        (xy 125.38 116.57)
        (xy 125.4 116.65)
        (xy 125.39 116.76)
        (xy 125.372329 116.822036)
        (xy 125.32 116.92)
        (xy 125.26 116.98)
        (xy 125.18 117.04)
        (xy 125.14 117.06)
        (xy 120.574118 118.28014)
        (xy 120.55 118.29)
        (xy 120.520665 118.315857)
        (xy 120.5 118.35)
        (xy 120.5 121.65)
        (xy 120.520665 121.684143)
        (xy 120.53 121.7)
        (xy 120.56 121.72)
        (xy 125.14 122.94)
        (xy 125.23 122.99)
        (xy 125.31 123.07)
        (xy 125.37 123.17)
        (xy 125.39 123.25)
        (xy 125.4 123.32)
        (xy 125.39 123.41)
        (xy 125.37 123.47)
        (xy 125.34 123.53)
        (xy 125.04 123.94)
        (xy 124.73 124.31)
        (xy 124.42 124.63)
        (xy 124.04 124.96)
        (xy 123.62 125.28)
        (xy 123.24 125.52)
        (xy 122.83 125.74)
        (xy 122.36 125.95)
        (xy 121.91 126.11)
        (xy 121.44 126.24)
        (xy 120.97 126.33)
        (xy 120.48 126.38)
        (xy 120 126.4)
        (xy 119.5 126.38)
        (xy 119.03 126.33)
        (xy 118.56 126.24)
        (xy 118.09 126.11)
        (xy 117.63 125.95)
        (xy 117.19 125.75)
        (xy 116.76 125.52)
        (xy 116.37 125.27)
        (xy 115.97 124.97)
        (xy 115.59 124.64)
        (xy 115.26 124.3)
        (xy 114.95 123.93)
        (xy 114.668624 123.540683)
        (xy 114.64 123.49)
        (xy 114.61 123.4)
        (xy 114.6 123.32)
        (xy 114.61 123.24)
        (xy 114.63 123.16)
        (xy 114.67 123.09)
        (xy 114.72 123.03)
        (xy 114.79 122.98)
        (xy 114.87 122.94)
        (xy 119.425882 121.71986)
        (xy 119.45 121.71)
        (xy 119.479352 121.684157)
        (xy 119.5 121.64)
        (xy 119.5 118.376733)
        (xy 119.49 118.33)
        (xy 119.479323 118.315859)
        (xy 119.46 118.3)
        (xy 119.43 118.28)
        (xy 114.898308 117.06698)
        (xy 114.82 117.04)
        (xy 114.74 116.98)
        (xy 114.69 116.93)
        (xy 114.65 116.87)
        (xy 114.62 116.8)
        (xy 114.61 116.75)
        (xy 114.6 116.68)
        (xy 114.61 116.59)
        (xy 114.64 116.51)
        (xy 114.668624 116.459317)
        (xy 114.97 116.04)
        (xy 115.3 115.65)
        (xy 115.66 115.29)
        (xy 116.05786 114.958222)
        (xy 116.47 114.66)
        (xy 116.92 114.39)
        (xy 117.4 114.15)
        (xy 117.849708 113.972045)
        (xy 117.9 113.96)
        (xy 117.96 113.96)
        (xy 118.04 113.97)
        (xy 118.11 114)
        (xy 118.17 114.05)
        (xy 118.21 114.1)
        (xy 118.24 114.18)
        (xy 118.25 114.25)
        (xy 118.25 114.42)
        (xy 118.27 114.6)
        (xy 118.32 114.78)
        (xy 118.37 114.94)
        (xy 118.44 115.1)
        (xy 118.53 115.25)
        (xy 118.63 115.39)
        (xy 118.71 115.48)
        (xy 118.75 115.53)
        (xy 118.88 115.64)
        (xy 119.01 115.74)
        (xy 119.17 115.84)
        (xy 119.32 115.91)
        (xy 119.49 115.97)
        (xy 119.65 116.01)
        (xy 119.82 116.04)
        (xy 119.98 116.05)
        (xy 120.16 116.04)
        (xy 120.33 116.02)
        (xy 120.48 115.98)
        (xy 120.68 115.91)
        (xy 120.85 115.83)
        (xy 120.95 115.77)
        (xy 121.06 115.69)
        (xy 121.15 115.62)
        (xy 121.26 115.51)
        (xy 121.35 115.41)
        (xy 121.46 115.26)
        (xy 121.53 115.15)
        (xy 121.59 115.03)
        (xy 121.64 114.9)
        (xy 121.68 114.79)
        (xy 121.7 114.71)
        (xy 121.72 114.62)
        (xy 121.74 114.47)
        (xy 121.75 114.3)
      )
    )
  )
)
