(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (gr_arc (start 148.706777 105.832566) (mid 148.527188 106.269604) (end 148.063805 106.36189) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 148.063805 106.36189) (mid 150 93.35) (end 151.936195 106.36189) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 151.936195 106.36189) (mid 151.47283 106.269581) (end 151.293223 105.832566) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 148.706777 105.832566) (mid 150 104.4) (end 151.293223 105.832566) (layer "Edge.Cuts") (width 0.1))
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (arc (start 151.749571 105.738752) (mid 151.873936 105.988657) (end 152.150292 106.027955))
        (arc (start 152.150292 106.027955) (mid 153.94214 105.041779) (end 155.331376 103.540683))
        (arc (start 155.331376 103.540683) (mid 155.37236 103.177962) (end 155.101692 102.93302))
        (arc (start 150.574118 101.71986) (mid 150.520677 101.684141) (end 150.5 101.623267))
        (arc (start 150.5 98.376733) (mid 150.520652 98.31584) (end 150.574118 98.28014))
        (arc (start 155.101692 97.06698) (mid 155.372327 96.822026) (end 155.331376 96.459317))
        (arc (start 155.331376 96.459317) (mid 150 93.6) (end 144.668624 96.459317))
        (arc (start 144.668624 96.459317) (mid 144.62764 96.822038) (end 144.898308 97.06698))
        (arc (start 149.425882 98.28014) (mid 149.479323 98.315859) (end 149.5 98.376733))
        (arc (start 149.5 101.623267) (mid 149.479348 101.68416) (end 149.425882 101.71986))
        (arc (start 144.898308 102.93302) (mid 144.627673 103.177974) (end 144.668624 103.540683))
        (arc (start 144.668624 103.540683) (mid 146.05786 105.041778) (end 147.849708 106.027955))
        (arc (start 147.849708 106.027955) (mid 148.126069 105.988664) (end 148.250429 105.738752))
        (arc (start 148.250429 105.738752) (mid 150 103.95) (end 151.749571 105.738752))
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (arc (start 149.15 98.515099) (mid 149.119004 98.423785) (end 149.038823 98.37021))
        (arc (start 144.616866 97.18535) (mid 144.340733 97.210887) (end 144.147561 97.409835))
        (arc (start 144.147561 97.409835) (mid 143.6 100) (end 144.147561 102.590165))
        (arc (start 144.147561 102.590165) (mid 144.340718 102.789143) (end 144.616866 102.81465))
        (arc (start 149.038823 101.62979) (mid 149.119003 101.576215) (end 149.15 101.484901))
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (arc (start 150.85 101.484901) (mid 150.880996 101.576215) (end 150.961177 101.62979))
        (arc (start 155.383134 102.81465) (mid 155.659267 102.789113) (end 155.852439 102.590165))
        (arc (start 155.852439 102.590165) (mid 156.4 100) (end 155.852439 97.409835))
        (arc (start 155.852439 97.409835) (mid 155.659282 97.210857) (end 155.383134 97.18535))
        (arc (start 150.961177 98.37021) (mid 150.880997 98.423785) (end 150.85 98.515099))
      )
    )
  )
)
