(footprint "tripad" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at -1.5 -3 unlocked) (layer "F.SilkS"))
  (fp_text value "tripad" (at 0 3 unlocked) (layer "F.Fab"))
  (fp_text user "${REFERENCE}" (at 0 4.5 unlocked) (layer "F.Fab"))
  (pad "1" smd custom (at 0 0) (size 0.001 0.001) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly
        (pts
          (xy -1 1)
          (xy -1.5 0)
          (xy -1 -1)
          (xy 1 -1)
          (xy 1.5 0)
          (xy 1 1)
        )
        (width 0.01) (fill yes))
    ))
  (pad "2" smd custom (at -2.5 0) (size 0.001 0.001) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly
        (pts
          (xy -1 1)
          (xy -1 -1)
          (xy 1 -1)
          (xy 0.5 0)
          (xy 1 1)
        )
        (width 0.01) (fill yes))
    ))
  (pad "3" smd custom (at 2.5 0 180) (size 0.001 0.001) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly
        (pts
          (xy -1 1)
          (xy -1 -1)
          (xy 1 -1)
          (xy 0.5 0)
          (xy 1 1)
        )
        (width 0.01) (fill yes))
    ))
)
