{"text_format":"3","workbook":"xls","n_sheets":9,"sheets":["ATtiny26","ATtiny2313","ATtiny261_461_861","ATmega8A","ATmega16","ATmega32A","ATmega64","ATmega_48_88_168_328","ATmega164_324_644_1284"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"ATtiny26","index":0,"n_rows":67,"n_cols":11,"rows_kept":67,"flags":["formulas_cached_only"]}
[null,null,"ATtiny26(L)"]
[]
["Address","Name",null,"Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["$3F ($5F)","SREG",null,"I","T","H","S","V","N","Z","C"]
["$3E ($5E)","Reserved"]
["$3D ($5D)","SP",null,"SP7","SP6","SP5","SP4","SP3","SP2","SP1","SP0"]
["$3C ($5C)","Reserved"]
["$3B ($5B)","GIMSK",null,"-","INT0","PCIE1","PCIE0","-","-","-","-"]
["$3A ($5A)","GIFR",null,"-","INTF0","PCIF","-","-","-","-","-"]
["$39 ($59)","TIMSK","Timer/Counter Interrupt Mask Register","-","OCIE1A","OCIE1B","-","-","TOIE1","TOIE0","-"]
["$38 ($58)","TIFR","Timer/Counter Interrupt Flag Register","-","OCF1A","OCF1B","-","-","TOV1","TOV0","-"]
["$37 ($57)","Reserved"]
["$36 ($56)","Reserved"]
["$35 ($55)","MCUCR",null,"-","PUD","SE","SM1","SM0","-","ISC01","ISC00"]
["$34 ($54)","MCUSR",null,"-","-","-","-","WDRF","BORF","EXTRF","PORF"]
["$33 ($53)","TCCR0","Timer/Counter0 Control Register","-","-","-","-","PSR0","CS02","CS01","CS00"]
["$32 ($52)","TCNT0","Timer/Counter0 (8-Bit)"]
["$31 ($51)","OSCCAL","Oscillator Calibration Register"]
["$30 ($50)","TCCR1A","Timer/Counter1 Control Register A","COM1A1","COM1A0","COM1B1","COM1B0","FOC1A","FOC1B","PWM1A","PWM1B"]
["$2F ($4F)","TCCR1B","Timer/Counter1 Control Register B","CTC1","PSR1","-","-","CS13","CS12","CS11","CS10"]
["$2E ($4E)","TCNT1","Timer/Counter1 (8-Bit)"]
["$2D ($4D)","OCR1A","Timer/Counter1 Output Compare Register A (8-Bit)"]
["$2C ($4C)","OCR1B","Timer/Counter1 Output Compare Register B (8-Bit)"]
["$2B ($4B)","OCR1C","Timer/Counter1 Output Compare Register C (8-Bit)"]
["$2A ($4A)","Reserved"]
["$29 ($49)","PLLCSR",null,"-","-","-","-","-","PCKE","PLLE","PLOCK"]
["$28 ($48)","Reserved"]
["$27 ($47)","Reserved"]
["$26 ($46)","Reserved"]
["$25 ($45)","Reserved"]
["$24 ($44)","Reserved"]
["$23 ($43)","Reserved"]
["$22 ($42)","Reserved"]
["$21 ($41)","WDTCR",null,"-","-","-","WDCE","WDE","WDP2","WDP1","WDP0"]
["$20 ($40)","Reserved"]
["$1F ($3F)","Reserved"]
["$1E ($3E)","EEAR",null,"-","EEAR6","EEAR5","EEAR4","EEAR3","EEAR2","EEAR1","EEAR0"]
["$1D ($3D)","EEDR","EEPROM Data Register (8-Bit)"]
["$1C ($3C)","EECR",null,"-","-","-","-","EERIE","EEMWE","EEWE","EERE"]
["$1B ($3B)","PORTA",null,"PORTA7","PORTA6","PORTA5","PORTA4","PORTA3","PORTA2","PORTA1","PORTA0"]
["$1A ($3A)","DDRA",null,"DDA7","DDA6","DDA5","DDA4","DDA3","DDA2","DDA1","DDA0"]
["$19 ($39)","PINA",null,"PINA7","PINA6","PINA5","PINA4","PINA3","PINA2","PINA1","PINA0"]
["$18 ($38)","PORTB",null,"PORTB7","PORTB6","PORTB5","PORTB4","PORTB3","PORTB2","PORTB1","PORTB0"]
["$17 ($37)","DDRB",null,"DDB7","DDB6","DDB5","DDB4","DDB3","DDB2","DDB1","DDB0"]
["$16 ($36)","PINB",null,"PINB7","PINB6","PINB5","PINB4","PINB3","PINB2","PINB1","PINB0"]
["$15 ($35)","Reserved"]
["$14 ($34)","Reserved"]
["$13 ($33)","Reserved"]
["$12 ($32)","Reserved"]
["$11 ($31)","Reserved"]
["$10 ($30)","Reserved"]
["$0F ($2F)","USIDR","Universal Serial Interface Data Register (8-Bit)"]
["$0E ($2E)","USISR",null,"USISIF","USIOIF","USIPF","USIDC","USICNT3","USICNT2","USICNT1","USICNT0"]
["$0D ($2D)","USICR",null,"USISIE","USIOIE","USIWM1","USIWM0","USICS1","USICS0","USICLK","USITC"]
["$0C ($2C)","Reserved"]
["$0B ($2)B","Reserved"]
["$0A ($2A)","Reserved"]
["$09 ($29)","Reserved"]
["$08 ($28)","ACSR",null,"ACD","ACBG","ACO","ACI","ACIE","ACME","ACIS1","ACIS0"]
["$07 ($27)","ADMUX",null,"REFS1","REFS0","ADLAR","MUX4","MUX3","MUX2","MUX1","MUX0"]
["$06 ($26)","ADCSR",null,"ADEN","ADSC","ADFR","ADIF","ADIE","ADPS2","ADPS1","ADPS0"]
["$05 ($25)","ADCH","ADC Data Register High Byte"]
["$04 ($24)","ADCL","ADC Data Register Low Byte"]
["$03 ($23)","Reserved"]
["$02 ($22)","Reserved"]
["$01 ($21)","Reserved"]
["$00 ($20)","Reserved"]

{"sheet":"ATtiny2313","index":1,"n_rows":68,"n_cols":11,"rows_kept":68,"flags":["formulas_cached_only"]}
[null,null,"ATtiny2313"]
[]
["Address","Name",null,"Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
[]
["0x3F (0x5F)","SREG",null,"I","T","H","S","V","N","Z","C"]
["0x3E (0x5E)","Reserved",null,"–","–","–","–","–","–","–","–"]
["0x3D (0x5D)","SPL",null,"SP7","SP6","SP5","SP4","SP3","SP2","SP1","SP0"]
["0x3C (0x5C)","OCR0B","Timer/Counter0 – Compare Register B"]
["0x3B (0x5B)","GIMSK",null,"INT1","INT0","PCIE","–","–","–","–","–"]
["0x3A (0x5A)","EIFR",null,"INTF1","INTF0","PCIF","–","–","–","–","–"]
["0x39 (0x59)","TIMSK","Timer/Counter Interrupt Mask Register","TOIE1","OCIE1A","OCIE1B","–","ICIE1","OCIE0B","TOIE0","OCIE0A"]
["0x38 (0x58)","TIFR","Timer/Counter Interrupt Flag Register","TOV1","OCF1A","OCF1B","–","ICF1","OCF0B","TOV0","OCF0A"]
["0x37 (0x57)","SPMCSR",null,"–","–","CTPB","RFLB","PGWRT","PGERS","SELFPRGEN"]
["0x36 (0x56)","OCR0A","Timer/Counter0 – Compare Register A"]
["0x35 (0x55)","MCUCR",null,"PUD","SM1","SE","SM0","ISC11","ISC10","ISC01","ISC00"]
["0x34 (0x54)","MCUSR",null,"–","–","–","–","WDRF","BORF","EXTRF","PORF"]
["0x33 (0x53)","TCCR0B","Timer/Counter0 Control Register B","FOC0A","FOC0B","–","–","WGM02","CS02","CS01","CS00"]
["0x32 (0x52)","TCNT0","Timer/Counter0 (8-bit)"]
["0x31 (0x51)","OSCCAL",null,"–","CAL6","CAL5","CAL4","CAL3","CAL2","CAL1","CAL0"]
["0x30 (0x50)","TCCR0A","Timer/Counter0 Control Register A","COM0A1","COM0A0","COM0B1","COM0B0","–","–","WGM01","WGM00"]
["0x2F (0x4F)","TCCR1A","Timer/Counter1 Control Register A","COM1A1","COM1A0","COM1B1","COM1BO","–","–","WGM11","WGM10"]
["0x2E (0x4E)","TCCR1B","Timer/Counter1 Control Register B","ICNC1","ICES1","–","WGM13","WGM12","CS12","CS11","CS10"]
["0x2D (0x4D)","TCNT1H","Timer/Counter1 – Counter Register High Byte"]
["0x2C (0x4C)","TCNT1L","Timer/Counter1 – Counter Register Low Byte"]
["0x2B (0x4B)","OCR1AH","Timer/Counter1 – Compare Register A High Byte"]
["0x2A (0x4A)","OCR1AL","Timer/Counter1 – Compare Register A Low Byte"]
["0x29 (0x49)","OCR1BH","Timer/Counter1 – Compare Register B High Byte"]
["0x28 (0x48)","OCR1BL","Timer/Counter1 – Compare Register B Low Byte"]
["0x27 (0x47)","Reserved",null,"–","–","–","–","–","–","–","–"]
["0x26 (0x46)","CLKPR",null,"CLKPCE","–","–","–","CLKPS3","CLKPS2","CLKPS1","CLKPS0"]
["0x25 (0x45)","ICR1H","Timer/Counter1 - Input Capture Register High Byte"]
["0x24 (0x44)","ICR1L","Timer/Counter1 - Input Capture Register Low Byte"]
["0x23 (0x43)","GTCCR",null,"–","–","–","–","–","–","–","PSR10"]
["0x22 (ox42)","TCCR1C","Timer/Counter1 Control Register C","FOC1A","FOC1B","–","–","–","–","–","–"]
["0x21 (0x41)","WDTCSR",null,"WDIF","WDIE","WDP3","WDCE","WDE","WDP2","WDP1","WDP0"]
["0x20 (0x40)","PCMSK",null,"PCINT7","PCINT6","PCINT5","PCINT4","PCINT3","PCINT2","PCINT1","PCINT0"]
["0x1F (0x3F)","Reserved",null,"–","–","–","–","–","–","–","–"]
["0x1E (0x3E)","EEAR",null,"–","EEPROM Address Register",16]
["0x1D (0x3D)","EEDR","EEPROM Data Register"]
["0x1C (0x3C)","EECR",null,"–","–","EEPM1","EEPM0","EERIE","EEMPE","EEPE","EERE"]
["0x1B (0x3B)","PORTA",null,"–","–","–","–","–","PORTA2","PORTA1","PORTA0"]
["0x1A (0x3A)","DDRA",null,"–","–","–","–","–","DDA2","DDA1","DDA0"]
["0x19 (0x39)","PINA",null,"–","–","–","–","–","PINA2","PINA1","PINA0"]
["0x18 (0x38)","PORTB",null,"PORTB7","PORTB6","PORTB5","PORTB4","PORTB3","PORTB2","PORTB1","PORTB0"]
["0x17 (0x37)","DDRB",null,"DDB7","DDB6","DDB5","DDB4","DDB3","DDB2","DDB1","DDB0"]
["0x16 (0x36)","PINB",null,"PINB7","PINB6","PINB5","PINB4","PINB3","PINB2","PINB1","PINB0"]
["0x15 (0x35)","GPIOR2","General Purpose I/O Register 2"]
["0x14 (0x34)","GPIOR1","General Purpose I/O Register 1"]
["0x13 (0x33)","GPIOR0","General Purpose I/O Register 0"]
["0x12 (0x32)","PORTD",null,"–","PORTD6","PORTD5","PORTD4","PORTD3","PORTD2","PORTD1","PORTD0"]
["0x11 (0x31)","DDRD",null,"–","DDD6","DDD5","DDD4","DDD3","DDD2","DDD1","DDD0"]
["0x10 (0x30)","PIND",null,"–","PIND6","PIND5","PIND4","PIND3","PIND2","PINBD1","PIND0"]
["0x0F (0x2F)","USIDR","USI Data Register"]
["0x0E (0x2E)","USISR",null,"USISIF","USIOIF","USIPF","USIDC","USICNT3","USICNT2","USICNT1","USICNT0"]
["0x0D (0x2D)","USICR",null,"USISIE","USIOIE","USIWM1","USIWM0","USICS1","USICS0","USICLK","USITC"]
["0x0C (0x2C)","UDR","UART Data Register (8-bit)"]
["0x0B (0x2B)","UCSRA",null,"RXC","TXC","UDRE","FE","DOR","UPE","U2X","MPCM"]
["0x0A (0x2A)","UCSRB",null,"RXCIE","TXCIE","UDRIE","RXEN","TXEN","UCSZ2","RXB8","TXB8"]
["0x09 (0x29)","UBRRL",null,"UBRRH[7:0]"]
["0x08 (0x28)","ACSR",null,"ACD","ACBG","ACO","ACI","ACIE","ACIC","ACIS1","ACIS0"]
["0x07 (0x27)","Reserved",null,"–","–","–","–","–","–","–","–"]
["0x06 (0x26)","Reserved",null,"–","–","–","–","–","–","–","–"]
["0x05 (0x25)","Reserved",null,"–","–","–","–","–","–","–","–"]
["0x04 (0x24)","Reserved",null,"–","–","–","–","–","–","–","–"]
["0x03 (0x23)","UCSRC",null,"–","UMSEL","UPM1","UPM0","USBS","UCSZ1","UCSZ0","UCPOL"]
["0x02 (0x22)","UBRRH",null,"–","–","–","–","UBRRH[11:8]"]
["0x01 (0x21)","DIDR",null,"–","–","–","–","–","–","AIN1D","AIN0D"]
["0x00 (0x20)","Reserved",null,"–","–","–","–","–","–","–","–"]

{"sheet":"ATtiny261_461_861","index":2,"n_rows":67,"n_cols":11,"rows_kept":67,"flags":["formulas_cached_only"]}
[null,null,"ATtiny261/461/861"]
[]
["Address","Name",null,"Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["0x3F (0x5F)","SREG",null,"I","T","H","S","V","N","Z","C"]
["0x3E (0x5E)","SPH",null,"–","–","–","–","–","SP10","SP9","SP8"]
["0x3D (0x5D)","SPL",null,"SP7","SP6","SP5","SP4","SP3","SP2","SP1","SP0"]
["0x3C (0x5C)","Reserved",null,"–"]
["0x3B (0x5B)","GIMSK",null,"INT1","INT0","PCIE1","PCIE0","–","–","–","–"]
["0x3A (0x5A)","GIFR",null,"INTF1","INTF0","PCIF","–","–","–","–","–"]
["0x39 (0x59)","TIMSK","Timer/Counter Interrupt Mask Register","OCIE1D","OCIE1A","OCIE1B","OCIE0A","OCIE0B","TOIE1","TOIE0","TICIE0"]
["0x38 (0x58)","TIFR","Timer/Counter Interrupt Flag Register","OCF1D","OCF1A","OCF1B","OCF0A","OCF0B","TOV1","TOV0","ICF0"]
["0x37 (0x57)","SPMCSR",null,"–","–","–","CTPB","RFLB","PGWRT","PGERS","SPMEN"]
["0x36 (0x56)","PRR",null,"PRTIM1","PRTIM0","PRUSI","PRADC","–","–","–","–"]
["0x35 (0x55)","MCUCR",null,"–","PUD","SE","SM1","SM0","–","ISC01","ISC00"]
["0x34 (0x54)","MCUSR",null,"–","–","–","–","WDRF","BORF","EXTRF","PORF"]
["0x33 (0x53)","TCCR0B","Timer/Counter0 Control Register B","–","–","–","TSM","PSR0","CS02","CS01","CS00"]
["0x32 (0x52)","TCNT0L"," Timer/Counter0 Counter Register Low Byte"]
["0x31 (0x51)","OSCCAL","Oscillator Calibration Register"]
["0x30 (0x50)","TCCR1A","Timer/Counter1 Control Register A","COM1A1","COM1A0","COM1B1","COM1B0","FOC1A","FOC1B","PWM1A","PWM1B"]
["0x2F (0x4F)","TCCR1B","Timer/Counter1 Control Register B","PWM1X","PSR1","DTPS11","DTPS10","CS13","CS12","CS11","CS10"]
["0x2E (0x4E)","TCNT1","Timer/Counter1 Counter Register"]
["0x2D (0x4D)","OCR1A","Timer/Counter1 Output Compare Register A"]
["0x2C (0x4C)","OCR1B","Timer/Counter1 Output Compare Register B"]
["0x2B (0x4B)","OCR1C","Timer/Counter1 Output Compare Register C"]
["0x2A (0x4A)","OCR1D","Timer/Counter1 Output Compare Register D"]
["0x29 (0x49)","PLLCSR",null,"LSM","PCKE","PLLE","PLOCK","–","–","–","–"]
["0x28 (0x48)","CLKPR",null,"CLKPCE","CLKPS3","CLKPS2","CLKPS1","CLKPS0","–","–","–"]
["0x27 (0x47)","TCCR1C","Timer/Counter1 Control Register C","COM1A1S","COM1A0S","COM1B1S","COM1B0S","COM1D1","COM1D0","FOC1D","PWM1D"]
["0x26 (0x46)","TCCR1D","Timer/Counter1 Control Register D","FPIE1","FPEN1","FPNC1","FPES1","FPAC1","FPF1","WGM11","WGM10"]
["0x25 (0x45)","TC1H","Timer/Counter1 HighByte","–","–","–","–","–","–","TC19","TC18"]
["0x24 (0x44)","DT1",null,"DT1H3","DT1H2","DT1H1","DT1H0","DT1L3","DT1L2","DT1L1","DT1L0"]
["0x23 (0x43)","PCMSK0",null,"PCINT7","PCINT6","PCINT5","PCINT4","PCINT3","PCINT2","PCINT1","PCINT0"]
["0x22 (0x42)","PCMSK1",null,"PCINT15","PCINT14","PCINT13","PCINT12","PCINT11","PCINT10","PCINT9","PCINT8"]
["0x21 (0x41)","WDTCR",null,"WDIF","WDIE","WDP3","WDCE","WDE","WDP2","WDP1","WDP0"]
["0x20 (0x40)","DWDR","debugWire Data Register"]
["0x1F (0x3F)","EEARH",{"$nulls":8},"EEAR8"]
["0x1E (0x3E)","EEARL",null,"EEAR7","EEAR6","EEAR5","EEAR4","EEAR3","EEAR2","EEAR1","EEAR0"]
["0x1D (0x3D)","EEDR","EEPROM Data Register"]
["0x1C (0x3C)","EECR",null,"–","–","EEPM1","EEPM0","EERIE","EEMPE","EEPE","EERE"]
["0x1B (0x3B)","PORTA",null,"PORTA7","PORTA6","PORTA5","PORTA4","PORTA3","PORTA2","PORTA1","PORTA0"]
["0x1A (0x3A)","DDRA",null,"DDA7","DDA6","DDA5","DDA4","DDA3","DDA2","DDA1","DDA0"]
["0x19 (0x39)","PINA",null,"PINA7","PINA6","PINA5","PINA4","PINA3","PINA2","PINA1","PINA0"]
["0x18 (0x38)","PORTB",null,"PORTB7","PORTB6","PORTB5","PORTB4","PORTB3","PORTB2","PORTB1","PORTB0"]
["0x17 (0x37)","DDRB",null,"DDB7","DDB6","DDB5","DDB4","DDB3","DDB2","DDB1","DDB0"]
["0x16 (0x36)","PINB",null,"PINB7","PINB6","PINB5","PINB4","PINB3","PINB2","PINB1","PINB0"]
["0x15 (0x35)","TCCR0A","Timer/Counter0 Control Register A","TCW0","ICEN0","ICNC0","ICES0","ACIC0","–","–","CTC0"]
["0x14 (0x34)","TCNT0H","Timer/Counter0 Counter Register High Byte"]
["0x13 (0x33)","OCR0A","Timer/Counter0 Output Compare Register A"]
["0x12 (0x32)","OCR0B","Timer/Counter0 Output Compare Register B"]
["0x11 (0x31)","USIPP","USI Pin Position","-","-","-","-","-","-","-","USIPOS"]
["0x10 (0x30)","USIBR","USI Buffer Register"]
["0x0F (0x2F)","USIDR","USI Data Register"]
["0x0E (0x2E)","USISR",null,"USISIF","USIOIF","USIPF","USIDC","USICNT3","USICNT2","USICNT1","USICNT0"]
["0x0D (0x2D)","USICR",null,"USISIE","USIOIE","USIWM1","USIWM0","USICS1","USICS0","USICLK","USITC"]
["0x0C (0x2C)","GPIOR2","General Purpose I/O Register 2"]
["0x0B (0x2B)","GPIOR1","General Purpose I/O Register 1"]
["0x0A (0x2A)","GPIOR0","General Purpose I/O Register 0"]
["0x09 (0x29)","ACSRB",null,"HSEL","HLEV","ACM2","ACM1","ACM0","-","-","-"]
["0x08 (0x28)","ACSRA",null,"ACD","ACBG","ACO","ACI","ACIE","ACME","ACIS1","ACIS0"]
["0x07 (0x27)","ADMUX",null,"REFS1","REFS0","ADLAR","MUX4","MUX3","MUX2","MUX1","MUX0"]
["0x06 (0x26)","ADCSRA",null,"ADEN","ADSC","ADATE","ADIF","ADIE","ADPS2","ADPS1","ADPS0"]
["0x05 (0x25)","ADCH","ADC Data Register High Byte"]
["0x04 (0x24)","ADCL","ADC Data Register Low Byte"]
["0x03 (0x23)","ADCSRB",null,"BIN","GSEL","REFS2","MUX5","ADTS2","ADTS1","ADTS0","-"]
["0x02 (0x22)","DIDR1",null,"ADC10D","ADC9D","ADC8D","ADC7D","-","-","-","-"]
["0x01 (0x21)","DIDR0",null,"ADC6D","ADC5D","ADC4D","ADC3D","AREFD","ADC2D","ADC1D","ADC0D"]
["0x00 (0x20)","TCCR1E","Timer/Counter1 Control Register E","–","-","OC1OE5","OC1OE4","OC1OE3","OC1OE2","OC1OE1","OC1OE0"]

{"sheet":"ATmega8A","index":3,"n_rows":68,"n_cols":11,"rows_kept":68,"flags":["formulas_cached_only"]}
[null,null,"ATmega8A"]
[]
["Address","Name",null,"Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["0x3F (0x5F)","SREG",null,"I","T","H","S","V","N","Z","C"]
["0x3E (0x5E)","SPH",null,"–","–","–","–","–","SP10","SP9","SP8"]
["0x3D (0x5D)","SPL",null,"SP7","SP6","SP5","SP4","SP3","SP2","SP1","SP0"]
["0x3C (0x5C)","Reserved"]
["0x3B (0x5B)","GICR",null,"INT1","INT0","–","–","–","–","IVSEL","IVCE"]
["0x3A (0x5A)","GIFR",null,"INTF1","INTF0","–","–","–","–","–","–"]
["0x39 (0x59)","TIMSK","Timer Interrupt Mask Register","OCIE2","TOIE2","TICIE1","OCIE1A","OCIE1B","TOIE1","–","TOIE0"]
["0x38 (0x58)","TIFR","Timer Interrupt Flag Register","OCF2","TOV2","ICF1","OCF1A","OCF1B","TOV1","–","TOV0"]
["0x37 (0x57)","SPMCR",null,"SPMIE","RWWSB","–","RWWSRE","BLBSET","PGWRT","PGERS","SPMEN"]
["0x36 (0x56)","TWCR",null,"TWINT","TWEA","TWSTA","TWSTO","TWWC","TWEN","–","TWIE"]
["0x35 (0x55)","MCUCR",null,"SE","SM2","SM1","SM0","ISC11","ISC10","ISC01","ISC00"]
["0x34 (0x54)","MCUCSR",null,"–","–","–","–","WDRF","BORF","EXTRF","PORF"]
["0x33 (0x53)","TCCR0","Timer/Counter0 Control Register","–","–","–","–","–","CS02","CS01","CS00"]
["0x32 (0x52)","TCNT0","Timer/Counter0 (8 Bits)"]
["0x31 (0x51)","OSCCAL","Oscillator Calibration Register"]
["0x30 (0x50)","SFIOR",null,"–","–","–","–","ACME","PUD","PSR2","PSR10"]
["0x2F (0x4F)","TCCR1A","Timer/Counter1 Control Register A","COM1A1","COM1A0","COM1B1","COM1B0","FOC1A","FOC1B","WGM11","WGM10"]
["0x2E (0x4E)","TCCR1B","Timer/Counter1 Control Register B","ICNC1","ICES1","–","WGM13","WGM12","CS12","CS11","CS10"]
["0x2D (0x4D)","TCNT1H","Timer/Counter1 – Counter Register High byte"]
["0x2C (0x4C)","TCNT1L","Timer/Counter1 – Counter Register Low byte"]
["0x2B (0x4B)","OCR1AH","Timer/Counter1 – Output Compare Register A High byte"]
["0x2A (0x4A)","OCR1AL","Timer/Counter1 – Output Compare Register A Low byte"]
["0x29 (0x49)","OCR1BH","Timer/Counter1 – Output Compare Register B High byte"]
["0x28 (0x48)","OCR1BL","Timer/Counter1 – Output Compare Register B Low byte"]
["0x27 (0x47)","ICR1H","Timer/Counter1 – Input Capture Register High byte"]
["0x26 (0x46)","ICR1L","Timer/Counter1 – Input Capture Register Low byte"]
["0x25 (0x45)","TCCR2","Timer/Counter2 Control Register","FOC2","WGM20","COM21","COM20","WGM21","CS22","CS21","CS20"]
["0x24 (0x44)","TCNT2","Timer/Counter2 (8 Bits)"]
["0x23 (0x43)","OCR2","Timer/Counter2 Output Compare Register"]
["0x22 (0x42)","ASSR",null,"–","–","–","–","AS2","TCN2UB","OCR2UB","TCR2UB"]
["0x21 (0x41)","WDTCR",null,"–","–","–","WDCE","WDE","WDP2","WDP1","WDP0"]
["0x20 )0x40)","UBRRH",null,"URSEL","–","–","–","UBRR[11:8]",147]
["0x20 )0x40)","UCSRC",null,"URSEL","UMSEL","UPM1","UPM0","USBS","UCSZ1","UCSZ0","UCPOL"]
["0x1F (0x3F)","EEARH",null,"–","–","–","–","–","–","–","EEAR8"]
["0x1E (0x3E)","EEARL",null,"EEAR7","EEAR6","EEAR5","EEAR4","EEAR3","EEAR2","EEAR1","EEAR0"]
["0x1D (0x3D)","EEDR"," EEPROM Data Register"]
["0x1C (0x3C)","EECR",null,"–","–","–","–","EERIE","EEMWE","EEWE","EERE"]
["0x1B (0x3B)","Reserved"]
["0x1A (0x3A)","Reserved"]
["0x19 (0x39)","Reserved"]
["0x18 (0x38)","PORTB",null,"PORTB7","PORTB6","PORTB5","PORTB4","PORTB3","PORTB2","PORTB1","PORTB0"]
["0x17 (0x37)","DDRB",null,"DDB7","DDB6","DDB5","DDB4","DDB3","DDB2","DDB1","DDB0"]
["0x16 (0x36)","PINB",null,"PINB7","PINB6","PINB5","PINB4","PINB3","PINB2","PINB1","PINB0"]
["0x15 (0x35)","PORTC",null,"–","PORTC6","PORTC5","PORTC4","PORTC3","PORTC2","PORTC1","PORTC0"]
["0x14 (0x34)","DDRC",null,"–","DDC6","DDC5","DDC4","DDC3","DDC2","DDC1","DDC0"]
["0x13 (0x33)","PINC",null,"–","PINC6","PINC5","PINC4","PINC3","PINC2","PINC1","PINC0"]
["0x12 (0x32)","PORTD",null,"PORTD7","PORTD6","PORTD5","PORTD4","PORTD3","PORTD2","PORTD1","PORTD0"]
["0x11 (0x31)","DDRD",null,"DDD7","DDD6","DDD5","DDD4","DDD3","DDD2","DDD1","DDD0"]
["0x10 (0x30)","PIND",null,"PIND7","PIND6","PIND5","PIND4","PIND3","PIND2","PIND1","PIND0"]
["0x0F (0x2F)","SPDR"," SPI Data Register"]
["0x0E (0x2E)","SPSR",null,"SPIF","WCOL","–","–","–","–","–","SPI2X"]
["0x0D (0x2D)","SPCR",null,"SPIE","SPE","DORD","MSTR","CPOL","CPHA","SPR1","SPR0"]
["0x0C (0x2C)","UDR"," USART I/O Data Register"]
["0x0B (0x2B)","UCSRA",null,"RXC","TXC","UDRE","FE","DOR","PE","U2X","MPCM"]
["0x0A (0x2A)","UCSRB",null,"RXCIE","TXCIE","UDRIE","RXEN","TXEN","UCSZ2","RXB8","TXB8"]
["0x09 (0x29)","UBRRL"," USART Baud Rate Register Low byte"]
["0x08 (0x28)","ACSR",null,"ACD","ACBG","ACO","ACI","ACIE","ACIC","ACIS1","ACIS0"]
["0x07 (0x27)","ADMUX",null,"REFS1","REFS0","ADLAR","–","MUX3","MUX2","MUX1","MUX0"]
["0x06 (0x26)","ADCSRA",null,"ADEN","ADSC","ADFR","ADIF","ADIE","ADPS2","ADPS1","ADPS0"]
["0x05 (0x25)","ADCH","ADC Data Register High byte"]
["0x04 (0x24)","ADCL","ADC Data Register Low byte"]
["0x03 (0x23)","TWDR","Two-wire Serial Interface Data Register"]
["0x02 (0x22)","TWAR",null,"TWA6","TWA5","TWA4","TWA3","TWA2","TWA1","TWA0","TWGCE"]
["0x01 (0x21)","TWSR",null,"TWS7","TWS6","TWS5","TWS4","TWS3","–","TWPS1","TWPS0"]
["0x00 (0x20)","TWBR","Two-wire Serial Interface Bit Rate Register"]

{"sheet":"ATmega16","index":4,"n_rows":70,"n_cols":11,"rows_kept":70,"flags":["formulas_cached_only"]}
[null,null,"ATmega16(L)"]
[]
["Address","Name","Beschreibung","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["$3F ($5F)","SREG",null,"I","T","H","S","V","N","Z","C"]
["$3E ($5E)","SPH",null,"–","–","–","–","–","SP10","SP9","SP8"]
["$3D ($5D)","SPL",null,"SP7","SP6","SP5","SP4","SP3","SP2","SP1","SP0"]
["$3C ($5C)","OCR0","Timer/Counter0 Output Compare Register","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["$3B ($5B)","GICR",null,"INT1","INT0","INT2","–","–","–","IVSEL","IVCE"]
["$3A ($5A)","GIFR",null,"INTF1","INTF0","INTF2","–","–","–","–","–"]
["$39 ($59)","TIMSK","Timer/Counter Interrupt Mask Register","OCIE2","TOIE2","TICIE1","OCIE1A","OCIE1B","TOIE1","OCIE0","TOIE0"]
["$38 ($58)","TIFR","Timer/CounterInterrupt Flag Register","OCF2","TOV2","ICF1","OCF1A","OCF1B","TOV1","OCF0","TOV0"]
["$37 ($57)","SPMCR",null,"SPMIE","RWWSB","–","RWWSRE","BLBSET","PGWRT","PGERS","SPMEN"]
["$36 ($56)","TWCR",null,"TWINT","TWEA","TWSTA","TWSTO","TWWC","TWEN","–","TWIE"]
["$35 ($55)","MCUCR",null,"SM2","SE","SM1","SM0","ISC11","ISC10","ISC01","ISC00"]
["$34 ($54)","MCUCSR",null,"JTD","ISC2","–","JTRF","WDRF","BORF","EXTRF","PORF"]
["$33 ($53)","TCCR0","Timer/Counter0 – Control  Register","FOC0","WGM00","COM01","COM00","WGM01","CS02","CS01","CS00"]
["$32 ($52)","TCNT0","Timer/Counter0 (8 Bits)","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["$31 ($51)","OSCCAL","Oscillator Calibration Register","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["$31 ($51)","OCDR","On-Chip Debug Register","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["$30 ($50)","SFIOR",null,"ADTS2","ADTS1","ADTS0","–","ACME","PUD","PSR2","PSR10"]
["$2F ($4F)","TCCR1A","Timer/Counter1 – Control  Register A","COM1A1","COM1A0","COM1B1","COM1B0","FOC1A","FOC1B","WGM11","WGM10"]
["$2E ($4E)","TCCR1B","Timer/Counter1 – Control  Register B","ICNC1","ICES1","–","WGM13","WGM12","CS12","CS11","CS10"]
["$2D ($4D)","TCNT1H","Timer/Counter1 – Counter Register High Byte","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["$2C ($4C)","TCNT1L","Timer/Counter1 – Counter Register Low Byte","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["$2B ($4B)","OCR1AH","Timer/Counter1 – Output Compare Register A High Byte","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["$2A ($4A)","OCR1AL","Timer/Counter1 – Output Compare Register A Low Byte","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["$29 ($49)","OCR1BH","Timer/Counter1 – Output Compare Register B High Byte","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["$28 ($48)","OCR1BL","Timer/Counter1 – Output Compare Register B Low Byte","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["$27 ($47)","ICR1H","Timer/Counter1 – Input Capture Register High Byte","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["$26 ($46)","ICR1L","Timer/Counter1 – Input Capture Register Low Byte","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["$25 ($45)","TCCR2","Timer/Counter2 – Control  Register","FOC2","WGM20","COM21","COM20","WGM21","CS22","CS21","CS20"]
["$24 ($44)","TCNT2","Timer/Counter2 (8 Bits)","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["$23 ($43)","OCR2","Timer/Counter2 Output Compare Register","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["$22 ($42)","ASSR",null,"–","–","–","–","AS2","TCN2UB","OCR2UB","TCR2UB"]
["$21 ($41)","WDTCR",null,"–","–","–","WDTOE","WDE","WDP2","WDP1","WDP0"]
["$20 ($40)","UBRRH",null,"URSEL","–","–","–","UBRR.11","UBRR.10","UBRR.9","UBRR.8"]
["$20 ($40)","UCSRC",null,"URSEL","UMSEL","UPM1","UPM0","USBS","UCSZ1","UCSZ0","UCPOL"]
["$1F ($3F)","EEARH",null,"–","–","–","–","–","–","–","EEAR8"]
["$1E ($3E)","EEARL","EEPROM Address Register Low Byte","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["$1D ($3D)","EEDR","EEPROM Data Register","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["$1C ($3C)","EECR",null,"–","–","–","–","EERIE","EEMWE","EEWE","EERE"]
["$1B ($3B)","PORTA",null,"PORTA7","PORTA6","PORTA5","PORTA4","PORTA3","PORTA2","PORTA1","PORTA0"]
["$1A ($3A)","DDRA",null,"DDA7","DDA6","DDA5","DDA4","DDA3","DDA2","DDA1","DDA0"]
["$19 ($39)","PINA",null,"PINA7","PINA6","PINA5","PINA4","PINA3","PINA2","PINA1","PINA0"]
["$18 ($38)","PORTB",null,"PORTB7","PORTB6","PORTB5","PORTB4","PORTB3","PORTB2","PORTB1","PORTB0"]
["$17 ($37)","DDRB",null,"DDB7","DDB6","DDB5","DDB4","DDB3","DDB2","DDB1","DDB0"]
["$16 ($36)","PINB",null,"PINB7","PINB6","PINB5","PINB4","PINB3","PINB2","PINB1","PINB0"]
["$15 ($35)","PORTC",null,"PORTC7","PORTC6","PORTC5","PORTC4","PORTC3","PORTC2","PORTC1","PORTC0"]
["$14 ($34)","DDRC",null,"DDC7","DDC6","DDC5","DDC4","DDC3","DDC2","DDC1","DDC0"]
["$13 ($33)","PINC",null,"PINC7","PINC6","PINC5","PINC4","PINC3","PINC2","PINC1","PINC0"]
["$12 ($32)","PORTD",null,"PORTD7","PORTD6","PORTD5","PORTD4","PORTD3","PORTD2","PORTD1","PORTD0"]
["$11 ($31)","DDRD",null,"DDD7","DDD6","DDD5","DDD4","DDD3","DDD2","DDD1","DDD0"]
["$10 ($30)","PIND",null,"PIND7","PIND6","PIND5","PIND4","PIND3","PIND2","PIND1","PIND0"]
["$0F ($2F)","SPDR"," SPI Data Register","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["$0E ($2E)","SPSR",null,"SPIF","WCOL","–","–","–","–","–","SPI2X"]
["$0D ($2D)","SPCR",null,"SPIE","SPE","DORD","MSTR","CPOL","CPHA","SPR1","SPR0"]
["$0C ($2C)","UDR"," USART I/O Data Register","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["$0B ($2B)","UCSRA",null,"RXC","TXC","UDRE","FE","DOR","PE","U2X","MPCM"]
["$0A ($2A)","UCSRB",null,"RXCIE","TXCIE","UDRIE","RXEN","TXEN","UCSZ2","RXB8","TXB8"]
["$09 ($29)","UBRRL"," USART Baud Rate Register Low Byte","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["$08 ($28)","ACSR",null,"ACD","ACBG","ACO","ACI","ACIE","ACIC","ACIS1","ACIS0"]
["$07 ($27)","ADMUX",null,"REFS1","REFS0","ADLAR","MUX4","MUX3","MUX2","MUX1","MUX0"]
["$06 ($26)","ADCSRA",null,"ADEN","ADSC","ADATE","ADIF","ADIE","ADPS2","ADPS1","ADPS0"]
["$05 ($25)","ADCH","ADC Data Register High Byte","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["$04 ($24)","ADCL","ADC Data Register Low Byte","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["$03 ($23)","TWDR","Two-wire Serial Interface Data Register","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["$02 ($22)","TWAR",null,"TWA6","TWA5","TWA4","TWA3","TWA2","TWA1","TWA0","TWGCE"]
["$01 ($21)","TWSR",null,"TWS7","TWS6","TWS5",null,"TWS4","TWS3","TWPS1","TWPS0"]
["$00 ($20)","TWBR","Two-wire Serial Interface Bit Rate Register","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
[" "]

{"sheet":"ATmega32A","index":5,"n_rows":70,"n_cols":11,"rows_kept":70,"flags":["formulas_cached_only"]}
[null,null,"ATmega32A"]
[]
["Address","Name","Description","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["$3F ($5F)","SREG",null,"I","T","H","S","V","N","Z","C"]
["$3E ($5E)","SPH",null,"–","–","–","–","SP11","SP10","SP9","SP8"]
["$3D ($5D)","SPL",null,"SP7","SP6","SP5","SP4","SP3","SP2","SP1","SP0"]
["$3C ($5C)","OCR0","Timer/Counter0 Output Compare Register"]
["$3B ($5B)","GICR",null,"INT1","INT0","INT2","–","–","–","IVSEL","IVCE"]
["$3A ($5A)","GIFR",null,"INTF1","INTF0","INTF2","–","–","–","–","–"]
["$39 ($59)","TIMSK","Timer/Counter Interrupt Mask Register","OCIE2","TOIE2","TICIE1","OCIE1A","OCIE1B","TOIE1","OCIE0","TOIE0"]
["$38 ($58)","TIFR","Timer/CounterInterrupt Flag Register","OCF2","TOV2","ICF1","OCF1A","OCF1B","TOV1","OCF0","TOV0"]
["$37 ($57)","SPMCR",null,"SPMIE","RWWSB","–","RWWSRE","BLBSET","PGWRT","PGERS","SPMEN"]
["$36 ($56)","TWCR",null,"TWINT","TWEA","TWSTA","TWSTO","TWWC","TWEN","–","TWIE"]
["$35 ($55)","MCUCR",null,"SE","SM2","SM1","SM0","ISC11","ISC10","ISC01","ISC00"]
["$34 ($54)","MCUCSR",null,"JTD","ISC2","–","JTRF","WDRF","BORF","EXTRF","PORF"]
["$33 ($53)","TCCR0","Timer/Counter0 – Control  Register ","FOC0","WGM00","COM01","COM00","WGM01","CS02","CS01","CS00"]
["$32 ($52)","TCNT0","Timer/Counter0 (8 Bits)"]
["$31 ($51)","OSCCAL","Oscillator Calibration Register"]
["$31 ($51)","OCDR","On-Chip Debug Register"]
["$30 ($50)","SFIOR",null,"ADTS2","ADTS1","ADTS0","–","ACME","PUD","PSR2","PSR10"]
["$2F ($4F)","TCCR1A","Timer/Counter1 – Control  Register A","COM1A1","COM1A0","COM1B1","COM1B0","FOC1A","FOC1B","WGM11","WGM10"]
["$2E ($4E)","TCCR1B","Timer/Counter1 – Control  Register B","ICNC1","ICES1","–","WGM13","WGM12","CS12","CS11","CS10"]
["$2D ($4D)","TCNT1H","Timer/Counter1 – Counter Register High Byte"]
["$2C ($4C)","TCNT1L","Timer/Counter1 – Counter Register Low Byte"]
["$2B ($4B)","OCR1AH","Timer/Counter1 – Output Compare Register A High Byte"]
["$2A ($4A)","OCR1AL","Timer/Counter1 – Output Compare Register A Low Byte"]
["$29 ($49)","OCR1BH","Timer/Counter1 – Output Compare Register B High Byte"]
["$28 ($48)","OCR1BL","Timer/Counter1 – Output Compare Register B Low Byte"]
["$27 ($47)","ICR1H","Timer/Counter1 – Input Capture Register High Byte"]
["$26 ($46)","ICR1L","Timer/Counter1 – Input Capture Register Low Byte"]
["$25 ($45)","TCCR2","Timer/Counter2 – Control  Register ","FOC2","WGM20","COM21","COM20","WGM21","CS22","CS21","CS20"]
["$24 ($44)","TCNT2","Timer/Counter2 (8 Bits)"]
["$23 ($43)","OCR2","Timer/Counter2 Output Compare Register"]
["$22 ($42)","ASSR",null,"–","–","–","–","AS2","TCN2UB","OCR2UB","TCR2UB"]
["$21 ($41)","WDTCR",null,"–","–","–","WDTOE","WDE","WDP2","WDP1","WDP0"]
["$20 ($40)","UBRRH",null,"URSEL","–","–","–","UBRR[11:8]",171]
["$20 ($40)","UCSRC",null,"URSEL","UMSEL","UPM1","UPM0","USBS","UCSZ1","UCSZ0","UCPOL"]
["$1F ($3F)","EEARH",null,"–","–","–","–","–","–","EEAR9","EEAR8"]
["$1E ($3E)","EEARL","EEPROM Address Register Low Byte"]
["$1D ($3D)","EEDR","EEPROM Data Register"]
["$1C ($3C)","EECR",null,"–","–","–","–","EERIE","EEMWE","EEWE","EERE"]
["$1B ($3B)","PORTA",null,"PORTA7","PORTA6","PORTA5","PORTA4","PORTA3","PORTA2","PORTA1","PORTA0"]
["$1A ($3A)","DDRA",null,"DDA7","DDA6","DDA5","DDA4","DDA3","DDA2","DDA1","DDA0"]
["$19 ($39)","PINA",null,"PINA7","PINA6","PINA5","PINA4","PINA3","PINA2","PINA1","PINA0"]
["$18 ($38)","PORTB",null,"PORTB7","PORTB6","PORTB5","PORTB4","PORTB3","PORTB2","PORTB1","PORTB0"]
["$17 ($37)","DDRB",null,"DDB7","DDB6","DDB5","DDB4","DDB3","DDB2","DDB1","DDB0"]
["$16 ($36)","PINB",null,"PINB7","PINB6","PINB5","PINB4","PINB3","PINB2","PINB1","PINB0"]
["$15 ($35)","PORTC",null,"PORTC7","PORTC6","PORTC5","PORTC4","PORTC3","PORTC2","PORTC1","PORTC0"]
["$14 ($34)","DDRC",null,"DDC7","DDC6","DDC5","DDC4","DDC3","DDC2","DDC1","DDC0"]
["$13 ($33)","PINC",null,"PINC7","PINC6","PINC5","PINC4","PINC3","PINC2","PINC1","PINC0"]
["$12 ($32)","PORTD",null,"PORTD7","PORTD6","PORTD5","PORTD4","PORTD3","PORTD2","PORTD1","PORTD0"]
["$11 ($31)","DDRD",null,"DDD7","DDD6","DDD5","DDD4","DDD3","DDD2","DDD1","DDD0"]
["$10 ($30)","PIND",null,"PIND7","PIND6","PIND5","PIND4","PIND3","PIND2","PIND1","PIND0"]
["$0F ($2F)","SPDR"," SPI Data Register"]
["$0E ($2E)","SPSR",null,"SPIF","WCOL","–","–","–","–","–","SPI2X"]
["$0D ($2D)","SPCR",null,"SPIE","SPE","DORD","MSTR","CPOL","CPHA","SPR1","SPR0"]
["$0C ($2C)","UDR"," USART I/O Data Register"]
["$0B ($2B)","UCSRA",null,"RXC","TXC","UDRE","FE","DOR","PE","U2X","MPCM"]
["$0A ($2A)","UCSRB",null,"RXCIE","TXCIE","UDRIE","RXEN","TXEN","UCSZ2","RXB8","TXB8"]
["$09 ($29)","UBRRL"," USART Baud Rate Register Low Byte"]
["$08 ($28)","ACSR",null,"ACD","ACBG","ACO","ACI","ACIE","ACIC","ACIS1","ACIS0"]
["$07 ($27)","ADMUX",null,"REFS1","REFS0","ADLAR","MUX4","MUX3","MUX2","MUX1","MUX0"]
["$06 ($26)","ADCSRA",null,"ADEN","ADSC","ADATE","ADIF","ADIE","ADPS2","ADPS1","ADPS0"]
["$05 ($25)","ADCH","ADC Data Register High Byte"]
["$04 ($24)","ADCL","ADC Data Register Low Byte"]
["$03 ($23)","TWDR","Two-wire Serial Interface Data Register"]
["$02 ($22)","TWAR",null,"TWA6","TWA5","TWA4","TWA3","TWA2","TWA1","TWA0","TWGCE"]
["TWS6","TWS5",null,"TWS4","TWS3","TWPS1","TWPS0"]
["$01 ($21)","TWSR",null,"TWS7","–","–","–","–","–","–","–"]
["$00 ($20)","TWBR","Two-wire Serial Interface Bit Rate Register"]

{"sheet":"ATmega64","index":6,"n_rows":132,"n_cols":11,"rows_kept":132,"flags":["formulas_cached_only"]}
[null,null,"ATmega64(L)"]
[]
["Address","Name",null,"Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["(0xFF)","Reserved",null,"–","–","–","–","–","–","–","–"]
["..","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x9E)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x9D)","UCSR1C",null,"–","UMSEL1","UPM11","UPM10","USBS1","UCSZ11","UCSZ10","UCPOL1"]
["(0x9C)","UDR1","USART1 I/O Data Register"]
["(0x9B)","UCSR1A",null,"RXC1","TXC1","UDRE1","FE1","DOR1","UPE1","U2X1","MPCM1"]
["(0x9A)","UCSR1B",null,"RXCIE1","TXCIE1","UDRIE1","RXEN1","TXEN1","UCSZ12","RXB81","TXB81"]
["(0x99)","UBRR1L","USART1 Baud Rate Register Low"]
["(0x98)","UBRR1H","USART1 Baud Rate Register High","–","–","–","–"]
["(0x97)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x96)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x95)","UCSR0C",null,"–","UMSEL0","UPM01","UPM00","USBS0","UCSZ01","UCSZ00","UCPOL0"]
["(0x94)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x93)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x92)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x91)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x90)","UBRR0H","USART0 Baud Rate Register High Byte","–","–","–","–"]
["(0x8F)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x8E)","ADCSRB",null,"–","–","–","–","–","ADTS2","ADTS1","ADTS0"]
["(0x8D)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x8C)","TCCR3C","Timer/Counter3 Control Register C","FOC3A","FOC3B","FOC3C","–","–","–","–","–"]
["(0x8B)","TCCR3A","Timer/Counter3 Control Register A","COM3A1","COM3A0","COM3B1","COM3B0","COM3C1","COM3C0","WGM31","WGM30"]
[" (0x8A)","TCCR3B","Timer/Counter3 Control Register B","ICNC3","ICES3","–","WGM33","WGM32","CS32","CS31","CS30"]
["(0x89)","TCNT3H","Timer/Counter3 – Counter Register High Byte"]
[" (0x88)","TCNT3L","Timer/Counter3 – Counter Register Low Byte"]
[" (0x87)","OCR3AH","Timer/Counter3 – Output Compare Register A High Byte"]
["(0x86)","OCR3AL","Timer/Counter3 – Output Compare Register A Low Byte"]
["(0x85)","OCR3BH","Timer/Counter3 – Output Compare Register B High Byte"]
["(0x84)","OCR3BL","Timer/Counter3 – Output Compare Register B Low Byte"]
["(0x83)","OCR3CH","Timer/Counter3 – Output Compare Register C High Byte"]
["(0x82)","OCR3CL","Timer/Counter3 – Output Compare Register C Low Byte"]
["(0x81)","ICR3H","Timer/Counter3 – Input Capture Register High Byte"]
["(0x80)","ICR3L","Timer/Counter3 – Input Capture Register Low Byte"]
["(0x7F)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x7E)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x7D)","ETIMSK",null,"–","–","TICIE3","OCIE3A","OCIE3B","TOIE3","OCIE3C","OCIE1C"]
[" (0x7C)","ETIFR",null,"–","–","ICF3","OCF3A","OCF3B","TOV3","OCF3C","OCF1C"]
["(0x7B)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x7A)","TCCR1C","Timer/Counter1 Control Register C","FOC1A","FOC1B","FOC1C","–","–","–","–","–"]
["(0x79)","OCR1CH","Timer/Counter1 – Output Compare Register C High Byte"]
["(0x78)","OCR1CL","Timer/Counter1 – Output Compare Register C Low Byte"]
["(0x77)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x76)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x75)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x74)","TWCR",null,"TWINT","TWEA","TWSTA","TWSTO","TWWC","TWEN","–","TWIE"]
["(0x73)","TWDR"," Two-wire Serial Interface Data Register"]
["(0x72)","TWAR",null,"TWA6","TWA5","TWA4","TWA3","TWA2","TWA1","TWA0","TWGCE"]
["(0x71)","TWSR",null,"TWS7","TWS6","TWS5","TWS4","TWS3","–","TWPS1","TWPS0"]
["(0x70)","TWBR","Two-wire Serial Interface Bit Rate Register"]
["(0x6F)","OSCCAL","Oscillator Calibration Register"]
["(0x6E)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x6D)","XMCRA",null,"–","SRL2","SRL1","SRL0","SRW01","SRW00","SRW11",32]
["(0x6C)","XMCRB",null,"XMBK","–","–","–","–","XMM2","XMM1","XMM0"]
["(0x6B)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x6A)","EICRA",null,"ISC31","ISC30","ISC21","ISC20","ISC11","ISC10","ISC01","ISC00"]
["(0x69)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x68)","SPMCSR",null,"SPMIE","RWWSB","–","RWWSRE","BLBSET","PGWRT","PGERS","SPMEN"]
["(0x67)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x66)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x65)","PORTG",null,"–","–","–","PORTG4","PORTG3","PORTG2","PORTG1","PORTG0"]
["(0x64)","DDRG",null,"–","–","–","DDG4","DDG3","DDG2","DDG1","DDG0"]
["(0x63)","PING",null,"–","–","–","PING4","PING3","PING2","PING1","PING0"]
["(0x62)","PORTF",null,"PORTF7","PORTF6","PORTF5","PORTF4","PORTF3","PORTF2","PORTF1","PORTF0"]
["(0x61)","DDRF",null,"DDF7","DDF6","DDF5","DDF4","DDF3","DDF2","DDF1","DDF0"]
["(0x60)","Reserved",null,"–","–","–","–","–","–","–","–"]
["0x3F (0x5F)","SREG",null,"I","T","H","S","V","N","Z","C"]
["0x3E (0x5E)","SPH",null,"SP15","SP14","SP13","SP12","SP11","SP10","SP9","SP8"]
["0x3D (0x5D)","SPL",null,"SP7","SP6","SP5","SP4","SP3","SP2","SP1","SP0"]
["0x3C (0x5C)","XDIV",null,"XDIVEN","XDIV6","XDIV5","XDIV4","XDIV3","XDIV2","XDIV1","XDIV0"]
["0x3B (0x5B)","Reserved",null,"–","–","–","–","–","–","–","–"]
["0x3A (0x5A)","EICRB",null,"ISC71","ISC70","ISC61","ISC60","ISC51","ISC50","ISC41","ISC40"]
["0x39 (0x59)","EIMSK",null,"INT7","INT6","INT5","INT4","INT3","INT2","INT1","INT0"]
["0x38 (0x58)","EIFR",null,"INTF7","INTF6","INTF5","INTF4","INTF3","INTF","INTF1","INTF0"]
["0x37 (0x57)","TIMSK","Timer/Counter Interrupt Mask Register","OCIE2","TOIE2","TICIE1","OCIE1A","OCIE1B","TOIE1","OCIE0","TOIE0"]
["0x36 (0x56)","TIFR","Timer/Counter Interrupt Flag Register","OCF2","TOV2","ICF1","OCF1A","OCF1B","TOV1","OCF0","TOV0"]
["0x35 (0x55)","MCUCR",null,"SRE","SRW10","SE","SM1","SM0","SM2","IVSEL","IVCE"]
["0x34 (0x54)","MCUCSR",null,"JTD","–","–","JTRF","WDRF","BORF","EXTRF","PORF"]
["0x33 (0x53)","TCCR0","Timer/Counter0 Control Register","FOC0","WGM00","COM01","COM00","WGM01","CS02","CS01","CS00"]
["0x32 (0x52)","TCNT0","Timer/Counter0 (8 Bit)"]
["0x31 (0x51)","OCR0","Timer/Counter0 Output Compare Register"]
["0x30 (0x50)","ASSR",null,"–","–","–","–","AS0","TCN0UB","OCR0UB","TCR0UB"]
["0x2F (0x4F)","TCCR1A","Timer/Counter1 Control Register A","COM1A1","COM1A0","COM1B1","COM1B0","COM1C1","COM1C0","WGM11","WGM10"]
["0x2E (0x4E)","TCCR1B","Timer/Counter1 Control Register B","ICNC1","ICES1","–","WGM13","WGM12","CS12","CS11","CS10"]
["0x2D (0x4D)","TCNT1H","Timer/Counter1 – Counter Register High Byte"]
["0x2C (0x4C)","TCNT1L","Timer/Counter1 – Counter Register Low Byte"]
["0x2B (0x4B)","OCR1AH","Timer/Counter1 – Output Compare Register A High Byte"]
["0x2A (0x4A)","OCR1AL","Timer/Counter1 – Output Compare Register A Low Byte"]
["0x29 (0x49)","OCR1BH","Timer/Counter1 – Output Compare Register B High Byte"]
["0x28 (0x48)","OCR1BL","Timer/Counter1 – Output Compare Register B Low Byte"]
["0x27 (0x47)","ICR1H","Timer/Counter1 – Input Capture Register High Byte"]
["0x26 (0x46)","ICR1L","Timer/Counter1 – Input Capture Register Low Byte"]
["0x25 (0x45)","TCCR2","Timer/Counter2 Control Register","FOC2","WGM20","COM21","COM20","WGM21","CS22","CS21","CS20"]
["0x24 (0x44)","TCNT2","Timer/Counter2 (8 Bit)"]
["0x23 (0x43)","OCR2","Timer/Counter2 Output Compare Register"]
["0x22 (0x42)","OCDR",null,"IDRD/OCDR7 ","OCDR6","OCDR5","OCDR4","OCDR3","OCDR2","OCDR1","OCDR0"]
["0x21 (0x41)","WDTCR",null,"–","–","–","WDCE","WDE","WDP2","WDP1","WDP0"]
["0x20 (0x40)","SFIOR",null,"TSM","–","–","–","ACME","PUD","PSR0","PSR321"]
["0x1F (0x3F)","EEARH","EEPROM Address Register High Byte","–","–","–","–","–"]
["0x1E (0x3E)","EEARL","EEPROM Address Register Low Byte"]
["0x1D (0x3D)","EEDR","EEPROM Data Register"]
["0x1C (0x3C)","EECR",null,"–","–","–","–","EERIE","EEMWE","EEWE","EERE"]
["0x1B (0x3B)","PORTA",null,"PORTA7","PORTA6","PORTA5","PORTA4","PORTA3","PORTA2","PORTA1","PORTA0"]
["0x1A (0x3A)","DDRA",null,"DDA7","DDA6","DDA5","DDA4","DDA3","DDA2","DDA1","DDA0"]
["0x19 (0x39)","PINA",null,"PINA7","PINA6","PINA5","PINA4","PINA3","PINA2","PINA1","PINA0"]
["0x18 (0x38)","PORTB",null,"PORTB7","PORTB6","PORTB5","PORTB4","PORTB3","PORTB2","PORTB1","PORTB0"]
["0x17 (0x37)","DDRB",null,"DDB7","DDB6","DDB5","DDB4","DDB3","DDB2","DDB1","DDB0"]
["0x16 (0x36)","PINB",null,"PINB7","PINB6","PINB5","PINB4","PINB3","PINB2","PINB1","PINB0"]
["0x15 (0x35)","PORTC",null,"PORTC7","PORTC6","PORTC5","PORTC4","PORTC3","PORTC2","PORTC1","PORTC0"]
["0x14 (0x34)","DDRC",null,"DDC7","DDC6","DDC5","DDC4","DDC3","DDC2","DDC1","DDC0"]
["0x13 (0x33)","PINC",null,"PINC7","PINC6","PINC5","PINC4","PINC3","PINC2","PINC1","PINC0"]
["0x12 (0x32)","PORTD",null,"PORTD7","PORTD6","PORTD5","PORTD4","PORTD3","PORTD2","PORTD1","PORTD0"]
["0x11 (0x31)","DDRD",null,"DDD7","DDD6","DDD5","DDD4","DDD3","DDD2","DDD1","DDD0"]
["0x10 (0x30)","PIND",null,"PIND7","PIND6","PIND5","PIND4","PIND3","PIND2","PIND1","PIND0"]
["0x0F (0x2F)","SPDR"," SPI Data Register"]
["0x0E (0x2E)","SPSR",null,"SPIF","WCOL","–","–","–","–","–","SPI2X"]
["0x0D (0x2D)","SPCR",null,"SPIE","SPE","DORD","MSTR","CPOL","CPHA","SPR1","SPR0"]
["0x0C (0x2C)","UDR0"," USART0 I/O Data Register"]
["0x0B (0x2B)","UCSR0A",null,"RXC0","TXC0","UDRE0","FE0","DOR0","UPE0","U2X0","MPCM0"]
["0x0A (0x2A)","UCSR0B",null,"RXCIE0","TXCIE0","UDRIE0","RXEN0","TXEN0","UCSZ02","RXB80","TXB80"]
["0x09 (0x29)","UBRR0L"," USART0 Baud Rate Register Low Byte"]
["0x08 (0x28)","ACSR",null,"ACD","ACBG","ACO","ACI","ACIE","ACIC","ACIS1","ACIS0"]
["0x07 (0x27)","ADMUX",null,"REFS1","REFS0","ADLAR","MUX4","MUX3","MUX2","MUX1","MUX0"]
["0x06 (0x26)","ADCSRA",null,"ADEN","ADSC","ADATE","ADIF","ADIE","ADPS2","ADPS1","ADPS0"]
["0x05 (0x25)","ADCH","ADC Data Register High Byte"]
["0x04 (0x24)","ADCL","ADC Data Register Low byte"]
["0x03 (0x23)","PORTE",null,"PORTE7","PORTE6","PORTE5","PORTE4","PORTE3","PORTE2","PORTE1","PORTE0"]
["0x02 (0x22)","DDRE",null,"DDE7","DDE6","DDE5","DDE4","DDE3","DDE2","DDE1","DDE0"]
["0x01 (0x21)","PINE",null,"PINE7","PINE6","PINE5","PINE4","PINE3","PINE2","PINE1","PINE0"]
["0x00 (0x20)","PINF",null,"PINF7","PINF6","PINF5","PINF4","PINF3","PINF2","PINF1","PINF0"]

{"sheet":"ATmega_48_88_168_328","index":7,"n_rows":227,"n_cols":11,"rows_kept":227,"flags":["formulas_cached_only"]}
[null,null,"ATmega48A-48PA-88A-88PA-168A-168PA-328-328P"]
[]
["Address","Name",null,"Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["(0xFF)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xFE)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xFD)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xFC)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xFB)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xFA)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xF9)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xF8)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xF7)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xF6)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xF5)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xF4)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xF3)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xF2)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xF1)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xF0)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xEF)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xEE)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xED)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xEC)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xEB)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xEA)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xE9)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xE8)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xE7)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xE6)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xE5)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xE4)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xE3)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xE2)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xE1)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xE0)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xDF)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xDE)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xDD)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xDC)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xDB)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xDA)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xD9)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xD8)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xD7)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xD6)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xD5)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xD4)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xD3)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xD2)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xD1)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xD0)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xCF)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xCE)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xCD)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xCC)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xCB)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xCA)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xC9)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xC8)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xC7)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xC6)","UDR0","USART I/O Data Register"]
["(0xC5)","UBRR0H","USART Baud Rate Register High"]
["(0xC4)","UBRR0L","USART Baud Rate Register Low"]
["(0xC3)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xC2)","UCSR0C",null,"UMSEL01","UMSEL00","UPM01","UPM00","USBS0","UCSZ01 /UDORD0","UCSZ00 / UCPHA0","UCPOL0"]
["(0xC1)","UCSR0B",null,"RXCIE0","TXCIE0","UDRIE0","RXEN0","TXEN0","UCSZ02","RXB80","TXB80"]
["(0xC0)","UCSR0A",null,"RXC0","TXC0","UDRE0","FE0","DOR0","UPE0","U2X0","MPCM0"]
["(0xBF)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xBE)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xBD)","TWAMR",null,"TWAM6","TWAM5","TWAM4","TWAM3","TWAM2","TWAM1","TWAM0","–"]
["(0xBC)","TWCR",null,"TWINT","TWEA","TWSTA","TWSTO","TWWC","TWEN","–","TWIE"]
["(0xBB)","TWDR"," 2-wire Serial Interface Data Register"]
["(0xBA)","TWAR",null,"TWA6","TWA5","TWA4","TWA3","TWA2","TWA1","TWA0","TWGCE"]
["(0xB9)","TWSR",null,"TWS7","TWS6","TWS5","TWS4","TWS3","–","TWPS1","TWPS0"]
["(0xB8)","TWBR"," 2-wire Serial Interface Bit Rate Register"]
["(0xB7)","Reserved",null,"–","–","–","–","–","–","–"]
["(0xB6)","ASSR",null,"–","EXCLK","AS2","TCN2UB","OCR2AUB","OCR2BUB","TCR2AUB","TCR2BUB"]
["(0xB5)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xB4)","OCR2B","Timer/Counter2 Output Compare Register B"]
["(0xB3)","OCR2A","Timer/Counter2 Output Compare Register A"]
["(0xB2)","TCNT2","Timer/Counter2 (8-bit)"]
["(0xB1)","TCCR2B","Timer/Counter2 – Control  Register B","FOC2A","FOC2B","–","–","WGM22","CS22","CS21","CS20"]
["(0xB0)","TCCR2A","Timer/Counter2 – Control  Register A","COM2A1","COM2A0","COM2B1","COM2B0","–","–","WGM21","WGM20"]
["(0xAF)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xAE)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xAD)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xAC)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xAB)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xAA)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xA9)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xA8)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xA7)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xA6)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xA5)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xA4)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xA3)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xA2)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xA1)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0xA0)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x9F)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x9E)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x9D)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x9C)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x9B)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x9A)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x99)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x98)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x97)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x96)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x95)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x94)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x93)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x92)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x91)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x90)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x8F)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x8E)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x8D)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x8C)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x8B)","OCR1BH","Timer/Counter1 - Output Compare Register B High Byte"]
[" (0x8A)","OCR1BL","Timer/Counter1 - Output Compare Register B Low Byte"]
["(0x89)","OCR1AH","Timer/Counter1 - Output Compare Register A High Byte"]
["(0x88)","OCR1AL","Timer/Counter1 - Output Compare Register A Low Byte"]
["(0x87)","ICR1H","Timer/Counter1 - Input Capture Register High Byte"]
["(0x86)","ICR1L","Timer/Counter1 - Input Capture Register Low Byte"]
["(0x85)","TCNT1H","Timer/Counter1 - Counter Register High Byte"]
["(0x84)","TCNT1L","Timer/Counter1 - Counter Register Low Byte"]
["(0x83)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x82)","TCCR1C","Timer/Counter1 – Control  Register C","FOC1A","FOC1B","–","–","–","–","–","–"]
["(0x81)","TCCR1B","Timer/Counter1 – Control  Register B","ICNC1","ICES1","–","WGM13","WGM12","CS12","CS11","CS10"]
["(0x80)","TCCR1A","Timer/Counter1 – Control  Register A","COM1A1","COM1A0","COM1B1","COM1B0","–","–","WGM11","WGM10"]
["(0x7F)","DIDR1",null,"–","–","–","–","–","–","AIN1D","AIN0D"]
["(0x7E)","DIDR0",null,"–","–","ADC5D","ADC4D","ADC3D","ADC2D","ADC1D","ADC0D"]
["(0x7D)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x7C)","ADMUX",null,"REFS1","REFS0","ADLAR","–","MUX3","MUX2","MUX1","MUX0"]
["(0x7B)","ADCSRB",null,"–","ACME","–","–","–","ADTS2","ADTS1","ADTS0"]
["(0x7A)","ADCSRA",null,"ADEN","ADSC","ADATE","ADIF","ADIE","ADPS2","ADPS1","ADPS0"]
["(0x79)","ADCH","ADC Data Register High byte"]
["(0x78)","ADCL","ADC Data Register Low byte"]
["(0x77)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x76)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x75)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x74)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x73)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x72)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x71)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x70)","TIMSK2",null,"–","–","–","–","–","OCIE2B","OCIE2A","TOIE2"]
["(0x6F)","TIMSK1",null,"–","–","ICIE1","–","–","OCIE1B","OCIE1A","TOIE1"]
["(0x6E)","TIMSK0",null,"–","–","–","–","–","OCIE0B","OCIE0A","TOIE0"]
["(0x6D)","PCMSK2",null,"PCINT23","PCINT22","PCINT21","PCINT20","PCINT19","PCINT18","PCINT17","PCINT16"]
["(0x6C)","PCMSK1",null,"–","PCINT14","PCINT13","PCINT12","PCINT11","PCINT10","PCINT9","PCINT8"]
["(0x6B)","PCMSK0",null,"PCINT7","PCINT6","PCINT5","PCINT4","PCINT3","PCINT2","PCINT1","PCINT0"]
["(0x6A)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x69)","EICRA",null,"–","–","–","–","ISC11","ISC10","ISC01","ISC00"]
["(0x68)","PCICR",null,"–","–","–","–","–","PCIE2","PCIE1","PCIE0"]
["(0x67)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x66)","OSCCAL","Oscillator Calibration Register"]
["(0x65)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x64)","PRR",null,"PRTWI","PRTIM2","PRTIM0","–","PRTIM1","PRSPI","PRUSART0","PRADC"]
["(0x63)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x62)","Reserved",null,"–","–","–","–","–","–","–","–"]
["(0x61)","CLKPR",null,"CLKPCE","–","–","–","CLKPS3","CLKPS2","CLKPS1","CLKPS0"]
["(0x60)","WDTCSR",null,"WDIF","WDIE","WDP3","WDCE","WDE","WDP2","WDP1","WDP0"]
["0x3F (0x5F)","SREG",null,"I","T","H","S","V","N","Z","C"]
["0x3E (0x5E)","SPH",null,"–","–","–","–","–","(SP10*) ","SP9","SP8"]
["0x3D (0x5D)","SPL",null,"SP7","SP6","SP5","SP4","SP3","SP2","SP1","SP0"]
["0x3C (0x5C)","Reserved",null,"–","–","–","–","–","–","–","–"]
["0x3B (0x5B)","Reserved",null,"–","–","–","–","–","–","–","–"]
["0x3A (0x5A)","Reserved",null,"–","–","–","–","–","–","–","–"]
["0x39 (0x59)","Reserved",null,"–","–","–","–","–","–","–","–"]
["0x38 (0x58)","Reserved",null,"–","–","–","–","–","–","–","–"]
["0x37 (0x57)","SPMCSR",null,"SPMIE","(RWWSB*)","SIGRD","(RWWSRE*)","BLBSET","PGWRT","PGERS","SPMEN"]
["0x36 (0x56)","Reserved",null,"–","–","–","–","–","–","–","–"]
["0x35 (0x55)","MCUCR",null,"–","BODS","BODSE","PUD","–","–","IVSEL","IVCE"]
["0x34 (0x54)","MCUSR",null,"–","–","–","–","WDRF","BORF","EXTRF","PORF"]
["0x33 (0x53)","SMCR",null,"–","–","–","–","SM2","SM1","SM0","SE"]
["0x32 (0x52)","Reserved",null,"–","–","–","–","–","–","–","–"]
["0x31 (0x51)","Reserved",null,"–","–","–","–","–","–","–","–"]
["0x30 (0x50)","ACSR",null,"ACD","ACBG","ACO","ACI","ACIE","ACIC","ACIS1","ACIS0"]
["0x2F (0x4F)","Reserved",null,"–","–","–","–","–","–","–","–"]
["0x2E (0x4E)","SPDR"," SPI Data Register"]
["0x2D (0x4D)","SPSR",null,"SPIF","WCOL","–","–","–","–","–","SPI2X"]
["0x2C (0x4C)","SPCR",null,"SPIE","SPE","DORD","MSTR","CPOL","CPHA","SPR1","SPR0"]
["0x2B (0x4B)","GPIOR2","General Purpose I/O Register 2"]
["0x2A (0x4A)","GPIOR1","General Purpose I/O Register 1"]
["0x29 (0x49)","Reserved",null,"–","–","–","–","–","–","–","–"]
["0x28 (0x48)","OCR0B","Timer/Counter0 Output Compare Register B"]
["0x27 (0x47)","OCR0A","Timer/Counter0 Output Compare Register A"]
["0x26 (0x46)","TCNT0","Timer/Counter0 (8-bit)"]
["0x25 (0x45)","TCCR0B","Timer/Counter0 – Control  Register B","FOC0A","FOC0B","–","–","WGM02","CS02","CS01","CS00"]
["0x24 (0x44)","TCCR0A","Timer/Counter0 – Control  Register A","COM0A1","COM0A0","COM0B1","COM0B0","–","–","WGM01","WGM00"]
["0x23 (0x43)","GTCCR",null,"TSM","–","–","–","–","–","PSRASY","PSRSYNC"]
["0x22 (0x42)","EEARH","(EEPROM Address Register High Byte*)"]
["0x21 (0x41)","EEARL","EEPROM Address Register Low Byte"]
["0x20 (0x40)","EEDR","EEPROM Data Register"]
["0x1F (0x3F)","EECR",null,"–","–","EEPM1","EEPM0","EERIE","EEMPE","EEPE","EERE"]
["0x1E (0x3E)","GPIOR0","General Purpose I/O Register 0"]
["0x1D (0x3D)","EIMSK",null,"–","–","–","–","–","–","INT1","INT0"]
["0x1C (0x3C)","EIFR",null,"–","–","–","–","–","–","INTF1","INTF0"]
["0x1B (0x3B)","PCIFR",null,"–","–","–","–","–","PCIF2","PCIF1","PCIF0"]
["0x1A (0x3A)","Reserved",null,"–","–","–","–","–","–","–","–"]
["0x19 (0x39)","Reserved",null,"–","–","–","–","–","–","–","–"]
["0x18 (0x38)","Reserved",null,"–","–","–","–","–","–","–","–"]
["0x17 (0x37)","TIFR2",null,"–","–","–","–","–","OCF2B","OCF2A","TOV2"]
["0x16 (0x36)","TIFR1",null,"–","–","ICF1","–","–","OCF1B","OCF1A","TOV1"]
["0x15 (0x35)","TIFR0",null,"–","–","–","–","–","OCF0B","OCF0A","TOV0"]
["0x14 (0x34)","Reserved",null,"–","–","–","–","–","–","–","–"]
["0x13 (0x33)","Reserved",null,"–","–","–","–","–","–","–","–"]
["0x12 (0x32)","Reserved",null,"–","–","–","–","–","–","–","–"]
["0x11 (0x31)","Reserved",null,"–","–","–","–","–","–","–","–"]
["0x10 (0x30)","Reserved",null,"–","–","–","–","–","–","–","–"]
["0x0F (0x2F)","Reserved",null,"–","–","–","–","–","–","–","–"]
["0x0E (0x2E)","Reserved",null,"–","–","–","–","–","–","–","–"]
["0x0D (0x2D)","Reserved",null,"–","–","–","–","–","–","–","–"]
["0x0C (0x2C)","Reserved",null,"–","–","–","–","–","–","–","–"]
["0x0B (0x2B)","PORTD",null,"PORTD7","PORTD6","PORTD5","PORTD4","PORTD3","PORTD2","PORTD1","PORTD0"]
["0x0A (0x2A)","DDRD",null,"DDD7","DDD6","DDD5","DDD4","DDD3","DDD2","DDD1","DDD0"]
["0x09 (0x29)","PIND",null,"PIND7","PIND6","PIND5","PIND4","PIND3","PIND2","PIND1","PIND0"]
["0x08 (0x28)","PORTC",null,"–","PORTC6","PORTC5","PORTC4","PORTC3","PORTC2","PORTC1","PORTC0"]
["0x07 (0x27)","DDRC",null,"–","DDC6","DDC5","DDC4","DDC3","DDC2","DDC1","DDC0"]
["0x06 (0x26)","PINC",null,"–","PINC6","PINC5","PINC4","PINC3","PINC2","PINC1","PINC0"]
["0x05 (0x25)","PORTB",null,"PORTB7","PORTB6","PORTB5","PORTB4","PORTB3","PORTB2","PORTB1","PORTB0"]
["0x04 (0x24)","DDRB",null,"DDB7","DDB6","DDB5","DDB4","DDB3","DDB2","DDB1","DDB0"]
["0x03 (0x23)","PINB",null,"PINB7","PINB6","PINB5","PINB4","PINB3","PINB2","PINB1","PINB0"]
["0x02 (0x22)","Reserved",null,"–","–","–","–","–","–","–","–"]
["0x01 (0x21)","Reserved",null,"–","–","–","–","–","–","–","–"]
["0x00 (0x20)","Reserved",null,"–","–","–","–","–","–","–","–"]

{"sheet":"ATmega164_324_644_1284","index":8,"n_rows":222,"n_cols":11,"rows_kept":222,"flags":["formulas_cached_only"]}
[null,null,"ATmega164A/PA/324A/PA/644A/PA/1284/P"]
[]
["Address","Name","Beschreibung","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["(0xFF)","Reserved",null,"-","-","-","-","-","-","-"]
["(0xFE)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xFD)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xFC)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xFB)","Reserved",null,"-","-","-","-","-","-","-"]
["(0xFA)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xF9)","Reserved",null,"-","-","-","-","-","-","-"]
["(0xF8)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xF7)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xF6)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xF5)","Reserved",null,"-","-","-","-","-","-","-"]
["(0xF4)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xF3)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xF2)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xF1)","Reserved",null,"-","-","-","-","-","-","-"]
["(0xF0)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xEF)","Reserved",null,"-","-","-","-","-","-","-"]
["(0xEE)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xED)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xEC)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xEB)","Reserved",null,"-","-","-","-","-","-","-"]
["(0xEA)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xE9)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xE8)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xE7)","Reserved",null,"-","-","-","-","-","-","-"]
["(0xE6)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xE5)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xE4)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xE3)","Reserved",null,"-","-","-","-","-","-","-"]
["(0xE2)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xE1)","Reserved",null,"-","-","-","-","-","-","-"]
["(0xE0)","Reserved",null,"-","-","-","-","-","-","-"]
["(0xDF)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xDE)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xDD)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xDC)","Reserved",null,"-","-","-","-","-","-","-"]
["(0xDB)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xDA)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xD9)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xD8)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xD7)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xD6)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xD5)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xD4)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xD3)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xD2)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xD1)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xD0)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xCF)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xCE)","UDR1"," USART1 I/O Data Register","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["(0xCD)","UBRR1H",null,"-","-","-","-","Bit 3","Bit 2","Bit 1","Bit 0"]
["(0xCC)","UBRR1L"," USART1 Baud Rate Register Low Byte","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["(0xCB)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xCA)","UCSR1C",null,"UMSEL11","UMSEL10","UPM11","UPM10","USBS1","UCSZ11/UDORD0","UCSZ10/UCPHA0","UCPOL1"]
["(0xC9)","UCSR1B",null,"RXCIE1","TXCIE1","UDRIE1","RXEN1","TXEN1","UCSZ12","RXB81","TXB81"]
["(0xC8)","UCSR1A",null,"RXC1","TXC1","UDRE1","FE1","DOR1","UPE1","U2X1","MPCM1"]
["(0xC7)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xC6)","UDR0"," USART0 I/O Data Register","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["(0xC5)","UBRR0H",null,"-","-","-","-","Bit 3","Bit 2","Bit 1","Bit 0"]
["(0xC4)","UBRR0L"," USART0 Baud Rate Register Low Byte","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["(0xC3)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xC2)","UCSR0C",null,"UMSEL01","UMSEL00","UPM01","UPM00","USBS0","UCSZ01/UDORD0","UCSZ00/UCPHA0","UCPOL0"]
["(0xC1)","UCSR0B",null,"RXCIE0","TXCIE0","UDRIE0","RXEN0","TXEN0","UCSZ02","RXB80","TXB80"]
["(0xC0)","UCSR0A",null,"RXC0","TXC0","UDRE0","FE0","DOR0","UPE0","U2X0","MPCM0"]
["(0xBA)","TWAR",null,"TWA6","TWA5","TWA4","TWA3","TWA2","TWA1","TWA0","TWGCE"]
["(0xB9)","TWSR",null,"TWS7","TWS6","TWS5","TWS4","TWS3","-","TWPS1","TWPS0"]
["(0xB8)","TWBR","two-wire Serial Interface Bit Rate Register","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["(0xB7)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xB6)","ASSR",null,"-","EXCLK","AS2","TCN2UB","OCR2AUB","OCR2BUB","TCR2AUB","TCR2BUB"]
["(0xB5)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xB4)","OCR2B"," Timer/Counter2 Output Compare Register B","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["(0xB3)","OCR2A"," Timer/Counter2 Output Compare Register A","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["(0xB2)","TCNT2"," Timer/Counter2 (8 Bit)","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["(0xB1)","TCCR2B","Timer/Counter2 – Control  Register B","FOC2A","FOC2B","-","-","WGM22","CS22","CS21","CS20"]
["(0xB0)","TCCR2A","Timer/Counter2 – Control  Register A","COM2A1","COM2A0","COM2B1","COM2B0","-","-","WGM21","WGM20"]
["(0xAF)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xAE)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xAD)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xAC)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xAB)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xAA)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xA9)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xA8)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xA7)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xA6)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xA5)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xA4)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xA3)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xA2)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xA1)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0xA0)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0x9F)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0x9E)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0x9D)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0x9C)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0x9B)","OCR3BH","Timer/Counter3 - Output Compare Register B High Byte","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["(0x9A)","OCR3BL","Timer/Counter3 - Output Compare Register B Low Byte","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["(0x99)","OCR3AH","Timer/Counter3 - Output Compare Register A High Byte","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["(0x98)","OCR3AL","Timer/Counter3 - Output Compare Register A Low Byte","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["(0x97)","ICR3H","Timer/Counter3 - Input Capture Register High Byte","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["(0x96)","ICR3L","Timer/Counter3 - Input Capture Register Low Byte","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["(0x95)","TCNT3H","Timer/Counter3 - Counter Register High Byte","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["(0x94)","TCNT3L","Timer/Counter3 - Counter Register Low Byte","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["(0x93)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0x92)","TCCR3C","Timer/Counter3 – Control  Register C","FOC3A","FOC3B","-","-","-","-","-","-"]
["(0x91)","TCCR3B","Timer/Counter3 – Control  Register B","ICNC3","ICES3","-","WGM33","WGM32","CS32","CS31","CS30"]
["(0x90)","TCCR3A","Timer/Counter3 – Control  Register A","COM3A1","COM3A0","COM3B1","COM3B0","-","-","WGM31","WGM30"]
["(0x8F)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0x8E)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0x8D)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0x8C)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0x8B)","OCR1BH","Timer/Counter1 - Output Compare Register B High Byte","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
[" (0x8A)","OCR1BL","Timer/Counter1 - Output Compare Register B Low Byte","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["(0x89)","OCR1AH","Timer/Counter1 - Output Compare Register A High Byte","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["(0x88)","OCR1AL","Timer/Counter1 - Output Compare Register A Low Byte","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["(0x87)","ICR1H","Timer/Counter1 - Input Capture Register High Byte","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["(0x86)","ICR1L","Timer/Counter1 - Input Capture Register Low Byte","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["(0x85)","TCNT1H","Timer/Counter1 - Counter Register High Byte","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["(0x84)","TCNT1L","Timer/Counter1 - Counter Register Low Byte","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["(0x83)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0x82)","TCCR1C","Timer/Counter1 – Control  Register C","FOC1A","FOC1B","-","-","-","-","-","-"]
["(0x81)","TCCR1B","Timer/Counter1 – Control  Register B","ICNC1","ICES1","-","WGM13","WGM12","CS12","CS11","CS10"]
["(0x80)","TCCR1A","Timer/Counter1 – Control  Register A","COM1A1","COM1A0","COM1B1","COM1B0","-","-","WGM11","WGM10"]
["(0x7F)","DIDR1",null,"-","-","-","-","-","-","AIN1D","AIN0D"]
["(0x7E)","DIDR0",null,"ADC7D","ADC6D","ADC5D","ADC4D","ADC3D","ADC2D","ADC1D","ADC0D"]
["(0x7D)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0x7C)","ADMUX",null,"REFS1","REFS0","ADLAR","MUX4","MUX3","MUX2","MUX1","MUX0"]
["(0x7B)","ADCSRB",null,"-","ACME","-","-","-","ADTS2","ADTS1","ADTS0"]
["(0x7A)","ADCSRA",null,"ADEN","ADSC","ADATE","ADIF","ADIE","ADPS2","ADPS1","ADPS0"]
["(0x79)","ADCH","ADC Data Register High byte","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["(0x78)","ADCL","ADC Data Register Low byte","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["(0x77)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0x76)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0x75)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0x74)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0x73)","PCMSK3",null,"PCINT31","PCINT30","PCINT29","PCINT28","PCINT27","PCINT26","PCINT25","PCINT24"]
["(0x72)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0x71)","TIMSK3","Timer/Counter Interrupt Mask Register 3","-","-","ICIE3","-","-","OCIE3B","OCIE3A","TOIE3"]
["(0x70)","TIMSK2","Timer/Counter Interrupt Mask Register 2","-","-","-","-","-","OCIE2B","OCIE2A","TOIE2"]
["(0x6F)","TIMSK1","Timer/Counter Interrupt Mask Register 1","-","-","ICIE1","-","-","OCIE1B","OCIE1A","TOIE1"]
["(0x6E)","TIMSK0","Timer/Counter Interrupt Mask Register 0","-","-","-","-","-","OCIE0B","OCIE0A","TOIE0"]
["(0x6D)","PCMSK2",null,"PCINT23","PCINT22","PCINT21","PCINT20","PCINT19","PCINT18","PCINT17","PCINT16"]
["(0x6C)","PCMSK1",null,"PCINT15","PCINT14","PCINT13","PCINT12","PCINT11","PCINT10","PCINT9","PCINT8"]
["(0x6B)","PCMSK0",null,"PCINT7","PCINT6","PCINT5","PCINT4","PCINT3","PCINT2","PCINT1","PCINT0"]
["(0x6A)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0x69)","EICRA",null,"-","-","ISC21","ISC20","ISC11","ISC10","ISC01","ISC00"]
["(0x68)","PCICR",null,"-","-","-","-","PCIE3","PCIE2","PCIE1","PCIE0"]
["(0x67)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0x66)","OSCCAL","Oscillator Calibration Register","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["(0x65)","PRR1",null,"-","-","-","-","-","-","-","PRTIM3"]
["(0x64)","PRR0",null,"PRTWI","PRTIM2","PRTIM0","PRUSART1","PRTIM1","PRSPI","PRUSART0","PRADC"]
["(0x63)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0x62)","Reserved",null,"-","-","-","-","-","-","-","-"]
["(0x61)","CLKPR",null,"CLKPCE","-","-","-","CLKPS3","CLKPS2","CLKPS1","CLKPS0"]
["(0x60)","WDTCSR",null,"WDIF","WDIE","WDP3","WDCE","WDE","WDP2","WDP1","WDP0"]
["0x3F (0x5F)","SREG",null,"I","T","H","S","V","N","Z","C"]
["0x3E (0x5E)","SPH",null,"SP15","SP14","SP13","SP12","SP11","SP10","SP9","SP8"]
["0x3D (0x5D)","SPL",null,"SP7","SP6","SP5","SP4","SP3","SP2","SP1","SP0"]
["0x3C (0x5C)","Reserved",null,"-","-","-","-","-","-","-","-"]
["0x3B (0x5B)","Reserved",null,"-","-","-","-","-","-","-","-"]
["0x3A (0x5A)","Reserved",null,"-","-","-","-","-","-","-","-"]
["0x39 (0x59)","Reserved",null,"-","-","-","-","-","-","-","-"]
["0x38 (0x58)","Reserved",null,"-","-","-","-","-","-","-","-"]
["0x37 (0x57)","SPMCSR",null,"SPMIE","RWWSB","SIGRD","RWWSRE","BLBSET","PGWRT","PGERS","SPMEN"]
["0x36 (0x56)","Reserved",null,"-","-","-","-","-","-","-","-"]
["0x35 (0x55)","MCUCR",null,"JTD","BODS","BODSE","PUD","-","-","IVSEL","IVCE"]
["0x34 (0x54)","MCUSR",null,"-","-","-","JTRF","WDRF","BORF","EXTRF","PORF"]
["0x33 (0x53)","SMCR",null,"-","-","-","-","SM2","SM1","SM0","SE"]
["0x32 (0x52)","Reserved",null,"-","-","-","-","-","-","-","-"]
["0x31 (0x51)","OCDR"," On-Chip Debug Register","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["0x30 (0x50)","ACSR",null,"ACD","ACBG","ACO","ACI","ACIE","ACIC","ACIS1","ACIS0"]
["0x2F (0x4F)","Reserved",null,"-","-","-","-","-","-","-","-"]
["0x2E (0x4E)","SPDR"," SPI 0 Data Register",166]
["0x2D (0x4D)","SPSR",null,"SPIF0","WCOL0","-","-","-","-","-","SPI2X0"]
["0x2C (0x4C)","SPCR",null,"SPIE0","SPE0","DORD0","MSTR0","CPOL0","CPHA0","SPR01","SPR00"]
["0x2B (0x4B)","GPIOR2","General Purpose I/O Register 2","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["0x2A (0x4A)","GPIOR1","General Purpose I/O Register 1","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["0x29 (0x49)","Reserved",null,"-","-","-","-","-","-","-","-"]
["0x28 (0x48)","OCR0B"," Timer/Counter0 Output Compare Register B","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["0x27 (0x47)","OCR0A"," Timer/Counter0 Output Compare Register A","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["0x26 (0x46)","TCNT0"," Timer/Counter0 (8 Bit)","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0"]
["0x25 (0x45)","TCCR0B","Timer/Counter0 – Control  Register B","FOC0A","FOC0B","-","-","WGM02","CS02","CS01","CS00"]
["0x24 (0x44)","TCCR0A","Timer/Counter0 – Control  Register A","COM0A1","COM0A0","COM0B1","COM0B0","-","-","WGM01","WGM00"]
["0x23 (0x43)","GTCCR",null,"TSM","-","-","-","-","-","PSRASY","PSRSYNC"]
["0x22 (0x42)","EEARH",null,"-","-","-","-","Bit 3","Bit 2","Bit 1","Bit 0"]
["0x21 (0x41)","EEARL","EEPROM Address Register Low Byte",24]
["0x20 (0x40)","EEDR","EEPROM Data Register",24]
["0x1F (0x3F)","EECR",null,"-","-","EEPM1","EEPM0","EERIE","EEMPE","EEPE","EERE"]
["0x1E (0x3E)","GPIOR0","General Purpose I/O Register 0",29]
["0x1D (0x3D)","EIMSK",null,"-","-","-","-","-","INT2","INT1","INT0"]
["0x1C (0x3C)","EIFR",null,"-","-","-","-","-","INTF2","INTF1","INTF0"]
["0x1B (0x3B)","PCIFR",null,"-","-","-","-","PCIF3","PCIF2","PCIF1","PCIF0"]
["0x1A (0x3A)","Reserved",null,"-","-","-","-","-","-","-","-"]
["0x19 (0x39)","Reserved",null,"-","-","-","-","-","-","-","-"]
["0x18 (0x38)","TIFR3","Timer/Counter Interrupt Flag Register 3","-","-","ICF3","-","-","OCF3B","OCF3A","TOV3"]
["0x17 (0x37)","TIFR2","Timer/Counter Interrupt Flag Register 2","-","-","-","-","-","OCF2B","OCF2A","TOV2"]
["0x16 (0x36)","TIFR1","Timer/Counter Interrupt Flag Register 1","-","-","ICF1","-","-","OCF1B","OCF1A","TOV1"]
["0x15 (0x35)","TIFR0","Timer/Counter Interrupt Flag Register 0","-","-","-","-","-","OCF0B","OCF0A","TOV0"]
["0x14 (0x34)","Reserved",null,"-","-","-","-","-","-","-","-"]
["0x13 (0x33)","Reserved",null,"-","-","-","-","-","-","-","-"]
["0x12 (0x32)","Reserved",null,"-","-","-","-","-","-","-","-"]
["0x11 (0x31)","Reserved",null,"-","-","-","-","-","-","-","-"]
["0x10 (0x30)","Reserved",null,"-","-","-","-","-","-","-","-"]
["0x0F (0x2F)","Reserved",null,"-","-","-","-","-","-","-","-"]
["0x0E (0x2E)","Reserved",null,"-","-","-","-","-","-","-","-"]
["0x0D (0x2D)","Reserved",null,"-","-","-","-","-","-","-","-"]
["0x0C (0x2C)","Reserved",null,"-","-","-","-","-","-","-","-"]
["0x0B (0x2B)","PORTD",null,"PORTD7","PORTD6","PORTD5","PORTD4","PORTD3","PORTD2","PORTD1","PORTD0"]
["0x0A (0x2A)","DDRD",null,"DDD7","DDD6","DDD5","DDD4","DDD3","DDD2","DDD1","DDD0"]
["0x09 (0x29)","PIND",null,"PIND7","PIND6","PIND5","PIND4","PIND3","PIND2","PIND1","PIND0"]
["0x08 (0x28)","PORTC",null,"PORTC7","PORTC6","PORTC5","PORTC4","PORTC3","PORTC2","PORTC1","PORTC0"]
["0x07 (0x27)","DDRC",null,"DDC7","DDC6","DDC5","DDC4","DDC3","DDC2","DDC1","DDC0"]
["0x06 (0x26)","PINC",null,"PINC7","PINC6","PINC5","PINC4","PINC3","PINC2","PINC1","PINC0"]
["0x05 (0x25)","PORTB",null,"PORTB7","PORTB6","PORTB5","PORTB4","PORTB3","PORTB2","PORTB1","PORTB0"]
["0x04 (0x24)","DDRB",null,"DDB7","DDB6","DDB5","DDB4","DDB3","DDB2","DDB1","DDB0"]
["0x03 (0x23)","PINB",null,"PINB7","PINB6","PINB5","PINB4","PINB3","PINB2","PINB1","PINB0"]
["0x02 (0x22)","PORTA",null,"PORTA7","PORTA6","PORTA5","PORTA4","PORTA3","PORTA2","PORTA1","PORTA0"]
["0x01 (0x21)","DDRA",null,"DDA7","DDA6","DDA5","DDA4","DDA3","DDA2","DDA1","DDA0"]
["0x00 (0x20)","PINA",null,"PINA7","PINA6","PINA5","PINA4","PINA3","PINA2","PINA1","PINA0"]