(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (title_block
    (comment 4 "AISLER Project ID: HIIXERFK")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "+3.3V")
  (net 2 "GNDD")
  (net 3 "Net-(U2-VOUT)")
  (net 4 "+12V")
  (net 5 "SPI_MISO")
  (net 6 "SPI_SCK")
  (net 7 "SPI_MOSI")
  (net 8 "+5V")
  (net 9 "Net-(Q1-B)")
  (net 10 "Net-(Q2-B)")
  (net 11 "Net-(Q3-B)")
  (net 12 "Net-(Q4-B)")
  (net 13 "Net-(Q5-B)")
  (net 14 "Net-(Q6-B)")
  (net 15 "/Steuerung/Stockwerkverteiler/W-Anf.-In")
  (net 16 "Net-(D3-A)")
  (net 17 "Net-(U2-A1{slash}AGR{slash}AERW)")
  (net 18 "unconnected-(U2-C1{slash}CR-Pad2)")
  (net 19 "unconnected-(U2-C2{slash}CG{slash}CE-Pad9)")
  (net 20 "/Steuerung/Relais-Ansteuerung/Rls_Out_Status_Pumpe")
  (net 21 "/Steuerung/Sensoren/Sen_Sensor_Aussen")
  (net 22 "/Steuerung/Sensoren/Sen_Sensor_VL1")
  (net 23 "/Steuerung/Sensoren/Sen_Sensor_VL2")
  (net 24 "/Steuerung/Sensoren/Sen_Sensor_RL1")
  (net 25 "/Steuerung/Sensoren/Sen_Sensor_RL2")
  (net 26 "/Eingabe/Taster_up")
  (net 27 "/Eingabe/Taster_dwn")
  (net 28 "/Eingabe/Taster_mnu")
  (net 29 "/Eingabe/Taster_light")
  (net 30 "/Steuerung/Strg_Taster_up")
  (net 31 "/Steuerung/Strg_Taster_dwn")
  (net 32 "/Steuerung/Strg_Taster_mnu")
  (net 33 "/Steuerung/Strg_Taster_light")
  (net 34 "/Steuerung/Strg_Display_Reset")
  (net 35 "/Steuerung/Strg_Display_CS")
  (net 36 "/Steuerung/Strg_Display_Light")
  (net 37 "/Display/Disp_SPI_SCK")
  (net 38 "/Display/Disp_SPI_MOSI")
  (net 39 "/Display/SPI_MISO")
  (net 40 "/Display/Disp_CS")
  (net 41 "/Display/Disp_Reset")
  (net 42 "/Display/Disp_Light")
  (net 43 "/Steuerung/Stockwerkverteiler/SWV_IN_Anforderung")
  (net 44 "/Steuerung/Relais-Ansteuerung/Rls_Pumpe_an")
  (net 45 "/Steuerung/Relais-Ansteuerung/Rls_Mischer_zu")
  (net 46 "/Steuerung/Relais-Ansteuerung/Rls_Mischer_auf")
  (net 47 "/Steuerung/Out_Anforderung/Out_Anf0")
  (net 48 "/Steuerung/Out_Anforderung/Out_Anf1")
  (net 49 "Guard")
  (net 50 "/Steuerung/RS485/ModBus_Rx")
  (net 51 "/Steuerung/RS485/ModBus_SE")
  (net 52 "/Steuerung/RS485/Modbus_Tx")
  (net 53 "/Steuerung/+5V")
  (net 54 "/Steuerung/Stockwerkverteiler/Pumpe Status C")
  (net 55 "/Steuerung/Stockwerkverteiler/Pumpe Status E")
  (net 56 "Net-(J5-Pin_5)")
  (net 57 "Net-(U3-XTAL1)")
  (net 58 "Net-(U3-XTAL2)")
  (net 59 "Net-(D1-A)")
  (net 60 "Net-(D2-K)")
  (net 61 "Net-(D2-A)")
  (net 62 "Net-(D3-K)")
  (net 63 "unconnected-(J1-Pin_5-Pad5)")
  (net 64 "unconnected-(J1-Pin_6-Pad6)")
  (net 65 "unconnected-(J2-Pin_10-Pad10)")
  (net 66 "unconnected-(J3-Pin_5-Pad5)")
  (net 67 "unconnected-(J3-Pin_6-Pad6)")
  (net 68 "unconnected-(J4-Pin_10-Pad10)")
  (net 69 "unconnected-(J5-Pin_2-Pad2)")
  (net 70 "Net-(U5-A)")
  (net 71 "Net-(U5-B)")
  (net 72 "Net-(Q1-C)")
  (net 73 "Net-(U1-MTI2{slash}GUARD)")
  (net 74 "Net-(U1-MTI0)")
  (net 75 "Net-(U1-MTI1)")
  (net 76 "Net-(U1-MTI3)")
  (net 77 "Net-(U1-MTI4)")
  (net 78 "Net-(R6-Pad2)")
  (net 79 "Net-(R16-Pad2)")
  (net 80 "Net-(U1-MTSA)")
  (net 81 "unconnected-(RV2-Pad1)")
  (net 82 "unconnected-(U3-PB3-Pad4)")
  (net 83 "unconnected-(U3-PB4-Pad5)")
  (net 84 "unconnected-(U3-PD2-Pad16)")
  (net 85 "unconnected-(U3-PD3-Pad17)")
  (net 86 "unconnected-(U3-PD5-Pad19)")
  (net 87 "unconnected-(U3-PD6-Pad20)")
  (net 88 "unconnected-(U3-PD7-Pad21)")
  (net 89 "unconnected-(U3-PC7-Pad29)")
  (net 90 "unconnected-(U3-AREF-Pad32)")
  (net 91 "unconnected-(U4-NC-Pad3)")
  (net 92 "unconnected-(U4-Pad6)")
  (net 93 "/Steuerung/Out_Anforderung/Anf_Out_0")
  (net 94 "/Steuerung/Out_Anforderung/Anf_Out_1")
  (net 95 "/Eingabe/Touch_S1")
  (net 96 "/Eingabe/Touch_S2")
  (net 97 "/Eingabe/Touch_S3")
  (net 98 "/Eingabe/Touch_S4")
  (footprint "wago-footprints:CONN_233-506_WAG" (layer "F.Cu")
    (at 60.96 120.65)
    (tags "233-506 ")
    (property "Sheetfile" "rs485.kicad_sch")
    (property "Sheetname" "RS485")
    (property "ki_keywords" "233-506")
    (attr through_hole)
    (fp_text reference "J10" (at 6.209995 2.5 unlocked) (layer "F.SilkS"))
    (fp_text value "ModBus" (at 6.209995 17.78 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 6.209995 2.5 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 2 "GNDD") (pinfunction "1") (pintype "unspecified"))
    (pad "2" thru_hole circle (at 0 5) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 2 "GNDD") (pinfunction "2") (pintype "unspecified"))
    (pad "3" thru_hole circle (at 2.54 0) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 70 "Net-(U5-A)") (pinfunction "3") (pintype "unspecified"))
    (pad "4" thru_hole circle (at 2.54 5) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 70 "Net-(U5-A)") (pinfunction "4") (pintype "unspecified"))
    (pad "5" thru_hole circle (at 5.08 0) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 71 "Net-(U5-B)") (pinfunction "5") (pintype "unspecified"))
    (pad "6" thru_hole circle (at 5.08 5) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 71 "Net-(U5-B)") (pinfunction "6") (pintype "unspecified"))
    (pad "7" thru_hole circle (at 7.62 0) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 2 "GNDD") (pinfunction "7") (pintype "unspecified"))
    (pad "8" thru_hole circle (at 7.62 5) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 2 "GNDD") (pinfunction "8") (pintype "unspecified"))
    (pad "9" thru_hole circle (at 10.16 0) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 70 "Net-(U5-A)") (pinfunction "9") (pintype "unspecified"))
    (pad "10" thru_hole circle (at 10.16 5) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 70 "Net-(U5-A)") (pinfunction "10") (pintype "unspecified"))
    (pad "11" thru_hole circle (at 12.7 0) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 71 "Net-(U5-B)") (pinfunction "11") (pintype "unspecified"))
    (pad "12" thru_hole circle (at 12.7 5) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 71 "Net-(U5-B)") (pinfunction "12") (pintype "unspecified"))
  )
  (footprint "wago-footprints:CONN_233-503_WAG" (layer "F.Cu")
    (at 45.72 120.65)
    (tags "233-503 ")
    (property "Feld2" "")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_keywords" "233-503")
    (attr through_hole)
    (fp_text reference "J7" (at 2.399995 2.5 unlocked) (layer "F.SilkS"))
    (fp_text value "Power" (at 2.399995 17.78 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.399995 2.5 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 2 "GNDD") (pinfunction "1") (pintype "unspecified"))
    (pad "2" thru_hole circle (at 0 5) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 2 "GNDD") (pinfunction "2") (pintype "unspecified"))
    (pad "3" thru_hole circle (at 2.54 0) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 53 "/Steuerung/+5V") (pinfunction "3") (pintype "unspecified"))
    (pad "4" thru_hole circle (at 2.54 5) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 53 "/Steuerung/+5V") (pinfunction "4") (pintype "unspecified"))
    (pad "5" thru_hole circle (at 5.08 0) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 4 "+12V") (pinfunction "5") (pintype "unspecified"))
    (pad "6" thru_hole circle (at 5.08 5) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 4 "+12V") (pinfunction "6") (pintype "unspecified"))
  )
  (footprint "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal" (layer "F.Cu")
    (at 57.15 44.45 180)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (property "Feld2" "")
    (property "Sheetfile" "relais.kicad_sch")
    (property "Sheetname" "Relais-Ansteuerung")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "400V 1A General Purpose Rectifier Diode, DO-41")
    (property "ki_keywords" "diode")
    (attr through_hole)
    (fp_text reference "D4" (at 5.08 -2.47) (layer "F.SilkS"))
    (fp_text value "1N4004" (at 5.08 2.47) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 5.47 0) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 4 "+12V") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 180) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 62 "Net-(D3-K)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (at 35.56 46.99 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Feld2" "")
    (property "Sheetfile" "relais.kicad_sch")
    (property "Sheetname" "Relais-Ansteuerung")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr through_hole)
    (fp_text reference "D2" (at -2.54 -1.27) (layer "F.SilkS"))
    (fp_text value "M-zu" (at 1.27 2.96) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 60 "Net-(D2-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 61 "Net-(D2-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_IDC:IDC-Header_2x05_P2.54mm_Vertical" (layer "F.Cu")
    (at 41.91 87.63)
    (descr "Through hole IDC box header, 2x05, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0")
    (tags "Through hole vertical IDC box header THT 2x05 2.54mm double row")
    (property "Sheetfile" "FBH_Mischer.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x10, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J2" (at 1.27 -6.1) (layer "F.SilkS"))
    (fp_text value "Display" (at -5.08 5.08 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 1.27 5.08 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.1470588235)
      (net 1 "+3.3V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 53 "/Steuerung/+5V") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GNDD") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 34 "/Steuerung/Strg_Display_Reset") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole circle (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 35 "/Steuerung/Strg_Display_CS") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "SPI_SCK") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole circle (at 0 7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "SPI_MOSI") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole circle (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "SPI_MISO") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole circle (at 0 10.16) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 36 "/Steuerung/Strg_Display_Light") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole circle (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 65 "unconnected-(J2-Pin_10-Pad10)") (pinfunction "Pin_10") (pintype "passive+no_connect"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_IDC.3dshapes/IDC-Header_2x05_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.2mm_W3.0mm_P5.00mm_FKS2_FKP2_MKS2_MKP2" (layer "F.Cu")
    (at 96.6 109.22)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*3.0mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 3.0mm Capacitor")
    (property "Field2" "")
    (property "Sheetfile" "Steuerung.kicad_sch")
    (property "Sheetname" "Steuerung")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C4" (at 2.5 -2.75) (layer "F.SilkS"))
    (fp_text value "100nF" (at 2.5 2.75) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 56 "Net-(J5-Pin_5)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.2mm_W3.0mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (layer "F.Cu")
    (at 135.89 50.8)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.8) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm_M3_DIN965_Pad" (at 0 3.8) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (layer "F.Cu")
    (at 128.27 25.4)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.8) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm_M3_DIN965_Pad" (at 0 3.8) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (layer "F.Cu")
    (at 109.22 44.45)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.8) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm_M3_DIN965_Pad" (at 0 3.8) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Capacitor_THT:C_Rect_L7.2mm_W3.0mm_P5.00mm_FKS2_FKP2_MKS2_MKP2" (layer "F.Cu")
    (at 79.97 81.28 180)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*3.0mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 3.0mm Capacitor")
    (property "Field2" "")
    (property "Sheetfile" "Steuerung.kicad_sch")
    (property "Sheetname" "Steuerung")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C3" (at -2.58 0) (layer "F.SilkS"))
    (fp_text value "100nF" (at 2.5 2.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+3.3V") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.2mm_W3.0mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (at 106.68 87.63)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "out_anforderung.kicad_sch")
    (property "Sheetname" "Out_Anforderung")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R23" (at 7.62 -2.37) (layer "F.SilkS"))
    (fp_text value "1k8" (at 3.81 -2.54) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 7.62 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 47 "/Steuerung/Out_Anforderung/Out_Anf0") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(Q5-B)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (at 35.56 40.64 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Feld2" "")
    (property "Sheetfile" "relais.kicad_sch")
    (property "Sheetname" "Relais-Ansteuerung")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr through_hole)
    (fp_text reference "D1" (at -2.54 0) (layer "F.SilkS"))
    (fp_text value "Pumpe" (at 1.27 2.96) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 20 "/Steuerung/Relais-Ansteuerung/Rls_Out_Status_Pumpe") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 59 "Net-(D1-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Converter_DCDC:Converter_DCDC_Murata_MEE3SxxxxSC_THT" (layer "F.Cu")
    (at 45.7975 111.9925 90)
    (descr "https://power.murata.com/pub/data/power/ncl/kdc_mee3.pdf")
    (tags "murata dc-dc transformer")
    (property "Feld2" "")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "3W, 1000 VDC isolated DC/DC converter, 12V input, 12V output, SIP")
    (property "ki_keywords" "murata DC/DC isolated converter")
    (attr through_hole)
    (fp_text reference "PS1" (at 4.0425 7.5425 90) (layer "F.SilkS"))
    (fp_text value "TBA 1-0510 (Traco)" (at -2.3075 3.7325 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.794 3.556) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.75 2.25) (drill 1.075) (layers "*.Cu" "*.Mask")
      (net 2 "GNDD") (pinfunction "-Vin") (pintype "power_in"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.75 2.25) (drill 1.075) (layers "*.Cu" "*.Mask")
      (net 53 "/Steuerung/+5V") (pinfunction "+Vin") (pintype "power_in"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.75 2.25) (drill 1.075) (layers "*.Cu" "*.Mask")
      (net 2 "GNDD") (pinfunction "-Vout") (pintype "power_out"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.75 2.25) (drill 1.075) (layers "*.Cu" "*.Mask")
      (net 1 "+3.3V") (pinfunction "+Vout") (pintype "power_out"))
    (model "${KICAD6_3DMODEL_DIR}/Converter_DCDC.3dshapes/Converter_DCDC_Murata_MEE3SxxxxSC_THT.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (at 77.47 43.18 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Feld2" "")
    (property "Sheetfile" "sensoren.kicad_sch")
    (property "Sheetname" "Sensoren")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R20" (at 5.08 -2.37 90) (layer "F.SilkS"))
    (fp_text value "4k7" (at 1.27 -2.54 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+3.3V") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 21 "/Steuerung/Sensoren/Sen_Sensor_Aussen") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "wago-footprints:CONN_233-504_WAG" (layer "F.Cu")
    (at 52.07 36.83 180)
    (tags "233-504 ")
    (property "Feld2" "")
    (property "Sheetfile" "relais.kicad_sch")
    (property "Sheetname" "Relais-Ansteuerung")
    (property "ki_keywords" "233-504")
    (attr through_hole)
    (fp_text reference "J8" (at 3.52999 2.5 180 unlocked) (layer "F.SilkS"))
    (fp_text value "Relais" (at 3.81 15.24 180 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.52999 2.5 180 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 4 "+12V") (pinfunction "1") (pintype "unspecified"))
    (pad "2" thru_hole circle (at 0 5 180) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 4 "+12V") (pinfunction "2") (pintype "unspecified"))
    (pad "3" thru_hole circle (at 2.54 0 180) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 20 "/Steuerung/Relais-Ansteuerung/Rls_Out_Status_Pumpe") (pinfunction "3") (pintype "unspecified"))
    (pad "4" thru_hole circle (at 2.54 5 180) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 20 "/Steuerung/Relais-Ansteuerung/Rls_Out_Status_Pumpe") (pinfunction "4") (pintype "unspecified"))
    (pad "5" thru_hole circle (at 5.08 0 180) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 60 "Net-(D2-K)") (pinfunction "5") (pintype "unspecified"))
    (pad "6" thru_hole circle (at 5.08 5 180) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 60 "Net-(D2-K)") (pinfunction "6") (pintype "unspecified"))
    (pad "7" thru_hole circle (at 7.62 0 180) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 62 "Net-(D3-K)") (pinfunction "7") (pintype "unspecified"))
    (pad "8" thru_hole circle (at 7.62 5 180) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 62 "Net-(D3-K)") (pinfunction "8") (pintype "unspecified"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (at 106.68 91.44)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "out_anforderung.kicad_sch")
    (property "Sheetname" "Out_Anforderung")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R24" (at 7.62 -2.37) (layer "F.SilkS"))
    (fp_text value "1k8" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.62 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 48 "/Steuerung/Out_Anforderung/Out_Anf1") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(Q6-B)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Crystal:Crystal_HC49-4H_Vertical" (layer "F.Cu")
    (at 83.91 110.49)
    (descr "Crystal THT HC-49-4H http://5hertz.com/pdfs/04404_D.pdf")
    (tags "THT crystalHC-49-4H")
    (property "Field2" "")
    (property "Sheetfile" "Steuerung.kicad_sch")
    (property "Sheetname" "Steuerung")
    (property "ki_description" "Two pin crystal")
    (property "ki_keywords" "quartz ceramic resonator oscillator")
    (attr through_hole)
    (fp_text reference "Y1" (at 2.44 -3.525) (layer "F.SilkS"))
    (fp_text value "3,6864MHz" (at 2.45 3.81) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.44 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 58 "Net-(U3-XTAL2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 4.88 0) (size 1.5 1.5) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 57 "Net-(U3-XTAL1)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Crystal_HC49-4H_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (layer "F.Cu")
    (at 59.69 78.74)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.8) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm_M3_DIN965_Pad" (at 0 3.8) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Package_TO_SOT_THT:TO-92_Inline_Wide" (layer "F.Cu")
    (at 54.61 60.96 90)
    (descr "TO-92 leads in-line, wide, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Feld2" "")
    (property "Sheetfile" "relais.kicad_sch")
    (property "Sheetname" "Relais-Ansteuerung")
    (property "ki_description" "0.8A Ic, 45V Vce, NPN Transistor, TO-92")
    (property "ki_keywords" "NPN Transistor")
    (attr through_hole)
    (fp_text reference "Q3" (at 2.54 -3.56 90) (layer "F.SilkS"))
    (fp_text value "BC337" (at 2.54 2.79 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.5 1.5) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 60 "Net-(D2-K)") (pinfunction "C") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 90) (size 1.5 1.5) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(Q3-B)") (pinfunction "B") (pintype "input"))
    (pad "3" thru_hole circle (at 5.08 0 90) (size 1.5 1.5) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GNDD") (pinfunction "E") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline_Wide.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "lokal2:prox-sense-cap-directional-19.05mm" (layer "F.Cu")
    (at 165.735 69.2)
    (property "Feld2" "")
    (property "Sheetfile" "eingabe.kicad_sch")
    (property "Sheetname" "Eingabe")
    (zone_connect 2)
    (attr smd)
    (fp_text reference "T2" (at 0 -0.5 unlocked) (layer "F.SilkS"))
    (fp_text value "~" (at 0 1 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 -7.62) (size 0.8 0.8) (drill 0.4) (layers "*.Cu") (remove_unused_layers) (keep_end_layers) (zone_layer_connections)
      (net 96 "/Eingabe/Touch_S2") (pinfunction "Sensor") (pintype "bidirectional"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (at 43.18 58.42 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Feld2" "")
    (property "Sheetfile" "relais.kicad_sch")
    (property "Sheetname" "Relais-Ansteuerung")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R12" (at 5.08 -2.37) (layer "F.SilkS"))
    (fp_text value "680" (at 5.08 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+3.3V") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 59 "Net-(D1-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "lokal2:prox-sense-cap-directional-19.05mm" (layer "F.Cu")
    (at 137.795 69.2)
    (property "Feld2" "")
    (property "Sheetfile" "eingabe.kicad_sch")
    (property "Sheetname" "Eingabe")
    (zone_connect 2)
    (attr smd allow_missing_courtyard)
    (fp_text reference "T3" (at 0 -0.5 unlocked) (layer "F.SilkS"))
    (fp_text value "~" (at 0 1 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 -7.62) (size 0.8 0.8) (drill 0.4) (layers "*.Cu") (remove_unused_layers) (keep_end_layers) (zone_layer_connections)
      (net 97 "/Eingabe/Touch_S3") (pinfunction "Sensor") (pintype "bidirectional"))
  )
  (footprint "Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm" (layer "F.Cu")
    (at 83.82 105.41)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
    (property "Field2" "")
    (property "Sheetfile" "Steuerung.kicad_sch")
    (property "Sheetname" "Steuerung")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C6" (at 2.54 -2.25) (layer "F.SilkS"))
    (fp_text value "22pF" (at -1.27 -2.54) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 58 "Net-(U3-XTAL2)") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal" (layer "F.Cu")
    (at 86.36 48.26)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (property "Sheetfile" "input.kicad_sch")
    (property "Sheetname" "Stockwerkverteiler")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "100V 0.15A standard switching diode, DO-35")
    (property "ki_keywords" "diode")
    (attr through_hole)
    (fp_text reference "D7" (at 3.81 -2.12) (layer "F.SilkS"))
    (fp_text value "1N4148" (at 3.81 2.12) (layer "F.SilkS"))
    (fp_text user "K" (at 0 -1.8) (layer "F.SilkS"))
    (fp_text user "K" (at 0 -1.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 4.11 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+3.3V") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 15 "/Steuerung/Stockwerkverteiler/W-Anf.-In") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-92_Inline_Wide" (layer "F.Cu")
    (at 48.82 60.96 90)
    (descr "TO-92 leads in-line, wide, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Feld2" "")
    (property "Sheetfile" "relais.kicad_sch")
    (property "Sheetname" "Relais-Ansteuerung")
    (property "ki_description" "0.8A Ic, 45V Vce, NPN Transistor, TO-92")
    (property "ki_keywords" "NPN Transistor")
    (attr through_hole)
    (fp_text reference "Q2" (at 2.54 -3.56 90) (layer "F.SilkS"))
    (fp_text value "BC337" (at 2.54 2.79 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.5 1.5) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 20 "/Steuerung/Relais-Ansteuerung/Rls_Out_Status_Pumpe") (pinfunction "C") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 90) (size 1.5 1.5) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(Q2-B)") (pinfunction "B") (pintype "input"))
    (pad "3" thru_hole circle (at 5.08 0 90) (size 1.5 1.5) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GNDD") (pinfunction "E") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline_Wide.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (at 90.17 60.96 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Feld2" "")
    (property "Sheetfile" "relais.kicad_sch")
    (property "Sheetname" "Relais-Ansteuerung")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R10" (at 5.08 -2.37) (layer "F.SilkS"))
    (fp_text value "1k8" (at 5.08 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 45 "/Steuerung/Relais-Ansteuerung/Rls_Mischer_zu") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(Q3-B)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (at 90.17 57.15 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Feld2" "")
    (property "Sheetfile" "relais.kicad_sch")
    (property "Sheetname" "Relais-Ansteuerung")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R11" (at 5.08 -2.37) (layer "F.SilkS"))
    (fp_text value "1k8" (at 2.54 2.37) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 46 "/Steuerung/Relais-Ansteuerung/Rls_Mischer_auf") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(Q4-B)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm" (layer "F.Cu")
    (at 100.37 44.45)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
    (property "Sheetfile" "input.kicad_sch")
    (property "Sheetname" "Stockwerkverteiler")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C7" (at 1.25 -2.25) (layer "F.SilkS"))
    (fp_text value "33nF" (at 1.25 2.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.92 -2.32) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 15 "/Steuerung/Stockwerkverteiler/W-Anf.-In") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "wago-footprints:CONN_233-506_WAG" (layer "F.Cu")
    (at 72.39 36.83 180)
    (tags "233-506 ")
    (property "Feld2" "")
    (property "Sheetfile" "sensoren.kicad_sch")
    (property "Sheetname" "Sensoren")
    (property "ki_keywords" "233-506")
    (attr through_hole)
    (fp_text reference "J12" (at 6.209995 2.5 180 unlocked) (layer "F.SilkS"))
    (fp_text value "Mischersensoren" (at 6.209995 15.24 180 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 6.209995 2.5 180 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 1 "+3.3V") (pinfunction "1") (pintype "unspecified"))
    (pad "2" thru_hole circle (at 0 5 180) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 1 "+3.3V") (pinfunction "2") (pintype "unspecified"))
    (pad "3" thru_hole circle (at 2.54 0 180) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 22 "/Steuerung/Sensoren/Sen_Sensor_VL1") (pinfunction "3") (pintype "unspecified"))
    (pad "4" thru_hole circle (at 2.54 5 180) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 22 "/Steuerung/Sensoren/Sen_Sensor_VL1") (pinfunction "4") (pintype "unspecified"))
    (pad "5" thru_hole circle (at 5.08 0 180) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 23 "/Steuerung/Sensoren/Sen_Sensor_VL2") (pinfunction "5") (pintype "unspecified"))
    (pad "6" thru_hole circle (at 5.08 5 180) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 23 "/Steuerung/Sensoren/Sen_Sensor_VL2") (pinfunction "6") (pintype "unspecified"))
    (pad "7" thru_hole circle (at 7.62 0 180) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 24 "/Steuerung/Sensoren/Sen_Sensor_RL1") (pinfunction "7") (pintype "unspecified"))
    (pad "8" thru_hole circle (at 7.62 5 180) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 24 "/Steuerung/Sensoren/Sen_Sensor_RL1") (pinfunction "8") (pintype "unspecified"))
    (pad "9" thru_hole circle (at 10.16 0 180) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 25 "/Steuerung/Sensoren/Sen_Sensor_RL2") (pinfunction "9") (pintype "unspecified"))
    (pad "10" thru_hole circle (at 10.16 5 180) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 25 "/Steuerung/Sensoren/Sen_Sensor_RL2") (pinfunction "10") (pintype "unspecified"))
    (pad "11" thru_hole circle (at 12.7 0 180) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 2 "GNDD") (pinfunction "11") (pintype "unspecified"))
    (pad "12" thru_hole circle (at 12.7 5 180) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 2 "GNDD") (pinfunction "12") (pintype "unspecified"))
  )
  (footprint "Package_DIP:DIP-8_W7.62mm_LongPads" (layer "F.Cu")
    (at 76.2 105.42 -90)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads")
    (property "Sheetfile" "rs485.kicad_sch")
    (property "Sheetname" "RS485")
    (property "ki_description" "Half duplex RS-485/RS-422, 2.5 Mbps, ±15kV electro-static discharge (ESD) protection, no slew-rate, no low-power shutdown, with receiver/driver enable, 32 receiver drive kapacitity, DIP-8 and SOIC-8")
    (property "ki_keywords" "Half duplex RS-485/RS-422, 2.5 Mbps, ±15kV electro-static discharge (ESD) protection, no slew-rate, no low-power shutdown, with receiver/driver enable, 32 receiver drive kapacitity, DIP-8 and SOIC-8")
    (attr through_hole)
    (fp_text reference "U5" (at 3.81 -2.33 90) (layer "F.SilkS"))
    (fp_text value "MAX485E" (at 3.81 9.95 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 3.81 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 50 "/Steuerung/RS485/ModBus_Rx") (pinfunction "RO") (pintype "output"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 51 "/Steuerung/RS485/ModBus_SE") (pinfunction "~{RE}") (pintype "input"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 51 "/Steuerung/RS485/ModBus_SE") (pinfunction "DE") (pintype "input"))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 52 "/Steuerung/RS485/Modbus_Tx") (pinfunction "DI") (pintype "input"))
    (pad "5" thru_hole oval (at 7.62 7.62 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GNDD") (pinfunction "GND") (pintype "power_in"))
    (pad "6" thru_hole oval (at 7.62 5.08 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 70 "Net-(U5-A)") (pinfunction "A") (pintype "bidirectional"))
    (pad "7" thru_hole oval (at 7.62 2.54 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 71 "Net-(U5-B)") (pinfunction "B") (pintype "bidirectional"))
    (pad "8" thru_hole oval (at 7.62 0 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+3.3V") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal" (layer "F.Cu")
    (at 57.15 52.07 180)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (property "Feld2" "")
    (property "Sheetfile" "relais.kicad_sch")
    (property "Sheetname" "Relais-Ansteuerung")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "400V 1A General Purpose Rectifier Diode, DO-41")
    (property "ki_keywords" "diode")
    (attr through_hole)
    (fp_text reference "D6" (at 5.08 -2.47) (layer "F.SilkS"))
    (fp_text value "1N4004" (at 5.08 2.47) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 5.47 0) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 4 "+12V") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 180) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 20 "/Steuerung/Relais-Ansteuerung/Rls_Out_Status_Pumpe") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (layer "F.Cu")
    (at 37.0127 77.753838)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.8) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm_M3_DIN965_Pad" (at 0 3.8) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (at 106.72 105.41 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Field2" "")
    (property "Sheetfile" "Steuerung.kicad_sch")
    (property "Sheetname" "Steuerung")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R8" (at 5.08 -2.37) (layer "F.SilkS"))
    (fp_text value "10k" (at 5.08 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+3.3V") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 56 "Net-(J5-Pin_5)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (layer "F.Cu")
    (at 111.992519 27.479985)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.8) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm_M3_DIN965_Pad" (at 0 3.8) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (layer "F.Cu")
    (at 37.013582 132.500864)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.8) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm_M3_DIN965_Pad" (at 0 3.8) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (at 69.85 43.18 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Feld2" "")
    (property "Sheetfile" "sensoren.kicad_sch")
    (property "Sheetname" "Sensoren")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R19" (at 5.08 -2.37 90) (layer "F.SilkS"))
    (fp_text value "4k7" (at 5.08 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+3.3V") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 23 "/Steuerung/Sensoren/Sen_Sensor_VL2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (layer "F.Cu")
    (at 48.26 69.85)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.8) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm_M3_DIN965_Pad" (at 0 3.8) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (layer "F.Cu")
    (at 37.015963 27.49956)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.8) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm_M3_DIN965_Pad" (at 0 3.8) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Display:EA_DOGS104X-A" (layer "F.Cu")
    (at 174.68 24.78 -90)
    (descr "LCD 4x10 character 3.3V VDD I2C or SPI http://www.lcd-module.com/fileadmin/eng/pdf/doma/dogs104e.pdf")
    (tags "LCD 4x10 character 3.3V VDD I2C or SPI")
    (property "Feld2" "")
    (property "Sheetfile" "spi.kicad_sch")
    (property "Sheetname" "Display")
    (property "ki_keywords" "EA DOGS164W-A")
    (attr through_hole)
    (fp_text reference "U2" (at 2.22 -7.73 90) (layer "F.SilkS"))
    (fp_text value "EA DOGS104W-A" (at 6.6 30.8 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 13.61 11.51 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.5 1.5) (drill 1) (layers "*.Cu" "*.Mask")
      (net 17 "Net-(U2-A1{slash}AGR{slash}AERW)") (pinfunction "A1/AGR/AERW") (pintype "power_in"))
    (pad "2" thru_hole circle (at 0 2.54 270) (size 1.5 1.5) (drill 1) (layers "*.Cu" "*.Mask")
      (net 18 "unconnected-(U2-C1{slash}CR-Pad2)") (pinfunction "C1/CR") (pintype "power_in+no_connect"))
    (pad "9" thru_hole circle (at 0 20.32 270) (size 1.5 1.5) (drill 1) (layers "*.Cu" "*.Mask")
      (net 19 "unconnected-(U2-C2{slash}CG{slash}CE-Pad9)") (pinfunction "C2/CG/CE") (pintype "power_in+no_connect"))
    (pad "10" thru_hole circle (at 0 22.86 270) (size 1.5 1.5) (drill 1) (layers "*.Cu" "*.Mask")
      (net 72 "Net-(Q1-C)") (pinfunction "A2/CW") (pintype "power_in"))
    (pad "11" thru_hole circle (at 25.4 22.86 270) (size 1.5 1.5) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(U2-VOUT)") (pinfunction "VOUT") (pintype "power_out"))
    (pad "12" thru_hole circle (at 25.4 20.32 270) (size 1.5 1.5) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "+3.3V") (pinfunction "IM1") (pintype "input"))
    (pad "13" thru_hole circle (at 25.4 17.78 270) (size 1.5 1.5) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "+3.3V") (pinfunction "VDD") (pintype "power_in"))
    (pad "14" thru_hole circle (at 25.4 15.24 270) (size 1.5 1.5) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GNDD") (pinfunction "VSS") (pintype "power_in"))
    (pad "15" thru_hole circle (at 25.4 12.7 270) (size 1.5 1.5) (drill 1) (layers "*.Cu" "*.Mask")
      (net 39 "/Display/SPI_MISO") (pinfunction "SOD") (pintype "output"))
    (pad "16" thru_hole circle (at 25.4 10.16 270) (size 1.5 1.5) (drill 1) (layers "*.Cu" "*.Mask")
      (net 38 "/Display/Disp_SPI_MOSI") (pinfunction "SID") (pintype "input"))
    (pad "17" thru_hole circle (at 25.4 7.62 270) (size 1.5 1.5) (drill 1) (layers "*.Cu" "*.Mask")
      (net 37 "/Display/Disp_SPI_SCK") (pinfunction "SCLK") (pintype "input"))
    (pad "18" thru_hole circle (at 25.4 5.08 270) (size 1.5 1.5) (drill 1) (layers "*.Cu" "*.Mask")
      (net 40 "/Display/Disp_CS") (pinfunction "-CS") (pintype "input"))
    (pad "19" thru_hole circle (at 25.4 2.54 270) (size 1.5 1.5) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GNDD") (pinfunction "SA0") (pintype "input"))
    (pad "20" thru_hole circle (at 25.4 0 270) (size 1.5 1.5) (drill 1) (layers "*.Cu" "*.Mask")
      (net 41 "/Display/Disp_Reset") (pinfunction "-RST") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Display.3dshapes/EA_DOGS104X-A.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "wago-footprints:CONN_233-503_WAG" (layer "F.Cu")
    (at 100.33 120.65)
    (tags "233-503 ")
    (property "Sheetfile" "out_anforderung.kicad_sch")
    (property "Sheetname" "Out_Anforderung")
    (property "ki_keywords" "233-503")
    (attr through_hole)
    (fp_text reference "J13" (at 2.399995 2.5 unlocked) (layer "F.SilkS"))
    (fp_text value "Anforderung" (at 2.54 17.78 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.399995 2.5 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 93 "/Steuerung/Out_Anforderung/Anf_Out_0") (pinfunction "1") (pintype "unspecified"))
    (pad "2" thru_hole circle (at 0 5) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 93 "/Steuerung/Out_Anforderung/Anf_Out_0") (pinfunction "2") (pintype "unspecified"))
    (pad "3" thru_hole circle (at 2.54 0) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 94 "/Steuerung/Out_Anforderung/Anf_Out_1") (pinfunction "3") (pintype "unspecified"))
    (pad "4" thru_hole circle (at 2.54 5) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 94 "/Steuerung/Out_Anforderung/Anf_Out_1") (pinfunction "4") (pintype "unspecified"))
    (pad "5" thru_hole circle (at 5.08 0) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 2 "GNDD") (pinfunction "5") (pintype "unspecified"))
    (pad "6" thru_hole circle (at 5.08 5) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 2 "GNDD") (pinfunction "6") (pintype "unspecified"))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (layer "F.Cu")
    (at 111.76 109.22)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.8) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm_M3_DIN965_Pad" (at 0 3.8) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Package_DIP:DIP-6_W7.62mm" (layer "F.Cu")
    (at 114.285 52.08 -90)
    (descr "6-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "input.kicad_sch")
    (property "Sheetname" "Stockwerkverteiler")
    (property "ki_description" "Optocoupler, Phototransistor Output, with Base Connection, Vce 70V, CTR 100%, Viso 5000V, DIP6")
    (property "ki_keywords" "NPN DC Optocoupler Base Connected")
    (attr through_hole)
    (fp_text reference "U4" (at 3.81 -2.33 90) (layer "F.SilkS"))
    (fp_text value "4N35" (at 3.81 7.41 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 79 "Net-(R16-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 20 "/Steuerung/Relais-Ansteuerung/Rls_Out_Status_Pumpe") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 91 "unconnected-(U4-NC-Pad3)") (pinfunction "NC") (pintype "no_connect"))
    (pad "4" thru_hole oval (at 7.62 5.08 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 55 "/Steuerung/Stockwerkverteiler/Pumpe Status E") (pintype "passive"))
    (pad "5" thru_hole oval (at 7.62 2.54 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 54 "/Steuerung/Stockwerkverteiler/Pumpe Status C") (pintype "passive"))
    (pad "6" thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 92 "unconnected-(U4-Pad6)") (pintype "passive+no_connect"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-6_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (layer "F.Cu")
    (at 112.014476 132.491077)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.8) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm_M3_DIN965_Pad" (at 0 3.8) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Package_DIP:DIP-40_W15.24mm" (layer "F.Cu")
    (at 53.34 100.33 90)
    (descr "40-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil")
    (property "Field2" "")
    (property "Sheetfile" "Steuerung.kicad_sch")
    (property "Sheetname" "Steuerung")
    (property "ki_description" "20MHz, 128kB Flash, 16kB SRAM, 4kB EEPROM, JTAG, DIP-40")
    (property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower")
    (attr through_hole)
    (fp_text reference "U3" (at 7.62 -2.33 90) (layer "F.SilkS"))
    (fp_text value "ATmega1284P-P" (at 7.62 50.59 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.62 24.13 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 36 "/Steuerung/Strg_Display_Light") (pinfunction "PB0") (pintype "bidirectional"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 34 "/Steuerung/Strg_Display_Reset") (pinfunction "PB1") (pintype "bidirectional"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 35 "/Steuerung/Strg_Display_CS") (pinfunction "PB2") (pintype "bidirectional"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 82 "unconnected-(U3-PB3-Pad4)") (pinfunction "PB3") (pintype "bidirectional+no_connect"))
    (pad "5" thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 83 "unconnected-(U3-PB4-Pad5)") (pinfunction "PB4") (pintype "bidirectional+no_connect"))
    (pad "6" thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "SPI_MOSI") (pinfunction "PB5") (pintype "bidirectional"))
    (pad "7" thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 5 "SPI_MISO") (pinfunction "PB6") (pintype "bidirectional"))
    (pad "8" thru_hole oval (at 0 17.78 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 6 "SPI_SCK") (pinfunction "PB7") (pintype "bidirectional"))
    (pad "9" thru_hole oval (at 0 20.32 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 56 "Net-(J5-Pin_5)") (pinfunction "~{RESET}") (pintype "input"))
    (pad "10" thru_hole oval (at 0 22.86 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+3.3V") (pinfunction "VCC") (pintype "power_in"))
    (pad "11" thru_hole oval (at 0 25.4 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GNDD") (pinfunction "GND") (pintype "power_in"))
    (pad "12" thru_hole oval (at 0 27.94 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 58 "Net-(U3-XTAL2)") (pinfunction "XTAL2") (pintype "output"))
    (pad "13" thru_hole oval (at 0 30.48 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 57 "Net-(U3-XTAL1)") (pinfunction "XTAL1") (pintype "input"))
    (pad "14" thru_hole oval (at 0 33.02 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 50 "/Steuerung/RS485/ModBus_Rx") (pinfunction "PD0") (pintype "bidirectional"))
    (pad "15" thru_hole oval (at 0 35.56 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 52 "/Steuerung/RS485/Modbus_Tx") (pinfunction "PD1") (pintype "bidirectional"))
    (pad "16" thru_hole oval (at 0 38.1 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 84 "unconnected-(U3-PD2-Pad16)") (pinfunction "PD2") (pintype "bidirectional+no_connect"))
    (pad "17" thru_hole oval (at 0 40.64 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 85 "unconnected-(U3-PD3-Pad17)") (pinfunction "PD3") (pintype "bidirectional+no_connect"))
    (pad "18" thru_hole oval (at 0 43.18 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 51 "/Steuerung/RS485/ModBus_SE") (pinfunction "PD4") (pintype "bidirectional"))
    (pad "19" thru_hole oval (at 0 45.72 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 86 "unconnected-(U3-PD5-Pad19)") (pinfunction "PD5") (pintype "bidirectional+no_connect"))
    (pad "20" thru_hole oval (at 0 48.26 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 87 "unconnected-(U3-PD6-Pad20)") (pinfunction "PD6") (pintype "bidirectional+no_connect"))
    (pad "21" thru_hole oval (at 15.24 48.26 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 88 "unconnected-(U3-PD7-Pad21)") (pinfunction "PD7") (pintype "bidirectional+no_connect"))
    (pad "22" thru_hole oval (at 15.24 45.72 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 21 "/Steuerung/Sensoren/Sen_Sensor_Aussen") (pinfunction "PC0") (pintype "bidirectional"))
    (pad "23" thru_hole oval (at 15.24 43.18 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 24 "/Steuerung/Sensoren/Sen_Sensor_RL1") (pinfunction "PC1") (pintype "bidirectional"))
    (pad "24" thru_hole oval (at 15.24 40.64 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 25 "/Steuerung/Sensoren/Sen_Sensor_RL2") (pinfunction "PC2") (pintype "bidirectional"))
    (pad "25" thru_hole oval (at 15.24 38.1 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 22 "/Steuerung/Sensoren/Sen_Sensor_VL1") (pinfunction "PC3") (pintype "bidirectional"))
    (pad "26" thru_hole oval (at 15.24 35.56 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 23 "/Steuerung/Sensoren/Sen_Sensor_VL2") (pinfunction "PC4") (pintype "bidirectional"))
    (pad "27" thru_hole oval (at 15.24 33.02 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 47 "/Steuerung/Out_Anforderung/Out_Anf0") (pinfunction "PC5") (pintype "bidirectional"))
    (pad "28" thru_hole oval (at 15.24 30.48 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 48 "/Steuerung/Out_Anforderung/Out_Anf1") (pinfunction "PC6") (pintype "bidirectional"))
    (pad "29" thru_hole oval (at 15.24 27.94 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 89 "unconnected-(U3-PC7-Pad29)") (pinfunction "PC7") (pintype "bidirectional+no_connect"))
    (pad "30" thru_hole oval (at 15.24 25.4 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+3.3V") (pinfunction "AVCC") (pintype "power_in"))
    (pad "31" thru_hole oval (at 15.24 22.86 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GNDD") (pinfunction "GND") (pintype "passive"))
    (pad "32" thru_hole oval (at 15.24 20.32 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 90 "unconnected-(U3-AREF-Pad32)") (pinfunction "AREF") (pintype "passive+no_connect"))
    (pad "33" thru_hole oval (at 15.24 17.78 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 46 "/Steuerung/Relais-Ansteuerung/Rls_Mischer_auf") (pinfunction "PA7") (pintype "bidirectional"))
    (pad "34" thru_hole oval (at 15.24 15.24 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 45 "/Steuerung/Relais-Ansteuerung/Rls_Mischer_zu") (pinfunction "PA6") (pintype "bidirectional"))
    (pad "35" thru_hole oval (at 15.24 12.7 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 44 "/Steuerung/Relais-Ansteuerung/Rls_Pumpe_an") (pinfunction "PA5") (pintype "bidirectional"))
    (pad "36" thru_hole oval (at 15.24 10.16 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 33 "/Steuerung/Strg_Taster_light") (pinfunction "PA4") (pintype "bidirectional"))
    (pad "37" thru_hole oval (at 15.24 7.62 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 32 "/Steuerung/Strg_Taster_mnu") (pinfunction "PA3") (pintype "bidirectional"))
    (pad "38" thru_hole oval (at 15.24 5.08 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 31 "/Steuerung/Strg_Taster_dwn") (pinfunction "PA2") (pintype "bidirectional"))
    (pad "39" thru_hole oval (at 15.24 2.54 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 30 "/Steuerung/Strg_Taster_up") (pinfunction "PA1") (pintype "bidirectional"))
    (pad "40" thru_hole oval (at 15.24 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 43 "/Steuerung/Stockwerkverteiler/SWV_IN_Anforderung") (pinfunction "PA0") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-40_W15.24mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (at 73.66 43.18 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Feld2" "")
    (property "Sheetfile" "sensoren.kicad_sch")
    (property "Sheetname" "Sensoren")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R18" (at 5.08 -2.37 90) (layer "F.SilkS"))
    (fp_text value "4k7" (at 5.08 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+3.3V") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 22 "/Steuerung/Sensoren/Sen_Sensor_VL1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (layer "F.Cu")
    (at 190.5 50.8)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.8) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm_M3_DIN965_Pad" (at 0 3.8) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal" (layer "F.Cu")
    (at 57.15 48.26 180)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (property "Feld2" "")
    (property "Sheetfile" "relais.kicad_sch")
    (property "Sheetname" "Relais-Ansteuerung")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "400V 1A General Purpose Rectifier Diode, DO-41")
    (property "ki_keywords" "diode")
    (attr through_hole)
    (fp_text reference "D5" (at 5.08 -2.47) (layer "F.SilkS"))
    (fp_text value "1N4004" (at 5.08 2.47) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 5.47 0) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 4 "+12V") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 180) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 60 "Net-(D2-K)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_IDC:IDC-Header_2x04_P2.54mm_Vertical" (layer "F.Cu")
    (at 72.39 73.66 90)
    (descr "Through hole IDC box header, 2x04, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0")
    (tags "Through hole vertical IDC box header THT 2x04 2.54mm double row")
    (property "Sheetfile" "FBH_Mischer.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x08, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J1" (at 1.27 -6.1 90) (layer "F.SilkS"))
    (fp_text value "Eingabe" (at 1.27 15.24 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 1.27 3.81) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.1470588235)
      (net 30 "/Steuerung/Strg_Taster_up") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 33 "/Steuerung/Strg_Taster_light") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 31 "/Steuerung/Strg_Taster_dwn") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 32 "/Steuerung/Strg_Taster_mnu") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole circle (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 63 "unconnected-(J1-Pin_5-Pad5)") (pinfunction "Pin_5") (pintype "passive+no_connect"))
    (pad "6" thru_hole circle (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 64 "unconnected-(J1-Pin_6-Pad6)") (pinfunction "Pin_6") (pintype "passive+no_connect"))
    (pad "7" thru_hole circle (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "+3.3V") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole circle (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GNDD") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_IDC.3dshapes/IDC-Header_2x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (at 43.18 54.61 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Feld2" "")
    (property "Sheetfile" "relais.kicad_sch")
    (property "Sheetname" "Relais-Ansteuerung")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R13" (at 5.08 -2.37) (layer "F.SilkS"))
    (fp_text value "680" (at 5.08 2.37) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+3.3V") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 61 "Net-(D2-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (layer "F.Cu")
    (at 38.1 109.22)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.8) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm_M3_DIN965_Pad" (at 0 3.8) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (at 33.02 71.12)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "input.kicad_sch")
    (property "Sheetname" "Stockwerkverteiler")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R16" (at 5.08 -2.37) (layer "F.SilkS"))
    (fp_text value "1k" (at 1.27 -2.54) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+3.3V") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 79 "Net-(R16-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (layer "F.Cu")
    (at 112.024263 77.751457)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.8) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm_M3_DIN965_Pad" (at 0 3.8) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (at 61.75 43.18 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Feld2" "")
    (property "Sheetfile" "sensoren.kicad_sch")
    (property "Sheetname" "Sensoren")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R22" (at 5.08 -2.37 90) (layer "F.SilkS"))
    (fp_text value "4k7" (at 5.08 2.37 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+3.3V") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 25 "/Steuerung/Sensoren/Sen_Sensor_RL2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (at 97.79 53.34 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "input.kicad_sch")
    (property "Sheetname" "Stockwerkverteiler")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R17" (at 5.08 -2.37 90) (layer "F.SilkS"))
    (fp_text value "10k" (at 5.08 2.37 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 15 "/Steuerung/Stockwerkverteiler/W-Anf.-In") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 43 "/Steuerung/Stockwerkverteiler/SWV_IN_Anforderung") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (layer "F.Cu")
    (at 40.64 44.45)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.8) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm_M3_DIN965_Pad" (at 0 3.8) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (at 65.8 43.18 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Feld2" "")
    (property "Sheetfile" "sensoren.kicad_sch")
    (property "Sheetname" "Sensoren")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R21" (at 5.08 -2.37 90) (layer "F.SilkS"))
    (fp_text value "4k7" (at 5.08 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+3.3V") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 24 "/Steuerung/Sensoren/Sen_Sensor_RL1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (layer "F.Cu")
    (at 196.85 25.4)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.8) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm_M3_DIN965_Pad" (at 0 3.8) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (layer "F.Cu")
    (at 88.9 78.74)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.8) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm_M3_DIN965_Pad" (at 0 3.8) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (at 86.36 44.45)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "input.kicad_sch")
    (property "Sheetname" "Stockwerkverteiler")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R15" (at 5.08 -2.37) (layer "F.SilkS"))
    (fp_text value "47k" (at 2.54 -2.54) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+3.3V") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 15 "/Steuerung/Stockwerkverteiler/W-Anf.-In") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm" (layer "F.Cu")
    (at 88.94 105.41)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
    (property "Field2" "")
    (property "Sheetfile" "Steuerung.kicad_sch")
    (property "Sheetname" "Steuerung")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C5" (at -0.04 -2.25) (layer "F.SilkS"))
    (fp_text value "22pF" (at 3.77 -2.54) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GNDD") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 57 "Net-(U3-XTAL1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_IDC:IDC-Header_2x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 85.09 124.46 90)
    (descr "Through hole IDC box header, 2x03, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0")
    (tags "Through hole vertical IDC box header THT 2x03 2.54mm double row")
    (property "Field2" "")
    (property "Sheetfile" "Steuerung.kicad_sch")
    (property "Sheetname" "Steuerung")
    (property "ki_description" "Generic connector, double row, 02x03, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J5" (at 1.27 -6.1 90) (layer "F.SilkS"))
    (fp_text value "SPI" (at -6.35 2.54 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 2.54) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.1470588235)
      (net 5 "SPI_MISO") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 69 "unconnected-(J5-Pin_2-Pad2)") (pinfunction "Pin_2") (pintype "passive+no_connect"))
    (pad "3" thru_hole circle (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "SPI_SCK") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "SPI_MOSI") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole circle (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 56 "Net-(J5-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GNDD") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_IDC.3dshapes/IDC-Header_2x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "lokal2:prox-sense-cap-directional-19.05mm" (layer "F.Cu")
    (at 196.215 69.2)
    (property "Feld2" "")
    (property "Sheetfile" "eingabe.kicad_sch")
    (property "Sheetname" "Eingabe")
    (zone_connect 2)
    (attr smd)
    (fp_text reference "T1" (at 0 -0.5 unlocked) (layer "F.SilkS"))
    (fp_text value "~" (at 0 1 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 -7.62) (size 0.8 0.8) (drill 0.4) (layers "*.Cu") (remove_unused_layers) (keep_end_layers) (zone_layer_connections)
      (net 95 "/Eingabe/Touch_S1") (pinfunction "Sensor") (pintype "bidirectional"))
  )
  (footprint "Package_TO_SOT_THT:TO-92_Inline_Wide" (layer "F.Cu")
    (at 114.3 101.6 90)
    (descr "TO-92 leads in-line, wide, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "out_anforderung.kicad_sch")
    (property "Sheetname" "Out_Anforderung")
    (property "ki_description" "0.8A Ic, 45V Vce, NPN Transistor, TO-92")
    (property "ki_keywords" "NPN Transistor")
    (attr through_hole)
    (fp_text reference "Q6" (at 2.54 -3.56 90) (layer "F.SilkS"))
    (fp_text value "BC337" (at 2.54 2.79 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.5 1.5) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 94 "/Steuerung/Out_Anforderung/Anf_Out_1") (pinfunction "C") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 90) (size 1.5 1.5) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(Q6-B)") (pinfunction "B") (pintype "input"))
    (pad "3" thru_hole circle (at 5.08 0 90) (size 1.5 1.5) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GNDD") (pinfunction "E") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline_Wide.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (layer "F.Cu")
    (at 102.87 69.85)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.8) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm_M3_DIN965_Pad" (at 0 3.8) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "wago-footprints:CONN_233-504_WAG" (layer "F.Cu")
    (at 101.6 36.83 180)
    (tags "233-504 ")
    (property "Sheetfile" "input.kicad_sch")
    (property "Sheetname" "Stockwerkverteiler")
    (property "ki_keywords" "233-504")
    (attr through_hole)
    (fp_text reference "J9" (at 3.52999 2.5 180 unlocked) (layer "F.SilkS"))
    (fp_text value "FBH-Verteiler" (at 2.54 15.24 180 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.52999 2.5 180 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 2 "GNDD") (pinfunction "1") (pintype "unspecified"))
    (pad "2" thru_hole circle (at 0 5 180) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 2 "GNDD") (pinfunction "2") (pintype "unspecified"))
    (pad "3" thru_hole circle (at 2.54 0 180) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 15 "/Steuerung/Stockwerkverteiler/W-Anf.-In") (pinfunction "3") (pintype "unspecified"))
    (pad "4" thru_hole circle (at 2.54 5 180) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 15 "/Steuerung/Stockwerkverteiler/W-Anf.-In") (pinfunction "4") (pintype "unspecified"))
    (pad "5" thru_hole circle (at 5.08 0 180) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 54 "/Steuerung/Stockwerkverteiler/Pumpe Status C") (pinfunction "5") (pintype "unspecified"))
    (pad "6" thru_hole circle (at 5.08 5 180) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 54 "/Steuerung/Stockwerkverteiler/Pumpe Status C") (pinfunction "6") (pintype "unspecified"))
    (pad "7" thru_hole circle (at 7.62 0 180) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 55 "/Steuerung/Stockwerkverteiler/Pumpe Status E") (pinfunction "7") (pintype "unspecified"))
    (pad "8" thru_hole circle (at 7.62 5 180) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 55 "/Steuerung/Stockwerkverteiler/Pumpe Status E") (pinfunction "8") (pintype "unspecified"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (at 43.18 62.23 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Feld2" "")
    (property "Sheetfile" "relais.kicad_sch")
    (property "Sheetname" "Relais-Ansteuerung")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R14" (at 5.08 -2.37) (layer "F.SilkS"))
    (fp_text value "680" (at 1.27 -2.54) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+3.3V") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(D3-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (layer "F.Cu")
    (at 130.175 92.06)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.8) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm_M3_DIN965_Pad" (at 0 3.8) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (layer "F.Cu")
    (at 203.835 92.06)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.8) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm_M3_DIN965_Pad" (at 0 3.8) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Package_TO_SOT_THT:TO-92_Inline_Wide" (layer "F.Cu")
    (at 60.4 60.96 90)
    (descr "TO-92 leads in-line, wide, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Feld2" "")
    (property "Sheetfile" "relais.kicad_sch")
    (property "Sheetname" "Relais-Ansteuerung")
    (property "ki_description" "0.8A Ic, 45V Vce, NPN Transistor, TO-92")
    (property "ki_keywords" "NPN Transistor")
    (attr through_hole)
    (fp_text reference "Q4" (at 2.54 -3.56 90) (layer "F.SilkS"))
    (fp_text value "BC337" (at 2.54 2.79 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.5 1.5) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 62 "Net-(D3-K)") (pinfunction "C") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 90) (size 1.5 1.5) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(Q4-B)") (pinfunction "B") (pintype "input"))
    (pad "3" thru_hole circle (at 5.08 0 90) (size 1.5 1.5) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GNDD") (pinfunction "E") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline_Wide.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (at 35.56 34.29 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Feld2" "")
    (property "Sheetfile" "relais.kicad_sch")
    (property "Sheetname" "Relais-Ansteuerung")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr through_hole)
    (fp_text reference "D3" (at -2.54 -1.27) (layer "F.SilkS"))
    (fp_text value "M-auf" (at 1.27 2.96) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 62 "Net-(D3-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(D3-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (at 90.17 64.77 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Feld2" "")
    (property "Sheetfile" "relais.kicad_sch")
    (property "Sheetname" "Relais-Ansteuerung")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R9" (at 5.08 -2.37) (layer "F.SilkS") hide)
    (fp_text value "1k8" (at 2.54 -2.06) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 44 "/Steuerung/Relais-Ansteuerung/Rls_Pumpe_an") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(Q2-B)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (layer "F.Cu")
    (at 180.975 61.58)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.8) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm_M3_DIN965_Pad" (at 0 3.8) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal" (layer "F.Cu")
    (at 96.52 48.26)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (property "Sheetfile" "input.kicad_sch")
    (property "Sheetname" "Stockwerkverteiler")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "100V 0.15A standard switching diode, DO-35")
    (property "ki_keywords" "diode")
    (attr through_hole)
    (fp_text reference "D8" (at 3.81 -2.12) (layer "F.SilkS"))
    (fp_text value "1N4148" (at 3.81 2.12) (layer "F.SilkS"))
    (fp_text user "K" (at 0 -1.8) (layer "F.SilkS"))
    (fp_text user "K" (at 0 -1.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 4.11 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 15 "/Steuerung/Stockwerkverteiler/W-Anf.-In") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GNDD") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-92_Inline_Wide" (layer "F.Cu")
    (at 108.31 101.6 90)
    (descr "TO-92 leads in-line, wide, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "out_anforderung.kicad_sch")
    (property "Sheetname" "Out_Anforderung")
    (property "ki_description" "0.8A Ic, 45V Vce, NPN Transistor, TO-92")
    (property "ki_keywords" "NPN Transistor")
    (attr through_hole)
    (fp_text reference "Q5" (at 2.54 -3.56 90) (layer "F.SilkS"))
    (fp_text value "BC337" (at 2.54 2.79 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.5 1.5) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 93 "/Steuerung/Out_Anforderung/Anf_Out_0") (pinfunction "C") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 90) (size 1.5 1.5) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(Q5-B)") (pinfunction "B") (pintype "input"))
    (pad "3" thru_hole circle (at 5.08 0 90) (size 1.5 1.5) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GNDD") (pinfunction "E") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline_Wide.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "wago-footprints:CONN_233-503_WAG" (layer "F.Cu")
    (at 85.09 36.83 180)
    (tags "233-503 ")
    (property "Feld2" "")
    (property "Sheetfile" "sensoren.kicad_sch")
    (property "Sheetname" "Sensoren")
    (property "ki_keywords" "233-503")
    (attr through_hole)
    (fp_text reference "J11" (at 2.399995 2.5 180 unlocked) (layer "F.SilkS"))
    (fp_text value "Aussentemperatur" (at 2.399995 15.24 180 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.399995 2.5 180 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 1 "+3.3V") (pinfunction "1") (pintype "unspecified"))
    (pad "2" thru_hole circle (at 0 5 180) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 1 "+3.3V") (pinfunction "2") (pintype "unspecified"))
    (pad "3" thru_hole circle (at 2.54 0 180) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 21 "/Steuerung/Sensoren/Sen_Sensor_Aussen") (pinfunction "3") (pintype "unspecified"))
    (pad "4" thru_hole circle (at 2.54 5 180) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 21 "/Steuerung/Sensoren/Sen_Sensor_Aussen") (pinfunction "4") (pintype "unspecified"))
    (pad "5" thru_hole circle (at 5.08 0 180) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 2 "GNDD") (pinfunction "5") (pintype "unspecified"))
    (pad "6" thru_hole circle (at 5.08 5 180) (size 1.6256 1.6256) (drill 1.1176) (layers "*.Cu" "*.Mask")
      (net 2 "GNDD") (pinfunction "6") (pintype "unspecified"))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (layer "F.Cu")
    (at 151.765 61.58)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.8) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm_M3_DIN965_Pad" (at 0 3.8) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "B.Cu")
    (at 173.41 90.995 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Feld2" "")
    (property "Sheetfile" "eingabe.kicad_sch")
    (property "Sheetname" "Eingabe")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R5" (at -2.745 0.055 -270) (layer "B.SilkS"))
    (fp_text value "10k" (at 0 -1.43 -270) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 98 "/Eingabe/Touch_S4") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "Net-(U1-MTI4)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D6.3mm_P2.50mm" (layer "B.Cu")
    (at 129.54 45.72 180)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (property "Feld2" "")
    (property "Sheetfile" "spi.kicad_sch")
    (property "Sheetname" "Display")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C8" (at 1.25 4.4) (layer "B.SilkS"))
    (fp_text value "1µ" (at 1.25 -4.4) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(U2-VOUT)") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-92_Inline_Wide" (layer "B.Cu")
    (at 191.77 44.45 180)
    (descr "TO-92 leads in-line, wide, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Feld2" "")
    (property "Sheetfile" "spi.kicad_sch")
    (property "Sheetname" "Display")
    (property "ki_description" "0.8A Ic, 45V Vce, NPN Transistor, TO-92")
    (property "ki_keywords" "NPN Transistor")
    (attr through_hole)
    (fp_text reference "Q1" (at 2.54 3.56) (layer "B.SilkS"))
    (fp_text value "BC337" (at 2.54 -2.79) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.5 1.5) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 72 "Net-(Q1-C)") (pinfunction "C") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 180) (size 1.5 1.5) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(Q1-B)") (pinfunction "B") (pintype "input"))
    (pad "3" thru_hole circle (at 5.08 0 180) (size 1.5 1.5) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GNDD") (pinfunction "E") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline_Wide.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "B.Cu")
    (at 178.49 90.995 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Feld2" "")
    (property "Sheetfile" "eingabe.kicad_sch")
    (property "Sheetname" "Eingabe")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R3" (at -2.745 0.055 90) (layer "B.SilkS"))
    (fp_text value "10k" (at 0 -1.43 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 96 "/Eingabe/Touch_S2") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 75 "Net-(U1-MTI1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Potentiometer_THT:Potentiometer_ACP_CA9-H5_Horizontal" (layer "B.Cu")
    (at 188 36.765)
    (descr "Potentiometer, horizontal, ACP CA9-H5, http://www.acptechnologies.com/wp-content/uploads/2017/05/02-ACP-CA9-CE9.pdf")
    (tags "Potentiometer horizontal ACP CA9-H5")
    (property "Feld2" "")
    (property "Sheetfile" "spi.kicad_sch")
    (property "Sheetname" "Display")
    (property "ki_description" "Trim-potentiometer")
    (property "ki_keywords" "resistor variable trimpot trimmer")
    (attr through_hole)
    (fp_text reference "RV2" (at 9.43 0.685) (layer "B.SilkS"))
    (fp_text value "Trim_100" (at 0 -8.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 2.4 -2.5) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.34 2.34) (drill 1.3) (layers "*.Cu" "*.Mask")
      (net 81 "unconnected-(RV2-Pad1)") (pinfunction "1") (pintype "passive+no_connect"))
    (pad "2" thru_hole circle (at 5 -2.5) (size 2.34 2.34) (drill 1.3) (layers "*.Cu" "*.Mask")
      (net 78 "Net-(R6-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 -5) (size 2.34 2.34) (drill 1.3) (layers "*.Cu" "*.Mask")
      (net 17 "Net-(U2-A1{slash}AGR{slash}AERW)") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_ACP_CA9-H5_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Potentiometer_SMD:Potentiometer_Bourns_3269P_Horizontal" (layer "B.Cu")
    (at 193.675 92.06 180)
    (descr "Potentiometer, horizontal, Bourns 3269P, https://www.bourns.com/docs/Product-Datasheets/3269.pdf")
    (tags "Potentiometer horizontal Bourns 3269P")
    (property "Feld2" "")
    (property "Sheetfile" "eingabe.kicad_sch")
    (property "Sheetname" "Eingabe")
    (property "ki_description" "Trim-potentiometer")
    (property "ki_keywords" "resistor variable trimpot trimmer")
    (attr smd)
    (fp_text reference "RV1" (at 0 4.425) (layer "B.SilkS"))
    (fp_text value "Trim_100k" (at 0 -4.425) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at -0.05 0) (layer "B.Fab"))
    (pad "1" smd rect (at 3.2 2.54 180) (size 3.3 1.19) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GNDD") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at -3.2 0 180) (size 3.3 1.19) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 80 "Net-(U1-MTSA)") (pinfunction "2") (pintype "passive"))
    (pad "3" smd rect (at 3.2 -2.54 180) (size 3.3 1.19) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "+3.3V") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_SMD.3dshapes/Potentiometer_Bourns_3269P_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_IDC:IDC-Header_2x05_P2.54mm_Vertical" (layer "B.Cu")
    (at 138.43 27.94 180)
    (descr "Through hole IDC box header, 2x05, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0")
    (tags "Through hole vertical IDC box header THT 2x05 2.54mm double row")
    (property "Sheetfile" "FBH_Mischer.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x10, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J4" (at 1.27 6.1) (layer "B.SilkS"))
    (fp_text value "Conn_01x10_Pin" (at 1.27 -16.26) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 -5.08 90) (layer "B.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.1470588235)
      (net 1 "+3.3V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "+5V") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GNDD") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at 2.54 -2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 41 "/Display/Disp_Reset") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole circle (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 40 "/Display/Disp_CS") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle (at 2.54 -5.08 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 37 "/Display/Disp_SPI_SCK") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole circle (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 38 "/Display/Disp_SPI_MOSI") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole circle (at 2.54 -7.62 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 39 "/Display/SPI_MISO") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole circle (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 42 "/Display/Disp_Light") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole circle (at 2.54 -10.16 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 68 "unconnected-(J4-Pin_10-Pad10)") (pinfunction "Pin_10") (pintype "passive+no_connect"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_IDC.3dshapes/IDC-Header_2x05_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D6.3mm_P2.50mm" (layer "B.Cu")
    (at 129.54 36.83 180)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (property "Feld2" "")
    (property "Sheetfile" "spi.kicad_sch")
    (property "Sheetname" "Display")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C1" (at 1.25 4.4) (layer "B.SilkS"))
    (fp_text value "1µ" (at 1.25 -4.4) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+3.3V") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_IDC:IDC-Header_2x04_P2.54mm_Vertical" (layer "B.Cu")
    (at 140.335 90.17 -90)
    (descr "Through hole IDC box header, 2x04, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0")
    (tags "Through hole vertical IDC box header THT 2x04 2.54mm double row")
    (property "Sheetfile" "FBH_Mischer.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x08, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J3" (at 0 2.54 90) (layer "B.SilkS"))
    (fp_text value "Conn_01x08_Pin" (at 1.27 -13.72 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 -3.81) (layer "B.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.1470588235)
      (net 26 "/Eingabe/Taster_up") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 29 "/Eingabe/Taster_light") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 27 "/Eingabe/Taster_dwn") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at 2.54 -2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 28 "/Eingabe/Taster_mnu") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole circle (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 66 "unconnected-(J3-Pin_5-Pad5)") (pinfunction "Pin_5") (pintype "passive+no_connect"))
    (pad "6" thru_hole circle (at 2.54 -5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 67 "unconnected-(J3-Pin_6-Pad6)") (pinfunction "Pin_6") (pintype "passive+no_connect"))
    (pad "7" thru_hole circle (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "+3.3V") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole circle (at 2.54 -7.62 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GNDD") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_IDC.3dshapes/IDC-Header_2x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "B.Cu")
    (at 167.005 90.995 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Feld2" "")
    (property "Sheetfile" "eingabe.kicad_sch")
    (property "Sheetname" "Eingabe")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at -2.745 0 90) (layer "B.SilkS"))
    (fp_text value "10k" (at 0 -1.43 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -360) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 49 "Guard") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 73 "Net-(U1-MTI2{slash}GUARD)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:TSSOP-14_4.4x5mm_P0.65mm" (layer "B.Cu")
    (at 161.1975 91.47 180)
    (descr "TSSOP, 14 Pin (JEDEC MO-153 Var AB-1 https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSSOP SO")
    (property "Feld2" "")
    (property "Sheetfile" "eingabe.kicad_sch")
    (property "Sheetname" "Eingabe")
    (attr smd)
    (fp_text reference "U1" (at 0 3.45) (layer "B.SilkS"))
    (fp_text value "MTCH105" (at 0 -3.45) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at -1.65 1.21) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.8625 1.95 180) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "+3.3V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd roundrect (at -2.8625 1.3 180) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 74 "Net-(U1-MTI0)") (pinfunction "MTI0") (pintype "input"))
    (pad "3" smd roundrect (at -2.8625 0.65 180) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 75 "Net-(U1-MTI1)") (pinfunction "MTI1") (pintype "input"))
    (pad "4" smd roundrect (at -2.8625 0 180) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "+3.3V") (pinfunction "MTPM") (pintype "input"))
    (pad "5" smd roundrect (at -2.8625 -0.65 180) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 73 "Net-(U1-MTI2{slash}GUARD)") (pinfunction "MTI2/GUARD") (pintype "input"))
    (pad "6" smd roundrect (at -2.8625 -1.3 180) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "Net-(U1-MTI3)") (pinfunction "MTI3") (pintype "input"))
    (pad "7" smd roundrect (at -2.8625 -1.95 180) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "Net-(U1-MTI4)") (pinfunction "MTI4") (pintype "input"))
    (pad "8" smd roundrect (at 2.8625 -1.95 180) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 29 "/Eingabe/Taster_light") (pinfunction "MTO4") (pintype "output"))
    (pad "9" smd roundrect (at 2.8625 -1.3 180) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 26 "/Eingabe/Taster_up") (pinfunction "MTO3") (pintype "output"))
    (pad "10" smd roundrect (at 2.8625 -0.65 180) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GNDD") (pinfunction "MTO2/GC") (pintype "bidirectional"))
    (pad "11" smd roundrect (at 2.8625 0 180) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 80 "Net-(U1-MTSA)") (pinfunction "MTSA") (pintype "input"))
    (pad "12" smd roundrect (at 2.8625 0.65 180) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 28 "/Eingabe/Taster_mnu") (pinfunction "MTO1") (pintype "output"))
    (pad "13" smd roundrect (at 2.8625 1.3 180) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 27 "/Eingabe/Taster_dwn") (pinfunction "MTO0") (pintype "output"))
    (pad "14" smd roundrect (at 2.8625 1.95 180) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GNDD") (pinfunction "VSS") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-14_4.4x5mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "B.Cu")
    (at 181.03 90.995 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Feld2" "")
    (property "Sheetfile" "eingabe.kicad_sch")
    (property "Sheetname" "Eingabe")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R2" (at -2.745 0.055 90) (layer "B.SilkS"))
    (fp_text value "10k" (at 0 -1.43 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 95 "/Eingabe/Touch_S1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 74 "Net-(U1-MTI0)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "B.Cu")
    (at 184.15 41.91 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Feld2" "")
    (property "Sheetfile" "spi.kicad_sch")
    (property "Sheetname" "Display")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R7" (at 5.08 2.37 90) (layer "B.SilkS"))
    (fp_text value "1k8" (at 5.08 -2.37 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(Q1-B)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 42 "/Display/Disp_Light") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "B.Cu")
    (at 170.87 90.995 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Feld2" "")
    (property "Sheetfile" "eingabe.kicad_sch")
    (property "Sheetname" "Eingabe")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R4" (at -2.745 0.055 -270) (layer "B.SilkS"))
    (fp_text value "10k" (at 0 -1.43 -270) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 97 "/Eingabe/Touch_S3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "Net-(U1-MTI3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "B.Cu")
    (at 184.15 27.94 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Feld2" "")
    (property "Sheetfile" "spi.kicad_sch")
    (property "Sheetname" "Display")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R6" (at 5.08 2.37 90) (layer "B.SilkS"))
    (fp_text value "75" (at 5.08 -2.37 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 8 "+5V") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 78 "Net-(R6-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 29.51 20) (end 119.51 140)
    (fill none) (layer "Edge.Cuts"))
  (gr_rect (start 122.61 57.15) (end 211.51 96.52)
    (fill none) (layer "Edge.Cuts"))
  (gr_rect (start 123.88 20.7) (end 201.35 53.99)
    (fill none) (layer "Edge.Cuts"))
  (gr_text "6U07151008139_6U-151008_DB" (at 60.96 146.05) (layer "F.Cu"))
  (gr_text "D" (at 82.690005 25.4 90) (layer "F.SilkS"))
  (gr_text "+" (at 72.39 26.67 90) (layer "F.SilkS"))
  (gr_text "C" (at 99.06 24.13 180) (layer "F.SilkS"))
  (gr_text "+" (at 85.09 25.4 90) (layer "F.SilkS"))
  (gr_text "GND" (at 102.87 24.13 180) (layer "F.SilkS"))
  (gr_text "GND" (at 60.96 134.62 90) (layer "F.SilkS"))
  (gr_text "Anf 1" (at 102.87 134.62 90) (layer "F.SilkS"))
  (gr_text "C" (at 96.52 24.13 180) (layer "F.SilkS"))
  (gr_text "FBH_Mischer A2" (at 200.66 49.53 90) (layer "F.SilkS"))
  (gr_text "zu" (at 46.99 26.67 90) (layer "F.SilkS"))
  (gr_text "RL2" (at 62.23 26.67 90) (layer "F.SilkS"))
  (gr_text "Anf 0" (at 100.33 134.62 90) (layer "F.SilkS"))
  (gr_text "RL1" (at 64.77 26.67 90) (layer "F.SilkS"))
  (gr_text "Pu" (at 49.53 25.4 90) (layer "F.SilkS"))
  (gr_text "GND" (at 80.01 24.13 90) (layer "F.SilkS"))
  (gr_text "FBH_Mischer A2" (at 118.11 45.72 90) (layer "F.SilkS"))
  (gr_text "auf" (at 44.45 26.67 90) (layer "F.SilkS"))
  (gr_text "GND" (at 59.69 24.13 90) (layer "F.SilkS"))
  (gr_text "B" (at 73.66 134.62 90) (layer "F.SilkS"))
  (gr_text "GND" (at 68.58 134.62 90) (layer "F.SilkS"))
  (gr_text "+12V" (at 52.07 26.67 90) (layer "F.SilkS"))
  (gr_text "+5V" (at 48.26 134.62 90) (layer "F.SilkS"))
  (gr_text "runter" (at 135.255 71.74) (layer "F.SilkS"))
  (gr_text "+12V" (at 50.8 134.62 90) (layer "F.SilkS"))
  (gr_text "FBH_Mischer A1" (at 208.915 80.63 90) (layer "F.SilkS"))
  (gr_text "B" (at 66.04 134.62 90) (layer "F.SilkS"))
  (gr_text "Pumpe" (at 95.25 22.86 180) (layer "F.SilkS"))
  (gr_text "VL2" (at 67.31 26.67 90) (layer "F.SilkS"))
  (gr_text "A" (at 71.12 134.62 90) (layer "F.SilkS"))
  (gr_text "VL1" (at 69.85 26.67 90) (layer "F.SilkS"))
  (gr_text "hoch" (at 193.675 71.74) (layer "F.SilkS"))
  (gr_text "W-Anf" (at 104.14 22.86 180) (layer "F.SilkS"))
  (gr_text "GND" (at 105.41 134.62 90) (layer "F.SilkS"))
  (gr_text "A" (at 63.5 134.62 90) (layer "F.SilkS"))
  (gr_text "E" (at 93.98 24.13 180) (layer "F.SilkS"))
  (gr_text "GND" (at 45.72 134.62 90) (layer "F.SilkS"))
  (zone (net 2) (net_name "GNDD") (layer "F.Cu") (hatch edge 0.5)
    (priority 2)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 123.825 88.25)
        (xy 123.825 95.87)
        (xy 210.185 95.87)
        (xy 210.185 88.25)
      )
    )
  )
  (zone (net 2) (net_name "GNDD") (layers "F&B.Cu") (hatch edge 0.5)
    (priority 3)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 124.46 21.59)
        (xy 200.66 21.59)
        (xy 200.66 53.34)
        (xy 124.46 53.34)
      )
    )
  )
  (zone (net 49) (net_name "Guard") (layers "F&B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 123.825 57.77)
        (xy 210.185 57.77)
        (xy 210.185 86.98)
        (xy 123.825 86.98)
      )
    )
  )
  (zone (net 2) (net_name "GNDD") (layer "B.Cu") (name "GNDD") (hatch edge 0.5)
    (priority 1)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 2) (island_area_min 10))
    (polygon
      (pts
        (xy 29.21 20.32)
        (xy 119.38 20.32)
        (xy 119.38 139.7)
        (xy 29.21 139.7)
      )
    )
  )
)
