(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (title_block
    (comment 4 "AISLER Project ID: SGCQPNMD")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "out1/")
    )
  )
  (net 0 "")
  (net 1 "Net-(J4-Pin_1)")
  (net 2 "Net-(J4-Pin_2)")
  (net 3 "Net-(J4-Pin_3)")
  (net 4 "Guard")
  (footprint "Library:Capacitive_touch_round_12" (layer "F.Cu")
    (at 31.12 147.32 180)
    (property "Feld2" "")
    (property "Sheetfile" "Eingabe.kicad_sch")
    (property "Sheetname" "Eingabe")
    (fp_text reference "T1" (at 0 2.54 180 unlocked) (layer "F.SilkS"))
    (fp_text value "~" (at 0 1 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 180 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 2.54 0 180) (size 1.524 1.524) (drill 0.762) (layers "*.Cu")
      (net 1 "Net-(J4-Pin_1)") (pinfunction "Sensor") (pintype "bidirectional"))
    (pad "2" thru_hole circle (at 6.943825 0.022019 180) (size 1.524 1.524) (drill 0.762) (layers "*.Cu")
      (net 4 "Guard") (pinfunction "Guard") (pintype "bidirectional"))
  )
  (footprint "Library:Capacitive_touch_round_12" (layer "F.Cu")
    (at 51.12 147.32 180)
    (property "Feld2" "")
    (property "Sheetfile" "Eingabe.kicad_sch")
    (property "Sheetname" "Eingabe")
    (fp_text reference "T2" (at 0 -0.5 180 unlocked) (layer "F.SilkS"))
    (fp_text value "~" (at 0 1 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 180 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 2.54 0 180) (size 1.524 1.524) (drill 0.762) (layers "*.Cu")
      (net 2 "Net-(J4-Pin_2)") (pinfunction "Sensor") (pintype "bidirectional"))
    (pad "2" thru_hole circle (at 6.943825 0.022019 180) (size 1.524 1.524) (drill 0.762) (layers "*.Cu")
      (net 4 "Guard") (pinfunction "Guard") (pintype "bidirectional"))
  )
  (footprint "Library:Capacitive_touch_round_12" (layer "F.Cu")
    (at 71.12 147.32 180)
    (property "Feld2" "")
    (property "Sheetfile" "Eingabe.kicad_sch")
    (property "Sheetname" "Eingabe")
    (fp_text reference "T3" (at 0 -0.5 180 unlocked) (layer "F.SilkS"))
    (fp_text value "~" (at 0 1 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 180 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 2.54 0 180) (size 1.524 1.524) (drill 0.762) (layers "*.Cu")
      (net 3 "Net-(J4-Pin_3)") (pinfunction "Sensor") (pintype "bidirectional"))
    (pad "2" thru_hole circle (at 6.943825 0.022019 180) (size 1.524 1.524) (drill 0.762) (layers "*.Cu")
      (net 4 "Guard") (pinfunction "Guard") (pintype "bidirectional"))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical_SMD_Pin1Left" (layer "B.Cu")
    (at 60.325 136.14 -90)
    (descr "surface-mounted straight pin header, 1x04, 2.54mm pitch, single row, style 1 (pin 1 left)")
    (tags "Surface mounted pin header SMD 1x04 2.54mm single row style1 pin1 left")
    (property "Feld2" "")
    (property "Sheetfile" "Eingabe.kicad_sch")
    (property "Sheetname" "Eingabe")
    (property "ki_description" "Generic connector, single row, 01x04, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J4" (at 0 6.14 90) (layer "B.SilkS"))
    (fp_text value "Conn_01x04_Pin" (at 0 -6.14 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -360) (layer "B.Fab"))
    (pad "1" smd rect (at -1.655 3.81 270) (size 2.51 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "Net-(J4-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd rect (at 1.655 1.27 270) (size 2.51 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "Net-(J4-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd rect (at -1.655 -1.27 270) (size 2.51 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "Net-(J4-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd rect (at 1.655 -3.81 270) (size 2.51 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "Guard") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical_SMD_Pin1Left.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 21.12 150.38) (end 28.12 157.38)
    (layer "Edge.Cuts"))
  (gr_line (start 21.12 150.38) (end 21.12 132.38)
    (layer "Edge.Cuts"))
  (gr_line (start 21.12 132.38) (end 81.12 132.38)
    (layer "Edge.Cuts"))
  (gr_line (start 81.12 132.38) (end 81.12 150.38)
    (layer "Edge.Cuts"))
  (gr_line (start 74.12 157.38) (end 28.12 157.38)
    (layer "Edge.Cuts"))
  (gr_line (start 74.12 157.38) (end 81.12 150.38)
    (layer "Edge.Cuts"))
  (zone (net 4) (net_name "Guard") (layers "F&B.Cu") (name "Guard") (hatch full 0.5)
    (connect_pads yes (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 21.59 132.715)
        (xy 21.59 149.86)
        (xy 28.575 156.845)
        (xy 73.66 156.845)
        (xy 80.645 149.86)
        (xy 80.645 132.715)
      )
    )
  )
  (zone (net 4) (net_name "Guard") (layer "B.Cu") (name "Guard") (hatch full 0.5)
    (priority 1)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 80.645 132.715)
        (xy 80.645 150.495)
        (xy 74.295 156.845)
        (xy 28.575 156.845)
        (xy 21.59 149.86)
        (xy 21.59 132.715)
        (xy 77.47 132.715)
      )
    )
  )
)
