(footprint "USB A Plug PCB" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 542BB0AF)
  (descr "USB A Plug on PCB")
  (attr exclude_from_pos_files exclude_from_bom)
  (fp_text reference "REF**" (at 0 -1 180) (layer "F.SilkS"))
  (fp_text value "USB-A" (at 0 -3) (layer "F.Fab"))
  (fp_text user "5V" (at 3.81 -7.5 90 unlocked) (layer "Dwgs.User"))
  (fp_text user "GND" (at -3.81 -6.5 90 unlocked) (layer "Dwgs.User"))
  (fp_text user "D+" (at -1.27 -8.5 90 unlocked) (layer "Dwgs.User"))
  (fp_text user "D-" (at 1.27 -8.5 90 unlocked) (layer "Dwgs.User"))
  (pad "1" connect rect (at 3.81 -5.45) (size 1.9 9.1) (layers "F.Cu" "F.Mask"))
  (pad "2" connect rect (at 1.3 -6) (size 2 8) (layers "F.Cu" "F.Mask"))
  (pad "3" connect rect (at -1.3 -6) (size 2 8) (layers "F.Cu" "F.Mask"))
  (pad "4" connect rect (at -3.81 -5.45) (size 1.9 9.1) (layers "F.Cu" "F.Mask"))
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints not_allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 6 0)
        (xy -6 0)
        (xy -6 -10.5)
        (xy 6 -10.5)
      )
    )
  )
)
