(kicad_sch
	(version 20231120)
	(generator "eeschema")
	(generator_version "8.0")
	(paper "A4")
	(lib_symbols
		(symbol "Connector_Generic:Conn_01x03"
			(pin_names
				(offset 1.016) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at 0 5.08 0)
			)
			(property "Value" "Conn_01x03"
				(at 0 -5.08 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
				(at 0 0 0)
			)
			(property "ki_keywords" "connector"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Connector*:*_1x??_*"
				(at 0 0 0)
			)
			(symbol "Conn_01x03_1_1"
				(rectangle
					(start -1.27 -2.413)
					(end 0 -2.667)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 0.127)
					(end 0 -0.127)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 2.667)
					(end 0 2.413)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 3.81)
					(end 1.27 -3.81)
					(fill
						(type background)
					)
				)
				(pin passive line
					(at -5.08 2.54 0)
					(length 3.81)
					(name "Pin_1")
					(number "1")
				)
				(pin passive line
					(at -5.08 0 0)
					(length 3.81)
					(name "Pin_2")
					(number "2")
				)
				(pin passive line
					(at -5.08 -2.54 0)
					(length 3.81)
					(name "Pin_3")
					(number "3")
				)
			)
		)
		(symbol "Connector_Generic:Conn_01x14"
			(pin_names
				(offset 1.016) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at 0 17.78 0)
			)
			(property "Value" "Conn_01x14"
				(at 0 -20.32 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Generic connector, single row, 01x14, script generated (kicad-library-utils/schlib/autogen/connector/)"
				(at 0 0 0)
			)
			(property "ki_keywords" "connector"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Connector*:*_1x??_*"
				(at 0 0 0)
			)
			(symbol "Conn_01x14_1_1"
				(rectangle
					(start -1.27 -17.653)
					(end 0 -17.907)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 -15.113)
					(end 0 -15.367)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 -12.573)
					(end 0 -12.827)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 -10.033)
					(end 0 -10.287)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 -7.493)
					(end 0 -7.747)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 -4.953)
					(end 0 -5.207)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 -2.413)
					(end 0 -2.667)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 0.127)
					(end 0 -0.127)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 2.667)
					(end 0 2.413)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 5.207)
					(end 0 4.953)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 7.747)
					(end 0 7.493)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 10.287)
					(end 0 10.033)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 12.827)
					(end 0 12.573)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 15.367)
					(end 0 15.113)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 16.51)
					(end 1.27 -19.05)
					(fill
						(type background)
					)
				)
				(pin passive line
					(at -5.08 15.24 0)
					(length 3.81)
					(name "Pin_1")
					(number "1")
				)
				(pin passive line
					(at -5.08 -7.62 0)
					(length 3.81)
					(name "Pin_10")
					(number "10")
				)
				(pin passive line
					(at -5.08 -10.16 0)
					(length 3.81)
					(name "Pin_11")
					(number "11")
				)
				(pin passive line
					(at -5.08 -12.7 0)
					(length 3.81)
					(name "Pin_12")
					(number "12")
				)
				(pin passive line
					(at -5.08 -15.24 0)
					(length 3.81)
					(name "Pin_13")
					(number "13")
				)
				(pin passive line
					(at -5.08 -17.78 0)
					(length 3.81)
					(name "Pin_14")
					(number "14")
				)
				(pin passive line
					(at -5.08 12.7 0)
					(length 3.81)
					(name "Pin_2")
					(number "2")
				)
				(pin passive line
					(at -5.08 10.16 0)
					(length 3.81)
					(name "Pin_3")
					(number "3")
				)
				(pin passive line
					(at -5.08 7.62 0)
					(length 3.81)
					(name "Pin_4")
					(number "4")
				)
				(pin passive line
					(at -5.08 5.08 0)
					(length 3.81)
					(name "Pin_5")
					(number "5")
				)
				(pin passive line
					(at -5.08 2.54 0)
					(length 3.81)
					(name "Pin_6")
					(number "6")
				)
				(pin passive line
					(at -5.08 0 0)
					(length 3.81)
					(name "Pin_7")
					(number "7")
				)
				(pin passive line
					(at -5.08 -2.54 0)
					(length 3.81)
					(name "Pin_8")
					(number "8")
				)
				(pin passive line
					(at -5.08 -5.08 0)
					(length 3.81)
					(name "Pin_9")
					(number "9")
				)
			)
		)
		(symbol "Device:LED"
			(pin_numbers hide)
			(pin_names
				(offset 1.016) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "D"
				(at 0 2.54 0)
			)
			(property "Value" "LED"
				(at 0 -2.54 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Light emitting diode"
				(at 0 0 0)
			)
			(property "ki_keywords" "LED diode"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "LED* LED_SMD:* LED_THT:*"
				(at 0 0 0)
			)
			(symbol "LED_0_1"
				(polyline
					(pts
						(xy -1.27 -1.27) (xy -1.27 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 0) (xy 1.27 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 -1.27) (xy 1.27 1.27) (xy -1.27 0) (xy 1.27 -1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -3.048 -0.762) (xy -4.572 -2.286) (xy -3.81 -2.286) (xy -4.572 -2.286) (xy -4.572 -1.524)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.778 -0.762) (xy -3.302 -2.286) (xy -2.54 -2.286) (xy -3.302 -2.286) (xy -3.302 -1.524)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "LED_1_1"
				(pin passive line
					(at -3.81 0 0)
					(length 2.54)
					(name "K")
					(number "1")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 2.54)
					(name "A")
					(number "2")
				)
			)
		)
		(symbol "Device:R"
			(pin_numbers hide)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 2.032 0 90)
			)
			(property "Value" "R"
				(at 0 0 90)
			)
			(property "Footprint" ""
				(at -1.778 0 90)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Resistor"
				(at 0 0 0)
			)
			(property "ki_keywords" "R res resistor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "R_*"
				(at 0 0 0)
			)
			(symbol "R_0_1"
				(rectangle
					(start -1.016 -2.54)
					(end 1.016 2.54)
					(fill
						(type none)
					)
				)
			)
			(symbol "R_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name "~")
					(number "2")
				)
			)
		)
		(symbol "SamacSys_Parts:IRLML2244TRPBF"
			(pin_names hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "Q"
				(at 11.43 3.81 0)
			)
			(property "Value" "IRLML2244TRPBF"
				(at 11.43 1.27 0)
			)
			(property "Footprint" "SOT95P237X112-3N"
				(at 11.43 -98.73 0)
			)
			(property "Datasheet" ""
				(at 11.43 -198.73 0)
			)
			(property "Description" "INFINEON - IRLML2244TRPBF - P CHANNEL POWER MOSFET, HEXFET, -20V, -4.3A, SOT-23"
				(at 0 0 0)
			)
			(property "Height" "1.12"
				(at 11.43 -398.73 0)
			)
			(property "Mouser Part Number" "942-IRLML2244TRPBF"
				(at 11.43 -498.73 0)
			)
			(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Infineon-Technologies/IRLML2244TRPBF?qs=9%252BKlkBgLFf2tCL30qYbaQQ%3D%3D"
				(at 11.43 -598.73 0)
			)
			(property "Manufacturer_Name" "Infineon"
				(at 11.43 -698.73 0)
			)
			(property "Manufacturer_Part_Number" "IRLML2244TRPBF"
				(at 11.43 -798.73 0)
			)
			(symbol "IRLML2244TRPBF_1_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 5.08 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 5.08) (xy 5.08 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.842 -0.508) (xy 5.842 0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.842 0) (xy 7.62 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.842 2.032) (xy 5.842 3.048)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.842 5.588) (xy 5.842 4.572)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 7.62 2.54) (xy 5.842 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 7.62 2.54) (xy 7.62 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 7.62 5.08) (xy 5.842 5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 7.62 5.08) (xy 7.62 7.62)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 7.62 2.54) (xy 6.604 3.048) (xy 6.604 2.032) (xy 7.62 2.54)
					)
					(fill
						(type outline)
					)
				)
				(circle
					(center 6.35 2.54)
					(radius 3.81)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "G")
					(number "1")
				)
				(pin passive line
					(at 7.62 -5.08 90)
					(length 2.54)
					(name "S")
					(number "2")
				)
				(pin passive line
					(at 7.62 10.16 270)
					(length 2.54)
					(name "D")
					(number "3")
				)
			)
		)
		(symbol "power:+3.3V"
			(power)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -3.81 0)
			)
			(property "Value" "+3.3V"
				(at 0 3.556 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"+3.3V\""
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "+3.3V_0_1"
				(polyline
					(pts
						(xy -0.762 1.27) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 2.54) (xy 0.762 1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "+3.3V_1_1"
				(pin power_in line
					(at 0 0 90)
					(length 0) hide
					(name "+3.3V")
					(number "1")
				)
			)
		)
		(symbol "power:+3.3VP"
			(power)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 3.81 -1.27 0)
			)
			(property "Value" "+3.3VP"
				(at 0 2.54 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"+3.3VP\""
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "+3.3VP_0_0"
				(pin power_in line
					(at 0 0 90)
					(length 0) hide
					(name "+3.3VP")
					(number "1")
				)
			)
			(symbol "+3.3VP_0_1"
				(polyline
					(pts
						(xy -0.762 1.27) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 2.54) (xy 0.762 1.27)
					)
					(fill
						(type none)
					)
				)
			)
		)
		(symbol "power:+5P"
			(power)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -3.81 0)
			)
			(property "Value" "+5P"
				(at 0 3.556 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"+5P\""
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "+5P_0_1"
				(polyline
					(pts
						(xy -0.762 1.27) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 2.54) (xy 0.762 1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "+5P_1_1"
				(pin power_in line
					(at 0 0 90)
					(length 0) hide
					(name "+5P")
					(number "1")
				)
			)
		)
		(symbol "power:GNDD"
			(power)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "GNDD"
				(at 0 -3.175 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"GNDD\" , digital ground"
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "GNDD_0_1"
				(rectangle
					(start -1.27 -1.524)
					(end 1.27 -2.032)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.524)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GNDD_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0) hide
					(name "GNDD")
					(number "1")
				)
			)
		)
		(symbol "power:PWR_FLAG"
			(power)
			(pin_numbers hide)
			(pin_names
				(offset 0) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#FLG"
				(at 0 1.905 0)
			)
			(property "Value" "PWR_FLAG"
				(at 0 3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Special symbol for telling ERC where power comes from"
				(at 0 0 0)
			)
			(property "ki_keywords" "flag power"
				(at 0 0 0)
			)
			(symbol "PWR_FLAG_0_0"
				(pin power_out line
					(at 0 0 90)
					(length 0)
					(name "pwr")
					(number "1")
				)
			)
			(symbol "PWR_FLAG_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 1.27) (xy -1.016 1.905) (xy 0 2.54) (xy 1.016 1.905) (xy 0 1.27)
					)
					(fill
						(type none)
					)
				)
			)
		)
	)
	(junction
		(at 88.9 93.98)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 109.22 172.72)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 116.84 138.43)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 121.92 165.1)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 96.52 172.72)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 109.22 146.05)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 116.84 165.1)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 121.92 138.43)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 96.52 93.98)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 101.6 172.72)
		(diameter 0)
		(color 0 0 0 0)
	)
	(no_connect
		(at 85.09 80.01)
	)
	(no_connect
		(at 85.09 82.55)
	)
	(wire
		(pts
			(xy 115.57 83.82) (xy 115.57 74.93)
		)
	)
	(wire
		(pts
			(xy 96.52 85.09) (xy 96.52 93.98)
		)
	)
	(wire
		(pts
			(xy 96.52 48.26) (xy 96.52 59.69)
		)
	)
	(wire
		(pts
			(xy 95.25 44.45) (xy 95.25 57.15)
		)
	)
	(wire
		(pts
			(xy 162.56 77.47) (xy 177.8 77.47)
		)
	)
	(wire
		(pts
			(xy 171.45 57.15) (xy 177.8 57.15)
		)
	)
	(wire
		(pts
			(xy 171.45 41.91) (xy 177.8 41.91)
		)
	)
	(wire
		(pts
			(xy 109.22 153.67) (xy 109.22 146.05)
		)
	)
	(wire
		(pts
			(xy 171.45 62.23) (xy 177.8 62.23)
		)
	)
	(wire
		(pts
			(xy 116.84 180.34) (xy 109.22 180.34)
		)
	)
	(wire
		(pts
			(xy 88.9 93.98) (xy 88.9 99.06)
		)
	)
	(wire
		(pts
			(xy 96.52 172.72) (xy 101.6 172.72)
		)
	)
	(wire
		(pts
			(xy 162.56 82.55) (xy 177.8 82.55)
		)
	)
	(wire
		(pts
			(xy 116.84 138.43) (xy 121.92 138.43)
		)
	)
	(wire
		(pts
			(xy 162.56 80.01) (xy 177.8 80.01)
		)
	)
	(wire
		(pts
			(xy 171.45 53.34) (xy 177.8 53.34)
		)
	)
	(wire
		(pts
			(xy 128.27 53.34) (xy 99.06 53.34)
		)
	)
	(wire
		(pts
			(xy 100.33 67.31) (xy 85.09 67.31)
		)
	)
	(wire
		(pts
			(xy 121.92 165.1) (xy 127 165.1)
		)
	)
	(wire
		(pts
			(xy 85.09 138.43) (xy 99.06 138.43)
		)
	)
	(wire
		(pts
			(xy 171.45 58.42) (xy 177.8 58.42)
		)
	)
	(wire
		(pts
			(xy 137.16 78.74) (xy 118.11 78.74)
		)
	)
	(wire
		(pts
			(xy 88.9 158.75) (xy 69.85 158.75)
		)
	)
	(wire
		(pts
			(xy 96.52 93.98) (xy 96.52 99.06)
		)
	)
	(wire
		(pts
			(xy 93.98 54.61) (xy 85.09 54.61)
		)
	)
	(wire
		(pts
			(xy 91.44 167.64) (xy 91.44 172.72)
		)
	)
	(wire
		(pts
			(xy 85.09 85.09) (xy 96.52 85.09)
		)
	)
	(wire
		(pts
			(xy 109.22 180.34) (xy 109.22 172.72)
		)
	)
	(wire
		(pts
			(xy 99.06 64.77) (xy 85.09 64.77)
		)
	)
	(wire
		(pts
			(xy 171.45 38.1) (xy 177.8 38.1)
		)
	)
	(wire
		(pts
			(xy 100.33 55.88) (xy 100.33 67.31)
		)
	)
	(wire
		(pts
			(xy 171.45 45.72) (xy 177.8 45.72)
		)
	)
	(wire
		(pts
			(xy 171.45 46.99) (xy 177.8 46.99)
		)
	)
	(wire
		(pts
			(xy 118.11 78.74) (xy 118.11 69.85)
		)
	)
	(wire
		(pts
			(xy 128.27 55.88) (xy 100.33 55.88)
		)
	)
	(wire
		(pts
			(xy 114.3 77.47) (xy 114.3 87.63)
		)
	)
	(wire
		(pts
			(xy 128.27 48.26) (xy 96.52 48.26)
		)
	)
	(wire
		(pts
			(xy 162.56 74.93) (xy 177.8 74.93)
		)
	)
	(wire
		(pts
			(xy 85.09 77.47) (xy 114.3 77.47)
		)
	)
	(wire
		(pts
			(xy 97.79 50.8) (xy 97.79 62.23)
		)
	)
	(wire
		(pts
			(xy 85.09 153.67) (xy 85.09 138.43)
		)
	)
	(wire
		(pts
			(xy 171.45 34.29) (xy 177.8 34.29)
		)
	)
	(wire
		(pts
			(xy 101.6 172.72) (xy 109.22 172.72)
		)
	)
	(wire
		(pts
			(xy 88.9 167.64) (xy 91.44 167.64)
		)
	)
	(wire
		(pts
			(xy 69.85 153.67) (xy 85.09 153.67)
		)
	)
	(wire
		(pts
			(xy 162.56 76.2) (xy 177.8 76.2)
		)
	)
	(wire
		(pts
			(xy 162.56 73.66) (xy 177.8 73.66)
		)
	)
	(wire
		(pts
			(xy 95.25 165.1) (xy 99.06 165.1)
		)
	)
	(wire
		(pts
			(xy 115.57 74.93) (xy 85.09 74.93)
		)
	)
	(wire
		(pts
			(xy 118.11 69.85) (xy 85.09 69.85)
		)
	)
	(wire
		(pts
			(xy 121.92 138.43) (xy 127 138.43)
		)
	)
	(wire
		(pts
			(xy 171.45 60.96) (xy 177.8 60.96)
		)
	)
	(wire
		(pts
			(xy 162.56 78.74) (xy 177.8 78.74)
		)
	)
	(wire
		(pts
			(xy 99.06 53.34) (xy 99.06 64.77)
		)
	)
	(wire
		(pts
			(xy 96.52 59.69) (xy 85.09 59.69)
		)
	)
	(wire
		(pts
			(xy 171.45 35.56) (xy 177.8 35.56)
		)
	)
	(wire
		(pts
			(xy 95.25 165.1) (xy 95.25 156.21)
		)
	)
	(wire
		(pts
			(xy 85.09 87.63) (xy 88.9 87.63)
		)
	)
	(wire
		(pts
			(xy 116.84 165.1) (xy 121.92 165.1)
		)
	)
	(wire
		(pts
			(xy 93.98 41.91) (xy 93.98 54.61)
		)
	)
	(wire
		(pts
			(xy 116.84 153.67) (xy 109.22 153.67)
		)
	)
	(wire
		(pts
			(xy 95.25 156.21) (xy 69.85 156.21)
		)
	)
	(wire
		(pts
			(xy 171.45 54.61) (xy 177.8 54.61)
		)
	)
	(wire
		(pts
			(xy 114.3 87.63) (xy 137.16 87.63)
		)
	)
	(wire
		(pts
			(xy 88.9 87.63) (xy 88.9 93.98)
		)
	)
	(wire
		(pts
			(xy 171.45 43.18) (xy 177.8 43.18)
		)
	)
	(wire
		(pts
			(xy 85.09 72.39) (xy 116.84 72.39)
		)
	)
	(wire
		(pts
			(xy 171.45 50.8) (xy 177.8 50.8)
		)
	)
	(wire
		(pts
			(xy 114.3 138.43) (xy 116.84 138.43)
		)
	)
	(wire
		(pts
			(xy 88.9 167.64) (xy 88.9 158.75)
		)
	)
	(wire
		(pts
			(xy 171.45 39.37) (xy 177.8 39.37)
		)
	)
	(wire
		(pts
			(xy 171.45 49.53) (xy 177.8 49.53)
		)
	)
	(wire
		(pts
			(xy 116.84 72.39) (xy 116.84 81.28)
		)
	)
	(wire
		(pts
			(xy 162.56 81.28) (xy 177.8 81.28)
		)
	)
	(wire
		(pts
			(xy 95.25 57.15) (xy 85.09 57.15)
		)
	)
	(wire
		(pts
			(xy 116.84 81.28) (xy 137.16 81.28)
		)
	)
	(wire
		(pts
			(xy 114.3 165.1) (xy 116.84 165.1)
		)
	)
	(wire
		(pts
			(xy 137.16 83.82) (xy 115.57 83.82)
		)
	)
	(wire
		(pts
			(xy 128.27 50.8) (xy 97.79 50.8)
		)
	)
	(wire
		(pts
			(xy 101.6 146.05) (xy 109.22 146.05)
		)
	)
	(wire
		(pts
			(xy 128.27 44.45) (xy 95.25 44.45)
		)
	)
	(wire
		(pts
			(xy 128.27 41.91) (xy 93.98 41.91)
		)
	)
	(wire
		(pts
			(xy 91.44 172.72) (xy 96.52 172.72)
		)
	)
	(wire
		(pts
			(xy 97.79 62.23) (xy 85.09 62.23)
		)
	)
	(text "Control-Anbindung\n\n14  RS485-Rx\n13  RS485-Tx\n12  RS485-Dir\n11  RS485 Mux-0\n10  RS485 Mux-1\n 9  RS485 Mux-2\n 8  Sensoren Mux-0\n 7  Sensoren Mux-1\n 6  Sensoren Mux-2\n 5  Anforderung Data\n 4  nc  \n 3  nc\n 2  +3.3V\n 1  GND\n"
		(exclude_from_sim no)
		(at 52.07 88.9 0)
	)
	(text "Power\n\n3 +5V\n2 +3.3V\n1 GND"
		(exclude_from_sim no)
		(at 49.53 153.67 0)
	)
	(symbol
		(lib_id "Device:LED")
		(at 116.84 176.53 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D2"
			(at 120.65 176.8475 90)
		)
		(property "Value" "Power_{3.3V}"
			(at 120.65 179.3875 90)
		)
		(property "Footprint" "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
			(at 116.84 176.53 0)
		)
		(property "Datasheet" "~"
			(at 116.84 176.53 0)
		)
		(property "Description" ""
			(at 116.84 176.53 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "FBH_Verteiler_Thermostatanbindung"
				(path
					(reference "D2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 116.84 142.24 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R1"
			(at 119.38 140.97 0)
		)
		(property "Value" "2k1"
			(at 119.38 143.51 0)
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 115.062 142.24 90)
		)
		(property "Datasheet" "~"
			(at 116.84 142.24 0)
		)
		(property "Description" ""
			(at 116.84 142.24 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "FBH_Verteiler_Thermostatanbindung"
				(path
					(reference "R1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:PWR_FLAG")
		(at 96.52 172.72 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#FLG03"
			(at 96.52 170.815 0)
		)
		(property "Value" "PWR_FLAG"
			(at 96.52 167.64 0)
		)
		(property "Footprint" ""
			(at 96.52 172.72 0)
		)
		(property "Datasheet" "~"
			(at 96.52 172.72 0)
		)
		(property "Description" ""
			(at 96.52 172.72 0)
		)
		(pin "1")
		(instances
			(project "FBH_Verteiler_Thermostatanbindung"
				(path
					(reference "#FLG03")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "SamacSys_Parts:IRLML2244TRPBF")
		(at 109.22 172.72 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "Q2"
			(at 106.68 157.48 90)
		)
		(property "Value" "IRLML2244TRPBF"
			(at 106.68 160.02 90)
		)
		(property "Footprint" "SamacSys_Parts:SOT95P237X112-3N"
			(at 207.95 161.29 0)
		)
		(property "Datasheet" ""
			(at 307.95 161.29 0)
		)
		(property "Description" ""
			(at 109.22 172.72 0)
		)
		(property "Height" "1.12"
			(at 507.95 161.29 0)
		)
		(property "Mouser Part Number" "942-IRLML2244TRPBF"
			(at 607.95 161.29 0)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Infineon-Technologies/IRLML2244TRPBF?qs=9%252BKlkBgLFf2tCL30qYbaQQ%3D%3D"
			(at 707.95 161.29 0)
		)
		(property "Manufacturer_Name" "Infineon"
			(at 807.95 161.29 0)
		)
		(property "Manufacturer_Part_Number" "IRLML2244TRPBF"
			(at 907.95 161.29 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(instances
			(project "FBH_Verteiler_Thermostatanbindung"
				(path
					(reference "Q2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 116.84 168.91 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R2"
			(at 119.38 167.64 0)
		)
		(property "Value" "1k8"
			(at 119.38 170.18 0)
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 115.062 168.91 90)
		)
		(property "Datasheet" "~"
			(at 116.84 168.91 0)
		)
		(property "Description" ""
			(at 116.84 168.91 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "FBH_Verteiler_Thermostatanbindung"
				(path
					(reference "R2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector_Generic:Conn_01x03")
		(at 64.77 156.21 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "J1"
			(at 64.77 147.32 0)
		)
		(property "Value" "Power"
			(at 64.77 149.86 0)
		)
		(property "Footprint" "Connector_Phoenix_MC:PhoenixContact_MCV_1,5_3-G-3.81_1x03_P3.81mm_Vertical"
			(at 64.77 156.21 0)
		)
		(property "Datasheet" "~"
			(at 64.77 156.21 0)
		)
		(property "Description" ""
			(at 64.77 156.21 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(instances
			(project "FBH_Verteiler_Thermostatanbindung"
				(path
					(reference "J1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:+5P")
		(at 127 138.43 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR05"
			(at 123.19 138.43 0)
		)
		(property "Value" "+5P"
			(at 130.81 138.43 90)
		)
		(property "Footprint" ""
			(at 127 138.43 0)
		)
		(property "Datasheet" ""
			(at 127 138.43 0)
		)
		(property "Description" ""
			(at 127 138.43 0)
		)
		(pin "1")
		(instances
			(project "FBH_Verteiler_Thermostatanbindung"
				(path
					(reference "#PWR05")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "SamacSys_Parts:IRLML2244TRPBF")
		(at 109.22 146.05 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "Q1"
			(at 106.68 130.81 90)
		)
		(property "Value" "IRLML2244TRPBF"
			(at 106.68 133.35 90)
		)
		(property "Footprint" "SamacSys_Parts:SOT95P237X112-3N"
			(at 207.95 134.62 0)
		)
		(property "Datasheet" ""
			(at 307.95 134.62 0)
		)
		(property "Description" ""
			(at 109.22 146.05 0)
		)
		(property "Height" "1.12"
			(at 507.95 134.62 0)
		)
		(property "Mouser Part Number" "942-IRLML2244TRPBF"
			(at 607.95 134.62 0)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Infineon-Technologies/IRLML2244TRPBF?qs=9%252BKlkBgLFf2tCL30qYbaQQ%3D%3D"
			(at 707.95 134.62 0)
		)
		(property "Manufacturer_Name" "Infineon"
			(at 807.95 134.62 0)
		)
		(property "Manufacturer_Part_Number" "IRLML2244TRPBF"
			(at 907.95 134.62 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(instances
			(project "FBH_Verteiler_Thermostatanbindung"
				(path
					(reference "Q1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:PWR_FLAG")
		(at 121.92 165.1 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#FLG05"
			(at 121.92 163.195 0)
		)
		(property "Value" "PWR_FLAG"
			(at 121.92 160.02 0)
		)
		(property "Footprint" ""
			(at 121.92 165.1 0)
		)
		(property "Datasheet" "~"
			(at 121.92 165.1 0)
		)
		(property "Description" ""
			(at 121.92 165.1 0)
		)
		(pin "1")
		(instances
			(project "FBH_Verteiler_Thermostatanbindung"
				(path
					(reference "#FLG05")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GNDD")
		(at 101.6 172.72 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR04"
			(at 101.6 179.07 0)
		)
		(property "Value" "GNDD"
			(at 101.6 176.53 0)
		)
		(property "Footprint" ""
			(at 101.6 172.72 0)
		)
		(property "Datasheet" ""
			(at 101.6 172.72 0)
		)
		(property "Description" ""
			(at 101.6 172.72 0)
		)
		(pin "1")
		(instances
			(project "FBH_Verteiler_Thermostatanbindung"
				(path
					(reference "#PWR04")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:LED")
		(at 116.84 149.86 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D1"
			(at 120.65 150.1775 90)
		)
		(property "Value" "Power_{5V}"
			(at 120.65 152.7175 90)
		)
		(property "Footprint" "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
			(at 116.84 149.86 0)
		)
		(property "Datasheet" "~"
			(at 116.84 149.86 0)
		)
		(property "Description" ""
			(at 116.84 149.86 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "FBH_Verteiler_Thermostatanbindung"
				(path
					(reference "D1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:+3.3VP")
		(at 127 165.1 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR06"
			(at 125.73 168.91 0)
		)
		(property "Value" "+3.3VP"
			(at 130.81 165.1 90)
		)
		(property "Footprint" ""
			(at 127 165.1 0)
		)
		(property "Datasheet" ""
			(at 127 165.1 0)
		)
		(property "Description" ""
			(at 127 165.1 0)
		)
		(pin "1")
		(instances
			(project "FBH_Verteiler_Thermostatanbindung"
				(path
					(reference "#PWR06")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GNDD")
		(at 88.9 99.06 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01"
			(at 88.9 105.41 0)
		)
		(property "Value" "GNDD"
			(at 88.9 102.87 0)
		)
		(property "Footprint" ""
			(at 88.9 99.06 0)
		)
		(property "Datasheet" ""
			(at 88.9 99.06 0)
		)
		(property "Description" ""
			(at 88.9 99.06 0)
		)
		(pin "1")
		(instances
			(project "FBH_Verteiler_Thermostatanbindung"
				(path
					(reference "#PWR01")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:PWR_FLAG")
		(at 121.92 138.43 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#FLG04"
			(at 121.92 136.525 0)
		)
		(property "Value" "PWR_FLAG"
			(at 121.92 133.35 0)
		)
		(property "Footprint" ""
			(at 121.92 138.43 0)
		)
		(property "Datasheet" "~"
			(at 121.92 138.43 0)
		)
		(property "Description" ""
			(at 121.92 138.43 0)
		)
		(pin "1")
		(instances
			(project "FBH_Verteiler_Thermostatanbindung"
				(path
					(reference "#FLG04")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:PWR_FLAG")
		(at 96.52 93.98 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#FLG02"
			(at 98.425 93.98 0)
		)
		(property "Value" "PWR_FLAG"
			(at 100.33 93.98 90)
		)
		(property "Footprint" ""
			(at 96.52 93.98 0)
		)
		(property "Datasheet" "~"
			(at 96.52 93.98 0)
		)
		(property "Description" ""
			(at 96.52 93.98 0)
		)
		(pin "1")
		(instances
			(project "FBH_Verteiler_Thermostatanbindung"
				(path
					(reference "#FLG02")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:+3.3V")
		(at 96.52 99.06 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR02"
			(at 96.52 95.25 0)
		)
		(property "Value" "+3.3V"
			(at 96.52 104.14 0)
		)
		(property "Footprint" ""
			(at 96.52 99.06 0)
		)
		(property "Datasheet" ""
			(at 96.52 99.06 0)
		)
		(property "Description" ""
			(at 96.52 99.06 0)
		)
		(pin "1")
		(instances
			(project "FBH_Verteiler_Thermostatanbindung"
				(path
					(reference "#PWR02")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector_Generic:Conn_01x14")
		(at 80.01 72.39 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "J2"
			(at 80.01 48.26 0)
		)
		(property "Value" "Conn_01x14"
			(at 80.01 50.8 0)
		)
		(property "Footprint" "Connector_IDC:IDC-Header_2x07_P2.54mm_Vertical"
			(at 80.01 72.39 0)
		)
		(property "Datasheet" "~"
			(at 80.01 72.39 0)
		)
		(property "Description" ""
			(at 80.01 72.39 0)
		)
		(pin "1")
		(pin "10")
		(pin "11")
		(pin "12")
		(pin "13")
		(pin "14")
		(pin "2")
		(pin "3")
		(pin "4")
		(pin "5")
		(pin "6")
		(pin "7")
		(pin "8")
		(pin "9")
		(instances
			(project "FBH_Verteiler_Thermostatanbindung"
				(path
					(reference "J2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GNDD")
		(at 101.6 146.05 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR03"
			(at 101.6 152.4 0)
		)
		(property "Value" "GNDD"
			(at 101.6 149.86 0)
		)
		(property "Footprint" ""
			(at 101.6 146.05 0)
		)
		(property "Datasheet" ""
			(at 101.6 146.05 0)
		)
		(property "Description" ""
			(at 101.6 146.05 0)
		)
		(pin "1")
		(instances
			(project "FBH_Verteiler_Thermostatanbindung"
				(path
					(reference "#PWR03")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:PWR_FLAG")
		(at 88.9 93.98 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#FLG01"
			(at 86.995 93.98 0)
		)
		(property "Value" "PWR_FLAG"
			(at 85.09 93.98 90)
		)
		(property "Footprint" ""
			(at 88.9 93.98 0)
		)
		(property "Datasheet" "~"
			(at 88.9 93.98 0)
		)
		(property "Description" ""
			(at 88.9 93.98 0)
		)
		(pin "1")
		(instances
			(project "FBH_Verteiler_Thermostatanbindung"
				(path
					(reference "#FLG01")
					(unit 1)
				)
			)
		)
	)
	(sheet
		(at 177.8 30.48)
		(size 36.83 54.61)
		(fields_autoplaced yes)
		(fill
			(color 0 0 0 0.0000)
		)
		(property "Sheetname" "Themostat_Anschluss"
			(at 177.8 29.7684 0)
		)
		(property "Sheetfile" "Themostat_Anschluss.kicad_sch"
			(at 177.8 85.6746 0)
		)
		(pin "Anf_{0}" output
			(at 177.8 73.66 180)
		)
		(pin "RS485-A_{1}" bidirectional
			(at 177.8 38.1 180)
		)
		(pin "RS485-A_{0}" bidirectional
			(at 177.8 34.29 180)
		)
		(pin "Anf_{1}" output
			(at 177.8 74.93 180)
		)
		(pin "RS485-B_{1}" bidirectional
			(at 177.8 39.37 180)
		)
		(pin "RS485-B_{0}" bidirectional
			(at 177.8 35.56 180)
		)
		(pin "RS485-B_{4}" bidirectional
			(at 177.8 50.8 180)
		)
		(pin "Anf_{4}" output
			(at 177.8 78.74 180)
		)
		(pin "RS485-A_{4}" bidirectional
			(at 177.8 49.53 180)
		)
		(pin "RS485-B_{7}" bidirectional
			(at 177.8 62.23 180)
		)
		(pin "RS485-A_{7}" bidirectional
			(at 177.8 60.96 180)
		)
		(pin "Anf_{7}" output
			(at 177.8 82.55 180)
		)
		(pin "Anf_{5}" output
			(at 177.8 80.01 180)
		)
		(pin "RS485-A_{6}" bidirectional
			(at 177.8 57.15 180)
		)
		(pin "RS485-B_{6}" bidirectional
			(at 177.8 58.42 180)
		)
		(pin "RS485-A_{5}" bidirectional
			(at 177.8 53.34 180)
		)
		(pin "Anf_{6}" output
			(at 177.8 81.28 180)
		)
		(pin "RS485-B_{5}" bidirectional
			(at 177.8 54.61 180)
		)
		(pin "RS485-B_{3}" bidirectional
			(at 177.8 46.99 180)
		)
		(pin "Anf_{3}" output
			(at 177.8 77.47 180)
		)
		(pin "RS485-A_{3}" bidirectional
			(at 177.8 45.72 180)
		)
		(pin "Anf_{2}" output
			(at 177.8 76.2 180)
		)
		(pin "RS485-B_{2}" bidirectional
			(at 177.8 43.18 180)
		)
		(pin "RS485-A_{2}" bidirectional
			(at 177.8 41.91 180)
		)
		(instances
			(project "FBH_Verteiler_Thermostatanbindung"
				(path
					(page "4")
				)
			)
		)
	)
	(sheet
		(at 137.16 71.12)
		(size 25.4 20.32)
		(fields_autoplaced yes)
		(fill
			(color 0 0 0 0.0000)
		)
		(property "Sheetname" "Anforderungen"
			(at 137.16 70.4084 0)
		)
		(property "Sheetfile" "anforderungen.kicad_sch"
			(at 137.16 92.0246 0)
		)
		(pin "Anf_T_{3}" input
			(at 162.56 77.47 0)
		)
		(pin "Anf_T_{0}" input
			(at 162.56 73.66 0)
		)
		(pin "Anf_T_{1}" input
			(at 162.56 74.93 0)
		)
		(pin "Anf_T_{7}" input
			(at 162.56 82.55 0)
		)
		(pin "Anf_T_{6}" input
			(at 162.56 81.28 0)
		)
		(pin "Anf_T_{2}" input
			(at 162.56 76.2 0)
		)
		(pin "Anf_T_{5}" input
			(at 162.56 80.01 0)
		)
		(pin "Anf_T_{4}" input
			(at 162.56 78.74 0)
		)
		(pin "Sens_MX_{1}" input
			(at 137.16 81.28 180)
		)
		(pin "Sens_Mx_{0}" input
			(at 137.16 78.74 180)
		)
		(pin "Sens_Mx_{2}" input
			(at 137.16 83.82 180)
		)
		(pin "Anf_Mxed" output
			(at 137.16 87.63 180)
		)
		(instances
			(project "FBH_Verteiler_Thermostatanbindung"
				(path
					(page "3")
				)
			)
		)
	)
	(sheet
		(at 128.27 30.48)
		(size 43.18 34.29)
		(fields_autoplaced yes)
		(fill
			(color 0 0 0 0.0000)
		)
		(property "Sheetname" "RS485_T"
			(at 128.27 29.7684 0)
		)
		(property "Sheetfile" "rs485_t.kicad_sch"
			(at 128.27 65.3546 0)
		)
		(pin "T_{0}_RS485_A" bidirectional
			(at 171.45 34.29 0)
		)
		(pin "T_{0}_RS485_B" bidirectional
			(at 171.45 35.56 0)
		)
		(pin "T_{1}_RS485_B" bidirectional
			(at 171.45 39.37 0)
		)
		(pin "T_RS485_MX_{2}" input
			(at 128.27 55.88 180)
		)
		(pin "T_RS485_MX_{0}" input
			(at 128.27 50.8 180)
		)
		(pin "T_RS485_MX_{1}" input
			(at 128.27 53.34 180)
		)
		(pin "T_RS485_Dir" input
			(at 128.27 48.26 180)
		)
		(pin "T_{1}_RS485_A" bidirectional
			(at 171.45 38.1 0)
		)
		(pin "T_{3}_RS485_B" bidirectional
			(at 171.45 46.99 0)
		)
		(pin "T_{2}_RS485_A" bidirectional
			(at 171.45 41.91 0)
		)
		(pin "T_{2}_RS485_B" bidirectional
			(at 171.45 43.18 0)
		)
		(pin "T_{6}_RS485_A" bidirectional
			(at 171.45 57.15 0)
		)
		(pin "T_{7}_RS485_B" bidirectional
			(at 171.45 62.23 0)
		)
		(pin "T_{7}_RS485_A" bidirectional
			(at 171.45 60.96 0)
		)
		(pin "T_{4}_RS485_A" bidirectional
			(at 171.45 49.53 0)
		)
		(pin "T_{4}_RS485_B" bidirectional
			(at 171.45 50.8 0)
		)
		(pin "T_{3}_RS485_A" bidirectional
			(at 171.45 45.72 0)
		)
		(pin "T_{6}_RS485_B" bidirectional
			(at 171.45 58.42 0)
		)
		(pin "T_{5}_RS485_A" bidirectional
			(at 171.45 53.34 0)
		)
		(pin "T_{5}_RS485_B" bidirectional
			(at 171.45 54.61 0)
		)
		(pin "T_RS485_Tx" input
			(at 128.27 44.45 180)
		)
		(pin "T_RS485_Rx" output
			(at 128.27 41.91 180)
		)
		(instances
			(project "FBH_Verteiler_Thermostatanbindung"
				(path
					(page "2")
				)
			)
		)
	)
	(sheet_instances
		(path
			(page "1")
		)
	)
)
