(footprint "CLIFF_FCR681465P"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "DC Power Socket, Barrel Jack")
	(property "Reference" "REF**"
		(at 7.9 -5.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "CLIFF_FCR681465P"
		(at 6.4 3 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Footprint" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 5.8 -2.5 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 4 4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 6.2 0)
		(size 4 4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 3.1 -5)
		(size 4 4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
)
