(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(title_block
		(title "Adapter_CANBridge")
		(date "2025-01-13")
		(rev "1.0")
	)
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "+3.3V")
	(net 2 "GND")
	(net 3 "Net-(JP4-A)")
	(net 4 "Net-(JP6-A)")
	(net 5 "Net-(JP1-B)")
	(net 6 "Net-(U1-RF_IN)")
	(net 7 "Net-(JP5-A)")
	(net 8 "RNBD_VDD_3V3")
	(net 9 "PIN_PA18_U3")
	(net 10 "PIN_PA15_U1")
	(net 11 "PIN_PA16_U2")
	(net 12 "PIN_PA17_V3")
	(net 13 "Net-(CONN_CAN0-Pin_1)")
	(net 14 "Net-(CONN_CAN0-Pin_3)")
	(net 15 "Net-(CONN_CAN1-Pin_3)")
	(net 16 "Net-(CONN_CAN1-Pin_1)")
	(net 17 "Net-(CONN_CAN2-Pin_3)")
	(net 18 "Net-(CONN_CAN2-Pin_1)")
	(net 19 "+5V")
	(net 20 "PIN_PC22_P18")
	(net 21 "PIN_PC25_K17")
	(net 22 "PIN_PA22_G4")
	(net 23 "PIN_PC21_P17")
	(net 24 "PIN_PC26_K18")
	(net 25 "PIN_PC8_M13")
	(net 26 "PIN_PC1_T17")
	(net 27 "PIN_PC9_M18")
	(net 28 "PIN_PC10_H17")
	(net 29 "unconnected-(CONN_X32_links1-Pin_17-Pad17)")
	(net 30 "PIN_PC2_T18_res")
	(net 31 "PIN_PC4_R18")
	(net 32 "PIN_PC13_F17_res")
	(net 33 "PIN_PE11_M6_res")
	(net 34 "PIN_PC11_H15")
	(net 35 "unconnected-(CONN_X32_links1-Pin_10-Pad10)")
	(net 36 "unconnected-(CONN_X32_links1-Pin_19-Pad19)")
	(net 37 "unconnected-(CONN_X32_rechts1-Pin_2-Pad2)")
	(net 38 "unconnected-(CONN_X32_rechts1-Pin_10-Pad10)")
	(net 39 "unconnected-(CONN_X32_rechts1-Pin_1-Pad1)")
	(net 40 "unconnected-(CONN_X32_rechts1-Pin_6-Pad6)")
	(net 41 "unconnected-(CONN_X32_rechts1-Pin_8-Pad8)")
	(net 42 "uBlox_UART_RX")
	(net 43 "uBlox_UART_TX")
	(net 44 "RNBD_UART-CTS")
	(net 45 "RNBD_UART-RTS")
	(net 46 "RNBD_UART-RX")
	(net 47 "RNBD_UART-TX")
	(net 48 "PIN_PC0_P15")
	(net 49 "uBlox_RST")
	(net 50 "PIN_PG9_K12")
	(net 51 "PIN_PG6_L15")
	(net 52 "PIN_PA23_G1")
	(net 53 "PIN_PG5_J17")
	(net 54 "PIN_PG7_L12")
	(net 55 "PIN_PD27_A8")
	(net 56 "PIN_PG10_G13")
	(net 57 "PIN_PD24_D11")
	(net 58 "PIN_PD25_D5")
	(net 59 "PIN_PD26_B9")
	(net 60 "PIN_PB11_14")
	(net 61 "PIN_AVDD")
	(net 62 "PIN_PC5_N15")
	(net 63 "PIN_PC6_N17")
	(net 64 "PIN_PC7_N18")
	(net 65 "Net-(JP1-A)")
	(net 66 "Net-(JP2-B)")
	(net 67 "Net-(JP3-A)")
	(net 68 "uBlox_USB-DM")
	(net 69 "Net-(U1-USB_DM)")
	(net 70 "uBlox_USB-DP")
	(net 71 "Net-(U1-USB_DP)")
	(net 72 "Net-(U1-EXTINT1)")
	(net 73 "Net-(U1-EXTINT0)")
	(net 74 "RNBD_NMCLR")
	(net 75 "RNBD_PB0")
	(net 76 "RNBD_PB3")
	(net 77 "RNBD_PB5")
	(net 78 "RNBD_PB7")
	(net 79 "RNBD_PB8")
	(net 80 "RNBD_PB10")
	(net 81 "RNBD_PB11")
	(net 82 "RNBD_PA0")
	(net 83 "RNBD_PA1")
	(net 84 "RNBD_PB12")
	(net 85 "RNBD_PB13")
	(net 86 "RNBD_PA8")
	(net 87 "RNBD_PA7")
	(net 88 "RNBD_PA10")
	(net 89 "RNBD_PA13")
	(net 90 "RNBD_PA14")
	(net 91 "RNBD_PA2")
	(net 92 "RNBD_PA3")
	(net 93 "RNBD_PB2")
	(net 94 "RNBD_PB1")
	(net 95 "RNBD_PB4")
	(net 96 "Net-(U1-VCC_RF)")
	(net 97 "Net-(U1-LNA_EN)")
	(net 98 "uBlox_SDA")
	(net 99 "unconnected-(U1-RESERVED-Pad17)")
	(net 100 "unconnected-(U1-RESERVED-Pad16)")
	(net 101 "uBlox_SCL")
	(net 102 "Net-(L1-1)")
	(net 103 "Net-(L1-4)")
	(net 104 "Net-(L3-1)")
	(net 105 "Net-(L3-4)")
	(net 106 "Net-(L2-4)")
	(net 107 "Net-(L2-1)")
	(net 108 "unconnected-(U2-PA9-Pad30)")
	(net 109 "unconnected-(U2-PA11-Pad9)")
	(net 110 "unconnected-(U2-PA12-Pad10)")
	(net 111 "unconnected-(U2-PB9-Pad15)")
	(net 112 "unconnected-(CONN_Arduino_Shield_links_oben1-Pin_1-Pad1)")
	(net 113 "unconnected-(CONN_Arduino_Shield_links_oben1-Pin_3-Pad3)")
	(net 114 "unconnected-(CONN_Arduino_Shield_links_oben1-Pin_8-Pad8)")
	(net 115 "PIN_PA28_T1")
	(net 116 "PIN_PA29_T2")
	(net 117 "PIN_PC3_R17_res")
	(net 118 "+5V_res")
	(net 119 "PIN_PC12_F18_res")
	(net 120 "PIN_PE1_H2_res")
	(net 121 "PIN_PE0_H1_res")
	(net 122 "PIN_PA18_U3_res")
	(net 123 "PIN_PE2_J1_res")
	(net 124 "PIN_PA31_G2_res")
	(net 125 "PIN_PA22_G4_res")
	(net 126 "PIN_PA8_K2_res")
	(net 127 "PIN_PC25_K17_res")
	(net 128 "PIN_PC21_P17_res")
	(net 129 "PIN_PC22_P18_res")
	(net 130 "PIN_PC26_K18_res")
	(net 131 "PIN_PA14_R2_res")
	(net 132 "+3.3V_res")
	(net 133 "PIN_PB27_V10_res")
	(net 134 "PIN_PC14_E17_res")
	(net 135 "PIN_PC15_G12_res")
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 126.25 65.25)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP7"
			(at -2.75 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "RNBD451_BLE")
		(sheetfile "RNBD451_BLE.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 78 "RNBD_PB7")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Würth_WE-CNSW:WE-CNSW_1812_744235510"
		(layer "F.Cu")
		(at 121 106.75 180)
		(descr "WE-CNSW SMT Common Mode Line Filter  Size: 1812")
		(property "Reference" "L2"
			(at 0.06 -2.65 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "744235510"
			(at -2.14 3.41 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Würth_WE-CNSW:WE-CNSW_1812_744235510"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "WE-CNSW SMD Common Mode Line Filter\n\nCharacteristics\n\nCurrent compensated data line filter\nHigh common mode noise suppression at high frequencies\nSmall influence on high speed signals through winding symmetry\nClimatic category 40/105/21 (Size 0603)\nClimatic category 40/125/21 (Size 0805/1206/1812)\nFlammability corresponding to UL 94 V-0\n\nApplications\n\nUSB 2.0\nIEEE 1394 (Firewire)\nLVDS\nHigh Speed Data Lines\nLAN\n\nhttps://katalog.we-online.com/media/images/v2/o14771v209%20we-cnsw_stroko_smd_gruppe.jpg\n\nDetails see: http://katalog.we-online.de/en/pbs/WE-CNSW http://katalog.we-online.de/en/pbs/WE-CNSW\n\nUpdated by  Ella Wu 2019-01-09\n2019 (C) Wurth Elektronik"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Stammblatt")
		(sheetfile "Adapter_CANBridge.kicad_sch")
		(pad "1" smd rect
			(at -1.825 1.125)
			(size 1.15 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 106 "Net-(L2-4)")
			(pinfunction "4")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 1.825 1.125)
			(size 1.15 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "Net-(CONN_CAN2-Pin_3)")
			(pinfunction "3")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "3" smd rect
			(at 1.825 -1.125)
			(size 1.15 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "Net-(CONN_CAN2-Pin_1)")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "4" smd rect
			(at -1.825 -1.125)
			(size 1.15 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 107 "Net-(L2-1)")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 150 67)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP16"
			(at 0 -1.448 0)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "RNBD451_BLE")
		(sheetfile "RNBD451_BLE.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 87 "RNBD_PA7")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
		(layer "F.Cu")
		(at 129 128 180)
		(descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U1_CAN0"
			(at -0.1 -4.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "MCP2562-H-SN"
			(at 0 3.4 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/25167A.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "High-Speed CAN Transceiver, 1Mbps, 5V supply, Vio pin, -40C to +150C, SOIC-8"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOIC*3.9x4.9mm*P1.27mm*")
		(sheetname "Stammblatt")
		(sheetfile "Adapter_CANBridge.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.475 -1.905 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 62 "PIN_PC5_N15")
			(pinfunction "TXD")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2.475 -0.635 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -2.475 0.635 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "Net-(JP4-A)")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at -2.475 1.905 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 31 "PIN_PC4_R18")
			(pinfunction "RXD")
			(pintype "output")
		)
		(pad "5" smd roundrect
			(at 2.475 1.905 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "+3.3V")
			(pinfunction "Vio")
			(pintype "power_in")
		)
		(pad "6" smd roundrect
			(at 2.475 0.635 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 103 "Net-(L1-4)")
			(pinfunction "CANL")
			(pintype "bidirectional")
		)
		(pad "7" smd roundrect
			(at 2.475 -0.635 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 102 "Net-(L1-1)")
			(pinfunction "CANH")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at 2.475 -1.905 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "STBY")
			(pintype "input")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 116 128 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R1"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "120R"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Stammblatt")
		(sheetfile "Adapter_CANBridge.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "Net-(CONN_CAN0-Pin_1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 14 "Net-(CONN_CAN0-Pin_3)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder"
		(layer "F.Cu")
		(at 156 107.6 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C5"
			(at -2.1 -0.1 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n_25V_X7R"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "uBlox_Neo-M9N")
		(sheetfile "untitled.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.5675 0 180)
			(size 0.735 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "Net-(JP1-B)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.5675 0 180)
			(size 0.735 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder"
		(layer "F.Cu")
		(at 126 102.75 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C3"
			(at 0 -1.16 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n_25V_X7R"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Stammblatt")
		(sheetfile "Adapter_CANBridge.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.5675 0 180)
			(size 0.735 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.5675 0 180)
			(size 0.735 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "RF_GPS:ublox_NEO"
		(layer "F.Cu")
		(at 162.5 115.5 90)
		(descr "ublox NEO 6/7/8, (https://www.u-blox.com/sites/default/files/NEO-8Q-NEO-M8-FW3_HardwareIntegrationManual_%28UBX-15029985%29_0.pdf)")
		(tags "GPS ublox NEO 6/7/8")
		(property "Reference" "U1"
			(at 0 -9 90)
			(layer "F.SilkS")
		)
		(property "Value" "NEO-M8T"
			(at 0 9.25 90)
			(layer "F.Fab")
		)
		(property "Footprint" "RF_GPS:ublox_NEO"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://content.u-blox.com/sites/default/files/documents/NEO-LEA-M8T-FW3_DataSheet_UBX-15025193.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "GNSS Module NEO M8, VCC 2.7V to 3.6V"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "ublox*NEO*")
		(sheetname "uBlox_Neo-M9N")
		(sheetfile "untitled.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -6 -7 90)
			(size 1.8 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 26 "PIN_PC1_T17")
			(pinfunction "TP2/~{SAFEBOOT}")
			(pintype "bidirectional")
		)
		(pad "2" smd roundrect
			(at -6 -5.9 90)
			(size 1.8 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 66 "Net-(JP2-B)")
			(pinfunction "D_SEL")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -6 -4.8 90)
			(size 1.8 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 48 "PIN_PC0_P15")
			(pinfunction "TIMEPULSE")
			(pintype "output")
		)
		(pad "4" smd roundrect
			(at -6 -3.7 90)
			(size 1.8 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 73 "Net-(U1-EXTINT0)")
			(pinfunction "EXTINT0")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -6 -2.6 90)
			(size 1.8 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 69 "Net-(U1-USB_DM)")
			(pinfunction "USB_DM")
			(pintype "bidirectional")
		)
		(pad "6" smd roundrect
			(at -6 -1.5 90)
			(size 1.8 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 71 "Net-(U1-USB_DP)")
			(pinfunction "USB_DP")
			(pintype "bidirectional")
		)
		(pad "7" smd roundrect
			(at -6 -0.4 90)
			(size 1.8 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 67 "Net-(JP3-A)")
			(pinfunction "VDD_USB")
			(pintype "power_in")
		)
		(pad "8" smd roundrect
			(at -6 2.6 90)
			(size 1.8 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 49 "uBlox_RST")
			(pinfunction "~{RESET}")
			(pintype "input")
		)
		(pad "9" smd roundrect
			(at -6 3.7 90)
			(size 1.8 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 96 "Net-(U1-VCC_RF)")
			(pinfunction "VCC_RF")
			(pintype "power_out")
		)
		(pad "10" smd roundrect
			(at -6 4.8 90)
			(size 1.8 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "11" smd roundrect
			(at -6 5.9 90)
			(size 1.8 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "Net-(U1-RF_IN)")
			(pinfunction "RF_IN")
			(pintype "input")
		)
		(pad "12" smd roundrect
			(at -6 7 90)
			(size 1.8 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "13" smd roundrect
			(at 6 7 90)
			(size 1.8 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "14" smd roundrect
			(at 6 5.9 90)
			(size 1.8 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 97 "Net-(U1-LNA_EN)")
			(pinfunction "LNA_EN")
			(pintype "output")
		)
		(pad "15" smd roundrect
			(at 6 4.8 90)
			(size 1.8 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 72 "Net-(U1-EXTINT1)")
			(pinfunction "EXTINT1")
			(pintype "input")
		)
		(pad "16" smd roundrect
			(at 6 3.7 90)
			(size 1.8 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 100 "unconnected-(U1-RESERVED-Pad16)")
			(pinfunction "RESERVED")
			(pintype "no_connect")
		)
		(pad "17" smd roundrect
			(at 6 2.6 90)
			(size 1.8 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 99 "unconnected-(U1-RESERVED-Pad17)")
			(pinfunction "RESERVED")
			(pintype "no_connect")
		)
		(pad "18" smd roundrect
			(at 6 -0.4 90)
			(size 1.8 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 98 "uBlox_SDA")
			(pinfunction "SDA/~{SPI_CS}")
			(pintype "bidirectional")
		)
		(pad "19" smd roundrect
			(at 6 -1.5 90)
			(size 1.8 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 101 "uBlox_SCL")
			(pinfunction "SCL/SPI_CLK")
			(pintype "input")
		)
		(pad "20" smd roundrect
			(at 6 -2.6 90)
			(size 1.8 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 43 "uBlox_UART_TX")
			(pinfunction "TXD/SPI_MISO")
			(pintype "output")
		)
		(pad "21" smd roundrect
			(at 6 -3.7 90)
			(size 1.8 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 42 "uBlox_UART_RX")
			(pinfunction "RXD/SPI_MOSI")
			(pintype "input")
		)
		(pad "22" smd roundrect
			(at 6 -4.8 90)
			(size 1.8 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 65 "Net-(JP1-A)")
			(pinfunction "V_BCKP")
			(pintype "power_in")
		)
		(pad "23" smd roundrect
			(at 6 -5.9 90)
			(size 1.8 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "Net-(JP1-B)")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "24" smd roundrect
			(at 6 -7 90)
			(size 1.8 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/RF_GPS.3dshapes/ublox_NEO.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder"
		(layer "F.Cu")
		(at 167.19 124.25 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C6_Shunt1"
			(at -5.1675 0.01 0)
			(layer "F.SilkS")
		)
		(property "Value" "adj"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "uBlox_Neo-M9N")
		(sheetfile "untitled.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.5675 0 180)
			(size 0.735 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "Net-(U1-RF_IN)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.5675 0 180)
			(size 0.735 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 130.5 70.5)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP9"
			(at 0.5 2 180)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "RNBD451_BLE")
		(sheetfile "RNBD451_BLE.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 80 "RNBD_PB10")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 120 60.5)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "JP8"
			(at 0 -1.8 0)
			(layer "F.SilkS")
		)
		(property "Value" "SolderJumper_2_Open"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "RNBD451_BLE")
		(sheetfile "RNBD451_BLE.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" smd custom
			(at -0.65 0)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 1 "+3.3V")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 8 "RNBD_VDD_3V3")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 131.65 124)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "JP4"
			(at 0 -1.8 0)
			(layer "F.SilkS")
		)
		(property "Value" "SolderJumper_2_Open"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "Stammblatt")
		(sheetfile "Adapter_CANBridge.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" smd custom
			(at -0.65 0)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 3 "Net-(JP4-A)")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 19 "+5V")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 116 106.75 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R2"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "120R"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Stammblatt")
		(sheetfile "Adapter_CANBridge.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 18 "Net-(CONN_CAN2-Pin_1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 17 "Net-(CONN_CAN2-Pin_3)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder"
		(layer "F.Cu")
		(at 126 124 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C1"
			(at 0 -1.16 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n_25V_X7R"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Stammblatt")
		(sheetfile "Adapter_CANBridge.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.5675 0 180)
			(size 0.735 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.5675 0 180)
			(size 0.735 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 133.5 70.5)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP11"
			(at 0.75 2.5 90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "RNBD451_BLE")
		(sheetfile "RNBD451_BLE.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 82 "RNBD_PA0")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 127.6 68.1)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP8"
			(at -1.25 1.75 0)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "RNBD451_BLE")
		(sheetfile "RNBD451_BLE.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 79 "RNBD_PB8")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Antennen:XDCR_W3011"
		(layer "F.Cu")
		(at 170.7 131)
		(property "Reference" "AE2"
			(at -1.5 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "W3011"
			(at 1.548 2.7452 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Antennen:XDCR_W3011"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "N/A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer recommendations"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "1.3 mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "PulseLarsen"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "uBlox_Neo-M9N")
		(sheetfile "untitled.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.475 -1.6)
			(size 0.65 0.8)
			(layers "F.Cu")
			(net 6 "Net-(U1-RF_IN)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.475 -1.6)
			(size 0.65 0.8)
			(layers "F.Cu")
			(net 2 "GND")
			(pintype "power_in")
		)
		(pad "3" smd rect
			(at 0 1.6)
			(size 1.6 0.8)
			(layers "F.Cu")
			(net 2 "GND")
			(pintype "power_in")
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder"
		(layer "F.Cu")
		(at 134.25 128 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C2"
			(at 0 -1.16 90)
			(layer "F.SilkS")
		)
		(property "Value" "100n_25V_X7R"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Stammblatt")
		(sheetfile "Adapter_CANBridge.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.5675 0 270)
			(size 0.735 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "Net-(JP4-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.5675 0 270)
			(size 0.735 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 146 51)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP24"
			(at 2.4 -0.7 0)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "RNBD451_BLE")
		(sheetfile "RNBD451_BLE.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 95 "RNBD_PB4")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Horizontal"
		(layer "F.Cu")
		(at 112.375 109.275 180)
		(descr "Through hole angled pin header, 1x03, 2.54mm pitch, 6mm pin length, single row")
		(tags "Through hole angled pin header THT 1x03 2.54mm single row")
		(property "Reference" "CONN_CAN2"
			(at 4.375 7.525 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x03"
			(at 4.385 7.35 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Horizontal"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Stammblatt")
		(sheetfile "Adapter_CANBridge.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.77 2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "Net-(CONN_CAN2-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "Net-(CONN_CAN2-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 146 65)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP15"
			(at 0 -1.448 0)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "RNBD451_BLE")
		(sheetfile "RNBD451_BLE.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 86 "RNBD_PA8")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 146 54)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP22"
			(at 0 -1.448 0)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "RNBD451_BLE")
		(sheetfile "RNBD451_BLE.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 93 "RNBD_PB2")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 121.8 52.5)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP4"
			(at -2.25 -0.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "RNBD451_BLE")
		(sheetfile "RNBD451_BLE.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 75 "RNBD_PB0")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Connector_Wire:SolderWirePad_1x01_SMD_1x2mm"
		(layer "F.Cu")
		(at 102 100 -90)
		(descr "Wire Pad, Square, SMD Pad,  1mm x 2mm,")
		(tags "MesurementPoint Square SMDPad 1mmx2mm ")
		(property "Reference" "PIN_PC5"
			(at 0 -6.25 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x01_Pin"
			(at 0 2.54 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Wire:SolderWirePad_1x01_SMD_1x2mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Stammblatt")
		(sheetfile "Adapter_CANBridge.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at 0 0 270)
			(size 1 2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 62 "PIN_PC5_N15")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 137.75 68)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP14"
			(at 1.75 1.8 -90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "RNBD451_BLE")
		(sheetfile "RNBD451_BLE.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 85 "RNBD_PB13")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 151 113.5 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R6"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "100k_adj"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "uBlox_Neo-M9N")
		(sheetfile "untitled.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 67 "Net-(JP3-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 146 57.25)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP20"
			(at 0 -1.448 0)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "RNBD451_BLE")
		(sheetfile "RNBD451_BLE.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 91 "RNBD_PA2")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Würth_WE-CNSW:WE-CNSW_1812_744235510"
		(layer "F.Cu")
		(at 121 128 180)
		(descr "WE-CNSW SMT Common Mode Line Filter  Size: 1812")
		(property "Reference" "L1"
			(at 0.06 -2.7 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "744235510"
			(at -2.14 3.41 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Würth_WE-CNSW:WE-CNSW_1812_744235510"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "WE-CNSW SMD Common Mode Line Filter\n\nCharacteristics\n\nCurrent compensated data line filter\nHigh common mode noise suppression at high frequencies\nSmall influence on high speed signals through winding symmetry\nClimatic category 40/105/21 (Size 0603)\nClimatic category 40/125/21 (Size 0805/1206/1812)\nFlammability corresponding to UL 94 V-0\n\nApplications\n\nUSB 2.0\nIEEE 1394 (Firewire)\nLVDS\nHigh Speed Data Lines\nLAN\n\nhttps://katalog.we-online.com/media/images/v2/o14771v209%20we-cnsw_stroko_smd_gruppe.jpg\n\nDetails see: http://katalog.we-online.de/en/pbs/WE-CNSW http://katalog.we-online.de/en/pbs/WE-CNSW\n\nUpdated by  Ella Wu 2019-01-09\n2019 (C) Wurth Elektronik"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Stammblatt")
		(sheetfile "Adapter_CANBridge.kicad_sch")
		(pad "1" smd rect
			(at -1.825 1.125)
			(size 1.15 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 103 "Net-(L1-4)")
			(pinfunction "4")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 1.825 1.125)
			(size 1.15 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "Net-(CONN_CAN0-Pin_3)")
			(pinfunction "3")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "3" smd rect
			(at 1.825 -1.125)
			(size 1.15 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "Net-(CONN_CAN0-Pin_1)")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "4" smd rect
			(at -1.825 -1.125)
			(size 1.15 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 102 "Net-(L1-1)")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 124 51.5)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP3"
			(at -2 -1.25 0)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "RNBD451_BLE")
		(sheetfile "RNBD451_BLE.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 74 "RNBD_NMCLR")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 150 52.5)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP23"
			(at 2.3 -0.9 0)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "RNBD451_BLE")
		(sheetfile "RNBD451_BLE.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 94 "RNBD_PB1")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "RNBD451PE:MOD39_15p5X20p7X2p8_ZSX_MCH"
		(layer "F.Cu")
		(at 135 53.6)
		(tags "RNBD451PE-I100 ")
		(property "Reference" "U2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "RNBD451PE-I100"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "RNBD451PE:MOD39_15p5X20p7X2p8_ZSX_MCH"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "RNBD451PE-I100"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MOD39_15p5X20p7X2p8_ZSX_MCH")
		(sheetname "RNBD451_BLE")
		(sheetfile "RNBD451_BLE.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -8.6827 -3.65 0)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -8.6827 -3.65 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -6.1173 -3.65 0)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -6.1173 -3.65 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -7.4 -3.650001)
			(size 1.2954 0.7112)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_out")
		)
		(pad "2" smd rect
			(at -7.4 -2.65)
			(size 1.2954 0.7112)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_out")
		)
		(pad "3" smd rect
			(at -7.4 -1.65)
			(size 1.2954 0.7112)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 74 "RNBD_NMCLR")
			(pinfunction "NMCLR")
			(pintype "input")
		)
		(pad "4" smd rect
			(at -7.4 -0.649999)
			(size 1.2954 0.7112)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 75 "RNBD_PB0")
			(pinfunction "PB0")
			(pintype "bidirectional")
		)
		(pad "5" smd rect
			(at -7.4 0.349999)
			(size 1.2954 0.7112)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 76 "RNBD_PB3")
			(pinfunction "PB3")
			(pintype "bidirectional")
		)
		(pad "6" smd rect
			(at -7.4 1.349999)
			(size 1.2954 0.7112)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 77 "RNBD_PB5")
			(pinfunction "PB5")
			(pintype "bidirectional")
		)
		(pad "7" smd rect
			(at -7.4 2.35)
			(size 1.2954 0.7112)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "RNBD_VDD_3V3")
			(pinfunction "VDD_A")
			(pintype "power_in")
		)
		(pad "8" smd rect
			(at -7.4 3.350001)
			(size 1.2954 0.7112)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_out")
		)
		(pad "9" smd rect
			(at -7.4 4.350001)
			(size 1.2954 0.7112)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 109 "unconnected-(U2-PA11-Pad9)")
			(pinfunction "PA11")
			(pintype "bidirectional")
		)
		(pad "10" smd rect
			(at -7.4 5.349999)
			(size 1.2954 0.7112)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 110 "unconnected-(U2-PA12-Pad10)")
			(pinfunction "PA12")
			(pintype "bidirectional")
		)
		(pad "11" smd rect
			(at -7.4 6.35)
			(size 1.2954 0.7112)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_out")
		)
		(pad "12" smd rect
			(at -7.4 7.35)
			(size 1.2954 0.7112)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 46 "RNBD_UART-RX")
			(pinfunction "PB6")
			(pintype "bidirectional")
		)
		(pad "13" smd rect
			(at -7.4 8.350001)
			(size 1.2954 0.7112)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 78 "RNBD_PB7")
			(pinfunction "PB7")
			(pintype "bidirectional")
		)
		(pad "14" smd rect
			(at -6.000001 10 90)
			(size 1.2954 0.7112)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 79 "RNBD_PB8")
			(pinfunction "PB8")
			(pintype "bidirectional")
		)
		(pad "15" smd rect
			(at -5 10 90)
			(size 1.2954 0.7112)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 111 "unconnected-(U2-PB9-Pad15)")
			(pinfunction "PB9")
			(pintype "bidirectional")
		)
		(pad "16" smd rect
			(at -4 10 90)
			(size 1.2954 0.7112)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 45 "RNBD_UART-RTS")
			(pinfunction "PA4")
			(pintype "bidirectional")
		)
		(pad "17" smd rect
			(at -2.999999 10 90)
			(size 1.2954 0.7112)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 80 "RNBD_PB10")
			(pinfunction "PB10")
			(pintype "bidirectional")
		)
		(pad "18" smd rect
			(at -2.000001 10 90)
			(size 1.2954 0.7112)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 81 "RNBD_PB11")
			(pinfunction "PB11")
			(pintype "bidirectional")
		)
		(pad "19" smd rect
			(at -1.000001 10 90)
			(size 1.2954 0.7112)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_out")
		)
		(pad "20" smd rect
			(at 0 10 90)
			(size 1.2954 0.7112)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 82 "RNBD_PA0")
			(pinfunction "PA0")
			(pintype "bidirectional")
		)
		(pad "21" smd rect
			(at 1.000001 10 90)
			(size 1.2954 0.7112)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 83 "RNBD_PA1")
			(pinfunction "PA1")
			(pintype "bidirectional")
		)
		(pad "22" smd rect
			(at 2.000001 10 90)
			(size 1.2954 0.7112)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 84 "RNBD_PB12")
			(pinfunction "PB12")
			(pintype "bidirectional")
		)
		(pad "23" smd rect
			(at 2.999999 10 90)
			(size 1.2954 0.7112)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 85 "RNBD_PB13")
			(pinfunction "PB13")
			(pintype "bidirectional")
		)
		(pad "24" smd rect
			(at 4 10 90)
			(size 1.2954 0.7112)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 47 "RNBD_UART-TX")
			(pinfunction "PA5")
			(pintype "bidirectional")
		)
		(pad "25" smd rect
			(at 5 10 90)
			(size 1.2954 0.7112)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 44 "RNBD_UART-CTS")
			(pinfunction "PA6")
			(pintype "bidirectional")
		)
		(pad "26" smd rect
			(at 6.000001 10 90)
			(size 1.2954 0.7112)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_out")
		)
		(pad "27" smd rect
			(at 7.4 8.350001)
			(size 1.2954 0.7112)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "RNBD_VDD_3V3")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "28" smd rect
			(at 7.4 7.35)
			(size 1.2954 0.7112)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "RNBD_VDD_3V3")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "29" smd rect
			(at 7.4 6.35)
			(size 1.2954 0.7112)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 86 "RNBD_PA8")
			(pinfunction "PA8")
			(pintype "bidirectional")
		)
		(pad "30" smd rect
			(at 7.4 5.349999)
			(size 1.2954 0.7112)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 108 "unconnected-(U2-PA9-Pad30)")
			(pinfunction "PA9")
			(pintype "bidirectional")
		)
		(pad "31" smd rect
			(at 7.4 4.350001)
			(size 1.2954 0.7112)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 87 "RNBD_PA7")
			(pinfunction "PA7")
			(pintype "bidirectional")
		)
		(pad "32" smd rect
			(at 7.4 3.350001)
			(size 1.2954 0.7112)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 88 "RNBD_PA10")
			(pinfunction "PA10")
			(pintype "bidirectional")
		)
		(pad "33" smd rect
			(at 7.4 2.35)
			(size 1.2954 0.7112)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 89 "RNBD_PA13")
			(pinfunction "PA13")
			(pintype "bidirectional")
		)
		(pad "34" smd rect
			(at 7.4 1.349999)
			(size 1.2954 0.7112)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 90 "RNBD_PA14")
			(pinfunction "PA14")
			(pintype "bidirectional")
		)
		(pad "35" smd rect
			(at 7.4 0.349999)
			(size 1.2954 0.7112)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 91 "RNBD_PA2")
			(pinfunction "PA2")
			(pintype "bidirectional")
		)
		(pad "36" smd rect
			(at 7.4 -0.649999)
			(size 1.2954 0.7112)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 92 "RNBD_PA3")
			(pinfunction "PA3")
			(pintype "bidirectional")
		)
		(pad "37" smd rect
			(at 7.4 -1.65)
			(size 1.2954 0.7112)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 93 "RNBD_PB2")
			(pinfunction "PB2")
			(pintype "bidirectional")
		)
		(pad "38" smd rect
			(at 7.4 -2.65)
			(size 1.2954 0.7112)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 94 "RNBD_PB1")
			(pinfunction "PB1")
			(pintype "bidirectional")
		)
		(pad "39" smd rect
			(at 7.4 -3.650001)
			(size 1.2954 0.7112)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 95 "RNBD_PB4")
			(pinfunction "PB4")
			(pintype "bidirectional")
		)
		(pad "40" smd rect
			(at -1.88 2.15)
			(size 0.889 0.889)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "TPAD_GND")
			(pintype "power_out")
		)
		(pad "41" smd rect
			(at -0.68 2.15)
			(size 0.889 0.889)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "TPAD_GND")
			(pintype "power_out")
		)
		(pad "42" smd rect
			(at 0.52 2.15)
			(size 0.889 0.889)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "TPAD_GND")
			(pintype "power_out")
		)
		(pad "43" smd rect
			(at -1.88 3.35)
			(size 0.889 0.889)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "TPAD_GND")
			(pintype "power_out")
		)
		(pad "44" smd rect
			(at -0.68 3.35)
			(size 0.889 0.889)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "TPAD_GND")
			(pintype "power_out")
		)
		(pad "45" smd rect
			(at 0.52 3.35)
			(size 0.889 0.889)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "TPAD_GND")
			(pintype "power_out")
		)
		(pad "46" smd rect
			(at -1.88 4.55)
			(size 0.889 0.889)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "TPAD_GND")
			(pintype "power_out")
		)
		(pad "47" smd rect
			(at -0.68 4.55)
			(size 0.889 0.889)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "TPAD_GND")
			(pintype "power_out")
		)
		(pad "48" smd rect
			(at 0.52 4.55)
			(size 0.889 0.889)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "TPAD_GND")
			(pintype "power_out")
		)
	)
	(footprint "Connector_Wire:SolderWirePad_1x01_SMD_1x2mm"
		(layer "F.Cu")
		(at 158.25 129.5 180)
		(descr "Wire Pad, Square, SMD Pad,  1mm x 2mm,")
		(tags "MesurementPoint Square SMDPad 1mmx2mm ")
		(property "Reference" "uBlox_USB-DM1"
			(at 0 -7.5 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x01_Pin"
			(at 0 2.54 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Wire:SolderWirePad_1x01_SMD_1x2mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "uBlox_Neo-M9N")
		(sheetfile "untitled.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at 0 0 180)
			(size 1 2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 68 "uBlox_USB-DM")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder"
		(layer "F.Cu")
		(at 134 117.25 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C7"
			(at 0 -1.16 90)
			(layer "F.SilkS")
		)
		(property "Value" "100n_25V_X7R"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Stammblatt")
		(sheetfile "Adapter_CANBridge.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.5675 0 270)
			(size 0.735 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "Net-(JP5-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.5675 0 270)
			(size 0.735 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Keystone_5019_Minature"
		(layer "F.Cu")
		(at 150.5 118.25 180)
		(descr "SMT Test Point- Micro Miniature 5019, http://www.keyelco.com/product-pdf.cfm?p=1357")
		(tags "Test Point")
		(property "Reference" "TP2"
			(at 0 -2.25 0)
			(layer "F.SilkS")
		)
		(property "Value" "uBlox_EXTINT0"
			(at 0 2.25 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Keystone_5019_Minature"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "uBlox_Neo-M9N")
		(sheetfile "untitled.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 0 180)
			(size 3.8 2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 73 "Net-(U1-EXTINT0)")
			(pinfunction "1")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/TestPoint.3dshapes/TestPoint_Keystone_5019_Minature.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 152.5 104.6 180)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "JP7"
			(at 0 -1.8 0)
			(layer "F.SilkS")
		)
		(property "Value" "SolderJumper_2_Open"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "uBlox_Neo-M9N")
		(sheetfile "untitled.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" smd custom
			(at -0.65 0 180)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 5 "Net-(JP1-B)")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0 180)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 1 "+3.3V")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 159.75 126 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R5"
			(at 0 1.5 90)
			(layer "F.SilkS")
		)
		(property "Value" "27R"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "uBlox_Neo-M9N")
		(sheetfile "untitled.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 70 "uBlox_USB-DP")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 71 "Net-(U1-USB_DP)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Keystone_5019_Minature"
		(layer "F.Cu")
		(at 167 103.25 90)
		(descr "SMT Test Point- Micro Miniature 5019, http://www.keyelco.com/product-pdf.cfm?p=1357")
		(tags "Test Point")
		(property "Reference" "TP1"
			(at 3.85 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "uBlox_EXTINT1"
			(at 0 2.25 90)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Keystone_5019_Minature"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "uBlox_Neo-M9N")
		(sheetfile "untitled.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 0 90)
			(size 3.8 2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 72 "Net-(U1-EXTINT1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/TestPoint.3dshapes/TestPoint_Keystone_5019_Minature.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
		(layer "F.Cu")
		(at 129 117.25 180)
		(descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U1_CAN1"
			(at 0.5 -3.55 0)
			(layer "F.SilkS")
		)
		(property "Value" "MCP2562-H-SN"
			(at 0 3.4 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/25167A.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "High-Speed CAN Transceiver, 1Mbps, 5V supply, Vio pin, -40C to +150C, SOIC-8"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOIC*3.9x4.9mm*P1.27mm*")
		(sheetname "Stammblatt")
		(sheetfile "Adapter_CANBridge.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.475 -1.905 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 64 "PIN_PC7_N18")
			(pinfunction "TXD")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2.475 -0.635 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -2.475 0.635 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "Net-(JP5-A)")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at -2.475 1.905 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 63 "PIN_PC6_N17")
			(pinfunction "RXD")
			(pintype "output")
		)
		(pad "5" smd roundrect
			(at 2.475 1.905 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "+3.3V")
			(pinfunction "Vio")
			(pintype "power_in")
		)
		(pad "6" smd roundrect
			(at 2.475 0.635 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 105 "Net-(L3-4)")
			(pinfunction "CANL")
			(pintype "bidirectional")
		)
		(pad "7" smd roundrect
			(at 2.475 -0.635 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 104 "Net-(L3-1)")
			(pinfunction "CANH")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at 2.475 -1.905 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "STBY")
			(pintype "input")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 158.25 126 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R4"
			(at 1.7 -1.25 90)
			(layer "F.SilkS")
		)
		(property "Value" "27R"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "uBlox_Neo-M9N")
		(sheetfile "untitled.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 68 "uBlox_USB-DM")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 69 "Net-(U1-USB_DM)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder"
		(layer "F.Cu")
		(at 124.5 58)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C9"
			(at 0 -1.16 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n_25V_X7R"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "RNBD451_BLE")
		(sheetfile "RNBD451_BLE.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.5675 0)
			(size 0.735 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "RNBD_VDD_3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.5675 0)
			(size 0.735 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 155.5 126.75 90)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "JP2"
			(at 0 -1.8 90)
			(layer "F.SilkS")
		)
		(property "Value" "SolderJumper_2_Open"
			(at 0 1.9 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "uBlox_Neo-M9N")
		(sheetfile "untitled.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" smd custom
			(at -0.65 0 90)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 2 "GND")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0 90)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 66 "Net-(JP2-B)")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 118.5 54.5)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP5"
			(at -2.5 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "RNBD451_BLE")
		(sheetfile "RNBD451_BLE.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 76 "RNBD_PB3")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 150 59.5)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP19"
			(at 0 -1.448 0)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "RNBD451_BLE")
		(sheetfile "RNBD451_BLE.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 90 "RNBD_PA14")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Horizontal"
		(layer "F.Cu")
		(at 112.375 130.525 180)
		(descr "Through hole angled pin header, 1x03, 2.54mm pitch, 6mm pin length, single row")
		(tags "Through hole angled pin header THT 1x03 2.54mm single row")
		(property "Reference" "CONN_CAN0"
			(at 4.375 7.525 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x03"
			(at 4.385 7.35 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Horizontal"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Stammblatt")
		(sheetfile "Adapter_CANBridge.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.77 2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(CONN_CAN0-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(CONN_CAN0-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 136.75 70.5)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP13"
			(at 0.25 3 -90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "RNBD451_BLE")
		(sheetfile "RNBD451_BLE.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 84 "RNBD_PB12")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 144 69 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C10"
			(at -3.5 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "4u7_25VX7R"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "RNBD451_BLE")
		(sheetfile "RNBD451_BLE.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 180)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 8 "RNBD_VDD_3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 180)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 132 102.75)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "JP6"
			(at 0 -1.8 0)
			(layer "F.SilkS")
		)
		(property "Value" "SolderJumper_2_Open"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "Stammblatt")
		(sheetfile "Adapter_CANBridge.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" smd custom
			(at -0.65 0)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 4 "Net-(JP6-A)")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 19 "+5V")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 116 117.25 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R3"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "120R"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Stammblatt")
		(sheetfile "Adapter_CANBridge.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 16 "Net-(CONN_CAN1-Pin_1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 15 "Net-(CONN_CAN1-Pin_3)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Horizontal"
		(layer "F.Cu")
		(at 112.375 119.65 180)
		(descr "Through hole angled pin header, 1x03, 2.54mm pitch, 6mm pin length, single row")
		(tags "Through hole angled pin header THT 1x03 2.54mm single row")
		(property "Reference" "CONN_CAN1"
			(at 4.385 7.4 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x03"
			(at 4.385 7.35 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Horizontal"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Stammblatt")
		(sheetfile "Adapter_CANBridge.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.77 2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(CONN_CAN1-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(CONN_CAN1-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Horizontal"
		(layer "F.Cu")
		(at 167.5 85.71)
		(descr "Through hole angled pin header, 1x04, 2.54mm pitch, 6mm pin length, single row")
		(tags "Through hole angled pin header THT 1x04 2.54mm single row")
		(property "Reference" "EXT2"
			(at 0 -2.51 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x04"
			(at 4.385 9.89 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Horizontal"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "RNBD451_BLE")
		(sheetfile "RNBD451_BLE.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.77 3.81 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "RNBD_UART-CTS")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "RNBD_UART-TX")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "RNBD_UART-RTS")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "RNBD_UART-RX")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 156.85 104.5 180)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "JP1"
			(at 0 -1.8 0)
			(layer "F.SilkS")
		)
		(property "Value" "SolderJumper_2_Open"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "uBlox_Neo-M9N")
		(sheetfile "untitled.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" smd custom
			(at -0.65 0 180)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 65 "Net-(JP1-A)")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0 180)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 5 "Net-(JP1-B)")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 132 113.25)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "JP5"
			(at 0 -1.8 0)
			(layer "F.SilkS")
		)
		(property "Value" "SolderJumper_2_Open"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "Stammblatt")
		(sheetfile "Adapter_CANBridge.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" smd custom
			(at -0.65 0)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 7 "Net-(JP5-A)")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 19 "+5V")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 152 110 90)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "JP3"
			(at 0 -1.8 90)
			(layer "F.SilkS")
		)
		(property "Value" "SolderJumper_2_Open"
			(at 0 1.9 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "uBlox_Neo-M9N")
		(sheetfile "untitled.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" smd custom
			(at -0.65 0 90)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 67 "Net-(JP3-A)")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0 90)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 5 "Net-(JP1-B)")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 123.75 60.5)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C8"
			(at -1.05 2.2 -90)
			(layer "F.SilkS")
		)
		(property "Value" "4u7_25V_X7R"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "RNBD451_BLE")
		(sheetfile "RNBD451_BLE.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 8 "RNBD_VDD_3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
		(layer "F.Cu")
		(at 129 106.75 180)
		(descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U1_CAN2"
			(at 1.9 -3.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "MCP2562-H-SN"
			(at 0 3.4 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/25167A.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "High-Speed CAN Transceiver, 1Mbps, 5V supply, Vio pin, -40C to +150C, SOIC-8"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOIC*3.9x4.9mm*P1.27mm*")
		(sheetname "Stammblatt")
		(sheetfile "Adapter_CANBridge.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.475 -1.905 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 24 "PIN_PC26_K18")
			(pinfunction "TXD")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2.475 -0.635 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -2.475 0.635 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "Net-(JP6-A)")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at -2.475 1.905 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 21 "PIN_PC25_K17")
			(pinfunction "RXD")
			(pintype "output")
		)
		(pad "5" smd roundrect
			(at 2.475 1.905 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "+3.3V")
			(pinfunction "Vio")
			(pintype "power_in")
		)
		(pad "6" smd roundrect
			(at 2.475 0.635 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 106 "Net-(L2-4)")
			(pinfunction "CANL")
			(pintype "bidirectional")
		)
		(pad "7" smd roundrect
			(at 2.475 -0.635 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 107 "Net-(L2-1)")
			(pinfunction "CANH")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at 2.475 -1.905 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "STBY")
			(pintype "input")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 134.5 68)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP12"
			(at 0.25 -2 0)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "RNBD451_BLE")
		(sheetfile "RNBD451_BLE.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 83 "RNBD_PA1")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Horizontal"
		(layer "F.Cu")
		(at 167.5 56.625)
		(descr "Through hole angled pin header, 1x08, 2.54mm pitch, 6mm pin length, single row")
		(tags "Through hole angled pin header THT 1x08 2.54mm single row")
		(property "Reference" "EXT1"
			(at 0 -2.125 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x08"
			(at 4.385 20.05 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Horizontal"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "uBlox_Neo-M9N")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.77 8.89 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "PIN_PC7_N18")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "uBlox_UART_RX")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "uBlox_UART_TX")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 101 "uBlox_SCL")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 98 "uBlox_SDA")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 0 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "uBlox_RST")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "PIN_PC1_T17")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 0 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "PIN_PC0_P15")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Keystone_5019_Minature"
		(layer "F.Cu")
		(at 170 103.25 90)
		(descr "SMT Test Point- Micro Miniature 5019, http://www.keyelco.com/product-pdf.cfm?p=1357")
		(tags "Test Point")
		(property "Reference" "TP26"
			(at 4.35 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "uBlox_LNA_EN"
			(at 0 2.25 90)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Keystone_5019_Minature"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "uBlox_Neo-M9N")
		(sheetfile "untitled.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 0 90)
			(size 3.8 2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 97 "Net-(U1-LNA_EN)")
			(pinfunction "1")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/TestPoint.3dshapes/TestPoint_Keystone_5019_Minature.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 122 56)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP6"
			(at -2.25 0.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "RNBD451_BLE")
		(sheetfile "RNBD451_BLE.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 77 "RNBD_PB5")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 131.1 68)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP10"
			(at -0.75 -1.75 0)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "RNBD451_BLE")
		(sheetfile "RNBD451_BLE.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 81 "RNBD_PB11")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 146 61)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP17"
			(at 0 -1.4 0)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "RNBD451_BLE")
		(sheetfile "RNBD451_BLE.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 88 "RNBD_PA10")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder"
		(layer "F.Cu")
		(at 143.5 67 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C11"
			(at -3 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n_25V_X7R"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "RNBD451_BLE")
		(sheetfile "RNBD451_BLE.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.5675 0 180)
			(size 0.735 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "RNBD_VDD_3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.5675 0 180)
			(size 0.735 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Würth_WE-CNSW:WE-CNSW_1812_744235510"
		(layer "F.Cu")
		(at 121 117.25 180)
		(descr "WE-CNSW SMT Common Mode Line Filter  Size: 1812")
		(property "Reference" "L3"
			(at -0.1 -2.65 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "744235510"
			(at -2.14 3.41 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Würth_WE-CNSW:WE-CNSW_1812_744235510"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "WE-CNSW SMD Common Mode Line Filter\n\nCharacteristics\n\nCurrent compensated data line filter\nHigh common mode noise suppression at high frequencies\nSmall influence on high speed signals through winding symmetry\nClimatic category 40/105/21 (Size 0603)\nClimatic category 40/125/21 (Size 0805/1206/1812)\nFlammability corresponding to UL 94 V-0\n\nApplications\n\nUSB 2.0\nIEEE 1394 (Firewire)\nLVDS\nHigh Speed Data Lines\nLAN\n\nhttps://katalog.we-online.com/media/images/v2/o14771v209%20we-cnsw_stroko_smd_gruppe.jpg\n\nDetails see: http://katalog.we-online.de/en/pbs/WE-CNSW http://katalog.we-online.de/en/pbs/WE-CNSW\n\nUpdated by  Ella Wu 2019-01-09\n2019 (C) Wurth Elektronik"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Stammblatt")
		(sheetfile "Adapter_CANBridge.kicad_sch")
		(pad "1" smd rect
			(at -1.825 1.125)
			(size 1.15 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 105 "Net-(L3-4)")
			(pinfunction "4")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 1.825 1.125)
			(size 1.15 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "Net-(CONN_CAN1-Pin_3)")
			(pinfunction "3")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "3" smd rect
			(at 1.825 -1.125)
			(size 1.15 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "Net-(CONN_CAN1-Pin_1)")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "4" smd rect
			(at -1.825 -1.125)
			(size 1.15 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 104 "Net-(L3-1)")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder"
		(layer "F.Cu")
		(at 134 106.75 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C4"
			(at 0 -1.16 90)
			(layer "F.SilkS")
		)
		(property "Value" "100n_25V_X7R"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Stammblatt")
		(sheetfile "Adapter_CANBridge.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.5675 0 270)
			(size 0.735 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "Net-(JP6-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.5675 0 270)
			(size 0.735 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 150 62.75)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP18"
			(at 0 -1.448 0)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "RNBD451_BLE")
		(sheetfile "RNBD451_BLE.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 89 "RNBD_PA13")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 150 56)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP21"
			(at 0 -1.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "RNBD451_BLE")
		(sheetfile "RNBD451_BLE.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 92 "RNBD_PA3")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Connector_Wire:SolderWirePad_1x01_SMD_1x2mm"
		(layer "F.Cu")
		(at 102 98.5 -90)
		(descr "Wire Pad, Square, SMD Pad,  1mm x 2mm,")
		(tags "MesurementPoint Square SMDPad 1mmx2mm ")
		(property "Reference" "PIN_PC6"
			(at 0 -7.5 180)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x01_Pin"
			(at 0 2.54 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Wire:SolderWirePad_1x01_SMD_1x2mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Stammblatt")
		(sheetfile "Adapter_CANBridge.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at 0 0 270)
			(size 1 2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 63 "PIN_PC6_N17")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder"
		(layer "F.Cu")
		(at 126 113.25 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C6"
			(at 0 -1.16 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n_25V_X7R"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Stammblatt")
		(sheetfile "Adapter_CANBridge.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.5675 0 180)
			(size 0.735 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.5675 0 180)
			(size 0.735 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Keystone_5019_Minature"
		(layer "F.Cu")
		(at 163.39 133.25 90)
		(descr "SMT Test Point- Micro Miniature 5019, http://www.keyelco.com/product-pdf.cfm?p=1357")
		(tags "Test Point")
		(property "Reference" "TP25"
			(at 0 -2.25 90)
			(layer "F.SilkS")
		)
		(property "Value" "uBlox_VCC_RF"
			(at 0 2.25 90)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Keystone_5019_Minature"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "uBlox_Neo-M9N")
		(sheetfile "untitled.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 0 90)
			(size 3.8 2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 96 "Net-(U1-VCC_RF)")
			(pinfunction "1")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/TestPoint.3dshapes/TestPoint_Keystone_5019_Minature.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Wire:SolderWirePad_1x01_SMD_1x2mm"
		(layer "F.Cu")
		(at 159.75 129.5 180)
		(descr "Wire Pad, Square, SMD Pad,  1mm x 2mm,")
		(tags "MesurementPoint Square SMDPad 1mmx2mm ")
		(property "Reference" "uBlox_USB-DP1"
			(at 0 -7.5 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x01_Pin"
			(at 0 2.54 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Wire:SolderWirePad_1x01_SMD_1x2mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "uBlox_Neo-M9N")
		(sheetfile "untitled.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at 0 0 180)
			(size 1 2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 70 "uBlox_USB-DP")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical"
		(layer "B.Cu")
		(at 112.33799 61.32863 180)
		(descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x08 2.54mm single row")
		(property "Reference" "CONN_Arduino_Shield_links_oben1"
			(at -2.66201 -5.67137 -90)
			(layer "B.SilkS")
		)
		(property "Value" "Conn_01x08"
			(at 0 -20.11 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Stammblatt")
		(sheetfile "Adapter_CANBridge.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 -8.89 90)
			(layer "B.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 112 "unconnected-(CONN_Arduino_Shield_links_oben1-Pin_1-Pad1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 -2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+3.3V")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 -5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 113 "unconnected-(CONN_Arduino_Shield_links_oben1-Pin_3-Pad3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 -7.62 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+3.3V")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 -10.16 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 118 "+5V_res")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 0 -12.7 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 -15.24 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 0 -17.78 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 114 "unconnected-(CONN_Arduino_Shield_links_oben1-Pin_8-Pad8)")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x10_P2.54mm_Vertical"
		(layer "B.Cu")
		(at 160.59799 75.0696)
		(descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x10 2.54mm single row")
		(property "Reference" "JCONN_Arduino_Shield_rechts_oben1"
			(at 2.40201 -11.0696 90)
			(layer "B.SilkS")
		)
		(property "Value" "Conn_01x10"
			(at 0 -25.19 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x10_P2.54mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x10, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Stammblatt")
		(sheetfile "Adapter_CANBridge.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 -11.43 90)
			(layer "B.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "PIN_PG10_G13")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 -2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "PIN_PB11_14")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 -5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 59 "PIN_PD26_B9")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 -7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "PIN_PD24_D11")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 -10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "PIN_PD27_A8")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 0 -12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "PIN_PD25_D5")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 -15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 0 -17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "PIN_AVDD")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 0 -20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "PIN_PC25_K17")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole oval
			(at 0 -22.86)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "PIN_PC26_K18")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical"
		(layer "B.Cu")
		(at 160.59799 96.90161)
		(descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x08 2.54mm single row")
		(property "Reference" "CONN_Arduino_Shield_rechts_unten1"
			(at -3 -8.90161 90)
			(layer "B.SilkS")
		)
		(property "Value" "Conn_01x08"
			(at 0 -20.11 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Stammblatt")
		(sheetfile "Adapter_CANBridge.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 -8.89 90)
			(layer "B.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "PIN_PC22_P18")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 -2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "PIN_PC21_P17")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 -5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "PIN_PG6_L15")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 -7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "PIN_PG5_J17")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 -10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "PIN_PG7_L12")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 0 -12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "PIN_PA23_G1")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 -15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "PIN_PA22_G4")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 0 -17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "PIN_PG9_K12")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_2x10_P2.54mm_Vertical"
		(layer "B.Cu")
		(at 133.46 161.16)
		(descr "Through hole straight pin header, 2x10, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x10 2.54mm double row")
		(property "Reference" "CONN_X32_links1"
			(at -2.46 -10.16 90)
			(layer "B.SilkS")
		)
		(property "Value" "Conn_02x10_Odd_Even"
			(at 1.27 -25.19 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_2x10_P2.54mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x10, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "Stammblatt")
		(sheetfile "Adapter_CANBridge.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 -11.43 90)
			(layer "B.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 -2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "PIN_PC9_M18")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 2.54 -2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "PIN_PC11_H15")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 -5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "PIN_PC8_M13")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 2.54 -5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "PIN_PC10_H17")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 -7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "PIN_PC13_F17_res")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 2.54 -7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "PIN_PE11_M6_res")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 0 -10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "PIN_PC12_F18_res")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole oval
			(at 2.54 -10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "unconnected-(CONN_X32_links1-Pin_10-Pad10)")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole oval
			(at 0 -12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "PIN_PC2_T18_res")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole oval
			(at 2.54 -12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "PIN_PC1_T17")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" thru_hole oval
			(at 0 -15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 117 "PIN_PC3_R17_res")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" thru_hole oval
			(at 2.54 -15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "PIN_PC4_R18")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(pad "15" thru_hole oval
			(at 0 -17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_15")
			(pintype "passive")
		)
		(pad "16" thru_hole oval
			(at 2.54 -17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_16")
			(pintype "passive")
		)
		(pad "17" thru_hole oval
			(at 0 -20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "unconnected-(CONN_X32_links1-Pin_17-Pad17)")
			(pinfunction "Pin_17")
			(pintype "passive")
		)
		(pad "18" thru_hole oval
			(at 2.54 -20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+3.3V")
			(pinfunction "Pin_18")
			(pintype "passive")
		)
		(pad "19" thru_hole oval
			(at 0 -22.86)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "unconnected-(CONN_X32_links1-Pin_19-Pad19)")
			(pinfunction "Pin_19")
			(pintype "passive")
		)
		(pad "20" thru_hole oval
			(at 2.54 -22.86)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 118 "+5V_res")
			(pinfunction "Pin_20")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x10_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical"
		(layer "B.Cu")
		(at 165.1973 156.07143)
		(descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x08 2.54mm single row")
		(property "Reference" "CONN_mikroBUS_rechts1"
			(at -2.1973 -7.07143 -90)
			(layer "B.SilkS")
		)
		(property "Value" "Conn_01x08"
			(at 0 -20.11 180)
			(layer "B.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Stammblatt")
		(sheetfile "Adapter_CANBridge.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 -8.89 -90)
			(layer "B.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 131 "PIN_PA14_R2_res")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 -2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 133 "PIN_PB27_V10_res")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 -5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 134 "PIN_PC14_E17_res")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 -7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "PIN_PC13_F17_res")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 -10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 135 "PIN_PC15_G12_res")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 0 -12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "PIN_PC12_F18_res")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 -15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 132 "+3.3V_res")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 0 -17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical"
		(layer "B.Cu")
		(at 142.34423 156.06782)
		(descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x08 2.54mm single row")
		(property "Reference" "CONN_mikroBUS_links1"
			(at -2.34423 -7.06782 -90)
			(layer "B.SilkS")
		)
		(property "Value" "Conn_01x08"
			(at 0 -20.11 180)
			(layer "B.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Stammblatt")
		(sheetfile "Adapter_CANBridge.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 -8.89 -90)
			(layer "B.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 125 "PIN_PA22_G4_res")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 -2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 126 "PIN_PA8_K2_res")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 -5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 129 "PIN_PC22_P18_res")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 -7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 128 "PIN_PC21_P17_res")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 -10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 130 "PIN_PC26_K18_res")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 0 -12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 127 "PIN_PC25_K17_res")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 -15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "+5V")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 0 -17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical"
		(layer "B.Cu")
		(at 112.33799 84.20763 180)
		(descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x06 2.54mm single row")
		(property "Reference" "CONN_Arduino_Shield_blau1"
			(at 0 2.33 0)
			(layer "B.SilkS")
		)
		(property "Value" "Conn_01x06"
			(at 0 -15.03 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Stammblatt")
		(sheetfile "Adapter_CANBridge.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 -6.35 90)
			(layer "B.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "PIN_PA18_U3")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 -2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "PIN_PA17_V3")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 -5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "PIN_PA16_U2")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 -7.62 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "PIN_PA15_U1")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 -10.16 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 116 "PIN_PA29_T2")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 0 -12.7 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 115 "PIN_PA28_T1")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_2x06_P2.54mm_Vertical"
		(layer "B.Cu")
		(at 171.56 151)
		(descr "Through hole straight pin header, 2x06, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x06 2.54mm double row")
		(property "Reference" "CONN_X32_rechts1"
			(at -2.275 -6.35 90)
			(layer "B.SilkS")
		)
		(property "Value" "Conn_02x06_Odd_Even"
			(at 1.27 -15.03 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_2x06_P2.54mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x06, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "Stammblatt")
		(sheetfile "Adapter_CANBridge.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 -6.35 90)
			(layer "B.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "unconnected-(CONN_X32_rechts1-Pin_1-Pad1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "unconnected-(CONN_X32_rechts1-Pin_2-Pad2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 -2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 120 "PIN_PE1_H2_res")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 2.54 -2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 122 "PIN_PA18_U3_res")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 -5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 123 "PIN_PE2_J1_res")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 2.54 -5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "unconnected-(CONN_X32_rechts1-Pin_6-Pad6)")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 -7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 121 "PIN_PE0_H1_res")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 2.54 -7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "unconnected-(CONN_X32_rechts1-Pin_8-Pad8)")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 0 -10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 124 "PIN_PA31_G2_res")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole oval
			(at 2.54 -10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "unconnected-(CONN_X32_rechts1-Pin_10-Pad10)")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole oval
			(at 0 -12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole oval
			(at 2.54 -12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x06_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_poly
		(pts
			(xy 100 49) (xy 172.5 49) (xy 172.5 134) (xy 177 134) (xy 177 164) (xy 129 164) (xy 129 134) (xy 100 134)
		)
		(fill none)
		(layer "Edge.Cuts")
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 100 49) (xy 172.5 49) (xy 172.5 129) (xy 167.75 129) (xy 167.75 133) (xy 172 133) (xy 172 134)
				(xy 177 134) (xy 177 164) (xy 129 164) (xy 129 134) (xy 100 134)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 100 49) (xy 172.5 49) (xy 172.5 129) (xy 167.75 129) (xy 167.75 133) (xy 172 133) (xy 172 134)
				(xy 177 134) (xy 177 164) (xy 129 164) (xy 129 134) (xy 100 134)
			)
		)
	)
)
