(kicad_sch
	(version 20231120)
	(generator "eeschema")
	(generator_version "8.0")
	(paper "A4")
	(title_block
		(title "Adapter_CANBridge")
		(date "2025-01-10")
		(rev "1.0")
	)
	(lib_symbols
		(symbol "Connector_Generic:Conn_01x03"
			(pin_names
				(offset 1.016) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at 0 5.08 0)
			)
			(property "Value" "Conn_01x03"
				(at 0 -5.08 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
				(at 0 0 0)
			)
			(property "ki_keywords" "connector"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Connector*:*_1x??_*"
				(at 0 0 0)
			)
			(symbol "Conn_01x03_1_1"
				(rectangle
					(start -1.27 -2.413)
					(end 0 -2.667)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 0.127)
					(end 0 -0.127)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 2.667)
					(end 0 2.413)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 3.81)
					(end 1.27 -3.81)
					(fill
						(type background)
					)
				)
				(pin passive line
					(at -5.08 2.54 0)
					(length 3.81)
					(name "Pin_1")
					(number "1")
				)
				(pin passive line
					(at -5.08 0 0)
					(length 3.81)
					(name "Pin_2")
					(number "2")
				)
				(pin passive line
					(at -5.08 -2.54 0)
					(length 3.81)
					(name "Pin_3")
					(number "3")
				)
			)
		)
		(symbol "Connector_Generic:Conn_01x06"
			(pin_names
				(offset 1.016) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at 0 7.62 0)
			)
			(property "Value" "Conn_01x06"
				(at 0 -10.16 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)"
				(at 0 0 0)
			)
			(property "ki_keywords" "connector"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Connector*:*_1x??_*"
				(at 0 0 0)
			)
			(symbol "Conn_01x06_1_1"
				(rectangle
					(start -1.27 -7.493)
					(end 0 -7.747)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 -4.953)
					(end 0 -5.207)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 -2.413)
					(end 0 -2.667)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 0.127)
					(end 0 -0.127)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 2.667)
					(end 0 2.413)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 5.207)
					(end 0 4.953)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 6.35)
					(end 1.27 -8.89)
					(fill
						(type background)
					)
				)
				(pin passive line
					(at -5.08 5.08 0)
					(length 3.81)
					(name "Pin_1")
					(number "1")
				)
				(pin passive line
					(at -5.08 2.54 0)
					(length 3.81)
					(name "Pin_2")
					(number "2")
				)
				(pin passive line
					(at -5.08 0 0)
					(length 3.81)
					(name "Pin_3")
					(number "3")
				)
				(pin passive line
					(at -5.08 -2.54 0)
					(length 3.81)
					(name "Pin_4")
					(number "4")
				)
				(pin passive line
					(at -5.08 -5.08 0)
					(length 3.81)
					(name "Pin_5")
					(number "5")
				)
				(pin passive line
					(at -5.08 -7.62 0)
					(length 3.81)
					(name "Pin_6")
					(number "6")
				)
			)
		)
		(symbol "Connector_Generic:Conn_01x08"
			(pin_names
				(offset 1.016) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at 0 10.16 0)
			)
			(property "Value" "Conn_01x08"
				(at 0 -12.7 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Generic connector, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)"
				(at 0 0 0)
			)
			(property "ki_keywords" "connector"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Connector*:*_1x??_*"
				(at 0 0 0)
			)
			(symbol "Conn_01x08_1_1"
				(rectangle
					(start -1.27 -10.033)
					(end 0 -10.287)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 -7.493)
					(end 0 -7.747)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 -4.953)
					(end 0 -5.207)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 -2.413)
					(end 0 -2.667)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 0.127)
					(end 0 -0.127)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 2.667)
					(end 0 2.413)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 5.207)
					(end 0 4.953)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 7.747)
					(end 0 7.493)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 8.89)
					(end 1.27 -11.43)
					(fill
						(type background)
					)
				)
				(pin passive line
					(at -5.08 7.62 0)
					(length 3.81)
					(name "Pin_1")
					(number "1")
				)
				(pin passive line
					(at -5.08 5.08 0)
					(length 3.81)
					(name "Pin_2")
					(number "2")
				)
				(pin passive line
					(at -5.08 2.54 0)
					(length 3.81)
					(name "Pin_3")
					(number "3")
				)
				(pin passive line
					(at -5.08 0 0)
					(length 3.81)
					(name "Pin_4")
					(number "4")
				)
				(pin passive line
					(at -5.08 -2.54 0)
					(length 3.81)
					(name "Pin_5")
					(number "5")
				)
				(pin passive line
					(at -5.08 -5.08 0)
					(length 3.81)
					(name "Pin_6")
					(number "6")
				)
				(pin passive line
					(at -5.08 -7.62 0)
					(length 3.81)
					(name "Pin_7")
					(number "7")
				)
				(pin passive line
					(at -5.08 -10.16 0)
					(length 3.81)
					(name "Pin_8")
					(number "8")
				)
			)
		)
		(symbol "Connector_Generic:Conn_01x10"
			(pin_names
				(offset 1.016) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at 0 12.7 0)
			)
			(property "Value" "Conn_01x10"
				(at 0 -15.24 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Generic connector, single row, 01x10, script generated (kicad-library-utils/schlib/autogen/connector/)"
				(at 0 0 0)
			)
			(property "ki_keywords" "connector"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Connector*:*_1x??_*"
				(at 0 0 0)
			)
			(symbol "Conn_01x10_1_1"
				(rectangle
					(start -1.27 -12.573)
					(end 0 -12.827)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 -10.033)
					(end 0 -10.287)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 -7.493)
					(end 0 -7.747)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 -4.953)
					(end 0 -5.207)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 -2.413)
					(end 0 -2.667)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 0.127)
					(end 0 -0.127)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 2.667)
					(end 0 2.413)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 5.207)
					(end 0 4.953)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 7.747)
					(end 0 7.493)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 10.287)
					(end 0 10.033)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 11.43)
					(end 1.27 -13.97)
					(fill
						(type background)
					)
				)
				(pin passive line
					(at -5.08 10.16 0)
					(length 3.81)
					(name "Pin_1")
					(number "1")
				)
				(pin passive line
					(at -5.08 -12.7 0)
					(length 3.81)
					(name "Pin_10")
					(number "10")
				)
				(pin passive line
					(at -5.08 7.62 0)
					(length 3.81)
					(name "Pin_2")
					(number "2")
				)
				(pin passive line
					(at -5.08 5.08 0)
					(length 3.81)
					(name "Pin_3")
					(number "3")
				)
				(pin passive line
					(at -5.08 2.54 0)
					(length 3.81)
					(name "Pin_4")
					(number "4")
				)
				(pin passive line
					(at -5.08 0 0)
					(length 3.81)
					(name "Pin_5")
					(number "5")
				)
				(pin passive line
					(at -5.08 -2.54 0)
					(length 3.81)
					(name "Pin_6")
					(number "6")
				)
				(pin passive line
					(at -5.08 -5.08 0)
					(length 3.81)
					(name "Pin_7")
					(number "7")
				)
				(pin passive line
					(at -5.08 -7.62 0)
					(length 3.81)
					(name "Pin_8")
					(number "8")
				)
				(pin passive line
					(at -5.08 -10.16 0)
					(length 3.81)
					(name "Pin_9")
					(number "9")
				)
			)
		)
		(symbol "Connector_Generic:Conn_02x06_Odd_Even"
			(pin_names
				(offset 1.016) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at 1.27 7.62 0)
			)
			(property "Value" "Conn_02x06_Odd_Even"
				(at 1.27 -10.16 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Generic connector, double row, 02x06, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
				(at 0 0 0)
			)
			(property "ki_keywords" "connector"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Connector*:*_2x??_*"
				(at 0 0 0)
			)
			(symbol "Conn_02x06_Odd_Even_1_1"
				(rectangle
					(start -1.27 -7.493)
					(end 0 -7.747)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 -4.953)
					(end 0 -5.207)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 -2.413)
					(end 0 -2.667)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 0.127)
					(end 0 -0.127)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 2.667)
					(end 0 2.413)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 5.207)
					(end 0 4.953)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 6.35)
					(end 3.81 -8.89)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 3.81 -7.493)
					(end 2.54 -7.747)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 3.81 -4.953)
					(end 2.54 -5.207)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 3.81 -2.413)
					(end 2.54 -2.667)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 3.81 0.127)
					(end 2.54 -0.127)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 3.81 2.667)
					(end 2.54 2.413)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 3.81 5.207)
					(end 2.54 4.953)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at -5.08 5.08 0)
					(length 3.81)
					(name "Pin_1")
					(number "1")
				)
				(pin passive line
					(at 7.62 -5.08 180)
					(length 3.81)
					(name "Pin_10")
					(number "10")
				)
				(pin passive line
					(at -5.08 -7.62 0)
					(length 3.81)
					(name "Pin_11")
					(number "11")
				)
				(pin passive line
					(at 7.62 -7.62 180)
					(length 3.81)
					(name "Pin_12")
					(number "12")
				)
				(pin passive line
					(at 7.62 5.08 180)
					(length 3.81)
					(name "Pin_2")
					(number "2")
				)
				(pin passive line
					(at -5.08 2.54 0)
					(length 3.81)
					(name "Pin_3")
					(number "3")
				)
				(pin passive line
					(at 7.62 2.54 180)
					(length 3.81)
					(name "Pin_4")
					(number "4")
				)
				(pin passive line
					(at -5.08 0 0)
					(length 3.81)
					(name "Pin_5")
					(number "5")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 3.81)
					(name "Pin_6")
					(number "6")
				)
				(pin passive line
					(at -5.08 -2.54 0)
					(length 3.81)
					(name "Pin_7")
					(number "7")
				)
				(pin passive line
					(at 7.62 -2.54 180)
					(length 3.81)
					(name "Pin_8")
					(number "8")
				)
				(pin passive line
					(at -5.08 -5.08 0)
					(length 3.81)
					(name "Pin_9")
					(number "9")
				)
			)
		)
		(symbol "Connector_Generic:Conn_02x10_Odd_Even"
			(pin_names
				(offset 1.016) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at 1.27 12.7 0)
			)
			(property "Value" "Conn_02x10_Odd_Even"
				(at 1.27 -15.24 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Generic connector, double row, 02x10, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
				(at 0 0 0)
			)
			(property "ki_keywords" "connector"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Connector*:*_2x??_*"
				(at 0 0 0)
			)
			(symbol "Conn_02x10_Odd_Even_1_1"
				(rectangle
					(start -1.27 -12.573)
					(end 0 -12.827)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 -10.033)
					(end 0 -10.287)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 -7.493)
					(end 0 -7.747)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 -4.953)
					(end 0 -5.207)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 -2.413)
					(end 0 -2.667)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 0.127)
					(end 0 -0.127)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 2.667)
					(end 0 2.413)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 5.207)
					(end 0 4.953)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 7.747)
					(end 0 7.493)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 10.287)
					(end 0 10.033)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 11.43)
					(end 3.81 -13.97)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 3.81 -12.573)
					(end 2.54 -12.827)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 3.81 -10.033)
					(end 2.54 -10.287)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 3.81 -7.493)
					(end 2.54 -7.747)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 3.81 -4.953)
					(end 2.54 -5.207)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 3.81 -2.413)
					(end 2.54 -2.667)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 3.81 0.127)
					(end 2.54 -0.127)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 3.81 2.667)
					(end 2.54 2.413)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 3.81 5.207)
					(end 2.54 4.953)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 3.81 7.747)
					(end 2.54 7.493)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 3.81 10.287)
					(end 2.54 10.033)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at -5.08 10.16 0)
					(length 3.81)
					(name "Pin_1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 3.81)
					(name "Pin_10")
					(number "10")
				)
				(pin passive line
					(at -5.08 -2.54 0)
					(length 3.81)
					(name "Pin_11")
					(number "11")
				)
				(pin passive line
					(at 7.62 -2.54 180)
					(length 3.81)
					(name "Pin_12")
					(number "12")
				)
				(pin passive line
					(at -5.08 -5.08 0)
					(length 3.81)
					(name "Pin_13")
					(number "13")
				)
				(pin passive line
					(at 7.62 -5.08 180)
					(length 3.81)
					(name "Pin_14")
					(number "14")
				)
				(pin passive line
					(at -5.08 -7.62 0)
					(length 3.81)
					(name "Pin_15")
					(number "15")
				)
				(pin passive line
					(at 7.62 -7.62 180)
					(length 3.81)
					(name "Pin_16")
					(number "16")
				)
				(pin passive line
					(at -5.08 -10.16 0)
					(length 3.81)
					(name "Pin_17")
					(number "17")
				)
				(pin passive line
					(at 7.62 -10.16 180)
					(length 3.81)
					(name "Pin_18")
					(number "18")
				)
				(pin passive line
					(at -5.08 -12.7 0)
					(length 3.81)
					(name "Pin_19")
					(number "19")
				)
				(pin passive line
					(at 7.62 10.16 180)
					(length 3.81)
					(name "Pin_2")
					(number "2")
				)
				(pin passive line
					(at 7.62 -12.7 180)
					(length 3.81)
					(name "Pin_20")
					(number "20")
				)
				(pin passive line
					(at -5.08 7.62 0)
					(length 3.81)
					(name "Pin_3")
					(number "3")
				)
				(pin passive line
					(at 7.62 7.62 180)
					(length 3.81)
					(name "Pin_4")
					(number "4")
				)
				(pin passive line
					(at -5.08 5.08 0)
					(length 3.81)
					(name "Pin_5")
					(number "5")
				)
				(pin passive line
					(at 7.62 5.08 180)
					(length 3.81)
					(name "Pin_6")
					(number "6")
				)
				(pin passive line
					(at -5.08 2.54 0)
					(length 3.81)
					(name "Pin_7")
					(number "7")
				)
				(pin passive line
					(at 7.62 2.54 180)
					(length 3.81)
					(name "Pin_8")
					(number "8")
				)
				(pin passive line
					(at -5.08 0 0)
					(length 3.81)
					(name "Pin_9")
					(number "9")
				)
			)
		)
		(symbol "Device:C_Small"
			(pin_numbers hide)
			(pin_names
				(offset 0.254) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 0.254 1.778 0)
			)
			(property "Value" "C_Small"
				(at 0.254 -2.032 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Unpolarized capacitor, small symbol"
				(at 0 0 0)
			)
			(property "ki_keywords" "capacitor cap"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "C_*"
				(at 0 0 0)
			)
			(symbol "C_Small_0_1"
				(polyline
					(pts
						(xy -1.524 -0.508) (xy 1.524 -0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.524 0.508) (xy 1.524 0.508)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "C_Small_1_1"
				(pin passive line
					(at 0 2.54 270)
					(length 2.032)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -2.54 90)
					(length 2.032)
					(name "~")
					(number "2")
				)
			)
		)
		(symbol "Device:R_Small"
			(pin_numbers hide)
			(pin_names
				(offset 0.254) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 0.762 0.508 0)
			)
			(property "Value" "R_Small"
				(at 0.762 -1.016 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Resistor, small symbol"
				(at 0 0 0)
			)
			(property "ki_keywords" "R resistor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "R_*"
				(at 0 0 0)
			)
			(symbol "R_Small_0_1"
				(rectangle
					(start -0.762 1.778)
					(end 0.762 -1.778)
					(fill
						(type none)
					)
				)
			)
			(symbol "R_Small_1_1"
				(pin passive line
					(at 0 2.54 270)
					(length 0.762)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -2.54 90)
					(length 0.762)
					(name "~")
					(number "2")
				)
			)
		)
		(symbol "Interface_CAN_LIN:MCP2562-H-SN"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at -10.16 8.89 0)
			)
			(property "Value" "MCP2562-H-SN"
				(at 2.54 8.89 0)
			)
			(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
				(at 0 -12.7 0)
			)
			(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/25167A.pdf"
				(at 0 0 0)
			)
			(property "Description" "High-Speed CAN Transceiver, 1Mbps, 5V supply, Vio pin, -40C to +150C, SOIC-8"
				(at 0 0 0)
			)
			(property "ki_keywords" "High-Speed CAN Transceiver"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
				(at 0 0 0)
			)
			(symbol "MCP2562-H-SN_0_1"
				(rectangle
					(start -10.16 7.62)
					(end 10.16 -7.62)
					(fill
						(type background)
					)
				)
			)
			(symbol "MCP2562-H-SN_1_1"
				(pin input line
					(at -12.7 5.08 0)
					(length 2.54)
					(name "TXD")
					(number "1")
				)
				(pin power_in line
					(at 0 -10.16 90)
					(length 2.54)
					(name "VSS")
					(number "2")
				)
				(pin power_in line
					(at 0 10.16 270)
					(length 2.54)
					(name "VDD")
					(number "3")
				)
				(pin output line
					(at -12.7 2.54 0)
					(length 2.54)
					(name "RXD")
					(number "4")
				)
				(pin power_in line
					(at -12.7 -2.54 0)
					(length 2.54)
					(name "Vio")
					(number "5")
				)
				(pin bidirectional line
					(at 12.7 -2.54 180)
					(length 2.54)
					(name "CANL")
					(number "6")
				)
				(pin bidirectional line
					(at 12.7 2.54 180)
					(length 2.54)
					(name "CANH")
					(number "7")
				)
				(pin input line
					(at -12.7 -5.08 0)
					(length 2.54)
					(name "STBY")
					(number "8")
				)
			)
		)
		(symbol "Jumper:SolderJumper_2_Open"
			(pin_numbers hide)
			(pin_names
				(offset 0) hide)
			(exclude_from_sim yes)
			(in_bom no)
			(on_board yes)
			(property "Reference" "JP"
				(at 0 2.032 0)
			)
			(property "Value" "SolderJumper_2_Open"
				(at 0 -2.54 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Solder Jumper, 2-pole, open"
				(at 0 0 0)
			)
			(property "ki_keywords" "solder jumper SPST"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "SolderJumper*Open*"
				(at 0 0 0)
			)
			(symbol "SolderJumper_2_Open_0_1"
				(arc
					(start -0.254 1.016)
					(mid -1.2656 0)
					(end -0.254 -1.016)
					(fill
						(type none)
					)
				)
				(arc
					(start -0.254 1.016)
					(mid -1.2656 0)
					(end -0.254 -1.016)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy -0.254 1.016) (xy -0.254 -1.016)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.254 1.016) (xy 0.254 -1.016)
					)
					(fill
						(type none)
					)
				)
				(arc
					(start 0.254 -1.016)
					(mid 1.2656 0)
					(end 0.254 1.016)
					(fill
						(type none)
					)
				)
				(arc
					(start 0.254 -1.016)
					(mid 1.2656 0)
					(end 0.254 1.016)
					(fill
						(type outline)
					)
				)
			)
			(symbol "SolderJumper_2_Open_1_1"
				(pin passive line
					(at -3.81 0 0)
					(length 2.54)
					(name "A")
					(number "1")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 2.54)
					(name "B")
					(number "2")
				)
			)
		)
		(symbol "Würth_WE-CNSW:WE-CNSW_1812_744235510"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "L"
				(at 0 3.81 0)
			)
			(property "Value" ""
				(at -5.08 -5.08 0)
			)
			(property "Footprint" "Eagle_WE-CNSW (rev19a):WE-CNSW_1812_744235510"
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" " WE-CNSW SMD Common Mode Line Filter\n\nCharacteristics\n\nCurrent compensated data line filter\nHigh common mode noise suppression at high frequencies\nSmall influence on high speed signals through winding symmetry\nClimatic category 40/105/21 (Size 0603)\nClimatic category 40/125/21 (Size 0805/1206/1812)\nFlammability corresponding to UL 94 V-0\n\nApplications\n\nUSB 2.0\nIEEE 1394 (Firewire)\nLVDS\nHigh Speed Data Lines\nLAN\n\nhttps://katalog.we-online.com/media/images/v2/o14771v209%20we-cnsw_stroko_smd_gruppe.jpg\n\nDetails see: http://katalog.we-online.de/en/pbs/WE-CNSW http://katalog.we-online.de/en/pbs/WE-CNSW\n\nUpdated by  Ella Wu 2019-01-09\n2019 (C) Wurth Elektronik"
				(at 0 0 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "WE-CNSW_1812_744235510_1_0"
				(circle
					(center -5.3 -0.6)
					(radius 0.1)
					(fill
						(type none)
					)
				)
				(circle
					(center -5.3 0.7)
					(radius 0.1)
					(fill
						(type none)
					)
				)
				(arc
					(start -5.08 2.54)
					(mid -3.81 1.27)
					(end -2.54 2.54)
					(fill
						(type none)
					)
				)
				(arc
					(start -2.54 -2.54)
					(mid -3.81 -1.27)
					(end -5.08 -2.54)
					(fill
						(type none)
					)
				)
				(arc
					(start -2.54 2.54)
					(mid -1.27 1.27)
					(end 0 2.54)
					(fill
						(type none)
					)
				)
				(arc
					(start 0 -2.54)
					(mid -1.27 -1.27)
					(end -2.54 -2.54)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -4.445 -0.635) (xy 4.445 -0.635)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -4.445 0.635) (xy 4.445 0.635)
					)
					(fill
						(type none)
					)
				)
				(arc
					(start 0 2.54)
					(mid 1.27 1.27)
					(end 2.54 2.54)
					(fill
						(type none)
					)
				)
				(arc
					(start 2.54 -2.54)
					(mid 1.27 -1.27)
					(end 0 -2.54)
					(fill
						(type none)
					)
				)
				(arc
					(start 2.54 2.54)
					(mid 3.81 1.27)
					(end 5.08 2.54)
					(fill
						(type none)
					)
				)
				(arc
					(start 5.08 -2.54)
					(mid 3.81 -1.27)
					(end 2.54 -2.54)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at -7.62 -2.54 0)
					(length 2.54)
					(name "4")
					(number "1")
				)
				(pin passive line
					(at 7.62 -2.54 180)
					(length 2.54)
					(name "3")
					(number "2")
				)
				(pin passive line
					(at 7.62 2.54 180)
					(length 2.54)
					(name "2")
					(number "3")
				)
				(pin passive line
					(at -7.62 2.54 0)
					(length 2.54)
					(name "1")
					(number "4")
				)
			)
		)
		(symbol "power:+3.3V"
			(power)
			(pin_numbers hide)
			(pin_names
				(offset 0) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -3.81 0)
			)
			(property "Value" "+3.3V"
				(at 0 3.556 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"+3.3V\""
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "+3.3V_0_1"
				(polyline
					(pts
						(xy -0.762 1.27) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 2.54) (xy 0.762 1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "+3.3V_1_1"
				(pin power_in line
					(at 0 0 90)
					(length 0)
					(name "~")
					(number "1")
				)
			)
		)
		(symbol "power:+5V"
			(power)
			(pin_numbers hide)
			(pin_names
				(offset 0) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -3.81 0)
			)
			(property "Value" "+5V"
				(at 0 3.556 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"+5V\""
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "+5V_0_1"
				(polyline
					(pts
						(xy -0.762 1.27) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 2.54) (xy 0.762 1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "+5V_1_1"
				(pin power_in line
					(at 0 0 90)
					(length 0)
					(name "~")
					(number "1")
				)
			)
		)
		(symbol "power:GND"
			(power)
			(pin_numbers hide)
			(pin_names
				(offset 0) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "GND"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "GND_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GND_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(name "~")
					(number "1")
				)
			)
		)
	)
	(junction
		(at 167.64 54.61)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 43.18 66.04)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 76.2 111.76)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 77.47 147.32)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 240.03 49.53)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 60.96 29.21)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 203.2 33.02)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 240.03 54.61)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 29.21 53.34)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 252.73 111.76)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 58.42 111.76)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 110.49 99.06)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 95.25 53.34)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 95.25 48.26)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 60.96 66.04)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 77.47 134.62)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 203.2 67.31)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 44.45 99.06)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 110.49 93.98)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 185.42 67.31)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 76.2 74.93)
		(diameter 0)
		(color 0 0 0 0)
	)
	(wire
		(pts
			(xy 116.84 173.99) (xy 114.3 173.99)
		)
	)
	(wire
		(pts
			(xy 250.19 53.34) (xy 250.19 52.07)
		)
	)
	(wire
		(pts
			(xy 236.22 49.53) (xy 240.03 49.53)
		)
	)
	(wire
		(pts
			(xy 194.31 113.03) (xy 193.04 113.03)
		)
	)
	(wire
		(pts
			(xy 60.96 60.96) (xy 60.96 66.04)
		)
	)
	(wire
		(pts
			(xy 204.47 110.49) (xy 204.47 111.76)
		)
	)
	(wire
		(pts
			(xy 54.61 168.91) (xy 58.42 168.91)
		)
	)
	(wire
		(pts
			(xy 167.64 67.31) (xy 185.42 67.31)
		)
	)
	(wire
		(pts
			(xy 46.99 48.26) (xy 48.26 48.26)
		)
	)
	(wire
		(pts
			(xy 34.29 137.16) (xy 38.1 137.16)
		)
	)
	(wire
		(pts
			(xy 180.34 110.49) (xy 175.26 110.49)
		)
	)
	(wire
		(pts
			(xy 29.21 59.69) (xy 29.21 66.04)
		)
	)
	(wire
		(pts
			(xy 240.03 62.23) (xy 240.03 54.61)
		)
	)
	(wire
		(pts
			(xy 34.29 144.78) (xy 38.1 144.78)
		)
	)
	(wire
		(pts
			(xy 92.71 53.34) (xy 95.25 53.34)
		)
	)
	(wire
		(pts
			(xy 44.45 111.76) (xy 58.42 111.76)
		)
	)
	(wire
		(pts
			(xy 187.96 49.53) (xy 190.5 49.53)
		)
	)
	(wire
		(pts
			(xy 92.71 48.26) (xy 95.25 48.26)
		)
	)
	(wire
		(pts
			(xy 53.34 29.21) (xy 53.34 30.48)
		)
	)
	(wire
		(pts
			(xy 29.21 54.61) (xy 29.21 53.34)
		)
	)
	(wire
		(pts
			(xy 236.22 54.61) (xy 240.03 54.61)
		)
	)
	(wire
		(pts
			(xy 116.84 184.15) (xy 110.49 184.15)
		)
	)
	(wire
		(pts
			(xy 107.95 60.96) (xy 95.25 60.96)
		)
	)
	(wire
		(pts
			(xy 116.84 171.45) (xy 114.3 171.45)
		)
	)
	(wire
		(pts
			(xy 243.84 109.22) (xy 243.84 111.76)
		)
	)
	(wire
		(pts
			(xy 185.42 67.31) (xy 203.2 67.31)
		)
	)
	(wire
		(pts
			(xy 29.21 53.34) (xy 29.21 50.8)
		)
	)
	(wire
		(pts
			(xy 181.61 139.7) (xy 185.42 139.7)
		)
	)
	(wire
		(pts
			(xy 44.45 100.33) (xy 44.45 99.06)
		)
	)
	(wire
		(pts
			(xy 252.73 111.76) (xy 252.73 114.3)
		)
	)
	(wire
		(pts
			(xy 68.58 81.28) (xy 68.58 82.55)
		)
	)
	(wire
		(pts
			(xy 243.84 111.76) (xy 252.73 111.76)
		)
	)
	(wire
		(pts
			(xy 110.49 106.68) (xy 110.49 99.06)
		)
	)
	(wire
		(pts
			(xy 44.45 99.06) (xy 63.5 99.06)
		)
	)
	(wire
		(pts
			(xy 60.96 66.04) (xy 60.96 71.12)
		)
	)
	(wire
		(pts
			(xy 58.42 111.76) (xy 76.2 111.76)
		)
	)
	(wire
		(pts
			(xy 77.47 139.7) (xy 91.44 139.7)
		)
	)
	(wire
		(pts
			(xy 43.18 55.88) (xy 43.18 66.04)
		)
	)
	(wire
		(pts
			(xy 157.48 93.98) (xy 157.48 92.71)
		)
	)
	(wire
		(pts
			(xy 53.34 35.56) (xy 53.34 36.83)
		)
	)
	(wire
		(pts
			(xy 261.62 109.22) (xy 261.62 111.76)
		)
	)
	(wire
		(pts
			(xy 57.15 186.69) (xy 57.15 184.15)
		)
	)
	(wire
		(pts
			(xy 76.2 74.93) (xy 76.2 86.36)
		)
	)
	(wire
		(pts
			(xy 215.9 54.61) (xy 220.98 54.61)
		)
	)
	(wire
		(pts
			(xy 88.9 93.98) (xy 92.71 93.98)
		)
	)
	(wire
		(pts
			(xy 203.2 33.02) (xy 203.2 41.91)
		)
	)
	(wire
		(pts
			(xy 193.04 92.71) (xy 215.9 92.71)
		)
	)
	(wire
		(pts
			(xy 116.84 166.37) (xy 114.3 166.37)
		)
	)
	(wire
		(pts
			(xy 193.04 110.49) (xy 204.47 110.49)
		)
	)
	(wire
		(pts
			(xy 107.95 93.98) (xy 110.49 93.98)
		)
	)
	(wire
		(pts
			(xy 215.9 92.71) (xy 215.9 93.98)
		)
	)
	(wire
		(pts
			(xy 215.9 49.53) (xy 220.98 49.53)
		)
	)
	(wire
		(pts
			(xy 116.84 168.91) (xy 114.3 168.91)
		)
	)
	(wire
		(pts
			(xy 76.2 111.76) (xy 76.2 114.3)
		)
	)
	(wire
		(pts
			(xy 167.64 55.88) (xy 167.64 54.61)
		)
	)
	(wire
		(pts
			(xy 138.43 134.62) (xy 143.51 134.62)
		)
	)
	(wire
		(pts
			(xy 116.84 176.53) (xy 114.3 176.53)
		)
	)
	(wire
		(pts
			(xy 105.41 50.8) (xy 107.95 50.8)
		)
	)
	(wire
		(pts
			(xy 31.75 181.61) (xy 31.75 177.8)
		)
	)
	(wire
		(pts
			(xy 43.18 66.04) (xy 60.96 66.04)
		)
	)
	(wire
		(pts
			(xy 138.43 152.4) (xy 143.51 152.4)
		)
	)
	(wire
		(pts
			(xy 194.31 115.57) (xy 193.04 115.57)
		)
	)
	(wire
		(pts
			(xy 91.44 147.32) (xy 77.47 147.32)
		)
	)
	(wire
		(pts
			(xy 181.61 149.86) (xy 185.42 149.86)
		)
	)
	(wire
		(pts
			(xy 203.2 67.31) (xy 203.2 72.39)
		)
	)
	(wire
		(pts
			(xy 91.44 142.24) (xy 73.66 142.24)
		)
	)
	(wire
		(pts
			(xy 73.66 142.24) (xy 73.66 139.7)
		)
	)
	(wire
		(pts
			(xy 107.95 53.34) (xy 107.95 60.96)
		)
	)
	(wire
		(pts
			(xy 181.61 132.08) (xy 185.42 132.08)
		)
	)
	(wire
		(pts
			(xy 29.21 53.34) (xy 48.26 53.34)
		)
	)
	(wire
		(pts
			(xy 246.38 109.22) (xy 243.84 109.22)
		)
	)
	(wire
		(pts
			(xy 73.66 53.34) (xy 77.47 53.34)
		)
	)
	(wire
		(pts
			(xy 138.43 139.7) (xy 143.51 139.7)
		)
	)
	(wire
		(pts
			(xy 138.43 142.24) (xy 143.51 142.24)
		)
	)
	(wire
		(pts
			(xy 118.11 144.78) (xy 118.11 147.32)
		)
	)
	(wire
		(pts
			(xy 44.45 99.06) (xy 44.45 96.52)
		)
	)
	(wire
		(pts
			(xy 54.61 171.45) (xy 58.42 171.45)
		)
	)
	(wire
		(pts
			(xy 167.64 54.61) (xy 190.5 54.61)
		)
	)
	(wire
		(pts
			(xy 76.2 73.66) (xy 76.2 74.93)
		)
	)
	(wire
		(pts
			(xy 77.47 134.62) (xy 91.44 134.62)
		)
	)
	(wire
		(pts
			(xy 34.29 142.24) (xy 38.1 142.24)
		)
	)
	(wire
		(pts
			(xy 203.2 30.48) (xy 203.2 33.02)
		)
	)
	(wire
		(pts
			(xy 116.84 181.61) (xy 91.44 181.61)
		)
	)
	(wire
		(pts
			(xy 195.58 33.02) (xy 203.2 33.02)
		)
	)
	(wire
		(pts
			(xy 261.62 111.76) (xy 252.73 111.76)
		)
	)
	(wire
		(pts
			(xy 68.58 74.93) (xy 76.2 74.93)
		)
	)
	(wire
		(pts
			(xy 157.48 92.71) (xy 180.34 92.71)
		)
	)
	(wire
		(pts
			(xy 185.42 57.15) (xy 185.42 67.31)
		)
	)
	(wire
		(pts
			(xy 60.96 27.94) (xy 60.96 29.21)
		)
	)
	(wire
		(pts
			(xy 60.96 19.05) (xy 60.96 20.32)
		)
	)
	(wire
		(pts
			(xy 181.61 137.16) (xy 185.42 137.16)
		)
	)
	(wire
		(pts
			(xy 250.19 52.07) (xy 252.73 52.07)
		)
	)
	(wire
		(pts
			(xy 252.73 62.23) (xy 240.03 62.23)
		)
	)
	(wire
		(pts
			(xy 76.2 106.68) (xy 76.2 111.76)
		)
	)
	(wire
		(pts
			(xy 138.43 132.08) (xy 143.51 132.08)
		)
	)
	(wire
		(pts
			(xy 181.61 134.62) (xy 185.42 134.62)
		)
	)
	(wire
		(pts
			(xy 120.65 97.79) (xy 120.65 96.52)
		)
	)
	(wire
		(pts
			(xy 91.44 144.78) (xy 77.47 144.78)
		)
	)
	(wire
		(pts
			(xy 77.47 144.78) (xy 77.47 147.32)
		)
	)
	(wire
		(pts
			(xy 57.15 184.15) (xy 58.42 184.15)
		)
	)
	(wire
		(pts
			(xy 190.5 57.15) (xy 185.42 57.15)
		)
	)
	(wire
		(pts
			(xy 34.29 147.32) (xy 38.1 147.32)
		)
	)
	(wire
		(pts
			(xy 29.21 66.04) (xy 43.18 66.04)
		)
	)
	(wire
		(pts
			(xy 167.64 54.61) (xy 167.64 52.07)
		)
	)
	(wire
		(pts
			(xy 240.03 49.53) (xy 252.73 49.53)
		)
	)
	(wire
		(pts
			(xy 120.65 96.52) (xy 123.19 96.52)
		)
	)
	(wire
		(pts
			(xy 105.41 52.07) (xy 105.41 50.8)
		)
	)
	(wire
		(pts
			(xy 76.2 64.77) (xy 76.2 66.04)
		)
	)
	(wire
		(pts
			(xy 181.61 147.32) (xy 185.42 147.32)
		)
	)
	(wire
		(pts
			(xy 44.45 105.41) (xy 44.45 111.76)
		)
	)
	(wire
		(pts
			(xy 73.66 48.26) (xy 77.47 48.26)
		)
	)
	(wire
		(pts
			(xy 203.2 21.59) (xy 203.2 22.86)
		)
	)
	(wire
		(pts
			(xy 91.44 181.61) (xy 91.44 179.07)
		)
	)
	(wire
		(pts
			(xy 68.58 74.93) (xy 68.58 76.2)
		)
	)
	(wire
		(pts
			(xy 60.96 29.21) (xy 60.96 40.64)
		)
	)
	(wire
		(pts
			(xy 123.19 106.68) (xy 110.49 106.68)
		)
	)
	(wire
		(pts
			(xy 167.64 60.96) (xy 167.64 67.31)
		)
	)
	(wire
		(pts
			(xy 107.95 99.06) (xy 110.49 99.06)
		)
	)
	(wire
		(pts
			(xy 77.47 147.32) (xy 77.47 148.59)
		)
	)
	(wire
		(pts
			(xy 138.43 137.16) (xy 143.51 137.16)
		)
	)
	(wire
		(pts
			(xy 259.08 109.22) (xy 261.62 109.22)
		)
	)
	(wire
		(pts
			(xy 95.25 60.96) (xy 95.25 53.34)
		)
	)
	(wire
		(pts
			(xy 143.51 144.78) (xy 118.11 144.78)
		)
	)
	(wire
		(pts
			(xy 77.47 134.62) (xy 77.47 139.7)
		)
	)
	(wire
		(pts
			(xy 181.61 144.78) (xy 185.42 144.78)
		)
	)
	(wire
		(pts
			(xy 54.61 176.53) (xy 58.42 176.53)
		)
	)
	(wire
		(pts
			(xy 46.99 45.72) (xy 48.26 45.72)
		)
	)
	(wire
		(pts
			(xy 54.61 173.99) (xy 58.42 173.99)
		)
	)
	(wire
		(pts
			(xy 123.19 99.06) (xy 123.19 106.68)
		)
	)
	(wire
		(pts
			(xy 53.34 29.21) (xy 60.96 29.21)
		)
	)
	(wire
		(pts
			(xy 54.61 179.07) (xy 58.42 179.07)
		)
	)
	(wire
		(pts
			(xy 116.84 179.07) (xy 114.3 179.07)
		)
	)
	(wire
		(pts
			(xy 181.61 142.24) (xy 185.42 142.24)
		)
	)
	(wire
		(pts
			(xy 54.61 166.37) (xy 58.42 166.37)
		)
	)
	(wire
		(pts
			(xy 58.42 101.6) (xy 58.42 111.76)
		)
	)
	(wire
		(pts
			(xy 110.49 93.98) (xy 123.19 93.98)
		)
	)
	(wire
		(pts
			(xy 63.5 101.6) (xy 58.42 101.6)
		)
	)
	(wire
		(pts
			(xy 138.43 149.86) (xy 143.51 149.86)
		)
	)
	(wire
		(pts
			(xy 110.49 184.15) (xy 110.49 187.96)
		)
	)
	(wire
		(pts
			(xy 88.9 99.06) (xy 92.71 99.06)
		)
	)
	(wire
		(pts
			(xy 187.96 46.99) (xy 190.5 46.99)
		)
	)
	(wire
		(pts
			(xy 175.26 110.49) (xy 175.26 111.76)
		)
	)
	(wire
		(pts
			(xy 95.25 48.26) (xy 107.95 48.26)
		)
	)
	(wire
		(pts
			(xy 203.2 62.23) (xy 203.2 67.31)
		)
	)
	(wire
		(pts
			(xy 34.29 139.7) (xy 38.1 139.7)
		)
	)
	(wire
		(pts
			(xy 252.73 54.61) (xy 252.73 62.23)
		)
	)
	(wire
		(pts
			(xy 138.43 147.32) (xy 143.51 147.32)
		)
	)
	(wire
		(pts
			(xy 34.29 134.62) (xy 38.1 134.62)
		)
	)
	(wire
		(pts
			(xy 58.42 181.61) (xy 31.75 181.61)
		)
	)
	(wire
		(pts
			(xy 48.26 55.88) (xy 43.18 55.88)
		)
	)
	(wire
		(pts
			(xy 77.47 133.35) (xy 77.47 134.62)
		)
	)
	(wire
		(pts
			(xy 138.43 129.54) (xy 143.51 129.54)
		)
	)
	(rectangle
		(start 16.51 123.19)
		(end 208.28 157.48)
		(fill
			(type none)
		)
	)
	(rectangle
		(start 27.94 162.56)
		(end 149.86 194.31)
		(fill
			(type none)
		)
	)
	(rectangle
		(start 152.4 82.55)
		(end 279.4 121.92)
		(fill
			(type none)
		)
	)
	(global_label "PIN_PA31_G2_res"
		(shape input)
		(at 246.38 106.68 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 227.1267 106.68 0)
		)
	)
	(global_label "PIN_PC15_G12_res"
		(shape input)
		(at 114.3 176.53 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 93.6558 176.53 0)
		)
	)
	(global_label "PIN_PE11_M6_res"
		(shape input)
		(at 193.04 100.33 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 212.5351 100.33 0)
		)
	)
	(global_label "PIN_PA8_K2_res"
		(shape input)
		(at 54.61 168.91 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 36.5662 168.91 0)
		)
	)
	(global_label "PIN_PC3_R17_res"
		(shape input)
		(at 180.34 107.95 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 160.9053 107.95 0)
		)
	)
	(global_label "PIN_PG9_K12"
		(shape input)
		(at 181.61 149.86 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 166.0458 149.86 0)
		)
	)
	(global_label "PIN_PA17_V3"
		(shape input)
		(at 34.29 137.16 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 19.0886 137.16 0)
		)
	)
	(global_label "PIN_PD25_D5"
		(shape input)
		(at 138.43 142.24 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 122.8658 142.24 0)
		)
	)
	(global_label "PIN_PC5_N15"
		(shape input)
		(at 46.99 45.72 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 31.3653 45.72 0)
		)
	)
	(global_label "PIN_PC12_F18_res"
		(shape input)
		(at 180.34 102.87 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 159.8772 102.87 0)
		)
	)
	(global_label "PIN_PC25_K17"
		(shape input)
		(at 187.96 49.53 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 171.1863 49.53 0)
		)
	)
	(global_label "PIN_PC2_T18_res"
		(shape input)
		(at 180.34 105.41 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 161.2077 105.41 0)
		)
	)
	(global_label "PIN_PC7_N18"
		(shape input)
		(at 63.5 91.44 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 47.8753 91.44 0)
		)
	)
	(global_label "PIN_PC21_P17_res"
		(shape input)
		(at 54.61 173.99 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 33.9658 173.99 0)
		)
	)
	(global_label "+3.3V"
		(shape output)
		(at 194.31 113.03 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 202.98 113.03 0)
		)
	)
	(global_label "PIN_PA23_G1"
		(shape input)
		(at 181.61 144.78 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 166.2272 144.78 0)
		)
	)
	(global_label "PIN_PG7_L12"
		(shape input)
		(at 181.61 142.24 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 166.2877 142.24 0)
		)
	)
	(global_label "PIN_PC14_E17_res"
		(shape input)
		(at 114.3 171.45 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 93.7768 171.45 0)
		)
	)
	(global_label "PIN_PA15_U1"
		(shape input)
		(at 34.29 142.24 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 18.8467 142.24 0)
		)
	)
	(global_label "PIN_PC11_H15"
		(shape input)
		(at 193.04 95.25 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 209.8742 95.25 0)
		)
	)
	(global_label "PIN_PG5_J17"
		(shape input)
		(at 181.61 139.7 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 166.3482 139.7 0)
		)
	)
	(global_label "+3.3V_res"
		(shape output)
		(at 91.44 179.07 90)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 91.44 166.5295 90)
		)
	)
	(global_label "PIN_AVDD"
		(shape input)
		(at 138.43 147.32 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 126.5547 147.32 0)
		)
	)
	(global_label "PIN_PC21_P17"
		(shape input)
		(at 181.61 134.62 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 164.8363 134.62 0)
		)
	)
	(global_label "PIN_PE1_H2_res"
		(shape input)
		(at 246.38 99.06 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 228.2153 99.06 0)
		)
	)
	(global_label "PIN_PC26_K18"
		(shape input)
		(at 138.43 152.4 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 121.6563 152.4 0)
		)
	)
	(global_label "PIN_PC12_F18_res"
		(shape input)
		(at 114.3 179.07 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 93.8372 179.07 0)
		)
	)
	(global_label "PIN_PC8_M13"
		(shape input)
		(at 180.34 97.79 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 164.5944 97.79 0)
		)
	)
	(global_label "PIN_PA22_G4_res"
		(shape input)
		(at 54.61 166.37 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 35.3567 166.37 0)
		)
	)
	(global_label "PIN_PC25_K17_res"
		(shape input)
		(at 54.61 179.07 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 33.9658 179.07 0)
		)
	)
	(global_label "PIN_PA14_R2_res"
		(shape input)
		(at 114.3 166.37 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 95.0467 166.37 0)
		)
	)
	(global_label "PIN_PC13_F17_res"
		(shape input)
		(at 180.34 100.33 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 159.8772 100.33 0)
		)
	)
	(global_label "PIN_PB11_14"
		(shape input)
		(at 138.43 132.08 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 122.9263 132.08 0)
		)
	)
	(global_label "PIN_PC22_P18"
		(shape input)
		(at 181.61 132.08 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 164.8363 132.08 0)
		)
	)
	(global_label "PIN_PA29_T2"
		(shape input)
		(at 34.29 144.78 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 19.2096 144.78 0)
		)
	)
	(global_label "PIN_PD26_B9"
		(shape input)
		(at 138.43 134.62 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 122.8658 134.62 0)
		)
	)
	(global_label "PIN_PA28_T1"
		(shape input)
		(at 34.29 147.32 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 19.2096 147.32 0)
		)
	)
	(global_label "PIN_PA22_G4"
		(shape input)
		(at 181.61 147.32 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 166.2272 147.32 0)
		)
	)
	(global_label "PIN_PD27_A8"
		(shape input)
		(at 138.43 139.7 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 123.0472 139.7 0)
		)
	)
	(global_label "PIN_PG10_G13"
		(shape input)
		(at 138.43 129.54 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 121.6563 129.54 0)
		)
	)
	(global_label "PIN_PC26_K18"
		(shape input)
		(at 187.96 46.99 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 171.1863 46.99 0)
		)
	)
	(global_label "PIN_PC1_T17"
		(shape input)
		(at 193.04 105.41 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 208.3018 105.41 0)
		)
	)
	(global_label "PIN_PB27_V10_res"
		(shape input)
		(at 114.3 168.91 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 93.8372 168.91 0)
		)
	)
	(global_label "PIN_PC13_F17_res"
		(shape input)
		(at 114.3 173.99 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 93.8372 173.99 0)
		)
	)
	(global_label "+5V_res"
		(shape output)
		(at 73.66 139.7 90)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 73.66 128.9738 90)
		)
	)
	(global_label "PIN_PC9_M18"
		(shape input)
		(at 180.34 95.25 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 164.5944 95.25 0)
		)
	)
	(global_label "PIN_PA18_U3_res"
		(shape input)
		(at 259.08 99.06 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 278.3938 99.06 0)
		)
	)
	(global_label "PIN_PC6_N17"
		(shape input)
		(at 63.5 93.98 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 47.8753 93.98 0)
		)
	)
	(global_label "PIN_PD24_D11"
		(shape input)
		(at 138.43 137.16 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 121.6563 137.16 0)
		)
	)
	(global_label "+3.3V"
		(shape output)
		(at 77.47 133.35 90)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 77.47 124.68 90)
		)
	)
	(global_label "PIN_PC25_K17"
		(shape input)
		(at 138.43 149.86 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 121.6563 149.86 0)
		)
	)
	(global_label "PIN_PA16_U2"
		(shape input)
		(at 34.29 139.7 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 18.8467 139.7 0)
		)
	)
	(global_label "PIN_PC4_R18"
		(shape input)
		(at 46.99 48.26 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 31.4258 48.26 0)
		)
	)
	(global_label "PIN_PC4_R18"
		(shape input)
		(at 193.04 107.95 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 208.6042 107.95 0)
		)
	)
	(global_label "PIN_PA18_U3"
		(shape input)
		(at 34.29 134.62 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 18.8467 134.62 0)
		)
	)
	(global_label "PIN_PC22_P18_res"
		(shape input)
		(at 54.61 171.45 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 33.9658 171.45 0)
		)
	)
	(global_label "PIN_PC26_K18_res"
		(shape input)
		(at 54.61 176.53 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 33.9658 176.53 0)
		)
	)
	(global_label "PIN_PE2_J1_res"
		(shape input)
		(at 246.38 101.6 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 228.5782 101.6 0)
		)
	)
	(global_label "+5V"
		(shape output)
		(at 31.75 177.8 90)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 31.75 172.0556 90)
		)
	)
	(global_label "PIN_PG6_L15"
		(shape input)
		(at 181.61 137.16 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 166.2877 137.16 0)
		)
	)
	(global_label "PIN_PC10_H17"
		(shape input)
		(at 193.04 97.79 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 209.8742 97.79 0)
		)
	)
	(global_label "PIN_PE0_H1_res"
		(shape input)
		(at 246.38 104.14 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 228.2153 104.14 0)
		)
	)
	(global_label "+5V_res"
		(shape output)
		(at 194.31 115.57 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 205.0362 115.57 0)
		)
	)
	(symbol
		(lib_id "Connector_Generic:Conn_02x10_Odd_Even")
		(at 185.42 102.87 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "CONN_X32_links1"
			(at 186.69 86.36 0)
		)
		(property "Value" "Conn_02x10_Odd_Even"
			(at 186.69 88.9 0)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_2x10_P2.54mm_Vertical"
			(at 185.42 102.87 0)
		)
		(property "Datasheet" "~"
			(at 185.42 102.87 0)
		)
		(property "Description" "Generic connector, double row, 02x10, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 185.42 102.87 0)
		)
		(pin "13")
		(pin "14")
		(pin "1")
		(pin "11")
		(pin "10")
		(pin "12")
		(pin "15")
		(pin "9")
		(pin "20")
		(pin "5")
		(pin "4")
		(pin "16")
		(pin "3")
		(pin "7")
		(pin "18")
		(pin "6")
		(pin "17")
		(pin "8")
		(pin "19")
		(pin "2")
		(instances
			(project ""
				(path
					(reference "CONN_X32_links1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C_Small")
		(at 195.58 35.56 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C4"
			(at 198.12 34.2962 0)
		)
		(property "Value" "100n_25V_X7R"
			(at 198.12 36.8362 0)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder"
			(at 195.58 35.56 0)
		)
		(property "Datasheet" "~"
			(at 195.58 35.56 0)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 195.58 35.56 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Adapter_CANBridge"
				(path
					(reference "C4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector_Generic:Conn_01x03")
		(at 128.27 96.52 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "CONN_CAN1"
			(at 130.81 95.2499 0)
		)
		(property "Value" "Conn_01x03"
			(at 130.81 97.7899 0)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Horizontal"
			(at 128.27 96.52 0)
		)
		(property "Datasheet" "~"
			(at 128.27 96.52 0)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 128.27 96.52 0)
		)
		(pin "2")
		(pin "3")
		(pin "1")
		(instances
			(project "Adapter_CANBridge"
				(path
					(reference "CONN_CAN1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 195.58 38.1 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR014"
			(at 195.58 44.45 0)
		)
		(property "Value" "GND"
			(at 195.58 43.18 0)
		)
		(property "Footprint" ""
			(at 195.58 38.1 0)
		)
		(property "Datasheet" ""
			(at 195.58 38.1 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 195.58 38.1 0)
		)
		(pin "1")
		(instances
			(project "Adapter_CANBridge"
				(path
					(reference "#PWR014")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector_Generic:Conn_01x08")
		(at 63.5 173.99 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "CONN_mikroBUS_links1"
			(at 66.04 173.9899 0)
		)
		(property "Value" "Conn_01x08"
			(at 66.04 176.5299 0)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical"
			(at 63.5 173.99 0)
		)
		(property "Datasheet" "~"
			(at 63.5 173.99 0)
		)
		(property "Description" "Generic connector, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 63.5 173.99 0)
		)
		(pin "5")
		(pin "2")
		(pin "1")
		(pin "6")
		(pin "4")
		(pin "3")
		(pin "7")
		(pin "8")
		(instances
			(project ""
				(path
					(reference "CONN_mikroBUS_links1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Interface_CAN_LIN:MCP2562-H-SN")
		(at 203.2 52.07 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U1_CAN2"
			(at 205.3941 39.37 0)
		)
		(property "Value" "MCP2562-H-SN"
			(at 205.3941 41.91 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 203.2 64.77 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/25167A.pdf"
			(at 203.2 52.07 0)
		)
		(property "Description" "High-Speed CAN Transceiver, 1Mbps, 5V supply, Vio pin, -40C to +150C, SOIC-8"
			(at 203.2 52.07 0)
		)
		(pin "8")
		(pin "2")
		(pin "5")
		(pin "3")
		(pin "1")
		(pin "4")
		(pin "6")
		(pin "7")
		(instances
			(project "Adapter_CANBridge"
				(path
					(reference "U1_CAN2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector_Generic:Conn_01x08")
		(at 190.5 139.7 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "CONN_Arduino_Shield_rechts_unten1"
			(at 171.45 128.778 0)
		)
		(property "Value" "Conn_01x08"
			(at 193.548 145.542 90)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical"
			(at 190.5 139.7 0)
		)
		(property "Datasheet" "~"
			(at 190.5 139.7 0)
		)
		(property "Description" "Generic connector, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 190.5 139.7 0)
		)
		(pin "2")
		(pin "5")
		(pin "6")
		(pin "7")
		(pin "4")
		(pin "8")
		(pin "1")
		(pin "3")
		(instances
			(project ""
				(path
					(reference "CONN_Arduino_Shield_rechts_unten1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 252.73 114.3 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR042"
			(at 252.73 120.65 0)
		)
		(property "Value" "GND"
			(at 252.73 119.38 0)
		)
		(property "Footprint" ""
			(at 252.73 114.3 0)
		)
		(property "Datasheet" ""
			(at 252.73 114.3 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 252.73 114.3 0)
		)
		(pin "1")
		(instances
			(project "Adapter_CANBridge"
				(path
					(reference "#PWR042")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 250.19 53.34 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR024"
			(at 250.19 59.69 0)
		)
		(property "Value" "GND"
			(at 250.19 58.42 0)
		)
		(property "Footprint" ""
			(at 250.19 53.34 0)
		)
		(property "Datasheet" ""
			(at 250.19 53.34 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 250.19 53.34 0)
		)
		(pin "1")
		(instances
			(project "Adapter_CANBridge"
				(path
					(reference "#PWR024")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C_Small")
		(at 44.45 102.87 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C6"
			(at 46.99 101.6062 0)
		)
		(property "Value" "100n_25V_X7R"
			(at 46.99 104.1462 0)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder"
			(at 44.45 102.87 0)
		)
		(property "Datasheet" "~"
			(at 44.45 102.87 0)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 44.45 102.87 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Adapter_CANBridge"
				(path
					(reference "C6")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector_Generic:Conn_01x08")
		(at 121.92 173.99 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "CONN_mikroBUS_rechts1"
			(at 124.46 173.9899 0)
		)
		(property "Value" "Conn_01x08"
			(at 124.46 176.5299 0)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical"
			(at 121.92 173.99 0)
		)
		(property "Datasheet" "~"
			(at 121.92 173.99 0)
		)
		(property "Description" "Generic connector, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 121.92 173.99 0)
		)
		(pin "5")
		(pin "2")
		(pin "1")
		(pin "6")
		(pin "4")
		(pin "3")
		(pin "7")
		(pin "8")
		(instances
			(project "Adapter_CANBridge"
				(path
					(reference "CONN_mikroBUS_rechts1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 68.58 82.55 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR026"
			(at 68.58 88.9 0)
		)
		(property "Value" "GND"
			(at 68.58 87.63 0)
		)
		(property "Footprint" ""
			(at 68.58 82.55 0)
		)
		(property "Datasheet" ""
			(at 68.58 82.55 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 68.58 82.55 0)
		)
		(pin "1")
		(instances
			(project "Adapter_CANBridge"
				(path
					(reference "#PWR026")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Jumper:SolderJumper_2_Open")
		(at 76.2 69.85 90)
		(unit 1)
		(exclude_from_sim yes)
		(in_bom no)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "JP5"
			(at 78.74 68.5799 90)
		)
		(property "Value" "SolderJumper_2_Open"
			(at 78.74 71.1199 90)
		)
		(property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
			(at 76.2 69.85 0)
		)
		(property "Datasheet" "~"
			(at 76.2 69.85 0)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 76.2 69.85 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project ""
				(path
					(reference "JP5")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 53.34 36.83 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR08"
			(at 53.34 43.18 0)
		)
		(property "Value" "GND"
			(at 53.34 41.91 0)
		)
		(property "Footprint" ""
			(at 53.34 36.83 0)
		)
		(property "Datasheet" ""
			(at 53.34 36.83 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 53.34 36.83 0)
		)
		(pin "1")
		(instances
			(project "Adapter_CANBridge"
				(path
					(reference "#PWR08")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:+3.3V")
		(at 29.21 50.8 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01"
			(at 29.21 54.61 0)
		)
		(property "Value" "+3.3V"
			(at 29.21 45.72 0)
		)
		(property "Footprint" ""
			(at 29.21 50.8 0)
		)
		(property "Datasheet" ""
			(at 29.21 50.8 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+3.3V\""
			(at 29.21 50.8 0)
		)
		(pin "1")
		(instances
			(project ""
				(path
					(reference "#PWR01")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:+3.3V")
		(at 167.64 52.07 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR013"
			(at 167.64 55.88 0)
		)
		(property "Value" "+3.3V"
			(at 167.64 46.99 0)
		)
		(property "Footprint" ""
			(at 167.64 52.07 0)
		)
		(property "Datasheet" ""
			(at 167.64 52.07 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+3.3V\""
			(at 167.64 52.07 0)
		)
		(pin "1")
		(instances
			(project "Adapter_CANBridge"
				(path
					(reference "#PWR013")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:+5V")
		(at 60.96 19.05 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR03"
			(at 60.96 22.86 0)
		)
		(property "Value" "+5V"
			(at 60.96 13.97 0)
		)
		(property "Footprint" ""
			(at 60.96 19.05 0)
		)
		(property "Datasheet" ""
			(at 60.96 19.05 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+5V\""
			(at 60.96 19.05 0)
		)
		(pin "1")
		(instances
			(project ""
				(path
					(reference "#PWR03")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 157.48 93.98 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR039"
			(at 157.48 100.33 0)
		)
		(property "Value" "GND"
			(at 157.48 99.06 0)
		)
		(property "Footprint" ""
			(at 157.48 93.98 0)
		)
		(property "Datasheet" ""
			(at 157.48 93.98 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 157.48 93.98 0)
		)
		(pin "1")
		(instances
			(project "Adapter_CANBridge"
				(path
					(reference "#PWR039")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C_Small")
		(at 167.64 58.42 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C3"
			(at 170.18 57.1562 0)
		)
		(property "Value" "100n_25V_X7R"
			(at 170.18 59.6962 0)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder"
			(at 167.64 58.42 0)
		)
		(property "Datasheet" "~"
			(at 167.64 58.42 0)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 167.64 58.42 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Adapter_CANBridge"
				(path
					(reference "C3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Würth_WE-CNSW:WE-CNSW_1812_744235510")
		(at 100.33 96.52 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "L3"
			(at 100.17 87.63 0)
		)
		(property "Value" "744235510"
			(at 100.17 91.44 0)
		)
		(property "Footprint" "Würth_WE-CNSW:WE-CNSW_1812_744235510"
			(at 100.33 96.52 0)
		)
		(property "Datasheet" ""
			(at 100.33 96.52 0)
		)
		(property "Description" "WE-CNSW SMD Common Mode Line Filter\n\nCharacteristics\n\nCurrent compensated data line filter\nHigh common mode noise suppression at high frequencies\nSmall influence on high speed signals through winding symmetry\nClimatic category 40/105/21 (Size 0603)\nClimatic category 40/125/21 (Size 0805/1206/1812)\nFlammability corresponding to UL 94 V-0\n\nApplications\n\nUSB 2.0\nIEEE 1394 (Firewire)\nLVDS\nHigh Speed Data Lines\nLAN\n\nhttps://katalog.we-online.com/media/images/v2/o14771v209%20we-cnsw_stroko_smd_gruppe.jpg\n\nDetails see: http://katalog.we-online.de/en/pbs/WE-CNSW http://katalog.we-online.de/en/pbs/WE-CNSW\n\nUpdated by  Ella Wu 2019-01-09\n2019 (C) Wurth Elektronik"
			(at 100.33 96.52 0)
		)
		(pin "2")
		(pin "3")
		(pin "4")
		(pin "1")
		(instances
			(project "Adapter_CANBridge"
				(path
					(reference "L3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 110.49 187.96 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR06"
			(at 110.49 194.31 0)
		)
		(property "Value" "GND"
			(at 110.49 193.04 0)
		)
		(property "Footprint" ""
			(at 110.49 187.96 0)
		)
		(property "Datasheet" ""
			(at 110.49 187.96 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 110.49 187.96 0)
		)
		(pin "1")
		(instances
			(project "Adapter_CANBridge"
				(path
					(reference "#PWR06")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 77.47 148.59 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR011"
			(at 77.47 154.94 0)
		)
		(property "Value" "GND"
			(at 77.47 153.67 0)
		)
		(property "Footprint" ""
			(at 77.47 148.59 0)
		)
		(property "Datasheet" ""
			(at 77.47 148.59 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 77.47 148.59 0)
		)
		(pin "1")
		(instances
			(project "Adapter_CANBridge"
				(path
					(reference "#PWR011")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C_Small")
		(at 68.58 78.74 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C7"
			(at 71.12 77.4762 0)
		)
		(property "Value" "100n_25V_X7R"
			(at 71.12 80.0162 0)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder"
			(at 68.58 78.74 0)
		)
		(property "Datasheet" "~"
			(at 68.58 78.74 0)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 68.58 78.74 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Adapter_CANBridge"
				(path
					(reference "C7")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:+5V")
		(at 76.2 64.77 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR027"
			(at 76.2 68.58 0)
		)
		(property "Value" "+5V"
			(at 76.2 59.69 0)
		)
		(property "Footprint" ""
			(at 76.2 64.77 0)
		)
		(property "Datasheet" ""
			(at 76.2 64.77 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+5V\""
			(at 76.2 64.77 0)
		)
		(pin "1")
		(instances
			(project "Adapter_CANBridge"
				(path
					(reference "#PWR027")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 204.47 111.76 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR041"
			(at 204.47 118.11 0)
		)
		(property "Value" "GND"
			(at 204.47 116.84 0)
		)
		(property "Footprint" ""
			(at 204.47 111.76 0)
		)
		(property "Datasheet" ""
			(at 204.47 111.76 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 204.47 111.76 0)
		)
		(pin "1")
		(instances
			(project "Adapter_CANBridge"
				(path
					(reference "#PWR041")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Würth_WE-CNSW:WE-CNSW_1812_744235510")
		(at 228.6 52.07 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "L2"
			(at 228.44 45.72 0)
		)
		(property "Value" "744235510"
			(at 228.44 48.26 0)
		)
		(property "Footprint" "Würth_WE-CNSW:WE-CNSW_1812_744235510"
			(at 228.6 52.07 0)
		)
		(property "Datasheet" ""
			(at 228.6 52.07 0)
		)
		(property "Description" "WE-CNSW SMD Common Mode Line Filter\n\nCharacteristics\n\nCurrent compensated data line filter\nHigh common mode noise suppression at high frequencies\nSmall influence on high speed signals through winding symmetry\nClimatic category 40/105/21 (Size 0603)\nClimatic category 40/125/21 (Size 0805/1206/1812)\nFlammability corresponding to UL 94 V-0\n\nApplications\n\nUSB 2.0\nIEEE 1394 (Firewire)\nLVDS\nHigh Speed Data Lines\nLAN\n\nhttps://katalog.we-online.com/media/images/v2/o14771v209%20we-cnsw_stroko_smd_gruppe.jpg\n\nDetails see: http://katalog.we-online.de/en/pbs/WE-CNSW http://katalog.we-online.de/en/pbs/WE-CNSW\n\nUpdated by  Ella Wu 2019-01-09\n2019 (C) Wurth Elektronik"
			(at 228.6 52.07 0)
		)
		(pin "1")
		(pin "4")
		(pin "3")
		(pin "2")
		(instances
			(project ""
				(path
					(reference "L2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 60.96 71.12 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR02"
			(at 60.96 77.47 0)
		)
		(property "Value" "GND"
			(at 60.96 76.2 0)
		)
		(property "Footprint" ""
			(at 60.96 71.12 0)
		)
		(property "Datasheet" ""
			(at 60.96 71.12 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 60.96 71.12 0)
		)
		(pin "1")
		(instances
			(project ""
				(path
					(reference "#PWR02")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 118.11 147.32 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR012"
			(at 118.11 153.67 0)
		)
		(property "Value" "GND"
			(at 118.11 152.4 0)
		)
		(property "Footprint" ""
			(at 118.11 147.32 0)
		)
		(property "Datasheet" ""
			(at 118.11 147.32 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 118.11 147.32 0)
		)
		(pin "1")
		(instances
			(project "Adapter_CANBridge"
				(path
					(reference "#PWR012")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector_Generic:Conn_01x10")
		(at 148.59 139.7 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "JCONN_Arduino_Shield_rechts_oben1"
			(at 123.952 155.194 0)
		)
		(property "Value" "Conn_01x10"
			(at 151.638 145.542 90)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x10_P2.54mm_Vertical"
			(at 148.59 139.7 0)
		)
		(property "Datasheet" "~"
			(at 148.59 139.7 0)
		)
		(property "Description" "Generic connector, single row, 01x10, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 148.59 139.7 0)
		)
		(pin "2")
		(pin "4")
		(pin "7")
		(pin "6")
		(pin "3")
		(pin "1")
		(pin "10")
		(pin "8")
		(pin "5")
		(pin "9")
		(instances
			(project ""
				(path
					(reference "JCONN_Arduino_Shield_rechts_oben1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Interface_CAN_LIN:MCP2562-H-SN")
		(at 76.2 96.52 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U1_CAN1"
			(at 78.3941 83.82 0)
		)
		(property "Value" "MCP2562-H-SN"
			(at 78.3941 86.36 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 76.2 109.22 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/25167A.pdf"
			(at 76.2 96.52 0)
		)
		(property "Description" "High-Speed CAN Transceiver, 1Mbps, 5V supply, Vio pin, -40C to +150C, SOIC-8"
			(at 76.2 96.52 0)
		)
		(pin "8")
		(pin "2")
		(pin "5")
		(pin "3")
		(pin "1")
		(pin "4")
		(pin "6")
		(pin "7")
		(instances
			(project "Adapter_CANBridge"
				(path
					(reference "U1_CAN1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R_Small")
		(at 95.25 50.8 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R1"
			(at 97.79 49.5299 0)
		)
		(property "Value" "120R"
			(at 97.79 52.0699 0)
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 95.25 50.8 0)
		)
		(property "Datasheet" "~"
			(at 95.25 50.8 0)
		)
		(property "Description" "Resistor, small symbol"
			(at 95.25 50.8 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Adapter_CANBridge"
				(path
					(reference "R1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:+5V")
		(at 203.2 21.59 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR015"
			(at 203.2 25.4 0)
		)
		(property "Value" "+5V"
			(at 203.2 16.51 0)
		)
		(property "Footprint" ""
			(at 203.2 21.59 0)
		)
		(property "Datasheet" ""
			(at 203.2 21.59 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+5V\""
			(at 203.2 21.59 0)
		)
		(pin "1")
		(instances
			(project "Adapter_CANBridge"
				(path
					(reference "#PWR015")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 215.9 93.98 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR035"
			(at 215.9 100.33 0)
		)
		(property "Value" "GND"
			(at 215.9 99.06 0)
		)
		(property "Footprint" ""
			(at 215.9 93.98 0)
		)
		(property "Datasheet" ""
			(at 215.9 93.98 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 215.9 93.98 0)
		)
		(pin "1")
		(instances
			(project "Adapter_CANBridge"
				(path
					(reference "#PWR035")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 203.2 72.39 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR016"
			(at 203.2 78.74 0)
		)
		(property "Value" "GND"
			(at 203.2 77.47 0)
		)
		(property "Footprint" ""
			(at 203.2 72.39 0)
		)
		(property "Datasheet" ""
			(at 203.2 72.39 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 203.2 72.39 0)
		)
		(pin "1")
		(instances
			(project "Adapter_CANBridge"
				(path
					(reference "#PWR016")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector_Generic:Conn_01x08")
		(at 96.52 139.7 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "CONN_Arduino_Shield_links_oben1"
			(at 85.344 128.524 0)
		)
		(property "Value" "Conn_01x08"
			(at 99.568 145.542 90)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical"
			(at 96.52 139.7 0)
		)
		(property "Datasheet" "~"
			(at 96.52 139.7 0)
		)
		(property "Description" "Generic connector, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 96.52 139.7 0)
		)
		(pin "2")
		(pin "3")
		(pin "7")
		(pin "4")
		(pin "1")
		(pin "5")
		(pin "6")
		(pin "8")
		(instances
			(project ""
				(path
					(reference "CONN_Arduino_Shield_links_oben1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Würth_WE-CNSW:WE-CNSW_1812_744235510")
		(at 85.09 50.8 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "L1"
			(at 84.93 44.45 0)
		)
		(property "Value" "744235510"
			(at 84.93 46.99 0)
		)
		(property "Footprint" "Würth_WE-CNSW:WE-CNSW_1812_744235510"
			(at 85.09 50.8 0)
		)
		(property "Datasheet" ""
			(at 85.09 50.8 0)
		)
		(property "Description" "WE-CNSW SMD Common Mode Line Filter\n\nCharacteristics\n\nCurrent compensated data line filter\nHigh common mode noise suppression at high frequencies\nSmall influence on high speed signals through winding symmetry\nClimatic category 40/105/21 (Size 0603)\nClimatic category 40/125/21 (Size 0805/1206/1812)\nFlammability corresponding to UL 94 V-0\n\nApplications\n\nUSB 2.0\nIEEE 1394 (Firewire)\nLVDS\nHigh Speed Data Lines\nLAN\n\nhttps://katalog.we-online.com/media/images/v2/o14771v209%20we-cnsw_stroko_smd_gruppe.jpg\n\nDetails see: http://katalog.we-online.de/en/pbs/WE-CNSW http://katalog.we-online.de/en/pbs/WE-CNSW\n\nUpdated by  Ella Wu 2019-01-09\n2019 (C) Wurth Elektronik"
			(at 85.09 50.8 0)
		)
		(pin "2")
		(pin "3")
		(pin "4")
		(pin "1")
		(instances
			(project ""
				(path
					(reference "L1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R_Small")
		(at 240.03 52.07 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R2"
			(at 242.57 50.7999 0)
		)
		(property "Value" "120R"
			(at 242.57 53.3399 0)
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 240.03 52.07 0)
		)
		(property "Datasheet" "~"
			(at 240.03 52.07 0)
		)
		(property "Description" "Resistor, small symbol"
			(at 240.03 52.07 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Adapter_CANBridge"
				(path
					(reference "R2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R_Small")
		(at 110.49 96.52 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R3"
			(at 113.03 95.2499 0)
		)
		(property "Value" "120R"
			(at 113.03 97.7899 0)
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 110.49 96.52 0)
		)
		(property "Datasheet" "~"
			(at 110.49 96.52 0)
		)
		(property "Description" "Resistor, small symbol"
			(at 110.49 96.52 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Adapter_CANBridge"
				(path
					(reference "R3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector_Generic:Conn_02x06_Odd_Even")
		(at 251.46 101.6 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "CONN_X32_rechts1"
			(at 252.73 90.17 0)
		)
		(property "Value" "Conn_02x06_Odd_Even"
			(at 252.73 92.71 0)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_2x06_P2.54mm_Vertical"
			(at 251.46 101.6 0)
		)
		(property "Datasheet" "~"
			(at 251.46 101.6 0)
		)
		(property "Description" "Generic connector, double row, 02x06, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 251.46 101.6 0)
		)
		(pin "6")
		(pin "5")
		(pin "10")
		(pin "11")
		(pin "12")
		(pin "7")
		(pin "9")
		(pin "2")
		(pin "8")
		(pin "4")
		(pin "1")
		(pin "3")
		(instances
			(project ""
				(path
					(reference "CONN_X32_rechts1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 76.2 114.3 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR028"
			(at 76.2 120.65 0)
		)
		(property "Value" "GND"
			(at 76.2 119.38 0)
		)
		(property "Footprint" ""
			(at 76.2 114.3 0)
		)
		(property "Datasheet" ""
			(at 76.2 114.3 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 76.2 114.3 0)
		)
		(pin "1")
		(instances
			(project "Adapter_CANBridge"
				(path
					(reference "#PWR028")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 105.41 52.07 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR023"
			(at 105.41 58.42 0)
		)
		(property "Value" "GND"
			(at 105.41 57.15 0)
		)
		(property "Footprint" ""
			(at 105.41 52.07 0)
		)
		(property "Datasheet" ""
			(at 105.41 52.07 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 105.41 52.07 0)
		)
		(pin "1")
		(instances
			(project "Adapter_CANBridge"
				(path
					(reference "#PWR023")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C_Small")
		(at 53.34 33.02 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C2"
			(at 55.88 31.7562 0)
		)
		(property "Value" "100n_25V_X7R"
			(at 55.88 34.2962 0)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder"
			(at 53.34 33.02 0)
		)
		(property "Datasheet" "~"
			(at 53.34 33.02 0)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 53.34 33.02 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project ""
				(path
					(reference "C2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector_Generic:Conn_01x06")
		(at 43.18 139.7 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "CONN_Arduino_Shield_blau1"
			(at 26.162 150.622 0)
		)
		(property "Value" "Conn_01x06"
			(at 45.72 146.05 90)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical"
			(at 43.18 139.7 0)
		)
		(property "Datasheet" "~"
			(at 43.18 139.7 0)
		)
		(property "Description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 43.18 139.7 0)
		)
		(pin "1")
		(pin "3")
		(pin "4")
		(pin "6")
		(pin "5")
		(pin "2")
		(instances
			(project ""
				(path
					(reference "CONN_Arduino_Shield_blau1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 120.65 97.79 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR029"
			(at 120.65 104.14 0)
		)
		(property "Value" "GND"
			(at 120.65 102.87 0)
		)
		(property "Footprint" ""
			(at 120.65 97.79 0)
		)
		(property "Datasheet" ""
			(at 120.65 97.79 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 120.65 97.79 0)
		)
		(pin "1")
		(instances
			(project "Adapter_CANBridge"
				(path
					(reference "#PWR029")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector_Generic:Conn_01x03")
		(at 257.81 52.07 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "CONN_CAN2"
			(at 260.35 50.7999 0)
		)
		(property "Value" "Conn_01x03"
			(at 260.35 53.3399 0)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Horizontal"
			(at 257.81 52.07 0)
		)
		(property "Datasheet" "~"
			(at 257.81 52.07 0)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 257.81 52.07 0)
		)
		(pin "1")
		(pin "3")
		(pin "2")
		(instances
			(project ""
				(path
					(reference "CONN_CAN2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C_Small")
		(at 29.21 57.15 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C1"
			(at 31.75 55.8862 0)
		)
		(property "Value" "100n_25V_X7R"
			(at 31.75 58.4262 0)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder"
			(at 29.21 57.15 0)
		)
		(property "Datasheet" "~"
			(at 29.21 57.15 0)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 29.21 57.15 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project ""
				(path
					(reference "C1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Jumper:SolderJumper_2_Open")
		(at 203.2 26.67 90)
		(unit 1)
		(exclude_from_sim yes)
		(in_bom no)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "JP6"
			(at 205.74 25.3999 90)
		)
		(property "Value" "SolderJumper_2_Open"
			(at 205.74 27.9399 90)
		)
		(property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
			(at 203.2 26.67 0)
		)
		(property "Datasheet" "~"
			(at 203.2 26.67 0)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 203.2 26.67 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project ""
				(path
					(reference "JP6")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 175.26 111.76 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR040"
			(at 175.26 118.11 0)
		)
		(property "Value" "GND"
			(at 175.26 116.84 0)
		)
		(property "Footprint" ""
			(at 175.26 111.76 0)
		)
		(property "Datasheet" ""
			(at 175.26 111.76 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 175.26 111.76 0)
		)
		(pin "1")
		(instances
			(project "Adapter_CANBridge"
				(path
					(reference "#PWR040")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Interface_CAN_LIN:MCP2562-H-SN")
		(at 60.96 50.8 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U1_CAN0"
			(at 63.1541 38.1 0)
		)
		(property "Value" "MCP2562-H-SN"
			(at 63.1541 40.64 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 60.96 63.5 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/25167A.pdf"
			(at 60.96 50.8 0)
		)
		(property "Description" "High-Speed CAN Transceiver, 1Mbps, 5V supply, Vio pin, -40C to +150C, SOIC-8"
			(at 60.96 50.8 0)
		)
		(pin "8")
		(pin "2")
		(pin "5")
		(pin "3")
		(pin "1")
		(pin "4")
		(pin "6")
		(pin "7")
		(instances
			(project ""
				(path
					(reference "U1_CAN0")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 57.15 186.69 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR04"
			(at 57.15 193.04 0)
		)
		(property "Value" "GND"
			(at 57.15 191.77 0)
		)
		(property "Footprint" ""
			(at 57.15 186.69 0)
		)
		(property "Datasheet" ""
			(at 57.15 186.69 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 57.15 186.69 0)
		)
		(pin "1")
		(instances
			(project "Adapter_CANBridge"
				(path
					(reference "#PWR04")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Jumper:SolderJumper_2_Open")
		(at 60.96 24.13 90)
		(unit 1)
		(exclude_from_sim yes)
		(in_bom no)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "JP4"
			(at 63.5 22.8599 90)
		)
		(property "Value" "SolderJumper_2_Open"
			(at 63.5 25.3999 90)
		)
		(property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
			(at 60.96 24.13 0)
		)
		(property "Datasheet" "~"
			(at 60.96 24.13 0)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 60.96 24.13 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project ""
				(path
					(reference "JP4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:+3.3V")
		(at 44.45 96.52 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR025"
			(at 44.45 100.33 0)
		)
		(property "Value" "+3.3V"
			(at 44.45 91.44 0)
		)
		(property "Footprint" ""
			(at 44.45 96.52 0)
		)
		(property "Datasheet" ""
			(at 44.45 96.52 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+3.3V\""
			(at 44.45 96.52 0)
		)
		(pin "1")
		(instances
			(project "Adapter_CANBridge"
				(path
					(reference "#PWR025")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector_Generic:Conn_01x03")
		(at 113.03 50.8 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "CONN_CAN0"
			(at 115.57 49.5299 0)
		)
		(property "Value" "Conn_01x03"
			(at 115.57 52.0699 0)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Horizontal"
			(at 113.03 50.8 0)
		)
		(property "Datasheet" "~"
			(at 113.03 50.8 0)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 113.03 50.8 0)
		)
		(pin "2")
		(pin "3")
		(pin "1")
		(instances
			(project ""
				(path
					(reference "CONN_CAN0")
					(unit 1)
				)
			)
		)
	)
	(sheet
		(at 302.26 27.94)
		(size 34.29 19.05)
		(fields_autoplaced yes)
		(fill
			(color 0 0 0 0.0000)
		)
		(property "Sheetname" "RNBD451_BLE"
			(at 302.26 27.2284 0)
		)
		(property "Sheetfile" "RNBD451_BLE.kicad_sch"
			(at 302.26 47.5746 0)
		)
		(instances
			(project "Adapter_CANBridge"
				(path
					(page "3")
				)
			)
		)
	)
	(sheet
		(at 302.126 0)
		(size 34.424 21.59)
		(fields_autoplaced yes)
		(fill
			(color 0 0 0 0.0000)
		)
		(property "Sheetname" "uBlox_Neo-M9N"
			(at 302.126 -0.7116 0)
		)
		(property "Sheetfile" "untitled.kicad_sch"
			(at 302.126 22.1746 0)
		)
		(instances
			(project "Adapter_CANBridge"
				(path
					(page "2")
				)
			)
		)
	)
	(sheet_instances
		(path
			(page "1")
		)
	)
)
