(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_575555ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "Net-(5V0-Pin_1)")
	(net 2 "Net-(12V0-Pin_2)")
	(net 3 "Net-(12V0-Pin_1)")
	(net 4 "Net-(ADC0-Pin_1)")
	(net 5 "Net-(ADC0-Pin_2)")
	(net 6 "Net-(ADC1-Pin_2)")
	(net 7 "Net-(ADC2-Pin_2)")
	(net 8 "Net-(ADC3-Pin_2)")
	(net 9 "Net-(ADC4_SCA0-Pin_2)")
	(net 10 "Net-(ADC5_SCL0-Pin_2)")
	(net 11 "Net-(ADC6-Pin_2)")
	(net 12 "Net-(ADC7-Pin_2)")
	(net 13 "Net-(BZ1--)")
	(net 14 "Net-(D5-K)")
	(net 15 "Net-(D1-K)")
	(net 16 "Net-(D1-A)")
	(net 17 "Net-(D2-A)")
	(net 18 "Net-(D3-A)")
	(net 19 "Net-(D4-A)")
	(net 20 "Net-(D13-A)")
	(net 21 "Net-(D9-K)")
	(net 22 "Net-(D10-K)")
	(net 23 "Net-(D11-K)")
	(net 24 "Net-(D12-K)")
	(net 25 "Net-(D13-K)")
	(net 26 "Net-(D14-K)")
	(net 27 "Net-(D15-K)")
	(net 28 "Net-(D16-K)")
	(net 29 "Net-(D17-K)")
	(net 30 "Net-(D18-K)")
	(net 31 "Net-(D19-K)")
	(net 32 "Net-(D20-K)")
	(net 33 "Net-(D21-K)")
	(net 34 "Net-(D22-K)")
	(net 35 "Net-(D23-K)")
	(net 36 "Net-(D24-K)")
	(net 37 "Net-(D25-K)")
	(net 38 "Net-(D26-A)")
	(net 39 "Net-(Digital2-Pin_2)")
	(net 40 "Net-(Digital2-Pin_3)")
	(net 41 "Net-(Digital2-Pin_1)")
	(net 42 "Net-(Digital3-Pin_2)")
	(net 43 "Net-(Digital4-Pin_3)")
	(net 44 "Net-(Digital4-Pin_1)")
	(net 45 "Net-(Digital4-Pin_2)")
	(net 46 "Net-(Digital7-Pin_2)")
	(net 47 "Net-(Digital7-Pin_1)")
	(net 48 "Net-(Digital7-Pin_3)")
	(net 49 "Net-(Digital8-Pin_3)")
	(net 50 "Net-(Digital8-Pin_2)")
	(net 51 "Net-(Digital8-Pin_1)")
	(net 52 "Net-(Digital12-Pin_2)")
	(net 53 "Net-(Q1-G)")
	(net 54 "Net-(Q2-G)")
	(net 55 "Net-(Q3-G)")
	(net 56 "Net-(Q4-G)")
	(net 57 "Net-(Q9-G)")
	(net 58 "Net-(TX0-Pin_13)")
	(net 59 "Net-(TX0-Pin_8)")
	(net 60 "Net-(TX0-Pin_9)")
	(net 61 "Net-(TX0-Pin_12)")
	(net 62 "Net-(TX0-Pin_14)")
	(net 63 "Net-(Vin0-Pin_15)")
	(net 64 "Net-(Reset0-Pin_2)")
	(net 65 "Net-(Serial0-Pin_2)")
	(net 66 "Net-(Serial0-Pin_3)")
	(net 67 "unconnected-(TX0-Pin_3-Pad3)")
	(net 68 "unconnected-(Vin0-Pin_1-Pad1)")
	(net 69 "unconnected-(Vin0-Pin_13-Pad13)")
	(net 70 "unconnected-(Vin0-Pin_14-Pad14)")
	(net 71 "Net-(Vin0-Pin_12)")
	(net 72 "Net-(Vin0-Pin_11)")
	(net 73 "Net-(BZ1-+)")
	(footprint "MountingHole:MountingHole_5.3mm_M5_ISO14580"
		(layer "F.Cu")
		(at 22.5 21)
		(descr "Mounting Hole 5.3mm, no annular, M5, ISO14580")
		(tags "mounting hole 5.3mm no annular m5 iso14580")
		(property "Reference" "M5"
			(at -0.148 5.924 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_5.3mm_M5_ISO14580"
			(at 0 5.25 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 5.3 5.3)
			(drill 5.3)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 109.782 62.738 90)
		(descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
		(tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
		(property "Reference" "D24"
			(at 5.48645 0.016886 90)
			(layer "F.SilkS")
		)
		(property "Value" "1N4733"
			(at 5.107892 -2.287937 90)
			(layer "F.SilkS")
		)
		(property "Datasheet" "https://www.vishay.com/docs/85816/1n4728a.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1300mW Silicon planar power Zener diodes, DO-41"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*DO?41*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at 0 -2.1 90)
			(layer "F.SilkS")
		)
		(fp_text user "K"
			(at 0 -2.1 90)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 5.47 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 2.2 2.2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "Net-(D24-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 2.2 2.2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(ADC0-Pin_1)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 68.58 90.932 90)
		(descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
		(tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
		(property "Reference" "D1"
			(at 3.81 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "1N4148"
			(at 3.81 1.905 90)
			(layer "F.SilkS")
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/1N4148_1N4448.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "100V 0.15A standard switching diode, DO-35"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*DO?35*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at 0 -1.8 90)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 4.11 0 90)
			(layer "F.Fab")
		)
		(fp_text user "K"
			(at 0 -1.8 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(D1-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Phoenix_MSTB:PhoenixContact_MSTBVA_2,5_3-G_1x03_P5.00mm_Vertical"
		(layer "F.Cu")
		(at 26.8915 90.09 90)
		(descr "Generic Phoenix Contact connector footprint for: MSTBVA_2,5/3-G; number of pins: 03; pin pitch: 5.00mm; Vertical || order number: 1755529 12A || order number: 1924208 16A (HC)")
		(tags "phoenix_contact connector MSTBVA_01x03_G_5.00mm")
		(property "Reference" "Digital8"
			(at 5 -6 90)
			(layer "F.SilkS")
		)
		(property "Value" "Screw_Terminal_01x03"
			(at 5 5 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5 -4.1 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 2 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.125)
			(net 51 "Net-(Digital8-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 5 0 90)
			(size 2 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "Net-(Digital8-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 10 0 90)
			(size 2 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "Net-(Digital8-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBVA_2,5_3-G_1x03_P5.00mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-92_Inline"
		(layer "F.Cu")
		(at 58.728 56.388)
		(descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
		(tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
		(property "Reference" "Q9"
			(at 1.27 -3.56 0)
			(layer "F.SilkS")
		)
		(property "Value" "2N7000"
			(at 1.27 2.79 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" "https://www.vishay.com/docs/70226/70226.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "0.2A Id, 200V Vds, N-Channel MOSFET, 2.6V Logic Level, TO-92"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO?92*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.05 1.5)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(12V0-Pin_2)")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 1.27 0)
			(size 1.05 1.5)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "Net-(Q9-G)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "3" thru_hole oval
			(at 2.54 0)
			(size 1.05 1.5)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(BZ1--)")
			(pinfunction "D")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Relay_THT:Relay_SPDT_SANYOU_SRD_Series_Form_C"
		(layer "F.Cu")
		(at 52.696 85.09 180)
		(descr "relay Sanyou SRD series Form C http://www.sanyourelay.ca/public/products/pdf/SRD.pdf")
		(tags "relay Sanyu SRD form C")
		(property "Reference" "K1"
			(at 8.1 9.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "SANYOU_SRD_Form_C"
			(at 8 -9.6 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" "http://www.sanyourelay.ca/public/products/pdf/SRD.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Sanyo SRD relay, Single Pole Miniature Power Relay,"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Relay*SPDT*SANYOU*SRD*Series*Form*C*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.1 0.025 0)
			(layer "F.Fab")
		)
		(fp_text user "1"
			(at 0 -2.3 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 3 3)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "Net-(Digital8-Pin_2)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.95 6.05 270)
			(size 2.5 2.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(D1-A)")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 14.15 6.05 270)
			(size 3 3)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "Net-(Digital8-Pin_3)")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 14.2 -6 270)
			(size 3 3)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "Net-(Digital8-Pin_1)")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 1.95 -5.95 270)
			(size 2.5 2.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(D1-K)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Relay_THT.3dshapes/Relay_SPDT_SANYOU_SRD_Series_Form_C.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Phoenix_MSTB:PhoenixContact_MSTBVA_2,5_2-G_1x02_P5.00mm_Vertical"
		(layer "F.Cu")
		(at 63.01 68.1045 180)
		(descr "Generic Phoenix Contact connector footprint for: MSTBVA_2,5/2-G; number of pins: 02; pin pitch: 5.00mm; Vertical || order number: 1755516 12A || order number: 1924198 16A (HC)")
		(tags "phoenix_contact connector MSTBVA_01x02_G_5.00mm")
		(property "Reference" "Reset0"
			(at 2.5 4.6045 180)
			(layer "F.SilkS")
		)
		(property "Value" "Screw_Terminal_01x02"
			(at 2.5 5 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 -4.1 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 180)
			(size 2 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.125)
			(net 4 "Net-(ADC0-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 5 0 180)
			(size 2 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "Net-(Reset0-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBVA_2,5_2-G_1x02_P5.00mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 97.536 146.05 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R9"
			(at 3.81 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "620R"
			(at 3.81 2.54 90)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(12V0-Pin_2)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "Net-(D13-K)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Phoenix_MSTB:PhoenixContact_MSTBVA_2,5_2-G_1x02_P5.00mm_Vertical"
		(layer "F.Cu")
		(at 116 150.355 -90)
		(descr "Generic Phoenix Contact connector footprint for: MSTBVA_2,5/2-G; number of pins: 02; pin pitch: 5.00mm; Vertical || order number: 1755516 12A || order number: 1924198 16A (HC)")
		(tags "phoenix_contact connector MSTBVA_01x02_G_5.00mm")
		(property "Reference" "Digital9"
			(at 4.077 -5.92 270)
			(layer "F.SilkS")
		)
		(property "Value" "Screw_Terminal_01x02"
			(at 2.5 5 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 -4.1 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 270)
			(size 2 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.125)
			(net 15 "Net-(D1-K)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 5 0 270)
			(size 2 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Net-(D20-K)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBVA_2,5_2-G_1x02_P5.00mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_THT:D_A-405_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 108.5 133.555 90)
		(descr "Diode, A-405 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
		(tags "Diode A-405 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
		(property "Reference" "D23"
			(at 5.533072 -0.026652 90)
			(layer "F.SilkS")
		)
		(property "Value" "BZW06-15"
			(at 5.08 2.450134 90)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Schottky diode"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at 0 -1.9 90)
			(layer "F.SilkS")
		)
		(fp_text user "K"
			(at 0 -1.9 90)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 5.47 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "Net-(D23-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(12V0-Pin_2)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_THT.3dshapes/D_A-405_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-220-3_Vertical"
		(layer "F.Cu")
		(at 58.491 80.772 -90)
		(descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
		(tags "TO-220-3 Vertical RM 2.54mm")
		(property "Reference" "Q1"
			(at 8.636 -0.9495 0)
			(layer "F.SilkS")
		)
		(property "Value" "IRLZ44N"
			(at 2.794 2.557 90)
			(layer "F.SilkS")
		)
		(property "Datasheet" "http://www.irf.com/product-info/datasheets/data/irlz44n.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "47A Id, 55V Vds, 22mOhm Rds Single N-Channel HEXFET Power MOSFET, TO-220AB"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO?220*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 8.636 -0.945 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "Net-(Q1-G)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 270)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(D1-A)")
			(pinfunction "D")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 5.08 0 270)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(12V0-Pin_2)")
			(pinfunction "S")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Phoenix_MSTB:PhoenixContact_MSTBVA_2,5_2-G_1x02_P5.00mm_Vertical"
		(layer "F.Cu")
		(at 116 128.475 -90)
		(descr "Generic Phoenix Contact connector footprint for: MSTBVA_2,5/2-G; number of pins: 02; pin pitch: 5.00mm; Vertical || order number: 1755516 12A || order number: 1924198 16A (HC)")
		(tags "phoenix_contact connector MSTBVA_01x02_G_5.00mm")
		(property "Reference" "Digital10"
			(at 3.605 -5.92 270)
			(layer "F.SilkS")
		)
		(property "Value" "Screw_Terminal_01x02"
			(at 2.5 5 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 -4.1 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 270)
			(size 2 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.125)
			(net 15 "Net-(D1-K)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 5 0 270)
			(size 2 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "Net-(D23-K)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBVA_2,5_2-G_1x02_P5.00mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 101 74.168)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R15"
			(at 3.81 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "300R"
			(at -3.302 0 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 59 "Net-(TX0-Pin_8)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "Net-(D14-K)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Phoenix_MSTB:PhoenixContact_MSTBVA_2,5_2-G_1x02_P5.00mm_Vertical"
		(layer "F.Cu")
		(at 116 85.585 -90)
		(descr "Generic Phoenix Contact connector footprint for: MSTBVA_2,5/2-G; number of pins: 02; pin pitch: 5.00mm; Vertical || order number: 1755516 12A || order number: 1924198 16A (HC)")
		(tags "phoenix_contact connector MSTBVA_01x02_G_5.00mm")
		(property "Reference" "Digital5"
			(at 3.315 -6 270)
			(layer "F.SilkS")
		)
		(property "Value" "Screw_Terminal_01x02"
			(at 2.5 5 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 -4.1 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 270)
			(size 2 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.125)
			(net 15 "Net-(D1-K)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 5 0 270)
			(size 2 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "Net-(D21-K)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBVA_2,5_2-G_1x02_P5.00mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 75.946 36.322)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R24"
			(at 2.286 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "2K"
			(at 5.588 0 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.286 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 72 "Net-(Vin0-Pin_11)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(ADC1-Pin_2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 68.072 52.324 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R18"
			(at 3.81 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "300R"
			(at -3.556 0 90)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "Net-(TX0-Pin_14)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "Net-(Q9-G)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 63.5 126.492 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R7"
			(at 3.81 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "620R"
			(at 3.81 -2.54 90)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "Net-(D3-A)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "Net-(D11-K)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 68.072 134.112 90)
		(descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
		(tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
		(property "Reference" "D3"
			(at 3.81 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "1N4148"
			(at 3.81 2.54 90)
			(layer "F.SilkS")
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/1N4148_1N4448.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "100V 0.15A standard switching diode, DO-35"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*DO?35*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at 0 -1.8 90)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 4.11 0 90)
			(layer "F.Fab")
		)
		(fp_text user "K"
			(at 0 -1.8 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(D1-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "Net-(D3-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 63.5 76.237665 180)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R1"
			(at 3.81 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at 10.746772 0 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "Net-(Q1-G)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(12V0-Pin_2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_THT:D_DO-15_P5.08mm_Vertical_AnodeUp"
		(layer "F.Cu")
		(at 40.486 71.12)
		(descr "Diode, DO-15 series, Axial, Vertical, pin pitch=5.08mm, , length*diameter=7.6*3.6mm^2, , http://www.diodes.com/_files/packages/DO-15.pdf")
		(tags "Diode DO-15 series Axial Vertical pin pitch 5.08mm  length 7.6mm diameter 3.6mm")
		(property "Reference" "D8"
			(at 8.282 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "BZW06-15"
			(at 2.186 -3.048 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Schottky diode"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "A"
			(at 3.18 1.2 0)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 8.282 0 0)
			(layer "F.Fab")
		)
		(fp_text user "A"
			(at 3.18 1.2 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(12V0-Pin_2)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 5.08 0)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(D1-K)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-15_P5.08mm_Vertical_AnodeUp.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinSocket_2.54mm:PinSocket_1x15_P2.54mm_Vertical"
		(locked yes)
		(layer "F.Cu")
		(at 71.628 62.992 180)
		(descr "Through hole straight socket strip, 1x15, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x15 2.54mm single row")
		(property "Reference" "Vin0"
			(at 0 -2.77 180)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x15_Socket"
			(at 0 38.33 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x15, script generated"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 17.78 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 68 "unconnected-(Vin0-Pin_1-Pad1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(ADC0-Pin_1)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "Net-(Reset0-Pin_2)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(5V0-Pin_1)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(ADC7-Pin_2)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 0 12.7 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(ADC6-Pin_2)")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 15.24 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(ADC5_SCL0-Pin_2)")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 0 17.78 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(ADC4_SCA0-Pin_2)")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 0 20.32 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(ADC3-Pin_2)")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole oval
			(at 0 22.86 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(ADC2-Pin_2)")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole oval
			(at 0 25.4 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 72 "Net-(Vin0-Pin_11)")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole oval
			(at 0 27.94 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 71 "Net-(Vin0-Pin_12)")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" thru_hole oval
			(at 0 30.48 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 69 "unconnected-(Vin0-Pin_13-Pad13)")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" thru_hole oval
			(at 0 33.02 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 70 "unconnected-(Vin0-Pin_14-Pad14)")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(pad "15" thru_hole oval
			(at 0 35.56 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 63 "Net-(Vin0-Pin_15)")
			(pinfunction "Pin_15")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x15_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Phoenix_MSTB:PhoenixContact_MSTBVA_2,5_3-G_1x03_P5.00mm_Vertical"
		(layer "F.Cu")
		(at 26.924 111.6 90)
		(descr "Generic Phoenix Contact connector footprint for: MSTBVA_2,5/3-G; number of pins: 03; pin pitch: 5.00mm; Vertical || order number: 1755529 12A || order number: 1924208 16A (HC)")
		(tags "phoenix_contact connector MSTBVA_01x03_G_5.00mm")
		(property "Reference" "Digital7"
			(at 5 -6 90)
			(layer "F.SilkS")
		)
		(property "Value" "Screw_Terminal_01x03"
			(at 5 5 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5 -4.1 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 2 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.125)
			(net 47 "Net-(Digital7-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 5 0 90)
			(size 2 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "Net-(Digital7-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 10 0 90)
			(size 2 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "Net-(Digital7-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBVA_2,5_3-G_1x03_P5.00mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Phoenix_MSTB:PhoenixContact_MSTBVA_2,5_2-G_1x02_P5.00mm_Vertical"
		(layer "F.Cu")
		(at 116 107.175 -90)
		(descr "Generic Phoenix Contact connector footprint for: MSTBVA_2,5/2-G; number of pins: 02; pin pitch: 5.00mm; Vertical || order number: 1755516 12A || order number: 1924198 16A (HC)")
		(tags "phoenix_contact connector MSTBVA_01x02_G_5.00mm")
		(property "Reference" "Digital6"
			(at 3.569 -6 270)
			(layer "F.SilkS")
		)
		(property "Value" "Screw_Terminal_01x02"
			(at 2.5 5 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 -4.1 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 270)
			(size 2 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.125)
			(net 15 "Net-(D1-K)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 5 0 270)
			(size 2 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "Net-(D22-K)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBVA_2,5_2-G_1x02_P5.00mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_THT:LED_D5.0mm"
		(layer "F.Cu")
		(at 66.548 143.256)
		(descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf, generated by kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D12"
			(at -3.22 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 6.35 0 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "Net-(D12-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(D1-K)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Phoenix_MSTB:PhoenixContact_MSTBVA_2,5_2-G_1x02_P5.00mm_Vertical"
		(layer "F.Cu")
		(at 98.642 29.21)
		(descr "Generic Phoenix Contact connector footprint for: MSTBVA_2,5/2-G; number of pins: 02; pin pitch: 5.00mm; Vertical || order number: 1755516 12A || order number: 1924198 16A (HC)")
		(tags "phoenix_contact connector MSTBVA_01x02_G_5.00mm")
		(property "Reference" "ADC4_SCA0"
			(at 2.5 -6 0)
			(layer "F.SilkS")
		)
		(property "Value" "Screw_Terminal_01x02"
			(at 2.5 5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 -4.1 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 2 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.125)
			(net 4 "Net-(ADC0-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 5 0)
			(size 2 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(ADC4_SCA0-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBVA_2,5_2-G_1x02_P5.00mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-220-3_Vertical"
		(layer "F.Cu")
		(at 102 153.416 90)
		(descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
		(tags "TO-220-3 Vertical RM 2.54mm")
		(property "Reference" "Q5"
			(at 8.89 -1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "IRLZ44N"
			(at 2.576406 2.219086 90)
			(layer "F.SilkS")
		)
		(property "Datasheet" "http://www.irf.com/product-info/datasheets/data/irlz44n.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "47A Id, 55V Vds, 22mOhm Rds Single N-Channel HEXFET Power MOSFET, TO-220AB"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO?220*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 8.89 -1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "Net-(D13-A)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 90)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Net-(D20-K)")
			(pinfunction "D")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 5.08 0 90)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(12V0-Pin_2)")
			(pinfunction "S")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_5.3mm_M5_ISO14580"
		(layer "F.Cu")
		(at 124.5 166)
		(descr "Mounting Hole 5.3mm, no annular, M5, ISO14580")
		(tags "mounting hole 5.3mm no annular m5 iso14580")
		(property "Reference" "M5"
			(at -5.628 2.148 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_5.3mm_M5_ISO14580"
			(at 0 5.25 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 5.3 5.3)
			(drill 5.3)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Connector_Phoenix_MSTB:PhoenixContact_MSTBVA_2,5_3-G_1x03_P5.00mm_Vertical"
		(layer "F.Cu")
		(at 100.892 52.992 -90)
		(descr "Generic Phoenix Contact connector footprint for: MSTBVA_2,5/3-G; number of pins: 03; pin pitch: 5.00mm; Vertical || order number: 1755529 12A || order number: 1924208 16A (HC)")
		(tags "phoenix_contact connector MSTBVA_01x03_G_5.00mm")
		(property "Reference" "Serial0"
			(at 4.412 9.452 270)
			(layer "F.SilkS")
		)
		(property "Value" "Screw_Terminal_01x03"
			(at 5 5 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5 -4.1 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 270)
			(size 2 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.125)
			(net 4 "Net-(ADC0-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 5 0 270)
			(size 2 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 65 "Net-(Serial0-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 10 0 270)
			(size 2 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "Net-(Serial0-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBVA_2,5_3-G_1x03_P5.00mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Relay_THT:Relay_SPDT_SANYOU_SRD_Series_Form_C"
		(layer "F.Cu")
		(at 52.496 106.68 180)
		(descr "relay Sanyou SRD series Form C http://www.sanyourelay.ca/public/products/pdf/SRD.pdf")
		(tags "relay Sanyu SRD form C")
		(property "Reference" "K2"
			(at 8.1 9.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "SANYOU_SRD_Form_C"
			(at 8 -9.6 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" "http://www.sanyourelay.ca/public/products/pdf/SRD.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Sanyo SRD relay, Single Pole Miniature Power Relay,"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Relay*SPDT*SANYOU*SRD*Series*Form*C*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.1 0.025 0)
			(layer "F.Fab")
		)
		(fp_text user "1"
			(at 0 -2.3 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 3 3)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "Net-(Digital7-Pin_2)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.95 6.05 270)
			(size 2.5 2.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "Net-(D2-A)")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 14.15 6.05 270)
			(size 3 3)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "Net-(Digital7-Pin_3)")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 14.2 -6 270)
			(size 3 3)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "Net-(Digital7-Pin_1)")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 1.95 -5.95 270)
			(size 2.5 2.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(D1-K)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Relay_THT.3dshapes/Relay_SPDT_SANYOU_SRD_Series_Form_C.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Phoenix_MSTB:PhoenixContact_MSTBVA_2,5_2-G_1x02_P5.00mm_Vertical"
		(layer "F.Cu")
		(at 113.12 29.1775)
		(descr "Generic Phoenix Contact connector footprint for: MSTBVA_2,5/2-G; number of pins: 02; pin pitch: 5.00mm; Vertical || order number: 1755516 12A || order number: 1924198 16A (HC)")
		(tags "phoenix_contact connector MSTBVA_01x02_G_5.00mm")
		(property "Reference" "ADC5_SCL0"
			(at 2.5 -6 0)
			(layer "F.SilkS")
		)
		(property "Value" "Screw_Terminal_01x02"
			(at 2.5 5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 -4.1 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 2 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.125)
			(net 4 "Net-(ADC0-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 5 0)
			(size 2 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(ADC5_SCL0-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBVA_2,5_2-G_1x02_P5.00mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Phoenix_MSTB:PhoenixContact_MSTBVA_2,5_2-G_1x02_P5.00mm_Vertical"
		(layer "F.Cu")
		(at 77 80)
		(descr "Generic Phoenix Contact connector footprint for: MSTBVA_2,5/2-G; number of pins: 02; pin pitch: 5.00mm; Vertical || order number: 1755516 12A || order number: 1924198 16A (HC)")
		(tags "phoenix_contact connector MSTBVA_01x02_G_5.00mm")
		(property "Reference" "ADC0"
			(at 4.788 -6.848 0)
			(layer "F.SilkS")
		)
		(property "Value" "Screw_Terminal_01x02"
			(at 2.5 5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 -4.1 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 2 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.125)
			(net 4 "Net-(ADC0-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 5 0)
			(size 2 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(ADC0-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBVA_2,5_2-G_1x02_P5.00mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_THT:D_DO-41_SOD81_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 108.5 99.06 180)
		(descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
		(tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
		(property "Reference" "D16"
			(at 4.205728 -0.000001 0)
			(layer "F.SilkS")
		)
		(property "Value" "1N4733"
			(at 12.192 0 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Zener diode"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at 1.82 0 0)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 4.2 0 0)
			(layer "F.Fab")
		)
		(fp_text user "K"
			(at 0 -2.1 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 2.2 2.2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "Net-(D16-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 180)
			(size 2.2 2.2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(12V0-Pin_2)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:CP_Radial_D12.5mm_P5.00mm"
		(layer "F.Cu")
		(at 61.251959 24.892 180)
		(descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=12.5mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 5.00mm  diameter 12.5mm Electrolytic Capacitor")
		(property "Reference" "C3"
			(at -3.772041 4.572 0)
			(layer "F.SilkS")
		)
		(property "Value" "C_Polarized"
			(at 2.5 7.5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(D1-K)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 180)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(12V0-Pin_2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D12.5mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Phoenix_MSTB:PhoenixContact_MSTBVA_2,5_2-G_1x02_P5.00mm_Vertical"
		(layer "F.Cu")
		(at 77 150)
		(descr "Generic Phoenix Contact connector footprint for: MSTBVA_2,5/2-G; number of pins: 02; pin pitch: 5.00mm; Vertical || order number: 1755516 12A || order number: 1924198 16A (HC)")
		(tags "phoenix_contact connector MSTBVA_01x02_G_5.00mm")
		(property "Reference" "ADC7"
			(at 2.5 -6 0)
			(layer "F.SilkS")
		)
		(property "Value" "Screw_Terminal_01x02"
			(at 2.5 5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 -4.1 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 2 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.125)
			(net 4 "Net-(ADC0-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 5 0)
			(size 2 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(ADC7-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBVA_2,5_2-G_1x02_P5.00mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-220-3_Vertical"
		(layer "F.Cu")
		(at 102 108.712 90)
		(descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
		(tags "TO-220-3 Vertical RM 2.54mm")
		(property "Reference" "Q7"
			(at 8.565 -1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "IRLZ44N"
			(at 2.206301 2.219086 90)
			(layer "F.SilkS")
		)
		(property "Datasheet" "http://www.irf.com/product-info/datasheets/data/irlz44n.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "47A Id, 55V Vds, 22mOhm Rds Single N-Channel HEXFET Power MOSFET, TO-220AB"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO?220*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 8.565 -1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "Net-(D16-K)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 90)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "Net-(D22-K)")
			(pinfunction "D")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 5.08 0 90)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(12V0-Pin_2)")
			(pinfunction "S")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 55.372 44.45 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R30"
			(at 3.81 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "300R"
			(at 3.81 -2.54 90)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 73 "Net-(BZ1-+)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(5V0-Pin_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-220-3_Vertical"
		(layer "F.Cu")
		(at 52.561 53.34 90)
		(descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
		(tags "TO-220-3 Vertical RM 2.54mm")
		(property "Reference" "U1"
			(at 3.048 -5.825 90)
			(layer "F.SilkS")
		)
		(property "Value" "L7805"
			(at 3.048 -4.301 90)
			(layer "F.SilkS")
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/41/4f/b3/b0/12/d4/47/88/CD00000444.pdf/files/CD00000444.pdf/jcr:content/translations/en.CD00000444.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Positive 1.5A 35V Linear Regulator, Fixed Output 5V, TO-220/TO-263/TO-252"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO?252* TO?263* TO?220*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.048 -5.825 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(D5-K)")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 90)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(12V0-Pin_2)")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" thru_hole oval
			(at 5.08 0 90)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(5V0-Pin_1)")
			(pinfunction "OUT")
			(pintype "power_out")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_THT:LED_D5.0mm"
		(layer "F.Cu")
		(at 115.240616 78.945 90)
		(descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf, generated by kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D15"
			(at 1.27 3.81 90)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 1.27 3.96 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "Net-(D15-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 90)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "Net-(D14-K)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Axial_L5.1mm_D3.1mm_P7.50mm_Horizontal"
		(layer "F.Cu")
		(at 50.286 40.64 180)
		(descr "C, Axial series, Axial, Horizontal, pin pitch=7.5mm, , length*diameter=5.1*3.1mm^2, http://www.vishay.com/docs/45231/arseries.pdf")
		(tags "C Axial series Axial Horizontal pin pitch 7.5mm  length 5.1mm diameter 3.1mm")
		(property "Reference" "C2"
			(at 3.75 -2.67 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 3.75 2.67 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.75 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(5V0-Pin_1)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.5 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(12V0-Pin_2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Axial_L5.1mm_D3.1mm_P7.50mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 101 117.348)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R17"
			(at 3.81 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "300R"
			(at -3.302 0 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "Net-(TX0-Pin_13)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "Net-(D18-K)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Phoenix_MSTB:PhoenixContact_MSTBVA_2,5_2-G_1x02_P5.00mm_Vertical"
		(layer "F.Cu")
		(at 77 122)
		(descr "Generic Phoenix Contact connector footprint for: MSTBVA_2,5/2-G; number of pins: 02; pin pitch: 5.00mm; Vertical || order number: 1755516 12A || order number: 1924198 16A (HC)")
		(tags "phoenix_contact connector MSTBVA_01x02_G_5.00mm")
		(property "Reference" "ADC3"
			(at 2.5 -6 0)
			(layer "F.SilkS")
		)
		(property "Value" "Screw_Terminal_01x02"
			(at 2.5 5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 -4.1 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 2 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.125)
			(net 4 "Net-(ADC0-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 5 0)
			(size 2 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(ADC3-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBVA_2,5_2-G_1x02_P5.00mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-220-3_Vertical"
		(layer "F.Cu")
		(at 102 130.048 90)
		(descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
		(tags "TO-220-3 Vertical RM 2.54mm")
		(property "Reference" "Q8"
			(at 8.89 -1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "IRLZ44N"
			(at 2.559583 2.202263 90)
			(layer "F.SilkS")
		)
		(property "Datasheet" "http://www.irf.com/product-info/datasheets/data/irlz44n.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "47A Id, 55V Vds, 22mOhm Rds Single N-Channel HEXFET Power MOSFET, TO-220AB"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO?220*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 8.89 -1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "Net-(D18-K)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 90)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "Net-(D23-K)")
			(pinfunction "D")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 5.08 0 90)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(12V0-Pin_2)")
			(pinfunction "S")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Phoenix_MSTB:PhoenixContact_MSTBVA_2,5_3-G_1x03_P5.00mm_Vertical"
		(layer "F.Cu")
		(at 26.924 154.86 90)
		(descr "Generic Phoenix Contact connector footprint for: MSTBVA_2,5/3-G; number of pins: 03; pin pitch: 5.00mm; Vertical || order number: 1755529 12A || order number: 1924208 16A (HC)")
		(tags "phoenix_contact connector MSTBVA_01x03_G_5.00mm")
		(property "Reference" "Digital2"
			(at 5 -6 90)
			(layer "F.SilkS")
		)
		(property "Value" "Screw_Terminal_01x03"
			(at 5 5 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5 -4.1 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 2 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.125)
			(net 41 "Net-(Digital2-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 5 0 90)
			(size 2 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "Net-(Digital2-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 10 0 90)
			(size 2 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "Net-(Digital2-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBVA_2,5_3-G_1x03_P5.00mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 63.5 104.648 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R6"
			(at 3.81 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "620R"
			(at 3.81 -2.54 90)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "Net-(D2-A)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "Net-(D10-K)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 101 96.012)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R16"
			(at 3.809999 -0.00089 0)
			(layer "F.SilkS")
		)
		(property "Value" "300R"
			(at -3.048 0 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "Net-(TX0-Pin_9)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "Net-(D16-K)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_THT:LED_D5.0mm"
		(layer "F.Cu")
		(at 59.177 35.56)
		(descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf, generated by kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D26"
			(at -3.297 -2.032 0)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 1.27 3.96 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(12V0-Pin_2)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "Net-(D26-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 63.5 140.716 180)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R4"
			(at 3.81 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at 10.16 0 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "Net-(Q4-G)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(12V0-Pin_2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_THT:D_DO-41_SOD81_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 108.5 77.216 180)
		(descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
		(tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
		(property "Reference" "D14"
			(at 4.173587 -0.038272 0)
			(layer "F.SilkS")
		)
		(property "Value" "1N4733"
			(at 11.938 0 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Zener diode"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at 0 -2.1 0)
			(layer "F.SilkS")
		)
		(fp_text user "K"
			(at 0 -2.1 0)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 4.2 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 2.2 2.2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "Net-(D14-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 180)
			(size 2.2 2.2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(12V0-Pin_2)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_THT:LED_D5.0mm"
		(layer "F.Cu")
		(at 115.090866 100.535 90)
		(descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf, generated by kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D17"
			(at 1.27 -3.96 90)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 1.27 3.96 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "Net-(D17-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 90)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "Net-(D16-K)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_5.3mm_M5_ISO14580"
		(layer "F.Cu")
		(at 22.5 166)
		(descr "Mounting Hole 5.3mm, no annular, M5, ISO14580")
		(tags "mounting hole 5.3mm no annular m5 iso14580")
		(property "Reference" "M5"
			(at 5.44 2.148 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_5.3mm_M5_ISO14580"
			(at 0 5.25 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 5.3 5.3)
			(drill 5.3)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 75.946 30.226)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R21"
			(at 2.286 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "2K"
			(at 5.588 0 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.286 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 71 "Net-(Vin0-Pin_12)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(ADC0-Pin_2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 62.992 97.536 180)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R2"
			(at 3.81 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at 10.668 0 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "Net-(Q2-G)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(12V0-Pin_2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 65.024 59.944 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R19"
			(at 3.81 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at -2.286 0 90)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "Net-(Q9-G)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(12V0-Pin_2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 68.58 112.268 90)
		(descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
		(tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
		(property "Reference" "D2"
			(at 3.81 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "1N4148"
			(at 3.81 2.12 90)
			(layer "F.SilkS")
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/1N4148_1N4448.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "100V 0.15A standard switching diode, DO-35"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*DO?35*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at 0 -1.8 90)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 4.11 0 90)
			(layer "F.Fab")
		)
		(fp_text user "K"
			(at 0 -1.8 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(D1-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "Net-(D2-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Relay_THT:Relay_SPDT_SANYOU_SRD_Series_Form_C"
		(layer "F.Cu")
		(at 52.696 149.86 180)
		(descr "relay Sanyou SRD series Form C http://www.sanyourelay.ca/public/products/pdf/SRD.pdf")
		(tags "relay Sanyu SRD form C")
		(property "Reference" "K4"
			(at 8.1 9.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "SANYOU_SRD_Form_C"
			(at 8 -9.6 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" "http://www.sanyourelay.ca/public/products/pdf/SRD.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Sanyo SRD relay, Single Pole Miniature Power Relay,"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Relay*SPDT*SANYOU*SRD*Series*Form*C*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.1 0.025 0)
			(layer "F.Fab")
		)
		(fp_text user "1"
			(at 0 -2.3 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 3 3)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "Net-(Digital2-Pin_2)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.95 6.05 270)
			(size 2.5 2.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "Net-(D4-A)")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 14.15 6.05 270)
			(size 3 3)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "Net-(Digital2-Pin_3)")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 14.2 -6 270)
			(size 3 3)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "Net-(Digital2-Pin_1)")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 1.95 -5.95 270)
			(size 2.5 2.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(D1-K)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Relay_THT.3dshapes/Relay_SPDT_SANYOU_SRD_Series_Form_C.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 97.028 81.28 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R10"
			(at 3.81 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "620R"
			(at 3.81 2.54 90)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(12V0-Pin_2)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "Net-(D15-K)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 63.5 147.828 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R8"
			(at 3.81 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "620R"
			(at 3.81 -2.54 90)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "Net-(D4-A)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "Net-(D12-K)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_THT:LED_D5.0mm"
		(layer "F.Cu")
		(at 115.151866 122.125 90)
		(descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf, generated by kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D19"
			(at 1.27 -3.96 90)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 1.27 3.96 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "Net-(D19-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 90)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "Net-(D18-K)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 63.246 119.620165 180)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R3"
			(at 3.81 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at 10.414 0.254 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "Net-(Q3-G)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(12V0-Pin_2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Phoenix_MSTB:PhoenixContact_MSTBVA_2,5_2-G_1x02_P5.00mm_Vertical"
		(layer "F.Cu")
		(at 77 108)
		(descr "Generic Phoenix Contact connector footprint for: MSTBVA_2,5/2-G; number of pins: 02; pin pitch: 5.00mm; Vertical || order number: 1755516 12A || order number: 1924198 16A (HC)")
		(tags "phoenix_contact connector MSTBVA_01x02_G_5.00mm")
		(property "Reference" "ADC2"
			(at 2.5 -6 0)
			(layer "F.SilkS")
		)
		(property "Value" "Screw_Terminal_01x02"
			(at 2.5 5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 -4.1 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 2 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.125)
			(net 4 "Net-(ADC0-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 5 0)
			(size 2 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(ADC2-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBVA_2,5_2-G_1x02_P5.00mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_THT:D_DO-15_P5.08mm_Vertical_AnodeUp"
		(layer "F.Cu")
		(at 26.516 71.12)
		(descr "Diode, DO-15 series, Axial, Vertical, pin pitch=5.08mm, , length*diameter=7.6*3.6mm^2, , http://www.diodes.com/_files/packages/DO-15.pdf")
		(tags "Diode DO-15 series Axial Vertical pin pitch 5.08mm  length 7.6mm diameter 3.6mm")
		(property "Reference" "D7"
			(at -3.656 0.508 0)
			(layer "F.SilkS")
		)
		(property "Value" "BZW06-15"
			(at 2.44 -3.048 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Schottky diode"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "A"
			(at 3.18 1.2 0)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at -3.656 0.508 0)
			(layer "F.Fab")
		)
		(fp_text user "A"
			(at 3.18 1.2 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(D1-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 5.08 0)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(12V0-Pin_2)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-15_P5.08mm_Vertical_AnodeUp.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Phoenix_MSTB:PhoenixContact_MSTBVA_2,5_2-G_1x02_P5.00mm_Vertical"
		(layer "F.Cu")
		(at 77 136)
		(descr "Generic Phoenix Contact connector footprint for: MSTBVA_2,5/2-G; number of pins: 02; pin pitch: 5.00mm; Vertical || order number: 1755516 12A || order number: 1924198 16A (HC)")
		(tags "phoenix_contact connector MSTBVA_01x02_G_5.00mm")
		(property "Reference" "ADC6"
			(at 2.5 -6 0)
			(layer "F.SilkS")
		)
		(property "Value" "Screw_Terminal_01x02"
			(at 2.5 5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 -4.1 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 2 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.125)
			(net 4 "Net-(ADC0-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 5 0)
			(size 2 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(ADC6-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBVA_2,5_2-G_1x02_P5.00mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_THT:D_DO-41_SOD81_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 108.5 142.24 180)
		(descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
		(tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
		(property "Reference" "D6"
			(at 4.200435 -0.003485 0)
			(layer "F.SilkS")
		)
		(property "Value" "1N4733"
			(at 11.938 0 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Zener diode"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at 0 -2.1 0)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 4.2 0 0)
			(layer "F.Fab")
		)
		(fp_text user "K"
			(at 0 -2.1 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 2.2 2.2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "Net-(D13-A)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 180)
			(size 2.2 2.2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(12V0-Pin_2)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Buzzer_Beeper:MagneticBuzzer_PUI_AT-0927-TT-6-R"
		(layer "F.Cu")
		(at 61.268 45.244 -90)
		(descr "Buzzer Magnetic 9mm AT-0927-TT-6-R, http://www.puiaudio.com/pdf/AT-0927-TT-6-R.pdf")
		(tags "Buzzer Magnetic 9mm AT-0927-TT-6-R")
		(property "Reference" "BZ1"
			(at 2 5.5 90)
			(layer "F.SilkS")
		)
		(property "Value" "Buzzer"
			(at 2 7 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Buzzer, polarized"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*Buzzer*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "+"
			(at -1.5 -0.1 90)
			(layer "F.SilkS")
		)
		(fp_text user "+"
			(at -1.5 -0.1 90)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 2 2 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 73 "Net-(BZ1-+)")
			(pinfunction "+")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 4 0 270)
			(size 1.6 1.6)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(BZ1--)")
			(pinfunction "-")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Buzzer_Beeper.3dshapes/MagneticBuzzer_PUI_AT-0927-TT-6-R.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 63.5 83.312 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R5"
			(at 3.81 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "620R"
			(at 3.81 -2.54 90)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(D1-A)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "Net-(D9-K)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-220-3_Vertical"
		(layer "F.Cu")
		(at 58.491 145.288 -90)
		(descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
		(tags "TO-220-3 Vertical RM 2.54mm")
		(property "Reference" "Q4"
			(at 8.636 -0.945 0)
			(layer "F.SilkS")
		)
		(property "Value" "IRLZ44N"
			(at 2.54 2.611 90)
			(layer "F.SilkS")
		)
		(property "Datasheet" "http://www.irf.com/product-info/datasheets/data/irlz44n.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "47A Id, 55V Vds, 22mOhm Rds Single N-Channel HEXFET Power MOSFET, TO-220AB"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO?220*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 8.636 -0.9495 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "Net-(Q4-G)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 270)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "Net-(D4-A)")
			(pinfunction "D")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 5.08 0 270)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(12V0-Pin_2)")
			(pinfunction "S")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_THT:LED_D5.0mm"
		(layer "F.Cu")
		(at 66.289 121.92)
		(descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf, generated by kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D11"
			(at -2.81 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 6.35 0 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "Net-(D11-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(D1-K)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 110.036 46.736 90)
		(descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
		(tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
		(property "Reference" "D25"
			(at 5.448646 0.037066 90)
			(layer "F.SilkS")
		)
		(property "Value" "1N4733"
			(at 5.08 -2.34 90)
			(layer "F.SilkS")
		)
		(property "Datasheet" "https://www.vishay.com/docs/85816/1n4728a.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1300mW Silicon planar power Zener diodes, DO-41"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*DO?41*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at 0 -2.1 90)
			(layer "F.SilkS")
		)
		(fp_text user "K"
			(at 0 -2.1 90)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 5.47 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 2.2 2.2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "Net-(D25-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 2.2 2.2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(ADC0-Pin_1)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 66.04 31.242 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R29"
			(at 3.81989 0.006531 90)
			(layer "F.SilkS")
		)
		(property "Value" "620R"
			(at 4.064 -2.54 90)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 63 "Net-(Vin0-Pin_15)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "Net-(D26-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-220-3_Vertical"
		(layer "F.Cu")
		(at 58.491 123.952 -90)
		(descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
		(tags "TO-220-3 Vertical RM 2.54mm")
		(property "Reference" "Q3"
			(at 8.636 -0.437 0)
			(layer "F.SilkS")
		)
		(property "Value" "IRLZ44N"
			(at 2.54 2.611 90)
			(layer "F.SilkS")
		)
		(property "Datasheet" "http://www.irf.com/product-info/datasheets/data/irlz44n.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "47A Id, 55V Vds, 22mOhm Rds Single N-Channel HEXFET Power MOSFET, TO-220AB"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO?220*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 8.636 -0.437 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "Net-(Q3-G)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 270)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "Net-(D3-A)")
			(pinfunction "D")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 5.08 0 270)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(12V0-Pin_2)")
			(pinfunction "S")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 121.4335 49.828 180)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R20"
			(at 3.81 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "1K"
			(at 9.6735 0.044 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "Net-(D25-K)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "Net-(Digital12-Pin_2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_THT:LED_D5.0mm"
		(layer "F.Cu")
		(at 66.04 100.076)
		(descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf, generated by kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D10"
			(at -3.4 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 6.35 0 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "Net-(D10-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(D1-K)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_THT:LED_D5.0mm"
		(layer "F.Cu")
		(at 66.797 78.74)
		(descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf, generated by kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D9"
			(at -2.99 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 6.35 0 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "Net-(D9-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(D1-K)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 97.028 122.682 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R12"
			(at 3.81 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "620R"
			(at 3.81 2.54 90)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(12V0-Pin_2)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "Net-(D19-K)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 52.886 65.278 90)
		(descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
		(tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
		(property "Reference" "D5"
			(at 4.064 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "1N4148"
			(at 4.318 1.978 90)
			(layer "F.SilkS")
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/1N4148_1N4448.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "100V 0.15A standard switching diode, DO-35"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*DO?35*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at 0 -1.8 90)
			(layer "F.SilkS")
		)
		(fp_text user "K"
			(at 0 -1.8 90)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 4.11 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(D5-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(5V0-Pin_1)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-220-3_Vertical"
		(layer "F.Cu")
		(at 58.42 102.108 -90)
		(descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
		(tags "TO-220-3 Vertical RM 2.54mm")
		(property "Reference" "Q2"
			(at 8.636 -1.016 0)
			(layer "F.SilkS")
		)
		(property "Value" "IRLZ44N"
			(at 2.54 2.176 90)
			(layer "F.SilkS")
		)
		(property "Datasheet" "http://www.irf.com/product-info/datasheets/data/irlz44n.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "47A Id, 55V Vds, 22mOhm Rds Single N-Channel HEXFET Power MOSFET, TO-220AB"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO?220*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 8.636 -1.016 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "Net-(Q2-G)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 270)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "Net-(D2-A)")
			(pinfunction "D")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 5.08 0 270)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(12V0-Pin_2)")
			(pinfunction "S")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Fuse:Fuseholder_Clip-5x20mm_Eaton_1A5601-01_Inline_P20.80x6.76mm_D1.70mm_Horizontal"
		(layer "F.Cu")
		(at 35.106 40.4 -90)
		(descr "Fuseholder Clips, 5x20mm Cylinder Fuse, Pins Inline, Horizontal, Eaton 1A5601-01, https://www.eaton.com/content/dam/eaton/products/electronic-components/resources/data-sheet/eaton-1axxxx-pcb-fuse-clips-atc-atm-blade-data-sheet.pdf")
		(tags "fuse clip open")
		(property "Reference" "F2"
			(at 12.432 -6.042 90)
			(layer "F.SilkS")
		)
		(property "Value" "1.5A"
			(at 8.876 -6.042 90)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Fuse"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*Fuse*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 10.4 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 270)
			(size 2.7 2.7)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 3 "Net-(12V0-Pin_1)")
			(pintype "passive")
		)
		(pad "1" thru_hole roundrect
			(at 6.76 0 270)
			(size 2.7 2.7)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 3 "Net-(12V0-Pin_1)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 14.04 0 270)
			(size 2.7 2.7)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(D5-K)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 20.8 0 270)
			(size 2.7 2.7)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(D5-K)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Fuse.3dshapes/Fuseholder_Clip-5x20mm_Eaton_1A5601-01_Inline_P20.80x6.76mm_D1.70mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 113.338 65.278)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R13"
			(at 3.81 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "1K"
			(at 9.598 -0.254 90)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "Net-(D24-K)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "Net-(Digital3-Pin_2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 97.028 102.362 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R11"
			(at 3.874071 0.007155 90)
			(layer "F.SilkS")
		)
		(property "Value" "620R"
			(at 3.81 2.54 90)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(12V0-Pin_2)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "Net-(D17-K)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Phoenix_MSTB:PhoenixContact_MSTBVA_2,5_2-G_1x02_P5.00mm_Vertical"
		(layer "F.Cu")
		(at 117.4345 55.154 -90)
		(descr "Generic Phoenix Contact connector footprint for: MSTBVA_2,5/2-G; number of pins: 02; pin pitch: 5.00mm; Vertical || order number: 1755516 12A || order number: 1924198 16A (HC)")
		(tags "phoenix_contact connector MSTBVA_01x02_G_5.00mm")
		(property "Reference" "Digital3"
			(at 4.282 -6.0095 270)
			(layer "F.SilkS")
		)
		(property "Value" "Screw_Terminal_01x02"
			(at 2.5 5 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 -4.1 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 270)
			(size 2 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.125)
			(net 4 "Net-(ADC0-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 5 0 270)
			(size 2 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "Net-(Digital3-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBVA_2,5_2-G_1x02_P5.00mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_5.3mm_M5_ISO14580"
		(layer "F.Cu")
		(at 124.5 21)
		(descr "Mounting Hole 5.3mm, no annular, M5, ISO14580")
		(tags "mounting hole 5.3mm no annular m5 iso14580")
		(property "Reference" "M5"
			(at -0.04 5.416 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_5.3mm_M5_ISO14580"
			(at 0 5.25 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 5.3 5.3)
			(drill 5.3)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Connector_Phoenix_MSTB:PhoenixContact_MSTBVA_2,5_2-G_1x02_P5.00mm_Vertical"
		(layer "F.Cu")
		(at 42.726 26.6375)
		(descr "Generic Phoenix Contact connector footprint for: MSTBVA_2,5/2-G; number of pins: 02; pin pitch: 5.00mm; Vertical || order number: 1755516 12A || order number: 1924198 16A (HC)")
		(tags "phoenix_contact connector MSTBVA_01x02_G_5.00mm")
		(property "Reference" "5V0"
			(at 2.5 -6 0)
			(layer "F.SilkS")
		)
		(property "Value" "Screw_Terminal_01x02"
			(at 2.5 5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 -4.1 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 2 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.125)
			(net 1 "Net-(5V0-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 5 0)
			(size 2 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(12V0-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBVA_2,5_2-G_1x02_P5.00mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Phoenix_MSTB:PhoenixContact_MSTBVA_2,5_2-G_1x02_P5.00mm_Vertical"
		(layer "F.Cu")
		(at 117.402 39.704 -90)
		(descr "Generic Phoenix Contact connector footprint for: MSTBVA_2,5/2-G; number of pins: 02; pin pitch: 5.00mm; Vertical || order number: 1755516 12A || order number: 1924198 16A (HC)")
		(tags "phoenix_contact connector MSTBVA_01x02_G_5.00mm")
		(property "Reference" "Digital12"
			(at 4.492 -6 270)
			(layer "F.SilkS")
		)
		(property "Value" "Screw_Terminal_01x02"
			(at 2.5 5 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 -4.1 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 270)
			(size 2 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.125)
			(net 4 "Net-(ADC0-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 5 0 270)
			(size 2 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "Net-(Digital12-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBVA_2,5_2-G_1x02_P5.00mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Relay_THT:Relay_SPDT_SANYOU_SRD_Series_Form_C"
		(layer "F.Cu")
		(at 52.696 128.27 180)
		(descr "relay Sanyou SRD series Form C http://www.sanyourelay.ca/public/products/pdf/SRD.pdf")
		(tags "relay Sanyu SRD form C")
		(property "Reference" "K3"
			(at 8.1 9.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "SANYOU_SRD_Form_C"
			(at 8 -9.6 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" "http://www.sanyourelay.ca/public/products/pdf/SRD.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Sanyo SRD relay, Single Pole Miniature Power Relay,"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Relay*SPDT*SANYOU*SRD*Series*Form*C*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "1"
			(at 0 -2.3 0)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 7.1 0.025 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 3 3)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "Net-(Digital4-Pin_2)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.95 6.05 270)
			(size 2.5 2.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "Net-(D3-A)")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 14.15 6.05 270)
			(size 3 3)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "Net-(Digital4-Pin_3)")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 14.2 -6 270)
			(size 3 3)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "Net-(Digital4-Pin_1)")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 1.95 -5.95 270)
			(size 2.5 2.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(D1-K)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Relay_THT.3dshapes/Relay_SPDT_SANYOU_SRD_Series_Form_C.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_THT:D_A-405_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 108.5 111.965 90)
		(descr "Diode, A-405 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
		(tags "Diode A-405 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
		(property "Reference" "D22"
			(at 5.453066 0.01048 90)
			(layer "F.SilkS")
		)
		(property "Value" "BZW06-15"
			(at 5.08 2.511134 90)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Schottky diode"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at 0 -1.9 90)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 5.47 0 90)
			(layer "F.Fab")
		)
		(fp_text user "K"
			(at 0 -1.9 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "Net-(D22-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(12V0-Pin_2)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_THT.3dshapes/D_A-405_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Fuse:Fuseholder_Clip-5x20mm_Eaton_1A5601-01_Inline_P20.80x6.76mm_D1.70mm_Horizontal"
		(layer "F.Cu")
		(at 26.216 40.4 -90)
		(descr "Fuseholder Clips, 5x20mm Cylinder Fuse, Pins Inline, Horizontal, Eaton 1A5601-01, https://www.eaton.com/content/dam/eaton/products/electronic-components/resources/data-sheet/eaton-1axxxx-pcb-fuse-clips-atc-atm-blade-data-sheet.pdf")
		(tags "fuse clip open")
		(property "Reference" "F1"
			(at 11.924 5.388 90)
			(layer "F.SilkS")
		)
		(property "Value" "4A"
			(at 8.876 5.388 90)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Fuse"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*Fuse*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 10.4 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 270)
			(size 2.7 2.7)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 3 "Net-(12V0-Pin_1)")
			(pintype "passive")
		)
		(pad "1" thru_hole roundrect
			(at 6.76 0 270)
			(size 2.7 2.7)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 3 "Net-(12V0-Pin_1)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 14.04 0 270)
			(size 2.7 2.7)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(D1-K)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 20.8 0 270)
			(size 2.7 2.7)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(D1-K)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Fuse.3dshapes/Fuseholder_Clip-5x20mm_Eaton_1A5601-01_Inline_P20.80x6.76mm_D1.70mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Phoenix_MSTB:PhoenixContact_MSTBVA_2,5_3-G_1x03_P5.00mm_Vertical"
		(layer "F.Cu")
		(at 26.924 133.02 90)
		(descr "Generic Phoenix Contact connector footprint for: MSTBVA_2,5/3-G; number of pins: 03; pin pitch: 5.00mm; Vertical || order number: 1755529 12A || order number: 1924208 16A (HC)")
		(tags "phoenix_contact connector MSTBVA_01x03_G_5.00mm")
		(property "Reference" "Digital4"
			(at 5 -6 90)
			(layer "F.SilkS")
		)
		(property "Value" "Screw_Terminal_01x03"
			(at 5 5 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5 -4.1 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 2 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.125)
			(net 44 "Net-(Digital4-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 5 0 90)
			(size 2 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "Net-(Digital4-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 10 0 90)
			(size 2 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "Net-(Digital4-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBVA_2,5_3-G_1x03_P5.00mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Phoenix_MSTB:PhoenixContact_MSTBVA_2,5_2-G_1x02_P5.00mm_Vertical"
		(layer "F.Cu")
		(at 77 94)
		(descr "Generic Phoenix Contact connector footprint for: MSTBVA_2,5/2-G; number of pins: 02; pin pitch: 5.00mm; Vertical || order number: 1755516 12A || order number: 1924198 16A (HC)")
		(tags "phoenix_contact connector MSTBVA_01x02_G_5.00mm")
		(property "Reference" "ADC1"
			(at 2.5 -6 0)
			(layer "F.SilkS")
		)
		(property "Value" "Screw_Terminal_01x02"
			(at 2.5 5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 -4.1 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 2 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.125)
			(net 4 "Net-(ADC0-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 5 0)
			(size 2 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(ADC1-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBVA_2,5_2-G_1x02_P5.00mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_THT:D_A-405_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 108.5 90.375 90)
		(descr "Diode, A-405 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
		(tags "Diode A-405 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
		(property "Reference" "D21"
			(at 5.464666 -0.039072 90)
			(layer "F.SilkS")
		)
		(property "Value" "BZW06-15"
			(at 5.08 2.244 90)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Schottky diode"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at 0 -1.9 90)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 5.47 0 90)
			(layer "F.Fab")
		)
		(fp_text user "K"
			(at 0 -1.9 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "Net-(D21-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(12V0-Pin_2)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_THT.3dshapes/D_A-405_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:Drahtbrücke_14mm"
		(layer "F.Cu")
		(at 67.681368 63.38123 -90)
		(property "Reference" "R25"
			(at 3 -8.5 270)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0R"
			(at 1.25 -7 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 2.54 2.54)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(ADC0-Pin_1)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 10 -10 270)
			(size 2.54 2.54)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(ADC0-Pin_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_THT:C_Axial_L5.1mm_D3.1mm_P7.50mm_Horizontal"
		(layer "F.Cu")
		(at 50.286 60.96 180)
		(descr "C, Axial series, Axial, Horizontal, pin pitch=7.5mm, , length*diameter=5.1*3.1mm^2, http://www.vishay.com/docs/45231/arseries.pdf")
		(tags "C Axial series Axial Horizontal pin pitch 7.5mm  length 5.1mm diameter 3.1mm")
		(property "Reference" "C1"
			(at 3.75 -2.67 0)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 3.75 2.67 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.75 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(D5-K)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.5 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(12V0-Pin_2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Axial_L5.1mm_D3.1mm_P7.50mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 83.566 33.274 180)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R23"
			(at 5.334 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "1K"
			(at 2.032 0 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.334 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(ADC0-Pin_1)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 72 "Net-(Vin0-Pin_11)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-220-3_Vertical"
		(layer "F.Cu")
		(at 102 87.376 90)
		(descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
		(tags "TO-220-3 Vertical RM 2.54mm")
		(property "Reference" "Q6"
			(at 8.89 -0.945 0)
			(layer "F.SilkS")
		)
		(property "Value" "IRLZ44N"
			(at 2.391353 2.18544 90)
			(layer "F.SilkS")
		)
		(property "Datasheet" "http://www.irf.com/product-info/datasheets/data/irlz44n.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "47A Id, 55V Vds, 22mOhm Rds Single N-Channel HEXFET Power MOSFET, TO-220AB"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO?220*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 8.89 -0.945 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "Net-(D14-K)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 90)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "Net-(D21-K)")
			(pinfunction "D")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 5.08 0 90)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(12V0-Pin_2)")
			(pinfunction "S")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinSocket_2.54mm:PinSocket_1x15_P2.54mm_Vertical"
		(locked yes)
		(layer "F.Cu")
		(at 86.868 62.992 180)
		(descr "Through hole straight socket strip, 1x15, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x15 2.54mm single row")
		(property "Reference" "TX0"
			(at 0 -2.77 180)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x15_Socket"
			(at 0 38.33 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x15, script generated"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 17.78 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "Net-(Serial0-Pin_3)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 65 "Net-(Serial0-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 67 "unconnected-(TX0-Pin_3-Pad3)")
			(pinfunction "Pin_3")
			(pintype "passive+no_connect")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(12V0-Pin_2)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "Net-(Q4-G)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 0 12.7 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "Net-(D24-K)")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 15.24 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "Net-(Q3-G)")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 0 17.78 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 59 "Net-(TX0-Pin_8)")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 0 20.32 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "Net-(TX0-Pin_9)")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole oval
			(at 0 22.86 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "Net-(Q2-G)")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole oval
			(at 0 25.4 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "Net-(Q1-G)")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole oval
			(at 0 27.94 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "Net-(TX0-Pin_12)")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" thru_hole oval
			(at 0 30.48 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "Net-(TX0-Pin_13)")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" thru_hole oval
			(at 0 33.02 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "Net-(TX0-Pin_14)")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(pad "15" thru_hole oval
			(at 0 35.56 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "Net-(D25-K)")
			(pinfunction "Pin_15")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x15_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 68.072 155.448 90)
		(descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
		(tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
		(property "Reference" "D4"
			(at 3.81 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "1N4148"
			(at 3.81 2.54 90)
			(layer "F.SilkS")
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/1N4148_1N4448.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "100V 0.15A standard switching diode, DO-35"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*DO?35*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at 0 -1.8 90)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 4.11 0 90)
			(layer "F.Fab")
		)
		(fp_text user "K"
			(at 0 -1.8 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(D1-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "Net-(D4-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_THT:LED_D5.0mm"
		(layer "F.Cu")
		(at 115.151866 143.715 90)
		(descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf, generated by kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D13"
			(at 1.275 -3.899866 90)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 1.27 5.08 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "Net-(D13-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 90)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "Net-(D13-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 83.566 27.178 180)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R22"
			(at 5.334 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "1K"
			(at 2.286 0 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.334 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(ADC0-Pin_1)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 71 "Net-(Vin0-Pin_12)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_THT:D_DO-41_SOD81_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 108.5 120.396 180)
		(descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
		(tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
		(property "Reference" "D18"
			(at 4.204735 0.029325 0)
			(layer "F.SilkS")
		)
		(property "Value" "1N4733"
			(at 11.938 0 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Zener diode"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at 0 -2.1 0)
			(layer "F.SilkS")
		)
		(fp_text user "K"
			(at 0 -2.1 0)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 4.2 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 2.2 2.2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "Net-(D18-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 180)
			(size 2.2 2.2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(12V0-Pin_2)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_THT:D_A-405_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 108.5 155.448 90)
		(descr "Diode, A-405 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
		(tags "Diode A-405 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
		(property "Reference" "D20"
			(at 5.497747 -0.000001 90)
			(layer "F.SilkS")
		)
		(property "Value" "BZW06-15"
			(at 5.08 2.54 90)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Schottky diode"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at 0 -1.9 90)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 5.47 0 90)
			(layer "F.Fab")
		)
		(fp_text user "K"
			(at 0 -1.9 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Net-(D20-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(12V0-Pin_2)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_THT.3dshapes/D_A-405_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Phoenix_MSTB:PhoenixContact_MSTBVA_2,5_2-G_1x02_P5.00mm_Vertical"
		(layer "F.Cu")
		(at 30.316 26.6375)
		(descr "Generic Phoenix Contact connector footprint for: MSTBVA_2,5/2-G; number of pins: 02; pin pitch: 5.00mm; Vertical || order number: 1755516 12A || order number: 1924198 16A (HC)")
		(tags "phoenix_contact connector MSTBVA_01x02_G_5.00mm")
		(property "Reference" "12V0"
			(at 2.5 -6 0)
			(layer "F.SilkS")
		)
		(property "Value" "Screw_Terminal_01x02"
			(at 2.5 5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 -4.1 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 2 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.125)
			(net 3 "Net-(12V0-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 5 0)
			(size 2 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(12V0-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBVA_2,5_2-G_1x02_P5.00mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 101 139.192)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R14"
			(at 3.81 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "300R"
			(at -3.302 0 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Nano Universal.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "Net-(TX0-Pin_12)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "Net-(D13-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_rect
		(start 17 16)
		(end 130 171)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_text "GND SIG"
		(at 74.676 71.628 0)
		(layer "F.SilkS")
	)
	(gr_text "GND SIG"
		(at 110.236 21.844 0)
		(layer "F.SilkS")
	)
	(gr_text "0-15V"
		(at 76.2 86.868 0)
		(layer "F.SilkS")
	)
	(gr_text "SIG GND"
		(at 125.984 36.576 90)
		(layer "F.SilkS")
	)
	(gr_text "JLCJLCJLCJLC"
		(at 35.56 153.924 0)
		(layer "F.SilkS")
	)
	(gr_text "GND SIG"
		(at 96.012 21.844 0)
		(layer "F.SilkS")
	)
	(gr_text "+  -"
		(at 41.148 20.32 0)
		(layer "F.SilkS")
	)
	(gr_text "+  -"
		(at 28.448 20.828 0)
		(layer "F.SilkS")
	)
	(gr_text "SIG GND"
		(at 125.984 52.832 90)
		(layer "F.SilkS")
	)
	(gr_text "GND SIG"
		(at 74.676 157.988 0)
		(layer "F.SilkS")
	)
	(gr_text "TX  RX  GND"
		(at 94.996 49.784 90)
		(layer "F.SilkS")
	)
	(gr_text "Nano Universal Power Board by Bastian Schilling\nRev 1.2"
		(at 30.48 168.148 0)
		(layer "F.SilkS")
	)
	(gr_text "GND SIG"
		(at 74.676 114.808 0)
		(layer "F.SilkS")
	)
	(gr_text "0-5V"
		(at 76.2 129.032 0)
		(layer "F.SilkS")
	)
	(dimension
		(type orthogonal)
		(layer "F.SilkS")
		(pts
			(xy 22.46 166.016) (xy 124.46 166.016)
		)
		(height 4.164)
		(orientation 0)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 0)
			(precision 4)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 2)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "102"
			(at 73.62 169.164 0)
			(layer "F.SilkS")
		)
	)
	(dimension
		(type orthogonal)
		(layer "F.SilkS")
		(pts
			(xy 124.5 21) (xy 124.5 166)
		)
		(height 3.77)
		(orientation 1)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 0)
			(precision 4)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "145"
			(at 127.17 93.5 90)
			(layer "F.SilkS")
		)
	)
	(embedded_fonts no)
)
