(footprint 629722000214 (layer F.Cu) (tedit 6823B148)
  (descr "")
  (attr smd)
  (fp_text reference REF** (at 0.0 -6.815 0) (layer F.SilkS))
  (fp_text value 629722000214 (at 0.0 4.185 0) (layer F.Fab))
  (pad S1 thru_hole circle (at -4.32 -4.18) (size 1.0 1.0) (drill 0.6) (layers *.Cu))
  (pad S2 thru_hole circle (at 4.32 -4.18) (size 1.0 1.0) (drill 0.6) (layers *.Cu))
  (pad S3 thru_hole circle (at -4.32 0.0) (size 1.0 1.0) (drill 0.6) (layers *.Cu))
  (pad S4 thru_hole circle (at 4.32 0.0) (size 1.0 1.0) (drill 0.6) (layers *.Cu))
  (pad A1 smd custom (at -3.35 -4.745) (size 0.3 1.15) (layers F.Cu) (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly
        (pts
          (xy -0.15 -0.575)
          (xy -0.15 0.575)
          (xy 0.45 0.575)
          (xy 0.45 -0.575)
        ) (width 0.01)
      )
    )
  )
  (pad B12 smd rect (at -3.05 -4.745) (size 0.3 1.15) (layers F.Cu))
  (pad A4 smd custom (at -2.55 -4.745) (size 0.3 1.15) (layers F.Cu) (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly
        (pts
          (xy -0.15 -0.575)
          (xy -0.15 0.575)
          (xy 0.45 0.575)
          (xy 0.45 -0.575)
        ) (width 0.01)
      )
    )
  )
  (pad B9 smd rect (at -2.25 -4.745) (size 0.3 1.15) (layers F.Cu))
  (pad B8 smd rect (at -1.75 -4.745) (size 0.3 1.15) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad A5 smd rect (at -1.25 -4.745) (size 0.3 1.15) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad B7 smd rect (at -0.75 -4.745) (size 0.3 1.15) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad A6 smd rect (at -0.25 -4.745) (size 0.3 1.15) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad A7 smd rect (at 0.25 -4.745) (size 0.3 1.15) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad B6 smd rect (at 0.75 -4.745) (size 0.3 1.15) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad A8 smd rect (at 1.25 -4.745) (size 0.3 1.15) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad B5 smd rect (at 1.75 -4.745) (size 0.3 1.15) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad A12 smd custom (at 3.35 -4.745) (size 0.3 1.15) (layers F.Cu) (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly
        (pts
          (xy -0.45 -0.575)
          (xy -0.45 0.575)
          (xy 0.15 0.575)
          (xy 0.15 -0.575)
        ) (width 0.01)
      )
    )
  )
  (pad B1 smd rect (at 3.05 -4.745) (size 0.3 1.15) (layers F.Cu))
  (pad A9 smd custom (at 2.55 -4.745) (size 0.3 1.15) (layers F.Cu) (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly
        (pts
          (xy -0.45 -0.575)
          (xy -0.45 0.575)
          (xy 0.15 0.575)
          (xy 0.15 -0.575)
        ) (width 0.01)
      )
    )
  )
  (pad B4 smd rect (at 2.25 -4.745) (size 0.3 1.15) (layers F.Cu))
  (pad None np_thru_hole circle (at -2.89 -3.68) (size 0.65 0.65) (drill 0.65) (layers *.Cu *.Mask))
  (pad None np_thru_hole circle (at 2.89 -3.68) (size 0.65 0.65) (drill 0.65) (layers *.Cu *.Mask))
  (fp_text user "Product Edge" (at 0.0 2.22) (layer Dwgs.User))
  (fp_text user "PCB Cutout Area" (at 4.3 -4.18) (layer Dwgs.User))
  (fp_text user "Milling Layer the hole size should  follow the Milling Layer" (at 5.6 0.42) (layer Dwgs.User))
  (fp_text user "PCB Cutout Area" (at 4.3 -4.18) (layer Edge.Cuts))
  (fp_text user "PCB Cutout Area" (at -4.3 -4.18) (layer Dwgs.User))
  (fp_text user "PCB Cutout Area" (at -4.3 -4.18) (layer Edge.Cuts))
  (fp_text user "PCB Cutout Area" (at -4.3 0.02) (layer Dwgs.User))
  (fp_text user "PCB Cutout Area" (at -4.3 0.02) (layer Edge.Cuts))
  (fp_text user "PCB Cutout Area" (at 4.3 0.02) (layer Dwgs.User))
  (fp_text user "PCB Cutout Area" (at 4.3 0.02) (layer Edge.Cuts))
  (fp_arc (start -4.32 -3.63) (end -4.62 -3.63) (angle -180.0) (layer Edge.Cuts) (width 0.01))
  (fp_line (start -4.62 -3.63) (end -4.62 -4.73) (layer Edge.Cuts) (width 0.01))
  (fp_arc (start -4.32 -4.73) (end -4.02 -4.73) (angle -180.0) (layer Edge.Cuts) (width 0.01))
  (fp_line (start -4.02 -4.73) (end -4.02 -3.63) (layer Edge.Cuts) (width 0.01))
  (fp_arc (start 4.32 -3.63) (end 4.62 -3.63) (angle 180.0) (layer Edge.Cuts) (width 0.01))
  (fp_line (start 4.62 -3.63) (end 4.62 -4.73) (layer Edge.Cuts) (width 0.01))
  (fp_arc (start 4.32 -4.73) (end 4.02 -4.73) (angle 180.0) (layer Edge.Cuts) (width 0.01))
  (fp_line (start 4.02 -4.73) (end 4.02 -3.63) (layer Edge.Cuts) (width 0.01))
  (fp_arc (start -4.32 0.4) (end -4.62 0.4) (angle -180.0) (layer Edge.Cuts) (width 0.01))
  (fp_line (start -4.62 0.4) (end -4.62 -0.4) (layer Edge.Cuts) (width 0.01))
  (fp_arc (start -4.32 -0.4) (end -4.02 -0.4) (angle -180.0) (layer Edge.Cuts) (width 0.01))
  (fp_line (start -4.02 -0.4) (end -4.02 0.4) (layer Edge.Cuts) (width 0.01))
  (fp_arc (start 4.32 0.4) (end 4.62 0.4) (angle 180.0) (layer Edge.Cuts) (width 0.01))
  (fp_line (start 4.62 0.4) (end 4.62 -0.4) (layer Edge.Cuts) (width 0.01))
  (fp_arc (start 4.32 -0.4) (end 4.02 -0.4) (angle 180.0) (layer Edge.Cuts) (width 0.01))
  (fp_line (start 4.02 -0.4) (end 4.02 0.4) (layer Edge.Cuts) (width 0.01))
)