(footprint "NETTIE4_CLOSE_THT"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Just a \"Net tie\" as an more or less elegant way to connect two different nets without disturbing ERC and DRC.")
	(tags "Just a \"Net tie\" as an more or less elegant way to connect two different nets without disturbing ERC and DRC.")
	(property "Reference" "REF**"
		(at 0 -1.905 0)
		(layer "F.SilkS")
		(hide yes)
	)
	(property "Value" "NETTIE4_CLOSE_THT"
		(at 0 1.905 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr exclude_from_pos_files exclude_from_bom)
	(pad "1" smd circle
		(at -5.08 0)
		(size 2 2)
		(layers "F.Cu")
	)
	(pad "2" smd circle
		(at 5.08 0)
		(size 2 2)
		(layers "B.Cu")
	)
	(pad "3" thru_hole circle
		(at 0 0)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.SilkS")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
)
