<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<library>
<description>Tubes devices</description>
<packages>
<package name="OKTAL">
</package>
<package name="NOVAL">
</package>
</packages>
<symbols>
<symbol name="HEATER_2">
<pin name="H1" direction="pas"/>
<pin name="H2" direction="pas"/>
<pin name="H3" direction="pas"/>
</symbol>
<symbol name="TRIODE">
<pin name="TA" direction="pas"/>
<pin name="TG" direction="pas"/>
<pin name="TK" direction="pas"/>
</symbol>
<symbol name="PENTODE">
<pin name="PSG" direction="pas"/>
<pin name="PG" direction="pas"/>
<pin name="PA" direction="pas"/>
<pin name="PK" direction="pas"/>
</symbol>
<symbol name="PENTODE/">
<pin name="PSG" direction="pas"/>
<pin name="PG" direction="pas"/>
<pin name="PA" direction="pas"/>
<pin name="PK" direction="pas"/>
<pin name="PBG" direction="pas"/>
</symbol>
<symbol name="HEATER_1">
<pin name="H1" direction="pas"/>
<pin name="H2" direction="pas"/>
</symbol>
<symbol name="PENT/">
</symbol>
<symbol name="PENT//">
</symbol>
<symbol name="HEAT/1">
</symbol>
<symbol name="HEAT/2">
</symbol>
</symbols>
<devicesets>
<deviceset name="6550A-P" prefix="V" uservalue="yes">
<gates>
<gate name="G$1" symbol="PENTODE"/>
<gate name="&quot;" symbol="HEATER_1"/>
</gates>
<devices>
<device name="" package="OKTAL">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ECL86-P" prefix="V" uservalue="yes">
<gates>
<gate name="A" symbol="PENTODE"/>
<gate name="B" symbol="TRIODE"/>
<gate name="&quot;" symbol="HEATER_1"/>
</gates>
<devices>
<device name="" package="NOVAL">
<connects>
<connect gate="&quot;" pin="H1" pad="4"/>
<connect gate="&quot;" pin="H2" pad="5"/>
<connect gate="A" pin="PA" pad="6"/>
<connect gate="A" pin="PG" pad="8"/>
<connect gate="A" pin="PK" pad="7"/>
<connect gate="A" pin="PSG" pad="3"/>
<connect gate="B" pin="TA" pad="9"/>
<connect gate="B" pin="TG" pad="1"/>
<connect gate="B" pin="TK" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EL34-P" prefix="V" uservalue="yes">
<gates>
<gate name="G$1" symbol="PENTODE/"/>
<gate name="&quot;" symbol="HEATER_1"/>
</gates>
<devices>
<device name="" package="OKTAL">
<connects>
<connect gate="&quot;" pin="H1" pad="2"/>
<connect gate="&quot;" pin="H2" pad="7"/>
<connect gate="G$1" pin="PA" pad="3"/>
<connect gate="G$1" pin="PBG" pad="1"/>
<connect gate="G$1" pin="PG" pad="5"/>
<connect gate="G$1" pin="PK" pad="8"/>
<connect gate="G$1" pin="PSG" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EL84-P" prefix="V" uservalue="yes">
<gates>
<gate name="G$1" symbol="PENTODE"/>
<gate name="&quot;" symbol="HEATER_1"/>
</gates>
<devices>
<device name="" package="NOVAL">
<connects>
<connect gate="&quot;" pin="H1" pad="4"/>
<connect gate="&quot;" pin="H2" pad="5"/>
<connect gate="G$1" pin="PA" pad="7"/>
<connect gate="G$1" pin="PG" pad="2"/>
<connect gate="G$1" pin="PK" pad="3"/>
<connect gate="G$1" pin="PSG" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EF86-P" prefix="V" uservalue="yes">
<gates>
<gate name="G$1" symbol="PENTODE/"/>
<gate name="&quot;" symbol="HEATER_1"/>
</gates>
<devices>
<device name="" package="NOVAL">
<connects>
<connect gate="&quot;" pin="H1" pad="4"/>
<connect gate="&quot;" pin="H2" pad="5"/>
<connect gate="G$1" pin="PA" pad="6"/>
<connect gate="G$1" pin="PBG" pad="8"/>
<connect gate="G$1" pin="PG" pad="9"/>
<connect gate="G$1" pin="PK" pad="3"/>
<connect gate="G$1" pin="PSG" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ECL82-P" prefix="V" uservalue="yes">
<gates>
<gate name="A" symbol="PENTODE"/>
<gate name="B" symbol="TRIODE"/>
<gate name="&quot;" symbol="HEATER_1"/>
</gates>
<devices>
<device name="" package="NOVAL">
<connects>
<connect gate="&quot;" pin="H1" pad="4"/>
<connect gate="&quot;" pin="H2" pad="5"/>
<connect gate="A" pin="PA" pad="6"/>
<connect gate="A" pin="PG" pad="3"/>
<connect gate="A" pin="PK" pad="2"/>
<connect gate="A" pin="PSG" pad="7"/>
<connect gate="B" pin="TA" pad="9"/>
<connect gate="B" pin="TG" pad="1"/>
<connect gate="B" pin="TK" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ECC82-P" prefix="V" uservalue="yes">
<gates>
<gate name="A" symbol="TRIODE"/>
<gate name="B" symbol="TRIODE"/>
<gate name="&quot;" symbol="HEATER_2"/>
</gates>
<devices>
<device name="" package="NOVAL">
<connects>
<connect gate="&quot;" pin="H1" pad="4"/>
<connect gate="&quot;" pin="H2" pad="9"/>
<connect gate="&quot;" pin="H3" pad="5"/>
<connect gate="A" pin="TA" pad="1"/>
<connect gate="A" pin="TG" pad="2"/>
<connect gate="A" pin="TK" pad="3"/>
<connect gate="B" pin="TA" pad="6"/>
<connect gate="B" pin="TG" pad="7"/>
<connect gate="B" pin="TK" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ECC81-P" prefix="V" uservalue="yes">
<gates>
<gate name="A" symbol="TRIODE"/>
<gate name="B" symbol="TRIODE"/>
<gate name="&quot;" symbol="HEATER_2"/>
</gates>
<devices>
<device name="" package="NOVAL">
<connects>
<connect gate="&quot;" pin="H1" pad="4"/>
<connect gate="&quot;" pin="H2" pad="9"/>
<connect gate="&quot;" pin="H3" pad="5"/>
<connect gate="A" pin="TA" pad="1"/>
<connect gate="A" pin="TG" pad="2"/>
<connect gate="A" pin="TK" pad="3"/>
<connect gate="B" pin="TA" pad="6"/>
<connect gate="B" pin="TG" pad="7"/>
<connect gate="B" pin="TK" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="KT77-P" prefix="V" uservalue="yes">
<gates>
<gate name="G$1" symbol="PENTODE/"/>
<gate name="&quot;" symbol="HEATER_1"/>
</gates>
<devices>
<device name="" package="OKTAL">
<connects>
<connect gate="&quot;" pin="H1" pad="2"/>
<connect gate="&quot;" pin="H2" pad="7"/>
<connect gate="G$1" pin="PA" pad="3"/>
<connect gate="G$1" pin="PBG" pad="1"/>
<connect gate="G$1" pin="PG" pad="5"/>
<connect gate="G$1" pin="PK" pad="8"/>
<connect gate="G$1" pin="PSG" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="KT66-P" prefix="V" uservalue="yes">
<gates>
<gate name="G$1" symbol="PENTODE"/>
<gate name="&quot;" symbol="HEATER_1"/>
</gates>
<devices>
<device name="" package="OKTAL">
<connects>
<connect gate="&quot;" pin="H1" pad="2"/>
<connect gate="&quot;" pin="H2" pad="7"/>
<connect gate="G$1" pin="PA" pad="3"/>
<connect gate="G$1" pin="PG" pad="5"/>
<connect gate="G$1" pin="PK" pad="8"/>
<connect gate="G$1" pin="PSG" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ECC808-P" prefix="V" uservalue="yes">
<gates>
<gate name="A" symbol="TRIODE"/>
<gate name="B" symbol="TRIODE"/>
<gate name="&quot;" symbol="HEATER_1"/>
</gates>
<devices>
<device name="" package="NOVAL">
<connects>
<connect gate="&quot;" pin="H1" pad="1"/>
<connect gate="&quot;" pin="H2" pad="2"/>
<connect gate="A" pin="TA" pad="6"/>
<connect gate="A" pin="TG" pad="5"/>
<connect gate="A" pin="TK" pad="4"/>
<connect gate="B" pin="TA" pad="7"/>
<connect gate="B" pin="TG" pad="8"/>
<connect gate="B" pin="TK" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCL805-P" prefix="V" uservalue="yes">
<gates>
<gate name="A" symbol="PENTODE"/>
<gate name="B" symbol="TRIODE"/>
<gate name="&quot;" symbol="HEATER_1"/>
</gates>
<devices>
<device name="" package="NOVAL">
<connects>
<connect gate="&quot;" pin="H1" pad="6"/>
<connect gate="&quot;" pin="H2" pad="5"/>
<connect gate="A" pin="PA" pad="4"/>
<connect gate="A" pin="PG" pad="1"/>
<connect gate="A" pin="PK" pad="2"/>
<connect gate="A" pin="PSG" pad="3"/>
<connect gate="B" pin="TA" pad="9"/>
<connect gate="B" pin="TG" pad="8"/>
<connect gate="B" pin="TK" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ECC83-P" prefix="V" uservalue="yes">
<gates>
<gate name="A" symbol="TRIODE"/>
<gate name="B" symbol="TRIODE"/>
<gate name="&quot;" symbol="HEATER_2"/>
</gates>
<devices>
<device name="" package="NOVAL">
<connects>
<connect gate="&quot;" pin="H1" pad="4"/>
<connect gate="&quot;" pin="H2" pad="9"/>
<connect gate="&quot;" pin="H3" pad="5"/>
<connect gate="A" pin="TA" pad="1"/>
<connect gate="A" pin="TG" pad="2"/>
<connect gate="A" pin="TK" pad="3"/>
<connect gate="B" pin="TA" pad="6"/>
<connect gate="B" pin="TG" pad="7"/>
<connect gate="B" pin="TK" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="KT88-P" prefix="V" uservalue="yes">
<gates>
<gate name="G$1" symbol="PENTODE"/>
<gate name="&quot;" symbol="HEATER_1"/>
</gates>
<devices>
<device name="" package="OKTAL">
<connects>
<connect gate="&quot;" pin="H1" pad="7"/>
<connect gate="&quot;" pin="H2" pad="2"/>
<connect gate="G$1" pin="PA" pad="6"/>
<connect gate="G$1" pin="PG" pad="4"/>
<connect gate="G$1" pin="PK" pad="1"/>
<connect gate="G$1" pin="PSG" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6SN7GT-P" prefix="V" uservalue="yes">
<gates>
<gate name="A" symbol="TRIODE"/>
<gate name="B" symbol="TRIODE"/>
<gate name="&quot;" symbol="HEATER_1"/>
</gates>
<devices>
<device name="" package="OKTAL">
<connects>
<connect gate="&quot;" pin="H1" pad="7"/>
<connect gate="&quot;" pin="H2" pad="8"/>
<connect gate="A" pin="TA" pad="2"/>
<connect gate="A" pin="TG" pad="1"/>
<connect gate="A" pin="TK" pad="3"/>
<connect gate="B" pin="TA" pad="5"/>
<connect gate="B" pin="TG" pad="4"/>
<connect gate="B" pin="TK" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6BL7GT-P" prefix="V" uservalue="yes">
<gates>
<gate name="A" symbol="TRIODE"/>
<gate name="B" symbol="TRIODE"/>
<gate name="&quot;" symbol="HEATER_1"/>
</gates>
<devices>
<device name="" package="OKTAL">
<connects>
<connect gate="&quot;" pin="H1" pad="7"/>
<connect gate="&quot;" pin="H2" pad="8"/>
<connect gate="A" pin="TA" pad="2"/>
<connect gate="A" pin="TG" pad="1"/>
<connect gate="A" pin="TK" pad="3"/>
<connect gate="B" pin="TA" pad="5"/>
<connect gate="B" pin="TG" pad="4"/>
<connect gate="B" pin="TK" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6AS7G-P" prefix="V" uservalue="yes">
<gates>
<gate name="A" symbol="TRIODE"/>
<gate name="B" symbol="TRIODE"/>
<gate name="&quot;" symbol="HEATER_1"/>
</gates>
<devices>
<device name="" package="OKTAL">
<connects>
<connect gate="&quot;" pin="H1" pad="7"/>
<connect gate="&quot;" pin="H2" pad="8"/>
<connect gate="A" pin="TA" pad="2"/>
<connect gate="A" pin="TG" pad="1"/>
<connect gate="A" pin="TK" pad="3"/>
<connect gate="B" pin="TA" pad="5"/>
<connect gate="B" pin="TG" pad="4"/>
<connect gate="B" pin="TK" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6DJ8-P" prefix="V" uservalue="yes">
<gates>
<gate name="A" symbol="TRIODE"/>
<gate name="B" symbol="TRIODE"/>
<gate name="&quot;" symbol="HEATER_2"/>
</gates>
<devices>
<device name="" package="NOVAL">
<connects>
<connect gate="&quot;" pin="H1" pad="4"/>
<connect gate="&quot;" pin="H2" pad="9"/>
<connect gate="&quot;" pin="H3" pad="5"/>
<connect gate="A" pin="TA" pad="1"/>
<connect gate="A" pin="TG" pad="2"/>
<connect gate="A" pin="TK" pad="3"/>
<connect gate="B" pin="TA" pad="6"/>
<connect gate="B" pin="TG" pad="7"/>
<connect gate="B" pin="TK" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6N1P-P" prefix="V" uservalue="yes">
<gates>
<gate name="A" symbol="TRIODE"/>
<gate name="B" symbol="TRIODE"/>
<gate name="&quot;" symbol="HEATER_2"/>
</gates>
<devices>
<device name="" package="NOVAL">
<connects>
<connect gate="&quot;" pin="H1" pad="4"/>
<connect gate="&quot;" pin="H2" pad="9"/>
<connect gate="&quot;" pin="H3" pad="5"/>
<connect gate="A" pin="TA" pad="1"/>
<connect gate="A" pin="TG" pad="2"/>
<connect gate="A" pin="TK" pad="3"/>
<connect gate="B" pin="TA" pad="6"/>
<connect gate="B" pin="TG" pad="7"/>
<connect gate="B" pin="TK" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="12BH7-P" prefix="V" uservalue="yes">
<gates>
<gate name="A" symbol="TRIODE"/>
<gate name="B" symbol="TRIODE"/>
<gate name="&quot;" symbol="HEATER_2"/>
</gates>
<devices>
<device name="" package="NOVAL">
<connects>
<connect gate="&quot;" pin="H1" pad="4"/>
<connect gate="&quot;" pin="H2" pad="9"/>
<connect gate="&quot;" pin="H3" pad="5"/>
<connect gate="A" pin="TA" pad="1"/>
<connect gate="A" pin="TG" pad="2"/>
<connect gate="A" pin="TK" pad="3"/>
<connect gate="B" pin="TA" pad="6"/>
<connect gate="B" pin="TG" pad="7"/>
<connect gate="B" pin="TK" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="12DW7-P" prefix="V" uservalue="yes">
<gates>
<gate name="A" symbol="TRIODE"/>
<gate name="B" symbol="TRIODE"/>
<gate name="&quot;" symbol="HEATER_2"/>
</gates>
<devices>
<device name="" package="NOVAL">
<connects>
<connect gate="&quot;" pin="H1" pad="4"/>
<connect gate="&quot;" pin="H2" pad="9"/>
<connect gate="&quot;" pin="H3" pad="5"/>
<connect gate="A" pin="TA" pad="1"/>
<connect gate="A" pin="TG" pad="2"/>
<connect gate="A" pin="TK" pad="3"/>
<connect gate="B" pin="TA" pad="6"/>
<connect gate="B" pin="TG" pad="7"/>
<connect gate="B" pin="TK" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7247-P" prefix="V" uservalue="yes">
<gates>
<gate name="A" symbol="TRIODE"/>
<gate name="B" symbol="TRIODE"/>
<gate name="&quot;" symbol="HEATER_2"/>
</gates>
<devices>
<device name="" package="NOVAL">
<connects>
<connect gate="&quot;" pin="H1" pad="4"/>
<connect gate="&quot;" pin="H2" pad="9"/>
<connect gate="&quot;" pin="H3" pad="5"/>
<connect gate="A" pin="TA" pad="1"/>
<connect gate="A" pin="TG" pad="2"/>
<connect gate="A" pin="TK" pad="3"/>
<connect gate="B" pin="TA" pad="6"/>
<connect gate="B" pin="TG" pad="7"/>
<connect gate="B" pin="TK" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="5879-P" prefix="V" uservalue="yes">
<gates>
<gate name="G$1" symbol="PENTODE/"/>
<gate name="&quot;" symbol="HEATER_1"/>
</gates>
<devices>
<device name="" package="NOVAL">
<connects>
<connect gate="&quot;" pin="H1" pad="4"/>
<connect gate="&quot;" pin="H2" pad="5"/>
<connect gate="G$1" pin="PA" pad="8"/>
<connect gate="G$1" pin="PBG" pad="9"/>
<connect gate="G$1" pin="PG" pad="1"/>
<connect gate="G$1" pin="PK" pad="3"/>
<connect gate="G$1" pin="PSG" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="5881-P" prefix="V" uservalue="yes">
<gates>
<gate name="G$1" symbol="PENTODE"/>
<gate name="&quot;" symbol="HEATER_1"/>
</gates>
<devices>
<device name="" package="OKTAL">
<connects>
<connect gate="&quot;" pin="H1" pad="2"/>
<connect gate="&quot;" pin="H2" pad="7"/>
<connect gate="G$1" pin="PA" pad="3"/>
<connect gate="G$1" pin="PG" pad="5"/>
<connect gate="G$1" pin="PK" pad="8"/>
<connect gate="G$1" pin="PSG" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6AN8-P" prefix="V" uservalue="yes">
<gates>
<gate name="A" symbol="TRIODE"/>
<gate name="B" symbol="PENTODE"/>
<gate name="&quot;" symbol="HEATER_1"/>
</gates>
<devices>
<device name="" package="NOVAL">
<connects>
<connect gate="&quot;" pin="H1" pad="4"/>
<connect gate="&quot;" pin="H2" pad="5"/>
<connect gate="A" pin="TA" pad="1"/>
<connect gate="A" pin="TG" pad="2"/>
<connect gate="A" pin="TK" pad="3"/>
<connect gate="B" pin="PA" pad="6"/>
<connect gate="B" pin="PG" pad="8"/>
<connect gate="B" pin="PK" pad="9"/>
<connect gate="B" pin="PSG" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6C5GT-P" prefix="V" uservalue="yes">
<gates>
<gate name="G$1" symbol="PENTODE"/>
<gate name="&quot;" symbol="HEATER_1"/>
</gates>
<devices>
<device name="" package="OKTAL">
<connects>
<connect gate="&quot;" pin="H1" pad="2"/>
<connect gate="&quot;" pin="H2" pad="7"/>
<connect gate="G$1" pin="PA" pad="3"/>
<connect gate="G$1" pin="PG" pad="5"/>
<connect gate="G$1" pin="PK" pad="8"/>
<connect gate="G$1" pin="PSG" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6CG7-P" prefix="V" uservalue="yes">
<gates>
<gate name="A" symbol="TRIODE"/>
<gate name="B" symbol="TRIODE"/>
<gate name="&quot;" symbol="HEATER_2"/>
</gates>
<devices>
<device name="" package="NOVAL">
<connects>
<connect gate="&quot;" pin="H1" pad="4"/>
<connect gate="&quot;" pin="H2" pad="9"/>
<connect gate="&quot;" pin="H3" pad="5"/>
<connect gate="A" pin="TA" pad="1"/>
<connect gate="A" pin="TG" pad="2"/>
<connect gate="A" pin="TK" pad="3"/>
<connect gate="B" pin="TA" pad="6"/>
<connect gate="B" pin="TG" pad="7"/>
<connect gate="B" pin="TK" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6FQ7-P" prefix="V" uservalue="yes">
<gates>
<gate name="A" symbol="TRIODE"/>
<gate name="B" symbol="TRIODE"/>
<gate name="&quot;" symbol="HEATER_2"/>
</gates>
<devices>
<device name="" package="NOVAL">
<connects>
<connect gate="&quot;" pin="H1" pad="4"/>
<connect gate="&quot;" pin="H2" pad="9"/>
<connect gate="&quot;" pin="H3" pad="5"/>
<connect gate="A" pin="TA" pad="1"/>
<connect gate="A" pin="TG" pad="2"/>
<connect gate="A" pin="TK" pad="3"/>
<connect gate="B" pin="TA" pad="6"/>
<connect gate="B" pin="TG" pad="7"/>
<connect gate="B" pin="TK" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6EU7-P" prefix="V" uservalue="yes">
<gates>
<gate name="A" symbol="TRIODE"/>
<gate name="B" symbol="TRIODE"/>
<gate name="&quot;" symbol="HEATER_1"/>
</gates>
<devices>
<device name="" package="NOVAL">
<connects>
<connect gate="&quot;" pin="H1" pad="1"/>
<connect gate="&quot;" pin="H2" pad="2"/>
<connect gate="A" pin="TA" pad="6"/>
<connect gate="A" pin="TG" pad="5"/>
<connect gate="A" pin="TK" pad="4"/>
<connect gate="B" pin="TA" pad="7"/>
<connect gate="B" pin="TG" pad="8"/>
<connect gate="B" pin="TK" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6F6GT-P" prefix="V" uservalue="yes">
<gates>
<gate name="G$1" symbol="PENTODE"/>
<gate name="&quot;" symbol="HEATER_1"/>
</gates>
<devices>
<device name="" package="OKTAL">
<connects>
<connect gate="&quot;" pin="H1" pad="2"/>
<connect gate="&quot;" pin="H2" pad="7"/>
<connect gate="G$1" pin="PA" pad="3"/>
<connect gate="G$1" pin="PG" pad="5"/>
<connect gate="G$1" pin="PK" pad="8"/>
<connect gate="G$1" pin="PSG" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6J5-P" prefix="V" uservalue="yes">
<gates>
<gate name="G$1" symbol="TRIODE"/>
<gate name="&quot;" symbol="HEATER_1"/>
</gates>
<devices>
<device name="" package="OKTAL">
<connects>
<connect gate="&quot;" pin="H1" pad="2"/>
<connect gate="&quot;" pin="H2" pad="7"/>
<connect gate="G$1" pin="TA" pad="3"/>
<connect gate="G$1" pin="TG" pad="5"/>
<connect gate="G$1" pin="TK" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6K6GT-P" prefix="V" uservalue="yes">
<gates>
<gate name="G$1" symbol="PENTODE"/>
<gate name="&quot;" symbol="HEATER_1"/>
</gates>
<devices>
<device name="" package="OKTAL">
<connects>
<connect gate="&quot;" pin="H1" pad="2"/>
<connect gate="&quot;" pin="H2" pad="7"/>
<connect gate="G$1" pin="PA" pad="3"/>
<connect gate="G$1" pin="PG" pad="5"/>
<connect gate="G$1" pin="PK" pad="8"/>
<connect gate="G$1" pin="PSG" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6L6GC-P" prefix="V" uservalue="yes">
<gates>
<gate name="G$1" symbol="PENTODE"/>
<gate name="&quot;" symbol="HEATER_1"/>
</gates>
<devices>
<device name="" package="OKTAL">
<connects>
<connect gate="&quot;" pin="H1" pad="2"/>
<connect gate="&quot;" pin="H2" pad="7"/>
<connect gate="G$1" pin="PA" pad="3"/>
<connect gate="G$1" pin="PG" pad="5"/>
<connect gate="G$1" pin="PK" pad="8"/>
<connect gate="G$1" pin="PSG" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6SJ7-P" prefix="V" uservalue="yes">
<gates>
<gate name="G$1" symbol="PENTODE/"/>
<gate name="&quot;" symbol="HEATER_1"/>
</gates>
<devices>
<device name="" package="OKTAL">
<connects>
<connect gate="&quot;" pin="H1" pad="2"/>
<connect gate="&quot;" pin="H2" pad="7"/>
<connect gate="G$1" pin="PA" pad="8"/>
<connect gate="G$1" pin="PBG" pad="3"/>
<connect gate="G$1" pin="PG" pad="4"/>
<connect gate="G$1" pin="PK" pad="5"/>
<connect gate="G$1" pin="PSG" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6SL7GT-P" prefix="V" uservalue="yes">
<gates>
<gate name="A" symbol="TRIODE"/>
<gate name="B" symbol="TRIODE"/>
<gate name="&quot;" symbol="HEATER_1"/>
</gates>
<devices>
<device name="" package="OKTAL">
<connects>
<connect gate="&quot;" pin="H1" pad="7"/>
<connect gate="&quot;" pin="H2" pad="8"/>
<connect gate="A" pin="TA" pad="2"/>
<connect gate="A" pin="TG" pad="1"/>
<connect gate="A" pin="TK" pad="3"/>
<connect gate="B" pin="TA" pad="5"/>
<connect gate="B" pin="TG" pad="4"/>
<connect gate="B" pin="TK" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6113-P" prefix="V" uservalue="yes">
<gates>
<gate name="A" symbol="TRIODE"/>
<gate name="B" symbol="TRIODE"/>
<gate name="&quot;" symbol="HEATER_1"/>
</gates>
<devices>
<device name="" package="OKTAL">
<connects>
<connect gate="&quot;" pin="H1" pad="7"/>
<connect gate="&quot;" pin="H2" pad="8"/>
<connect gate="A" pin="TA" pad="2"/>
<connect gate="A" pin="TG" pad="1"/>
<connect gate="A" pin="TK" pad="3"/>
<connect gate="B" pin="TA" pad="5"/>
<connect gate="B" pin="TG" pad="4"/>
<connect gate="B" pin="TK" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6U8-P" prefix="V" uservalue="yes">
<gates>
<gate name="A" symbol="TRIODE"/>
<gate name="&quot;" symbol="HEATER_1"/>
<gate name="B" symbol="PENTODE"/>
</gates>
<devices>
<device name="" package="NOVAL">
<connects>
<connect gate="&quot;" pin="H1" pad="4"/>
<connect gate="&quot;" pin="H2" pad="5"/>
<connect gate="A" pin="TA" pad="1"/>
<connect gate="A" pin="TG" pad="9"/>
<connect gate="A" pin="TK" pad="8"/>
<connect gate="B" pin="PA" pad="6"/>
<connect gate="B" pin="PG" pad="2"/>
<connect gate="B" pin="PK" pad="7"/>
<connect gate="B" pin="PSG" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ECF82-P" prefix="V" uservalue="yes">
<gates>
<gate name="A" symbol="TRIODE"/>
<gate name="B" symbol="PENTODE"/>
<gate name="&quot;" symbol="HEATER_1"/>
</gates>
<devices>
<device name="" package="NOVAL">
<connects>
<connect gate="&quot;" pin="H1" pad="4"/>
<connect gate="&quot;" pin="H2" pad="5"/>
<connect gate="A" pin="TA" pad="1"/>
<connect gate="A" pin="TG" pad="9"/>
<connect gate="A" pin="TK" pad="8"/>
<connect gate="B" pin="PA" pad="6"/>
<connect gate="B" pin="PG" pad="2"/>
<connect gate="B" pin="PK" pad="7"/>
<connect gate="B" pin="PSG" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6V6GT-P" prefix="V" uservalue="yes">
<gates>
<gate name="G$1" symbol="PENTODE"/>
<gate name="&quot;" symbol="HEATER_1"/>
</gates>
<devices>
<device name="" package="OKTAL">
<connects>
<connect gate="&quot;" pin="H1" pad="2"/>
<connect gate="&quot;" pin="H2" pad="7"/>
<connect gate="G$1" pin="PA" pad="3"/>
<connect gate="G$1" pin="PG" pad="5"/>
<connect gate="G$1" pin="PK" pad="8"/>
<connect gate="G$1" pin="PSG" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7184-P" prefix="V" uservalue="yes">
<gates>
<gate name="G$1" symbol="PENTODE"/>
<gate name="&quot;" symbol="HEATER_1"/>
</gates>
<devices>
<device name="" package="OKTAL">
<connects>
<connect gate="&quot;" pin="H1" pad="2"/>
<connect gate="&quot;" pin="H2" pad="7"/>
<connect gate="G$1" pin="PA" pad="3"/>
<connect gate="G$1" pin="PG" pad="5"/>
<connect gate="G$1" pin="PK" pad="8"/>
<connect gate="G$1" pin="PSG" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7027-P" prefix="V" uservalue="yes">
<gates>
<gate name="G$1" symbol="PENTODE"/>
<gate name="G$2" symbol="HEATER_1"/>
</gates>
<devices>
<device name="" package="OKTAL">
<connects>
<connect gate="G$1" pin="PA" pad="3"/>
<connect gate="G$1" pin="PG" pad="5"/>
<connect gate="G$1" pin="PK" pad="8"/>
<connect gate="G$1" pin="PSG" pad="4"/>
<connect gate="G$2" pin="H1" pad="2"/>
<connect gate="G$2" pin="H2" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7199-P" prefix="V" uservalue="yes">
<gates>
<gate name="A" symbol="TRIODE"/>
<gate name="B" symbol="PENTODE"/>
<gate name="&quot;" symbol="HEATER_1"/>
</gates>
<devices>
<device name="" package="NOVAL">
<connects>
<connect gate="&quot;" pin="H1" pad="4"/>
<connect gate="&quot;" pin="H2" pad="5"/>
<connect gate="A" pin="TA" pad="1"/>
<connect gate="A" pin="TG" pad="9"/>
<connect gate="A" pin="TK" pad="8"/>
<connect gate="B" pin="PA" pad="2"/>
<connect gate="B" pin="PG" pad="7"/>
<connect gate="B" pin="PK" pad="6"/>
<connect gate="B" pin="PSG" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7868-P" prefix="V" uservalue="yes">
<gates>
<gate name="G$1" symbol="PENTODE"/>
<gate name="&quot;" symbol="HEATER_1"/>
</gates>
<devices>
<device name="" package="NOVAL">
<connects>
<connect gate="&quot;" pin="H1" pad="4"/>
<connect gate="&quot;" pin="H2" pad="5"/>
<connect gate="G$1" pin="PA" pad="9"/>
<connect gate="G$1" pin="PG" pad="2"/>
<connect gate="G$1" pin="PK" pad="3"/>
<connect gate="G$1" pin="PSG" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ECC86-P" prefix="V" uservalue="yes">
<gates>
<gate name="A" symbol="TRIODE"/>
<gate name="B" symbol="TRIODE"/>
<gate name="&quot;" symbol="HEATER_2"/>
</gates>
<devices>
<device name="" package="NOVAL">
<connects>
<connect gate="&quot;" pin="H1" pad="4"/>
<connect gate="&quot;" pin="H2" pad="9"/>
<connect gate="&quot;" pin="H3" pad="5"/>
<connect gate="A" pin="TA" pad="1"/>
<connect gate="A" pin="TG" pad="2"/>
<connect gate="A" pin="TK" pad="3"/>
<connect gate="B" pin="TA" pad="6"/>
<connect gate="B" pin="TG" pad="7"/>
<connect gate="B" pin="TK" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ECC40-P" prefix="V" uservalue="yes">
<gates>
<gate name="A" symbol="TRIODE"/>
<gate name="B" symbol="TRIODE"/>
<gate name="&quot;" symbol="HEATER_1"/>
</gates>
<devices>
<device name="" package="NOVAL">
<connects>
<connect gate="&quot;" pin="H1" pad="1"/>
<connect gate="&quot;" pin="H2" pad="8"/>
<connect gate="A" pin="TA" pad="2"/>
<connect gate="A" pin="TG" pad="3"/>
<connect gate="A" pin="TK" pad="4"/>
<connect gate="B" pin="TA" pad="5"/>
<connect gate="B" pin="TG" pad="6"/>
<connect gate="B" pin="TK" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="12AT7-P" prefix="V" uservalue="yes">
<gates>
<gate name="A" symbol="TRIODE"/>
<gate name="B" symbol="TRIODE"/>
<gate name="&quot;" symbol="HEATER_2"/>
</gates>
<devices>
<device name="" package="NOVAL">
<connects>
<connect gate="&quot;" pin="H1" pad="4"/>
<connect gate="&quot;" pin="H2" pad="9"/>
<connect gate="&quot;" pin="H3" pad="5"/>
<connect gate="A" pin="TA" pad="1"/>
<connect gate="A" pin="TG" pad="2"/>
<connect gate="A" pin="TK" pad="3"/>
<connect gate="B" pin="TA" pad="6"/>
<connect gate="B" pin="TG" pad="7"/>
<connect gate="B" pin="TK" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="12AU7-P" prefix="V" uservalue="yes">
<gates>
<gate name="A" symbol="TRIODE"/>
<gate name="B" symbol="TRIODE"/>
<gate name="&quot;" symbol="HEATER_2"/>
</gates>
<devices>
<device name="" package="NOVAL">
<connects>
<connect gate="&quot;" pin="H1" pad="4"/>
<connect gate="&quot;" pin="H2" pad="9"/>
<connect gate="&quot;" pin="H3" pad="5"/>
<connect gate="A" pin="TA" pad="1"/>
<connect gate="A" pin="TG" pad="2"/>
<connect gate="A" pin="TK" pad="3"/>
<connect gate="B" pin="TA" pad="6"/>
<connect gate="B" pin="TG" pad="7"/>
<connect gate="B" pin="TK" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="12AX7-P" prefix="V" uservalue="yes">
<gates>
<gate name="A" symbol="TRIODE"/>
<gate name="B" symbol="TRIODE"/>
<gate name="&quot;" symbol="HEATER_2"/>
</gates>
<devices>
<device name="" package="NOVAL">
<connects>
<connect gate="&quot;" pin="H1" pad="4"/>
<connect gate="&quot;" pin="H2" pad="9"/>
<connect gate="&quot;" pin="H3" pad="5"/>
<connect gate="A" pin="TA" pad="1"/>
<connect gate="A" pin="TG" pad="2"/>
<connect gate="A" pin="TK" pad="3"/>
<connect gate="B" pin="TA" pad="6"/>
<connect gate="B" pin="TG" pad="7"/>
<connect gate="B" pin="TK" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ECC84-P" prefix="V" uservalue="yes">
<gates>
<gate name="A" symbol="TRIODE"/>
<gate name="B" symbol="TRIODE"/>
<gate name="&quot;" symbol="HEATER_2"/>
</gates>
<devices>
<device name="" package="NOVAL">
<connects>
<connect gate="&quot;" pin="H1" pad="4"/>
<connect gate="&quot;" pin="H2" pad="9"/>
<connect gate="&quot;" pin="H3" pad="5"/>
<connect gate="A" pin="TA" pad="1"/>
<connect gate="A" pin="TG" pad="2"/>
<connect gate="A" pin="TK" pad="3"/>
<connect gate="B" pin="TA" pad="6"/>
<connect gate="B" pin="TG" pad="7"/>
<connect gate="B" pin="TK" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6CW7-P" prefix="V" uservalue="yes">
<gates>
<gate name="A" symbol="TRIODE"/>
<gate name="B" symbol="TRIODE"/>
<gate name="&quot;" symbol="HEATER_2"/>
</gates>
<devices>
<device name="" package="NOVAL">
<connects>
<connect gate="&quot;" pin="H1" pad="4"/>
<connect gate="&quot;" pin="H2" pad="9"/>
<connect gate="&quot;" pin="H3" pad="5"/>
<connect gate="A" pin="TA" pad="1"/>
<connect gate="A" pin="TG" pad="2"/>
<connect gate="A" pin="TK" pad="3"/>
<connect gate="B" pin="TA" pad="6"/>
<connect gate="B" pin="TG" pad="7"/>
<connect gate="B" pin="TK" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ECC88-P" prefix="V" uservalue="yes">
<gates>
<gate name="A" symbol="TRIODE"/>
<gate name="B" symbol="TRIODE"/>
<gate name="&quot;" symbol="HEATER_2"/>
</gates>
<devices>
<device name="" package="NOVAL">
<connects>
<connect gate="&quot;" pin="H1" pad="4"/>
<connect gate="&quot;" pin="H2" pad="9"/>
<connect gate="&quot;" pin="H3" pad="5"/>
<connect gate="A" pin="TA" pad="1"/>
<connect gate="A" pin="TG" pad="2"/>
<connect gate="A" pin="TK" pad="3"/>
<connect gate="B" pin="TA" pad="6"/>
<connect gate="B" pin="TG" pad="7"/>
<connect gate="B" pin="TK" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6BM8-P" prefix="V" uservalue="yes">
<gates>
<gate name="A" symbol="TRIODE"/>
<gate name="B" symbol="PENTODE"/>
<gate name="&quot;" symbol="HEATER_1"/>
</gates>
<devices>
<device name="" package="NOVAL">
<connects>
<connect gate="&quot;" pin="H1" pad="4"/>
<connect gate="&quot;" pin="H2" pad="5"/>
<connect gate="A" pin="TA" pad="9"/>
<connect gate="A" pin="TG" pad="1"/>
<connect gate="A" pin="TK" pad="8"/>
<connect gate="B" pin="PA" pad="6"/>
<connect gate="B" pin="PG" pad="3"/>
<connect gate="B" pin="PK" pad="2"/>
<connect gate="B" pin="PSG" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6GW8-P" prefix="V" uservalue="yes">
<gates>
<gate name="A" symbol="TRIODE"/>
<gate name="B" symbol="PENTODE"/>
<gate name="&quot;" symbol="HEATER_1"/>
</gates>
<devices>
<device name="" package="NOVAL">
<connects>
<connect gate="&quot;" pin="H1" pad="4"/>
<connect gate="&quot;" pin="H2" pad="5"/>
<connect gate="A" pin="TA" pad="9"/>
<connect gate="A" pin="TG" pad="1"/>
<connect gate="A" pin="TK" pad="2"/>
<connect gate="B" pin="PA" pad="6"/>
<connect gate="B" pin="PG" pad="8"/>
<connect gate="B" pin="PK" pad="7"/>
<connect gate="B" pin="PSG" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EF40-P" prefix="V" uservalue="yes">
<gates>
<gate name="G$1" symbol="PENTODE/"/>
<gate name="G$2" symbol="HEATER_1"/>
</gates>
<devices>
<device name="" package="OKTAL">
<connects>
<connect gate="G$1" pin="PA" pad="2"/>
<connect gate="G$1" pin="PBG" pad="4"/>
<connect gate="G$1" pin="PG" pad="5"/>
<connect gate="G$1" pin="PK" pad="7"/>
<connect gate="G$1" pin="PSG" pad="6"/>
<connect gate="G$2" pin="H1" pad="1"/>
<connect gate="G$2" pin="H2" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6BK8-P" prefix="V" uservalue="yes">
<gates>
<gate name="G$1" symbol="PENTODE/"/>
<gate name="&quot;" symbol="HEATER_1"/>
</gates>
<devices>
<device name="" package="NOVAL">
<connects>
<connect gate="&quot;" pin="H1" pad="4"/>
<connect gate="&quot;" pin="H2" pad="5"/>
<connect gate="G$1" pin="PA" pad="6"/>
<connect gate="G$1" pin="PBG" pad="8"/>
<connect gate="G$1" pin="PG" pad="9"/>
<connect gate="G$1" pin="PK" pad="3"/>
<connect gate="G$1" pin="PSG" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6CA7-P" prefix="V" uservalue="yes">
<gates>
<gate name="G$1" symbol="PENTODE/"/>
<gate name="&quot;" symbol="HEATER_1"/>
</gates>
<devices>
<device name="" package="OKTAL">
<connects>
<connect gate="&quot;" pin="H1" pad="2"/>
<connect gate="&quot;" pin="H2" pad="7"/>
<connect gate="G$1" pin="PA" pad="3"/>
<connect gate="G$1" pin="PBG" pad="1"/>
<connect gate="G$1" pin="PG" pad="5"/>
<connect gate="G$1" pin="PK" pad="8"/>
<connect gate="G$1" pin="PSG" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EL41-P" prefix="V" uservalue="yes">
<gates>
<gate name="G$1" symbol="PENTODE"/>
<gate name="&quot;" symbol="HEATER_1"/>
</gates>
<devices>
<device name="" package="OKTAL">
<connects>
<connect gate="&quot;" pin="H1" pad="1"/>
<connect gate="&quot;" pin="H2" pad="8"/>
<connect gate="G$1" pin="PA" pad="2"/>
<connect gate="G$1" pin="PG" pad="6"/>
<connect gate="G$1" pin="PK" pad="7"/>
<connect gate="G$1" pin="PSG" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6CK5-P" prefix="V" uservalue="yes">
<gates>
<gate name="G$1" symbol="PENTODE"/>
<gate name="&quot;" symbol="HEATER_1"/>
</gates>
<devices>
<device name="" package="OKTAL">
<connects>
<connect gate="&quot;" pin="H1" pad="1"/>
<connect gate="&quot;" pin="H2" pad="8"/>
<connect gate="G$1" pin="PA" pad="2"/>
<connect gate="G$1" pin="PG" pad="6"/>
<connect gate="G$1" pin="PK" pad="7"/>
<connect gate="G$1" pin="PSG" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EL42-P" prefix="V" uservalue="yes">
<gates>
<gate name="G$1" symbol="PENTODE"/>
<gate name="&quot;" symbol="HEATER_1"/>
</gates>
<devices>
<device name="" package="OKTAL">
<connects>
<connect gate="&quot;" pin="H1" pad="1"/>
<connect gate="&quot;" pin="H2" pad="8"/>
<connect gate="G$1" pin="PA" pad="2"/>
<connect gate="G$1" pin="PG" pad="6"/>
<connect gate="G$1" pin="PK" pad="7"/>
<connect gate="G$1" pin="PSG" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6BQ5-P" prefix="V" uservalue="yes">
<gates>
<gate name="G$1" symbol="PENTODE"/>
<gate name="&quot;" symbol="HEATER_1"/>
</gates>
<devices>
<device name="" package="NOVAL">
<connects>
<connect gate="&quot;" pin="H1" pad="4"/>
<connect gate="&quot;" pin="H2" pad="5"/>
<connect gate="G$1" pin="PA" pad="7"/>
<connect gate="G$1" pin="PG" pad="2"/>
<connect gate="G$1" pin="PK" pad="3"/>
<connect gate="G$1" pin="PSG" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EL86-P" prefix="V" uservalue="yes">
<gates>
<gate name="G$1" symbol="PENTODE"/>
<gate name="&quot;" symbol="HEATER_1"/>
</gates>
<devices>
<device name="" package="NOVAL">
<connects>
<connect gate="&quot;" pin="H1" pad="4"/>
<connect gate="&quot;" pin="H2" pad="5"/>
<connect gate="G$1" pin="PA" pad="7"/>
<connect gate="G$1" pin="PG" pad="2"/>
<connect gate="G$1" pin="PK" pad="3"/>
<connect gate="G$1" pin="PSG" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6CW5-P" prefix="V" uservalue="yes">
<gates>
<gate name="G$1" symbol="PENTODE"/>
<gate name="&quot;" symbol="HEATER_1"/>
</gates>
<devices>
<device name="" package="NOVAL">
<connects>
<connect gate="&quot;" pin="H1" pad="4"/>
<connect gate="&quot;" pin="H2" pad="5"/>
<connect gate="G$1" pin="PA" pad="7"/>
<connect gate="G$1" pin="PG" pad="2"/>
<connect gate="G$1" pin="PK" pad="3"/>
<connect gate="G$1" pin="PSG" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7025-P" prefix="V" uservalue="yes">
<gates>
<gate name="A" symbol="TRIODE"/>
<gate name="B" symbol="TRIODE"/>
<gate name="&quot;" symbol="HEATER_2"/>
</gates>
<devices>
<device name="" package="NOVAL">
<connects>
<connect gate="&quot;" pin="H1" pad="4"/>
<connect gate="&quot;" pin="H2" pad="9"/>
<connect gate="&quot;" pin="H3" pad="5"/>
<connect gate="A" pin="TA" pad="1"/>
<connect gate="A" pin="TG" pad="2"/>
<connect gate="A" pin="TK" pad="3"/>
<connect gate="B" pin="TA" pad="6"/>
<connect gate="B" pin="TG" pad="7"/>
<connect gate="B" pin="TK" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="12DM7-P" prefix="V" uservalue="yes">
<gates>
<gate name="A" symbol="TRIODE"/>
<gate name="B" symbol="TRIODE"/>
<gate name="&quot;" symbol="HEATER_2"/>
</gates>
<devices>
<device name="" package="NOVAL">
<connects>
<connect gate="&quot;" pin="H1" pad="4"/>
<connect gate="&quot;" pin="H2" pad="9"/>
<connect gate="&quot;" pin="H3" pad="5"/>
<connect gate="A" pin="TA" pad="1"/>
<connect gate="A" pin="TG" pad="2"/>
<connect gate="A" pin="TK" pad="3"/>
<connect gate="B" pin="TA" pad="6"/>
<connect gate="B" pin="TG" pad="7"/>
<connect gate="B" pin="TK" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6680-P" prefix="V" uservalue="yes">
<gates>
<gate name="A" symbol="TRIODE"/>
<gate name="B" symbol="TRIODE"/>
<gate name="&quot;" symbol="HEATER_2"/>
</gates>
<devices>
<device name="" package="NOVAL">
<connects>
<connect gate="&quot;" pin="H1" pad="4"/>
<connect gate="&quot;" pin="H2" pad="9"/>
<connect gate="&quot;" pin="H3" pad="5"/>
<connect gate="A" pin="TA" pad="1"/>
<connect gate="A" pin="TG" pad="2"/>
<connect gate="A" pin="TK" pad="3"/>
<connect gate="B" pin="TA" pad="6"/>
<connect gate="B" pin="TG" pad="7"/>
<connect gate="B" pin="TK" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6681-P" prefix="V" uservalue="yes">
<gates>
<gate name="A" symbol="TRIODE"/>
<gate name="B" symbol="TRIODE"/>
<gate name="&quot;" symbol="HEATER_2"/>
</gates>
<devices>
<device name="" package="NOVAL">
<connects>
<connect gate="&quot;" pin="H1" pad="4"/>
<connect gate="&quot;" pin="H2" pad="9"/>
<connect gate="&quot;" pin="H3" pad="5"/>
<connect gate="A" pin="TA" pad="1"/>
<connect gate="A" pin="TG" pad="2"/>
<connect gate="A" pin="TK" pad="3"/>
<connect gate="B" pin="TA" pad="6"/>
<connect gate="B" pin="TG" pad="7"/>
<connect gate="B" pin="TK" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6679-P" prefix="V" uservalue="yes">
<gates>
<gate name="A" symbol="TRIODE"/>
<gate name="B" symbol="TRIODE"/>
<gate name="&quot;" symbol="HEATER_2"/>
</gates>
<devices>
<device name="" package="NOVAL">
<connects>
<connect gate="&quot;" pin="H1" pad="4"/>
<connect gate="&quot;" pin="H2" pad="9"/>
<connect gate="&quot;" pin="H3" pad="5"/>
<connect gate="A" pin="TA" pad="1"/>
<connect gate="A" pin="TG" pad="2"/>
<connect gate="A" pin="TK" pad="3"/>
<connect gate="B" pin="TA" pad="6"/>
<connect gate="B" pin="TG" pad="7"/>
<connect gate="B" pin="TK" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6201-P" prefix="V" uservalue="yes">
<gates>
<gate name="A" symbol="TRIODE"/>
<gate name="B" symbol="TRIODE"/>
<gate name="&quot;" symbol="HEATER_2"/>
</gates>
<devices>
<device name="" package="NOVAL">
<connects>
<connect gate="&quot;" pin="H1" pad="4"/>
<connect gate="&quot;" pin="H2" pad="9"/>
<connect gate="&quot;" pin="H3" pad="5"/>
<connect gate="A" pin="TA" pad="1"/>
<connect gate="A" pin="TG" pad="2"/>
<connect gate="A" pin="TK" pad="3"/>
<connect gate="B" pin="TA" pad="6"/>
<connect gate="B" pin="TG" pad="7"/>
<connect gate="B" pin="TK" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6267-P" prefix="V" uservalue="yes">
<gates>
<gate name="G$1" symbol="PENTODE/"/>
<gate name="&quot;" symbol="HEATER_1"/>
</gates>
<devices>
<device name="" package="NOVAL">
<connects>
<connect gate="&quot;" pin="H1" pad="4"/>
<connect gate="&quot;" pin="H2" pad="5"/>
<connect gate="G$1" pin="PA" pad="6"/>
<connect gate="G$1" pin="PBG" pad="8"/>
<connect gate="G$1" pin="PG" pad="9"/>
<connect gate="G$1" pin="PK" pad="3"/>
<connect gate="G$1" pin="PSG" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6KX8-P" prefix="V" uservalue="yes">
<gates>
<gate name="A" symbol="TRIODE"/>
<gate name="B" symbol="TRIODE"/>
<gate name="&quot;" symbol="HEATER_2"/>
</gates>
<devices>
<device name="" package="NOVAL">
<connects>
<connect gate="&quot;" pin="H1" pad="4"/>
<connect gate="&quot;" pin="H2" pad="6"/>
<connect gate="&quot;" pin="H3" pad="5"/>
<connect gate="A" pin="TA" pad="3"/>
<connect gate="A" pin="TG" pad="1"/>
<connect gate="A" pin="TK" pad="2"/>
<connect gate="B" pin="TA" pad="7"/>
<connect gate="B" pin="TG" pad="9"/>
<connect gate="B" pin="TK" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6CL6-P" prefix="V" uservalue="yes">
<gates>
<gate name="&quot;" symbol="HEATER_1"/>
<gate name="G$1" symbol="PENTODE"/>
</gates>
<devices>
<device name="" package="NOVAL">
<connects>
<connect gate="&quot;" pin="H1" pad="4"/>
<connect gate="&quot;" pin="H2" pad="5"/>
<connect gate="G$1" pin="PA" pad="6"/>
<connect gate="G$1" pin="PG" pad="2"/>
<connect gate="G$1" pin="PK" pad="1"/>
<connect gate="G$1" pin="PSG" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6922-P" prefix="V" uservalue="yes">
<gates>
<gate name="A" symbol="TRIODE"/>
<gate name="B" symbol="TRIODE"/>
<gate name="&quot;" symbol="HEATER_2"/>
</gates>
<devices>
<device name="" package="NOVAL">
<connects>
<connect gate="&quot;" pin="H1" pad="4"/>
<connect gate="&quot;" pin="H2" pad="9"/>
<connect gate="&quot;" pin="H3" pad="5"/>
<connect gate="A" pin="TA" pad="1"/>
<connect gate="A" pin="TG" pad="2"/>
<connect gate="A" pin="TK" pad="3"/>
<connect gate="B" pin="TA" pad="6"/>
<connect gate="B" pin="TG" pad="7"/>
<connect gate="B" pin="TK" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="5687-P" prefix="V" uservalue="yes">
<gates>
<gate name="A" symbol="TRIODE"/>
<gate name="B" symbol="TRIODE"/>
<gate name="&quot;" symbol="HEATER_2"/>
</gates>
<devices>
<device name="" package="NOVAL">
<connects>
<connect gate="&quot;" pin="H1" pad="4"/>
<connect gate="&quot;" pin="H2" pad="8"/>
<connect gate="&quot;" pin="H3" pad="5"/>
<connect gate="A" pin="TA" pad="1"/>
<connect gate="A" pin="TG" pad="2"/>
<connect gate="A" pin="TK" pad="3"/>
<connect gate="B" pin="TA" pad="9"/>
<connect gate="B" pin="TG" pad="7"/>
<connect gate="B" pin="TK" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="12B4-P" prefix="V" uservalue="yes">
<gates>
<gate name="G$1" symbol="TRIODE"/>
<gate name="&quot;" symbol="HEATER_2"/>
</gates>
<devices>
<device name="" package="NOVAL">
<connects>
<connect gate="&quot;" pin="H1" pad="4"/>
<connect gate="&quot;" pin="H2" pad="3"/>
<connect gate="&quot;" pin="H3" pad="5"/>
<connect gate="G$1" pin="TA" pad="9"/>
<connect gate="G$1" pin="TG" pad="7"/>
<connect gate="G$1" pin="TK" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6080-P" prefix="V" uservalue="yes">
<gates>
<gate name="A" symbol="TRIODE"/>
<gate name="B" symbol="TRIODE"/>
<gate name="&quot;" symbol="HEATER_1"/>
</gates>
<devices>
<device name="" package="OKTAL">
<connects>
<connect gate="&quot;" pin="H1" pad="7"/>
<connect gate="&quot;" pin="H2" pad="8"/>
<connect gate="A" pin="TA" pad="2"/>
<connect gate="A" pin="TG" pad="1"/>
<connect gate="A" pin="TK" pad="3"/>
<connect gate="B" pin="TA" pad="5"/>
<connect gate="B" pin="TG" pad="4"/>
<connect gate="B" pin="TK" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="5691-P" prefix="V" uservalue="yes">
<gates>
<gate name="A" symbol="TRIODE"/>
<gate name="B" symbol="TRIODE"/>
<gate name="&quot;" symbol="HEATER_1"/>
</gates>
<devices>
<device name="" package="OKTAL">
<connects>
<connect gate="&quot;" pin="H1" pad="7"/>
<connect gate="&quot;" pin="H2" pad="8"/>
<connect gate="A" pin="TA" pad="2"/>
<connect gate="A" pin="TG" pad="1"/>
<connect gate="A" pin="TK" pad="3"/>
<connect gate="B" pin="TA" pad="5"/>
<connect gate="B" pin="TG" pad="4"/>
<connect gate="B" pin="TK" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="5692-P" prefix="V" uservalue="yes">
<gates>
<gate name="A" symbol="TRIODE"/>
<gate name="B" symbol="TRIODE"/>
<gate name="&quot;" symbol="HEATER_1"/>
</gates>
<devices>
<device name="" package="OKTAL">
<connects>
<connect gate="&quot;" pin="H1" pad="7"/>
<connect gate="&quot;" pin="H2" pad="8"/>
<connect gate="A" pin="TA" pad="2"/>
<connect gate="A" pin="TG" pad="1"/>
<connect gate="A" pin="TK" pad="3"/>
<connect gate="B" pin="TA" pad="5"/>
<connect gate="B" pin="TG" pad="4"/>
<connect gate="B" pin="TK" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ECC34-P" prefix="V" uservalue="yes">
<gates>
<gate name="A" symbol="TRIODE"/>
<gate name="B" symbol="TRIODE"/>
<gate name="&quot;" symbol="HEATER_1"/>
</gates>
<devices>
<device name="" package="OKTAL">
<connects>
<connect gate="&quot;" pin="H1" pad="7"/>
<connect gate="&quot;" pin="H2" pad="8"/>
<connect gate="A" pin="TA" pad="2"/>
<connect gate="A" pin="TG" pad="1"/>
<connect gate="A" pin="TK" pad="3"/>
<connect gate="B" pin="TA" pad="5"/>
<connect gate="B" pin="TG" pad="4"/>
<connect gate="B" pin="TK" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ECC35-P" prefix="V" uservalue="yes">
<gates>
<gate name="A" symbol="TRIODE"/>
<gate name="B" symbol="TRIODE"/>
<gate name="&quot;" symbol="HEATER_1"/>
</gates>
<devices>
<device name="" package="OKTAL">
<connects>
<connect gate="&quot;" pin="H1" pad="7"/>
<connect gate="&quot;" pin="H2" pad="8"/>
<connect gate="A" pin="TA" pad="2"/>
<connect gate="A" pin="TG" pad="1"/>
<connect gate="A" pin="TK" pad="3"/>
<connect gate="B" pin="TA" pad="5"/>
<connect gate="B" pin="TG" pad="4"/>
<connect gate="B" pin="TK" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6BX7-P" prefix="V" uservalue="yes">
<gates>
<gate name="A" symbol="TRIODE"/>
<gate name="B" symbol="TRIODE"/>
<gate name="&quot;" symbol="HEATER_1"/>
</gates>
<devices>
<device name="" package="OKTAL">
<connects>
<connect gate="&quot;" pin="H1" pad="7"/>
<connect gate="&quot;" pin="H2" pad="8"/>
<connect gate="A" pin="TA" pad="2"/>
<connect gate="A" pin="TG" pad="1"/>
<connect gate="A" pin="TK" pad="3"/>
<connect gate="B" pin="TA" pad="5"/>
<connect gate="B" pin="TG" pad="4"/>
<connect gate="B" pin="TK" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7119-P" prefix="V" uservalue="yes">
<gates>
<gate name="A" symbol="TRIODE"/>
<gate name="B" symbol="TRIODE"/>
<gate name="&quot;" symbol="HEATER_2"/>
</gates>
<devices>
<device name="" package="NOVAL">
<connects>
<connect gate="&quot;" pin="H1" pad="4"/>
<connect gate="&quot;" pin="H2" pad="8"/>
<connect gate="&quot;" pin="H3" pad="5"/>
<connect gate="A" pin="TA" pad="1"/>
<connect gate="A" pin="TG" pad="2"/>
<connect gate="A" pin="TK" pad="3"/>
<connect gate="B" pin="TA" pad="9"/>
<connect gate="B" pin="TG" pad="7"/>
<connect gate="B" pin="TK" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="E182CC-P" prefix="V" uservalue="yes">
<gates>
<gate name="A" symbol="TRIODE"/>
<gate name="B" symbol="TRIODE"/>
<gate name="&quot;" symbol="HEATER_2"/>
</gates>
<devices>
<device name="" package="NOVAL">
<connects>
<connect gate="&quot;" pin="H1" pad="4"/>
<connect gate="&quot;" pin="H2" pad="8"/>
<connect gate="&quot;" pin="H3" pad="5"/>
<connect gate="A" pin="TA" pad="1"/>
<connect gate="A" pin="TG" pad="2"/>
<connect gate="A" pin="TK" pad="3"/>
<connect gate="B" pin="TA" pad="9"/>
<connect gate="B" pin="TG" pad="7"/>
<connect gate="B" pin="TK" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="E88CC-P" prefix="V" uservalue="yes">
<gates>
<gate name="A" symbol="TRIODE"/>
<gate name="B" symbol="TRIODE"/>
<gate name="&quot;" symbol="HEATER_2"/>
</gates>
<devices>
<device name="" package="NOVAL">
<connects>
<connect gate="&quot;" pin="H1" pad="4"/>
<connect gate="&quot;" pin="H2" pad="9"/>
<connect gate="&quot;" pin="H3" pad="5"/>
<connect gate="A" pin="TA" pad="1"/>
<connect gate="A" pin="TG" pad="2"/>
<connect gate="A" pin="TK" pad="3"/>
<connect gate="B" pin="TA" pad="6"/>
<connect gate="B" pin="TG" pad="7"/>
<connect gate="B" pin="TK" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEATER1" prefix="V" uservalue="yes">
<gates>
<gate name="G$1" symbol="HEAT/1"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEATER2" prefix="V" uservalue="yes">
<gates>
<gate name="G$1" symbol="HEAT/2"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PENTODE1" prefix="V" uservalue="yes">
<gates>
<gate name="G$1" symbol="PENT/"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PENTODE2" prefix="V" uservalue="yes">
<gates>
<gate name="G$1" symbol="PENT//"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
