ROM VER: 2.1.0
CFG 09
B
.
.
.

*

ROM VER: 2.1.0
CFG 09
B
.
.
.

*
*
*
*
Detected PXB4583el V1.2-2000

(AVM) EVA Revision: 1.3229

(C) Copyright 2005 AVM Date: Nov 30 2016 Time: 17:40:36 (0) 3 0x0-0x46409

[NAND:] 512MB TOSHIBA 4096 Pagesize 256k Blocksize 2048 Blocks
[SYSTEM:] GRX5 (ID 0x24 Revision 2) on 1000MHz/600MHz/666MHz
..

Eva_AVM >#Loading compressed kernel to 0x85244550
………………………………………………………………………………………………Device Tree Blob for SubRevision 2 not found.
Using Device Tree Blob of SubRevision 0 

—————————————————————

      Switching to Bootcore Console

—————————————————————
[    0.000000] Linux version 4.9.198 (jenkins@jenkins-ci.avm.de) (gcc version 8.3.0 (Buildroot 2018.11.4-gb385ae7957) ) #1 2021-04-13
[    0.000000] avm_check_isa_features: isa_level 0x00000031
[    0.000000] avm_check_cpu_features: mips-options (cache flags preliminary!): 0x000000c00059638b ases 0x00000001
[    0.000000] avm_check_cpu_features: (preliminary flags: MIPS_CPU_CACHE_CDEX_P MIPS_CPU_PREFETCH MIPS_CPU_INCLUSIVE_CACHES MIPS_CPU_CACHE_CDEX_S)
[    0.000000] SoC: GRX500 rev 1.2
[    0.000000] bootconsole [early0] enabled
[    0.000000] CPU0 revision is: 00019074 (MIPS 4KEc)
[    0.000000] MIPS: machine is GRX550 ANYWAN BOOTCORE (MIPS 4Kec)
[    0.000000] bootconsole [early0] enabled
[    0.000000] Determined physical RAM map:
[    0.000000]  memory: 02000000 @ 0e000000 (usable)
[    0.000000]  memory: 00001b2d @ 0e781030 (reserved)
[    0.000000]  memory: 00040000 @ 0dfc0000 (reserved)
[    0.000000] Initial ramdisk at: 0x8e000000 (4194304 bytes)
[    0.000000] avm_check_pcache_features: mips-options (preliminary MIPS_CPU_CACHE_CDEX_S flag): 0x000000c0005d638b icache.flags 0x00000000 dcache.flags 0x00000004
[    0.000000] Primary instruction cache 32kB, VIPT, 4-way, linesize 16 bytes.
[    0.000000] Primary data cache 32kB, 4-way, VIPT, cache aliases, linesize 16 bytes
[    0.000000] avm_check_scache_features: mips-options: 0x000000c0005d638b
[    0.000000] Zone ranges:
[    0.000000]   Normal   [mem 0x000000000e000000-0x000000000fffffff]
[    0.000000] Movable zone start for each node
[    0.000000] Early memory node ranges
[    0.000000]   node   0: [mem 0x000000000e000000-0x000000000fffffff]
[    0.000000] Initmem setup node 0 [mem 0x000000000e000000-0x000000000fffffff]
[    0.000000] On node 0 totalpages: 8192
[    0.000000] free_area_init_node: node 0, pgdat 8e780620, node_mem_map 8f005720
[    0.000000]   Normal zone: 64 pages used for memmap
[    0.000000]   Normal zone: 0 pages reserved
[    0.000000]   Normal zone: 8192 pages, LIFO batch:0
[    0.000000] [fw-info] Version 07.30
[    0.000000] pcpu-alloc: s0 r0 d32768 u32768 alloc=1*32768
[    0.000000] pcpu-alloc: [0] 0 
[    0.000000] Built 1 zonelists in Zone order, mobility grouping on.  Total pages: 8128
[    0.000000] Kernel command line: console=ttyLTQ0,115200n8r root=/dev/ram rw loglevel=8
[    0.000000] PID hash table entries: 128 (order: -3, 512 bytes)
[    0.000000] Dentry cache hash table entries: 4096 (order: 2, 16384 bytes)
[    0.000000] Inode-cache hash table entries: 2048 (order: 1, 8192 bytes)
[    0.000000] Memory: 24076K/32768K available (2651K kernel code, 394K rwdata, 736K rodata, 180K init, 258K bss, 8692K reserved, 0K cma-reserved)
[    0.000000] SLUB: HWalign=32, Order=0-3, MinObjects=0, CPUs=1, Nodes=1
[    0.000000] NR_IRQS:527
[    0.000000] grx500_bootcore_register_static_irq: irq_in = 0x0000001f, irq_out = 0x0000001f
[    0.000000] grx500_bootcore_register_static_irq: mapper_reg = 0x0000015c, mapper_offset = 0x00000000
[    0.000000] EXCEP_remap_line: int_line = 0x0000001f, map_address = 0x0000015c, num = 0x00000000 
[    0.000000] EXCEP_remap_line: org_map = 0x00000000, result_map = 0x0000001f 
[    0.000000] CPU Clock: 300MHz
[    0.000000] clocksource: MIPS: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 12741736309 ns
[    0.000020] sched_clock: 32 bits at 150MHz, resolution 6ns, wraps every 14316557820ns
[    0.015341] : grx500_bootcore_console_init: call register
[    0.025706] console [ttyLTQ0] enabled
[    0.025706] console [ttyLTQ0] enabled
[    0.036176] bootconsole [early0] disabled
[    0.036176] bootconsole [early0] disabled
[    0.047703] bootconsole [early0] disabled
[    0.047703] bootconsole [early0] disabled
[    0.055687] Calibrating delay loop… 299.26 BogoMIPS (lpj=598528)
[    0.094094] pid_max: default: 32768 minimum: 301
[    0.099160] Mount-cache hash table entries: 1024 (order: 0, 4096 bytes)
[    0.105588] Mountpoint-cache hash table entries: 1024 (order: 0, 4096 bytes)
[    0.121420] devtmpfs: initialized
[    0.129232] ngi: Protecting Bootcore: [0x2e000000, 0x2fffffff]
[    0.134901] ngi: 512MB attached. Protecting: [0x40000000, 0x9fffffff]
[    0.141244] ngi: Unattached: [0x60000000, 0x9fffffff]
[    0.146256] ngi: Unattached: [0x40000000, 0x5fffffff]
[    0.151858] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 7645041785100000 ns
[    0.161478] futex hash table entries: 256 (order: -1, 3072 bytes)
[    0.167746] pinctrl core: initialized pinctrl subsystem
[    0.174269] NET: Registered protocol family 16
[    0.192606] irq: no irq domain found for /interrupt-controller@0x14900140 !
[    0.282297] clocksource: Switched to clocksource MIPS
[    0.309648] NET: Registered protocol family 2
[    0.316061] TCP established hash table entries: 1024 (order: 0, 4096 bytes)
[    0.323053] TCP bind hash table entries: 1024 (order: 0, 4096 bytes)
[    0.329270] TCP: Hash tables configured (established 1024 bind 1024)
[    0.336126] UDP hash table entries: 256 (order: 0, 4096 bytes)
[    0.341931] UDP-Lite hash table entries: 256 (order: 0, 4096 bytes)
[    0.348595] NET: Registered protocol family 1
[    0.356906] Unpacking initramfs…
[    1.106312] random: fast init done
[    1.255838] Freeing initrd memory: 4096K
[    1.266723] workingset: timestamp_bits=30 max_order=13 bucket_order=0
[    1.331952] Serial: grx500_bootcore driver init
[    1.339993] libphy: Fixed MDIO Bus: probed
[    1.347509] NET: Registered protocol family 10
[    1.361850] NET: Registered protocol family 17
[    1.373396] Serial: grx500_bootcore driver startup
[    1.378147] grx500_bootcore_register_static_irq: irq_in = 0x0000001c, irq_out = 0x00000008
[    1.386211] grx500_bootcore_register_static_irq: mapper_reg = 0x00000158, mapper_offset = 0x00000003
[    1.395297] EXCEP_remap_line: int_line = 0x00000008, map_address = 0x00000158, num = 0x00000003 
[    1.404005] EXCEP_remap_line: org_map = 0x00000000, result_map = 0x00040000 
[    1.415744] Freeing unused kernel memory: 180K
[    1.420080] This architecture does not have kernel memory protection.
[    1.601011] eip123_hw: module license ‚Proprietary‘ taints kernel.
[    1.607192] Disabling lock debugging due to kernel taint
[    1.619234] eip123 1e000000.eip123: Detected hardware version 2.2.2
[    1.625476] eip123 1e000000.eip123: my_id=0 master_id=0 num_mailboxes=4 mailbox_size=256
[    1.633369] eip123 1e000000.eip123: Configured mailbox lockout: 0x00000000
[    1.640187] eip123 1e000000.eip123: Linked mailbox number 1
[    1.670369] eip123 1e000000.eip123: Sysinfo: FWVersion=2.4.2 HWVersion=2.2.2 MemorySize=32768 HostId=0 Identity=0 NVMAnomaly=0 NVMAnomalyLocation=0
[    1.906312] eip123 1e000000.eip123: eip123_hw init successful
[    1.939099] random: crng init done
[    1.966340] eip123 1e000000.eip123: Device responded with error_src=0x0 error=0x1 opcode=0x1c
[    1.974710] eip123 1e000000.eip123: Could not find rootkey in OTP
[    1.981380] eip123 1e000000.eip123: Unlinked mailboxes
[    2.032763] cpunet 1f107400.cpunet: slots=16 mtu=8192 mailbox_size=0x4c mempool_size=0x20000
[    2.041275] cpunet 1f107400.cpunet: Initialized mailbox: rx=0xbf201100 tx=0xbf201000
[    2.049366] cpunet 1f107400.cpunet: Initialized mempool: rx=0x8dfe0000 tx=0x8dfc0000 min_align=64
[    2.058055] grx500_bootcore_register_static_irq: irq_in = 0x00000016, irq_out = 0x0000000b
[    2.066222] grx500_bootcore_register_static_irq: mapper_reg = 0x00000154, mapper_offset = 0x00000003
[    2.075305] EXCEP_remap_line: int_line = 0x0000000b, map_address = 0x00000154, num = 0x00000003 
[    2.084040] EXCEP_remap_line: org_map = 0x00000000, result_map = 0x00058000 
[    2.091127] cpunet 1f107400.cpunet: hw init successful
[    2.143776] interaptiv_start: starting interaptiv
ºH¨©©©©©©©©©©©©©©©©©©©©©©©©©©©©©©©©©©©©©©©©©©©H¨H¨H¨HšÝ¥Ñ¡¥¹to Interaptiv Console

—————————————————————
..
Device Tree Blob for SubRevision 2 not found.
Using Device Tree Blob of SubRevision 1 
[    0.000000] Linux version 4.9.198 (jenkins@jenkins-ci.avm.de) (gcc version 8.3.0 (Buildroot 2018.11.4-gc73018b701) ) #1 SMP 2021-07-20

[    0.000000] avm_check_isa_features: isa_level 0x00000031

[    0.000000] avm_check_cpu_features: mips-options (cache flags preliminary!): 0x000088c40e69638b ases 0x00000030

[    0.000000] avm_check_cpu_features: (preliminary flags: MIPS_CPU_CACHE_CDEX_P MIPS_CPU_PREFETCH MIPS_CPU_INCLUSIVE_CACHES MIPS_CPU_CACHE_CDEX_S)

[    0.000000] SoC: GRX500 rev 1.2

[    0.000000] bootconsole [early0] enabled

[    0.000000] CPU0 revision is: 0001a120 (MIPS interAptiv (multi))

[    0.000000] Enhanced Virtual Addressing (EVA Legacy 512MB) activated

[    0.000000] MIPS: machine is AVM7580 vrx318 (GRX550, HW225-1) Main model

[    0.000000] Coherence Manager IOCU detected

[    0.000000] Hardware DMA cache coherency disabled

[    0.000000] OF: fdt:Reserved memory (avm): reserved region for property ‚urlader‘: base 0x20010000, size 0x00030000

[    0.000000] OF: fdt:Reserved memory (avm): reserved region for property ‚VMB‘: base 0x20000000, size 0x00001000

[    0.000000] OF: fdt:Reserved memory (avm): reserved region for property ‚avm_reboot_string‘: base 0x20001000, size 0x00000200

[    0.000000] Determined physical RAM map:

[    0.000000]  memory: 10000000 @ 30000000 (usable)

[    0.000000]  memory: 0e000000 @ 20000000 (usable)

[    0.000000]  memory: 0000bc01 @ 20fc1038 (reserved)

[    0.000000]  memory: 00040000 @ 2dfc0000 (reserved)

[    0.000000]  memory: 00400000 @ 20100000 (reserved)

[    0.000000]  memory: 00030000 @ 20010000 (reserved)

[    0.000000]  memory: 00001200 @ 20000000 (reserved)

[    0.000000] cma: Reserved 64 MiB at 0x24000000

[    0.000000] SMPCMP: CPU0: cmp_smp_setup

[    0.000000] VPE topology {2,2} total 4

[    0.000000] Detected 3 available secondary CPU(s)

[    0.000000] avm_check_pcache_features: mips-options (preliminary MIPS_CPU_CACHE_CDEX_S flag): 0x000088c40e6d638b icache.flags 0x00000000 dcache.flags 0x00000020

[    0.000000] Primary instruction cache 32kB, VIPT, 4-way, linesize 32 bytes.

[    0.000000] Primary data cache 32kB, 4-way, PIPT, no aliases, linesize 32 bytes

[    0.000000] MIPS secondary cache 256kB, 8-way, linesize 32 bytes.

[    0.000000] avm_check_scache_features: mips-options: 0x000088c40e6d638b

[    0.000000] Zone ranges:

[    0.000000]   DMA      [mem 0x0000000020000000-0x0000000027ffffff]

[    0.000000]   Normal   [mem 0x0000000028000000-0x000000003fffffff]

[    0.000000] Movable zone start for each node

[    0.000000] Early memory node ranges

[    0.000000]   node   0: [mem 0x0000000020000000-0x000000002dffffff]

[    0.000000]   node   0: [mem 0x0000000030000000-0x000000003fffffff]

[    0.000000] Initmem setup node 0 [mem 0x0000000020000000-0x000000003fffffff]

[    0.000000] [fw-info] Version 07.30

[    0.000000] [module-mem] Use 0x284a6000-0x28e55fff (mapped at 884a6000-88e55fff) for 83 modules

[    0.000000] percpu: Embedded 12 pages/cpu s18224 r8192 d22736 u49152

[    0.000000] Built 1 zonelists in Zone order, mobility grouping on.  Total pages: 121728

[    0.000000] Kernel command line: console=ttyLTQ0,115200 audit=1

[    0.000000] audit: enabled (after initialization)

[    0.000000] PID hash table entries: 2048 (order: 1, 8192 bytes)

[    0.000000] Dentry cache hash table entries: 65536 (order: 6, 262144 bytes)

[    0.000000] Inode-cache hash table entries: 32768 (order: 5, 131072 bytes)

[    0.000000] Writing ErrCtl register=00000000

[    0.000000] Readback ErrCtl register=00000000

[    0.000000] Memory: 388420K/491520K available (7764K kernel code, 1538K rwdata, 1708K rodata, 372K init, 6120K bss, 37564K reserved, 65536K cma-reserved)

[    0.000000] SLUB: HWalign=32, Order=0-3, MinObjects=0, CPUs=4, Nodes=1

[    0.000000] Hierarchical RCU implementation.

[    0.000000] NR_IRQS:527

[    0.000000] EIC is off

[    0.000000] VINT is on

[    0.000000] CPU Clock: 1000000000Hz  mips_hpt_frequency 500000000Hz

[    0.000000] clocksource: gptc: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 9556302233 ns

[    0.000009] sched_clock: 32 bits at 200MHz, resolution 5ns, wraps every 10737418237ns

[    0.008424] Calibrating delay loop… 718.84 BogoMIPS (lpj=1437696)

[    0.040921] pid_max: default: 32768 minimum: 301

[    0.045749] Security Framework initialized

[    0.049818] AppArmor: AppArmor initialized

[    0.054006] Mount-cache hash table entries: 1024 (order: 0, 4096 bytes)

[    0.060642] Mountpoint-cache hash table entries: 1024 (order: 0, 4096 bytes)

[    0.069234] CCA is coherent, multi-core is fine

[    0.073680] avm_register_cpuid: cpu_id=0: LINUX core=0 tc=0

[    0.079359] Performance counters: mips/interAptiv PMU enabled, 2 32-bit counters available to each CPU, irq 9

GOT IPI to launch from CPU 1 
GOT IPI to launch from CPU 2 
GOT IPI to launch from CPU 3 
[    0.092722] avm_check_isa_features: isa_level 0x00000031

[    0.092762] avm_check_cpu_features: mips-options (cache flags preliminary!): 0x000088c40e6d638b ases 0x00000030

[    0.092767] avm_check_cpu_features: (preliminary flags: MIPS_CPU_CACHE_CDEX_P MIPS_CPU_PREFETCH MIPS_CPU_INCLUSIVE_CACHES MIPS_CPU_CACHE_CDEX_S)

[    0.092788] avm_check_pcache_features: mips-options (preliminary MIPS_CPU_CACHE_CDEX_S flag): 0x000088c40e6d638b icache.flags 0x00000000 dcache.flags 0x00000020

[    0.092794] Primary instruction cache 32kB, VIPT, 4-way, linesize 32 bytes.

[    0.092800] Primary data cache 32kB, 4-way, PIPT, no aliases, linesize 32 bytes

[    0.092812] MIPS secondary cache 256kB, 8-way, linesize 32 bytes.

[    0.092816] avm_check_scache_features: mips-options: 0x000088c40e6d638b

[    0.093100] CPU1 revision is: 0001a120 (MIPS interAptiv (multi))

[    0.120678] avm_register_cpuid: cpu_id=1: LINUX core=0 tc=1

[    0.122955] avm_check_isa_features: isa_level 0x00000031

[    0.122992] avm_check_cpu_features: mips-options (cache flags preliminary!): 0x000088c40e6d638b ases 0x00000030

[    0.122997] avm_check_cpu_features: (preliminary flags: MIPS_CPU_CACHE_CDEX_P MIPS_CPU_PREFETCH MIPS_CPU_INCLUSIVE_CACHES MIPS_CPU_CACHE_CDEX_S)

[    0.123016] avm_check_pcache_features: mips-options (preliminary MIPS_CPU_CACHE_CDEX_S flag): 0x000088c40e6d638b icache.flags 0x00000000 dcache.flags 0x00000020

[    0.123023] Primary instruction cache 32kB, VIPT, 4-way, linesize 32 bytes.

[    0.123029] Primary data cache 32kB, 4-way, PIPT, no aliases, linesize 32 bytes

[    0.123040] MIPS secondary cache 256kB, 8-way, linesize 32 bytes.

[    0.123044] avm_check_scache_features: mips-options: 0x000088c40e6d638b

[    0.123191] CPU2 revision is: 0001a120 (MIPS interAptiv (multi))

[    0.150958] avm_register_cpuid: cpu_id=2: LINUX core=1 tc=0

[    0.153232] avm_check_isa_features: isa_level 0x00000031

[    0.153269] avm_check_cpu_features: mips-options (cache flags preliminary!): 0x000088c40e6d638b ases 0x00000030

[    0.153273] avm_check_cpu_features: (preliminary flags: MIPS_CPU_CACHE_CDEX_P MIPS_CPU_PREFETCH MIPS_CPU_INCLUSIVE_CACHES MIPS_CPU_CACHE_CDEX_S)

[    0.153291] avm_check_pcache_features: mips-options (preliminary MIPS_CPU_CACHE_CDEX_S flag): 0x000088c40e6d638b icache.flags 0x00000000 dcache.flags 0x00000020

[    0.153297] Primary instruction cache 32kB, VIPT, 4-way, linesize 32 bytes.

[    0.153303] Primary data cache 32kB, 4-way, PIPT, no aliases, linesize 32 bytes

[    0.153313] MIPS secondary cache 256kB, 8-way, linesize 32 bytes.

[    0.153317] avm_check_scache_features: mips-options: 0x000088c40e6d638b

[    0.153444] CPU3 revision is: 0001a120 (MIPS interAptiv (multi))

[    0.181255] avm_register_cpuid: cpu_id=3: LINUX core=1 tc=1

[    0.181525] Brought up 4 CPUs

[    0.430175] avm_yield_setup: YIELD_PCMFRAME_ID       : id=0x0004000f: cpu=0 tc=4 prio=3 signal=15

[    0.439108] avm_yield_setup: YIELD_PCMLINK_ID        : id=0x0003000c: cpu=0 tc=3 prio=2 signal=12

[    0.448049] avm_yield_setup: YIELD_MONITOR_IPI0_ID   : id=0x0002000e: cpu=0 tc=2 prio=1 signal=14

[    0.449560] random: fast init done

[    0.460461] avm_yield_setup: YIELD_PROFILE_IPI0_ID   : id=0x0002000d: cpu=0 tc=2 prio=1 signal=13

[    0.469854] [0][yield_context_init] cpu=0 tc=2 mask=6000 tc_prio=1

[    0.476307] [0][yield_context_init] cpu=0 tc=3 mask=1000 tc_prio=2

[    0.482756] [0][yield_context_init] cpu=0 tc=4 mask=8000 tc_prio=3

[    0.488985] avm_yield_setup: YIELD_MONITOR_IPI1_ID   : id=0x0202000e: cpu=2 tc=2 prio=1 signal=14

[    0.497753] avm_yield_setup: YIELD_PROFILE_IPI1_ID   : id=0x0202000d: cpu=2 tc=2 prio=1 signal=13

[    0.506717] avm_yield_setup: YIELD_GPTC_ID           : id=0x02030002: cpu=2 tc=3 prio=3 signal= 2

[    0.515962] [2][yield_context_init] cpu=2 tc=2 mask=6000 tc_prio=1

[    0.522357] [2][yield_context_init] cpu=2 tc=3 mask=0004 tc_prio=3

[    0.529380] devtmpfs: initialized

[    0.542753] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 7645041785100000 ns

[    0.552746] futex hash table entries: 1024 (order: 3, 32768 bytes)

[    0.563872] pinctrl core: initialized pinctrl subsystem

[    0.570329] NET: Registered protocol family 16

[    0.578141] dma-grx500 1e300000.dma: dma3 base address be300000 chained_irq 24 irq_base 25

[    0.589089] dma-grx500 1e300000.dma: Init done - rev: a, ports: 1, channels: 64

[    0.599019] dma-grx500 1c100000.dma: dma2tx base address bc100000 chained_irq 100 irq_base 101

[    0.609122] dma-grx500 1c100000.dma: Init done - rev: a, ports: 1, channels: 16

[    0.616887] dma-grx500 1c200000.dma: dma2rx base address bc200000 chained_irq 117 irq_base 118

[    0.627387] dma-grx500 1c200000.dma: Init done - rev: a, ports: 1, channels: 32

[    0.635531] dma-grx500 1a100000.dma: dma1tx base address ba100000 chained_irq 150 irq_base 151

[    0.645619] dma-grx500 1a100000.dma: Init done - rev: a, ports: 1, channels: 16

[    0.653389] dma-grx500 1a200000.dma: dma1rx base address ba200000 chained_irq 167 irq_base 168

[    0.663346] dma-grx500 1a200000.dma: Init done - rev: a, ports: 1, channels: 12

[    0.676936] dma0-grx500 16e00000.dma: base address b6e00000 chained_irq 215 irq_base 216

[    0.684953] dma0-grx500 16e00000.dma: Init done - hw rev: A, ports: 4, channels: 16

[    0.692934] intel-pinctrl 16c80000.pinctrl: pinbank id: 0, reg: 0xb6c80000, pinbase: 0, pin number: 32, pinmap: 0xf1efefff

[    0.703893] intel-pinctrl 16c80000.pinctrl: pinbank id: 1, reg: 0xb6c80100, pinbase: 32, pin number: 32, pinmap: 0x3bff0c1f

[    0.715283] intel-pinctrl 16c80000.pinctrl: Total 10 groups, 8 functions

[    0.722714] intel-pinctrl 16c80000.pinctrl: gpiochip membase: 0xb6c00000

[    0.729908] intel-pinctrl 16c80000.pinctrl: gpiochip membase: 0xb6c00100

[    0.746113] gic_timer_probe

[    0.748920] gic_timer_probe: irq=284 freq=1000000000

[    0.787778] avm_alloc_page_extension node_extension_table[0] entries=131072 (size=524288)  alloced

[    0.796706] Reboot Status is: Power-On 

[    0.800906] cqm_platdev_init is called

[    0.804491] dev falcon-cqm

[    0.807248] [parse_dts] .. [30]

[    0.810551] Unable to get node cqm for falcon-cqm

[    0.815252] add_cqm_dev(#116): parse_dts fail for falcon-cqm

[    0.820981] dev grx500-cbm

[    0.823756] [parse_dts] .. [30]

[    0.827047] num_res 12

[    0.829421] intr 89

[    0.831584] intr 90

[    0.833732] intr 91

[    0.835928] intr 92

[    0.838072] intr 93

[    0.840258] intr 0

[    0.842319] No rcu reset for cbm

[    0.845671] No syscon phandle specified for wan mux

[    0.850579] parse dts done

[    0.853369] adding resources

[    0.856296] resources added

[    0.859396]  Successfully Registered Platform device grx500-cbm.

[    0.865273] device added

[    0.937518] [cbm] { cbm_xrx500_probe : 5557 }reserving 18874368 bytes @ 84000000 for CBM

[    0.976696] [cbm] { cbm_xrx500_probe : 5567 }reserving 8388608 bytes @ 85200000 for CBM

[    0.984647] [cbm] { cbm_xrx500_probe : 5575 }89 irq

[    0.989692] [cbm] { cbm_xrx500_probe : 5598 }2

[    0.994119] [drv_tmu_ll] { get_cbm_clock : 7605 }CBM Clock: 600000000Hz=600MHZ

[    1.001391] Initializing TMU with Base Address=be700000: …

[    1.009990] TMU Initialization Done

[    1.013325] 0x84000000 0x1200000 0x800

[    1.017149] 0x84000000 0x1200000

[    1.020420] 0x85200000 0x800000 0x2000

[    1.024257] 0x85200000 0x800000

[    1.027770] [cbm] { init_fsqm_buf_std : 1138 }init fsqm std successfully

[    1.034339] [cbm] { init_fsqm_buf_jumbo : 1178 }init fsqm jbo successfully

[    1.041247] [cbm] { init_fsqm : 1201 }fsqm init successfully

[    1.046980] [cbm] { init_cbm_basic : 1236 }PHY ADDR STD 0x24000000

[    1.053226] [cbm] { init_cbm_basic : 1237 }PHY ADDR JBO 0x25200000

[    1.059706] [cbm] { init_cbm_basic : 1255 }init basic CBM successfully

[    1.066085] [cbm] { cbm_hw_init : 2156 }CBM HW init

[    1.071133] [cbm] { setup_DMA_p2p : 4992 }setup_DMA_p2p executed

[    1.077114] [cbm] { reserved_ports_highest : 5051 }2 2 19 35

[    1.082836] [cbm] { init_cbm_dqm_cpu_port : 1402 }2

[    1.087819] [cbm] { assign_port_from_DT : 631 }0x0 2

[    1.092828] [cbm] { assign_port_from_DT : 631 }0x20 2

[    1.098132] [cbm] { cbm_add_to_list : 427 }1

[    1.102283] [cbm] { reserved_ports_highest : 5051 }1 1 18 34

[    1.108011] [cbm] { init_cbm_dqm_cpu_port : 1402 }1

[    1.112965] [cbm] { assign_port_from_DT : 631 }0x80 1

[    1.118086] [cbm] { reserved_ports_highest : 5051 }3 3 20 36

[    1.123805] [cbm] { init_cbm_dqm_cpu_port : 1402 }3

[    1.128770] [cbm] { assign_port_from_DT : 631 }0x2000000 3

[    1.134310] [cbm] { cbm_add_to_list : 427 }1

[    1.138658] [cbm] { reserved_ports_highest : 5051 }6 6 0 16

[    1.144293] [cbm] { dma_port_enable : 4560 }6 0x4

[    1.149084] [cbm] { reserved_ports_highest : 5051 }7 7 1 17

[    1.154708] [cbm] { dma_port_enable : 4560 }7 0x4

[    1.159499] [cbm] { reserved_ports_highest : 5051 }8 8 2 18

[    1.165134] [cbm] { dma_port_enable : 4560 }8 0x4

[    1.169914] [cbm] { reserved_ports_highest : 5051 }9 9 3 19

[    1.175541] [cbm] { dma_port_enable : 4560 }9 0x4

[    1.180332] [cbm] { reserved_ports_highest : 5051 }10 10 4 20

[    1.186130] [cbm] { dma_port_enable : 4560 }10 0x4

[    1.191008] [cbm] { reserved_ports_highest : 5051 }11 11 5 21

[    1.196807] [cbm] { dma_port_enable : 4560 }11 0x4

[    1.201685] [cbm] { reserved_ports_highest : 5051 }12 12 6 22

[    1.207484] [cbm] { dma_port_enable : 4560 }12 0x4

[    1.212362] [cbm] { reserved_ports_highest : 5051 }13 13 7 23

[    1.218161] [cbm] { dma_port_enable : 4560 }13 0x4

[    1.223038] [cbm] { reserved_ports_highest : 5051 }14 14 8 24

[    1.228837] [cbm] { dma_port_enable : 4560 }14 0x4

[    1.233719] [cbm] { reserved_ports_highest : 5051 }15 15 9 25

[    1.239523] [cbm] { dma_port_enable : 4560 }15 0x4

[    1.244391] [cbm] { reserved_ports_highest : 5051 }16 16 10 26

[    1.250277] [cbm] { dma_port_enable : 4560 }16 0x4

[    1.255151] [cbm] { reserved_ports_highest : 5051 }17 17 11 27

[    1.261041] [cbm] { dma_port_enable : 4560 }17 0x4

[    1.265914] [cbm] { reserved_ports_highest : 5051 }18 18 -16 0

[    1.271805] [cbm] { dma_port_enable : 4560 }18 0x4

[    1.276693] [cbm] { reserved_ports_highest : 5051 }19 19 12 28

[    1.282569] [cbm] { dma_port_enable : 4560 }19 0x4

[    1.287441] [cbm] { reserved_ports_highest : 5051 }20 20 13 29

[    1.293332] [cbm] { dma_port_enable : 4560 }20 0x4

[    1.298203] [cbm] { init_special_ports : 5058 }20

[    1.302969] [cbm] { cbm_add_to_list : 427 }1

[    1.307311] [cbm] { reserved_ports_highest : 5051 }21 21 14 30

[    1.313209] [cbm] { dma_port_enable : 4560 }21 0x4

[    1.318082] [cbm] { init_special_ports : 5058 }21

[    1.322844] [cbm] { cbm_add_to_list : 427 }1

[    1.327188] [cbm] { reserved_ports_highest : 5051 }22 22 25 41

[    1.333087] [cbm] { dma_port_enable : 4560 }22 0x4

[    1.337961] [cbm] { reserved_ports_highest : 5051 }23 23 15 31

[    1.343851] [cbm] { init_cbm_dqm_ldma_port : 1441 }23

[    1.348985] [cbm] { reserved_ports_highest : 5051 }5 5 21 37

[    1.354702] [cbm] { init_cbm_dqm_scpu_port : 1422 }5

[    1.359922] [cbm] { reserved_ports_highest : 5051 }4 4 16 32

[    1.365465] [cbm] { init_cbm_dqm_cpu_port : 1402 }4

[    1.370424] [cbm] { assign_port_from_DT : 631 }0x18 4

[    1.375535] [cbm] { reserved_ports_highest : 5051 }24 24 22 38

[    1.381437] [cbm] { init_cbm_dqm_cpu_port : 1402 }24

[    1.386480] [cbm] { assign_port_from_DT : 631 }0x8 24

[    1.391596] [cbm] { reserved_ports_highest : 5051 }25 25 23 39

[    1.397498] [cbm] { init_cbm_dqm_cpu_port : 1402 }25

[    1.402541] [cbm] { assign_port_from_DT : 631 }0x8 25

[    1.407653] [cbm] { reserved_ports_highest : 5051 }26 26 24 40

[    1.413555] [cbm] { init_cbm_dqm_cpu_port : 1402 }26

[    1.418596] [cbm] { assign_port_from_DT : 631 }0x8 26

[    1.423711] [cbm] { init_cbm_eqm_cpu_port : 1262 }0

[    1.428656] [cbm] { init_cbm_eqm_cpu_port : 1262 }1

[    1.433611] [cbm] { init_cbm_eqm_cpu_port : 1262 }2

[    1.438552] [cbm] { init_cbm_eqm_cpu_port : 1262 }3

[    1.443503] [cbm] { dma_port_enable : 4560 }5 0x1

[    1.448282] [cbm] { dma_port_enable : 4560 }5 0x2

[    1.453053] [cbm] { dma_port_enable : 4560 }6 0x1

[    1.457824] [cbm] { dma_port_enable : 4560 }6 0x2

[    1.462599] [cbm] { dma_port_enable : 4560 }7 0x1

[    1.467372] [cbm] { dma_port_enable : 4560 }7 0x2

[    1.472149] [cbm] { dma_port_enable : 4560 }8 0x1

[    1.476920] [cbm] { dma_port_enable : 4560 }8 0x2

[    1.481697] [cbm] { dma_toe_port_enable : 4587 }9 0x1

[    1.486816] [cbm] { dma_vrx318_port_enable : 4599 }15 0x1

[    1.492297] [cbm] { init_cbm_dqm_cpu_port : 1402 }0

[    1.497230] [cbm] { init_cbm_dqm_cpu_port : 1402 }1

[    1.502180] [cbm] { init_cbm_dqm_cpu_port : 1402 }2

[    1.507126] [cbm] { init_cbm_dqm_cpu_port : 1402 }3

[    1.512077] Load spreader init successfully

[    1.516475] [cbm] { cbm_xrx500_probe : 5654 }CBM Clock: 600000000Hz

[    1.522670] [cbm] { cbm_xrx500_probe : 5656 }EQM delay Enabled

[    1.528567] [cbm] { igp_delay_set : 4672 }port0 delay16

[    1.533864] [cbm] { igp_delay_set : 4672 }port1 delay16

[    1.539156] [cbm] { igp_delay_set : 4672 }port2 delay16

[    1.544454] [cbm] { igp_delay_set : 4672 }port3 delay16

[    1.549746] [cbm] { igp_delay_set : 4672 }port4 delay16

[    1.555043] [cbm] { igp_delay_set : 4672 }port5 delay16

[    1.560337] [cbm] { igp_delay_set : 4672 }port6 delay16

[    1.565633] [cbm] { igp_delay_set : 4672 }port7 delay16

[    1.570926] [cbm] { igp_delay_set : 4672 }port8 delay16

[    1.576223] [cbm] { igp_delay_set : 4672 }port9 delay16

[    1.581516] [cbm] { igp_delay_set : 4672 }port10 delay16

[    1.586900] [cbm] { igp_delay_set : 4672 }port11 delay16

[    1.592279] [cbm] { igp_delay_set : 4672 }port12 delay16

[    1.597664] [cbm] { igp_delay_set : 4672 }port13 delay16

[    1.603043] [cbm] { igp_delay_set : 4672 }port14 delay16

[    1.608427] [cbm] { igp_delay_set : 4672 }port15 delay16

[    1.613808] [cbm] { dequeue_dma_port_init : 4526 }6 0x0 2 1

[    1.619462] [cbm] { dequeue_dma_port_init : 4526 }7 0x0 2 2

[    1.625095] [cbm] { dequeue_dma_port_init : 4526 }8 0x0 2 3

[    1.630740] [cbm] { dequeue_dma_port_init : 4526 }9 0x0 2 4

[    1.636382] [cbm] { dequeue_dma_port_init : 4526 }10 0x0 2 5

[    1.642111] [cbm] { dequeue_dma_port_init : 4526 }11 0x0 2 6

[    1.647838] [cbm] { dequeue_dma_port_init : 4526 }12 0x0 2 9

[    1.653569] [cbm] { dequeue_dma_port_init : 4526 }13 0x0 2 10

[    1.659383] [cbm] { dequeue_dma_port_init : 4526 }14 0x0 2 11

[    1.665201] [cbm] { dequeue_dma_port_init : 4526 }15 0x0 2 12

[    1.671014] [cbm] { dequeue_dma_port_init : 4526 }16 0x0 2 13

[    1.676833] [cbm] { dequeue_dma_port_init : 4526 }17 0x0 2 14

[    1.682646] [cbm] { dequeue_dma_port_init : 4526 }18 0x0 1 13

[    1.688465] [cbm] { dequeue_dma_port_init : 4526 }19 0x0 1 15

[    1.694278] [cbm] { dequeue_dma_port_init : 4526 }20 0x0 1 5

[    1.700009] [cbm] { dequeue_dma_port_init : 4526 }21 0x0 1 6

[    1.705735] [cbm] { dequeue_dma_port_init : 4526 }22 0x0 1 11

[    1.711563] [cbm] { enqueue_dma_port_init : 4471 }5 0x2 2 0 30

[    1.717463] [cbm] { enqueue_dma_port_init : 4471 }5 0x1 2 14 0

[    1.723359] [cbm] { enqueue_dma_port_init : 4471 }6 0x2 2 0 31

[    1.729261] [cbm] { enqueue_dma_port_init : 4471 }6 0x1 2 15 0

[    1.735164] [cbm] { enqueue_dma_port_init : 4471 }7 0x2 1 0 6

[    1.740980] [cbm] { enqueue_dma_port_init : 4471 }7 0x1 1 0 0

[    1.746796] [cbm] { enqueue_dma_port_init : 4471 }8 0x2 1 0 11

[    1.752697] [cbm] { enqueue_dma_port_init : 4471 }8 0x1 1 5 0

[    1.758544] [cbm] { cbm_xrx500_probe : 5715 }CBM: Init Done !![    1.765231] pstore: using zlib compression

[    1.769239] pstore: Registered ramoops as persistent store backend

[    1.775434] ramoops: attached 0x400000@0x20100000, ecc: 0/0

[    1.812218] SCSI subsystem initialized

[    1.816512] usbcore: registered new interface driver usbfs

[    1.822053] usbcore: registered new interface driver hub

[    1.827448] usbcore: registered new device driver usb

[    1.833160] mp8864 0-0068: MP8864 probe started.

[    1.842752] mp8864 0-0068: [MP8864 Init] Status is 0x11 Vsel is 0x37 Syscntl is 0xa5

[    1.850378] i2c-gpio i2c: using pins 501 (SDA) and 502 (SCL)

[    1.856255] try to register spd_mon driver[    1.860259] spdmon 16080110.speedm: base address: 0xb6080110	

[    1.865872] spdmon 16080110.speedm: PHY base address: 0x16080110

[    1.871925] device number :253

[    1.875729] spdmon 16080110.speedm: spd_mon driver : init done !!

[    1.886275] spd_mon driver registered

[    1.890782] AVM PA for Linux version 4.9.198 (jenkins@jenkins-ci.avm.de) (gcc version 8.3.0 (Buildroot 2018.11.4-gc73018b701) ) #1 SMP 2021-07-20

[    1.890782]  (early init)

[    1.906928] NET: Registered protocol family 8

[    1.911190] NET: Registered protocol family 20

[    1.916358] clocksource: Switched to clocksource gptc

[    1.944030] AppArmor: AppArmor Filesystem Enabled

[    1.951820] NET: Registered protocol family 2

[    1.976618] TCP established hash table entries: 4096 (order: 2, 16384 bytes)

[    1.983626] TCP bind hash table entries: 4096 (order: 3, 32768 bytes)

[    1.990115] TCP: Hash tables configured (established 4096 bind 4096)

[    1.996562] UDP hash table entries: 256 (order: 1, 8192 bytes)

[    2.002395] UDP-Lite hash table entries: 256 (order: 1, 8192 bytes)

[    2.009088] avm_pa: try to activate hw accelaration for pid 3 (ipv4) called from avm_pa_dev_pidhandle_register_with_ingress

[    2.020125] NET: Registered protocol family 1

[    2.025774] yield_probe: cpu 0 irq 272

[    2.029607] yield_probe: cpu 1 irq 273

[    2.033583] yield_probe: cpu 2 irq 274

[    2.037272] yield_probe: cpu 3 irq 275

[    2.041271] yield_probe: interrupts set up

[    2.047201] audit: initializing netlink subsys (enabled)

[    2.052504] audit: type=2000 audit(1.520:1): initialized

[    2.058646] workingset: timestamp_bits=14 max_order=17 bucket_order=3

[    2.081860] squashfs: version 4.0 (2009/01/31) Phillip Lougher

[    2.087582] ANTFS Module: Version 2.46

[    2.091595] jffs2: version 2.2 (NAND) (SUMMARY) (LZMA) (RTIME) (CMODE_PRIORITY) (c) 2001-2006 Red Hat, Inc.

[    2.101973] fuse init (API version 7.26)

[    2.113023] io scheduler noop registered

[    2.116809] io scheduler deadline registered (default)

[    2.122446] bthelper_probe: core 0 initialized

[    2.126750] bthelper_probe: core 1 initialized

[    2.132096] intel-pcie-slim-phy 18500000.pciephy: PCIe slim phy[0] init success!

[    2.139615] intel-pcie-slim-phy 18000000.pciephy: PCIe slim phy[1] init success!

[    2.147093] intel-pcie-slim-phy 18a00000.pciephy: PCIe slim phy[2] init success!

[    2.154807] 1a400000.phy supply vbus not found, using dummy regulator

[    2.161496] 1a600000.phy supply vbus not found, using dummy regulator

[    2.276371] OF: PCI: host bridge /pcie@18900000 ranges:

[    2.281502] OF: PCI:   MEM 0xb8000000..0xbaffffff -> 0xb8000000

[    2.287450] OF: PCI:    IO 0xbb800000..0xbb80ffff -> 0xbb800000

[    2.295782] intel-pcie-slim-phy 18500000.pciephy: PCIe LCPLL SSC Mode Enabled

[    3.140474] random: crng init done

[    3.408381] intel-pcie 18900000.pcie: intel_pcie_wait_phy_link_up port 0 timeout

[    3.416941] intel-pcie: probe of 18900000.pcie failed with error -145

[    3.528369] OF: PCI: host bridge /pcie@18400000 ranges:

[    3.533457] OF: PCI:   MEM 0xb4000000..0xb6ffffff -> 0xb4000000

[    3.539435] OF: PCI:    IO 0xb7800000..0xb780ffff -> 0xb7800000

[    3.547729] intel-pcie-slim-phy 18000000.pciephy: PCIe LCPLL SSC Mode Enabled

[    3.687248] intel-pcie 18400000.pcie: PCI host bridge to bus 0001:00

[    3.693489] pci_bus 0001:00: root bus resource [bus 00-08]

[    3.699003] pci_bus 0001:00: root bus resource [mem 0xb4000000-0xb6ffffff]

[    3.705945] pci_bus 0001:00: root bus resource [io  0xb7800000-0xb780ffff]

[    3.713315] pci 0001:00:00.0: bridge configuration invalid ([bus 00-00]), reconfiguring

[    3.721805] pci 0001:00:00.0: PCI bridge to [bus 01-08]

[    3.727137] pci 0001:00:00.0: BAR 8: assigned [mem 0xb4000000-0xb41fffff]

[    3.733771] pci 0001:00:00.0: BAR 9: assigned [mem 0xb4200000-0xb42fffff pref]

[    3.741065] pci 0001:00:00.0: BAR 7: assigned [io  0xb7800000-0xb7800fff]

[    3.747929] pci 0001:01:00.0: BAR 0: assigned [mem 0xb4000000-0xb41fffff 64bit]

[    3.755307] pci 0001:00:00.0: PCI bridge to [bus 01]

[    3.760341] pci 0001:00:00.0:   bridge window [io  0xb7800000-0xb7800fff]

[    3.767185] pci 0001:00:00.0:   bridge window [mem 0xb4000000-0xb41fffff]

[    3.774043] pci 0001:00:00.0:   bridge window [mem 0xb4200000-0xb42fffff pref]

[    3.781469] pcieport 0001:00:00.0: enabling device (0000 -> 0003)

[    3.787717] intel-pcie 18400000.pcie: Intel AXI PCIe Root Complex Port 1 Init Done

[    3.900358] OF: PCI: host bridge /pcie@18e00000 ranges:

[    3.905463] OF: PCI:   MEM 0xbc000000..0xbeffffff -> 0xbc000000

[    3.911428] OF: PCI:    IO 0xbf800000..0xbf80ffff -> 0xbf800000

[    3.918523] intel-pcie-slim-phy 18a00000.pciephy: SSC has been enabled, count: 2!

[    4.034663] intel-pcie 18e00000.pcie: PCI host bridge to bus 0002:00

[    4.040898] pci_bus 0002:00: root bus resource [bus 00-08]

[    4.046421] pci_bus 0002:00: root bus resource [mem 0xbc000000-0xbeffffff]

[    4.053364] pci_bus 0002:00: root bus resource [io  0xbf800000-0xbf80ffff]

[    4.060736] pci 0002:00:00.0: bridge configuration invalid ([bus 00-00]), reconfiguring

[    4.069315] pci 0002:00:00.0: PCI bridge to [bus 01-08]

[    4.074700] pci 0002:00:00.0: BAR 9: assigned [mem 0xbc000000-0xbc7fffff pref]

[    4.081770] pci 0002:00:00.0: BAR 8: assigned [mem 0xbc800000-0xbc8fffff]

[    4.088632] pci 0002:00:00.0: BAR 7: assigned [io  0xbf800000-0xbf800fff]

[    4.095496] pci 0002:01:00.0: BAR 0: assigned [mem 0xbc000000-0xbc7fffff pref]

[    4.102781] pci 0002:00:00.0: PCI bridge to [bus 01]

[    4.107803] pci 0002:00:00.0:   bridge window [io  0xbf800000-0xbf800fff]

[    4.114667] pci 0002:00:00.0:   bridge window [mem 0xbc800000-0xbc8fffff]

[    4.121524] pci 0002:00:00.0:   bridge window [mem 0xbc000000-0xbc7fffff pref]

[    4.128950] pcieport 0002:00:00.0: enabling device (0000 -> 0003)

[    4.135182] intel-pcie 18e00000.pcie: Intel AXI PCIe Root Complex Port 2 Init Done

[    4.144596] UMT initialize success on processor: 0 !

[    4.149424] HW MCPY driver: Version: 1.1.0, Init Done!

[    4.155633] 16600000.serial: ttyLTQ0 at MMIO 0x16600000 (irq = 210, base_baud = 0) is a lantiq,asc

[    4.164730] console [ttyLTQ0] enabled
[    4.164730] console [ttyLTQ0] enabled

[    4.171923] bootconsole [early0] disabled
[    4.171923] bootconsole [early0] disabled

[    4.181325] avm_net_trace: Up and running.
[    4.184667] [loadcontrol] set auto - scale=1
[    4.188210] [avm] configured: watchdog event debug [    4.192926] 
[    4.194368] AVM_WATCHDOG: Watchdog Driver for AR7 Hardware (Version 1.0)
[    4.201271] ar7wdt_hw_shim: ar7wdt_hw_init: No watchdog device available (yet)
[    4.208606] Register push button event to receive the set_factory_kernel event
[    4.234036] zram: Added device: zram0
[    4.238078] nand: device found, Manufacturer ID: 0x98, Chip ID: 0xdc
[    4.243016] nand: Toshiba NAND 512MiB 3,3V 8-bit
[    4.247589] nand: 512 MiB, SLC, erase size: 256 KiB, page size: 4096, OOB size: 128
[    4.255233] try_avm_ecc_fixup: AVM ecc fixup is not yet implemented - skipping check
[    4.262961] Scanning device for bad blocks
[    4.587253] Bad eraseblock 1298 at 0x000014480000
[    4.649043] Bad eraseblock 1536 at 0x000018000000
[    4.652397] Bad eraseblock 1537 at 0x000018040000
[    4.782668] 5 ofpart partitions found on MTD device 17c00000.nand-parts
[    4.787822] Creating 5 MTD partitions on „17c00000.nand-parts“:
[    4.793760] 0x000000500000-0x000000d00000 : „kernel“
[    4.800779] 0x000000000000-0x000000100000 : „urlader“
[    4.806134] 0x000000100000-0x000000500000 : „nand-tffs“
[    4.811682] 0x000000d00000-0x000001500000 : „reserved-kernel“
[    4.817875] 0x000001500000-0x000020000000 : „ubi“
[    4.825754] [TFFS3_Register_Panic_CB] registering panic callback for mtd 17c00000.nand-parts
[    4.833766] libphy: Fixed MDIO Bus: probed
[    4.837599] Node name /ssx1@1c000000/gswitch@000000
[    4.842749] Node name /ssx2@1a000000/gswitch@000000
[    4.848202] ::::::: SWAPI Reached :::::: 
[    4.850797] GSWIP devid = 0
[    4.853537] memres->start = 0x1c000000 memres->end = 0x1c002fff
[    4.859554] addr_gswl = 0xbc000000
[    4.862829] /GU/KERNEL_grx5_build/linux/drivers/net/ethernet/lantiq/switch-api/gsw_init.c:ltq_gsw_api_register:933 (Register l base:0xbc000000)
[    4.875701] SWAPI: Registered char device [switch_api] with major no [81]
[    4.882445] addr_gswl = 0xbc000000
[    4.885841] 
[    4.885841] ########## Switch Core INIT for device = 0 ##########
[    4.893390] Switch Core Base Address = 0xbc000000
[    4.898081] 
[    4.898081] GSWIP 3.0 HardWare Capability
[    4.903540] ——————————————
[    4.903540] 
[    4.909010] Switch Version ID                =  0x30
[    4.913953] 
[    4.915414] Number of logical port           =  7
[    4.920121] Number of ports including V port =  8
[    4.924810] Number of queues                 =  32
[    4.929580] Number of meter instance         =  16
[    4.934358] Number of shapers                =  32
[    4.939130] Number of PMAC                   =  1
[    4.943823] Number of CPU PORT               =  0
[    4.948508] 
[    4.949964] PPPOE table size                 =  16
[    4.954760] IP packet length table size      =  16
[    4.959526] Protocol table size              =  32
[    4.964322] MAC DA/SA table size             =  64
[    4.969081] Application table size           =  64
[    4.973849] IP DA/SA MSB table size          =  64
[    4.978630] IP DA/SA LSB table size          =  64
[    4.983398] Multicast table size             =  64
[    4.988179] Multicast Hw Snoop               =  0
[    4.992867] TFLOW table size                 =  64
[    4.997635] MAC bridge table size            =  2048
[    5.002594] TFLOW RMON counter table Size    =  256
[    5.007453] Payload Table Size               =  64
[    5.012224] Extend VLAN Table Size table     =  0
[    5.016913] VlanFilter table Size            =  0
[    5.016913] 
[    5.023073] 
[    5.024581] Enter PCE micro-code init
[    5.028449] Exit PCE micro-code init
[    5.031737] Switch API: PCE MicroCode loaded !!
[    5.036413] ::::::: SWAPI Reached :::::: 
[    5.040244] GSWIP devid = 1
[    5.043047] memres->start = 0x1a000000 memres->end = 0x1a002fff
[    5.049006] addr_gswr = 0xba000000
[    5.052338] /GU/KERNEL_grx5_build/linux/drivers/net/ethernet/lantiq/switch-api/gsw_init.c:ltq_gsw_api_register:944 (Register r base:0xba000000)
[    5.065188] 
[    5.065188] ########## Switch Core INIT for device = 1 ##########
[    5.072734] Switch Core Base Address = 0xba000000
[    5.077427] 
[    5.077427] GSWIP 3.0 HardWare Capability
[    5.082881] ——————————————
[    5.082881] 
[    5.088357] Switch Version ID                =  0x30
[    5.093303] 
[    5.094759] Number of logical port           =  2
[    5.099462] Number of ports including V port =  17
[    5.104242] Number of queues                 =  32
[    5.109018] Number of meter instance         =  64
[    5.113785] Number of shapers                =  32
[    5.118569] Number of PMAC                   =  1
[    5.123255] Number of CPU PORT               =  0
[    5.127940] 
[    5.129423] PPPOE table size                 =  16
[    5.134193] IP packet length table size      =  16
[    5.138965] Protocol table size              =  32
[    5.143740] MAC DA/SA table size             =  64
[    5.148520] Application table size           =  64
[    5.153289] IP DA/SA MSB table size          =  64
[    5.158063] IP DA/SA LSB table size          =  64
[    5.162837] Multicast table size             =  64
[    5.167612] Multicast Hw Snoop               =  0
[    5.172304] TFLOW table size                 =  512
[    5.177166] MAC bridge table size            =  2048
[    5.182109] TFLOW RMON counter table Size    =  256
[    5.186969] Payload Table Size               =  64
[    5.191744] Extend VLAN Table Size table     =  0
[    5.196433] VlanFilter table Size            =  0
[    5.196433] 
[    5.202594] 
[    5.204072] Enter PCE micro-code init
[    5.207974] Exit PCE micro-code init
[    5.211276] Switch API: PCE MicroCode loaded !!
[    5.222001] lro_sram_membase_res0 from DT: a2013000 
[    5.225806] ltq_toe_membase: e2000000 and lro_sram_membase_res0: e2013000
[    5.232940] TOE Init Done !!
[    5.880938] i2c /dev entries driver
[    5.886245] grx500wdt 12000000.watchdog: [grx500wdt_probe]:[325] cpu_clk=1000000000
[    5.892546] grx500wdt 12000000.watchdog: [grx500wdt_probe]WDT reset is Bit31, RCU_IAP_WDT_RST_STAT=0x21000c08
[    5.902365] grx500wdt 12000000.watchdog: [grx500wdt_probe]Not WDT reset.
[    5.909054] grx500wdt 12000000.watchdog: [grx500wdt_probe]:[373] wdd = 88e5c2d0
[    5.916364] watchdog: AVM driver enabled, not creating device file #0 for Hardware Watchdog for GRX500
[    5.925621] ar7wdt_hw_shim: Device #0 attached (Hardware Watchdog for GRX500)
[    5.932732] ar7wdt_hw_shim: Starting watchdog
[    5.937087] grx500wdt 12000000.watchdog: [grx500wdt_probe]:[373] wdd = 88e682d0
[    5.944370] watchdog: AVM driver enabled, not creating device file #1 for Hardware Watchdog for GRX500
[    5.953657] ar7wdt_hw_shim: Device #1 attached (Hardware Watchdog for GRX500)
[    5.960774] ar7wdt_hw_shim: Starting watchdog
[    5.965134] grx500wdt 12000000.watchdog: [grx500wdt_probe]:[373] wdd = 88e742d0
[    5.972410] watchdog: AVM driver enabled, not creating device file #2 for Hardware Watchdog for GRX500
[    5.981695] ar7wdt_hw_shim: Device #2 attached (Hardware Watchdog for GRX500)
[    5.988809] ar7wdt_hw_shim: Starting watchdog
[    5.993163] grx500wdt 12000000.watchdog: [grx500wdt_probe]:[373] wdd = 88e802d0
[    6.000446] watchdog: AVM driver enabled, not creating device file #3 for Hardware Watchdog for GRX500
[    6.009734] ar7wdt_hw_shim: Device #3 attached (Hardware Watchdog for GRX500)
[    6.016848] ar7wdt_hw_shim: Starting watchdog
[    6.021203] grx500wdt 12000000.watchdog: H/w Watchdog Timer: (max 4) (nowayout= 0)
[    6.035001] AVM PA for Linux Linux version 4.9.198 (jenkins@jenkins-ci.avm.de) (gcc version 8.3.0 (Buildroot 2018.11.4-gc73018b701) ) #1 SMP 2021-07-20
[    6.035001]  (late init)
[    6.050324] Mirror/redirect action on
[    6.053397] u32 classifier
[    6.055971]     Performance counters on
[    6.059816]     input device check on
[    6.063459]     Actions configured
[    6.067159] ipip: IPv4 and MPLS over IPv4 tunneling driver
[    6.073475] Initializing XFRM netlink socket
[    6.076688] IPsec XFRM device driver
[    6.081490] NET: Registered protocol family 10
[    6.086683] avm_pa: try to activate hw accelaration for pid 4 (ipv6) called from avm_pa_dev_pidhandle_register_with_ingress
[    6.096633] NET: Registered protocol family 17
[    6.101002] Bridge flood ratelimiter registered
[    6.105411] bridge: filtering via arp/ip/ip6tables is no longer available by default. Update your scripts to load br_netfilter if you need this.
[    6.118300] lec:lane_module_init: lec.c: initialized
[    6.123215] mpoa:atm_mpoa_init: mpc.c: initialized
[    6.128027] KOAM is loaded successfully.
[    6.131939] l2tp_core: L2TP core driver, V2.0
[    6.136229] l2tp_ip: L2TP IP encapsulation support (L2TPv3)
[    6.141865] l2tp_netlink: L2TP netlink interface
[    6.146466] l2tp_eth: L2TP ethernet pseudowire support (L2TPv3)
[    6.152294] l2tp_ip6: L2TP IP encapsulation support for IPv6 (L2TPv3)
[    6.159169] 8021q: 802.1Q VLAN Support v1.8
[    6.165198] audit: type=1400 audit(5.632:2): apparmor=„STATUS“ info=„AppArmor sha1 policy hashing enabled“ pid=1 comm=„swapper/0“
[    6.175451] AppArmor: AppArmor sha1 policy hashing enabled
[    6.183957] [TFFS3_Init] Called.
[    6.185878] [TFFS3_CACHE_Configure] Setting up caching for backend nand
[    6.192363] [TFFS3-CACHE] Caching module for TFFS 3.x
[    6.197385] [TFFS3-NAND] NAND storage backend for TFFS 3.x
[    6.500924] [TFFS3-NAND] Initialisation successful, 16/16/16 NAND blocks active, fill rate 23%
[    6.508537] TFFS: tiny flash file system driver. GPL (c) AVM Berlin (Version 3.0)
[    6.515661] Adam2 environment variables API installed.
[    6.521972] ubi0: attaching mtd4
[    6.897415] ubi0: scanning is finished
[    6.930115] ubi0: attached mtd4 (name „ubi“, size 491 MiB)
[    6.934196] ubi0: PEB size: 262144 bytes (256 KiB), LEB size: 258048 bytes
[    6.941014] ubi0: min./max. I/O unit sizes: 4096/4096, sub-page size 1024
[    6.947777] ubi0: VID header offset: 1024 (aligned 1024), data offset: 4096
[    6.954728] ubi0: good PEBs: 1961, bad PEBs: 3, corrupted PEBs: 0
[    6.960805] ubi0: user volume: 4, internal volumes: 1, max. volumes count: 128
[    6.968012] ubi0: max/mean erase counter: 38/25, WL threshold: 4096, image sequence number: 1192175580
[    6.977299] ubi0: available PEBs: 0, total reserved PEBs: 1961, PEBs reserved for bad PEB handling: 37
[    6.986619] ubi0: background thread „ubi_bgt0d“ started, PID 621
[    6.988475] [announce_root] filesystem (/dev/mtdblock5) will be used as [    7.009319] VFS: Mounted root (squashfs filesystem) readonly on device 31:5.
[    7.020592] devtmpfs: mounted
[    7.023184] Freeing unused kernel: 372k freed
[    7.026502] This architecture does not have kernel memory protection.
[    8.275188] eip123_hw: loading out-of-tree module taints kernel.
[    8.279831] eip123_hw: module license ‚Proprietary‘ taints kernel.
[    8.285999] Disabling lock debugging due to kernel taint
[    8.291749] [module-mem] give 0x4000 bytes at 884a8000 to module ‚eip123_hw‘ (0x9aa000 bytes left)
[    8.302723] [module-mem] give 0x2000 bytes at 884ac000 to module ‚eip123‘ (0x9a8000 bytes left)
[    8.311275] eip123 1e000000.eip123: Detected hardware version 2.2.2
[    8.316312] eip123 1e000000.eip123: my_id=3 master_id=0 num_mailboxes=4 mailbox_size=256
[    8.324444] eip123 1e000000.eip123: Linked mailbox number 1
[    8.356401] eip123 1e000000.eip123: Sysinfo: FWVersion=2.4.2 HWVersion=2.2.2 MemorySize=32768 HostId=3 Identity=0 NVMAnomaly=0 NVMAnomalyLocation=0
[    8.588460] eip123 1e000000.eip123: eip123_hw init successful
[    8.648480] eip123 1e000000.eip123: Device responded with error_src=0x0 error=0x1 opcode=0x1c
[    8.655632] eip123 1e000000.eip123: Could not find rootkey in OTP
[    8.933300] [module-mem] give 0x31000 bytes at 884ae000 to module ‚led_module‘ (0x977000 bytes left)
[    8.951424] [LED] use GPIO 13 for ‚gpio_avm_led_power‘
[    8.955348] [LED] use GPIO 16 for ‚gpio_avm_led_internet‘
[    8.960583] [LED] use GPIO 14 for ‚gpio_avm_led_wlan‘
[    8.965613] [LED] use GPIO 15 for ‚gpio_avm_led_fon‘
[    8.970565] [LED] use GPIO 18 for ‚gpio_avm_led_info‘
[    8.975598] [LED] use GPIO 17 for ‚gpio_avm_led_info_red‘
[    8.980977] [LED] use GPIO 3 for ‚gpio_avm_led_output_enable‘
[    8.986853] [BUTTON] use GPIO 10 for ‚gpio_avm_button_dect‘
[    8.992263] [BUTTON] use GPIO 11 for ‚gpio_avm_button_wlan‘
[    8.997833] [BUTTON] use GPIO 12 for ‚gpio_avm_button_wps‘
[    9.003600] [avm_connect][state_machine_init] starting event worker thread
[    9.011195] led_module: Waiting for event system to be ready…
[    9.078943] [TFFS_Cache] Allocate segement buffer cache (size=4072)
[    9.086472] TFFS Name Table N
[    9.451136] [module-mem] give 0x3000 bytes at 884df000 to module ‚cpunet‘ (0x974000 bytes left)
[    9.461018] cpunet 1f107400.cpunet: slots=16 mtu=8192 mailbox_size=0x4c mempool_size=0x20000
[    9.468776] cpunet 1f107400.cpunet: Initialized mailbox: rx=0xbf201000 tx=0xbf201100
[    9.476025] cpunet 1f107400.cpunet: Initialized mempool: rx=0x8dfc0000 tx=0x8dfe0000 min_align=64
[    9.484988] cpunet 1f107400.cpunet: hw init successful
[    9.492196] IPv6: ADDRCONF(NETDEV_UP): lo: link is not ready
[    9.497163] IPv6: ADDRCONF(NETDEV_UP): cpunet0: link is not ready
[    9.596967] [0]system-load  55% loadavg 0.8 0.2 0.1 - pgstat: sum=216627 free=101959 slab=1924 alloc=955/s fault=320/s ai_sys:0.40/s 0x884a9624 endian_convert_array+0x20/0x38 [eip12 (sleep 2)
[   13.796778] AVM_WATCHDOG: System Init Ueberwachung 120 Sekunden
[   14.400115] udevd[931]: starting version 3.2.5
[   14.433651] udevd[931]: specified group ‚tty‘ unknown
[   14.438279] udevd[931]: specified group ‚dialout‘ unknown
[   14.443453] udevd[931]: specified group ‚kmem‘ unknown
[   14.448715] udevd[931]: specified group ‚input‘ unknown
[   14.453780] udevd[931]: specified group ‚video‘ unknown
[   14.459006] udevd[931]: specified group ‚audio‘ unknown
[   14.464302] udevd[931]: specified group ‚lp‘ unknown
[   14.469043] udevd[931]: specified group ‚disk‘ unknown
[   14.474030] udevd[931]: specified group ‚cdrom‘ unknown
[   14.483448] udevd[931]: starting eudev-3.2.5
[   14.775991] [module-mem] give 0x3000 bytes at 884e2000 to module ‚vrx318_common‘ (0x971000 bytes left)
[   14.788501] ltq_pcie 0002:01:00.0: enabling device (0000 -> 0002)
[   14.796177] iATU Inbound
[   14.797365] PCIE_PL_IATU_VIEWPORT: 80000000
[   14.802542] PCIE_PL_IATU_REGION_LOWER_BASE_ADDR: 00000000
[   14.806960] PCIE_PL_IATU_REGION_UPPER_BASE_ADDR: 00000000
[   14.813954] PCIE_PL_IATU_REGION_LIMIT: 00000fff
[   14.817925] PCIE_PL_IATU_REGION_LOWER_TARGET_ADDR: 1e000000
[   14.824705] PCIE_PL_IATU_REGION_UPPER_TARGET_ADDR: 00000000
[   14.829233] [module-mem] give 0x1000 bytes at 884e5000 to module ‚xrx500_phy_fw‘ (0x970000 bytes left)
[   14.839708] phy-xrx500 phy-xrx500: requesting ltq_fw_PHY11G_IP_xRx5xx_A21.bin
[   14.847531] PCIE_PL_IATU_REGION_CTRL1: 00000000
[   14.852036] PCIE_PL_IATU_REGION_CTRL2: c0000000
[   14.856555] iATU Outbound
[   14.858725] [module-mem] Module ‚vrx318_common‘ already allocated
[   14.866926] PCIE_PL_IATU_VIEWPORT: 00000000
[   14.869892] PCIE_PL_IATU_REGION_LOWER_BASE_ADDR: 20000000
[   14.871493] [module-mem] Module ‚xrx500_phy_fw‘ already allocated
[   14.881735] PCIE_PL_IATU_REGION_UPPER_BASE_ADDR: 00000000
[   14.887309] PCIE_PL_IATU_REGION_LIMIT: 5fffffff
[   14.891667] PCIE_PL_IATU_REGION_LOWER_TARGET_ADDR: 00000000
[   14.896663] PCIE_PL_IATU_REGION_UPPER_TARGET_ADDR: 00000000
[   14.903447] PCIE_PL_IATU_REGION_CTRL1: 00000000
[   14.906807] PCIE_PL_IATU_REGION_CTRL2: 80000000
[   14.911319] ltq_pcie 0002:01:00.0: Total cards found 1
[   14.916554] ltq_pcie 0002:01:00.0: card 0 attached
[   14.917831] phy-xrx500 phy-xrx500: booting GPHY0 firmware at 25A10000 for GRX500
[   14.917884] phy-xrx500 phy-xrx500: booting GPHY1 firmware at 25A10000 for GRX500
[   14.917942] phy-xrx500 phy-xrx500: booting GPHY2 firmware at 25A10000 for GRX500
[   14.918012] phy-xrx500 phy-xrx500: booting GPHY3 firmware at 25A10000 for GRX500
[   14.918087] phy-xrx500 phy-xrx500: booting GPHY4 firmware at 25A10000 for GRX500
[   14.920583] [module-mem] give 0xe000 bytes at 884e6000 to module ‚eip97‘ (0x962000 bytes left)
[   14.968053] ltq_pcie 0002:01:00.0: irq base 200 irq numbers 4
[   14.972465] ltq_pcie 0002:01:00.0: its own phy membase  0xbc000000 virtual membase 0xfc000000 size 0x00800000
[   14.982657] Lantiq VRX318 Version 3.0.0 [   15.095348] [module-mem] give 0x7000 bytes at 884f4000 to module ‚ltq_eth_drv_xrx500‘ (0x95b000 bytes left)
[   15.105582] [ltq_eth_drv_xrx500] { ltq_gsw_pmac_init : 881 }PMAC_EG_CFG_SET for GSW-L
[   15.112251] [ltq_eth_drv_xrx500] { ltq_gsw_pmac_init : 928 }PMAC_IG_CFG_SET for GSW-L
[   15.119862] [ltq_eth_drv_xrx500] { ltq_gsw_pmac_init : 1007 }PMAC_EG_CFG_SET for GSW-R
[   15.131376] [ltq_eth_drv_xrx500] { ltq_gsw_pmac_init : 1065 }PMAC_IG_CFG_SET for GSW-R
[   15.138116] [ltq_eth_drv_xrx500] { ltq_gsw_pmac_init : 1138 }
[   15.138116] 	 GSW PMAC Init Done!!!
[   15.147077] [ltq_eth_drv_xrx500] { xrx500_of_mdio : 1707 }registering one of MII bus
[   15.154998] libphy: lantiq,xrx500-mdio: probed
[   15.184872] [ltq_eth_drv_xrx500] { xrx500_of_mdio : 1707 }registering one of MII bus
[   15.191456] libphy: lantiq,xrx500-mdio: probed
[   15.201356] [datapath_proc] { dp_sub_proc_install_30 : 3491 }dp_sub_proc_install ok
[   15.207634] Rmon clear for CTP RX/TX —Logical Port 0
[   15.212612] Rmon clear for CTP RX/TX —Logical Port 1
[   15.217645] Rmon clear for CTP RX/TX —Logical Port 2
[   15.222673] Rmon clear for CTP RX/TX —Logical Port 3
[   15.227704] Rmon clear for CTP RX/TX —Logical Port 4
[   15.232746] Rmon clear for CTP RX/TX —Logical Port 5
[   15.237784] Rmon clear for CTP RX/TX —Logical Port 6
[   15.242842] Rmon clear for CTP RX/TX —Logical Port 0
[   15.247855] Rmon clear for CTP RX/TX —Logical Port 1
[   15.252893] Rmon clear for CTP RX/TX —Logical Port 2
[   15.257923] Rmon clear for CTP RX/TX —Logical Port 3
[   15.262954] Rmon clear for CTP RX/TX —Logical Port 4
[   15.267994] Rmon clear for CTP RX/TX —Logical Port 5
[   15.273024] Rmon clear for CTP RX/TX —Logical Port 6
[   15.278064] Rmon clear for CTP RX/TX —Logical Port 7
[   15.283093] Rmon clear for CTP RX/TX —Logical Port 8
[   15.288133] Rmon clear for CTP RX/TX —Logical Port 9
[   15.293169] Rmon clear for CTP RX/TX —Logical Port 10
[   15.298283] Rmon clear for CTP RX/TX —Logical Port 11
[   15.303411] Rmon clear for CTP RX/TX —Logical Port 12
[   15.308528] Rmon clear for CTP RX/TX —Logical Port 13
[   15.313655] Rmon clear for CTP RX/TX —Logical Port 14
[   15.318771] Rmon clear for CTP RX/TX —Logical Port 15
[   15.323892] Rmon clear for CTP RX/TX —Logical Port 16
[   15.329057] [datapath_api] { dp_init_module : 2748 }datapath init done
[   15.335599] [cbm] { dp_port_alloc : 3193 }flags 0x2
[   15.340406] [cbm] { cbm_add_to_list : 427 }2
[   15.344661] [cbm] { dp_port_alloc : 3342 }disabling q 17 port 7
[   15.350553] [cbm] { dp_port_alloc : 3348 }first time LOOKUP prgrm
[   15.357029] [cbm] { dp_port_alloc : 3353 }1024
[   15.361454] [ltq_eth_drv_xrx500] { xrx500_of_iface : 1598 }xrx500_of_iface: rx csum offload is enabled !
[   15.370697] [ltq_eth_drv_xrx500] { xrx500_mdio_probe : 1796 }trying to connect: eth3 to device: 0:02 with irq: 289
[   15.533680] [ltq_eth_drv_xrx500] { xrx500_mdio_probe : 1814 }eth3: attached PHY [Lantiq XWAY VR9 GPHY 11G v1.4] (phy_addr=0:02, irq=289)
[   15.550800] [cbm] { dp_enable : 3657 }ep=2 tmu_port=7 queue=17 sid=1
[   15.555732] [cbm] { dp_enable : 3698 }enable queue 17
[   15.560711] [cbm] { dp_enable : 3699 }flag 1 refcnt 1024
[   15.567786] [ltq_eth_drv_xrx500] { setup_avm_pa_eth_dev : 1350 }[setup_avm_pa_eth_dev] dev eth3
[   15.575396] [cbm] { dp_port_alloc : 3193 }flags 0x2
[   15.579932] [cbm] { cbm_add_to_list : 427 }2
[   15.584176] [cbm] { dp_port_alloc : 3342 }disabling q 18 port 8
[   15.590074] [cbm] { dp_port_alloc : 3348 }first time LOOKUP prgrm
[   15.596589] [cbm] { dp_port_alloc : 3353 }1024
[   15.600929] [ltq_eth_drv_xrx500] { xrx500_of_iface : 1598 }xrx500_of_iface: rx csum offload is enabled !
[   15.610103] [ltq_eth_drv_xrx500] { xrx500_mdio_probe : 1796 }trying to connect: eth2 to device: 0:03 with irq: 290
[   15.769293] [ltq_eth_drv_xrx500] { xrx500_mdio_probe : 1814 }eth2: attached PHY [Lantiq XWAY VR9 GPHY 11G v1.4] (phy_addr=0:03, irq=290)
[   15.786473] [cbm] { dp_enable : 3657 }ep=3 tmu_port=8 queue=18 sid=2
[   15.791399] [cbm] { dp_enable : 3698 }enable queue 18
[   15.796378] [cbm] { dp_enable : 3699 }flag 1 refcnt 1024
[   15.803211] [ltq_eth_drv_xrx500] { setup_avm_pa_eth_dev : 1350 }[setup_avm_pa_eth_dev] dev eth2
[   15.810788] [cbm] { dp_port_alloc : 3193 }flags 0x2
[   15.815356] [cbm] { cbm_add_to_list : 427 }2
[   15.819593] [cbm] { dp_port_alloc : 3342 }disabling q 19 port 9
[   15.825498] [cbm] { dp_port_alloc : 3348 }first time LOOKUP prgrm
[   15.831984] [cbm] { dp_port_alloc : 3353 }1024
[   15.836415] [ltq_eth_drv_xrx500] { xrx500_of_iface : 1598 }xrx500_of_iface: rx csum offload is enabled !
[   15.845486] [ltq_eth_drv_xrx500] { xrx500_mdio_probe : 1796 }trying to connect: eth1 to device: 0:04 with irq: 291
[   16.001271] [ltq_eth_drv_xrx500] { xrx500_mdio_probe : 1814 }eth1: attached PHY [Lantiq XWAY VR9 GPHY 11G v1.4] (phy_addr=0:04, irq=291)
[   16.018452] [cbm] { dp_enable : 3657 }ep=4 tmu_port=9 queue=19 sid=3
[   16.023377] [cbm] { dp_enable : 3698 }enable queue 19
[   16.028356] [cbm] { dp_enable : 3699 }flag 1 refcnt 1024
[   16.035239] [ltq_eth_drv_xrx500] { setup_avm_pa_eth_dev : 1350 }[setup_avm_pa_eth_dev] dev eth1
[   16.042827] [cbm] { dp_port_alloc : 3193 }flags 0x2
[   16.047386] [cbm] { cbm_add_to_list : 427 }2
[   16.051624] [cbm] { dp_port_alloc : 3342 }disabling q 20 port 10
[   16.057614] [cbm] { dp_port_alloc : 3348 }first time LOOKUP prgrm
[   16.064100] [cbm] { dp_port_alloc : 3353 }1024
[   16.068502] [ltq_eth_drv_xrx500] { xrx500_of_iface : 1598 }xrx500_of_iface: rx csum offload is enabled !
[   16.077615] [ltq_eth_drv_xrx500] { xrx500_mdio_probe : 1796 }trying to connect: eth0 to device: 0:05 with irq: 292
[   16.233302] [ltq_eth_drv_xrx500] { xrx500_mdio_probe : 1814 }eth0: attached PHY [Lantiq XWAY VR9 GPHY 11G v1.4] (phy_addr=0:05, irq=292)
[   16.250482] [cbm] { dp_enable : 3657 }ep=5 tmu_port=10 queue=20 sid=4
[   16.255494] [cbm] { dp_enable : 3698 }enable queue 20
[   16.260472] [cbm] { dp_enable : 3699 }flag 1 refcnt 1024
[   16.267299] [ltq_eth_drv_xrx500] { setup_avm_pa_eth_dev : 1350 }[setup_avm_pa_eth_dev] dev eth0
[   16.274885] [cbm] { dp_port_alloc : 3193 }flags 0x4
[   16.279459] [cbm] { cbm_add_to_list : 427 }1
[   16.283688] [cbm] { dp_port_alloc : 3342 }disabling q 28 port 19
[   16.289679] [cbm] { dp_port_alloc : 3348 }first time LOOKUP prgrm
[   16.296167] [cbm] { dp_port_alloc : 3353 }1024
[   16.300557] [ltq_eth_drv_xrx500] { xrx500_of_iface : 1598 }xrx500_of_iface: rx csum offload is enabled !
[   16.309685] [ltq_eth_drv_xrx500] { xrx500_mdio_probe : 1796 }trying to connect: wan to device: 1:01 with irq: 293
[   16.464095] [ltq_eth_drv_xrx500] { xrx500_mdio_probe : 1814 }wan: attached PHY [Lantiq XWAY VR9 GPHY 11G v1.4] (phy_addr=1:01, irq=293)
[   16.481131] [cbm] { dp_enable : 3657 }ep=15 tmu_port=19 queue=28 sid=12
[   16.486326] [cbm] { dp_enable : 3698 }enable queue 28
[   16.491304] [cbm] { dp_enable : 3699 }flag 1 refcnt 1024
[   16.498112] [ltq_eth_drv_xrx500] { setup_avm_pa_eth_dev : 1350 }[setup_avm_pa_eth_dev] dev wan
[   16.505558] [ltq_eth_drv_xrx500] { ltq_eth_drv_init : 2234 }Lantiq ethernet driver for XRX500 init.
[   16.599101] 
[   16.599101] [avm_debug] redirecting kernel-messages (/dev/debug)

starting pid 746, tty ‚/dev/ttyLTQ0‘: ‚-/bin/sh‘

BusyBox v1.29.3 (2020-11-18 13:04:24 CET) built-in shell (ash)

*ermittle die aktuelle TTY
tty is „/dev/ttyLTQ0“
[50;132qSerielles Terminal
disable start/stop characters and flowcontrol
# 
# ********[   20.296159][3]
[   20.340355][1][piglet]dect_file_process: upload of ‚/lib/modules/dectfw_secondlevel_441.hex‘ successfull
[   20.840646][1][1]system-load  25% loadavg 0.35 0.8 0.3 - task runtime:13% max:modprobe 7%  pgstat: sum=213365 free=98921 slab=2559 alloc=2368/s fault=1565/s (sleep 2)
[   21.392983][2][2]system-load  26% loadavg 0.35 0.8 0.3 - pgstat: sum=213365 free=98921 slab=2559 alloc=2029/s fault=1341/s (sleep 1)
[   22.352684][1][piglet]bitfile ‚/lib/modules/bitfile.bit‘
[   22.352796][1][piglet]try to preload in progress-context: /lib/modules/bitfile.bit
[   23.428546][1][piglet] bitfile 72761 bytes in 1076 ms done
[   23.528717][1][piglet]TDM: FS: 8005 Hz CLK: 1222900 Hz
[   23.529852][3][3]system-load  39% loadavg 0.35 0.8 0.3 - task runtime:13% max:modprobe 13%  pgstat: sum=213379 free=98921 slab=2559 alloc=2083/s fault=1373/s (sleep 6)
[Supervisor] Info: piglet.service exit success
[Supervisor] Info: start capi.service
[Supervisor] Info: start modules-load.service
[   23.606637][0][module-mem] give 0xc000 bytes at 88507000 to module ‚directconnect_datapath‘ (0x943000 bytes left)
[   23.627577][3][module-mem] give 0x7000 bytes at 88513000 to module ‚dc_mode0_xrx500‘ (0x93c000 bytes left)
[   23.670834][1][module-mem] give 0x1000 bytes at 8851a000 to module ‚eth_oam_handler‘ (0x93b000 bytes left)
[   23.671573][1]Loading eth_oam driver for WAN interface ptm0
[   23.673261][1]eth_oam driver: given ethwan device not present; waiting for its registration
[   23.673344][1]Init eth_oam driver succeeded
[   23.691085][3][module-mem] give 0x3000 bytes at 8851b000 to module ‚cprocfsmod‘ (0x938000 bytes left)
[   23.693681][3][module-mem] module ‚cchardev‘ reserved size 24576 is to great for demand size 20480 - waste 4096 (module_alloc_waste=4096)
[   23.693738][3][module-mem] give 0x5000 bytes at 8851e000 to module ‚cchardev‘ (0x933000 bytes left)
[   23.694996][3]cchardevice: loaded
[   23.717892][0][module-mem] give 0x68000 bytes at 88523000 to module ‚pcmlink‘ (0x8cb000 bytes left)
[   23.725880][0]Could not find Env ‚kernel_args‘ in the device tree 
[   24.235594][2][module-mem] give 0x150000 bytes at 8858b000 to module ‚isdn_fbox_fon5‘ (0x77b000 bytes left)
[   24.264697][2][capi_oslib]avm_stack_attach: cpu2 -> cpu0
[   24.271978][0][avm-gpio-shim] avm_get_hw_config: ignoring p_param pointer!
[   24.272208][0][avm-gpio-shim] avm_get_hw_config: ignoring p_param pointer!
[   24.272306][0][tdmlink]ltq_tdm_request_gpioresource: ERROR: no gpio_avm_pcmlink_di exist
[   24.274683][0]tdm_get_irqdata(0): irq 270 flags 1028
[   24.274739][0]tdm_get_irqdata(1): irq 271 flags 1025
[   24.288449][0][isdn]PCMLINK: (fpga2) Codecslots=13 Slics=2 Pots=1 TE=2 NT=2 DECT=4 (CLARE2)  DSP-EC: 0
[   24.748312][0][module-mem] give 0x5d000 bytes at 886db000 to module ‚capi_codec‘ (0x71e000 bytes left)
[   24.955543][2][module-mem] give 0x1aa000 bytes at 88738000 to module ‚kdsldmod‘ (0x574000 bytes left)
[   25.005930][0][module-mem] give 0x50000 bytes at 888e2000 to module ‚avm_dect‘ (0x524000 bytes left)
[   25.014074][2]kdsld: init start (sizeof(struct sk_buff) = 464)
[   25.014158][2]kdsld: Initialisation of debughandles …
[   25.014260][2]kdsld: Initialisation of debughandles [OK]
[   25.014286][2]kdsld: Initialisation of global …
[   25.015183][2]kdsld: Initialisation of global [OK]
[   25.015243][2]kdsld: Initialisation of procfs …
[   25.015327][2]kdsld: Initialisation of procfs [OK]
[   25.015352][2]kdsld: Initialisation of kmod_debugctl …
[   25.015406][2]kdsld: Initialisation of kmod_debugctl [OK]
[   25.015430][2]kdsld: Initialisation of cenv …
[   25.015451][2]kdsld: Initialisation of cenv [OK]
[   25.015469][2]kdsld: Initialisation of ctimer …
[   25.015957][2]kdsld: Initialisation of ctimer [OK]
[   25.015994][2]kdsld: Initialisation of dsld_setup …
[   25.016031][2]kdsld: Initialisation of dsld_setup [OK]
[   25.016053][2]kdsld: Initialisation of adsl_net …
[   25.018441][2]kdsld: Initialisation of adsl_net [OK]
[   25.018526][2]kdsld: Initialisation of ppptty_net …
[   25.020595][2]kdsld: Initialisation of ppptty_net [OK]
[   25.020676][2]kdsld: Initialisation of ingress_shaping …
[   25.021579][0][module-mem] give 0x6000 bytes at 88932000 to module ‚dect_io‘ (0x51e000 bytes left)
[   25.025230][2]kdsld: Initialisation of ingress_shaping [OK]
[   25.025318][2]kdsld: Initialisation of pppdp …
[   25.052512][1][DECTDRV_ERR] fpCap ext data queueSize 20, avmTpui 16/390, etsiTpui 406/40
[Supervisor] Info: capi.service exit success
[   25.068467][2]kdsld: Initialisation of pppdp [OK]
[   25.068545][2]kdsld: Initialisation of kmodcmddev …
[   25.068661][2]kdsld: Initialisation of kmodcmddev [OK]
[   25.068690][2]kdsld: Initialisation of kdsldev …
[   25.068803][2]kdsld: Initialisation of kdsldev [OK]
[   25.068844][2]kdsld: Initialisation of kvpnd …
[   25.068897][2]kdsld: Initialisation of kvpnd [OK]
[   25.068920][2]kdsld: Initialisation of kdsluserdev …
[   25.068949][2]kdsld: Initialisation of kdsluserdev [OK]
[   25.068975][2]kdsld: Initialisation of kdsltrafficdev …
[   25.069010][2]kdsld: Initialisation of kdsltrafficdev [OK]
[   25.069033][2]kdsld: Initialisation of kdslmiscdev …
[   25.069068][2]kdsld: Initialisation of kdslmiscdev [OK]
[   25.069094][2]kdsld: Initialisation of packettrace …
[   25.069237][2]kdsld: Initialisation of packettrace [OK]
[   25.069270][2]kdsld: Initialisation of nqos …
[   25.070057][2]CHRDEV „avmtrackdquery“ major number 233 goes below the dynamic allocation range
[   25.070325][2]kdsld: Initialisation of nqos [OK]
[   25.070353][2]kdsld: Initialisation of http_filter …
[   25.070378][2]CHRDEV „userman_url“ major number 232 goes below the dynamic allocation range
[   25.070408][2]userman: device registerd (userman_url) with major=232
[   25.070430][2]kdsld: Initialisation of http_filter [OK]
[   25.070452][2]kdsld: Initialisation of atmvcchook …
[   25.070475][2]kdsld: Initialisation of atmvcchook [OK]
[   25.070495][2]kdsld: Initialisation of timer …
[   25.070543][2]kdsld: Initialisation of timer [OK]
[   25.070565][2]kdsld: Initialisation of netdevice_notifier …
[   25.070695][2]kdsld: Initialisation of netdevice_notifier [OK]
[   25.070724][2]kdsld: Initialisation of ttychannel_ldisc …
[   25.070753][2]kdsld: ttychannel: ldisc 8 registered
[   25.070776][2]kdsld: Initialisation of ttychannel_ldisc [OK]
[   25.070802][2]kdsld: Initialisation of guestflt …
[   25.073114][2]kdsld: Initialisation of guestflt [OK]
[   25.073174][2]kdsld: Initialisation of bridgeflt …
[   25.073208][2]CHRDEV „bridgeflt“ major number 231 goes below the dynamic allocation range
[   25.073458][2]kdsld: Initialisation of bridgeflt [OK]
[   25.073498][2]kdsld: Initialisation of krextd …
[   25.073524][2]kdsld: Initialisation of krextd:debughandles …
[   25.073575][2]kdsld: Initialisation of krextd:debughandles [OK]
[   25.073604][2]kdsld: Initialisation of krextd:global …
[   25.073641][2]kdsld: Initialisation of krextd:global [OK]
[   25.073666][2]kdsld: Initialisation of krextd:memcache …
[   25.073916][2]kdsld: Initialisation of krextd:memcache [OK]
[   25.073958][2]kdsld: Initialisation of krextd:igmpcompr …
[   25.073998][2]kdsld: Initialisation of krextd:igmpcompr [OK]
[   25.074024][2]kdsld: Initialisation of krextd:krextdev …
[   25.074079][2]CHRDEV „krextd“ major number 230 goes below the dynamic allocation range
[   25.074179][2]kdsld: Initialisation of krextd:krextdev [OK]
[   25.074210][2]kdsld: Initialisation of krextd:krextdev_wland …
[   25.074252][2]CHRDEV „krextd_wlan“ major number 229 goes below the dynamic allocation range
[   25.074285][2]kdsld: Initialisation of krextd:krextdev_wland [OK]
[   25.074315][2]kdsld: Initialisation of krextd:netdevice_notifier …
[Supervisor] Info: modules-load.service exit success
[   25.074392][2]kdsld: Initialisation of krextd:netdevice_notifier [OK]
[   25.074420][2]kdsld: Initialisation of krextd:krextdprocfs …
[   25.074520][2]kdsld: Initialisation of krextd:krextdprocfs [OK]
[   25.074551][2]kdsld: Initialisation of krextd:krextdtimer …
[   25.074589][2]kdsld: Initialisation of krextd:krextdtimer [OK]
[   25.074616][2]kdsld: Initialisation of krextd [OK]
[   25.074638][2]kdsld: Initialisation of kdsldprocfs …
[   25.074709][2]kdsld: Initialisation of kdsldprocfs [OK]
[   25.074738][2]kdsld: Initialisation of pcp …
[   25.076926][2]kdsld: Initialisation of pcp [OK]
[   25.076991][2]kdsld: Initialisation [OK]
[   25.138741][2][module-mem] give 0x1000 bytes at 88938000 to module ‚offload_util‘ (0x51d000 bytes left)
[   25.168884][0][module-mem] give 0x1000 bytes at 88939000 to module ‚ktestdrive‘ (0x51c000 bytes left)
[   25.172940][0][module-mem] module ‚offload_dp‘ reserved size 40960 is to great for demand size 36864 - waste 4096 (module_alloc_waste=8192)
[   25.172999][0][module-mem] give 0x9000 bytes at 8893a000 to module ‚offload_dp‘ (0x513000 bytes left)
[   25.175537][0][cbm] { dp_port_alloc : 3193 }flags 0x20
[   25.175596][0][cbm] { cbm_add_to_list : 427 }1
[   25.175837][0][cbm] { dp_enable : 3657 }ep=7 tmu_port=2 queue=35 sid=19
[   25.175856][0][cbm] { dp_enable : 3664 }egp_type 0x20
[   25.176359][0][cbm] { dp_enable : 3698 }enable queue 35
[   25.176376][0][cbm] { dp_enable : 3699 }flag 1 refcnt 1488
[   25.179133][0][module-mem] give 0x2000 bytes at 88943000 to module ‚offload_qos‘ (0x511000 bytes left)
[   25.261873][0][module-mem] give 0x16000 bytes at 88945000 to module ‚offload_pa‘ (0x4fb000 bytes left)
[   25.267203][0]avm_pa: try to activate hw accelaration for pid 3 (ipv4) called from avm_pa_register_hardware_pa
[   25.267445][0]avm_pa: tx channel activated, pid 3 (ipv4)
[   25.267475][0]avm_pa: try to activate hw accelaration for pid 4 (ipv6) called from avm_pa_register_hardware_pa
[   25.267492][0]avm_pa: tx channel activated, pid 4 (ipv6)
[   25.284225][0][module-mem] give 0x2000 bytes at 8895b000 to module ‚sch_hw‘ (0x4f9000 bytes left)
[   25.309285][0][module-mem] give 0x3000 bytes at 8895d000 to module ‚sch_llq‘ (0x4f6000 bytes left)
[   25.346858][1][module-mem] give 0x2000 bytes at 88960000 to module ‚sch_tbf‘ (0x4f4000 bytes left)
[Supervisor] Info: start devnodes.service
[Supervisor] Info: devnodes.service exit success
[Supervisor] Info: start grx.service
[   26.129435][2]sch_hw: adjust excessive latency to ~5ms (687500 Bytes)
[   26.137944][1]sch_hw: adjust excessive latency to ~5ms (687500 Bytes)
[   26.146542][3]sch_hw: adjust excessive latency to ~5ms (687500 Bytes)
[   26.154859][1]sch_hw: adjust excessive latency to ~5ms (687500 Bytes)
net.ipv4.tcp_min_tso_segs = 100
[Supervisor] Info: grx.service exit success
[Supervisor] Info: start apparmor.service
[Supervisor] Info: start filesystem.service
[   26.228023][2]UBIFS (ubi0:3): background thread „ubifs_bgt0_3“ started, PID 1583
[   26.232062][1]audit: type=1400 audit(25.696:3): apparmor=„STATUS“ operation=„profile_load“ name=„/sbin/nqcs“ pid=1580 comm=„dd“
0+1 records in
0+1 records out
[Supervisor] Info: apparmor.service exit success
[   26.515095][0]UBIFS (ubi0:3): recovery needed
[   27.094036][0]UBIFS (ubi0:3): recovery completed
[   27.094286][0]UBIFS (ubi0:3): UBIFS: mounted UBI device 0, volume 3, name „avm_userdata“
[   27.094311][0]UBIFS (ubi0:3): LEB size: 258048 bytes (252 KiB), min./max. I/O unit sizes: 4096 bytes/4096 bytes
[   27.094338][0]UBIFS (ubi0:3): FS size: 397651968 bytes (379 MiB, 1541 LEBs), journal size 19869696 bytes (18 MiB, 77 LEBs)
[   27.094359][0]UBIFS (ubi0:3): reserved for root: 4952683 bytes (4836 KiB)
[   27.094385][0]UBIFS (ubi0:3): media format: w4/r0 (latest is w4/r0), UUID 71FDC8A6-5329-4674-9C5B-E81BF69E5306, small LPT model
[32m[INFO][0m /dev/ubi0_3 mounted at /var/media/ftp
[Supervisor] Info: filesystem.service exit success
[Supervisor] Info: start default-files.service
TAM: create directory /data/tam
[   27.272123][1][avm_power]pm_ressourceinfo_scriptparse: powerdevice_analog: norm_power_rate=200 act_rate=0 mul=141 div=10 offset=100 NormP=2920 mW -> SumNormP=2920 mW
[   27.272222][1][avm_power]pm_ressourceinfo_scriptparse: powerdevice_usb_host: norm_power_rate=500 act_rate=0 mul=5 div=1 offset=0 NormP=2500 mW -> SumNormP=5420 mW
[   27.272422][1][avm_power]pm_ressourceinfo_scriptparse: powerdevice_usb_host2: norm_power_rate=500 act_rate=0 mul=5 div=1 offset=0 NormP=2500 mW -> SumNormP=7920 mW
[   27.272556][1][avm_power]pm_ressourceinfo_scriptparse: powerdevice_wlan: norm_power_rate=100 act_rate=0 mul=130 div=10 offset=100 NormP=1400 mW -> SumNormP=9320 mW
[   27.272614][1][avm_power]pm_ressourceinfo_scriptparse: powerdevice_dect: norm_power_rate=100 act_rate=0 mul=200 div=78 offset=150 NormP=406 mW -> SumNormP=9726 mW
[   27.272677][1][avm_power]pm_ressourceinfo_scriptparse: powerdevice_cpuclock: norm_power_rate=100 act_rate=100 mul=0 div=1 offset=0 NormP=0 mW -> SumNormP=9726 mW
[   27.272743][1][avm_power]pm_ressourceinfo_scriptparse: powerdevice_loadrate: norm_power_rate=100 act_rate=43 mul=15 div=1 offset=0 NormP=1500 mW -> SumNormP=11226 mW
[   27.272813][1][avm_power]pm_ressourceinfo_scriptparse: powerdevice_dspclock: norm_power_rate=100 act_rate=100 mul=0 div=1 offset=1000 NormP=1000 mW -> SumNormP=12226 mW
[   27.272876][1][avm_power]pm_ressourceinfo_scriptparse: powerdevice_systemclock: norm_power_rate=100 act_rate=100 mul=0 div=1 offset=2000 NormP=2000 mW -> SumNormP=14226 mW
[   27.272938][1][avm_power]pm_ressourceinfo_scriptparse: powerdevice_isdnnt: norm_power_rate=100 act_rate=0 mul=1 div=1 offset=0 NormP=100 mW -> SumNormP=14326 mW
[   27.273000][1][avm_power]pm_ressourceinfo_scriptparse: powerdevice_ethernet: norm_power_rate=2817 act_rate=268435456 mul=1 div=1 offset=50 NormP=2867 mW -> SumNormP=17193 mW
[Supervisor] Info: default-files.service exit success
[Supervisor] Info: start config.service
[Supervisor] Info: start debug.service
[Supervisor] Info: start sysctl.service
net.ipv4.tcp_min_snd_mss = 536
vm.laptop_mode = 2
vm.dirty_expire_centisecs = 100
vm.dirty_writeback_centisecs = 100
kernel.panic_on_oops = 1
vm.panic_on_oom = 2
kernel.printk = 4
net.ipv4.ip_forward = 1
net.ipv4.tcp_min_tso_segs = 100
net.ipv4.conf.all.rp_filter = 1
net.ipv4.conf.default.rp_filter = 1
[Supervisor] Info: sysctl.service exit success
[32m[INFO][0m have to stop cat /dev/debug.
[   27.331790] sysrq: SysRq : Changing Loglevel
[   27.331861][2]sysrq: Loglevel set to 4
cat: read error: Broken pipe
[Supervisor] Info: debug.service exit success
[Supervisor] Info: config.service exit success
[Supervisor] Info: start avmipcd.service
[Supervisor] Info: start boxnotify.service
[Supervisor] Info: start capitcp.service
[Supervisor] Info: start dsl.service
[Supervisor] Info: start psupport-init-prenet.service
[Supervisor] Info: start run_clock.service
[Supervisor] Info: avmipcd.service exit success
[Supervisor] Info: start avmnexusd.service
[Supervisor] Info: start psetd.service
[Supervisor] Info: boxnotify.service exit success
[Supervisor] Info: psupport-init-prenet.service exit success
[Supervisor] Info: start net.service
run_clock demon started

[Supervisor] Info: run_clock.service exit success
/etc/ewnw_devfiles.sh: checking /dev files ….
/etc/ewnw_devfiles.sh: /dev/kdsld already exists
/etc/ewnw_devfiles.sh: mknod /dev/kvpnd c 240 0
/etc/ewnw_devfiles.sh: /dev/kdsldptrace0 already exists
/etc/ewnw_devfiles.sh: /dev/kdsldptrace1 already exists
/etc/ewnw_devfiles.sh: /dev/kdsldptrace2 already exists
/etc/ewnw_devfiles.sh: /dev/kdsldptrace3 already exists
/etc/ewnw_devfiles.sh: /dev/kdsldptrace4 already exists
/etc/ewnw_devfiles.sh: mknod /dev/kdsldptrace5 c 236 5
/etc/ewnw_devfiles.sh: mknod /dev/kdsldptrace6 c 236 6
/etc/ewnw_devfiles.sh: mknod /dev/kdsldptrace7 c 236 7
/etc/ewnw_devfiles.sh: mknod /dev/kdsldptrace8 c 236 8
/etc/ewnw_devfiles.sh: mknod /dev/kdsldptrace9 c 236 9
/etc/ewnw_devfiles.sh: mknod /dev/kdsldptrace10 c 236 10
/etc/ewnw_devfiles.sh: mknod /dev/kdsldptrace11 c 236 11
/etc/ewnw_devfiles.sh: mknod /dev/kdsldptrace12 c 236 12
[Supervisor] Info: capitcp.service exit success
/etc/ewnw_devfiles.sh: mknod /dev/kdsldptrace13 c 236 13
/etc/ewnw_devfiles.sh: mknod /dev/kdsldptrace14 c 236 14
/etc/ewnw_devfiles.sh: mknod /dev/kdsldptrace15 c 236 15
/etc/ewnw_devfiles.sh: mknod /dev/kdsldptrace16 c 236 16
/etc/ewnw_devfiles.sh: /dev/kdsldptrace17 already exists
/etc/ewnw_devfiles.sh: /dev/kdsldptrace18 already exists
/etc/ewnw_devfiles.sh: /dev/kdsldptrace19 already exists
/etc/ewnw_devfiles.sh: /dev/kdsldptrace20 already exists
/etc/ewnw_devfiles.sh: mknod /dev/kdsldptrace21 c 236 21
[Supervisor] Info: psetd.service exit success
/etc/ewnw_devfiles.sh: mknod /dev/kdsldptrace22 c 236 22
/etc/ewnw_devfiles.sh: mknod /dev/kdsldptrace23 c 236 23
/etc/ewnw_devfiles.sh: mknod /dev/kdsldptrace24 c 236 24
/etc/ewnw_devfiles.sh: mknod /dev/kdsldptrace25 c 236 25
/etc/ewnw_devfiles.sh: mknod /dev/kdsldptrace26 c 236 26
/etc/ewnw_devfiles.sh: mknod /dev/kdsldptrace27 c 236 27
/etc/ewnw_devfiles.sh: mknod /dev/kdsldptrace28 c 236 28
/etc/ewnw_devfiles.sh: mknod /dev/kdsldptrace29 c 236 29
/etc/ewnw_devfiles.sh: mknod /dev/kdsldptrace30 c 236 30
/etc/ewnw_devfiles.sh: mknod /dev/kdsldptrace31 c 236 31
/etc/ewnw_devfiles.sh: mknod /dev/kdsldptrace32 c 236 32
/etc/ewnw_devfiles.sh: mknod /dev/knqos c 235 0
/etc/ewnw_devfiles.sh: mknod /dev/avmtrackd c 234 0
/etc/ewnw_devfiles.sh: mknod /dev/avmtrackdquery c 233 0
/etc/ewnw_devfiles.sh: mknod /dev/bridgeflt c 231 0
/etc/ewnw_devfiles.sh: mknod /dev/krextd c 230 0
/etc/ewnw_devfiles.sh: mknod /dev/krextd_wlan c 229 0
/etc/ewnw_devfiles.sh: /dev files checked
[dsl sus] dsl line test calib factory file available
avmnexusd[1634]: starting … (normal)
1970-01-01 01:00:27 avmnexusd[1634]: ready (0sec)
[Supervisor] Info: avmnexusd.service exit success
l2tpv3d[1800]: starting … (normal)
[dsl get xtse] ANNEX=B DSLMODE=0
[dsl get xtse] setting ADSL Annex B/J and VDSL2 oISDN
[dsl get xtse] 10 00 10 40 00 04 01 07
[dsl sus] AVM MEI diag enabled
[dsl sus] starting vr10 dsp…
[dsl sus] ANNEX=B DSLMODE=0
1970-01-01 01:00:28 l2tpv3d[1800]: ready (0sec)
l2tpv3d[1804]: started.
l2tpv3d[1804]: verbose: DISABLED
[dsl sus] loaded vr10 mei driver: /lib/modules/4.9.198/kernel/drivers/mei/vr10/drv_mei_cpe.ko with params: , avmDslDiagEnabled=1
sh: can’t create /sys/devices/system/cpu/cpu0/cpufreq/stats/time_in_state: Permission denied
[dsl sus] loaded vr10 dsl driver: /lib/modules/4.9.198/kernel/drivers/dsl/vr10/drv_dsl_cpe_api.ko with params: 
[dsl sus] created vr10 dsl device node /dev/dsl_vr10/0 (major: 227 , minor: 0)
[dsl sus] created vr10 mei device node /dev/mei_cpe/0 (major: 228 , minor: 0)
[dsl sus] started /usr/sbin/vr10/dsl_control (configuration: -i10_00_10_40_00_04_01_07 -f/lib/modules/dsp_vr10/vr10-B-dsl.bin -n/etc/dsl/notify/vr10/dsl_notify.sh  )
nohup: appending output to nohup.out
0
[dsl sus] started dsl_monitor
[dsl sus] ….vr10 dsp started
[dsl sus] ….vr10 vrx318_tc driver started
[dsl sus] xdslmode=0
[dsl sus] atm loaded
[dsl sus] /usr/sbin/vr10/oamd started
nohup: appending output to nohup.out
[Supervisor] Info: dsl.service exit success
[Supervisor] Info: start inetd.service
[Supervisor] Info: inetd.service exit success
ctlmgr[1814]: pcpc_create_ctx: no pcpserver found
vpnd[1866]: /var/flash/vpn.cfg: is empty
vpnd[1866]: load_config(vpn): file empty - factory default loaded
vpnd[1866]: starting … (normal)
vpnd[1872]: /var/flash/vpn.cfg: is empty
vpnd[1872]: load_config(vpn): file empty - factory default loaded
vpnd[1872]: [main]: startup ($Revision$$CompileDate: Sep  2 2023 09:51:41 $)
1970-01-01 01:00:30 vpnd[1866]: ready (1sec)
ctlmgr[1862]: /var/flash/ahausr.cfg: is empty
ctlmgr[1862]: load_config(ahausr): file empty - factory default loaded
ctlmgr[1862]: /var/flash/ewnwstatus.cfg: is empty
ctlmgr[1862]: load_config(ewnwstatus): file empty - factory default loaded
upnpd[1938]: starting … (normal)
1970-01-01 01:00:31 upnpd[1938]: ready (0sec)
multid[1951]: /var/flash/vpn.cfg: is empty
multid[1951]: load_config(vpn): file empty - factory default loaded
multid[1951]: startup ($Revision$$CompileDate: Sep  2 2023 09:51:41 $)
multid[1951]: starting … (normal)
multid[1955]: HWRevision=225
multid[1955]: br->interfaces: remove wan
multid[1955]: /var/flash/vpn.cfg: is empty
multid[1955]: load_config(vpn): file empty - factory default loaded
multid[1955]: opt_without_tr069discover=0, tr069disc=1, AR7CFG->vinax_hsi_lan_ports=(null), multid.tcom_targetarch=0, is_eth_switch_installed()=0, multid.cpmac_no_ata_possible=0, pppoeiface=ptm0
multid[1955]: URLAlreadyContacted=no in /var/flash/tr069.cfg
multid[1955]: tr069discover_prepare_ata: multid.wan_iface_name=wan, multid.tr069disc.org_pppoeiface=ptm0, pppoeiface=wan
multid[1955]: bridge_configured: nqos_bridge_active=0, bridge_port_set=0x0, igmp_flt_portset=0x0
ctlmgr[1862]: SAR: trigger avm_event_id_dsl_get ts=34:153340650 => now = 34153 ms. last = 0 ms
ctlmgr[1862]: SAR: avm_event_id_dsl_get read data ts=34153
ctlmgr[1862]: SAR: avm_event_id_dsl_get read data req_ts=34153 now_ts=34153
multid[1955]: flood ratelimiting on bridge lan is supported
multid[1955]: list[0]=lan
multid[1955]: list[0]=lan
multid[1955]: list[0]=lan
multid[1955]: list[0]=lan
ctlmgr[1862]: dsl_utils_get_dslparams: Config from dsl_manager: ControlBits 0x00000000 DsMargin 0 DsINP 0 RFI_mode 0 UsNoiseBits 0 DisableUs1WhenDs1LatnIsAboveDb 0 DisableUs2WhenDs1LatnIsAboveDb 0
ctlmgr[1862]: SAR: trigger avm_event_id_dsl_get ts=34:655418025 => now = 34655 ms. last = 34153 ms
ctlmgr[1862]: dsl_utils_get_dslparams: data newer than 1500 msec or ts==0 (ts=34153)
multid[1955]: flood ratelimiting on bridge guest is supported
multid[1955]: mrouter: using IGMPv3 for upstream interface dsl
multid[1955]: mrouter: using IGMPv3 for other interfaces
multid[1955]: resolv.conf with 127.0.0.1 written
multid[1955]: DHCPD on lan
multid[1955]: DHCPD on lan:0 skipped, is virtual interface
ctlmgr[1862]: WLANLIB: wlan_plugin_init:868: prj revision 0x1c35e1c
multid[1955]: DHCPD on guest
multid[1955]: open(/dev/userman) - No such file or directory (2)
multid[1955]: Warning: dnsd_start: no dns server added
multid[1955]: interface lo up.
multid[1955]: interface lo carrier up
multid[1955]: interface cpunet0 up.
multid[1955]: interface cpunet0 carrier up
multid[1955]: list[0]=lan
multid[1955]: list[1]=guest
multid[1955]: br_get_interfaces(guest)=0
multid[1955]: interface eth3 up.
multid[1955]: list[0]=lan
multid[1955]: list[1]=guest
multid[1955]: br_get_interfaces(guest)=0
multid[1955]: interface eth2 up.
multid[1955]: list[0]=lan
multid[1955]: list[1]=guest
multid[1955]: br_get_interfaces(guest)=0
multid[1955]: interface eth1 up.
multid[1955]: list[0]=lan
multid[1955]: list[1]=guest
multid[1955]: br_get_interfaces(guest)=0
multid[1955]: interface eth0 up.
multid[1955]: interface wan up.
ctlmgr[1862]: WLANLIB: wlan_libs_nexus_init:260: Get Nexus info failed: try again later.
multid[1955]: DHCPD on lan
multid[1955]: interface lan up.
multid[1955]: DHCPD on lan
multid[1955]: mrouter: lan: vif 0 if_index 13
multid[1955]: interface guest up.
multid[1955]: DHCPD on guest
multid[1955]: mrouter: lan: vif 0 if_index 13
multid[1955]: mrouter: guest: vif 1 if_index 14
multid[1955]: verbose: DISABLED
1970-01-01 01:00:35 multid[1951]: ready (2sec)
ddnsd[2049]: br->interfaces: remove wan
ddnsd[2049]: /var/flash/vpn.cfg: is empty
ddnsd[2049]: load_config(vpn): file empty - factory default loaded
ddnsd[2049]: startup ($Revision$$CompileDate: Sep  2 2023 09:51:41 $)
ddnsd[2049]: starting … (normal)
ddnsd[2053]: DDNS: no valid accounts
1970-01-01 01:00:36 ddnsd[2049]: [2049]: Daemon start failed (0sec)
ddnsd[2053]: [2053] Start failed
FATAL: ddnsd not running after started
pcpd[2055]: startup (Sep  2 2023 09:51:41)
pcpd[2055]: starting … (normal)
pcpd[2057]: Local v4 address: 192.168.178.1
pcpd[2057]: verbose: DISABLED
1970-01-01 01:00:36 pcpd[2055]: ready (0sec)
rc.wlan: Start WLAN…
ctlmgr[1862]: WLANLIB: wcsi_socket_connect:313: Establishing RPC connection failed with TIMEOUT
ctlmgr[1862]: /var/flash/stat.cfg: is empty
ctlmgr[1862]: /etc/default/avm/stat.cfg: is empty
ctlmgr[1862]: load_config(stat): file empty - factory default loaded
WLAND:[02069]:01:00.37/[0037.180]:[VER]Registered new module default, DEFAULT, 0
WLAND:[02069]:01:00.37/[0037.180]:[VER]Registered new module global, GLOBAL, 0
WLAND:[02069]:01:00.37/[0037.180]:[ALW]BUILD: Jul 13 2022, 17:28:39
dsld[2073]: set no arch
dsld[2073]: br->interfaces: remove wan
dsld[2073]: /var/flash/vpn.cfg: is empty
dsld[2073]: load_config(vpn): file empty - factory default loaded
dsld[2073]: set no arch
dsld[2073]: startup ($Revision$$CompileDate: Sep  2 2023 09:51:41 $)
dsld[2073]: starting ... (normal)
dsld[2078]: DSL Mac e0:28:6d:6d:c1:22
dsld[2078]: VOIP Mac e0:28:6d:6d:c1:23
dsld[2078]: VCC2 Mac e0:28:6d:6d:c1:24
dsld[2078]: VCC3 Mac e0:28:6d:6d:c1:26
dsld[2078]: voip: ppptarget voip disabled, ignored
dsld[2078]: interface lo carrier_up.
dsld[2078]: interface cpunet0 carrier_up.
dsld[2078]: /var/flash/stat.cfg: is empty
dsld[2078]: /etc/default/avm/stat.cfg: is empty
dsld[2078]: load_config(stat): file empty - factory default loaded
dsld[2078]: interface adsl carrier_up.
dsld[2078]: interface ppptty carrier_up.
1970-01-01 01:00:37 dsld[2073]: ready (0sec)
dsld[2078]: <<< 220 vpnd ready.
dsld[2078]: >>> ipsecassoc proxyarp_update lan
cloudmsgd[2082]: starting … (normal)
deviceinfod[2102]: starting … (normal)
1970-01-01 01:00:38 deviceinfod[2102]: ready (0sec)
[Supervisor] Info: net.service exit success
[Supervisor] Info: start aha.service
[Supervisor] Info: start kpid.service
[Supervisor] Info: start meshd.service
[Supervisor] Info: start plcd.service
[Supervisor] Info: start ptest_release.service
[Supervisor] Info: start usb.service
kpid: Sending section system failed with error -1:
sysfs_system 1 {„sv“:“gen/v1“,“kpi“:{„spd_mon“:{„raw_slow“:0,“raw_fast“:132,“raw_medium“:68,“raw_fused_svt“:100,“raw_fused_vddmin“:107},“temperatures“:{„cpu-thermal_min“:null,“cpu-thermal_max“:null,“cpu-thermal_avg“:null}}}
kpid: Sending section usb failed with error -1:
sysfs_usb 1 {„sv“:“gen/v1“,“kpi“:{}}
kpid: Sending section hwpa failed with error -1:
sysfs_hwpa 1 {„sv“:“gen/v1“,“kpi“:{}}
mount: mounting usbfs on /proc/bus/usb failed: No such file or directory
[Supervisor] Info: ptest_release.service exit success
[Supervisor] Info: start configd.service
[Supervisor] Info: start voip.service
[Supervisor] Info: configd.service exit success
plcd[2110]: event=Opening the HomePlug library. str1= str2= str3=
plcd[2110]: event=Service started. str1= str2= str3=
ctlmgr[1862]: /var/flash/vpn.cfg: is empty
ctlmgr[1862]: load_config(vpn): file empty - factory default loaded
plcd[2110]: event=Client connected. str1= str2= str3=
ctlmgr[1862]: /var/flash/vpn.cfg: is empty
ctlmgr[1862]: load_config(vpn): file empty - factory default loaded
starting XHCI driver
XHCI USB 3.0 Host with port_config:0 started
XHCI Platform Driver started
[Supervisor] Info: usb.service exit success
telefon[2158]: use clock_gettime(CLOCK_MONOTONIC)!
telefon[2158]: NoOldMSNNames
telefon: SIGCHLD PID 2489 received!
telefon[2158]: INFO No MOH file ‚/data/tam/fx_moh‘ !
dsld[2078]: avmipc: connect
dsld[2078]: connect
telefon: SIGCHLD PID 2607 received!
meshd[2109]: LOG: main: Hello from meshd.
meshd[2109]: starting … (normal)
meshd[2615]: verbose: DISABLED
telefon[2527]: NoOldMSNNames
1970-01-01 01:00:42 meshd[2109]: ready (0sec)
plcd[2110]: event=Client connected. str1= str2= str3=
[Supervisor] Info: meshd.service exit success
[Supervisor] Info: start meshd_config.service
voipd[2590]: starting … (normal)
[Supervisor] Info: meshd_config.service exit success
voipd[2639]: internet: dns_context: internet (ref 1)
voipd[2639]: internet: dns_context: ipv4 only, dns, 0, 2/5 300, 1
voipd[2639]: internet: dns_context: 1 name server:
voipd[2639]: internet: dns_context: 127.0.0.1 0
voipd[2639]: internet: if  (0) nr 0 connection 0
voipd[2639]: internet: dnscctx internet stay online 0 natstate normal
voipd[2639]: internet: stackmode_off
voipd[2639]: internet: dns_context: internet (ref 1)
voipd[2639]: internet: dns_context: ipv4 only, dns, 0, 2/5 300, 1
voipd[2639]: internet: dns_context: 1 name server:
voipd[2639]: internet: dns_context: 127.0.0.1 0
voipd[2639]: voip: dns_context: voip (ref 1)
voipd[2639]: voip: dns_context: ipv4 only, sipdns, 0, 2/5 300, 1
voipd[2639]: voip: dns_context: 1 name server:
voipd[2639]: voip: dns_context: 127.0.0.1 0
voipd[2639]: voip: if  (0) nr -1 connection 0
voipd[2639]: voip: dnscctx voip stay online 0 natstate normal
voipd[2639]: voip: stackmode_off
voipd[2639]: voip: dns_context: voip (ref 1)
voipd[2639]: voip: dns_context: ipv4 only, sipdns, 0, 2/5 300, 1
voipd[2639]: voip: dns_context: 1 name server:
voipd[2639]: voip: dns_context: 127.0.0.1 0
voipd[2639]: mta: if mta0 (0) netmark 2
voipd[2639]: mta: dnscctx mta stay online 1 natstate no NAT
voipd[2639]: mta: ipv4 no sync
voipd[2639]: mta: ipv6 no sync
voipd[2639]: mta: stackmode_dual
voipd[2639]: mta: dns_context: mta (ref 1)
voipd[2639]: mta: dns_context: ipv4 only, none, 0, 2/5 300, 1
voipd[2639]: homenet: dns_context: homenet (ref 1)
voipd[2639]: homenet: dns_context: ipv4 only, none, 0, 2/5 300, 1
voipd[2639]: homenet: dns_context: 1 name server:
voipd[2639]: homenet: dns_context: 127.0.0.1 0
voipd[2639]: homenet: dns_context: from 127.0.0.1
voipd[2639]: homenet: if lan (13)
voipd[2639]: homenet: dnscctx homenet stay online 1 natstate no NAT
voipd[2639]: homenet: ipv4 connected
voipd[2639]: homenet: stackmode_ipv4
voipd[2639]: homenet: dns_context: homenet (ref 1)
voipd[2639]: homenet: dns_context: ipv4 only, none, 0, 2/5 300, 1
voipd[2639]: homenet: dns_context: 1 name server:
voipd[2639]: homenet: dns_context: 127.0.0.1 0
voipd[2639]: homenet: dns_context: from 127.0.0.1
voipd[2639]: homenet: dns_context: homenet (ref 1)
voipd[2639]: homenet: dns_context: ipv4 only, none, 0, 2/5 300, 1
voipd[2639]: homenet: dns_context: 1 name server:
voipd[2639]: homenet: dns_context: 127.0.0.1 0
voipd[2639]: vpn: if  (0) nr 0 connection 0
voipd[2639]: vpn: dnscctx homenet stay online 0 natstate normal
voipd[2639]: vpn: stackmode_off
voipd[2639]: homenet: dns_context: homenet (ref 1)
voipd[2639]: homenet: dns_context: ipv4 only, none, 0, 2/5 300, 1
voipd[2639]: homenet: dns_context: 1 name server:
voipd[2639]: homenet: dns_context: 127.0.0.1 0
voipd[2639]: tunnel: dns_context: tunnel (ref 1)
voipd[2639]: tunnel: dns_context: ipv4 only, none, 0, 2/5 300, 1
voipd[2639]: tunnel: dns_context: 1 name server:
voipd[2639]: tunnel: dns_context: 127.0.0.1 0
voipd[2639]: tunnel: if tun0 (0)
voipd[2639]: tunnel: dnscctx tunnel stay online 1 natstate no NAT
voipd[2639]: tunnel: ipv4 no sync
voipd[2639]: tunnel: ipv6 no sync
voipd[2639]: tunnel: stackmode_dual
voipd[2639]: tunnel: dns_context: tunnel (ref 1)
voipd[2639]: tunnel: dns_context: ipv4 only, none, 0, 2/5 300, 1
voipd[2639]: tunnel: dns_context: 1 name server:
voipd[2639]: tunnel: dns_context: 127.0.0.1 0
dsld[2078]: avmipc: voipdready
1970-01-01 01:00:43 voipd[2590]: ready (1sec)
[Supervisor] Info: voip.service exit success
[Supervisor] Info: start voipkpid.service
[Supervisor] Info: voipkpid.service exit success
[Supervisor] Info: all Services loaded.
usermand[2860]: /var/flash/userstat.cfg: is empty
usermand[2860]: /etc/default/avm/userstat.cfg: is empty
usermand[2860]: load_config(userstat): file empty - factory default loaded
usermand[2860]: /var/flash/userstat.cfg: is empty
usermand[2860]: /etc/default/avm/userstat.cfg: is empty
usermand[2860]: load_config(userstat): file empty - factory default loaded
usermand[2860]: starting … (normal)
contfiltd[2662]: starting … (normal)
telefon[2527]: Stop DECT
ctlmgr[1862]: WLANLIB: _wlanlib_csi_get_stations_cb:1001: EXIT: status=0xffffffea
[Supervisor] Info: start smb2.service
[Supervisor] Info: smb2.service exit success
dsld[2078]: avmipc: connect
dsld[2078]: connect
upnpd[1940]: initlib libtcloud
dsld[2078]: avmipc: connect
dsld[2078]: connect
dsld[2078]: avmipc: connect
dsld[2078]: connect

# 
# 
# 
# telefon: SIGCHLD PID 2867 received!
telefon: SIGCHLD PID 2613 received!
dsld[2078]: avmipc: connect
dsld[2078]: connect
dsld[2078]: avmipc: connect
dsld[2078]: connect
dsld[2078]: avmipc: connect
dsld[2078]: connect
dsld[2078]: avmipc: connect
dsld[2078]: connect
dsld[2078]: avmipc: connect
dsld[2078]: connect
dsld[2078]: avmipc: connect
dsld[2078]: connect
dsld[2078]: avmipc: connect
dsld[2078]: connect

——————————————BEGIN_WLAN_SUBSYSTEM_LOG——————————————
——————————————BEGIN_META——————————————
class: WLAN-Subsystem Restart
error: 0102
count: 1
reason: Error initializing WLAN hardware
——————————————END_META——————————————

——————————————BEGIN_WLAND_SUPPORT——————————————
01:00:37: open
01:00.37/[0037.620]:[INF]derived config ‚AP-only mode 2G‘, ID: 2 (0x00000000)
01:00.37/[0037.670]:[ERR]scan_module_env_get_channel_list_by_band:1118: Invalid param.
01:00.37/[0037.670]:[ERR]scan_module_env_get_channel_list_by_band:1118: Invalid param.
01:00.37/[0037.750]:[INF]nexus_init: Initialize Nexus API 
01:00.37/[0037.750]:[ERR]nexus_comm_device_get_info: Cannot determine nexus right now - check again later(try again later)
01:00.37/[0037.750]:[ERR]lib_hal_env_get_channel_list:585: Invalid param.
01:00.41/[0041.800]:[INF]config_exchange_master_init:982: ENTER
01:00.44/[0044.910]:[ERR]lib_hal_get_client_list_by_id:273: No iface name found for station 1.
01:00.46/[0046.660]:[ERR]lib_hal_env_get_channel_list:620: Exit: Query channel_list failed: No such device (19)
01:00.46/[0046.690]:[ERR]lib_hal_env_get_channel_list:620: Exit: Query channel_list failed: No such device (19)
01:00.47/[0047.930]:[INF]nexus_init: Initialize Nexus API 
01:01.02/[0062.660]:[ERR]lib_hal_env_get_channel_list:620: Exit: Query channel_list failed: No such device (19)
01:01.18/[0078.660]:[ERR]lib_hal_env_get_channel_list:620: Exit: Query channel_list failed: No such device (19)
01:01.34/[0094.650]:[ERR]lib_hal_env_get_channel_list:620: Exit: Query channel_list failed: No such device (19)
01:01.37/[0097.910]:[ERR]lib_hal_env_get_channel_list:620: Exit: Query channel_list failed: No such device (19)
01:01.42/[0102.500]:[ERR]wifi_registration_timer_cb:343: wait for hardware interfaces timed out
01:01.42/[0102.500]:[ERR]cfg_mgr_event_handler_cb:2428: Hardware initialization failed with status 0x00000002

—END_WLAND_SUPPORT—

—BEGIN_PCI_DEVICES—
0000	1bef0030	11d	               0	               0	               0	               0	               0	               0	               0	               0	               0	               0	               0	               0	               0	               0	pcieport
0100	168c0046	11d	        b4000004	               0	               0	               0	               0	               0	               0	          200000	               0	               0	               0	               0	               0	               0	ath_ol_pci
0000	1bef0030	11e	               0	               0	               0	               0	               0	               0	               0	               0	               0	               0	               0	               0	               0	               0	pcieport
0100	1bef0020	c8	        bc000008	               0	               0	               0	               0	               0	               0	          800000	               0	               0	               0	               0	               0	               0	ltq_pcie
—END_PCI_DEVICES—

—BEGIN_DEV_DEBUG—
 nss_nwifi_offload 0
[   50.198005] ol_ath_set_default_tgt_config : AC Minfree buffer allocation through module param (umac.ko)
[   50.198020]  OL_ACBKMinfree : 0
[   50.198034]  OL_ACBEMinfree : 0
[   50.198049]  OL_ACVIMinfree : 0
[   50.198065]  OL_ACVOMinfree : 0
[   50.198086] hif_enable_fastpath, Enabling fastpath mode
[   50.198102] +HWT
[   50.198193] hif_completion_thread_startup: pipe_num:0 pipe_info:0x9c11c6b4
[   50.198235] hif_completion_thread_startup: pipe_num:3 pipe_info:0x9c11c78c
[   50.198261] hif_completion_thread_startup: pipe_num:4 pipe_info:0x9c11c7d4
[   50.207396] -HWT
[   50.207515] Startup Mode-0 set
[   50.207523] 
               <=== cfg max peer id 1056 ====>
[   50.209558] htt_peer_map_timer_init Enter pdev 9ab58000 hrtimer 9ab5c980
[   50.209595] 
                htt_alloc_peer_map_mem : Alloc Success : host q vaddr 9c1cc000 paddr 3c1cc000
[   50.209602] 
                htt_alloc_peer_map_mem : Flush Interval Configured to 256 pkts
[   50.209717] htt_avm_offload_init:206 registered irq 276 for wifi0-avm_offload_rx_refill on wifi0
[   50.209758] htt_avm_offload_init:229 registered irq 277 for wifi0-avm_offload_tx_free on wifi0
[   50.211944] ol_txrx_pdev_attach: 2500 tx desc’s allocated ; range starts from 9c160000
[   50.214634] Firmware_Build_Number:114 
[   50.214658] FW wireless modes: 0x7f9001
[   50.214670] num_rf_chain:0x00000004  
[   50.214676] ht_cap_info:0x0000185b  
[   50.214680] vht_cap_info:0x339b79fa  
[   50.214684] vht_supp_mcs:0x0000ffaa
[   50.214694] wmi_service_coex_gpio 0, wmi_service_4_wire_coex_support 0, coex_version 0
[   50.214706] 
               Sending Ext resource cfg: HOST PLATFORM as 1
               fw_feature_bitmap as 50 to TGT
[   50.214740] ol_ath_service_ready_event: tt_support: 1
[   50.214800] ol_ath_service_ready_event: periodic_chan_stats: 1
[   50.214805] ol_ath_service_ready_event: sw_cal_support_check_flag: 1
[   50.214813] Peer Caching Enabled ; num_peers = 530, num_active_peers = 52 num_tids = 104, num_vdevs = 17
[   50.214862] EXT NSS Supported
[   50.214892] idx 1 req 2  num_units 1 num_unit_info 12 unit size 256 actual units 53 
[   50.215246] ol_ath_alloc_host_mem_chunk req_id 2 idx 0 num_units 53 unit_len 256,
[   50.215254] idx 2 req 3  num_units 1 num_unit_info 12 unit size 1024 actual units 53 
[   50.215504] ol_ath_alloc_host_mem_chunk req_id 3 idx 1 num_units 53 unit_len 1024,
[   50.215512] idx 3 req 4  num_units 1 num_unit_info 12 unit size 4096 actual units 53 
[   50.216145] ol_ath_alloc_host_mem_chunk req_id 4 idx 2 num_units 53 unit_len 4096,
[   50.216166] idx 8 req 9  num_units 1 num_unit_info 8 unit size 32768 actual units 1 
[   50.216910] ol_ath_alloc_host_mem_chunk req_id 9 idx 3 num_units 1 unit_len 32768,
[   50.216923] idx 0 req 1  num_units 0 num_unit_info 2 unit size 2192 actual units 531 
[   50.221593] ol_ath_alloc_host_mem_chunk req_id 1 idx 4 num_units 531 unit_len 2192,
[   50.221618] idx 4 req 6  num_units 35 num_unit_info 0 unit size 3072 actual units 35 
[   50.222066] ol_ath_alloc_host_mem_chunk req_id 6 idx 5 num_units 35 unit_len 3072,
[   50.222074] idx 5 req 7  num_units 1 num_unit_info 0 unit size 12288 actual units 1 
[   50.222319] ol_ath_alloc_host_mem_chunk req_id 7 idx 6 num_units 1 unit_len 12288,
[   50.222326] idx 6 req 5  num_units 0 num_unit_info 2 unit size 2112 actual units 531 
[   50.226240] ol_ath_alloc_host_mem_chunk req_id 5 idx 7 num_units 531 unit_len 2112,
[   50.226262] Support not added yet for Service 91
[   50.226266] Support not added yet for Service 92
[   50.226269] No EXT_MSG send INIT now
[   50.226294] chunk 0 len 13568 requested , ptr  0x25a7c000
[   50.226298] chunk 1 len 54272 requested , ptr  0x25b90000
[   50.226303] chunk 2 len 217088 requested , ptr  0x25ba0000
[   50.226307] chunk 3 len 32768 requested , ptr  0x25b88000
[   50.226313] chunk 4 len 1163952 requested , ptr  0x25be0000
[   50.226317] chunk 5 len 107520 requested , ptr  0x25d00000
[   50.226321] chunk 6 len 12288 requested , ptr  0x25bd8000
[   50.226326] chunk 7 len 1121472 requested , ptr  0x25d20000
[   50.226330] chunk 8 len 0 requested , ptr  0x25b00000
[   50.226731] smart_log_init: Smart logging Enabled buf=9c300000 (size=65536)
[   50.226737] Not enabling smart log FW initiated packetlog feature since packetlog is not available at host
[   50.238554] wmi_control_rx :event handler is not registered: event id 0x9047
[   50.271848] wmi_control_rx :event handler is not registered: event id 0x9047
[   50.284615] wmi_control_rx :event handler is not registered: event id 0x9047
[   50.297335] wmi_control_rx :event handler is not registered: event id 0x9047
[   50.302213] Version = 16777216 3  status = 0
[   50.302252] ol_ath_connect_htc() WMI is ready
[   50.302318] htt_h2t_frag_desc_bank_cfg_msg - HTT_H2T_MSG_TYPE_FRAG_DESC_BANK_CFG sent to FW for radio ID = 0
[   50.302332] target uses HTT version 2.2; host uses 2.2
[   50.307850] ol_ath_attach() connect HTC. 
[   50.307855] bypasswmi : 0
[   50.307867] ol_regdmn_start: reg-domain param: regdmn=0, countryName=, wModeSelect=FFFFFFFF, netBand=FFFFFFFF, extendedChanMode=0.
[   50.307926] ol_regdmn_init_channels: !avail mode 0x7f9001 (0x2) flags 0x2150
[   50.307966] ol_regdmn_init_channels: !avail mode 0x7f9001 (0x4) flags 0xa0
[   50.307971] ol_regdmn_init_channels: !avail mode 0x7f9001 (0x8) flags 0xc0
[   50.307976] ol_regdmn_init_channels: !avail mode 0x7f9001 (0x20) flags 0xd0
[   50.307981] ol_regdmn_init_channels: !avail mode 0x7f9001 (0x40) flags 0x150
[   50.307987] ol_regdmn_init_channels: !avail mode 0x7f9001 (0x800) flags 0x10080
[   50.307993] ol_regdmn_init_channels: !avail mode 0x7f9001 (0x2000) flags 0x20080
[   50.307998] ol_regdmn_init_channels: !avail mode 0x7f9001 (0x4000) flags 0x40080
[   50.308069] Add VHT80 channel: 5210
[   50.308073] Add VHT80 channel: 5290
[   50.308077] Add VHT80 channel: 5530
[   50.308081] Add VHT80 channel: 5610
[   50.308084] Add VHT80 channel: 5690
[   50.308088] Add VHT80 channel: 5775
[   50.308109] Skipping VHT80 channel 5825
[   50.308123] Add VHT160/VHT80_80 pri80 and sec80 centers: 5210,5290
[   50.308127] Add VHT160/VHT80_80 pri80 and sec80 centers: 5290,5210
[   50.308131] Add VHT160/VHT80_80 pri80 and sec80 centers: 5530,5610
[   50.308135] Add VHT160/VHT80_80 pri80 and sec80 centers: 5610,5530
[   50.308222] Add VHT160/VHT80_80 pri80 and sec80 centers: 5210,5530
[   50.308226] Add VHT160/VHT80_80 pri80 and sec80 centers: 5530,5210
[   50.308230] Add VHT160/VHT80_80 pri80 and sec80 centers: 5210,5610
[   50.308235] Add VHT160/VHT80_80 pri80 and sec80 centers: 5610,5210
[   50.308239] Add VHT160/VHT80_80 pri80 and sec80 centers: 5210,5690
[   50.308243] Add VHT160/VHT80_80 pri80 and sec80 centers: 5690,5210
[   50.308247] Add VHT160/VHT80_80 pri80 and sec80 centers: 5210,5775
[   50.308251] Add VHT160/VHT80_80 pri80 and sec80 centers: 5775,5210
[   50.308255] Add VHT160/VHT80_80 pri80 and sec80 centers: 5290,5530
[   50.308259] Add VHT160/VHT80_80 pri80 and sec80 centers: 5530,5290
[   50.308263] Add VHT160/VHT80_80 pri80 and sec80 centers: 5290,5610
[   50.308267] Add VHT160/VHT80_80 pri80 and sec80 centers: 5610,5290
[   50.308271] Add VHT160/VHT80_80 pri80 and sec80 centers: 5290,5690
[   50.308275] Add VHT160/VHT80_80 pri80 and sec80 centers: 5690,5290
[   50.308280] Add VHT160/VHT80_80 pri80 and sec80 centers: 5290,5775
[   50.308284] Add VHT160/VHT80_80 pri80 and sec80 centers: 5775,5290
[   50.308288] Add VHT160/VHT80_80 pri80 and sec80 centers: 5530,5690
[   50.308292] Add VHT160/VHT80_80 pri80 and sec80 centers: 5690,5530
[   50.308296] Add VHT160/VHT80_80 pri80 and sec80 centers: 5530,5775
[   50.308300] Add VHT160/VHT80_80 pri80 and sec80 centers: 5775,5530
[   50.308305] Add VHT160/VHT80_80 pri80 and sec80 centers: 5610,5775
[   50.308334] Add VHT160/VHT80_80 pri80 and sec80 centers: 5775,5610
[   50.308339] Add VHT160/VHT80_80 pri80 and sec80 centers: 5690,5775
[   50.308343] Add VHT160/VHT80_80 pri80 and sec80 centers: 5775,5690
[   50.310124] ol_ath_phyerr_attach: called
[   50.310143] AVM/WLAN: cc=840. Clearing potential non valid maxpwr entries
[   50.310247] freq=58 
[   50.310251] freq=106 
[   50.310253] freq=122 
[   50.310337] OL Resmgr Init-ed
[   50.310661] ieee80211_cbs_init 
[   50.310666] CBS Inited
[   50.310682] ieee80211_bsteering_attach: Band steering initialized
[   50.310745] acfg_attach: 3056: Netlink socket created:9f436800
[   50.310758] ol_if_spectral_setup
[   50.310783] SPECTRAL : get_capability not registered
[   50.310787] HAL_CAP_PHYDIAG : Capable
[   50.310793] SPECTRAL : Need to fix the capablity check for RADAR (spectral_attach : 242)
[   50.310796] SPECTRAL : get_capability not registered
[   50.310799] HAL_CAP_RADAR   : Capable
[   50.310804] SPECTRAL : Need to fix the capablity check for SPECTRAL
                (spectral_attach : 247)
[   50.310807] SPECTRAL : get_capability not registered
[   50.310810] HAL_CAP_SPECTRAL_SCAN : Capable
[   50.310814] SPECTRAL : get_tsf64 not registered
[   50.310832] spectral_init_netlink 85 NULL SKB
[   50.310869] GreenAP on wifi0: Attached
[   50.310873] Green-AP : Attached
[   50.310878] rate power table override is only supported for AR98XX
[   50.310969] ol_if_dfs_setup: called 
[   50.311020] ol_if_dfs_attach: called; ptr=9c34198c, radar_info=9abafb58
[   50.311027] dfs_attach: event log enabled by default
[   50.312010] ol_ath_rtt_meas_report_attach: called
[   50.312021] ol_ath_lowi_wmi_event_attach: called
[   50.312041] >>>> CB Set 00000000
[   50.313458] ol_ath_attach() UMAC attach . 
[   50.313468] 
                BURSTING enabled by default
[   50.313528] ol_ath_attach: Set global_ic[1] ..ptr:88bf60d0
[   50.313602] ath_lowi_if_netlink_init LOWI Netlink successfully created
[   50.313618] cfr_netlink_init CFR Netlink successfully created
[   50.313670] ath_adhoc_netlink_init NETLINK_KERNEL_CREATE FAILED
[   50.313702] osif_wrap_attach:444 osif wrap attached
[   50.313741] osif_wrap_devt_init:405 osif wrap dev table init done
[   50.313748]  Wrap Attached: Wrap_com =9aa1b800 ic->ic_wrap_com=9aa1b800 &wrap_com->wc_devt=9aa1b800 
[   50.313754] __ol_ath_attach: needed_headroom reservation 60
[   50.317075] AVM/WLAN: __ol_ath_thermal_mitigation_attach -> temperature callback registered for wifi0 as Wifi-5GHz!
[   50.317098] ol_ath_thermal_mitigation_attach: —
[   50.317206] ol_ath_pci_probe num_radios=0, wifi_radios[0].sc = 9aac04a0 wifi_radio_type = 2
[   50.317301] ath_sysfs_diag_init: diag_fsattr 
[   50.317430] Suspending Target  scn=9aac04a0
[   50.317459] waiting for target paused event from target 
[   50.323796] ol_ath_thermal_mitigation_detach: ++
[   50.323914] AVM/WLAN: __ol_ath_thermal_mitigation_detach -> temperature callback deregistered for wifi0!
[   50.323976] ol_ath_thermal_mitigation_detach: —
[   50.324109] freq=58 
[   50.324118] freq=106 
[   50.324122] freq=122 
[   50.324147] DFS clear list erased
[   50.324169] ol_if_dfs_clist_update: called, cmd=1, nollist=00000000, nentries=0
[   50.327566] ce_h2t_tx_ce_cleanup 1089 Fastpath mode ON, Cleaning up HTT Tx CE
[   50.327735] smart_log_deinit: Smart logging Disabled
[   50.328236] ol_tx_me_exit: Already Disabled !!!
[   50.331078] htt_avm_offload_deinit:251 unregistered irq 276 for wifi0-avm_offload_rx_refill on wifi0
[   50.331108] htt_avm_offload_deinit:257 unregistered irq 277 for wifi0-avm_offload_tx_free on wifi0
[   50.331626] 
               ol_ath_free_tgt_iram() iram free paddr: 0x980000 host paddr 0x25b00000 Radio id 0
[   50.331680] hif_pci_device_reset: Reset Device
[   50.338376] hif_pci_disable_bus: X
[   50.338388] hif_disable: X
[   50.352448] hif_napi_destroy: NAPI 6 destroyed
[   50.352488] hif_napi_destroy: no NAPI instances. Zapped.
[   50.352715] ath_sysfs_diag_fini: diag_fsattr 
[   50.352736] ol_ath_pci_probe:207: EXIT(OK)
[   51.166412] [1]system-load  37% loadavg 1.14 0.30 0.10 - task runtime:9% max:kworker/u8:4 7%  pgstat: sum=186426 free=75733 slab=4388 alloc=2808/s fault=2719/s (sleep 0)
[   51.689636] [2]system-load  42% loadavg 1.14 0.30 0.10 - task runtime:1% max:kworker/0:1H 0%  pgstat: sum=186463 free=75749 slab=4389 alloc=2465/s fault=2392/s (sleep 0)
[   52.720421] start slab_allocator-trace now  (use cat /proc/slab_allocators)
—END_DEV_DEBUG—

—BEGIN_HOSTAPD_SUPPORT—
—END_HOSTAPD_SUPPORT—

—BEGIN_WPA_SUPP_SUPPORT—
—END_WPA_SUPP_SUPPORT—

—BEGIN_HOSTAPD_SOCKETS—
—END_HOSTAPD_SOCKETS—

—BEGIN_WPA_SUPP_SOCKETS—
—END_WPA_SUPP_SOCKETS—

—BEGIN_WLANCFG_SSIDS—
        ssid = „FRITZ!Box 7580 AX“;
        ssid_scnd = „FRITZ!Box 7580 AX“;
        ssid_thrd = „FRITZ!Box 7580 AX“;
        hidden_ssid = 0;
        WDS_ssid = „“;
        guest_ssid_set = no;
        guest_ssid = „FRITZ!Box Gastzugang“;
        STA_ssid = „“;
        STA_ssid_scnd = „“;
        STA_ssid_thrd = „“;
—END_WLANCFG_SSIDS—

—BEGIN_EMPTY_PSKS—
Empty PSKs: guest_pskvalue STA_pskvalue STA_pskvalue_scnd STA_pskvalue_thrd
WLAN key is set in Urlader-Env
—END_EMPTY_PSKS—

—BEGIN_ACS_DECISION_INFO—

—END_ACS_DECISION_INFO—
——————————————END_WLAN_SUBSYSTEM_LOG——————————————
killall: hostapd: no process killed
dsld[2078]: avmipc: connect
dsld[2078]: connect
dsld[2078]: avmipc: connect
dsld[2078]: connect
dsld[2078]: avmipc: connect
dsld[2078]: connect
dsld[2078]: avmipc: connect
dsld[2078]: connect

# 
# dsld[2078]: avmipc: connect
dsld[2078]: connect