(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
		(47 "User.5" user)
		(49 "User.6" user)
		(51 "User.7" user)
		(53 "User.8" user)
		(55 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions yes)
			(usegerberattributes no)
			(usegerberadvancedattributes no)
			(creategerberjobfile no)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 6)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk yes)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "AVR-Transistortester-SMD-Adapterboard-gerbers")
		)
	)
	(net 0 "")
	(net 1 "1")
	(net 2 "2")
	(net 3 "3")
	(net 4 "TEST3")
	(net 5 "TESTZ+")
	(net 6 "TEST1")
	(net 7 "TEST2")
	(net 8 "TESTZ-")
	(footprint "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.3x1.5mm"
		(layer "F.Cu")
		(at 105.9 88.3 -90)
		(descr "8-Lead Plastic Dual Flat, No Lead Package (8MA2) - 2x3x0.6 mm Body [UDFN] (see Atmel-8815-SEEPROM-AT24CS01-02-Datasheet.pdf)")
		(tags "DFN 0.5")
		(property "Reference" "REF**"
			(at 0 -2.05 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "DFN-8-1EP_3x2mm_P0.5mm_EP1.3x1.5mm"
			(at 0 2.05 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "" smd rect
			(at -0.325 -0.375 270)
			(size 0.5 0.6)
			(layers "F.Paste")
		)
		(pad "" smd rect
			(at -0.325 0.375 270)
			(size 0.5 0.6)
			(layers "F.Paste")
		)
		(pad "" smd rect
			(at 0.325 -0.375 270)
			(size 0.5 0.6)
			(layers "F.Paste")
		)
		(pad "" smd rect
			(at 0.325 0.375 270)
			(size 0.5 0.6)
			(layers "F.Paste")
		)
		(pad "1" smd rect
			(at -1.45 -0.75 270)
			(size 0.75 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "2" smd rect
			(at -1.45 -0.25 270)
			(size 0.75 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "3" smd rect
			(at -1.45 0.25 270)
			(size 0.75 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "4" smd rect
			(at -1.45 0.75 270)
			(size 0.75 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "5" smd rect
			(at 1.45 0.75 270)
			(size 0.75 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "6" smd rect
			(at 1.45 0.25 270)
			(size 0.75 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "7" smd rect
			(at 1.45 -0.25 270)
			(size 0.75 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "8" smd rect
			(at 1.45 -0.75 270)
			(size 0.75 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "9" smd rect
			(at 0 0 270)
			(size 1.3 1.5)
			(layers "F.Cu" "F.Mask")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/DFN-8-1EP_3x2mm_P0.5mm_EP1.3x1.5mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1210_3225Metric"
		(layer "F.Cu")
		(at 135.075 54.9475)
		(descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "1210"
			(at 0 -2.28 0)
			(layer "F.SilkS")
		)
		(property "Value" "R"
			(at -1.27 2.28 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0)
			(size 1.125 2.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2222222222)
			(net 6 "TEST1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0)
			(size 1.125 2.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2222222222)
			(net 7 "TEST2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DFN_QFN:DFN-8_2x2mm_P0.5mm"
		(layer "F.Cu")
		(at 104.965 92.085 -90)
		(descr "DFN8 2x2, 0.5P; No exposed pad - Ref http://pdfserv.maximintegrated.com/land_patterns/90-0349.PDF")
		(tags "DFN 0.5")
		(property "Reference" "REF**"
			(at 0 -2.075 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "DFN-8_2x2mm_P0.5mm"
			(at 0 2.075 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(pad "1" smd rect
			(at -0.95 -0.75 270)
			(size 0.85 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "2" smd rect
			(at -0.95 -0.25 270)
			(size 0.85 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "3" smd rect
			(at -0.95 0.25 270)
			(size 0.85 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "4" smd rect
			(at -0.95 0.75 270)
			(size 0.85 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "5" smd rect
			(at 0.95 0.75 270)
			(size 0.85 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "6" smd rect
			(at 0.95 0.25 270)
			(size 0.85 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "7" smd rect
			(at 0.95 -0.25 270)
			(size 0.85 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "8" smd rect
			(at 0.95 -0.75 270)
			(size 0.85 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/DFN-8_2x2mm_P0.5mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_MiniMELF"
		(layer "F.Cu")
		(at 142.7 86.85)
		(descr "Diode Mini-MELF (SOD-80)")
		(tags "Diode Mini-MELF (SOD-80)")
		(property "Reference" "miniMELF"
			(at 0 -2 0)
			(layer "F.SilkS")
		)
		(property "Value" "D"
			(at 0 1.75 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.75 0)
			(size 1.3 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "TEST1")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.75 0)
			(size 1.3 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "TEST2")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SMA"
		(layer "F.Cu")
		(at 131.2 83.35)
		(descr "Diode SMA (DO-214AC)")
		(tags "Diode SMA (DO-214AC)")
		(property "Reference" "SMA"
			(at 0 -2.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "D"
			(at 0 2.6 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2 0)
			(size 2.5 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "TEST1")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2 0)
			(size 2.5 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "TEST2")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
		(layer "F.Cu")
		(at 123.95 92.1 90)
		(descr "module CMS SOT223 4 pins")
		(tags "CMS SOT")
		(property "Reference" "SOT223-3"
			(at 5.334 -0.254 180)
			(layer "F.SilkS")
		)
		(property "Value" "BC807"
			(at 0 4.5 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.15 -2.3 90)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "TEST1")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -3.15 0 90)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "TEST2")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 3.15 0 90)
			(size 2 3.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "TEST2")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -3.15 2.3 90)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "TEST3")
			(pinfunction "C")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 127.5375 54.9475)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "1206"
			(at 0 -1.82 0)
			(layer "F.SilkS")
		)
		(property "Value" "R"
			(at 0 1.82 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2222222222)
			(net 6 "TEST1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2222222222)
			(net 7 "TEST2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-18-3"
		(layer "F.Cu")
		(at 141.364724 70.534724)
		(descr "TO-18-3")
		(tags "TO-18-3")
		(property "Reference" "TO18"
			(at 1.339276 -4.248724 0)
			(layer "F.SilkS")
		)
		(property "Value" "TO-18-3"
			(at 1.27 4.02 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" thru_hole oval
			(at 0 0)
			(size 1.6 1.2)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "TEST1")
		)
		(pad "2" thru_hole oval
			(at 1.27 1.27)
			(size 1.2 1.2)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "TEST2")
		)
		(pad "3" thru_hole oval
			(at 2.54 0)
			(size 1.2 1.2)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "TEST3")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-18-3.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:TO-252-2"
		(layer "F.Cu")
		(at 135.2 69.45 90)
		(descr "TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-3-1/")
		(tags "DPAK TO-252 DPAK-3 TO-252-3 SOT-428")
		(property "Reference" "TO252-2"
			(at 6.604 -0.254 0)
			(layer "F.SilkS")
		)
		(property "Value" "BC807"
			(at 0 4.5 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.402 -0.25 90)
			(layer "F.Fab")
		)
		(pad "" smd rect
			(at 0.425 -1.525 90)
			(size 3.05 2.75)
			(layers "F.Paste")
		)
		(pad "" smd rect
			(at 0.425 1.525 90)
			(size 3.05 2.75)
			(layers "F.Paste")
		)
		(pad "" smd rect
			(at 3.775 -1.525 90)
			(size 3.05 2.75)
			(layers "F.Paste")
		)
		(pad "" smd rect
			(at 3.775 1.525 90)
			(size 3.05 2.75)
			(layers "F.Paste")
		)
		(pad "1" smd rect
			(at -4.2 -2.28 90)
			(size 2.2 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "TEST1")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 2.1 0 90)
			(size 6.4 5.8)
			(layers "F.Cu" "F.Mask")
			(net 7 "TEST2")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -4.2 2.28 90)
			(size 2.2 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "TEST3")
			(pinfunction "C")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/TO-252-2.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Fiducial:Fiducial_1mm_Mask2mm"
		(layer "F.Cu")
		(at 105.2 100.1)
		(descr "Fiducial, circular marking, 1mm bare copper, 2mm soldermask opening (Level A)")
		(tags "fiducial")
		(property "Reference" "REF**"
			(at 0 -1.95 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Fiducial_1mm_Mask2mm"
			(at 0 1.95 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(solder_mask_margin 0.5)
			(clearance 0.6)
		)
		(embedded_fonts no)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-6"
		(layer "F.Cu")
		(at 129.2275 59.065)
		(descr "SOT, 6 Pin (JEDEC MO-178 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "REF**"
			(at 0 -2.4 0)
			(layer "F.SilkS")
		)
		(property "Value" "SOT-23-6"
			(at 0 2.4 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "2" smd roundrect
			(at -1.1375 0)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "5" smd roundrect
			(at 1.1375 0)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "6" smd roundrect
			(at 1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SOD-123"
		(layer "F.Cu")
		(at 135.45 78.1)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "SOD123"
			(at 0 -2 0)
			(layer "F.SilkS")
		)
		(property "Value" "D"
			(at 0 2.1 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.65 0)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "TEST1")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.65 0)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "TEST2")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SMB"
		(layer "F.Cu")
		(at 131.95 89.35)
		(descr "Diode SMB (DO-214AA)")
		(tags "Diode SMB (DO-214AA)")
		(property "Reference" "SMB"
			(at 0 -3 0)
			(layer "F.SilkS")
		)
		(property "Value" "D"
			(at 0 3.1 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -3 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.15 0)
			(size 2.5 2.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "TEST1")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.15 0)
			(size 2.5 2.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "TEST2")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMB.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 119.45 83.35 90)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "SOT23"
			(at 2.75 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "BC807"
			(at 0 2.4 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "TEST1")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "TEST2")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "TEST3")
			(pinfunction "C")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SOD-323"
		(layer "F.Cu")
		(at 130 79.1)
		(descr "SOD-323")
		(tags "SOD-323")
		(property "Reference" "SOD323"
			(at 0 -1.85 0)
			(layer "F.SilkS")
		)
		(property "Value" "D"
			(at 0.1 1.9 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.85 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.05 0)
			(size 0.6 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "TEST1")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0)
			(size 0.6 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "TEST2")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-323.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_MicroMELF"
		(layer "F.Cu")
		(at 143.7 82.85)
		(descr "Diode, MicroMELF, Reflow Soldering, http://www.vishay.com/docs/85597/bzm55.pdf")
		(tags "MicroMELF Diode")
		(property "Reference" "µMELF"
			(at 0 -1.544 0)
			(layer "F.SilkS")
		)
		(property "Value" "D"
			(at 0 1.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.5 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.8 0)
			(size 0.8 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "1")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.8 0)
			(size 0.8 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "TEST2")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MicroMELF.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SON:VSON-8-1EP_3x3mm_P0.65mm_EP1.6x2.4mm"
		(layer "F.Cu")
		(at 101.5 87.6)
		(descr "VSON, 8 Pin (https://www.ti.com/lit/ds/symlink/thvd1450.pdf#page=37), generated with kicad-footprint-generator ipc_noLead_generator.py")
		(tags "VSON NoLead")
		(property "Reference" "REF**"
			(at 0 -2.45 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "VSON-8-1EP_3x3mm_P0.65mm_EP1.6x2.4mm"
			(at 0 2.45 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at 0 -0.6)
			(size 1.29 0.97)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0 0.6)
			(size 1.29 0.97)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -1.4375 -0.975)
			(size 0.875 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "2" smd roundrect
			(at -1.4375 -0.325)
			(size 0.875 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "3" smd roundrect
			(at -1.4375 0.325)
			(size 0.875 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "4" smd roundrect
			(at -1.4375 0.975)
			(size 0.875 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "5" smd roundrect
			(at 1.4375 0.975)
			(size 0.875 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "6" smd roundrect
			(at 1.4375 0.325)
			(size 0.875 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "7" smd roundrect
			(at 1.4375 -0.325)
			(size 0.875 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "8" smd roundrect
			(at 1.4375 -0.975)
			(size 0.875 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "9" smd rect
			(at 0 0)
			(size 1.6 2.4)
			(property pad_prop_heatsink)
			(layers "F.Cu" "F.Mask")
			(zone_connect 2)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SON.3dshapes/VSON-8-1EP_3x3mm_P0.65mm_EP1.6x2.4mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_ISO7380_Pad"
		(layer "F.Cu")
		(at 142.7 97.6)
		(descr "Mounting Hole 3.2mm, M3, ISO7380")
		(tags "mounting hole 3.2mm m3 iso7380")
		(property "Reference" "REF**"
			(at 0 -3.85 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_3.2mm_M3_ISO7380_Pad"
			(at 0 3.85 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 5.7 5.7)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint "Fiducial:Fiducial_1mm_Mask2mm"
		(layer "F.Cu")
		(at 105.45 57.35)
		(descr "Fiducial, circular marking, 1mm bare copper, 2mm soldermask opening (Level A)")
		(tags "fiducial")
		(property "Reference" "REF**"
			(at 0 -1.95 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Fiducial_1mm_Mask2mm"
			(at 0 1.95 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(solder_mask_margin 0.5)
			(clearance 0.6)
		)
		(embedded_fonts no)
	)
	(footprint "Diode_SMD:D_SOD-523"
		(layer "F.Cu")
		(at 129.95 75.6)
		(descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
		(tags "Diode SOD523")
		(property "Reference" "SOD523"
			(at -1.5 -1.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "D"
			(at 1.905 0.13 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(pad "1" smd rect
			(at -0.7 0 180)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "TEST1")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0 180)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "TEST2")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-523.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kikad_lib:R0603"
		(layer "F.Cu")
		(at 115.535 54.6655)
		(property "Reference" "0603"
			(at 0.765 -1.3655 180)
			(layer "F.SilkS")
		)
		(property "Value" "R0603"
			(at 0 1.7 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(pad "1" smd rect
			(at -0.762 0)
			(size 0.889 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "TEST1")
		)
		(pad "2" smd rect
			(at 0.762 0)
			(size 0.889 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "TEST2")
		)
		(embedded_fonts no)
	)
	(footprint "Diode_SMD:D_SOD-128"
		(layer "F.Cu")
		(at 142.45 78.35)
		(descr "D_SOD-128 (CFP5 SlimSMAW), https://assets.nexperia.com/documents/outline-drawing/SOD128.pdf")
		(tags "D_SOD-128")
		(property "Reference" "SOD128"
			(at 0.27 -2.225 0)
			(layer "F.SilkS")
		)
		(property "Value" "D"
			(at 0 2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(pad "1" smd rect
			(at -2.2 0)
			(size 1.4 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "TEST1")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.2 0)
			(size 1.4 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "TEST2")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-128.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-89-3"
		(layer "F.Cu")
		(at 124.45 82.85 90)
		(descr "SOT-89-3, http://ww1.microchip.com/downloads/en/DeviceDoc/3L_SOT-89_MB_C04-029C.pdf")
		(tags "SOT-89-3")
		(property "Reference" "SOT89-3"
			(at 3.404 0.25 180)
			(layer "F.SilkS")
		)
		(property "Value" "BC807"
			(at 0.3 3.5 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.5 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.65 -1.5 90)
			(size 1.3 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "TEST1")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd custom
			(at -1.5625 0 90)
			(size 1.475 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "TEST2")
			(pinfunction "E")
			(pintype "passive")
			(zone_connect 2)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy 3.8625 0.8665) (xy 0.7375 0.8665) (xy 0.7375 -0.8665) (xy 3.8625 -0.8665)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "3" smd rect
			(at -1.65 1.5 90)
			(size 1.3 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "TEST3")
			(pinfunction "C")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-89-3.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 120.5375 54.9475)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "0805"
			(at 0.7625 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "R"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902439)
			(net 6 "TEST1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902439)
			(net 7 "TEST2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0201_0603Metric"
		(layer "F.Cu")
		(at 107.355 54.6655)
		(descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "0201"
			(at -1.155 -1.1655 0)
			(layer "F.SilkS")
		)
		(property "Value" "R_0201_0603Metric"
			(at 0 1.05 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "TEST1")
		)
		(pad "2" smd roundrect
			(at 0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "TEST2")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-8_5.3x5.3mm_P1.27mm"
		(layer "F.Cu")
		(at 101.2 89.1 90)
		(descr "SOIC, 8 Pin (JEITA/EIAJ ED-7311-19 variation 08-001-BBA and Atmel/Microchip, 208 mils width, https://www.jeita.or.jp/japanese/standard/book/ED-7311-19/#target/page_no=21, https://ww1.microchip.com/downloads/en/DeviceDoc/20005045C.pdf#page=23, https://ww1.microchip.com/downloads/en/DeviceDoc/doc2535.pdf#page=162), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO P-SOP SOP SOP-8 SO SO-8 8S2 S2AE/F K04-056 CASE-751BE SO8W 8-Pin-SOIC PSA W8-2 W8-4 W8MS-1 FPT-8P-M08")
		(property "Reference" "REF**"
			(at 0 -3.6 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SOIC-8_5.3x5.3mm_P1.27mm"
			(at 0 3.6 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(pad "1" smd roundrect
			(at -3.5875 -1.905 90)
			(size 1.625 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "2" smd roundrect
			(at -3.5875 -0.635 90)
			(size 1.625 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "3" smd roundrect
			(at -3.5875 0.635 90)
			(size 1.625 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "4" smd roundrect
			(at -3.5875 1.905 90)
			(size 1.625 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "5" smd roundrect
			(at 3.5875 1.905 90)
			(size 1.625 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "6" smd roundrect
			(at 3.5875 0.635 90)
			(size 1.625 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "7" smd roundrect
			(at 3.5875 -0.635 90)
			(size 1.625 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "8" smd roundrect
			(at 3.5875 -1.905 90)
			(size 1.625 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_5.3x5.3mm_P1.27mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_ISO7380_Pad"
		(layer "F.Cu")
		(at 142.7 55.6)
		(descr "Mounting Hole 3.2mm, M3, ISO7380")
		(tags "mounting hole 3.2mm m3 iso7380")
		(property "Reference" "REF**"
			(at 0 -3.85 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_3.2mm_M3_ISO7380_Pad"
			(at 0 3.85 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 5.7 5.7)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint "Diode_SMD:D_MELF"
		(layer "F.Cu")
		(at 142.2 91.85)
		(descr "Diode, MELF,,")
		(tags "Diode MELF ")
		(property "Reference" "MELF"
			(at 1.5 -2.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "D"
			(at -0.25 2.5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(pad "1" smd rect
			(at -2.4 0)
			(size 1.5 2.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "TEST1")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.4 0)
			(size 1.5 2.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "TEST2")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MELF.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-353_SC-70-5"
		(layer "F.Cu")
		(at 101.75 90.5)
		(descr "SOT-353, SC-70-5")
		(tags "SOT-353 SC-70-5")
		(property "Reference" "REF**"
			(at 0 -2.25 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SOT-353_SC-70-5"
			(at 0 2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.95 -0.65)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "2" smd roundrect
			(at -0.95 0)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "3" smd roundrect
			(at -0.95 0.65)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "4" smd roundrect
			(at 0.95 0.65)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "5" smd roundrect
			(at 0.95 -0.65)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-353_SC-70-5.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SMC"
		(layer "F.Cu")
		(at 133.422 96.97)
		(descr "Diode SMC (DO-214AB)")
		(tags "Diode SMC (DO-214AB)")
		(property "Reference" "SMC"
			(at 0 -4.1 0)
			(layer "F.SilkS")
		)
		(property "Value" "D"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.9 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.4 0 90)
			(size 3.3 2.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "TEST1")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 3.4 0 90)
			(size 3.3 2.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "TEST2")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMC.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:TO-263-2"
		(layer "F.Cu")
		(at 122.7 70.225 90)
		(descr "TO-263 / D2PAK / DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-3-1/")
		(tags "D2PAK DDPAK TO-263 D2PAK-3 TO-263-3 SOT-404")
		(property "Reference" "TO263-2"
			(at 10 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "BC807"
			(at 0 6.65 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(pad "" smd rect
			(at 0.95 -2.775 90)
			(size 4.55 5.25)
			(layers "F.Paste")
		)
		(pad "" smd rect
			(at 0.95 2.775 90)
			(size 4.55 5.25)
			(layers "F.Paste")
		)
		(pad "" smd rect
			(at 5.8 -2.775 90)
			(size 4.55 5.25)
			(layers "F.Paste")
		)
		(pad "" smd rect
			(at 5.8 2.775 90)
			(size 4.55 5.25)
			(layers "F.Paste")
		)
		(pad "1" smd rect
			(at -5.775 -2.54 90)
			(size 4.6 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "TEST1")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 3.375 0 90)
			(size 9.4 10.8)
			(layers "F.Cu" "F.Mask")
			(net 7 "TEST2")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -5.775 2.54 90)
			(size 4.6 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "TEST3")
			(pinfunction "C")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/TO-263-2.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_ISO7380_Pad"
		(layer "F.Cu")
		(at 100.7 97.6)
		(descr "Mounting Hole 3.2mm, M3, ISO7380")
		(tags "mounting hole 3.2mm m3 iso7380")
		(property "Reference" "REF**"
			(at 0 -3.85 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_3.2mm_M3_ISO7380_Pad"
			(at 0 3.85 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 5.7 5.7)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint "Diode_SMD:D_SMF"
		(layer "F.Cu")
		(at 138.2 82.85)
		(descr "Diode SMF (DO-219AB), http://www.vishay.com/docs/95572/smf_do-219ab.pdf")
		(tags "Diode SMF (DO-214AB)")
		(property "Reference" "SMF"
			(at 0 -2 0)
			(layer "F.SilkS")
		)
		(property "Value" "D"
			(at 0 2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.45 0)
			(size 1.3 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "TEST1")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.45 0)
			(size 1.3 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "TEST2")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMF.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_CSP:WLCSP-6_1.4x1.0mm_P0.4mm"
		(layer "F.Cu")
		(at 101.75 90.5 -90)
		(descr "6pin Pitch 0.4mm")
		(tags "6pin Pitch 0.4mm WLCSP")
		(property "Reference" "REF**"
			(at 0 -1.7 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "WLCSP-6_1.4x1.0mm_P0.4mm"
			(at 0 1.8 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(pad "A1" smd circle
			(at -0.4 -0.2)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(solder_mask_margin 0.1)
		)
		(pad "A2" smd circle
			(at -0.4 0.2)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(solder_mask_margin 0.1)
		)
		(pad "B1" smd circle
			(at 0 -0.2)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(solder_mask_margin 0.1)
		)
		(pad "B2" smd circle
			(at 0 0.2)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(solder_mask_margin 0.1)
		)
		(pad "C1" smd circle
			(at 0.4 -0.2)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(solder_mask_margin 0.1)
		)
		(pad "C2" smd circle
			(at 0.4 0.2)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(solder_mask_margin 0.1)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_CSP.3dshapes/WLCSP-6_1.4x1.0mm_P0.4mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_ISO7380_Pad"
		(layer "F.Cu")
		(at 100.7 55.6)
		(descr "Mounting Hole 3.2mm, M3, ISO7380")
		(tags "mounting hole 3.2mm m3 iso7380")
		(property "Reference" "REF**"
			(at 0 -3.85 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_3.2mm_M3_ISO7380_Pad"
			(at 0 3.85 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 5.7 5.7)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint "kikad_lib:R0402"
		(layer "F.Cu")
		(at 111.035 54.6655)
		(property "Reference" "0402"
			(at 0.165 -1.1655 0)
			(layer "F.SilkS")
		)
		(property "Value" "R0402"
			(at 0 1.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(pad "1" smd rect
			(at -0.4445 0)
			(size 0.635 0.635)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "TEST1")
		)
		(pad "2" smd rect
			(at 0.4445 0)
			(size 0.635 0.635)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "TEST2")
		)
		(embedded_fonts no)
	)
	(footprint "Package_SO:MSOP-8_3x3mm_P0.65mm"
		(layer "F.Cu")
		(at 101.45 87.6)
		(descr "MSOP, 8 Pin (https://www.jedec.org/system/files/docs/mo-187F.pdf variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "MSOP SO")
		(property "Reference" "REF**"
			(at 0 -2.45 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MSOP-8_3x3mm_P0.65mm"
			(at 0 2.45 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(pad "1" smd roundrect
			(at -2.1125 -0.975)
			(size 1.625 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "2" smd roundrect
			(at -2.1125 -0.325)
			(size 1.625 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "3" smd roundrect
			(at -2.1125 0.325)
			(size 1.625 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "4" smd roundrect
			(at -2.1125 0.975)
			(size 1.625 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "5" smd roundrect
			(at 2.1125 0.975)
			(size 1.625 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "6" smd roundrect
			(at 2.1125 0.325)
			(size 1.625 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "7" smd roundrect
			(at 2.1125 -0.325)
			(size 1.625 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "8" smd roundrect
			(at 2.1125 -0.975)
			(size 1.625 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/MSOP-8_3x3mm_P0.65mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:TSOT-23-5_HandSoldering"
		(layer "F.Cu")
		(at 101.595 90.5)
		(descr "5-pin TSOT23 package, http://cds.linear.com/docs/en/packaging/SOT_5_05-08-1635.pdf")
		(tags "TSOT-23-5 Hand-soldering")
		(property "Reference" "REF**"
			(at 0 -2.45 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TSOT-23-5_HandSoldering"
			(at 0 2.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(pad "1" smd roundrect
			(at -1.71 -0.95)
			(size 2 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "2" smd roundrect
			(at -1.71 0)
			(size 2 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "3" smd roundrect
			(at -1.71 0.95)
			(size 2 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "4" smd roundrect
			(at 1.71 0.95)
			(size 2 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "5" smd roundrect
			(at 1.71 -0.95)
			(size 2 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/TSOT-23-5.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
		(layer "B.Cu")
		(at 120.16 99.1 -90)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "J1"
			(at 0 2.33 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x02"
			(at 0 -7.41 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.88 -13.025 0)
			(layer "B.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "TEST1")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 -2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "TEST2")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 -5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "TEST3")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "1X05"
		(layer "B.Cu")
		(at 100.49 72.82 -90)
		(descr "PIN HEADER")
		(property "Reference" "JP5"
			(at -6.4262 1.8288 90)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TESTSMD"
			(at -6.35 -3.175 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "1" thru_hole oval
			(at -5.08 0 180)
			(size 3.2512 1.6256)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "TEST1")
			(solder_mask_margin 0.0508)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole oval
			(at -2.54 0 180)
			(size 3.2512 1.6256)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "TEST2")
			(solder_mask_margin 0.0508)
			(thermal_bridge_angle 0)
		)
		(pad "3" thru_hole oval
			(at 0 0 180)
			(size 3.2512 1.6256)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "TEST3")
			(solder_mask_margin 0.0508)
			(thermal_bridge_angle 0)
		)
		(pad "4" thru_hole oval
			(at 2.54 0 180)
			(size 3.2512 1.6256)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "TESTZ+")
			(solder_mask_margin 0.0508)
			(thermal_bridge_angle 0)
		)
		(pad "5" thru_hole oval
			(at 5.08 0 180)
			(size 3.2512 1.6256)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "TESTZ-")
			(solder_mask_margin 0.0508)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(gr_line
		(start 146.7 51.6)
		(end 146.7 101.6)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 96.7 51.6)
		(end 146.7 51.6)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.95 83.615)
		(end 117 83.615)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 117 83.615)
		(end 117 58.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.95 58.85)
		(end 97.95 83.615)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 96.7 101.6)
		(end 96.7 51.6)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.95 58.85)
		(end 117 58.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 146.7 101.6)
		(end 96.7 101.6)
		(layer "Edge.Cuts")
	)
	(gr_text "Z-"
		(at 99.22 81.329 0)
		(layer "F.SilkS")
	)
	(gr_text "2"
		(at 125.617 62.023 0)
		(layer "F.SilkS")
	)
	(gr_text "1"
		(at 140.037 64.632 0)
		(layer "F.SilkS")
	)
	(gr_text "2"
		(at 142.45 64.632 0)
		(layer "F.SilkS")
	)
	(gr_text "2"
		(at 112.936 77.392 0)
		(layer "F.SilkS")
	)
	(gr_text "1"
		(at 128.668 62.438 0)
		(layer "F.SilkS")
	)
	(gr_text "3"
		(at 144.736 64.632 0)
		(layer "F.SilkS")
	)
	(gr_text "3"
		(at 114.46 74.598 0)
		(layer "F.SilkS")
	)
	(gr_text "1"
		(at 112.301 74.598 0)
		(layer "F.SilkS")
	)
	(gr_text "3"
		(at 117.164 82.334 0)
		(layer "F.SilkS")
	)
	(gr_text "Z+"
		(at 113.063 81.329 0)
		(layer "F.SilkS")
	)
	(gr_text "AVR Transistor-Tester\nSMD Adapterboard\n(20251207)"
		(at 151.7 78.6 270)
		(layer "B.SilkS")
	)
	(zone
		(net 1)
		(net_name "1")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 142.069 62.95563) (xy 139.529 63.97163) (xy 139.529 61.93963)
			)
		)
	)
	(zone
		(net 4)
		(net_name "TEST3")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads yes
			(clearance 0.000001)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.304)
			(thermal_bridge_width 0.304)
		)
		(polygon
			(pts
				(xy 116.492 71.677) (xy 111.666 71.677) (xy 111.666 66.724) (xy 107.729 66.724) (xy 107.729 64.565)
				(xy 106.967 64.565) (xy 106.967 59.358) (xy 116.492 59.358)
			)
		)
	)
	(zone
		(net 5)
		(net_name "TESTZ+")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads
			(clearance 0.000001)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.304)
			(thermal_bridge_width 0.304)
		)
		(polygon
			(pts
				(xy 116.492 83.107) (xy 105.951 83.107) (xy 105.951 79.043) (xy 116.492 79.043)
			)
		)
	)
	(zone
		(net 7)
		(net_name "TEST2")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads yes
			(clearance 0.000001)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.304)
			(thermal_bridge_width 0.304)
		)
		(polygon
			(pts
				(xy 107.475 66.978) (xy 111.412 66.978) (xy 111.412 78.027) (xy 102.268 78.027) (xy 102.268 71.042)
				(xy 99.093 71.042) (xy 99.093 69.518) (xy 102.268 69.518) (xy 102.268 66.978) (xy 106.205 66.978)
				(xy 106.205 64.819) (xy 107.475 64.819)
			)
		)
	)
	(zone
		(net 8)
		(net_name "TESTZ-")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads
			(clearance 0.000001)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.304)
			(thermal_bridge_width 0.304)
		)
		(polygon
			(pts
				(xy 101.887 79.043) (xy 105.697 79.043) (xy 105.697 83.107) (xy 99.093 83.107) (xy 99.093 77.773)
				(xy 101.887 77.773)
			)
		)
	)
	(zone
		(net 6)
		(net_name "TEST1")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads
			(clearance 0.3)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.3)
			(thermal_bridge_width 0.3)
		)
		(polygon
			(pts
				(xy 109.22 86.36) (xy 114.3 86.36) (xy 114.3 91.44) (xy 109.22 91.44)
			)
		)
	)
	(zone
		(net 3)
		(net_name "3")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 142.882598 62.945966) (xy 145.422598 61.929966) (xy 145.422598 63.961966)
			)
		)
	)
	(zone
		(net 6)
		(net_name "TEST1")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads
			(clearance 0.000001)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.304)
			(thermal_bridge_width 0.304)
		)
		(polygon
			(pts
				(xy 106.713 64.565) (xy 105.951 64.565) (xy 105.951 66.724) (xy 101.887 66.724) (xy 101.887 68.502)
				(xy 99.093 68.502) (xy 99.093 59.358) (xy 106.713 59.358)
			)
		)
	)
	(zone
		(net 2)
		(net_name "2")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 142.45 62.6) (xy 141.434 60.06) (xy 143.466 60.06)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Mask")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads
			(clearance 0.000001)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.304)
			(thermal_bridge_width 0.304)
		)
		(polygon
			(pts
				(xy 105.697 83.107) (xy 102.903 83.107) (xy 102.903 79.043) (xy 105.697 79.043)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Mask")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads
			(clearance 0.000001)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.304)
			(thermal_bridge_width 0.304)
		)
		(polygon
			(pts
				(xy 106.713 64.565) (xy 105.951 64.565) (xy 105.951 66.724) (xy 99.093 66.724) (xy 99.093 59.358)
				(xy 106.713 59.358)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Mask")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads
			(clearance 0.000001)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.304)
			(thermal_bridge_width 0.304)
		)
		(polygon
			(pts
				(xy 107.475 66.978) (xy 111.412 66.978) (xy 111.412 78.027) (xy 102.268 78.027) (xy 102.268 66.978)
				(xy 106.205 66.978) (xy 106.205 64.819) (xy 107.475 64.819)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Mask")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads
			(clearance 0.000001)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.304)
			(thermal_bridge_width 0.304)
		)
		(polygon
			(pts
				(xy 112.555 83.107) (xy 105.951 83.107) (xy 105.951 79.043) (xy 112.555 79.043)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Mask")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads
			(clearance 0.000001)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.304)
			(thermal_bridge_width 0.304)
		)
		(polygon
			(pts
				(xy 116.492 71.677) (xy 111.666 71.677) (xy 111.666 66.724) (xy 107.729 66.724) (xy 107.729 64.565)
				(xy 106.967 64.565) (xy 106.967 59.358) (xy 116.492 59.358)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 146.7 101.6) (xy 96.7 101.6) (xy 96.7 51.6) (xy 146.7 51.6)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.SilkS")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads
			(clearance 0.000001)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.304)
			(thermal_bridge_width 0.304)
		)
		(polygon
			(pts
				(xy 116.492 78.027) (xy 115.222 78.027) (xy 115.222 76.376) (xy 116.492 76.376)
			)
		)
	)
	(embedded_fonts no)
)
