(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A5")
	(title_block
		(title "Interface_1")
		(date "12.01.2026")
		(rev "0.0-1")
		(company "Hügli Präzisions-Mechanik")
	)
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_575555ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "../../Gerber/Interface_1/")
		)
	)
	(net 0 "")
	(net 1 "Net-(KL1-Pin_1)")
	(net 2 "Net-(D1-K)")
	(net 3 "Net-(C2-Pad1)")
	(net 4 "Net-(KL5-Pin_1)")
	(net 5 "Net-(D1-A)")
	(net 6 "Net-(D2-A)")
	(net 7 "Net-(D3-K)")
	(net 8 "Net-(D4-K)")
	(net 9 "Net-(J1-Pin_2)")
	(net 10 "Net-(Q1-B)")
	(net 11 "Net-(Q2-B)")
	(net 12 "Net-(J1-Pin_3)")
	(net 13 "Net-(Q3-B)")
	(net 14 "Net-(Q3-C)")
	(net 15 "Net-(Q4-S)")
	(net 16 "unconnected-(K1-Pad4)")
	(net 17 "Net-(K2-Pad3)")
	(net 18 "unconnected-(K2-Pad4)")
	(net 19 "Net-(ZD5-A)")
	(net 20 "Net-(ZD5-K)")
	(footprint "Eigene Footpriths:Relay_1 x Um_Print_SRD"
		(layer "F.Cu")
		(at 92.6084 72.4438)
		(descr "relay Sanyou SRD series Form C http://www.sanyourelay.ca/public/products/pdf/SRD.pdf")
		(tags "relay Sanyu SRD form C")
		(property "Reference" "K2"
			(at 14.2494 -0.1808 0)
			(layer "F.SilkS")
		)
		(property "Value" "Relay_SRD"
			(at 8.4836 -9.144 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Relay SPDT, monostable, EN50005"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Relay?SPDT*")
		(sheetname "/")
		(sheetfile "Interface_1.kicad_sch")
		(attr through_hole)
		(fp_text user "Rel"
			(at 9.7028 -1.27 0)
			(layer "F.SilkS")
		)
		(fp_text user "1"
			(at 0 -2.3 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 4 3.5)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.4285714286)
			(net 2 "Net-(D1-K)")
			(pintype "passive")
		)
		(pad "2" thru_hole roundrect
			(at 2 6 90)
			(size 4 4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.375)
			(net 2 "Net-(D1-K)")
			(pintype "passive")
		)
		(pad "3" thru_hole roundrect
			(at 14.2 6 90)
			(size 4 4)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.375)
			(net 17 "Net-(K2-Pad3)")
			(pintype "passive")
		)
		(pad "4" thru_hole roundrect
			(at 14.2 -6 90)
			(size 4 4)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.375)
			(net 18 "unconnected-(K2-Pad4)")
			(pintype "passive+no_connect")
		)
		(pad "5" thru_hole roundrect
			(at 2 -6 90)
			(size 4 4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.375)
			(net 6 "Net-(D2-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Relay_THT.3dshapes/Relay_SPDT_SANYOU_SRD_Series_Form_C.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Eigene Footpriths:C-Keramic"
		(layer "F.Cu")
		(at 71.77295 47.3066 180)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm diameter 5mm width 2.5mm Capacitor")
		(property "Reference" "C1"
			(at 2.4892 -0.1524 0)
			(layer "F.SilkS")
		)
		(property "Value" "C_Small"
			(at 2.5 2.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "Interface_1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole roundrect
			(at 0 0 180)
			(size 2 3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 1 "Net-(KL1-Pin_1)")
			(pintype "passive")
		)
		(pad "2" thru_hole roundrect
			(at 5 0 180)
			(size 2 3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 15 "Net-(Q4-S)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Eigene Footpriths:Schraubklemme"
		(layer "F.Cu")
		(at 110.06535 40.7026)
		(descr "2 Pin")
		(tags "Klemme")
		(property "Reference" "KL4"
			(at 2.4892 -3.1496 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Schraubklemme"
			(at 2.54 -3.81 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Klemme Rot"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "/")
		(sheetfile "Interface_1.kicad_sch")
		(attr through_hole allow_missing_courtyard)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 3.5 4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.2857142857)
			(net 6 "Net-(D2-A)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0)
			(clearance 0)
		)
		(pad "2" thru_hole roundrect
			(at 5.08 0)
			(size 3.5 4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.3333333333)
			(net 6 "Net-(D2-A)")
			(pinfunction "Pin_2")
			(pintype "passive")
			(clearance 0)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Same_Sky_TB006-508-02BE.igs"
			(offset
				(xyz -5.08 -4.1 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -90)
			)
		)
	)
	(footprint "Eigene Footpriths:Schraubklemme"
		(layer "F.Cu")
		(at 120.88575 40.7534)
		(descr "2 Pin")
		(tags "Klemme")
		(property "Reference" "KL5"
			(at 2.54 -3.2004 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Schraubklemme"
			(at 2.54 -3.81 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Klemme Rot"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "/")
		(sheetfile "Interface_1.kicad_sch")
		(attr through_hole allow_missing_courtyard)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 3.5 4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.2857142857)
			(net 4 "Net-(KL5-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0)
			(clearance 0)
		)
		(pad "2" thru_hole roundrect
			(at 5.08 0)
			(size 3.5 4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.3333333333)
			(net 12 "Net-(J1-Pin_3)")
			(pinfunction "Pin_2")
			(pintype "passive")
			(clearance 0)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Same_Sky_TB006-508-02BE.igs"
			(offset
				(xyz -5.08 -4.1 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -90)
			)
		)
	)
	(footprint "Eigene Footpriths:Z-Diode"
		(layer "F.Cu")
		(at 67.24095 52.1834)
		(descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, length*diameter=5.2*2.7mm^2, https://www.diodes.com/assets/Package-Files/DO-41-Plastic.pdf")
		(tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
		(property "Reference" "ZD5"
			(at 5.08 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "Z-Diode 9.1V"
			(at 5.08 2.47 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.vishay.com/docs/85816/1n4728a.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1300mW Silicon planar power Zener diodes, DO-41"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*DO?41*")
		(sheetname "/")
		(sheetfile "Interface_1.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at 1.92325 -0.7484 0)
			(layer "F.SilkS")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 3 3)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.3333333333)
			(net 20 "Net-(ZD5-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole roundrect
			(at 10.16 0)
			(size 3 3)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.3333333333)
			(net 19 "Net-(ZD5-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Eigene Footpriths:TO-220-3_Vertical"
		(layer "F.Cu")
		(at 75.4126 47.1678)
		(descr "TO-247-3, Vertical, RM 5.45mm, see https://toshiba.semicon-storage.com/us/product/mosfet/to-247-4l.html, generated with kicad-footprint-generator TO_SOT_THT_generate.py")
		(tags "TO-247-3 Vertical RM 5.45mm")
		(property "Reference" "Q4"
			(at 2.1844 2.7432 0)
			(layer "F.SilkS")
		)
		(property "Value" "MOSFET_P-Kanal_TO220"
			(at 3.429 2.8448 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "kicad-embed://irf9530.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "P-MOSFET transistor, drain/gate/source"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "Interface_1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 2 3)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 14 "Net-(Q3-C)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" thru_hole roundrect
			(at 2.54 0)
			(size 2 3)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 2 "Net-(D1-K)")
			(pinfunction "D")
			(pintype "passive")
		)
		(pad "3" thru_hole roundrect
			(at 5.08 0)
			(size 2 3)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.2)
			(net 15 "Net-(Q4-S)")
			(pinfunction "S")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Eigene Footpriths:Widerstand 15.24  mm"
		(layer "F.Cu")
		(at 67.64735 72.5542 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=15.24mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 15.24mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R2"
			(at 7.62 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "1K"
			(at 7.6 3 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Interface_1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 4 4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 13 "Net-(Q3-B)")
			(pintype "passive")
		)
		(pad "2" thru_hole roundrect
			(at 15.24 0 90)
			(size 4 4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 19 "Net-(ZD5-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P15.24mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Eigene Footpriths:Schraubklemme"
		(layer "F.Cu")
		(at 87.91655 40.6518)
		(descr "2 Pin")
		(tags "Klemme")
		(property "Reference" "KL2"
			(at 2.4384 -3.048 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Schraubklemme"
			(at 2.54 -3.81 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Klemme Rot"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "/")
		(sheetfile "Interface_1.kicad_sch")
		(attr through_hole allow_missing_courtyard)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 3.5 4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.2857142857)
			(net 2 "Net-(D1-K)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0)
			(clearance 0)
		)
		(pad "2" thru_hole roundrect
			(at 5.08 0)
			(size 3.5 4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.3333333333)
			(net 12 "Net-(J1-Pin_3)")
			(pinfunction "Pin_2")
			(pintype "passive")
			(clearance 0)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Same_Sky_TB006-508-02BE.igs"
			(offset
				(xyz -5.08 -4.1 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -90)
			)
		)
	)
	(footprint "Eigene Footpriths:Stiftanschluss_3_Pin"
		(layer "F.Cu")
		(at 58.75735 84.201 180)
		(descr "Through hole straight pin header, 1x03, 1.00mm pitch, single row")
		(tags "Through hole pin header THT 1x03 1.00mm single row")
		(property "Reference" "J1"
			(at -0.19605 6.9596 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x03_Pin"
			(at 0.6096 7.1628 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "Interface_1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole roundrect
			(at 0 0 180)
			(size 3 2)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 2 "Net-(D1-K)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole roundrect
			(at 0 2.54 180)
			(size 3 2)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 9 "Net-(J1-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole roundrect
			(at 0 5.08 180)
			(size 3 2)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 12 "Net-(J1-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Eigene Footpriths:Diode 12.7mm"
		(layer "F.Cu")
		(at 72.5678 71.3994 90)
		(descr "Diode, A-405 series, Axial, Horizontal, pin pitch=12.7mm, length*diameter=5.2*2.7mm^2, http://www.diodes.com/_files/packages/A-405.pdf")
		(tags "Diode A-405 series Axial Horizontal pin pitch 12.7mm  length 5.2mm diameter 2.7mm")
		(property "Reference" "D4"
			(at 6.35 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "1N4007"
			(at 6.35 3 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1000V 1A General Purpose Rectifier Diode, DO-41"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*DO?41*")
		(sheetname "/")
		(sheetfile "Interface_1.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at 2.8584 -0.90725 90)
			(layer "F.SilkS")
		)
		(fp_text user "K"
			(at 0 -1.9 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 4 4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 8 "Net-(D4-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole roundrect
			(at 12.7 0 90)
			(size 4 4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 6 "Net-(D2-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_THT.3dshapes/D_A-405_P12.70mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Eigene Footpriths:Widerstand 15.24  mm"
		(layer "F.Cu")
		(at 121.9962 84.455 180)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=15.24mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 15.24mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R1"
			(at 4.4196 -0.0996 0)
			(layer "F.SilkS")
		)
		(property "Value" "120R"
			(at 7.6 3 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Interface_1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole roundrect
			(at 0 0 180)
			(size 4 4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 3 "Net-(C2-Pad1)")
			(pintype "passive")
		)
		(pad "2" thru_hole roundrect
			(at 15.24 0 180)
			(size 4 4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 17 "Net-(K2-Pad3)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P15.24mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Eigene Footpriths:Schalter Anschluss"
		(layer "F.Cu")
		(at 73.6854 40.9702)
		(descr "2 Pin")
		(tags "Klemme")
		(property "Reference" "SW1"
			(at 2.286 -8.6868 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Ein/Aus Schalter"
			(at 2.54 -3.81 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Schalter Anschluss"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Jumper* TestPoint*2Pads* TestPoint*Bridge*")
		(sheetname "/")
		(sheetfile "Interface_1.kicad_sch")
		(attr through_hole allow_missing_courtyard)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 3.5 4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.2857142857)
			(net 1 "Net-(KL1-Pin_1)")
			(pinfunction "A")
			(pintype "passive")
			(solder_mask_margin 0)
			(clearance 0)
		)
		(pad "2" thru_hole roundrect
			(at 5.08 0)
			(size 3.5 4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.3333333333)
			(net 15 "Net-(Q4-S)")
			(pinfunction "B")
			(pintype "passive")
			(clearance 0)
		)
		(embedded_fonts no)
	)
	(footprint "Eigene Footpriths:Diode 12.7mm"
		(layer "F.Cu")
		(at 85.8266 47.2694 -90)
		(descr "Diode, A-405 series, Axial, Horizontal, pin pitch=12.7mm, length*diameter=5.2*2.7mm^2, http://www.diodes.com/_files/packages/A-405.pdf")
		(tags "Diode A-405 series Axial Horizontal pin pitch 12.7mm  length 5.2mm diameter 2.7mm")
		(property "Reference" "D2"
			(at 6.35 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1N4001"
			(at 6.35 3 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "50V 1A General Purpose Rectifier Diode, DO-41"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*DO?41*")
		(sheetname "/")
		(sheetfile "Interface_1.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at 2.7748 -0.99635 90)
			(layer "F.SilkS")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 270)
			(size 4 4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 2 "Net-(D1-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole roundrect
			(at 12.7 0 270)
			(size 4 4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 6 "Net-(D2-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_THT.3dshapes/D_A-405_P12.70mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Eigene Footpriths:Transistor TO-92"
		(layer "F.Cu")
		(at 76.1746 78.105 180)
		(descr "TO-92 leads molded, narrow, drill 0.75mm (see NXP sot054_po.pdf)")
		(tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
		(property "Reference" "Q2"
			(at 1.143 0.9008 180)
			(layer "F.SilkS")
		)
		(property "Value" "BC337"
			(at 1.277034 2.769889 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://diotec.com/tl_files/diotec/files/pdf/datasheets/bc337.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "0.8A Ic, 45V Vce, NPN Transistor, TO-92"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "NPN"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=C 2=B 3=E"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO?92*")
		(sheetname "/")
		(sheetfile "Interface_1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole roundrect
			(at -1.27 0 180)
			(size 2.2 3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.3636363636)
			(net 8 "Net-(D4-K)")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "2" thru_hole roundrect
			(at 1.27 -1.27 180)
			(size 1.8 3)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.5)
			(net 11 "Net-(Q2-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "3" thru_hole roundrect
			(at 3.81 0 180)
			(size 2.2 3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.3636363636)
			(net 12 "Net-(J1-Pin_3)")
			(pinfunction "E")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Eigene Footpriths:Transistor TO-92"
		(layer "F.Cu")
		(at 66.6242 78.0542 180)
		(descr "TO-92 leads molded, narrow, drill 0.75mm (see NXP sot054_po.pdf)")
		(tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
		(property "Reference" "Q3"
			(at 1.22635 0.9516 180)
			(layer "F.SilkS")
		)
		(property "Value" "BC337"
			(at 1.277034 2.769889 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://diotec.com/tl_files/diotec/files/pdf/datasheets/bc337.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "0.8A Ic, 45V Vce, NPN Transistor, TO-92"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "NPN"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=C 2=B 3=E"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO?92*")
		(sheetname "/")
		(sheetfile "Interface_1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole roundrect
			(at -1.27 0 180)
			(size 2.2 3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.3636363636)
			(net 14 "Net-(Q3-C)")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "2" thru_hole roundrect
			(at 1.27 -1.27 180)
			(size 1.8 3)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.5)
			(net 13 "Net-(Q3-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "3" thru_hole roundrect
			(at 3.81 0 180)
			(size 2.2 3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.3636363636)
			(net 12 "Net-(J1-Pin_3)")
			(pinfunction "E")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Eigene Footpriths:Elko_3300µF_100V"
		(layer "F.Cu")
		(at 128.8542 70.1294 90)
		(descr "C, Radial series, Radial, pin pitch=7.50mm, diameter=16mm, height=31.5mm, Non-Polar Electrolytic Capacitor")
		(tags "C Radial series Radial pin pitch 7.50mm diameter 16mm height 31.5mm Non-Polar Electrolytic Capacitor")
		(property "Reference" "C2"
			(at 5.59 -3.89 90)
			(layer "F.SilkS")
		)
		(property "Value" "3300µF"
			(at 5.31 4.55 90)
			(layer "F.SilkS")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/")
		(sheetfile "Interface_1.kicad_sch")
		(attr through_hole)
		(fp_text user "C"
			(at 5.5 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 5 5)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.3)
			(net 3 "Net-(C2-Pad1)")
			(pintype "passive")
		)
		(pad "2" thru_hole roundrect
			(at 11 0 90)
			(size 5 5)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.2)
			(net 12 "Net-(J1-Pin_3)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D30.0mm_P10.00mm_SnapIn.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Eigene Footpriths:C-Keramic"
		(layer "F.Cu")
		(at 115.7878 47.5742)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm diameter 5mm width 2.5mm Capacitor")
		(property "Reference" "C3"
			(at 2.4892 0.014 0)
			(layer "F.SilkS")
		)
		(property "Value" "C_Small"
			(at 2.5 2.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "Interface_1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 2 3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 12 "Net-(J1-Pin_3)")
			(pintype "passive")
		)
		(pad "2" thru_hole roundrect
			(at 5 0)
			(size 2 3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 4 "Net-(KL5-Pin_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Eigene Footpriths:Schraubklemme"
		(layer "F.Cu")
		(at 99.04175 40.7026)
		(descr "2 Pin")
		(tags "Klemme")
		(property "Reference" "KL3"
			(at 2.5908 -3.3528 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Schraubklemme"
			(at 2.54 -3.81 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Klemme Rot"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "/")
		(sheetfile "Interface_1.kicad_sch")
		(attr through_hole allow_missing_courtyard)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 3.5 4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.2857142857)
			(net 6 "Net-(D2-A)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0)
			(clearance 0)
		)
		(pad "2" thru_hole roundrect
			(at 5.08 0)
			(size 3.5 4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.3333333333)
			(net 6 "Net-(D2-A)")
			(pinfunction "Pin_2")
			(pintype "passive")
			(clearance 0)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Same_Sky_TB006-508-02BE.igs"
			(offset
				(xyz -5.08 -4.1 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -90)
			)
		)
	)
	(footprint "Eigene Footpriths:Schraubklemme"
		(layer "F.Cu")
		(at 65.3542 40.9702 180)
		(descr "2 Pin")
		(tags "Klemme")
		(property "Reference" "KL1"
			(at 2.54 3.6576 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Schraubklemme"
			(at 2.54 -3.81 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Klemme Rot"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "/")
		(sheetfile "Interface_1.kicad_sch")
		(attr through_hole allow_missing_courtyard)
		(pad "1" thru_hole roundrect
			(at 0 0 180)
			(size 3.5 4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.2857142857)
			(net 1 "Net-(KL1-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0)
			(clearance 0)
		)
		(pad "2" thru_hole roundrect
			(at 5.08 0 180)
			(size 3.5 4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.3333333333)
			(net 12 "Net-(J1-Pin_3)")
			(pinfunction "Pin_2")
			(pintype "passive")
			(clearance 0)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Same_Sky_TB006-508-02BE.igs"
			(offset
				(xyz -5.08 -4.1 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -90)
			)
		)
	)
	(footprint "Eigene Footpriths:Widerstand 15.24  mm"
		(layer "F.Cu")
		(at 77.65495 57.4666 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=15.24mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 15.24mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R4"
			(at 7.62 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at 7.6 3 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Interface_1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole roundrect
			(at 0 0 270)
			(size 4 4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 15 "Net-(Q4-S)")
			(pintype "passive")
		)
		(pad "2" thru_hole roundrect
			(at 15.24 0 270)
			(size 4 4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 14 "Net-(Q3-C)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P15.24mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Eigene Footpriths:Transistor TO-92"
		(layer "F.Cu")
		(at 59.11295 73.4178)
		(descr "TO-92 leads molded, narrow, drill 0.75mm (see NXP sot054_po.pdf)")
		(tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
		(property "Reference" "Q1"
			(at 1.21205 0.928 0)
			(layer "F.SilkS")
		)
		(property "Value" "BC337"
			(at 1.277034 2.769889 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://diotec.com/tl_files/diotec/files/pdf/datasheets/bc337.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "0.8A Ic, 45V Vce, NPN Transistor, TO-92"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "NPN"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=C 2=B 3=E"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO?92*")
		(sheetname "/")
		(sheetfile "Interface_1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole roundrect
			(at -1.27 0)
			(size 2.2 3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.3636363636)
			(net 7 "Net-(D3-K)")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "2" thru_hole roundrect
			(at 1.27 -1.27)
			(size 1.8 3)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.5)
			(net 10 "Net-(Q1-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "3" thru_hole roundrect
			(at 3.81 0)
			(size 2.2 3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.3636363636)
			(net 12 "Net-(J1-Pin_3)")
			(pinfunction "E")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Eigene Footpriths:Trim_Potentiometer__Horizontal"
		(layer "F.Cu")
		(at 58.96055 60.667)
		(descr "Potentiometer, horizontal, Piher PT-10-H01, http://www.piher-nacesa.com/pdf/12-PT10v03.pdf")
		(tags "Potentiometer horizontal Piher PT-10-H01")
		(property "Reference" "RV2"
			(at 3.1496 -1.2992 0)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at 2.928 6.7116 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Potentiometer"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Potentiometer*")
		(sheetname "/")
		(sheetfile "Interface_1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 3.5 2.5)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.5)
			(net 3 "Net-(C2-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole roundrect
			(at 2.5 2.5)
			(size 3 2.5)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.48)
			(net 10 "Net-(Q1-B)")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0)
		)
		(pad "3" thru_hole roundrect
			(at 0 5)
			(size 3.5 2.5)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.5)
			(net 10 "Net-(Q1-B)")
			(pinfunction "3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Piher_PT-10-H01_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer.stp"
			(offset
				(xyz 0 12.5 -1.7)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -90)
			)
		)
	)
	(footprint "Eigene Footpriths:Widerstand 15.24  mm"
		(layer "F.Cu")
		(at 79.2226 84.7598 180)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=15.24mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 15.24mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R3"
			(at 4.318 0.1192 0)
			(layer "F.SilkS")
		)
		(property "Value" "220R"
			(at 7.6 3 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Interface_1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole roundrect
			(at 0 0 180)
			(size 4 4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 11 "Net-(Q2-B)")
			(pintype "passive")
		)
		(pad "2" thru_hole roundrect
			(at 15.24 0 180)
			(size 4 4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 9 "Net-(J1-Pin_2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P15.24mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Eigene Footpriths:Trim_Potentiometer__Horizontal"
		(layer "F.Cu")
		(at 58.86975 48.6674)
		(descr "Potentiometer, horizontal, Piher PT-10-H01, http://www.piher-nacesa.com/pdf/12-PT10v03.pdf")
		(tags "Potentiometer horizontal Piher PT-10-H01")
		(property "Reference" "RV1"
			(at 3.3528 -1.35 0)
			(layer "F.SilkS")
		)
		(property "Value" "50K"
			(at 2.9464 6.778 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Potentiometer"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Potentiometer*")
		(sheetname "/")
		(sheetfile "Interface_1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 3.5 2.5)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.5)
			(net 15 "Net-(Q4-S)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole roundrect
			(at 2.5 2.5)
			(size 3 2.5)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.48)
			(net 20 "Net-(ZD5-K)")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0)
		)
		(pad "3" thru_hole roundrect
			(at 0 5)
			(size 3.5 2.5)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.5)
			(net 12 "Net-(J1-Pin_3)")
			(pinfunction "3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Piher_PT-10-H01_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer.stp"
			(offset
				(xyz 0 12.5 -1.7)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -90)
			)
		)
	)
	(footprint "Eigene Footpriths:Diode 12.7mm"
		(layer "F.Cu")
		(at 85.52895 78.955 90)
		(descr "Diode, A-405 series, Axial, Horizontal, pin pitch=12.7mm, length*diameter=5.2*2.7mm^2, http://www.diodes.com/_files/packages/A-405.pdf")
		(tags "Diode A-405 series Axial Horizontal pin pitch 12.7mm  length 5.2mm diameter 2.7mm")
		(property "Reference" "D1"
			(at 6.35 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "1N4001"
			(at 6.35 3 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "50V 1A General Purpose Rectifier Diode, DO-41"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*DO?41*")
		(sheetname "/")
		(sheetfile "Interface_1.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at 2.882 -0.87075 90)
			(layer "F.SilkS")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 4 4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 2 "Net-(D1-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole roundrect
			(at 12.7 0 90)
			(size 4 4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 5 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_THT.3dshapes/D_A-405_P12.70mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Eigene Footpriths:Diode 12.7mm"
		(layer "F.Cu")
		(at 85.0646 84.4042)
		(descr "Diode, A-405 series, Axial, Horizontal, pin pitch=12.7mm, length*diameter=5.2*2.7mm^2, http://www.diodes.com/_files/packages/A-405.pdf")
		(tags "Diode A-405 series Axial Horizontal pin pitch 12.7mm  length 5.2mm diameter 2.7mm")
		(property "Reference" "D3"
			(at 6.35 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "1N4007"
			(at 6.35 3 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1000V 1A General Purpose Rectifier Diode, DO-41"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*DO?41*")
		(sheetname "/")
		(sheetfile "Interface_1.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at 2.7432 -0.9144 0)
			(layer "F.SilkS")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 4 4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 7 "Net-(D3-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole roundrect
			(at 12.7 0)
			(size 4 4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 5 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_THT.3dshapes/D_A-405_P12.70mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Eigene Footpriths:Relay_1 x Um_Print_SRD"
		(layer "F.Cu")
		(at 92.6084 54.229)
		(descr "relay Sanyou SRD series Form C http://www.sanyourelay.ca/public/products/pdf/SRD.pdf")
		(tags "relay Sanyu SRD form C")
		(property "Reference" "K1"
			(at 14.351 0.6604 0)
			(layer "F.SilkS")
		)
		(property "Value" "Relay_SRD"
			(at 8.4836 -9.144 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Relay SPDT, monostable, EN50005"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Relay?SPDT*")
		(sheetname "/")
		(sheetfile "Interface_1.kicad_sch")
		(attr through_hole)
		(fp_text user "Rel"
			(at 9.7028 -1.27 0)
			(layer "F.SilkS")
		)
		(fp_text user "1"
			(at 0 -2.3 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 4 3.5)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.4285714286)
			(net 4 "Net-(KL5-Pin_1)")
			(pintype "passive")
		)
		(pad "2" thru_hole roundrect
			(at 2 6 90)
			(size 4 4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.375)
			(net 2 "Net-(D1-K)")
			(pintype "passive")
		)
		(pad "3" thru_hole roundrect
			(at 14.2 6 90)
			(size 4 4)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.375)
			(net 2 "Net-(D1-K)")
			(pintype "passive")
		)
		(pad "4" thru_hole roundrect
			(at 14.2 -6 90)
			(size 4 4)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.375)
			(net 16 "unconnected-(K1-Pad4)")
			(pintype "passive+no_connect")
		)
		(pad "5" thru_hole roundrect
			(at 2 -6 90)
			(size 4 4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.375)
			(net 5 "Net-(D1-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Relay_THT.3dshapes/Relay_SPDT_SANYOU_SRD_Series_Form_C.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_circle
		(center 142.2822 92.9502)
		(end 143.8822 92.9502)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 142.2822 32.9502)
		(end 143.8822 32.9502)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 52.2822 32.9502)
		(end 53.8822 32.9502)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_rect
		(start 47.2822 27.9502)
		(end 147.2822 97.9502)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 52.2822 92.9502)
		(end 53.8822 92.9502)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_text " + Ext -\n12 VDC Out\n"
		(at 89.535 35.4838 0)
		(layer "F.SilkS")
	)
	(gr_text "- VCC +\n12 VDC\n"
		(at 62.0522 35.2806 0)
		(layer "F.SilkS")
	)
	(gr_text "Externe Module (Open Colector)"
		(at 100.457 34.7218 0)
		(layer "F.SilkS")
	)
	(gr_text "Hügli Präzisions-Mechanik"
		(at 53.5686 82.423 90)
		(layer "F.SilkS")
	)
	(gr_text "On/Off"
		(at 76.1238 35.5346 0)
		(layer "F.SilkS")
	)
	(gr_text "Interface_1"
		(at 73.6854 96.1898 0)
		(layer "F.SilkS")
	)
	(gr_text "-"
		(at 132.1054 60.833 0)
		(layer "F.SilkS")
	)
	(gr_text "+"
		(at 131.9022 72.0598 0)
		(layer "F.SilkS")
	)
	(dimension
		(type orthogonal)
		(layer "F.SilkS")
		(pts
			(xy 147.2822 27.9502) (xy 47.2822 27.9502)
		)
		(height -5.522)
		(orientation 0)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 0)
			(precision 4)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "100"
			(at 97.2822 21.3282 0)
			(layer "F.SilkS")
		)
	)
	(dimension
		(type orthogonal)
		(layer "F.SilkS")
		(pts
			(xy 147.2822 27.9502) (xy 147.2822 97.9502)
		)
		(height 6.5148)
		(orientation 1)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 0)
			(precision 4)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "70"
			(at 152.697 62.9502 90)
			(layer "F.SilkS")
		)
	)
	(embedded_fonts no)
	(embedded_files
		(file
			(name "Blatt_A4.kicad_wks")
			(type worksheet)
		)
	)
)
