Format: Log Type - Time(microsec) - Message - Optional Info
Log Type: B - Since Boot(Power On Reset),  D - Delta,  S - Statistic
S - QC_IMAGE_VERSION_STRING=AVM_BOOT.BF.3.1.1
S - IMAGE_VARIANT_STRING=DAABANAZA
S - OEM_IMAGE_VERSION_STRING=1214
S - Boot Config, 0x00000025
S - Reset status Config, 0x00000000
S - Core 0 Frequency, 0 MHz
B -       262 - PBL, Start
B -      1344 - bootable_media_detect_entry, Start
B -      2616 - bootable_media_detect_success, Start
B -      2631 - elf_loader_entry, Start
B -      4062 - auth_hash_seg_entry, Start
B -      6028 - auth_hash_seg_exit, Start
B -    106516 - elf_segs_hash_verify_entry, Start
B -    300720 - PBL, End
B -         0 - SBL1, Start
B -    401269 - pm_device_init, Start
D -         9 - pm_device_init, Delta
B -    402414 - boot_flash_init, Start
D -     80233 - boot_flash_init, Delta
B -    486897 - boot_config_data_table_init, Start
D -     14109 - boot_config_data_table_init, Delta - (419 Bytes)
B -    503477 - clock_init, Start
D -      7431 - clock_init, Delta
B -    513885 - CDT version:2,Platform ID:8,Major 
B -    515190 - sbl1_ddr_set_params, Start
B -    519899 - cpr_init, Start
D -         4 - cpr_init, Delta
B -    524978 - Pre_DDR_clock_init, Start
D -         5 - Pre_DDR_clock_init, Delta
D -     13025 - sbl1_ddr_set_params, Delta
B -    538370 - pm_driver_init, Start
D -         4 - pm_driver_init, Delta
B -    573624 - sbl1_wait_for_ddr_training, Start
D -        31 - sbl1_wait_for_ddr_training, Delta
B -    589714 - Image Verify, Start 0:QSEE
D -    284308 - QSEE Image Loaded, Delta - (293400 Bytes)
B -    874337 - Image Verify, Start 0:QSEE_B
D -    287081 - QSEE Image Loaded, Delta - (293400 Bytes)
B -   1161777 - Selected TZ0: 15788 (0:QSEE)
B -   1164836 - Image Load, Start
D -    286996 - QSEE Image Loaded, Delta - (293400 Bytes)
B -   1452144 - Image Load, Start
D -      2024 - SEC Image Loaded, Delta - (2048 Bytes)
B -   1465689 - Image Verify, Start 0:APPSBL
D -    143109 - APPSBL Image Loaded, Delta - (137884 Bytes)
B -   1609120 - Image Verify, Start 0:APPSBL_B
D -    146433 - APPSBL Image Loaded, Delta - (137884 Bytes)
B -   1755896 - Selected EVA0: 11090 (0:APPSBL)
B -   1759743 - Image Load, Start
D -    145428 - APPSBL Image Loaded, Delta - (137884 Bytes)
B -   1905488 - QSEE Execution, Start
D -        60 - QSEE Execution, Delta
B -   1911668 - SBL1, End
D -   1913799 - SBL1, Delta
S - Flash Throughput, 2129 KB/s  (1296319 Bytes,  608877 us)
S - DDR Frequency, 672 MHz
NAND corrected 1 @ page: 8D5
NAND corrected 1 @ page: 8D5
NAND corrected 1 @ page: 8D5
NAND corrected 1 @ page: 11CB
NAND corrected 1 @ page: 11CB
NAND corrected 1 @ page: 11CB

(AVM) EVA Revision: 1.11090

(C) Copyright 2018 AVM Date: Jul  8 2020 Time: 12:57:50 (0) 3 0x0-0x46409

[NAND:] 128MB MACRONIX 2048 Pagesize 128k Blocksize 1024 Blocks HW
[SYSTEM:] CortexA9 

Eva_AVM >NAND corrected 1 @ page: 1BA2
…………………………………………………………….[    0.000000][0] Booting Linux on physical CPU 0x0
[    0.000000][0] Linux version 4.4.271 (kbuild-team@core.avm.de) (gcc version 5.5.0 (Buildroot 2020.02.1-g758ac3ed) ) #1 SMP PREEMPT 2024-01-11
[    0.000000][0] CPU: ARMv7 Processor [410fc075] revision 5 (ARMv7), cr=10c5387d
[    0.000000][0] CPU: PIPT / VIPT nonaliasing data cache, VIPT aliasing instruction cache
[    0.000000][0] Machine model: AVM FRITZ!Powerline 1260v2
[    0.000000][0] Memory policy: Data cache writealloc
[    0.000000][0] [fw-info] Version 07.58 buildnr=113256 buildtype=1
[    0.000000][0] [module-mem] Use 0x81000000-0x81012fff (mapped at c1000000-c1012fff) for 1 modules
[    0.000000][0] [module-mem] Using whitelist, set default strict_mode=1
[    0.000000][0] PERCPU: Embedded 11 pages/cpu @cfdb7000 s15756 r8192 d21108 u45056
[    0.000000][0] Built 1 zonelists in Zone order, mobility grouping on.  Total pages: 60928
[    0.000000][0] Kernel command line:  clk_ignore_unused audit=1 slub_debug=FL 
[    0.000000][0] audit: enabled (after initialization)
[    0.000000][0] setup_slub_debug: slub_debug = DEBUG_FREE STORE_USER_LITE
[    0.000000][0] PID hash table entries: 1024 (order: 0, 4096 bytes)
[    0.000000][0] Dentry cache hash table entries: 32768 (order: 5, 131072 bytes)
[    0.000000][0] Inode-cache hash table entries: 16384 (order: 4, 65536 bytes)
[    0.000000][0] Memory: 229488K/245760K available (6287K kernel code, 1400K rwdata, 2112K rodata, 240K init, 2703K bss, 16272K reserved, 0K cma-reserved, 0K highmem)
[    0.000000][0] Virtual kernel memory layout:
[    0.000000][0]     vector  : 0xffff0000 - 0xffff1000   (   4 kB)
[    0.000000][0]     fixmap  : 0xffc00000 - 0xfff00000   (3072 kB)
[    0.000000][0]     vmalloc : 0xd0800000 - 0xff800000   ( 752 MB)
[    0.000000][0]     lowmem  : 0xc0000000 - 0xd0000000   ( 256 MB)
[    0.000000][0]     pkmap   : 0xbfe00000 - 0xc0000000   (   2 MB)
[    0.000000][0]     modules : 0xbf000000 - 0xbfe00000   (  14 MB)
[    0.000000][0]       .text : 0xc0208000 - 0xc0a3bf8c   (8400 kB)
[    0.000000][0]       .init : 0xc0a3c000 - 0xc0a78000   ( 240 kB)
[    0.000000][0]       .data : 0xc0a78000 - 0xc0bd6000   (1400 kB)
[    0.000000][0]        .bss : 0xc0bd8000 - 0xc0e7bcc4   (2704 kB)
[    0.000000][0] SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=4, Nodes=1
[    0.000000][0] Preemptible hierarchical RCU implementation.
[    0.000000][0] 	Build-time adjustment of leaf fanout to 32.
[    0.000000][0] NR_IRQS:16 nr_irqs:16 16
[    0.000000][0] Architected cp15 timer(s) running at 48.00MHz (virt).
[    0.000000][0] clocksource: arch_sys_counter: mask: 0xffffffffffffff max_cycles: 0xb11fd3bfb, max_idle_ns: 440795203732 ns
[    0.000000][0] sched_clock: 56 bits at 48MHz, resolution 20ns, wraps every 4398046511096ns
[    0.000000][0] Switching to timer-based delay loop, resolution 20ns
[    0.000316][0] Calibrating delay loop (skipped), value calculated using timer frequency.. 96.00 BogoMIPS (lpj=192000)
[    0.000357][0] pid_max: default: 32768 minimum: 301
[    0.000510][0] Security Framework initialized
[    0.000553][0] AppArmor: AppArmor initialized
[    0.000650][0] Mount-cache hash table entries: 1024 (order: 0, 4096 bytes)
[    0.000679][0] Mountpoint-cache hash table entries: 1024 (order: 0, 4096 bytes)
[    0.001464][0] CPU: Testing write buffer coherency: ok
[    0.001970][0] CPU0: thread -1, cpu 0, socket 0, mpidr 80000000
[    0.002076][0] Setting up static identity map for 0x802082c0 - 0x80208318
[    0.040527][1] CPU1: thread -1, cpu 1, socket 0, mpidr 80000001
[    0.052578][2] CPU2: thread -1, cpu 2, socket 0, mpidr 80000002
[    0.064656][3] CPU3: thread -1, cpu 3, socket 0, mpidr 80000003
[    0.064768][0] Brought up 4 CPUs
[    0.064827][0] SMP: Total of 4 processors activated (384.00 BogoMIPS).
[    0.064850][0] CPU: All CPU(s) started in SVC mode.
[    0.066060][0] devtmpfs: initialized
[    0.077615][0] VFP support v0.3: implementor 41 architecture 2 part 30 variant 7 rev 5
[    0.077836][0] [rte_ipi] Available IPIs 6
[    0.078262][0] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 7645041785100000 ns
[    0.078315][0] futex hash table entries: 1024 (order: 4, 65536 bytes)
[    0.078863][0] pinctrl core: initialized pinctrl subsystem
[    0.080864][0] NET: Registered protocol family 16
[    0.082499][0] DMA: preallocated 2048 KiB pool for atomic coherent allocations
[    0.083061][0] console [avm0] enabled
[    0.092521][0] cpuidle: using governor ladder
[    0.104540][0] cpuidle: using governor menu
[    0.104583][0] Creating Config Table
[    0.108880][0] [qcom:qtimer_probe] WARNING avm,clk-rate not set in dt, using built in default
[    0.112805][0] [qcom_wdt] wdt_ipq40xx_probe …
[    0.121328][0] hw-breakpoint: debug architecture 0x5 unsupported.
[    0.124181][0] CPU: IPQ8064, SoC Version: 4294967274.4294967274
[    0.124355][0] <CORE> glink_init: IPC Logging Disabled
[    0.125063][0] avm_alloc_page_extension node_extension_table[0] entries=65536 (size=262144)  alloced
[    0.125249][0] [fdt_get_reserved_mem_resource] mem_count = 6; search name = „avm_reboot_string“
[    0.125286][0] Reboot Status is: Power-On 
[    0.125973][0] IPC logging disabled
[    0.126002][0] IPC logging disabled
[    0.126023][0] IPC logging disabled
[    0.126044][0] IPC logging disabled
[    0.126065][0] IPC logging disabled
[    0.126535][0] sps:sps is ready.
[    0.127805][0] console [pstore0] enabled
[    0.128117][0] pstore: Registered ramoops as persistent store backend
[    0.128152][0] ramoops: attached 0x100000@0x86000000, ecc: 0/0
[    0.151587][0] SCSI subsystem initialized
[    0.152128][0] usbcore: registered new interface driver usbfs
[    0.152248][0] usbcore: registered new interface driver hub
[    0.152341][0] usbcore: registered new device driver usb
[    0.154410][0] Advanced Linux Sound Architecture Driver Initialized.
[    0.155413][0] AVM PA for Linux version 4.4.271 (kbuild-team@core.avm.de) (gcc version 5.5.0 (Buildroot 2020.02.1-g758ac3ed) ) #1 SMP PREEMPT 2024-01-11
[    0.155413][0]  (early init)
[    0.155916][0] NET: Registered protocol family 8
[    0.155951][0] NET: Registered protocol family 20
[    0.156213][0] TZ-pin nr 15 reprioritized to 60
[    0.156252][0] TZ-pin nr 36 reprioritized to 60
[    0.156354][0] TZ-pin nr 206 reprioritized to 60
[    0.156383][0] TZ-pin nr 213 reprioritized to 60
[    0.156414][0] TZ-pin nr 225 reprioritized to 60
[    0.156440][0] TZ-pin nr 226 reprioritized to 60
[    0.156466][0] TZ-pin nr 227 reprioritized to 60
[    0.156493][0] TZ-pin nr 228 reprioritized to 60
[    0.156520][0] TZ-pin nr 229 reprioritized to 60
[    0.156546][0] TZ-pin nr 230 reprioritized to 60
[    0.156574][0] TZ-pin nr 231 reprioritized to 60
[    0.156600][0] TZ-pin nr 232 reprioritized to 60
[    0.156626][0] TZ-pin nr 233 reprioritized to 60
[    0.156667][0] TZ-pin nr 269 reprioritized to 60
[    0.157086][2] [AVM_FIQ] FIQ disabled on CPU2 to install new vector!
[    0.157093][3] [AVM_FIQ] FIQ disabled on CPU3 to install new vector!
[    0.157101][1] [AVM_FIQ] FIQ disabled on CPU1 to install new vector!
[    0.157146][0] [AVM_FIQ] FIQ disabled on CPU0 to install new vector!
[    0.157175][0] [AVM_FIQ] Vector installed!
[    0.157199][0] [avm_scm] Set FIQ handler address
[    0.157230][3] [AVM_FIQ] FIQ enabled again on CPU3!
[    0.157235][1] [AVM_FIQ] FIQ enabled again on CPU1!
[    0.157241][2] [AVM_FIQ] FIQ enabled again on CPU2!
[    0.157289][0] [AVM_FIQ] FIQ enabled again on CPU0!
[    0.157332][0] [AVM_FIQ] (Version 1.0)(TZ 15788)
[    0.157478][0] clocksource: Switched to clocksource arch_sys_counter
[    0.158236][0] AppArmor: AppArmor Filesystem Enabled
[    0.160790][0] NET: Registered protocol family 2
[    0.173735][0] TCP established hash table entries: 2048 (order: 1, 8192 bytes)
[    0.173807][0] TCP bind hash table entries: 2048 (order: 2, 16384 bytes)
[    0.173873][0] TCP: Hash tables configured (established 2048 bind 2048)
[    0.173986][0] UDP hash table entries: 256 (order: 1, 8192 bytes)
[    0.174039][0] UDP-Lite hash table entries: 256 (order: 1, 8192 bytes)
[    0.174378][0] NET: Registered protocol family 1
[    0.174913][0] hw perfevents: enabled with armv7_cortex_a7 PMU driver, 5 counters available
[    0.177388][0] audit: initializing netlink subsys (enabled)
[    0.177552][0] audit: type=2000 audit(0.175:1): initialized
[    0.205164][0] squashfs: version 4.0 (2009/01/31) Phillip Lougher
[    0.205900][0] ANTFS Module: Version 2.53
[    0.206206][0] jffs2: version 2.2 (NAND) (SUMMARY) (ZLIB) (LZO) (LZMA) (RTIME) (CMODE_PRIORITY) (c) 2001-2006 Red Hat, Inc.
[    0.209078][0] fuse init (API version 7.23)
[    0.216729][0] Key type asymmetric registered
[    0.216778][0] Asymmetric key parser ‚x509‘ registered
[    0.216871][0] io scheduler noop registered
[    0.216907][0] io scheduler deadline registered (default)
[    0.224915][0] glink_loopback_server_init: IPC Logging disabled
[    0.226592][0] NET: Registered protocol family 27
[    0.226630][0] IPC_RTR: ipc_router_create_log_ctx: IPC Logging disabled
[    0.226671][0] qmi_log_init: IPC Logging disabled
[    0.226696][0] qmi_log_init: IPC Logging disabled
[    0.227023][0] tcsr 194b000.tcsr: setting usb hs phy mode select = e700e7
[    0.227141][0] tcsr 1953000.ess_tcsr: setting ess interface select = 1
[    0.227244][0] tcsr 1949000.tcsr: setting wifi_glb_cfg = 41000000
[    0.227330][0] tcsr 1957000.tcsr: setting wifi_noc_memtype_m0_m2 = 2222222
[    0.227599][0] TZ Log : Will warn on Access Violation, as paniconaccessviolation is not set
[    0.228768][0] msm_serial 78af000.serial: msm_serial: detected port #0
[    0.228913][0] msm_dectuart_probe: set dectuart_port to ttyMSM0
[    0.228984][0] msm_serial 78af000.serial: uartclk = 1843200
[    0.229057][0] 78af000.serial: ttyMSM0 at MMIO 0x78af000 (irq = 24, base_baud = 115200) is a MSM
[    0.229107][0] msm_serial: console setup on port #0
[    1.101750][0] console [ttyMSM0] enabled
[    1.106942][0] msm_serial: driver initialized
[    1.110845][0] msm_serial_hsl_init: driver initialized
[    1.115053][0] [avm_power]avm_power_pm_qos_init
[    1.120150][0] [loadcontrol] set auto - scale=1
[    1.124232] [avm] configured: watchdog event debug 
[    1.133838][0] Register push button event to receive the set_factory_kernel event
[    1.145854][0] AVM Simple Profiling enabled Version 3.0
[    1.145916][0] [simple-profiling]:4 performance counters implemented
[    1.149967][0] [simple-profiling]all cpus:performance-mode: round-robin
[    1.156570][0] [simple-profiling]all cpus:performance-mode: round-robin
[    1.162890][0] [simple-profiling]all cpus:performance-mode: round-robin
[    1.169499][0] [simple-profiling]all cpus:performance-mode: round-robin
[    1.176157][0] AVM_WATCHDOG: Watchdog Driver for AR7 Hardware (Version 1.0)
[    1.182870][0] [qcom_wdt] ar7wdt_hw_init…
[    1.189726][0] [avm_request_fiq_on] Virtual IRQ numbers are not supported. Use HWIRQ (35) for requested IRQ (25)
[    1.193819][0] [qcom_wdt] [register_wdt_bark_irq] watchdog as fastirq(35) on all cpus registered with its default prio
[    1.204188][0] [avm_request_fiq_on] Forcing HW-IRQ 36 instead
[    1.214718][0] [qcom_wdt] [register_wdt_bark_irq] watchdog as fastirq(36) on all cpus registered with highest prio
[    1.220506][0] [avm_request_fiq_on] Forcing HW-IRQ 213 instead
[    1.230779][0] [qcom_wdt] [register_secure_wdt_bark_irq] secure watchdog as fastirq(213) on all cpus registered with highest prio
[    1.245570][0] [qcom_wdt] [ar7wdt_hw_init] Wdt bark time: 320000, bite time: 640000
[    1.248277][0] [qcom_wdt] [ar7wdt_hw_init] Secure watchdog: bark: 20s, bite time: 40s
[    1.256845][0] avm_net_trace: Up and running.
[    1.267197][0] loop: module loaded
[    1.269233][0] zram: Added device: zram0
[    1.273171][0] QPIC controller hw version Major:1, Minor:4
[    1.275926][0] nand: device found, Manufacturer ID: 0xc2, Chip ID: 0xf1
[    1.280758][0] nand: ONFI 10-Compliant Macronix MX30LF1G18AC
[    1.287257][0] nand: 128 MiB, SLC, erase size: 128 KiB, page size: 2048, OOB size: 64
[    1.293192][0] [TFFS3_Register_Panic_CB] registering panic callback for mtd qcom_nand.0
[    1.300962][0] 5 ofpart partitions found on MTD device qcom_nand.0
[    1.308700][0] Creating 5 MTD partitions on „qcom_nand.0“:
[    1.314951][0] 0x000000b00000-0x000000f00000 : „kernel“
[    1.326381][0] 0x000000000000-0x0000002c0000 : „urlader“
[    1.331093][0] 0x0000002c0000-0x000000b00000 : „nand-tffs“
[    1.341133][0] 0x000000f00000-0x000001300000 : „reserved-kernel“
[    1.347033][0] 0x000001300000-0x000008000000 : „ubi“
[    1.458290][0] libphy: Fixed MDIO Bus: probed
[    1.459052][0] qca-mdio 90000.mdio: Skipping early reset
[    1.461892][0] libphy: qca_mdio: probed
[    1.469993][0] qca-mdio 90000.mdio: qca-mdio driver was registered
[    1.470720][0] tun: Universal TUN/TAP device driver, 1.6
[    1.476877][0] tun: (C) 1999-2004 Max Krasnyansky <maxk@qualcomm.com>
[    1.988350][0] i2c /dev entries driver
[    1.990565][0] sdhci: Secure Digital Host Controller Interface driver
[    1.991014][0] sdhci: Copyright(c) Pierre Ossman
[    1.997582][0] sdhci-pltfm: SDHCI platform and OF driver helper
[    2.005007][0] AVM PA 2.138.1.16-release_move21-move21 for Linux Linux version 4.4.271 (kbuild-team@core.avm.de) (gcc version 5.5.0 (Buildroot 2020.02.1-g758ac3ed) ) #1 SMP PREEMPT 2024-01-11
[    2.005007][0]  (late init)
[    2.008630][0] gre: GRE over IPv4 demultiplexor driver
[    2.027760][0] Initializing XFRM netlink socket
[    2.032912][0] IPsec XFRM device driver
[    2.039322][0] NET: Registered protocol family 10
[    2.047514][0] sit: IPv6 over IPv4 tunneling driver
[    2.048564][0] NET: Registered protocol family 17
[    2.051625][0] Bridge broadcast ratelimiter registered
[    2.056159][0] bridge: automatic filtering via arp/ip/ip6tables has been deprecated. Update your scripts to load br_netfilter if you need this.
[    2.061238][0] Bridge firewalling registered
[    2.073935][0] KOAM is loaded successfully.
[    2.078451][0] l2tp_core: L2TP core driver, V2.0
[    2.082329][0] l2tp_ip: L2TP IP encapsulation support (L2TPv3)
[    2.087467][0] l2tp_netlink: L2TP netlink interface
[    2.092895][0] l2tp_eth: L2TP ethernet pseudowire support (L2TPv3)
[    2.097627][0] l2tp_ip6: L2TP IP encapsulation support for IPv6 (L2TPv3)
[    2.104130][0] 8021q: 802.1Q VLAN Support v1.8
[    2.110866][0] Registering SWP/SWPB emulation handler
[    2.115032][0] [fdt_get_reserved_mem_resource] mem_count = 6; search name = „avm_sbl_boot_string“
[    2.120095][0] SBL Boot Info Version 1214 Boot TZ 0 Boot Eva 0
[    2.128933] TZ0 Version 15788 
[    2.134658][0] TZ1 Version 15788
[    2.137758][0] EVA0 Version 11090
[    2.141056][0] EVA1 Version 11090
[    2.144510][0] [rte_ipi] Requested ipi RTE monitor (nr=9, prio=00, flags=0x00800001)
[    2.147794][0] [rte_ipi] Requested ipi RTE linux (nr=10, prio=80, flags=0x00800000)
[    2.155478][0] [fdt_get_reserved_mem_resource] mem_count = 6; search name = „avm_sbl_boot_string“
[    2.165831][1] Could not find Env ‚kernel_args‘ in the device tree
[    2.171935][1] [TFFS3_Init] Called.
[    2.177925][1] [TFFS3_CACHE_Configure] Setting up caching for backend nand
[    2.181254][1] [TFFS3-CACHE] Caching module for TFFS 3.x
[    2.188234][1] [TFFS3-NAND] NAND storage backend for TFFS 3.x on mtd2
[    2.555979][0] random: nonblocking pool is initialized
[    5.156563][1] [TFFS3-NAND] Initialisation successful, 66/66/66 NAND blocks active, fill rate 6%
[    5.156644][1] [TFFS_Cache] Allocate segement buffer cache (size=2024)
[    5.164540][1] tffs/panic: have_new_logentry: Error reading crashenv: -2
[    5.170826][1] tffs/panic: have_new_logentry: Error reading crashenv: -2
[    5.177875][1] TFFS: tiny flash file system driver. GPL (c) AVM Berlin (Version 3.0)
[    5.184417][1] Adam2 environment variables API installed.
[    5.193161][1] ubi0: attaching mtd4
[    5.773376][1] ubi0: scanning is finished
[    5.784232][1] ubi0: attached mtd4 (name „ubi“, size 109 MiB)
[    5.784290][1] ubi0: PEB size: 131072 bytes (128 KiB), LEB size: 126976 bytes
[    5.789030][1] ubi0: min./max. I/O unit sizes: 2048/2048, sub-page size 2048
[    5.796133][1] ubi0: VID header offset: 2048 (aligned 2048), data offset: 4096
[    5.803241][1] ubi0: good PEBs: 872, bad PEBs: 0, corrupted PEBs: 0
[    5.810310][1] ubi0: user volume: 3, internal volumes: 1, max. volumes count: 128
[    5.816440][1] ubi0: max/mean erase counter: 2/1, WL threshold: 4096, image sequence number: 2726414984
[    5.824078][1] ubi0: available PEBs: 0, total reserved PEBs: 872, PEBs reserved for bad PEB handling: 20
[    5.833316][0] ubi0: background thread „ubi_bgt0d“ started, PID 96
[    5.844818][1] mtd: device 5 (filesystem) set to be root filesystem
[    5.852611][1] hctosys: unable to open rtc device (rtc0)
[    5.860579][1] clk: Not disabling unused clocks
[    5.860689][1] ALSA device list:
[    5.864984][1]   No soundcards found.
[    5.872269][1] VFS: Mounted root (squashfs filesystem) readonly on device 31:5.
[    5.875700][1] devtmpfs: mounted
[    5.880356][1] Freeing unused kernel memory: 240K

starting pid 105, tty ‚‘: ‚/etc/boot.d/1‘
[    6.664256][0] hui: loading out-of-tree module taints kernel.
[    6.670887][0] [hui] Initialize hardware user interface
[    6.673642][0] [avm_connect][state_machine_init] starting event worker thread
mknod: /dev/led: File exists
[    6.727872][2] TFFS Name Table N
[Supervisor] Info: start svlogd.service
[Supervisor] Info: svlogd.service notified: ready
[Supervisor] Info: start disable_ipv6.service
[Supervisor] Info: start tffs.service
[Supervisor] Info: disable_ipv6.service exit success

Please press Enter to activate this console. [Supervisor] Info: tffs.service exit success
[Supervisor] Info: start rekey.service
firmwarecfg config_rekey: done
[Supervisor] Info: rekey.service exit success
[Supervisor] Info: start environment.service
[    9.094502][0] [0]system-load  82% loadavg 0.16 0.3 0.1 - softirqs:5.31% (vchan_complete 63%) pgstat: sum=56198 free=51388 slab=1717 alloc=1443/s fault=1061/s (sleep 1)
[    9.168446][1] [1]system-load  79% loadavg 0.16 0.3 0.1 - task runtime:1% max:rc.conf 1%  pgstat: sum=55693 free=51443 slab=1717 alloc=1600/s fault=1191/s (sleep 0)
[Supervisor] Info: environment.service exit success
[Supervisor] Info: start watchdog.service
[    9.780774][0] AVM_WATCHDOG: System Init Ueberwachung 120 Sekunden
[Supervisor] Info: watchdog.service exit success
[Supervisor] Info: start udev.service
[Supervisor] Info: start udevadm.service
[    9.996810][2] udevd[314]: starting version 3.2.5
[   10.022065][2] udevd[314]: specified group ‚tty‘ unknown
[   10.022501][2] udevd[314]: specified group ‚dialout‘ unknown
[   10.026808][2] udevd[314]: specified group ‚kmem‘ unknown
[   10.032450][2] udevd[314]: specified group ‚input‘ unknown
[   10.038019][2] udevd[314]: specified group ‚video‘ unknown
[   10.043267][2] udevd[314]: specified group ‚audio‘ unknown
[   10.048809][2] udevd[314]: specified group ‚lp‘ unknown
[   10.054184][2] udevd[314]: specified group ‚disk‘ unknown
[   10.059175][2] udevd[314]: specified group ‚cdrom‘ unknown
[   10.064863][2] udevd[314]: specified group ‚tape‘ unknown
[   10.073157][2] udevd[314]: starting eudev-3.2.5
[   10.293799][2] [2]system-load  74% loadavg 0.39 0.8 0.3 - task runtime:19% max:udevd 9%  pgstat: sum=55532 free=50246 slab=2011 alloc=2147/s fault=1706/s (sleep 1)
[   10.706272][0] ssdk_switch_device_num_init[1340]:INFO:ess-switch dts node number: 1
[   10.706367][0] ssdk_dt_get_switch_node[1143]:INFO:ess-switch DT exist!
[   10.712815][0] ssdk_dt_parse_access_mode[1029]:INFO:switch_access_mode: local bus
[   10.719389][0] ssdk_dt_parse_access_mode[1042]:INFO:switchreg_base_addr: 0xc000000
[   10.726933][0] ssdk_dt_parse_access_mode[1043]:INFO:switchreg_size: 0x80000
[   10.734400][0] ssdk_dt_parse_mac_mode[361]:INFO:mac mode = 0x1 (PORT_WRAPPER_PSGMII_RGMII5)
[   10.741255][0] ssdk_dt_parse_mac_mode[367]:INFO:mac mode1 doesn’t exit!
[   10.749587][0] ssdk_dt_parse_mac_mode[377]:INFO:mac mode2 doesn’t exit!
[   10.756184][0] ssdk_dt_parse_phy_info[645]:INFO:qcom,port_phyinfo DT doesn’t exist!
[   10.762794][0] ssdk_dt_parse_mdio[806]:INFO:mdio DT exist!
[   10.770475][0] ssdk_dt_parse_led[1116]:INFO:current dts led_source_num is 0
[   10.775993][0] ssdk_dt_parse_psgmii[994]:INFO:ess-psgmii DT exist!
[   10.782849][0] ssdk_plat_init start
[   10.789246][0] ssdk_plat_init[1624]:INFO:Enable ess clk
[   10.975110][0] malibu_phy_api_ops_init[2869]:INFO:qca probe malibu phy driver succeeded!
[   10.976034][0] regi_init[4080]:INFO:Initializing DESS!!
[   11.117520][1] avm_power: [avm_power_temperature] No cpu sensor registered
[   11.824726][0] ssdk_switch_register[1965]:INFO:Chip version 0x1401
[   11.824820][0] ssdk_switch_register[1991]:INFO:polling is selected
[   11.829857][0] regi_init[4090]:INFO:Initializing DESS Done!!
[   11.837289][3] [3]system-load  71% loadavg 0.39 0.8 0.3 - task runtime:23% max:udevd 22%  pgstat: sum=55695 free=50065 slab=2051 alloc=1170/s fault=915/s (sleep 3)
[   11.855740][0] regi_init[4162]:INFO:qca-ssdk module init succeeded!
[   11.881239][0] [module-mem] give 0x11000 bytes at c1001000 to module ‚essedma‘ (0x1000 bytes left)
[   11.883462][0] Using 2 netdevs
[   11.890189][0] EDMA  Dev eth0 (0) —> phy mdio 3
[   11.892162][0] EDMA  Dev plc (1) —> phy mdio 24
[   11.897200][0] [avm_request_fiq_on] Virtual IRQ numbers are not supported. Use HWIRQ (272) for requested IRQ (77)
[Supervisor] Info: udevadm.service exit success
[Supervisor] Info: start cortexa9.service
SBL ACK done
[TZ-Update]
[tz-update] bound mibib block at page 524288.
[tz-update] 2 trustzones found. update index 0 first.
[tz-update] tz0 already up to date. version: 15788
[tz-update] tz1 already up to date. version: 15788
… tz not updated
[Supervisor] Info: cortexa9.service exit success
[Supervisor] Info: start capi-config.service
[Supervisor] Info: start modules-load.service
[Supervisor] Info: start piglet.service
[Supervisor] Info: capi-config.service exit success
[Supervisor] Info: piglet.service exit error
[Supervisor] Info: start capi.service
[Supervisor] Info: capi.service exit success
[   12.234231][0] cprocfs: loaded
[   12.236113][0] kspeedtest: kspeedtest_init: second timer started 
[   12.236269][0] kspeedtest: Starting default task on discard port 9
[   12.242497][0] kspeedtest: listening on port 9
[   12.248483][0] kspeedtest: kspeedtest_init done
[   12.284706][0] cchardevice: loaded
[   12.380763][0] krextdmod: module license ‚unspecified‘ taints kernel.
[   12.380827][0] Disabling lock debugging due to kernel taint
[   12.421710][0] krextd[0]: Initialisation of debughandles …
[   12.421773][0] krextd[0]: Initialisation of debughandles [OK]
[   12.426514][0] krextd[0]: Initialisation of cmemstack …
[   12.432132][0] krextd[0]: Initialisation of cmemstack [OK]
[   12.437514][0] krextd[0]: Initialisation of procfs …
[   12.442970][0] krextd[0]: Initialisation of procfs [OK]
[   12.448020][0] krextd[0]: Initialisation of kmod_debugctl …
[   12.453149][0] krextd[0]: Initialisation of kmod_debugctl [OK]
[   12.459051][0] krextd[0]: Initialisation of cenv …
[   12.464765][0] krextd[0]: Initialisation of cenv [OK]
[   12.469917][0] krextd[0]: Initialisation of ctimer …
[   12.475268][0] krextd[0]: Initialisation of ctimer [OK]
[   12.479912][0] krextd[0]: Initialisation of kmodcmddev …
[   12.485023][0] krextd[0]: Initialisation of kmodcmddev [OK]
[   12.490576][0] krextd[0]: Initialisation of packettrace …
[   12.496113][0] cchardevice: device_create(kdsldptrace%d): 240,0
[   12.501894][0] cchardevice: device_create(kdsldptrace%d): 240,1
[   12.507883][0] krextd[0]: Initialisation of packettrace [OK]
[   12.513403][0] krextd[0]: Initialisation of nqos …
[   12.519419][0] cchardevice: device_create(knqos): 239,0
[   12.526152][0] cchardevice: device_create(avmtrackd): 238,0
[   12.529635][0] cchardevice: device_create(avmtrackdquery): 237,0
[   12.535220][0] krextd[0]: Initialisation of nqos [OK]
[   12.541027][0] krextd[0]: Initialisation of bridgeflt …
[   12.546071][0] cchardevice: device_create(bridgeflt): 236,0
[   12.551686][0] krextd[0]: Initialisation of bridgeflt [OK]
[   12.556747][0] krextd[0]: Initialisation of krextd …
[   12.562271][0] krextd[0]: Initialisation of krextd:debughandles …
[   12.567385][0] krextd[0]: Initialisation of krextd:debughandles [OK]
[   12.573556][0] krextd[0]: Initialisation of krextd:global …
[   12.580145][0] krextd[0]: Initialisation of krextd:global [OK]
[   12.585775][0] krextd[0]: Initialisation of krextd:memcache …
[   12.593099][0] krextd[0]: Initialisation of krextd:memcache [OK]
[   12.597367][0] krextd[0]: Initialisation of krextd:igmpcompr …
[   12.603585][0] krextd[0]: Initialisation of krextd:igmpcompr [OK]
[   12.609586][0] krextd[0]: Initialisation of krextd:krextdev …
[   12.615667][0] cchardevice: device_create(krextd): 235,0
[   12.621662][0] krextd[0]: Initialisation of krextd:krextdev [OK]
[   12.626891][0] krextd[0]: Initialisation of krextd:krextdev_wland …
[   12.632939][0] cchardevice: device_create(krextd_wlan): 234,0
[   12.639537][0] krextd[0]: Initialisation of krextd:krextdev_wland [OK]
[   12.644956][0] krextd[0]: Initialisation of krextd:netdevice_notifier …
[   12.651396][0] krextd[0]: Initialisation of krextd:netdevice_notifier [OK]
[   12.658198][0] krextd[0]: Initialisation of krextd:krextdprocfs …
[   12.665023][0] krextd[0]: Initialisation of krextd:krextdprocfs [OK]
[   12.671121][0] krextd[0]: Initialisation of krextd:krextdtimer …
[   12.677775][0] krextd[0]: Initialisation of krextd:krextdtimer [OK]
[   12.683695][0] krextd[0]: Initialisation of krextd [OK]
[   12.689854][0] krextd[0]: Initialisation of guestflt …
[   12.695167][0] krextd[0]: Initialisation of guestflt [OK]
[   12.700622][0] krextd[0]: Initialisation of krextdprocfs …
[   12.705938][0] krextd[0]: Initialisation of krextdprocfs [OK]
[   12.711661][0] krextd[0]: Initialisation [OK]
[Supervisor] Info: modules-load.service exit success
[Supervisor] Info: start devnodes.service
[Supervisor] Info: devnodes.service exit success
[Supervisor] Info: start apparmor.service
[Supervisor] Info: start filesystem.service
[Supervisor] Info: apparmor.service exit success
[Supervisor] Info: filesystem.service exit success
[Supervisor] Info: start default-files.service
[   12.964269][0] [avm_power]pm_ressourceinfo_scriptparse: powerdevice_cpuclock: norm_power_rate=100 act_rate=100 mul=0 div=1 offset=0 NormP=0 mW -> SumNormP=0 mW
[   12.964374][0] [avm_power]pm_ressourceinfo_scriptparse: powerdevice_loadrate: norm_power_rate=100 act_rate=23 mul=29 div=10 offset=0 NormP=290 mW -> SumNormP=290 mW
[   12.977456][0] [avm_power]pm_ressourceinfo_scriptparse: powerdevice_systemclock: norm_power_rate=100 act_rate=100 mul=0 div=1 offset=1500 NormP=1500 mW -> SumNormP=1790 mW
[   12.992374][0] [avm_power]pm_ressourceinfo_scriptparse: powerdevice_plc: norm_power_rate=100 act_rate=0 mul=1220 div=100 offset=0 NormP=1220 mW -> SumNormP=3010 mW
[   13.007404][0] [avm_power]pm_ressourceinfo_scriptparse: powerdevice_wlan: norm_power_rate=100 act_rate=0 mul=84 div=10 offset=100 NormP=940 mW -> SumNormP=3950 mW
[   13.021967][0] [avm_power]pm_ressourceinfo_scriptparse: powerdevice_ethernet: norm_power_rate=617 act_rate=16777216 mul=1 div=1 offset=50 NormP=667 mW -> SumNormP=4617 mW
[Supervisor] Info: default-files.service exit success
[Supervisor] Info: start config.service
[Supervisor] Info: start debug.service
[Supervisor] Info: start sysctl.service
net.ipv4.tcp_min_snd_mss = 536
kernel.panic_on_oops = 1
vm.panic_on_oom = 2
kernel.printk = 4
net.ipv4.ip_forward = 1
net.ipv4.tcp_min_tso_segs = 100
net.ipv4.conf.all.rp_filter = 1
net.ipv4.conf.default.rp_filter = 1
[Supervisor] Info: sys[   13.109435][3] sysrq: Changing Loglevel
[   13.112615][3] sysrq: Loglevel set to 4
[   13.119315][3] 
[   13.119315][3] [avm_debug] redirecting kernel-messages (/dev/debug)
ctl.service exit success
[Supervisor] Info: debug.service exit success
[Supervisor] Info: config.service exit success
[Supervisor] Info: start boxnotify.service
[Supervisor] Info: start inetd.service
[Supervisor] Info: start psupport-init-prenet.service
[Supervisor] Info: start run_clock.service
[Supervisor] Info: inetd.service exit success
run_clock demon started

[Supervisor] Info: run_clock.service exit success
[Supervisor] Info: psupport-init-prenet.service exit success
[Supervisor] Info: start net_basic.service
[Supervisor] Info: boxnotify.service exit success
[Supervisor] Info: net_basic.service exit success
[Supervisor] Info: start avmipcd.service
[Supervisor] Info: avmipcd.service notified: ready
[Supervisor] Info: start avmnexusd.service
[Supervisor] Info: start ctlmgr.service
[Supervisor] Info: start l2tpv3d.service
[Supervisor] Info: start psetd.service
[Supervisor] Info: start rextd.service
[Supervisor] Info: start upnpd.service
Jan  1 01:00:13 l2tpv3d[431]: starting … (avminit)

Jan  1 01:00:13 l2tpv3d[431]: started.

[Supervisor] Info: l2tpv3d.service notified: ready
Jan  1 01:00:13 l2tpv3d[431]: verbose: DISABLED

Jan  1 01:00:13 rextd[433]: starting … (avminit)

Jan  1 01:00:13 rextd[433]: netlink: bridge_mdb_add - Invalid argument (22)

[Supervisor] Info: rextd.service notified: ready
[Supervisor] Info: start avmntpd.service
Jan  1 01:00:13 rextd[433]: verbose: DISABLED

Jan  1 01:00:13 avmnexusd[429]: starting … (avminit)

Jan  1 01:00:14 upnpd[434]: starting … (avminit)

Jan  1 01:00:14 avmntpd[511]: starting … (avminit)

Jan  1 01:00:14 avmntpd[511]: verbose: DISABLED

Jan  1 01:00:14 upnpd[434]: verbose: DISABLED

[Supervisor] Info: avmntpd.service notified: ready
[Supervisor] Info: upnpd.service notified: ready
Jan  1 01:00:14 avmnexusd[429]: 12([::]:53805) (dgram) ‚nexus discovery‘: failed to send datagram from unspecified to [ff02::1]:53805 - Cannot assign requested address (99)

[Supervisor] Info: avmnexusd.service notified: ready
[Supervisor] Info: start deviceinfod.service
Jan  1 01:00:14 avmnexusd[429]: verbose: DISABLED

Jan  1 01:00:14 deviceinfod[557]: starting … (avminit)

Jan  1 01:00:14 ctlmgr[430]: starting … (avminit)

[Supervisor] Info: ctlmgr.service notified: ready
Jan  1 01:00:14 deviceinfod[557]: verbose: DISABLED

[Supervisor] Info: deviceinfod.service notified: ready
[Supervisor] Info: start kpid.service
[Supervisor] Info: start meshd.service
[Supervisor] Info: start plcd.service
[Supervisor] Info: start ptest_release.service
[Supervisor] Info: start wifi.service
Jan  1 01:00:14 avmnexusd[429]: 12([::]:53805) (dgram) ‚nexus discovery‘: failed to send datagram from unspecified to [ff02::1]:53805 - Cannot assign requested address (99)

rc.wlan: Start WLAN…
[Supervisor] Info: ptest_release.service exit success
[Supervisor] Info: start configd.service
[Supervisor] Info: start plchost.service
kpid: Sending section usb failed with error -1:
sysfs_usb 1 {„sv“:“gen/v1“,“kpi“:{}}
kpid: Sending section hwpa failed with error -1:
sysfs_hwpa 1 {„sv“:“gen/v1“,“kpi“:{}}
kpid: Sending section system failed with error -1:
sysfs_system 1 {„sv“:“gen/v1“,“kpi“:{„chip“:{„value0“:2425,“value1“:0,“value2“:121043162,“value3“:542671104,“value4“:39716265,“value5“:68814354,“value6“:0,“value7“:0},“temperatures“:{}}}
[Supervisor] Info: configd.service exit success
[Supervisor] Info: psetd.service exit success
Jan  1 01:00:15 plcd[576]: event=Opening the HomePlug library. str1= str2= str3=

Jan  1 01:00:15 plcd[576]: event=Service started. str1= str2= str3=

WLAND:[00595]:01:00.15/[0015.370]:[ALW]Set level of module ‚no_module_log‘ to level ‚VERBOSE‘.
WLAND:[00595]:01:00.15/[0015.380]:[ALW]BUILD: Feb 26 2024, 18:35:48, build-type=1, C-standard=201112
[Supervisor] Info: wifi.service exit success
Jan  1 01:00:16 meshd[575]: starting … (avminit)

Jan  1 01:00:16 meshd[575]: LOG: main: Hello from meshd version: 1.189.1.5.1.9-MOVE21NL1-RC9-0-g704c8ee0

Jan  1 01:00:16 meshd[575]: verbose: DISABLED

Jan  1 01:00:16 plcd[576]: event=Client connected. str1= str2= str3=

[Supervisor] Info: meshd.service notified: ready
[Supervisor] Info: start meshd_config.service
plchost: Network is down: readpacket can’t read plc, error 100
Jan  1 01:00:16 ctlmgr[430]: WLANLIB: wlan_plugin_init:923: prj revision 0xf75551cf5760130a

Jan  1 01:00:16 ctlmgr[430]: 29() (connecting to /var/rpc/timer_if): connect to /var/rpc/timer_if failed - No such file or directory (2)

Jan  1 01:00:16 ctlmgr[430]: WLANLIB: wlan_libs_nexus_init:274: Get Nexus info failed: try again later.

[Supervisor] Info: meshd_config.service exit success
[Supervisor] Info: all Services loaded.
Jan  1 01:00:17 ctlmgr[430]: WLANLIB: wcsi_socket_connect:431: Establishing RPC connection failed with TIMEOUT

Jan  1 01:00:18 plcd[576]: event=Client connected. str1= str2= str3=

[Supervisor] Info: upnpd.service ExecReload exit success

Format: Log Type - Time(microsec) - Message - Optional Info
Log Type: B - Since Boot(Power On Reset),  D - Delta,  S - Statistic
S - QC_IMAGE_VERSION_STRING=AVM_BOOT.BF.3.1.1
S - IMAGE_VARIANT_STRING=DAABANAZA
S - OEM_IMAGE_VERSION_STRING=1214
S - Boot Config, 0x00000025
S - Reset status Config, 0x00000000
S - Core 0 Frequency, 0 MHz
B -       262 - PBL, Start
B -      1344 - bootable_media_detect_entry, Start
B -      2616 - bootable_media_detect_success, Start
B -      2631 - elf_loader_entry, Start
B -      4061 - auth_hash_seg_entry, Start
B -      6026 - auth_hash_seg_exit, Start
B -    106510 - elf_segs_hash_verify_entry, Start
B -    300550 - PBL, End
B -         0 - SBL1, Start
B -    401092 - pm_device_init, Start
D -         9 - pm_device_init, Delta
B -    402235 - boot_flash_init, Start
D -     80218 - boot_flash_init, Delta
B -    486706 - boot_config_data_table_init, Start
D -     14090 - boot_config_data_table_init, Delta - (419 Bytes)
B -    503267 - clock_init, Start
D -      7436 - clock_init, Delta
B -    513673 - CDT version:2,Platform ID:8,Major 
B -    514978 - sbl1_ddr_set_params, Start
B -    519688 - cpr_init, Start
D -         4 - cpr_init, Delta
B -    524767 - Pre_DDR_clock_init, Start
D -         5 - Pre_DDR_clock_init, Delta
D -     13024 - sbl1_ddr_set_params, Delta
B -    538159 - pm_driver_init, Start
D -         4 - pm_driver_init, Delta
B -    573426 - sbl1_wait_for_ddr_training, Start
D -        31 - sbl1_wait_for_ddr_training, Delta
B -    589548 - Image Verify, Start 0:QSEE
D -    284521 - QSEE Image Loaded, Delta - (293400 Bytes)
B -    874383 - Image Verify, Start 0:QSEE_B
D -    287307 - QSEE Image Loaded, Delta - (293400 Bytes)
B -   1162138 - Selected TZ0: 15788 (0:QSEE)
B -   1165088 - Image Load, Start
D -    287199 - QSEE Image Loaded, Delta - (293400 Bytes)
B -   1452600 - Image Load, Start
D -      2033 - SEC Image Loaded, Delta - (2048 Bytes)
B -   1466164 - Image Verify, Start 0:APPSBL
D -    143167 - APPSBL Image Loaded, Delta - (137884 Bytes)
B -   1609650 - Image Verify, Start 0:APPSBL_B
D -    146539 - APPSBL Image Loaded, Delta - (137884 Bytes)
B -   1756621 - Selected EVA0: 11090 (0:APPSBL)
B -   1760358 - Image Load, Start
D -    145596 - APPSBL Image Loaded, Delta - (137884 Bytes)
B -   1906273 - QSEE Execution, Start
D -        60 - QSEE Execution, Delta
B -   1912452 - SBL1, End
D -   1914587 - SBL1, Delta
S - Flash Throughput, 2126 KB/s  (1296319 Bytes,  609732 us)
S - DDR Frequency, 672 MHz
NAND corrected 1 @ page: 8D5
NAND corrected 1 @ page: 8D5
NAND corrected 1 @ page: 8D5
NAND corrected 1 @ page: 11CB
NAND corrected 1 @ page: 11CB
NAND corrected 1 @ page: 11CB

(AVM) EVA Revision: 1.11090

(C) Copyright 2018 AVM Date: Jul  8 2020 Time: 12:57:50 (1) 3 0x0-0x46409

[NAND:] 128MB MACRONIX 2048 Pagesize 128k Blocksize 1024 Blocks HW
[SYSTEM:] CortexA9 
NAND corrected 1 @ page: 1BA2
…………………………………………………………….[    0.000000][0] Booting Linux on physical CPU 0x0
[    0.000000][0] Linux version 4.4.271 (kbuild-team@core.avm.de) (gcc version 5.5.0 (Buildroot 2020.02.1-g758ac3ed) ) #1 SMP PREEMPT 2024-01-11
[    0.000000][0] CPU: ARMv7 Processor [410fc075] revision 5 (ARMv7), cr=10c5387d
[    0.000000][0] CPU: PIPT / VIPT nonaliasing data cache, VIPT aliasing instruction cache
[    0.000000][0] Machine model: AVM FRITZ!Powerline 1260v2
[    0.000000][0] Memory policy: Data cache writealloc
[    0.000000][0] [fw-info] Version 07.58 buildnr=113256 buildtype=1
[    0.000000][0] [module-mem] Use 0x81000000-0x81012fff (mapped at c1000000-c1012fff) for 1 modules
[    0.000000][0] [module-mem] Using whitelist, set default strict_mode=1
[    0.000000][0] PERCPU: Embedded 11 pages/cpu @cfdb7000 s15756 r8192 d21108 u45056
[    0.000000][0] Built 1 zonelists in Zone order, mobility grouping on.  Total pages: 60928
[    0.000000][0] Kernel command line:  clk_ignore_unused audit=1 slub_debug=FL 
[    0.000000][0] audit: enabled (after initialization)
[    0.000000][0] setup_slub_debug: slub_debug = DEBUG_FREE STORE_USER_LITE
[    0.000000][0] PID hash table entries: 1024 (order: 0, 4096 bytes)
[    0.000000][0] Dentry cache hash table entries: 32768 (order: 5, 131072 bytes)
[    0.000000][0] Inode-cache hash table entries: 16384 (order: 4, 65536 bytes)
[    0.000000][0] Memory: 229488K/245760K available (6287K kernel code, 1400K rwdata, 2112K rodata, 240K init, 2703K bss, 16272K reserved, 0K cma-reserved, 0K highmem)
[    0.000000][0] Virtual kernel memory layout:
[    0.000000][0]     vector  : 0xffff0000 - 0xffff1000   (   4 kB)
[    0.000000][0]     fixmap  : 0xffc00000 - 0xfff00000   (3072 kB)
[    0.000000][0]     vmalloc : 0xd0800000 - 0xff800000   ( 752 MB)
[    0.000000][0]     lowmem  : 0xc0000000 - 0xd0000000   ( 256 MB)
[    0.000000][0]     pkmap   : 0xbfe00000 - 0xc0000000   (   2 MB)
[    0.000000][0]     modules : 0xbf000000 - 0xbfe00000   (  14 MB)
[    0.000000][0]       .text : 0xc0208000 - 0xc0a3bf8c   (8400 kB)
[    0.000000][0]       .init : 0xc0a3c000 - 0xc0a78000   ( 240 kB)
[    0.000000][0]       .data : 0xc0a78000 - 0xc0bd6000   (1400 kB)
[    0.000000][0]        .bss : 0xc0bd8000 - 0xc0e7bcc4   (2704 kB)
[    0.000000][0] SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=4, Nodes=1
[    0.000000][0] Preemptible hierarchical RCU implementation.
[    0.000000][0] 	Build-time adjustment of leaf fanout to 32.
[    0.000000][0] NR_IRQS:16 nr_irqs:16 16
[    0.000000][0] Architected cp15 timer(s) running at 48.00MHz (virt).
[    0.000000][0] clocksource: arch_sys_counter: mask: 0xffffffffffffff max_cycles: 0xb11fd3bfb, max_idle_ns: 440795203732 ns
[    0.000000][0] sched_clock: 56 bits at 48MHz, resolution 20ns, wraps every 4398046511096ns
[    0.000000][0] Switching to timer-based delay loop, resolution 20ns
[    0.000314][0] Calibrating delay loop (skipped), value calculated using timer frequency.. 96.00 BogoMIPS (lpj=192000)
[    0.000355][0] pid_max: default: 32768 minimum: 301
[    0.000506][0] Security Framework initialized
[    0.000549][0] AppArmor: AppArmor initialized
[    0.000645][0] Mount-cache hash table entries: 1024 (order: 0, 4096 bytes)
[    0.000675][0] Mountpoint-cache hash table entries: 1024 (order: 0, 4096 bytes)
[    0.001459][0] CPU: Testing write buffer coherency: ok
[    0.001959][0] CPU0: thread -1, cpu 0, socket 0, mpidr 80000000
[    0.002066][0] Setting up static identity map for 0x802082c0 - 0x80208318
[    0.040535][1] CPU1: thread -1, cpu 1, socket 0, mpidr 80000001
[    0.052582][2] CPU2: thread -1, cpu 2, socket 0, mpidr 80000002
[    0.064661][3] CPU3: thread -1, cpu 3, socket 0, mpidr 80000003
[    0.064775][0] Brought up 4 CPUs
[    0.064833][0] SMP: Total of 4 processors activated (384.00 BogoMIPS).
[    0.064856][0] CPU: All CPU(s) started in SVC mode.
[    0.066066][0] devtmpfs: initialized
[    0.077625][0] VFP support v0.3: implementor 41 architecture 2 part 30 variant 7 rev 5
[    0.077844][0] [rte_ipi] Available IPIs 6
[    0.078278][0] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 7645041785100000 ns
[    0.078333][0] futex hash table entries: 1024 (order: 4, 65536 bytes)
[    0.078875][0] pinctrl core: initialized pinctrl subsystem
[    0.080890][0] NET: Registered protocol family 16
[    0.082529][0] DMA: preallocated 2048 KiB pool for atomic coherent allocations
[    0.083096][0] console [avm0] enabled
[    0.092530][0] cpuidle: using governor ladder
[    0.104549][0] cpuidle: using governor menu
[    0.104590][0] Creating Config Table
[    0.108887][0] [qcom:qtimer_probe] WARNING avm,clk-rate not set in dt, using built in default
[    0.112806][0] [qcom_wdt] wdt_ipq40xx_probe …
[    0.121319][0] hw-breakpoint: debug architecture 0x5 unsupported.
[    0.124163][0] CPU: IPQ8064, SoC Version: 4294967274.4294967274
[    0.124338][0] <CORE> glink_init: IPC Logging Disabled
[    0.125050][0] avm_alloc_page_extension node_extension_table[0] entries=65536 (size=262144)  alloced
[    0.125241][0] [fdt_get_reserved_mem_resource] mem_count = 6; search name = „avm_reboot_string“
[    0.125344][0] Reboot Status is: Short-PowerOff-Reboot(SHORTPOWERCUT) SUM(1) - SHORTPOWERCUT(1)
[    0.126038][0] IPC logging disabled
[    0.126067][0] IPC logging disabled
[    0.126088][0] IPC logging disabled
[    0.126109][0] IPC logging disabled
[    0.126130][0] IPC logging disabled
[    0.126594][0] sps:sps is ready.
[    0.128072][0] console [pstore0] enabled
[    0.128396][0] pstore: Registered ramoops as persistent store backend
[    0.128430][0] ramoops: attached 0x100000@0x86000000, ecc: 0/0
[    0.151605][0] SCSI subsystem initialized
[    0.152148][0] usbcore: registered new interface driver usbfs
[    0.152268][0] usbcore: registered new interface driver hub
[    0.152363][0] usbcore: registered new device driver usb
[    0.154445][0] Advanced Linux Sound Architecture Driver Initialized.
[    0.155448][0] AVM PA for Linux version 4.4.271 (kbuild-team@core.avm.de) (gcc version 5.5.0 (Buildroot 2020.02.1-g758ac3ed) ) #1 SMP PREEMPT 2024-01-11
[    0.155448][0]  (early init)
[    0.155946][0] NET: Registered protocol family 8
[    0.155982][0] NET: Registered protocol family 20
[    0.156243][0] TZ-pin nr 15 reprioritized to 60
[    0.156282][0] TZ-pin nr 36 reprioritized to 60
[    0.156383][0] TZ-pin nr 206 reprioritized to 60
[    0.156412][0] TZ-pin nr 213 reprioritized to 60
[    0.156444][0] TZ-pin nr 225 reprioritized to 60
[    0.156470][0] TZ-pin nr 226 reprioritized to 60
[    0.156496][0] TZ-pin nr 227 reprioritized to 60
[    0.156522][0] TZ-pin nr 228 reprioritized to 60
[    0.156548][0] TZ-pin nr 229 reprioritized to 60
[    0.156574][0] TZ-pin nr 230 reprioritized to 60
[    0.156601][0] TZ-pin nr 231 reprioritized to 60
[    0.156627][0] TZ-pin nr 232 reprioritized to 60
[    0.156653][0] TZ-pin nr 233 reprioritized to 60
[    0.156695][0] TZ-pin nr 269 reprioritized to 60
[    0.157040][1] [AVM_FIQ] FIQ disabled on CPU1 to install new vector!
[    0.157046][2] [AVM_FIQ] FIQ disabled on CPU2 to install new vector!
[    0.157053][3] [AVM_FIQ] FIQ disabled on CPU3 to install new vector!
[    0.157100][0] [AVM_FIQ] FIQ disabled on CPU0 to install new vector!
[    0.157129][0] [AVM_FIQ] Vector installed!
[    0.157153][0] [avm_scm] Set FIQ handler address
[    0.157183][3] [AVM_FIQ] FIQ enabled again on CPU3!
[    0.157188][2] [AVM_FIQ] FIQ enabled again on CPU2!
[    0.157194][1] [AVM_FIQ] FIQ enabled again on CPU1!
[    0.157243][0] [AVM_FIQ] FIQ enabled again on CPU0!
[    0.157285][0] [AVM_FIQ] (Version 1.0)(TZ 15788)
[    0.157430][0] clocksource: Switched to clocksource arch_sys_counter
[    0.158180][0] AppArmor: AppArmor Filesystem Enabled
[    0.160734][0] NET: Registered protocol family 2
[    0.173686][0] TCP established hash table entries: 2048 (order: 1, 8192 bytes)
[    0.173758][0] TCP bind hash table entries: 2048 (order: 2, 16384 bytes)
[    0.173825][0] TCP: Hash tables configured (established 2048 bind 2048)
[    0.173939][0] UDP hash table entries: 256 (order: 1, 8192 bytes)
[    0.173991][0] UDP-Lite hash table entries: 256 (order: 1, 8192 bytes)
[    0.174326][0] NET: Registered protocol family 1
[    0.174860][0] hw perfevents: enabled with armv7_cortex_a7 PMU driver, 5 counters available
[    0.177322][0] audit: initializing netlink subsys (enabled)
[    0.177486][0] audit: type=2000 audit(0.175:1): initialized
[    0.205066][0] squashfs: version 4.0 (2009/01/31) Phillip Lougher
[    0.205794][0] ANTFS Module: Version 2.53
[    0.206098][0] jffs2: version 2.2 (NAND) (SUMMARY) (ZLIB) (LZO) (LZMA) (RTIME) (CMODE_PRIORITY) (c) 2001-2006 Red Hat, Inc.
[    0.208979][0] fuse init (API version 7.23)
[    0.216616][0] Key type asymmetric registered
[    0.216666][0] Asymmetric key parser ‚x509‘ registered
[    0.216760][0] io scheduler noop registered
[    0.216796][0] io scheduler deadline registered (default)
[    0.224711][0] glink_loopback_server_init: IPC Logging disabled
[    0.226321][0] NET: Registered protocol family 27
[    0.226360][0] IPC_RTR: ipc_router_create_log_ctx: IPC Logging disabled
[    0.226400][0] qmi_log_init: IPC Logging disabled
[    0.226425][0] qmi_log_init: IPC Logging disabled
[    0.226759][0] tcsr 194b000.tcsr: setting usb hs phy mode select = e700e7
[    0.226876][0] tcsr 1953000.ess_tcsr: setting ess interface select = 1
[    0.226984][0] tcsr 1949000.tcsr: setting wifi_glb_cfg = 41000000
[    0.227070][0] tcsr 1957000.tcsr: setting wifi_noc_memtype_m0_m2 = 2222222
[    0.227343][0] TZ Log : Will warn on Access Violation, as paniconaccessviolation is not set
[    0.228528][0] msm_serial 78af000.serial: msm_serial: detected port #0
[    0.228674][0] msm_dectuart_probe: set dectuart_port to ttyMSM0
[    0.228743][0] msm_serial 78af000.serial: uartclk = 1843200
[    0.228815][0] 78af000.serial: ttyMSM0 at MMIO 0x78af000 (irq = 24, base_baud = 115200) is a MSM
[    0.228866][0] msm_serial: console setup on port #0
[    1.106109][0] console [ttyMSM0] enabled
[    1.111298][0] msm_serial: driver initialized
[    1.115198][0] msm_serial_hsl_init: driver initialized
[    1.119410][0] [avm_power]avm_power_pm_qos_init
[    1.124501][0] [loadcontrol] set auto - scale=1
[    1.128592] [avm] configured: watchdog event debug 
[    1.138192][0] Register push button event to receive the set_factory_kernel event
[    1.149809][0] AVM Simple Profiling enabled Version 3.0
[    1.149871][0] [simple-profiling]:4 performance counters implemented
[    1.153921][0] [simple-profiling]all cpus:performance-mode: round-robin
[    1.160522][0] [simple-profiling]all cpus:performance-mode: round-robin
[    1.166844][0] [simple-profiling]all cpus:performance-mode: round-robin
[    1.173452][0] [simple-profiling]all cpus:performance-mode: round-robin
[    1.180112][0] AVM_WATCHDOG: Watchdog Driver for AR7 Hardware (Version 1.0)
[    1.186825][0] [qcom_wdt] ar7wdt_hw_init…
[    1.193678][0] [avm_request_fiq_on] Virtual IRQ numbers are not supported. Use HWIRQ (35) for requested IRQ (25)
[    1.197777][0] [qcom_wdt] [register_wdt_bark_irq] watchdog as fastirq(35) on all cpus registered with its default prio
[    1.208143][0] [avm_request_fiq_on] Forcing HW-IRQ 36 instead
[    1.218674][0] [qcom_wdt] [register_wdt_bark_irq] watchdog as fastirq(36) on all cpus registered with highest prio
[    1.224461][0] [avm_request_fiq_on] Forcing HW-IRQ 213 instead
[    1.234732][0] [qcom_wdt] [register_secure_wdt_bark_irq] secure watchdog as fastirq(213) on all cpus registered with highest prio
[    1.249524][0] [qcom_wdt] [ar7wdt_hw_init] Wdt bark time: 320000, bite time: 640000
[    1.252232][0] [qcom_wdt] [ar7wdt_hw_init] Secure watchdog: bark: 20s, bite time: 40s
[    1.260792][0] avm_net_trace: Up and running.
[    1.271150][0] loop: module loaded
[    1.273189][0] zram: Added device: zram0
[    1.277135][0] QPIC controller hw version Major:1, Minor:4
[    1.279885][0] nand: device found, Manufacturer ID: 0xc2, Chip ID: 0xf1
[    1.284711][0] nand: ONFI 10-Compliant Macronix MX30LF1G18AC
[    1.291210][0] nand: 128 MiB, SLC, erase size: 128 KiB, page size: 2048, OOB size: 64
[    1.297147][0] [TFFS3_Register_Panic_CB] registering panic callback for mtd qcom_nand.0
[    1.304913][0] 5 ofpart partitions found on MTD device qcom_nand.0
[    1.312652][0] Creating 5 MTD partitions on „qcom_nand.0“:
[    1.318903][0] 0x000000b00000-0x000000f00000 : „kernel“
[    1.330349][0] 0x000000000000-0x0000002c0000 : „urlader“
[    1.335054][0] 0x0000002c0000-0x000000b00000 : „nand-tffs“
[    1.345101][0] 0x000000f00000-0x000001300000 : „reserved-kernel“
[    1.351010][0] 0x000001300000-0x000008000000 : „ubi“
[    1.462366][0] libphy: Fixed MDIO Bus: probed
[    1.463127][0] qca-mdio 90000.mdio: Skipping early reset
[    1.465969][0] libphy: qca_mdio: probed
[    1.474073][0] qca-mdio 90000.mdio: qca-mdio driver was registered
[    1.474795][0] tun: Universal TUN/TAP device driver, 1.6
[    1.480954][0] tun: (C) 1999-2004 Max Krasnyansky <maxk@qualcomm.com>
[    1.992305][0] i2c /dev entries driver
[    1.994530][0] sdhci: Secure Digital Host Controller Interface driver
[    1.994970][0] sdhci: Copyright(c) Pierre Ossman
[    2.001535][0] sdhci-pltfm: SDHCI platform and OF driver helper
[    2.008947][0] AVM PA 2.138.1.16-release_move21-move21 for Linux Linux version 4.4.271 (kbuild-team@core.avm.de) (gcc version 5.5.0 (Buildroot 2020.02.1-g758ac3ed) ) #1 SMP PREEMPT 2024-01-11
[    2.008947][0]  (late init)
[    2.012599][0] gre: GRE over IPv4 demultiplexor driver
[    2.031712][0] Initializing XFRM netlink socket
[    2.036870][0] IPsec XFRM device driver
[    2.043272][0] NET: Registered protocol family 10
[    2.047457][0] sit: IPv6 over IPv4 tunneling driver
[    2.050979][0] NET: Registered protocol family 17
[    2.054978][0] Bridge broadcast ratelimiter registered
[    2.059499][0] bridge: automatic filtering via arp/ip/ip6tables has been deprecated. Update your scripts to load br_netfilter if you need this.
[    2.064611][0] Bridge firewalling registered
[    2.077318][0] KOAM is loaded successfully.
[    2.081837][0] l2tp_core: L2TP core driver, V2.0
[    2.085713][0] l2tp_ip: L2TP IP encapsulation support (L2TPv3)
[    2.090853][0] l2tp_netlink: L2TP netlink interface
[    2.096275][0] l2tp_eth: L2TP ethernet pseudowire support (L2TPv3)
[    2.100995][0] l2tp_ip6: L2TP IP encapsulation support for IPv6 (L2TPv3)
[    2.107524][0] 8021q: 802.1Q VLAN Support v1.8
[    2.114247][0] Registering SWP/SWPB emulation handler
[    2.118417][0] [fdt_get_reserved_mem_resource] mem_count = 6; search name = „avm_sbl_boot_string“
[    2.123480][0] SBL Boot Info Version 1214 Boot TZ 0 Boot Eva 0
[    2.132318] TZ0 Version 15788 
[    2.138040][0] TZ1 Version 15788
[    2.141143][0] EVA0 Version 11090
[    2.144462][0] EVA1 Version 11090
[    2.147896][0] [rte_ipi] Requested ipi RTE monitor (nr=9, prio=00, flags=0x00800001)
[    2.151181][0] [rte_ipi] Requested ipi RTE linux (nr=10, prio=80, flags=0x00800000)
[    2.158862][0] [fdt_get_reserved_mem_resource] mem_count = 6; search name = „avm_sbl_boot_string“
[    2.169347][0] Could not find Env ‚kernel_args‘ in the device tree
[    2.175391][0] [TFFS3_Init] Called.
[    2.181287][0] [TFFS3_CACHE_Configure] Setting up caching for backend nand
[    2.184673][0] [TFFS3-CACHE] Caching module for TFFS 3.x
[    2.191611][0] [TFFS3-NAND] NAND storage backend for TFFS 3.x on mtd2
[    2.559500][0] random: nonblocking pool is initialized
[    5.161886][0] [TFFS3-NAND] Initialisation successful, 66/66/66 NAND blocks active, fill rate 6%
[    5.161966][0] [TFFS_Cache] Allocate segement buffer cache (size=2024)
[    5.169849][0] tffs/panic: have_new_logentry: Error reading crashenv: -2
[    5.176151][0] tffs/panic: have_new_logentry: Error reading crashenv: -2
[    5.183192][0] TFFS: tiny flash file system driver. GPL (c) AVM Berlin (Version 3.0)
[    5.189772][0] Adam2 environment variables API installed.
[    5.198460][0] ubi0: attaching mtd4
[    5.794033][0] ubi0: scanning is finished
[    5.805105][0] ubi0: attached mtd4 (name „ubi“, size 109 MiB)
[    5.805162][0] ubi0: PEB size: 131072 bytes (128 KiB), LEB size: 126976 bytes
[    5.809906][0] ubi0: min./max. I/O unit sizes: 2048/2048, sub-page size 2048
[    5.817061][0] ubi0: VID header offset: 2048 (aligned 2048), data offset: 4096
[    5.824121][0] ubi0: good PEBs: 872, bad PEBs: 0, corrupted PEBs: 0
[    5.831144][0] ubi0: user volume: 3, internal volumes: 1, max. volumes count: 128
[    5.837309][0] ubi0: max/mean erase counter: 2/1, WL threshold: 4096, image sequence number: 2726414984
[    5.844953][0] ubi0: available PEBs: 0, total reserved PEBs: 872, PEBs reserved for bad PEB handling: 20
[    5.854190][2] ubi0: background thread „ubi_bgt0d“ started, PID 96
[    5.865736][0] mtd: device 5 (filesystem) set to be root filesystem
[    5.873675][0] hctosys: unable to open rtc device (rtc0)
[    5.881395][0] clk: Not disabling unused clocks
[    5.881570][0] ALSA device list:
[    5.885838][0]   No soundcards found.
[    5.893156][0] VFS: Mounted root (squashfs filesystem) readonly on device 31:5.
[    5.896521][0] devtmpfs: mounted
[    5.901181][0] Freeing unused kernel memory: 240K

starting pid 105, tty ‚‘: ‚/etc/boot.d/1‘
[    6.683606][0] hui: loading out-of-tree module taints kernel.
[    6.690195][0] [hui] Initialize hardware user interface
[    6.692897][0] [avm_connect][state_machine_init] starting event worker thread
mknod: /dev/led: File exists
[    6.746916][3] TFFS Name Table N
[Supervisor] Info: start svlogd.service
[Supervisor] Info: svlogd.service notified: ready
[Supervisor] Info: start disable_ipv6.service
[Supervisor] Info: start tffs.service
[Supervisor] Info: disable_ipv6.service exit success

Please press Enter to activate this console. [Supervisor] Info: tffs.service exit success
[Supervisor] Info: start rekey.service
firmwarecfg config_rekey: done
[Supervisor] Info: rekey.service exit success
[Supervisor] Info: start environment.service
[    9.005963][0] [0]system-load  79% loadavg 0.16 0.3 0.1 - softirqs:5.64% (vchan_complete 60%) pgstat: sum=55825 free=51433 slab=1721 alloc=1547/s fault=1134/s (sleep 1)
[Supervisor] Info: environment.service exit success
[Supervisor] Info: start watchdog.service
[    9.803907][0] AVM_WATCHDOG: System Init Ueberwachung 120 Sekunden
[Supervisor] Info: watchdog.service exit success
[Supervisor] Info: start udev.service
[Supervisor] Info: start udevadm.service
[    9.986180][1] [1]system-load  60% loadavg 0.16 0.3 0.1 - task runtime:6% max:udevadm 3%  pgstat: sum=55704 free=51162 slab=1743 alloc=1971/s fault=1601/s (sleep 1)
[   10.020471][1] udevd[314]: starting version 3.2.5
[   10.045591][1] udevd[314]: specified group ‚tty‘ unknown
[   10.046037][1] udevd[314]: specified group ‚dialout‘ unknown
[   10.050325][1] udevd[314]: specified group ‚kmem‘ unknown
[   10.055964][1] udevd[314]: specified group ‚input‘ unknown
[   10.061464][1] udevd[314]: specified group ‚video‘ unknown
[   10.066792][1] udevd[314]: specified group ‚audio‘ unknown
[   10.072335][1] udevd[314]: specified group ‚lp‘ unknown
[   10.077740][1] udevd[314]: specified group ‚disk‘ unknown
[   10.082681][1] udevd[314]: specified group ‚cdrom‘ unknown
[   10.088392][1] udevd[314]: specified group ‚tape‘ unknown
[   10.096717][1] udevd[314]: starting eudev-3.2.5
[   10.262621][2] [2]system-load  62% loadavg 0.39 0.8 0.3 - task runtime:46% max:udevd 23%  pgstat: sum=55876 free=50667 slab=2017 alloc=2095/s fault=1707/s (sleep 1)
[   10.730805][2] ssdk_switch_device_num_init[1340]:INFO:ess-switch dts node number: 1
[   10.730902][2] ssdk_dt_get_switch_node[1143]:INFO:ess-switch DT exist!
[   10.737353][2] ssdk_dt_parse_access_mode[1029]:INFO:switch_access_mode: local bus
[   10.743920][2] ssdk_dt_parse_access_mode[1042]:INFO:switchreg_base_addr: 0xc000000
[   10.751464][2] ssdk_dt_parse_access_mode[1043]:INFO:switchreg_size: 0x80000
[   10.758931][2] ssdk_dt_parse_mac_mode[361]:INFO:mac mode = 0x1 (PORT_WRAPPER_PSGMII_RGMII5)
[   10.765788][2] ssdk_dt_parse_mac_mode[367]:INFO:mac mode1 doesn’t exit!
[   10.774119][2] ssdk_dt_parse_mac_mode[377]:INFO:mac mode2 doesn’t exit!
[   10.780712][2] ssdk_dt_parse_phy_info[645]:INFO:qcom,port_phyinfo DT doesn’t exist!
[   10.787328][2] ssdk_dt_parse_mdio[806]:INFO:mdio DT exist!
[   10.795025][2] ssdk_dt_parse_led[1116]:INFO:current dts led_source_num is 0
[   10.800527][2] ssdk_dt_parse_psgmii[994]:INFO:ess-psgmii DT exist!
[   10.807387][2] ssdk_plat_init start
[   10.813774][2] ssdk_plat_init[1624]:INFO:Enable ess clk
[   10.917695][3] [3]system-load  62% loadavg 0.39 0.8 0.3 - task runtime:29% max:udevd 21%  pgstat: sum=55701 free=50113 slab=2063 alloc=2168/s fault=1697/s (sleep 2)
[   10.999352][2] malibu_phy_api_ops_init[2869]:INFO:qca probe malibu phy driver succeeded!
[   11.000264][2] regi_init[4080]:INFO:Initializing DESS!!
[   11.121475][1] avm_power: [avm_power_temperature] No cpu sensor registered
[   11.848981][2] ssdk_switch_register[1965]:INFO:Chip version 0x1401
[   11.849055][2] ssdk_switch_register[1991]:INFO:polling is selected
[   11.854110][2] regi_init[4090]:INFO:Initializing DESS Done!!
[   11.879627][2] regi_init[4162]:INFO:qca-ssdk module init succeeded!
[   11.904833][2] [module-mem] give 0x11000 bytes at c1001000 to module ‚essedma‘ (0x1000 bytes left)
[   11.907086][2] Using 2 netdevs
[   11.913802][2] EDMA  Dev eth0 (0) —> phy mdio 3
[   11.915754][2] EDMA  Dev plc (1) —> phy mdio 24
[   11.920780][2] [avm_request_fiq_on] Virtual IRQ numbers are not supported. Use HWIRQ (272) for requested IRQ (77)
[Supervisor] Info: udevadm.service exit success
[Supervisor] Info: start cortexa9.service
SBL ACK done
[TZ-Update]
[tz-update] bound mibib block at page 524288.
[tz-update] 2 trustzones found. update index 0 first.
[tz-update] tz0 already up to date. version: 15788
[tz-update] tz1 already up to date. version: 15788
… tz not updated
[Supervisor] Info: cortexa9.service exit success
[Supervisor] Info: start capi-config.service
[Supervisor] Info: start modules-load.service
[Supervisor] Info: start piglet.service
[Supervisor] Info: capi-config.service exit success
[Supervisor] Info: piglet.service exit error
[Supervisor] Info: start capi.service
[Supervisor] Info: capi.service exit success
[   12.258187][3] cprocfs: loaded
[   12.260082][3] kspeedtest: kspeedtest_init: second timer started 
[   12.260227][3] kspeedtest: Starting default task on discard port 9
[   12.266458][3] kspeedtest: listening on port 9
[   12.272432][3] kspeedtest: kspeedtest_init done
[   12.309078][3] cchardevice: loaded
[   12.404978][0] krextdmod: module license ‚unspecified‘ taints kernel.
[   12.405041][0] Disabling lock debugging due to kernel taint
[   12.445941][0] krextd[0]: Initialisation of debughandles …
[   12.446004][0] krextd[0]: Initialisation of debughandles [OK]
[   12.450721][0] krextd[0]: Initialisation of cmemstack …
[   12.456417][0] krextd[0]: Initialisation of cmemstack [OK]
[   12.461765][0] krextd[0]: Initialisation of procfs …
[   12.467149][0] krextd[0]: Initialisation of procfs [OK]
[   12.472239][0] krextd[0]: Initialisation of kmod_debugctl …
[   12.477379][0] krextd[0]: Initialisation of kmod_debugctl [OK]
[   12.483279][0] krextd[0]: Initialisation of cenv …
[   12.488990][0] krextd[0]: Initialisation of cenv [OK]
[   12.494111][0] krextd[0]: Initialisation of ctimer …
[   12.500124][0] krextd[0]: Initialisation of ctimer [OK]
[   12.504360][0] krextd[0]: Initialisation of kmodcmddev …
[   12.509270][0] krextd[0]: Initialisation of kmodcmddev [OK]
[   12.514801][0] krextd[0]: Initialisation of packettrace …
[   12.520862][0] cchardevice: device_create(kdsldptrace%d): 240,0
[   12.526191][0] cchardevice: device_create(kdsldptrace%d): 240,1
[   12.532076][0] krextd[0]: Initialisation of packettrace [OK]
[   12.537639][0] krextd[0]: Initialisation of nqos …
[   12.543626][0] cchardevice: device_create(knqos): 239,0
[   12.551340][0] cchardevice: device_create(avmtrackd): 238,0
[   12.553863][0] cchardevice: device_create(avmtrackdquery): 237,0
[   12.559502][0] krextd[0]: Initialisation of nqos [OK]
[   12.565265][0] krextd[0]: Initialisation of bridgeflt …
[   12.570263][0] cchardevice: device_create(bridgeflt): 236,0
[   12.575878][0] krextd[0]: Initialisation of bridgeflt [OK]
[   12.580977][0] krextd[0]: Initialisation of krextd …
[   12.586499][0] krextd[0]: Initialisation of krextd:debughandles …
[   12.591616][0] krextd[0]: Initialisation of krextd:debughandles [OK]
[   12.597785][0] krextd[0]: Initialisation of krextd:global …
[   12.604374][0] krextd[0]: Initialisation of krextd:global [OK]
[   12.610008][0] krextd[0]: Initialisation of krextd:memcache …
[   12.617309][0] krextd[0]: Initialisation of krextd:memcache [OK]
[   12.621583][0] krextd[0]: Initialisation of krextd:igmpcompr …
[   12.627804][0] krextd[0]: Initialisation of krextd:igmpcompr [OK]
[   12.633815][0] krextd[0]: Initialisation of krextd:krextdev …
[   12.639889][0] cchardevice: device_create(krextd): 235,0
[   12.645857][0] krextd[0]: Initialisation of krextd:krextdev [OK]
[   12.651110][0] krextd[0]: Initialisation of krextd:krextdev_wland …
[   12.657196][0] cchardevice: device_create(krextd_wlan): 234,0
[   12.663741][0] krextd[0]: Initialisation of krextd:krextdev_wland [OK]
[   12.669168][0] krextd[0]: Initialisation of krextd:netdevice_notifier …
[   12.675586][0] krextd[0]: Initialisation of krextd:netdevice_notifier [OK]
[   12.682419][0] krextd[0]: Initialisation of krextd:krextdprocfs …
[   12.689254][0] krextd[0]: Initialisation of krextd:krextdprocfs [OK]
[   12.695336][0] krextd[0]: Initialisation of krextd:krextdtimer …
[   12.702001][0] krextd[0]: Initialisation of krextd:krextdtimer [OK]
[   12.707928][0] krextd[0]: Initialisation of krextd [OK]
[   12.714086][0] krextd[0]: Initialisation of guestflt …
[   12.719366][0] krextd[0]: Initialisation of guestflt [OK]
[   12.724900][0] krextd[0]: Initialisation of krextdprocfs …
[   12.730177][0] krextd[0]: Initialisation of krextdprocfs [OK]
[   12.735886][0] krextd[0]: Initialisation [OK]
[Supervisor] Info: modules-load.service exit success
[Supervisor] Info: start devnodes.service
[Supervisor] Info: devnodes.service exit success
[Supervisor] Info: start apparmor.service
[Supervisor] Info: start filesystem.service
[Supervisor] Info: apparmor.service exit success
[Supervisor] Info: filesystem.service exit success
[Supervisor] Info: start default-files.service
[   12.989703][1] [avm_power]pm_ressourceinfo_scriptparse: powerdevice_cpuclock: norm_power_rate=100 act_rate=100 mul=0 div=1 offset=0 NormP=0 mW -> SumNormP=0 mW
[   12.989838][1] [avm_power]pm_ressourceinfo_scriptparse: powerdevice_loadrate: norm_power_rate=100 act_rate=23 mul=29 div=10 offset=0 NormP=290 mW -> SumNormP=290 mW
[   13.002903][1] [avm_power]pm_ressourceinfo_scriptparse: powerdevice_systemclock: norm_power_rate=100 act_rate=100 mul=0 div=1 offset=1500 NormP=1500 mW -> SumNormP=1790 mW
[   13.017819][1] [avm_power]pm_ressourceinfo_scriptparse: powerdevice_plc: norm_power_rate=100 act_rate=0 mul=1220 div=100 offset=0 NormP=1220 mW -> SumNormP=3010 mW
[   13.032818][1] [avm_power]pm_ressourceinfo_scriptparse: powerdevice_wlan: norm_power_rate=100 act_rate=0 mul=84 div=10 offset=100 NormP=940 mW -> SumNormP=3950 mW
[   13.047412][1] [avm_power]pm_ressourceinfo_scriptparse: powerdevice_ethernet: norm_power_rate=617 act_rate=16777216 mul=1 div=1 offset=50 NormP=667 mW -> SumNormP=4617 mW
[Supervisor] Info: default-files.service exit success
[Supervisor] Info: start config.service
[Supervisor] Info: start debug.service
[Supervisor] Info: start sysctl.service
net.ipv4.tcp_min_snd_mss = 536
kernel.panic_on_oops = 1
vm.panic_on_oom = 2
kernel.printk = 4
net.ipv4.ip_forward = 1
net.ipv4.tcp_min_tso_segs = 100
net.ipv4.conf.all.rp_filter = 1
net.ipv4.conf.default.rp_filter = 1
[Supervisor] Info: sysctl.service exit success
[   13.141639][2] sysrq: Changing Loglevel
[   13.141694][2] sysrq: Loglevel set to 4
[   13.147179][2] 
[   13.147179][2] [avm_debug] redirecting kernel-messages (/dev/debug)
[Supervisor] Info: debug.service exit success
[Supervisor] Info: config.service exit success
[Supervisor] Info: start boxnotify.service
[Supervisor] Info: start inetd.service
[Supervisor] Info: start psupport-init-prenet.service
[Supervisor] Info: start run_clock.service
[Supervisor] Info: inetd.service exit success
run_clock demon started

[Supervisor] Info: run_clock.service exit success
[Supervisor] Info: psupport-init-prenet.service exit success
[Supervisor] Info: start net_basic.service
[Supervisor] Info: boxnotify.service exit success
[Supervisor] Info: net_basic.service exit success
[Supervisor] Info: start avmipcd.service
[Supervisor] Info: avmipcd.service notified: ready
[Supervisor] Info: start avmnexusd.service
[Supervisor] Info: start ctlmgr.service
[Supervisor] Info: start l2tpv3d.service
[Supervisor] Info: start psetd.service
[Supervisor] Info: start rextd.service
[Supervisor] Info: start upnpd.service
Jan  1 01:00:13 l2tpv3d[430]: starting … (avminit)

Jan  1 01:00:13 l2tpv3d[430]: started.

[Supervisor] Info: l2tpv3d.service notified: ready
Jan  1 01:00:13 l2tpv3d[430]: verbose: DISABLED

Jan  1 01:00:13 rextd[432]: starting … (avminit)

Jan  1 01:00:13 upnpd[433]: starting … (avminit)

Jan  1 01:00:14 avmnexusd[428]: starting … (avminit)

Jan  1 01:00:14 rextd[432]: netlink: bridge_mdb_add - Invalid argument (22)

Jan  1 01:00:14 upnpd[433]: verbose: DISABLED

Jan  1 01:00:14 rextd[432]: verbose: DISABLED

[Supervisor] Info: upnpd.service notified: ready
[Supervisor] Info: rextd.service notified: ready
[Supervisor] Info: start avmntpd.service
Jan  1 01:00:14 avmntpd[516]: starting … (avminit)

Jan  1 01:00:14 avmntpd[516]: verbose: DISABLED

[Supervisor] Info: avmntpd.service notified: ready
Jan  1 01:00:14 avmnexusd[428]: 12([::]:53805) (dgram) ‚nexus discovery‘: failed to send datagram from unspecified to [ff02::1]:53805 - Cannot assign requested address (99)

Jan  1 01:00:14 avmnexusd[428]: verbose: DISABLED

[Supervisor] Info: avmnexusd.service notified: ready
[Supervisor] Info: start deviceinfod.service
Jan  1 01:00:14 avmnexusd[428]: 12([::]:53805) (dgram) ‚nexus discovery‘: failed to send datagram from unspecified to [ff02::1]:53805 - Cannot assign requested address (99)

Jan  1 01:00:14 deviceinfod[549]: starting … (avminit)

[Supervisor] Info: deviceinfod.service notified: ready
Jan  1 01:00:14 deviceinfod[549]: verbose: DISABLED

Jan  1 01:00:14 ctlmgr[429]: starting … (avminit)

[Supervisor] Info: ctlmgr.service notified: ready
[Supervisor] Info: start kpid.service
[Supervisor] Info: start meshd.service
[Supervisor] Info: start plcd.service
[Supervisor] Info: start ptest_release.service
[Supervisor] Info: start wifi.service
Jan  1 01:00:14 avmnexusd[428]: 12([::]:53805) (dgram) ‚nexus discovery‘: failed to send datagram from unspecified to [ff02::1]:53805 - Cannot assign requested address (99)

rc.wlan: Start WLAN…
[Supervisor] Info: ptest_release.service exit success
[Supervisor] Info: start configd.service
[Supervisor] Info: start plchost.service
kpid: Sending section usb failed with error -1:
sysfs_usb 1 {„sv“:“gen/v1“,“kpi“:{}}
kpid: Sending section hwpa failed with error -1:
sysfs_hwpa 1 {„sv“:“gen/v1“,“kpi“:{}}
kpid: Sending section system failed with error -1:
sysfs_system 1 {„sv“:“gen/v1“,“kpi“:{„chip“:{„value0“:2425,“value1“:0,“value2“:121043162,“value3“:542671104,“value4“:39716265,“value5“:68814354,“value6“:0,“value7“:0},“temperatures“:{}}}
[Supervisor] Info: configd.service exit success
[Supervisor] Info: psetd.service exit success
Jan  1 01:00:15 plcd[576]: event=Opening the HomePlug library. str1= str2= str3=

Jan  1 01:00:15 plcd[576]: event=Service started. str1= str2= str3=

WLAND:[00595]:01:00.15/[0015.430]:[ALW]Set level of module ‚no_module_log‘ to level ‚VERBOSE‘.
WLAND:[00595]:01:00.15/[0015.430]:[ALW]BUILD: Feb 26 2024, 18:35:48, build-type=1, C-standard=201112
[Supervisor] Info: wifi.service exit success
plchost: Network is down: readpacket can’t read plc, error 100
Jan  1 01:00:16 meshd[575]: starting … (avminit)

Jan  1 01:00:16 ctlmgr[429]: WLANLIB: wlan_plugin_init:923: prj revision 0xf75551cf5760130a

Jan  1 01:00:16 meshd[575]: LOG: main: Hello from meshd version: 1.189.1.5.1.9-MOVE21NL1-RC9-0-g704c8ee0

Jan  1 01:00:16 meshd[575]: verbose: DISABLED

Jan  1 01:00:16 plcd[576]: event=Client connected. str1= str2= str3=

[Supervisor] Info: meshd.service notified: ready
[Supervisor] Info: start meshd_config.service
Jan  1 01:00:16 ctlmgr[429]: 29() (connecting to /var/rpc/timer_if): connect to /var/rpc/timer_if failed - No such file or directory (2)

Jan  1 01:00:16 ctlmgr[429]: WLANLIB: wlan_libs_nexus_init:274: Get Nexus info failed: try again later.

[Supervisor] Info: meshd_config.service exit success
[Supervisor] Info: all Services loaded.
Jan  1 01:00:17 ctlmgr[429]: WLANLIB: wcsi_socket_connect:431: Establishing RPC connection failed with TIMEOUT

Jan  1 01:00:18 plcd[576]: event=Client connected. str1= str2= str3=

[Supervisor] Info: upnpd.service ExecReload exit success