[/][-][\][|][/][-][\][|][/][-][\][|][/][-][\][|][/][-][\][|][/][-][\][|][/][-][\][|][/][-][\][|][/][-][\][|][/][-][\][|][/][-][\][|][/][-]

(AVM) EVA Revision: 1.11013

(C) Copyright 2018 AVM Date: May 20 2020 Time: 14:58:06 (0) 3 0x0-0x240D

[FLASH:] MACRONIX Uniform-Flash 64MB 256 Bytes WriteBuffer
[FLASH:](Eraseregion [0] 1024 sectors a 64kB) 
[SYSTEM:] QCA956x on 775/650/258MHz
[athr_gmac_sgmii_setup] Max resets limit reached exiting…

Eva_AVM >[athr_gmac_sgmii_setup] Max resets limit reached exiting…
[athr_gmac_sgmii_setup] Max resets limit reached exiting…
[athr_gmac_sgmii_setup] Max resets limit reached exiting…
[athr_gmac_sgmii_setup] Max resets limit reached exiting…
[athr_gmac_sgmii_setup] Max resets limit reached exiting…
[athr_gmac_sgmii_setup] Max resets limit reached exiting…
…………………………………………ExecuteProgram
[    0.000000] Linux version 4.4.271 (kbuild-team@core.avm.de) (gcc version 5.5.0 (Buildroot 2020.02.1-g758ac3ed) ) #1 2023-10-06
[    0.000000] DT @ 80750030: d0 0d fe ed 00 00 1d d6
[    0.000000] MIPS: machine is AVM FRITZ!Repeater 2400
[    0.000000] CPU0 revision is: 00019750 (MIPS 74Kc)
[    0.000000] Set Port base
[    0.000000] detect_sys_type
[    0.000000] SoC: Qualcomm Atheros QCA5502 ver 1 rev 0
[    0.000000] [plat_mem_setup] memsize 0x8000000, memstart 0x00000000
[    0.000000] Determined physical RAM map:
[    0.000000]  memory: 08000000 @ 00000000 (usable)
[    0.000000] Zone ranges:
[    0.000000]   Normal   [mem 0x0000000000000000-0x0000000007ffffff]
[    0.000000] Movable zone start for each node
[    0.000000] Early memory node ranges
[    0.000000]   node   0: [mem 0x0000000000000000-0x0000000007ffffff]
[    0.000000] Initmem setup node 0 [mem 0x0000000000000000-0x0000000007ffffff]
[    0.000000] [fw-info] Version 07.58 buildnr=111615 buildtype=1
[    0.000000] [module-mem] Use 0x01107000-0x015cefff (mapped at 81107000-815cefff) for 30 modules
[    0.000000] Primary instruction cache 64kB, VIPT, 4-way, linesize 32 bytes.
[    0.000000] Primary data cache 32kB, 4-way, VIPT, cache aliases, linesize 32 bytes
[    0.000000] Built 1 zonelists in Zone order, mobility grouping on.  Total pages: 32512
[    0.000000] Kernel command line:  slub_debug=-  gocommand console=ttyS0,115200n8r nor_size=0 sflash_size=64MB nand_size=0MB ethaddr=0C:72:74:33:07:9D
[    0.000000] setup_slub_debug: slub_debug =
[    0.000000] PID hash table entries: 512 (order: -1, 2048 bytes)
[    0.000000] Dentry cache hash table entries: 16384 (order: 4, 65536 bytes)
[    0.000000] Inode-cache hash table entries: 8192 (order: 3, 32768 bytes)
[    0.000000] Writing ErrCtl register=00000000
[    0.000000] Readback ErrCtl register=00000000
[    0.000000] [mips_nmi_setup] setup NMI vector to base 0x80000380
[    0.000000] Memory: 116316K/131072K available (4768K kernel code, 640K rwdata, 1740K rodata, 288K init, 769K bss, 14756K reserved, 0K cma-reserved)
[    0.000000] SLUB: HWalign=32, Order=0-3, MinObjects=0, CPUs=1, Nodes=1
[    0.000000] [nmi] VA:PA c0000000:40000000 wired at entry 0x1
[    0.000000] NR_IRQS:91
[    0.000000] Clocks: CPU:775.000MHz, DDR:650.000MHz, AHB:258.333MHz, Ref:25.000MHz
[    0.000000] clocksource: MIPS: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 4932285024 ns
[    0.000007] sched_clock: 32 bits at 387MHz, resolution 2ns, wraps every 5541893118ns
[    0.228188] console [ttyS0] enabled
[    0.231814] Calibrating delay loop… 385.02 BogoMIPS (lpj=770048)
[    0.266456] pid_max: default: 32768 minimum: 301
[    0.271278] Security Framework initialized
[    0.275446] AppArmor: AppArmor initialized
[    0.279666] Mount-cache hash table entries: 1024 (order: 0, 4096 bytes)
[    0.286453] Mountpoint-cache hash table entries: 1024 (order: 0, 4096 bytes)
[    0.294722] Performance counters: mips/74K PMU enabled, 4 32-bit counters available to each CPU, irq 21
[    0.307648] devtmpfs: initialized
[    0.314160] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 7645041785100000 ns
[    0.324188] futex hash table entries: 256 (order: -1, 3072 bytes)
[    0.331318] NET: Registered protocol family 16
[    0.336414] console [avm0] enabled
[    0.340190] cpuidle: using governor ladder
[    0.344372] cpuidle: using governor menu
[    0.348386] Creating Config Table
[    0.351954] Enabling UART-Input for Pin 18
[    0.358969] MIPS: machine is AVM FritzRepeater 2400
[    0.363992] [avm_pmu] Set reg 18116cc4 to 0x00300000
[    0.370397] avm_check_cpu_features: mips-options: 0x40006d638b icache.flags 0x00000000 dcache.flags 0x00000004 isa_level 0x00000031 ases 00000051
[    0.384025] avm_alloc_page_extension node_extension_table[0] entries=32768 (size=131072)  alloced
[    0.393235] no support for hwid 241
[    0.396763] Reboot Status is: Power-On 
[    0.400762] [avmnet] [avmnet_cfg_init] initializing
[    0.406092] pstore: Registered ramoops as persistent store backend
[    0.412420] ramoops: attached 0x80000@0xf80000, ecc: 0/0
[    0.418141] [find_nmi_vector] no nmi vector found
[    0.427780] SCSI subsystem initialized
[    0.431826] usbcore: registered new interface driver usbfs
[    0.437486] usbcore: registered new interface driver hub
[    0.442957] usbcore: registered new device driver usb
[    0.747063] registering PCI controller with io_map_base unset
[    0.753080] PCI host bridge to bus 0000:00
[    0.757250] pci_bus 0000:00: root bus resource [mem 0x12000000-0x13ffffff]
[    0.764306] pci_bus 0000:00: root bus resource [io  0x0001]
[    0.770039] pci_bus 0000:00: root bus resource [??? 0x00000000 flags 0x0]
[    0.777028] pci_bus 0000:00: No busn resource found for root bus, will use [bus 00-ff]
[    0.785662] pci 0000:00:00.0: BAR 0: assigned [mem 0x12000000-0x121fffff 64bit]
[    0.793178] pci 0000:00:00.0: using irq 80 for pin 1
[    0.798828] AVM PA for Linux version 4.4.271 (kbuild-team@core.avm.de) (gcc version 5.5.0 (Buildroot 2020.02.1-g758ac3ed) ) #1 2023-10-06
[    0.798828]  (early init)
[    0.814681] clocksource: Switched to clocksource MIPS
[    0.820328] AppArmor: AppArmor Filesystem Enabled
[    0.827151] NET: Registered protocol family 2
[    0.832234] TCP established hash table entries: 1024 (order: 0, 4096 bytes)
[    0.839402] TCP bind hash table entries: 1024 (order: 0, 4096 bytes)
[    0.845908] TCP: Hash tables configured (established 1024 bind 1024)
[    0.852524] UDP hash table entries: 256 (order: 0, 4096 bytes)
[    0.858511] UDP-Lite hash table entries: 256 (order: 0, 4096 bytes)
[    0.865219] NET: Registered protocol family 1
[    0.870658] audit: initializing netlink subsys (disabled)
[    0.876284] audit: type=2000 audit(0.544:1): initialized
[    0.891190] squashfs: version 4.0 (2009/01/31) Phillip Lougher
[    0.897520] ANTFS Module: Version 2.53
[    0.901500] fuse init (API version 7.23)
[    0.907465] io scheduler noop registered
[    0.911500] io scheduler deadline registered (default)
[    0.921790] ttyS0 at MMIO 0x18020000 (irq = 19, base_baud = 1562500) is a PORT_16550A
[    0.930256] [avm_power]avm_power_pm_qos_init
[    0.934924] [loadcontrol] set auto - scale=1
[    0.939293] [avm] configured: watchdog event debug 
[    0.944500] Register push button event to receive the set_factory_kernel event
[    0.953033] AVM Simple Profiling enabled Version 3.0
[    0.958132] [simple-profiling]:4 performance counters implemented, OLD_34K
[    0.965170] AVM_WATCHDOG: Watchdog Driver for AR7 Hardware (Version 1.0)
[    0.972245] [ath:watchdog] activate nmi-mode
[    0.977094] avm_net_trace: Up and running.
[    0.981631] ath79_spi_fixup_mac_addr: No eth0 node in DT (-1)
[    0.987526] ath79_spi_fixup_mac_addr: Set local-mac-address failed for eth0 (-4)
[    0.995161] ath79_spi_fixup_mac_addr: No eth1 node in DT (-1)
[    1.001022] ath79_spi_fixup_mac_addr: Set local-mac-address failed for eth1 (-4)
[    1.009651] Registering ATH-flash-driver…
[    1.013983] [ath_flash] Use 4 byte addressing
[    1.050360] 6 avm_squashfs partitions found on MTD device ath-nor
[    1.056581] [TFFS3_Register_Panic_CB] registering panic callback for mtd ath-nor
[    1.064195] Creating 6 MTD partitions on „ath-nor“:
[    1.069222] 0x0000002dd000-0x000002000000 : „rootfs“
[    1.075539] [rootfs] use mtd0 (rootfs) as root
[    1.080126] mtdsplit: no squashfs found in „rootfs“
[    1.085099] 0x000000090000-0x0000002dd000 : „kernel“
[    1.091334] 0x000000000000-0x000000020000 : „urlader“
[    1.097602] 0x000000020000-0x000000090000 : „tffs (1)“
[    1.103994] 0x000002020000-0x000002090000 : „tffs (2)“
[    1.110359] 0x000002090000-0x000004000000 : „reserved-kernel“
[    1.117423] tun: Universal TUN/TAP device driver, 1.6
[    1.122604] tun: (C) 1999-2004 Max Krasnyansky <maxk@qualcomm.com>
[    1.129149] ehci_hcd: USB 2.0 ‚Enhanced‘ Host Controller (EHCI) Driver
[    1.135866] ehci-pci: EHCI PCI platform driver
[    1.140667] usbcore: registered new interface driver usblp
[    1.146344] usbcore: registered new interface driver usb-storage
[    1.152479] i2c /dev entries driver
[    1.156352] AVM PA 2.138.1.16-release_move21-move21 for Linux Linux version 4.4.271 (kbuild-team@core.avm.de) (gcc version 5.5.0 (Buildroot 2020.02.1-g758ac3ed) ) #1 2023-10-06
[    1.156352]  (late init)
[    1.175728] gre: GRE over IPv4 demultiplexor driver
[    1.181445] NET: Registered protocol family 10
[    1.187064] NET: Registered protocol family 17
[    1.191673] Bridge broadcast ratelimiter registered
[    1.196647] bridge: automatic filtering via arp/ip/ip6tables has been deprecated. Update your scripts to load br_netfilter if you need this.
[    1.209669] Bridge firewalling registered
[    1.213785] l2tp_core: L2TP core driver, V2.0
[    1.218243] l2tp_ip: L2TP IP encapsulation support (L2TPv3)
[    1.224018] l2tp_netlink: L2TP netlink interface
[    1.228761] l2tp_eth: L2TP ethernet pseudowire support (L2TPv3)
[    1.234817] l2tp_ip6: L2TP IP encapsulation support for IPv6 (L2TPv3)
[    1.241640] 8021q: 802.1Q VLAN Support v1.8
[    1.246062] [nmi] copy_nmi_trampoline done
[    1.251494] [TFFS3_Init] Called.
[    1.254794] [TFFS3_Init] No storage module registered, trying legacy fallback
[    1.262111] [TFFS3_CACHE_Configure] Setting up caching for backend legacy
[    1.269093] [TFFS3-CACHE] Caching module for TFFS 3.x
[    1.274294] [TFFS3_LGCY_Setup] using mtd3(tffs (1)), mtd4(tffs (2))
[    1.280750] [TFFS3_LGCY_Setup] mtd „tffs (1)“: segment value 8
[    1.286752] [TFFS3_LGCY_Setup] mtd „tffs (2)“: segment value 7
[    1.292749] [TFFS3_LGCY_Setup] Using segment 8 (avail: 8 + 7)
[    1.298661] [TFFS3_LGCY_Setup] mtd3 size=0x70000
[    1.305247] [TFFS_Cache] Allocate segement buffer cache (size=32784)
[    1.311772] tffs/panic: have_new_logentry: Error reading crashenv: -2
[    1.318368] tffs/panic: have_new_logentry: Error reading crashenv: -2
[    1.325136] TFFS: tiny flash file system driver. GPL (c) AVM Berlin (Version 3.0)
[    1.332846] Adam2 environment variables API installed.
[    1.341355] [avm_fair_share] change trip level 0 -> -1 for temp 26500
[    1.348201] lm75 0-0048: hwmon0: sensor ‚lm75‘
[    1.356486] i2c-gpio i2c@0: using pins 16 (SDA) and 17 (SCL)
[    1.362645] {avmnet_cfg_netinit}
[    1.365946] [avmnet] No config found for HWRev 241, HWSubRev 1, Profile-ID 0, trying base config for HWSubRev
[    1.376123] [avmnet] No config found for HWRev 241, HWSubRev 1, trying base config for HWRev
[    1.791872] [avmnet] [setup_phy] Giving up on hanging PHY ar8033 ID 0x0
[    1.798688] [avmnet_set_macaddr] Setup Mac Addr for Device(eth0): 0c:72:74:33:07:9d 
[    1.807389] CPU 0 Unable to handle kernel paging request at virtual address 00000000, epc == 00000000, ra == 80381b54
[    1.818317] PCI: int=00000000 aer=00000000 uer=00000000 cer=00000000 debug=00004111 mac_phy=0000884f phy_mac=03804ba4 err_cnt=00000000
[    1.830760] set_reboot_status: Soft-Reboot(KCRASH)  - KCRASH(1)SUM(1)UP(1)UTC(1)FW(07.58)HW(241)HWS(1)BV(1.11013)BN(111615)FS(07.58)BT(1)BD(0)
[    1.843920] Oops[#1]:
[    1.846219] CPU: 0 PID: 1 Comm: swapper Not tainted 4.4.271 #1
[    1.852233] task: 87c30000 ti: 87c34000 task.ti: 87c34000
[    1.857781] $ 0   : 00000000 00000000 00000000 00000000
[    1.863145] $ 4   : 87f1e800 87c37dac 00000000 00000004
[    1.868521] $ 8   : 80820000 000000ff 8081cc28 000005dc
[    1.873897] $12   : 00000000 00000000 00000000 00000000
[    1.879273] $16   : 00000000 80820000 8081cc28 8081cc28
[    1.884649] $20   : 8072ab80 00000001 00000002 00000003
[    1.890025] $24   : 00000002 00000000                  
[    1.895402] $28   : 87c34000 87c37d90 807ae354 80381b54
[    1.900777] Hi    : 00000096
[    1.903746] Lo    : 00000093
[    1.906702] Status: 1100dc03	KERNEL EXL IE 
[    1.910995] Cause : 00800008 exc_code:2 TLBL
[    1.915393] BadVA : 00000000
[    1.918341] epc   : 00000000   (null)
[    1.922145] ra    : 80381b54 0x80381b54 avmnet_mgmt_init+0x144/0x244
[    1.928654]     Not tainted
[    1.931521] PrId  : 00019750 (MIPS 74Kc)
[    1.935579] Classified pointer on registers:
[    1.939948]  $ 4 : 87f1e800 [slab: type:kmalloc-2048 size:2048 start:0x87f1e800+0x0]
[    1.947925]  $ 5 : 87c37dac [stack(swapper): 87c34000+0x3dac]
[    1.953846]  $ 8 : 80820000 pa_data+0xb90/0x478c0
[    1.958696]  $10 : 8081cc28 avmnet_mgmt+0x0/0xb0
[    1.963440]  $17 : 80820000 pa_data+0xb90/0x478c0
[    1.968264]  $18 : 8081cc28 avmnet_mgmt+0x0/0xb0
[    1.973012]  $19 : 8081cc28 avmnet_mgmt+0x0/0xb0
[    1.977768]  $20 : 8072ab80 avmnet_hw241_avm_device_0+0x0/0x2e0
[    1.983870]  $26 : 8072ab80 avmnet_hw241_avm_device_0+0x0/0x2e0
[    1.989955]  $27 : 87ed4800 [slab: type:kmalloc-256 size:256 start:0x87ed4800+0x0]
[    1.997743]  $28 : 87c34000 [threadinfo(swapper): 87c34000+0x0]
[    2.003835]  $29 : 87c37d90 [stack(swapper): 87c34000+0x3d90]
[    2.009758]  $30 : 807ae354 __initcall_avmnet_timer_init7+0x0/0x4
[    2.016025]  $31 : 80381b54 avmnet_mgmt_init+0x144/0x244
[    2.021479] Modules linked in:
[    2.024611] Process swapper (pid: 1, threadinfo=87c34000, task=87c30000, tls=00000000)
[    2.032769] Stack : 80820000 87ee2980 807ae354 80284acc 8072ab80 8072ab80 87ee2940 8072ab80
	  87ee2940 00000000 00000000 803768f0 87c94480 000000f1 8072aa40 87f1e800
	  00000001 00000001 00000000 8072aa40 80820000 80680000 000000f1 00000000
	  80728574 00000008 807b0000 80376d24 807b0000 000000f1 00000001 00000000
	  00000000 806664fc 80783250 87ec4e40 80376968 00000007 806d0000 00000000
	  …
[    2.069321] Classified pointer on stack:
[    2.073363] 80820000 pa_data+0xb90/0x478c0
[    2.077587] 87ee2980 [slab: type:kmalloc-64 size:64 start:0x87ee2980+0x0]
[    2.084567] 807ae354 __initcall_avmnet_timer_init7+0x0/0x4
[    2.090220] 80284acc snprintf+0x18/0x24
[    2.094153] 8072ab80 avmnet_hw241_avm_device_0+0x0/0x2e0
[    2.099628] 87ee2940 [slab: type:kmalloc-64 size:64 start:0x87ee2940+0x0]
[    2.106617] 803768f0 avmnet_create_netdevices+0x764/0x7dc
[    2.112167] 87c94480 [slab: type:kmalloc-96 size:96 start:0x87c94480+0x0]
[    2.119155] 8072aa40 avmnet_hw241+0x0/0x130
[    2.123459] 87f1e800 [slab: type:kmalloc-2048 size:2048 start:0x87f1e800+0x0]
[    2.130803] 8072aa40 avmnet_hw241+0x0/0x130
[    2.135105] 80680000 spi_nor_ids+0x77c/0xf60
[    2.139498] 80728574 avmnet_hw_config_table+0x18/0x64
[    2.144693] 80376d24 avmnet_cfg_netinit+0x3bc/0x40c
[    2.149722] 806664fc fops_fpuemu_stat+0x26228/0x37c84
[    2.154909] 80783250 ubi_init+0x0/0x344
[    2.158849] 87ec4e40 [slab: type:kmalloc-32 size:32 start:0x87ec4e40+0x0]
[    2.165833] 80376968 avmnet_cfg_netinit+0x0/0x40c
[    2.170690] 80768300 repair_env_string+0x0/0xa4
[    2.175341] 8006ec98 do_one_initcall+0x208/0x230
[    2.180078] 80180e5c proc_create_data+0xa0/0xcc
[    2.184737] 80376968 avmnet_cfg_netinit+0x0/0x40c
[    2.189593] 80790000 tmp_cmdline.43815+0x2f4/0x1000
[    2.194593] 80180b54 proc_register+0x2c/0x108
[    2.199080] 87c10c80 [slab: type:kmalloc-128 size:128 start:0x87c10c80+0x0]
[    2.206252] 806e3fa4 irq_desc+0x32a0/0x3330
[    2.210542] Call Trace:
[    2.213064] 3da0: [<80284acc>] 0x80284acc snprintf+0x18/0x24
[    2.218882] 3dc0: [<803768f0>] 0x803768f0 avmnet_create_netdevices+0x764/0x7dc
[    2.226318] 3e00: [<80376d24>] 0x80376d24 avmnet_cfg_netinit+0x3bc/0x40c
[    2.233216] 3e1c: [<80783250>] 0x80783250 ubi_init+0x0/0x344
[    2.239039] 3e24: [<80376968>] 0x80376968 avmnet_cfg_netinit+0x0/0x40c
[    2.245761] 3e34: [<80768300>] 0x80768300 repair_env_string+0x0/0xa4
[    2.252302] 3e38: [<8006ec98>] 0x8006ec98 do_one_initcall+0x208/0x230
[    2.258930] 3e40: [<80180e5c>] 0x80180e5c proc_create_data+0xa0/0xcc
[    2.265470] 3e44: [<80376968>] 0x80376968 avmnet_cfg_netinit+0x0/0x40c
[    2.272190] 3e50: [<80180b54>] 0x80180b54 proc_register+0x2c/0x108
[    2.278563] 3e68: [<800a2900>] 0x800a2900 parse_args+0x344/0x494
[    2.284740] 3e78: [<80770000>] 0x80770000 _gp+0x0/0x3f0
[    2.290112] 3ebc: [<80768300>] 0x80768300 repair_env_string+0x0/0xa4
[    2.296652] 3ec0: [<80768ee4>] 0x80768ee4 kernel_init_freeable+0x16c/0x230
[    2.303730] 3ee0: [<80768300>] 0x80768300 repair_env_string+0x0/0xa4
[    2.310284] 3f10: [<80069c74>] 0x80069c74 kernel_init+0x14/0x118
[    2.316455] 3f24: [<80069c60>] 0x80069c60 kernel_init+0x0/0x118
[    2.322546] 3f28: [<80060470>] 0x80060470 ret_from_kernel_thread+0x10/0x18
[    2.329620] 
[    2.331139] 
Code:
[    2.333103]  (Bad address in epc)
[    2.336693] 
[    2.338209] —[ end trace 1c02f0c0b7b185fa ]—
[    2.344765] Kernel panic - not syncing: Fatal exception 
[    2.351859] thermal_sys: thermal_zone0(package-thermal): 26500 Â°C
[    2.365328] Rebooting in 3 seconds..