(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "Hongfa HFD2/012-S-L2-D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "Hongfa HFD2/012-S-L2-D"
			(at 16.51 1.27 0)
		)
		(property "Footprint" ""
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://cdn-reichelt.de/documents/datenblatt/C300/DS_HFD2NEU.pdf"
			(at 0 -17.78 0)
		)
		(property "Description" "Subminiatur DIP Relay"
			(at 0 -12.7 0)
		)
		(property "ki_keywords" "HONGFA set-reset polarized"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Omron*G6AK*"
			(at 0 0 0)
		)
		(symbol "Hongfa HFD2/012-S-L2-D_0_0"
			(text "+"
				(at -12.065 2.667 0)
			)
			(text "+"
				(at -12.065 -2.413 0)
			)
			(text "S"
				(at -10.033 2.794 0)
			)
			(text "R"
				(at -10.033 -2.921 0)
			)
		)
		(symbol "Hongfa HFD2/012-S-L2-D_0_1")
		(symbol "Hongfa HFD2/012-S-L2-D_1_1"
			(pin passive line
				(at -12.7 7.62 270)
				(length 2.54)
				(name "~")
				(number "16")
			)
			(pin passive line
				(at -12.7 -7.62 90)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "15")
			)
			(pin passive line
				(at -7.62 -7.62 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "~")
				(number "13")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 6.35 7.62 270)
				(length 2.54)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at 6.35 -7.62 90)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 12.7 7.62 270)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 12.7 -7.62 90)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "_1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 0 0)
		)
		(property "Value" ""
			(at 0 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "_1_0_1")
		(symbol "_1_1_1"
			(pin input line
				(at -40.64 7.62 270)
				(length 2.54)
				(name "-")
				(number "16")
			)
			(pin input line
				(at -40.64 -7.62 90)
				(length 2.54)
				(name "+")
				(number "1")
			)
			(pin input line
				(at -35.56 7.62 270)
				(length 2.54)
				(name "-")
				(number "15")
			)
			(pin input line
				(at -35.56 -7.62 90)
				(length 2.54)
				(name "+")
				(number "2")
			)
			(pin input line
				(at -27.94 7.62 270)
				(length 2.54)
				(name "~")
				(number "13")
			)
			(pin input line
				(at -27.94 -7.62 90)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin output line
				(at -21.59 7.62 270)
				(length 2.54)
				(name "~")
				(number "11")
			)
			(pin output line
				(at -21.59 -7.62 90)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin output line
				(at -15.24 7.62 270)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin output line
				(at -15.24 -7.62 90)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "hongfa_hfd2/012-s-l2-d"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 0 0)
		)
		(property "Value" ""
			(at 0 0 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Omron_G6AK"
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "hongfa_hfd2/012-s-l2-d_0_1")
		(symbol "hongfa_hfd2/012-s-l2-d_1_1"
			(pin input line
				(at -40.64 7.62 270)
				(length 2.54)
				(name "-")
				(number "16")
			)
			(pin input line
				(at -40.64 -7.62 90)
				(length 2.54)
				(name "+")
				(number "1")
			)
			(pin input line
				(at -35.56 7.62 270)
				(length 2.54)
				(name "-")
				(number "15")
			)
			(pin input line
				(at -35.56 -7.62 90)
				(length 2.54)
				(name "+")
				(number "2")
			)
			(pin input line
				(at -27.94 7.62 270)
				(length 2.54)
				(name "~")
				(number "13")
			)
			(pin input line
				(at -27.94 -7.62 90)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin output line
				(at -21.59 7.62 270)
				(length 2.54)
				(name "~")
				(number "11")
			)
			(pin output line
				(at -21.59 -7.62 90)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin output line
				(at -15.24 7.62 270)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin output line
				(at -15.24 -7.62 90)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
)
