(kicad_sch
	(version 20250114)
	(generator "eeschema")
	(generator_version "9.0")
	(paper "A5" portrait)
	(title_block
		(title "RPi5 Advanced Power Button")
		(date "2026-02-02")
		(rev "0.08")
		(company "BL")
	)
	(lib_symbols
		(symbol "Connector_Generic:Conn_01x06"
			(pin_names
				(offset 1.016)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at 0 7.62 0)
			)
			(property "Value" "Conn_01x06"
				(at 0 -10.16 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)"
				(at 0 0 0)
			)
			(property "ki_keywords" "connector"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Connector*:*_1x??_*"
				(at 0 0 0)
			)
			(symbol "Conn_01x06_1_1"
				(rectangle
					(start -1.27 6.35)
					(end 1.27 -8.89)
					(fill
						(type background)
					)
				)
				(rectangle
					(start -1.27 5.207)
					(end 0 4.953)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 2.667)
					(end 0 2.413)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 0.127)
					(end 0 -0.127)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 -2.413)
					(end 0 -2.667)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 -4.953)
					(end 0 -5.207)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 -7.493)
					(end 0 -7.747)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at -5.08 5.08 0)
					(length 3.81)
					(name "Pin_1")
					(number "1")
				)
				(pin passive line
					(at -5.08 2.54 0)
					(length 3.81)
					(name "Pin_2")
					(number "2")
				)
				(pin passive line
					(at -5.08 0 0)
					(length 3.81)
					(name "Pin_3")
					(number "3")
				)
				(pin passive line
					(at -5.08 -2.54 0)
					(length 3.81)
					(name "Pin_4")
					(number "4")
				)
				(pin passive line
					(at -5.08 -5.08 0)
					(length 3.81)
					(name "Pin_5")
					(number "5")
				)
				(pin passive line
					(at -5.08 -7.62 0)
					(length 3.81)
					(name "Pin_6")
					(number "6")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Device:R"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 2.032 0 90)
			)
			(property "Value" "R"
				(at 0 0 90)
			)
			(property "Footprint" ""
				(at -1.778 0 90)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Resistor"
				(at 0 0 0)
			)
			(property "ki_keywords" "R res resistor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "R_*"
				(at 0 0 0)
			)
			(symbol "R_0_1"
				(rectangle
					(start -1.016 -2.54)
					(end 1.016 2.54)
					(fill
						(type none)
					)
				)
			)
			(symbol "R_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name "~")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Diode:1N4148"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "D"
				(at 0 2.54 0)
			)
			(property "Value" "1N4148"
				(at 0 -2.54 0)
			)
			(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
				(at 0 0 0)
			)
			(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/1N4148_1N4448.pdf"
				(at 0 0 0)
			)
			(property "Description" "100V 0.15A standard switching diode, DO-35"
				(at 0 0 0)
			)
			(property "Sim.Device" "D"
				(at 0 0 0)
			)
			(property "Sim.Pins" "1=K 2=A"
				(at 0 0 0)
			)
			(property "ki_keywords" "diode"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "D*DO?35*"
				(at 0 0 0)
			)
			(symbol "1N4148_0_1"
				(polyline
					(pts
						(xy -1.27 1.27) (xy -1.27 -1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 1.27) (xy 1.27 -1.27) (xy -1.27 0) (xy 1.27 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 0) (xy -1.27 0)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "1N4148_1_1"
				(pin passive line
					(at -3.81 0 0)
					(length 2.54)
					(name "K")
					(number "1")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 2.54)
					(name "A")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Diode:BZV55B3V3"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "D"
				(at 0 2.54 0)
			)
			(property "Value" "BZV55B3V3"
				(at 0 -2.54 0)
			)
			(property "Footprint" "Diode_SMD:D_MiniMELF"
				(at 0 -4.445 0)
			)
			(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
				(at 0 0 0)
			)
			(property "Description" "3.3V, 500mW, 2%, Zener diode, MiniMELF"
				(at 0 0 0)
			)
			(property "ki_keywords" "zener diode"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "D*MiniMELF*"
				(at 0 0 0)
			)
			(symbol "BZV55B3V3_0_1"
				(polyline
					(pts
						(xy -1.27 -1.27) (xy -1.27 1.27) (xy -0.762 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 0) (xy -1.27 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 -1.27) (xy 1.27 1.27) (xy -1.27 0) (xy 1.27 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "BZV55B3V3_1_1"
				(pin passive line
					(at -3.81 0 0)
					(length 2.54)
					(name "K")
					(number "1")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 2.54)
					(name "A")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Interface_Optical:TSOP45xx"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at -10.16 7.62 0)
			)
			(property "Value" "TSOP45xx"
				(at -10.16 -7.62 0)
			)
			(property "Footprint" "OptoDevice:Vishay_MOLD-3Pin"
				(at -1.27 -9.525 0)
			)
			(property "Datasheet" "http://www.vishay.com/docs/82460/tsop45.pdf"
				(at 16.51 7.62 0)
			)
			(property "Description" "IR Receiver Modules for Remote Control Systems"
				(at 0 0 0)
			)
			(property "ki_keywords" "opto IR receiver"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Vishay*MOLD*"
				(at 0 0 0)
			)
			(symbol "TSOP45xx_0_0"
				(arc
					(start -10.287 -1.778)
					(mid -11.0899 -0.1905)
					(end -10.287 1.397)
					(fill
						(type background)
					)
				)
				(polyline
					(pts
						(xy 1.905 5.08) (xy 0.127 5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.905 -5.08) (xy 0.127 -5.08)
					)
					(fill
						(type none)
					)
				)
				(text "DEMOD"
					(at -3.175 0.254 900)
				)
			)
			(symbol "TSOP45xx_0_1"
				(polyline
					(pts
						(xy -8.763 0.381) (xy -9.652 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -8.763 0.381) (xy -9.271 0.381)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -8.763 0.381) (xy -8.763 0.889)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -8.636 -0.635) (xy -9.525 0.254)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -8.636 -0.635) (xy -9.144 -0.635)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -8.636 -0.635) (xy -8.636 -0.127)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -8.382 0.635) (xy -6.731 0.635) (xy -7.62 -1.016) (xy -8.382 0.635)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy -8.382 -1.016) (xy -6.731 -1.016)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -6.096 5.588)
					(end 0.127 -5.588)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -6.096 1.397) (xy -7.62 1.397) (xy -7.62 -1.778) (xy -6.096 -1.778)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 -1.905) (xy 1.27 -3.81)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 -2.54) (xy 1.905 -1.905) (xy 1.905 0) (xy 2.54 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 -2.921) (xy 0.127 -2.921)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 -3.175) (xy 1.905 -3.81) (xy 1.905 -5.08) (xy 2.54 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.397 -3.556) (xy 1.524 -3.556)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.651 -3.556) (xy 1.524 -3.556)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.651 -3.556) (xy 1.651 -3.302)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.905 4.445) (xy 1.905 5.08) (xy 2.54 5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.905 0) (xy 1.905 1.27)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 2.54 1.27)
					(end 1.27 4.445)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 7.62 6.35)
					(end -10.16 -6.35)
					(fill
						(type background)
					)
				)
			)
			(symbol "TSOP45xx_1_1"
				(pin power_in line
					(at 10.16 5.08 180)
					(length 2.54)
					(name "Vs")
					(number "3")
				)
				(pin output line
					(at 10.16 0 180)
					(length 2.54)
					(name "OUT")
					(number "1")
				)
				(pin power_in line
					(at 10.16 -5.08 180)
					(length 2.54)
					(name "GND")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "MCU_Microchip_ATtiny:ATtiny412-SS"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at -12.7 13.97 0)
			)
			(property "Value" "ATtiny412-SS"
				(at 2.54 -13.97 0)
			)
			(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
				(at 0 0 0)
			)
			(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001911A.pdf"
				(at 0 0 0)
			)
			(property "Description" "20MHz, 4kB Flash, 256B SRAM, 128B EEPROM, SOIC-8"
				(at 0 0 0)
			)
			(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
				(at 0 0 0)
			)
			(symbol "ATtiny412-SS_0_1"
				(rectangle
					(start -12.7 -12.7)
					(end 12.7 12.7)
					(fill
						(type background)
					)
				)
			)
			(symbol "ATtiny412-SS_1_1"
				(pin power_in line
					(at 0 15.24 270)
					(length 2.54)
					(name "VCC")
					(number "1")
				)
				(pin power_in line
					(at 0 -15.24 90)
					(length 2.54)
					(name "GND")
					(number "8")
				)
				(pin bidirectional line
					(at 15.24 7.62 180)
					(length 2.54)
					(name "~{RESET}/PA0")
					(number "6")
				)
				(pin bidirectional line
					(at 15.24 5.08 180)
					(length 2.54)
					(name "PA1")
					(number "4")
				)
				(pin bidirectional line
					(at 15.24 2.54 180)
					(length 2.54)
					(name "PA2")
					(number "5")
				)
				(pin bidirectional line
					(at 15.24 0 180)
					(length 2.54)
					(name "PA3")
					(number "7")
				)
				(pin bidirectional line
					(at 15.24 -2.54 180)
					(length 2.54)
					(name "PA6")
					(number "2")
				)
				(pin bidirectional line
					(at 15.24 -5.08 180)
					(length 2.54)
					(name "PA7")
					(number "3")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Switch:SW_Push_LED"
			(pin_names
				(offset 1.016)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "SW"
				(at 0 7.62 0)
			)
			(property "Value" "SW_Push_LED"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 7.62 0)
			)
			(property "Datasheet" "~"
				(at 0 7.62 0)
			)
			(property "Description" "Push button switch with LED, generic"
				(at 0 0 0)
			)
			(property "ki_keywords" "switch normally-open pushbutton push-button LED"
				(at 0 0 0)
			)
			(symbol "SW_Push_LED_0_0"
				(polyline
					(pts
						(xy -2.54 0) (xy 2.54 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.286 -1.524) (xy -2.286 -2.159) (xy -1.651 -2.159)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.286 -2.159) (xy -1.016 -0.889)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.016 -1.524) (xy -1.016 -2.159) (xy -0.381 -2.159)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.016 -2.159) (xy 0.254 -0.889)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.635 1.27) (xy -0.635 -1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.635 0) (xy 1.27 1.27) (xy 1.27 -1.27) (xy -0.635 0)
					)
					(fill
						(type outline)
					)
				)
			)
			(symbol "SW_Push_LED_0_1"
				(circle
					(center -2.032 2.54)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 3.81) (xy 0 5.588)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 2.032 2.54)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.54 3.81) (xy -2.54 3.81)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at -5.08 2.54 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at -5.08 0 0)
					(length 2.54)
					(name "K")
					(number "3")
				)
				(pin passive line
					(at 5.08 2.54 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
				(pin passive line
					(at 5.08 0 180)
					(length 2.54)
					(name "A")
					(number "4")
				)
			)
			(symbol "SW_Push_LED_1_1"
				(rectangle
					(start -3.175 5.715)
					(end 3.175 -2.54)
					(fill
						(type background)
					)
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:+3.3V"
			(power)
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -3.81 0)
			)
			(property "Value" "+3.3V"
				(at 0 3.556 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"+3.3V\""
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "+3.3V_0_1"
				(polyline
					(pts
						(xy -0.762 1.27) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 2.54) (xy 0.762 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "+3.3V_1_1"
				(pin power_in line
					(at 0 0 90)
					(length 0)
					(name "~")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:+5V"
			(power)
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -3.81 0)
			)
			(property "Value" "+5V"
				(at 0 3.556 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"+5V\""
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "+5V_0_1"
				(polyline
					(pts
						(xy -0.762 1.27) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 2.54) (xy 0.762 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "+5V_1_1"
				(pin power_in line
					(at 0 0 90)
					(length 0)
					(name "~")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:GND"
			(power)
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "GND"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "GND_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GND_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(name "~")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
	)
	(text "1 | +5V (Allways has +5v)\n2 | +3.3V (Low when RPi5 is powered off)\n3 | GND\n4 | GPIO Output (Set high by Python script)\n5 | GPIO input (IR receiver)\n6 | Power button (Pins next to RTC connector)"
		(exclude_from_sim no)
		(at 79.248 65.278 0)
	)
	(junction
		(at 66.04 110.49)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 46.99 66.04)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 45.72 40.64)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 102.87 34.29)
		(diameter 0)
		(color 0 0 0 0)
	)
	(wire
		(pts
			(xy 54.61 132.08) (xy 66.04 132.08)
		)
	)
	(wire
		(pts
			(xy 46.99 66.04) (xy 46.99 67.31)
		)
	)
	(wire
		(pts
			(xy 54.61 134.62) (xy 88.9 134.62)
		)
	)
	(wire
		(pts
			(xy 97.79 132.08) (xy 99.06 132.08)
		)
	)
	(wire
		(pts
			(xy 66.04 86.36) (xy 85.09 86.36)
		)
	)
	(wire
		(pts
			(xy 102.87 34.29) (xy 102.87 35.56)
		)
	)
	(wire
		(pts
			(xy 66.04 66.04) (xy 66.04 86.36)
		)
	)
	(wire
		(pts
			(xy 54.61 40.64) (xy 68.58 40.64)
		)
	)
	(wire
		(pts
			(xy 62.23 137.16) (xy 54.61 137.16)
		)
	)
	(wire
		(pts
			(xy 96.52 134.62) (xy 99.06 134.62)
		)
	)
	(wire
		(pts
			(xy 66.04 88.9) (xy 66.04 96.52)
		)
	)
	(wire
		(pts
			(xy 66.04 88.9) (xy 85.09 88.9)
		)
	)
	(wire
		(pts
			(xy 55.88 66.04) (xy 66.04 66.04)
		)
	)
	(wire
		(pts
			(xy 62.23 142.24) (xy 54.61 142.24)
		)
	)
	(wire
		(pts
			(xy 46.99 66.04) (xy 48.26 66.04)
		)
	)
	(wire
		(pts
			(xy 62.23 139.7) (xy 54.61 139.7)
		)
	)
	(wire
		(pts
			(xy 44.45 40.64) (xy 45.72 40.64)
		)
	)
	(wire
		(pts
			(xy 66.04 110.49) (xy 87.63 110.49)
		)
	)
	(wire
		(pts
			(xy 102.87 34.29) (xy 104.14 34.29)
		)
	)
	(wire
		(pts
			(xy 97.79 129.54) (xy 97.79 132.08)
		)
	)
	(wire
		(pts
			(xy 68.58 81.28) (xy 85.09 81.28)
		)
	)
	(wire
		(pts
			(xy 68.58 40.64) (xy 68.58 81.28)
		)
	)
	(wire
		(pts
			(xy 54.61 129.54) (xy 88.9 129.54)
		)
	)
	(wire
		(pts
			(xy 96.52 129.54) (xy 97.79 129.54)
		)
	)
	(wire
		(pts
			(xy 45.72 40.64) (xy 45.72 41.91)
		)
	)
	(wire
		(pts
			(xy 66.04 110.49) (xy 66.04 132.08)
		)
	)
	(wire
		(pts
			(xy 45.72 66.04) (xy 46.99 66.04)
		)
	)
	(wire
		(pts
			(xy 54.61 91.44) (xy 85.09 91.44)
		)
	)
	(wire
		(pts
			(xy 102.87 33.02) (xy 102.87 34.29)
		)
	)
	(wire
		(pts
			(xy 45.72 40.64) (xy 46.99 40.64)
		)
	)
	(wire
		(pts
			(xy 66.04 104.14) (xy 66.04 110.49)
		)
	)
	(global_label "RPi5 power state"
		(shape input)
		(at 44.45 40.64 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 24.9549 40.64 0)
		)
	)
	(global_label "RPi5 power state"
		(shape input)
		(at 62.23 139.7 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 81.7251 139.7 0)
		)
	)
	(global_label "RPI5 ready state"
		(shape input)
		(at 62.23 142.24 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 81.3622 142.24 0)
		)
	)
	(global_label "RPI5 ready state"
		(shape input)
		(at 45.72 66.04 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 26.5878 66.04 0)
		)
	)
	(global_label "RPi5 power button"
		(shape input)
		(at 62.23 137.16 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 83.0554 137.16 0)
		)
	)
	(global_label "RPi5 power button"
		(shape input)
		(at 46.99 91.44 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 26.1646 91.44 0)
		)
	)
	(symbol
		(lib_id "power:+3.3V")
		(at 39.37 121.92 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR07"
			(at 39.37 125.73 0)
		)
		(property "Value" "+3.3V"
			(at 39.37 116.84 0)
		)
		(property "Footprint" ""
			(at 39.37 121.92 0)
		)
		(property "Datasheet" ""
			(at 39.37 121.92 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+3.3V\""
			(at 39.37 121.92 0)
		)
		(pin "1")
		(instances
			(project "RPi5 Advanced Power Button"
				(path
					(reference "#PWR07")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "MCU_Microchip_ATtiny:ATtiny412-SS")
		(at 39.37 137.16 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "U2"
			(at 39.37 137.16 0)
		)
		(property "Value" "ATtiny412-SS"
			(at 39.37 141.224 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 39.37 137.16 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001911A.pdf"
			(at 39.37 137.16 0)
		)
		(property "Description" "20MHz, 4kB Flash, 256B SRAM, 128B EEPROM, SOIC-8"
			(at 39.37 137.16 0)
		)
		(pin "6")
		(pin "2")
		(pin "8")
		(pin "3")
		(pin "1")
		(pin "5")
		(pin "4")
		(pin "7")
		(instances
			(project ""
				(path
					(reference "U2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 85.09 83.82 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR011"
			(at 78.74 83.82 0)
		)
		(property "Value" "GND"
			(at 81.28 83.8199 90)
		)
		(property "Footprint" ""
			(at 85.09 83.82 0)
		)
		(property "Datasheet" ""
			(at 85.09 83.82 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 85.09 83.82 0)
		)
		(pin "1")
		(instances
			(project "RPi5 Advanced Power Button"
				(path
					(reference "#PWR011")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 109.22 132.08 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR02"
			(at 115.57 132.08 0)
		)
		(property "Value" "GND"
			(at 113.03 132.0799 90)
		)
		(property "Footprint" ""
			(at 109.22 132.08 0)
		)
		(property "Datasheet" ""
			(at 109.22 132.08 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 109.22 132.08 0)
		)
		(pin "1")
		(instances
			(project "RPi5 Advanced Power Button"
				(path
					(reference "#PWR02")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 46.99 71.12 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R6"
			(at 49.53 69.8499 0)
		)
		(property "Value" "10K"
			(at 49.53 72.3899 0)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 48.768 71.12 90)
		)
		(property "Datasheet" "~"
			(at 46.99 71.12 0)
		)
		(property "Description" "Resistor"
			(at 46.99 71.12 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "RPi5 Advanced Power Button"
				(path
					(reference "R6")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:+3.3V")
		(at 104.14 34.29 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR05"
			(at 100.33 34.29 0)
		)
		(property "Value" "+3.3V"
			(at 107.95 34.2899 90)
		)
		(property "Footprint" ""
			(at 104.14 34.29 0)
		)
		(property "Datasheet" ""
			(at 104.14 34.29 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+3.3V\""
			(at 104.14 34.29 0)
		)
		(pin "1")
		(instances
			(project "RPi5 Advanced Power Button v0.08"
				(path
					(reference "#PWR05")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 52.07 66.04 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R5"
			(at 52.07 59.69 90)
		)
		(property "Value" "1K"
			(at 52.07 62.23 90)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 52.07 67.818 90)
		)
		(property "Datasheet" "~"
			(at 52.07 66.04 0)
		)
		(property "Description" "Resistor"
			(at 52.07 66.04 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "RPi5 Advanced Power Button"
				(path
					(reference "R5")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 92.71 129.54 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R1"
			(at 92.71 123.19 90)
		)
		(property "Value" "36K"
			(at 92.71 125.73 90)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 92.71 127.762 90)
		)
		(property "Datasheet" "~"
			(at 92.71 129.54 0)
		)
		(property "Description" "Resistor"
			(at 92.71 129.54 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "RPi5 Advanced Power Button"
				(path
					(reference "R1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 39.37 152.4 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR03"
			(at 39.37 158.75 0)
		)
		(property "Value" "GND"
			(at 39.37 157.48 0)
		)
		(property "Footprint" ""
			(at 39.37 152.4 0)
		)
		(property "Datasheet" ""
			(at 39.37 152.4 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 39.37 152.4 0)
		)
		(pin "1")
		(instances
			(project "RPi5 Advanced Power Button"
				(path
					(reference "#PWR03")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 45.72 49.53 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR06"
			(at 45.72 55.88 0)
		)
		(property "Value" "GND"
			(at 45.72 54.61 0)
		)
		(property "Footprint" ""
			(at 45.72 49.53 0)
		)
		(property "Datasheet" ""
			(at 45.72 49.53 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 45.72 49.53 0)
		)
		(pin "1")
		(instances
			(project "RPi5 Advanced Power Button"
				(path
					(reference "#PWR06")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 92.71 134.62 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R2"
			(at 92.71 138.43 90)
		)
		(property "Value" "200"
			(at 92.71 140.97 90)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 92.71 132.842 90)
		)
		(property "Datasheet" "~"
			(at 92.71 134.62 0)
		)
		(property "Description" "Resistor"
			(at 92.71 134.62 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "RPi5 Advanced Power Button"
				(path
					(reference "R2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 102.87 29.21 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R8"
			(at 105.41 27.9399 0)
		)
		(property "Value" "150"
			(at 105.41 30.4799 0)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 101.092 29.21 90)
		)
		(property "Datasheet" "~"
			(at 102.87 29.21 0)
		)
		(property "Description" "Resistor"
			(at 102.87 29.21 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "RPi5 Advanced Power Button v0.08"
				(path
					(reference "R8")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 102.87 43.18 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR09"
			(at 102.87 49.53 0)
		)
		(property "Value" "GND"
			(at 102.87 48.26 0)
		)
		(property "Footprint" ""
			(at 102.87 43.18 0)
		)
		(property "Datasheet" ""
			(at 102.87 43.18 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 102.87 43.18 0)
		)
		(pin "1")
		(instances
			(project "RPi5 Advanced Power Button v0.08"
				(path
					(reference "#PWR09")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 50.8 91.44 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R7"
			(at 50.8 85.09 90)
		)
		(property "Value" "1K"
			(at 50.8 87.63 90)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 50.8 93.218 90)
		)
		(property "Datasheet" "~"
			(at 50.8 91.44 0)
		)
		(property "Description" "Resistor"
			(at 50.8 91.44 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "RPi5 Advanced Power Button"
				(path
					(reference "R7")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:+3.3V")
		(at 87.63 115.57 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR010"
			(at 91.44 115.57 0)
		)
		(property "Value" "+3.3V"
			(at 83.82 115.5699 90)
		)
		(property "Footprint" ""
			(at 87.63 115.57 0)
		)
		(property "Datasheet" ""
			(at 87.63 115.57 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+3.3V\""
			(at 87.63 115.57 0)
		)
		(pin "1")
		(instances
			(project "RPi5 Advanced Power Button v5"
				(path
					(reference "#PWR010")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Interface_Optical:TSOP45xx")
		(at 97.79 110.49 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U1"
			(at 110.49 109.2199 0)
		)
		(property "Value" "TSOP4838"
			(at 110.49 111.7599 0)
		)
		(property "Footprint" "OptoDevice:Vishay_MOLD-3Pin"
			(at 99.06 100.965 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/82460/tsop45.pdf"
			(at 81.28 118.11 0)
		)
		(property "Description" "IR Receiver Modules for Remote Control Systems"
			(at 97.79 110.49 0)
		)
		(pin "1")
		(pin "3")
		(pin "2")
		(instances
			(project ""
				(path
					(reference "U1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 45.72 45.72 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R4"
			(at 48.26 44.4499 0)
		)
		(property "Value" "10K"
			(at 48.26 46.9899 0)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 47.498 45.72 90)
		)
		(property "Datasheet" "~"
			(at 45.72 45.72 0)
		)
		(property "Description" "Resistor"
			(at 45.72 45.72 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "RPi5 Advanced Power Button"
				(path
					(reference "R4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector_Generic:Conn_01x06")
		(at 90.17 83.82 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "J2"
			(at 92.71 83.8199 0)
		)
		(property "Value" "To/from RPi5"
			(at 92.71 86.3599 0)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical"
			(at 90.17 83.82 0)
		)
		(property "Datasheet" "~"
			(at 90.17 83.82 0)
		)
		(property "Description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 90.17 83.82 0)
		)
		(pin "1")
		(pin "3")
		(pin "2")
		(pin "4")
		(pin "6")
		(pin "5")
		(instances
			(project ""
				(path
					(reference "J2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 87.63 105.41 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR08"
			(at 81.28 105.41 0)
		)
		(property "Value" "GND"
			(at 83.82 105.4099 90)
		)
		(property "Footprint" ""
			(at 87.63 105.41 0)
		)
		(property "Datasheet" ""
			(at 87.63 105.41 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 87.63 105.41 0)
		)
		(pin "1")
		(instances
			(project "RPi5 Advanced Power Button v5"
				(path
					(reference "#PWR08")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:+5V")
		(at 102.87 25.4 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR04"
			(at 102.87 29.21 0)
		)
		(property "Value" "+5V"
			(at 102.87 20.32 0)
		)
		(property "Footprint" ""
			(at 102.87 25.4 0)
		)
		(property "Datasheet" ""
			(at 102.87 25.4 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+5V\""
			(at 102.87 25.4 0)
		)
		(pin "1")
		(instances
			(project "RPi5 Advanced Power Button v0.08"
				(path
					(reference "#PWR04")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 50.8 40.64 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R3"
			(at 50.8 34.29 90)
		)
		(property "Value" "1K"
			(at 50.8 36.83 90)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 50.8 42.418 90)
		)
		(property "Datasheet" "~"
			(at 50.8 40.64 0)
		)
		(property "Description" "Resistor"
			(at 50.8 40.64 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "RPi5 Advanced Power Button"
				(path
					(reference "R3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4148")
		(at 66.04 100.33 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D2"
			(at 68.58 99.0599 90)
		)
		(property "Value" "1N4148"
			(at 68.58 101.5999 90)
		)
		(property "Footprint" "Diode_THT:D_T-1_P5.08mm_Horizontal"
			(at 66.04 100.33 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/1N4148_1N4448.pdf"
			(at 66.04 100.33 0)
		)
		(property "Description" "100V 0.15A standard switching diode, DO-35"
			(at 66.04 100.33 0)
		)
		(property "Sim.Device" "D"
			(at 66.04 100.33 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 66.04 100.33 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "RPi5 Advanced Power Button v5"
				(path
					(reference "D2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 109.22 134.62 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01"
			(at 115.57 134.62 0)
		)
		(property "Value" "GND"
			(at 113.03 134.6199 90)
		)
		(property "Footprint" ""
			(at 109.22 134.62 0)
		)
		(property "Datasheet" ""
			(at 109.22 134.62 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 109.22 134.62 0)
		)
		(pin "1")
		(instances
			(project ""
				(path
					(reference "#PWR01")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:+5V")
		(at 85.09 78.74 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR015"
			(at 88.9 78.74 0)
		)
		(property "Value" "+5V"
			(at 81.28 78.7399 90)
		)
		(property "Footprint" ""
			(at 85.09 78.74 0)
		)
		(property "Datasheet" ""
			(at 85.09 78.74 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+5V\""
			(at 85.09 78.74 0)
		)
		(pin "1")
		(instances
			(project "RPi5 Advanced Power Button v0.05"
				(path
					(reference "#PWR015")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:BZV55B3V3")
		(at 102.87 39.37 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D1"
			(at 105.41 38.0999 90)
		)
		(property "Value" "BZX55C3V3"
			(at 105.41 40.6399 90)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 98.425 39.37 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 102.87 39.37 0)
		)
		(property "Description" "3.3V, 500mW, 2%, Zener diode, MiniMELF"
			(at 102.87 39.37 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project ""
				(path
					(reference "D1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 46.99 74.93 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR012"
			(at 46.99 81.28 0)
		)
		(property "Value" "GND"
			(at 46.99 80.01 0)
		)
		(property "Footprint" ""
			(at 46.99 74.93 0)
		)
		(property "Datasheet" ""
			(at 46.99 74.93 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 46.99 74.93 0)
		)
		(pin "1")
		(instances
			(project "RPi5 Advanced Power Button"
				(path
					(reference "#PWR012")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Switch:SW_Push_LED")
		(at 104.14 134.62 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "SW1"
			(at 104.14 142.24 0)
		)
		(property "Value" "SW_Push_LED"
			(at 104.14 139.7 0)
		)
		(property "Footprint" "Button_12x12Led:SW_12x12_Led"
			(at 104.14 127 0)
		)
		(property "Datasheet" "~"
			(at 104.14 127 0)
		)
		(property "Description" "Push button switch with LED, generic"
			(at 104.14 134.62 0)
		)
		(pin "1")
		(pin "3")
		(pin "4")
		(pin "2")
		(instances
			(project ""
				(path
					(reference "SW1")
					(unit 1)
				)
			)
		)
	)
	(sheet_instances
		(path
			(page "1")
		)
	)
	(embedded_fonts no)
)
