# # # # # # # # # # # # KomBoard Version File # # # # # # # # # # # #


# # # # # # # # # # # # # # # # # # # # # # # # # # #
Version: SW_4_11 #
# # # # # # # # # # # # # # # # # # # # # # # # # # #
Date: 29/04/2013

changes:
     - Real-time clock is used and can be set via the menu.
     - Pop-up menu when the system time is not set.
     - Pop-up menu Date / time added. It is always performed when a valid time is not set.
     - BUG - Fixed S0-Input/Output
     - Events with explicit event code is shown as "Event code: xxx"
     - IP addresses are now displayed without leading zeros (instead of 192.168.001.001 now 192.168.1.1)
     - Popup Menu update failed / successful must now be confirmed. (After 1 hr. KomBoard the reboot automatically)
     - Fixed minor BUGs (eg communication portal, menu display update process)


# # # # # # # # # # # # # # # # # # # #
Version: SW_04_09 #
# # # # # # # # # # # # # # # # # # # #
Date: 01.10.2012

changes:
    - The RS485 address is now updated on the web when it is changed in the menu.
    - The update process is now correctly displayed in the display
    - Corrected an error in the total Yield when performimg an update or restoring 
      to factory settings
    - Added support of the update process to older versions -
    - Changed default ISP for GSM modem (kostal.ic.t-mobile)

# # # # # # # # # # # # # # # # # # # #
Version: SW_04_08 #
# # # # # # # # # # # # # # # # # # # #
Date: 25.09.2012

Changes:
   - An update now displays the following information with an hourglass:
     "Receive Update", "Update is processed", "Update successful", "update failed"
   - Added ID for GSM modem UNSGSM V2.1
   - IP addresses are displayed without leading 0


# # # # # # # # # # # # # # # # # # # #
Version: SW_04_07 #
# # # # # # # # # # # # # # # # # # # #
Date: 08/21/2012

Changes:
   - System time to update no longer set to 2356959646th
     Has a KB before updating this value or greater, the system time is set to 0.


# # # # # # # # # # # # # # # # # # # #
Version: SW_04_06 #
# # # # # # # # # # # # # # # # # # # #
Date: 08/03/2012

Changes:
   - New "Select Country" menu
   - Implemented security question regarding Country again -
   - Portal Menu added
   - In most settings menus are now "accept" button instead of the "ok" button.
     That the value is only accepted but nciht more directly jump back one level.
     Confirm after the system automatically switches to de "back" button.
   - ZWR 485 - address only the 255 possible


# # # # # # # # # # # # # # # # # # # #
Version: SW_04_05 #
# # # # # # # # # # # # # # # # # # # #
Date: 06/19/2012

Changes:
   - IGAK: Automatic Address
   - HMI texts completed
   - Verdana font 10x12 lowercase modeled on the capital letter


# # # # # # # # # # # # # # # # # # # #
Version: SW_04_04 #
# # # # # # # # # # # # # # # # # # # #
Date: 06/04/2012 CB

Changes:
   - Battery access functions implemented
   - Fix: Send KB1 KB2 on router
   - Zertifkatsmenü implemented and fully tested
   - Address assignment IGAK optimized
   - Optimized data handling IGAK
   - Fix demo mode: Constant power mode now works correctly for 3 phases
   - Locale reset now possible with Instalateur password
   - IGAK addressing and retrieval implemented
   - Amended text in Auto-IP Auto IP / DHCP -
   - CCIDs modem with a length of 18-20 are now allowed
   - Heating control menu
   - Bugfix for GSM connectivity issues -
   - Data exchange KB2 -> EM_TYP2 (CAN / CANopen) implemented.
   - Battery data handling implemented.
   - Added memory alternating ass judge menu.
   - Improved software update module.
   - GSM modem hardware improves recognition.


# # # # # # # # # # # # # # # # # # # #
Version: SW_04_03 #
# # # # # # # # # # # # # # # # # # # #
Date: 14/03/2012

Change:
   - Added menu for Lichtbogendedektion -
   - Dynamic scaling of display values
   - Eigenverbraussteuerung implemented
   - New password is entered in the service (now contains a user ID and password password level)
   - Optimization of probes
   - Adaptation of the data ZWR
   - Screen saver is deactivated in error
   - Languages ??now fully supported
   - Removed temporarily DC display the main menu -
   - AFD module release version implemented
   - Error implemented new menu
   - Error codes implemented new menu
   - Status display new menu implemented
   - Added menu for event messages -


# # # # # # # # # # # # # # # # # # # #
Version: SW_04_02 #
# # # # # # # # # # # # # # # # # # # #
Date: 01.02.2012

Change:
   - Bugfix regarding Bonjour / MDNS / dnssd
   - Power reduction for ZWR
   - Added debug counters for POR, power reduction and RSE (count of times sent to control unit)
   - Added support KB1 the permissions -.
   - Arc Detection optimizes visualization
   - Removed ads performance optimization for ZWR -
   - IGAK address assignment implemented
   - Visualization of events in the Web server
   - Ripple control signal detection for central inverters (including variable time of signal detection)
   - Software update for ZWR (control / regulation)
   - Workaround for time jumps in the log data
   - Fix: RS485 driver, VarDat
   - Reading of the ripple control signals from the control of the ZWR
   - Added heating control for central inverters -
   - Optimization of event security at the RS485 interface improves
   - Event Manager and Data Xchange service modules added
   - Improved IGAK module


# # # # # # # # # # # # # # # # # # # #
Version: SW_04_01 #
# # # # # # # # # # # # # # # # # # # #

Date: 15/09/2011

Changes:
- Maximum limited to transfer records to the portal per connection -
- Timeout for HTTP server, SOAP server and WSC increased Connections
- Fixed bug in Software Update Service -
- Save Log-muted
- Optimized interface
- Buttons in the SWR optimized
- Menu fan test last updated
- Network drivers adjusted.
- HW-/SW - Version transmission (portal)
- With LED control optimized (no false flash)



# # # # # # # # # # # # # # # # # # # #
Version: SW_04_00 #
# # # # # # # # # # # # # # # # # # # #

Date: 28/06/2011

Changes:
   - Initial Release

