(kicad_pcb
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(4 "In1.Cu" signal)
		(6 "In2.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "prepreg")
				(thickness 0.1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In1.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 2"
				(type "core")
				(thickness 1.24)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In2.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 3"
				(type "prepreg")
				(thickness 0.1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints yes)
		)
		(pad_to_mask_clearance 0)
		(solder_mask_min_width 0.1)
		(allow_soldermask_bridges_in_footprints no)
		(tenting
			(front yes)
			(back yes)
		)
		(covering
			(front no)
			(back no)
		)
		(plugging
			(front no)
			(back no)
		)
		(capping no)
		(filling no)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12)
			(dashed_line_gap_ratio 3)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "./")
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 188.2917 109.7883)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R25"
			(at 0.7283 1.6517 0)
			(layer "F.SilkS")
		)
		(property "Value" "1kΩ"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "/RIGHT_DIR")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(U4-PH{slash}IN2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 187.3742 103.5083)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing)")
		(tags "capacitor")
		(property "Reference" "C6"
			(at 0 -1.68 0)
			(layer "F.SilkS")
		)
		(property "Value" "100 nF"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/FOLD_IN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 177.9792 86.3508)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R23"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "1kΩ"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "/LEFT_SLEEP")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(U3-nSLEEP)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 195.4667 114.8833 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R19"
			(at 0 -1.43 270)
			(layer "F.SilkS")
		)
		(property "Value" "22 kΩ"
			(at 0 1.43 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(U4-VREF)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 187.9667 82.6958 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R17"
			(at 0 -1.43 270)
			(layer "F.SilkS")
		)
		(property "Value" "22 kΩ"
			(at 0 1.43 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(U3-VREF)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 192.1542 105.0083 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C18"
			(at 0 -1.43 180)
			(layer "F.SilkS")
		)
		(property "Value" "22 nF"
			(at 0 1.43 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(U4-CPL)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.00mm"
		(layer "F.Cu")
		(at 168.161795 74.551061)
		(descr "CP, Radial series, Radial, pin pitch=2.00mm, diameter=5mm, height=7mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 2.00mm diameter 5mm height 7mm Electrolytic Capacitor")
		(property "Reference" "C27"
			(at 1 -3.75 0)
			(layer "F.SilkS")
		)
		(property "Value" "47µF, 35V"
			(at 1 3.75 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "capacitor/THT/other"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 1 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15625)
			(net "+12V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 191.8417 115.9458)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R28"
			(at 0.3283 2.3942 0)
			(layer "F.SilkS")
		)
		(property "Value" "3,3 kΩ"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(U4-IPROPI)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 172.3542 88.5383 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R21"
			(at 0 -1.65 180)
			(layer "F.SilkS")
		)
		(property "Value" "1kΩ"
			(at 0 1.65 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "/LEFT_EN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(U3-EN{slash}IN1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 155.1867 112.8833 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing)")
		(tags "capacitor")
		(property "Reference" "C12"
			(at 0 -1.68 180)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.68 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 168.9167 103.8508)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R13"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100 Ω"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "/SHUTDOWN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(U2-*SHUTDOWN)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 137.8742 99.9958 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R3"
			(at 0 -1.65 270)
			(layer "F.SilkS")
		)
		(property "Value" "33kΩ"
			(at 0 1.65 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "/IGN_12V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(C3-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SamacSys_Parts:19635391"
		(layer "F.Cu")
		(at 129.03 82.16 -90)
		(descr "1-963539-1-5")
		(tags "Connector")
		(property "Reference" "J1"
			(at 10.16 8.006 90)
			(layer "F.SilkS")
		)
		(property "Value" "1-963539-1"
			(at 10.16 8.006 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=963539&DocType=Customer%20Drawing&DocLang=English&DocFormat=pdf&PartCntxt=1-963539-1"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "PCB Mount Header, Horizontal, Wire-to-Board, 18 Position, 2.54 mm [.1 in] Centerline, Fully Shrouded, Tin (Sn), Through Hole - Solder, Signal, Black"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "17"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "TE Connectivity"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "1-963539-1"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "571-1-963539-1"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/TE-Connectivity-AMP/1-963539-1?qs=Ykyshr6pipIKqs3XGcMqgw%3D%3D"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Part Number" "1-963539-1"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Price/Stock" "https://www.arrow.com/en/products/1-963539-1/te-connectivity?utm_currency=USD&region=europe"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2" "3" "4" "5" "6" "7" "8" "9" "10" "11" "12" "13" "14" "15"
					"16" "17" "18"
				)
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 10.16 8.006 90)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -5.08 -2.54 270)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 25.4 -2.54 270)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/VBAT")
			(pinfunction "1_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 270)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "2_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 5.08 0 270)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "3_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 7.62 0 270)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/LOCK_12V")
			(pinfunction "4_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 10.16 0 270)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/UNLOCK_12V")
			(pinfunction "5_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 12.7 0 270)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/IGN_12V")
			(pinfunction "6_6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 15.24 0 270)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(J1-Pad7)")
			(pinfunction "7_7")
			(pintype "passive+no_connect")
		)
		(pad "8" thru_hole circle
			(at 17.78 0 270)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(J1-Pad8)")
			(pinfunction "8_8")
			(pintype "passive+no_connect")
		)
		(pad "9" thru_hole circle
			(at 20.32 0 270)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/FOLD_BUTTON")
			(pinfunction "9_9")
			(pintype "passive")
		)
		(pad "10" thru_hole circle
			(at 0 -2.54 270)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/MOTOR_L+")
			(pinfunction "10_10")
			(pintype "passive")
		)
		(pad "11" thru_hole circle
			(at 2.54 -2.54 270)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/MOTOR_L-")
			(pinfunction "11_11")
			(pintype "passive")
		)
		(pad "12" thru_hole circle
			(at 5.08 -2.54 270)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(J1-Pad12)")
			(pinfunction "12_12")
			(pintype "passive+no_connect")
		)
		(pad "13" thru_hole circle
			(at 7.62 -2.54 270)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(J1-Pad13)")
			(pinfunction "13_13")
			(pintype "passive+no_connect")
		)
		(pad "14" thru_hole circle
			(at 10.16 -2.54 270)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(J1-Pad14)")
			(pinfunction "14_14")
			(pintype "passive+no_connect")
		)
		(pad "15" thru_hole circle
			(at 12.7 -2.54 270)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(J1-Pad15)")
			(pinfunction "15_15")
			(pintype "passive+no_connect")
		)
		(pad "16" thru_hole circle
			(at 15.24 -2.54 270)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(J1-Pad16)")
			(pinfunction "16_16")
			(pintype "passive+no_connect")
		)
		(pad "17" thru_hole circle
			(at 17.78 -2.54 270)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/MOTOR_R+")
			(pinfunction "17_17")
			(pintype "passive")
		)
		(pad "18" thru_hole circle
			(at 20.32 -2.54 270)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/MOTOR_R-")
			(pinfunction "18_18")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "G:\\\\SamacSys_Parts.3dshapes\\1-963539-1.stp"
			(offset
				(xyz 0.05999999776 -24.13999903 8.779999601)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "VITO:DGN8_1P98X1P88"
		(layer "F.Cu")
		(at 160.048 114.7912 90)
		(tags "TPA2005D1TDGNRQ1 ")
		(property "Reference" "U2"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "TPA2005D1TDGNRQ1"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/tpa2005d1-q1"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DGN8_1P98X1P88 DGN8_1P98X1P88-M DGN8_1P98X1P88-L")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2" "3" "4" "7" "6" "EPAD" "8" "5")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "*"
			(at -2.428999 -2.5488 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -2.428999 -2.5488 270)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -2.428999 -2.5488 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -2.428999 -2.5488 270)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.174999 -0.974999 90)
			(size 1.4112 0.4308)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(U2-*SHUTDOWN)")
			(pinfunction "*SHUTDOWN_1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -2.174999 -0.325001 90)
			(size 1.4112 0.4308)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(U2-NC-Pad2)")
			(pinfunction "NC_2")
			(pintype "unspecified+no_connect")
		)
		(pad "3" smd rect
			(at -2.174999 0.325001 90)
			(size 1.4112 0.4308)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(U2-IN+)")
			(pinfunction "IN+_3")
			(pintype "input")
		)
		(pad "4" smd rect
			(at -2.174999 0.974999 90)
			(size 1.4112 0.4308)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(U2-IN-)")
			(pinfunction "IN-_4")
			(pintype "input")
		)
		(pad "5" smd rect
			(at 2.174999 0.974999 90)
			(size 1.4112 0.4308)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(U2-VO+)")
			(pinfunction "VO+_5")
			(pintype "output")
		)
		(pad "6" smd rect
			(at 2.174999 0.325001 90)
			(size 1.4112 0.4308)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "+5V")
			(pinfunction "VDD_6")
			(pintype "power_in")
		)
		(pad "7" smd rect
			(at 2.174999 -0.325001 90)
			(size 1.4112 0.4308)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pinfunction "GND_7")
			(pintype "power_in")
		)
		(pad "8" smd rect
			(at 2.174999 -0.974999 90)
			(size 1.4112 0.4308)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(U2-VO-)")
			(pinfunction "VO-_8")
			(pintype "output")
		)
		(pad "EPAD" thru_hole circle
			(at -0.3937 -0.3937 90)
			(size 0.508 0.508)
			(drill 0.254)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "EPAD_EPAD")
			(pintype "power_in")
		)
		(pad "EPAD" thru_hole circle
			(at -0.3937 0.3937 90)
			(size 0.508 0.508)
			(drill 0.254)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "EPAD_EPAD")
			(pintype "power_in")
		)
		(pad "EPAD" smd rect
			(at 0 0 90)
			(size 1.88 1.98)
			(layers "F.Cu")
			(net "GND")
			(pinfunction "EPAD_EPAD")
			(pintype "power_in")
		)
		(pad "EPAD" thru_hole circle
			(at 0.3937 -0.3937 90)
			(size 0.508 0.508)
			(drill 0.254)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "EPAD_EPAD")
			(pintype "power_in")
		)
		(pad "EPAD" thru_hole circle
			(at 0.3937 0.3937 90)
			(size 0.508 0.508)
			(drill 0.254)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "EPAD_EPAD")
			(pintype "power_in")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 168.9367 100.6958 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing)")
		(tags "capacitor")
		(property "Reference" "C10"
			(at -0.3633 1.6658 180)
			(layer "F.SilkS")
		)
		(property "Value" "100nF 25V XR7"
			(at 0 1.68 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/AUDIO")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(C10-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:HTSSOP-16-1EP_4.4x5mm_P0.65mm_EP3.4x5mm_Mask2.46x2.31mm_ThermalVias"
		(layer "F.Cu")
		(at 197.779077 107.7483 90)
		(descr "HTSSOP, 16 Pin (Texas Instruments PWP0016C, based on JEDEC MO-153 variation ABT, 1.00mm body thickness, https://www.ti.com/lit/ml/pptd023ac/pptd023ac.pdf, https://www.ti.com/lit/ds/symlink/drv8833.pdf#page=27, https://www.jedec.org/document_search?search_api_views_fulltext=MO-153)")
		(tags "HTSSOP SO Texas_PWP0016C Texas_PowerPAD-TSSOP")
		(property "Reference" "U4"
			(at 0 -3.45 270)
			(layer "F.SilkS")
		)
		(property "Value" "DRV8874QPWPRQ1"
			(at 0 3.45 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "package/gullwing"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "12" "13" "14" "1" "2" "3" "5" "16" "7" "15" "11" "9" "17" "8"
					"10" "4" "6"
				)
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.615 0 90)
			(size 0.99 1.86)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd rect
			(at 0 0 90)
			(size 2.46 2.31)
			(layers "F.Mask")
		)
		(pad "" smd roundrect
			(at 0.615 0 90)
			(size 0.99 1.86)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -2.8625 -2.275 90)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(U4-EN{slash}IN1)")
			(pinfunction "EN/IN1_1")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2.8625 -1.625 90)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(U4-PH{slash}IN2)")
			(pinfunction "PH/IN2_2")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -2.8625 -0.975 90)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(U4-nSLEEP)")
			(pinfunction "nSLEEP_3")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -2.8625 -0.325 90)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(U4-nFAULT)")
			(pinfunction "nFAULT_4")
			(pintype "open_collector")
		)
		(pad "5" smd roundrect
			(at -2.8625 0.325 90)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(U4-VREF)")
			(pinfunction "VREF_5")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -2.8625 0.975 90)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(U4-IPROPI)")
			(pinfunction "IPROPI_6")
			(pintype "output")
		)
		(pad "7" smd roundrect
			(at -2.8625 1.625 90)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pinfunction "IMODE_7")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at -2.8625 2.275 90)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/MOTOR_R+")
			(pinfunction "OUT1_8")
			(pintype "power_out")
		)
		(pad "9" smd roundrect
			(at 2.8625 2.275 90)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pinfunction "PGND_9")
			(pintype "power_in")
		)
		(pad "10" smd roundrect
			(at 2.8625 1.625 90)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/MOTOR_R-")
			(pinfunction "OUT2_10")
			(pintype "power_out")
		)
		(pad "11" smd roundrect
			(at 2.8625 0.975 90)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+12V")
			(pinfunction "VM_11")
			(pintype "power_in")
		)
		(pad "12" smd roundrect
			(at 2.8625 0.325 90)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(U4-VCP)")
			(pinfunction "VCP_12")
			(pintype "passive")
		)
		(pad "13" smd roundrect
			(at 2.8625 -0.325 90)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(U4-CPH)")
			(pinfunction "CPH_13")
			(pintype "passive")
		)
		(pad "14" smd roundrect
			(at 2.8625 -0.975 90)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(U4-CPL)")
			(pinfunction "CPL_14")
			(pintype "passive")
		)
		(pad "15" smd roundrect
			(at 2.8625 -1.625 90)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pinfunction "GND_15")
			(pintype "power_in")
		)
		(pad "16" smd roundrect
			(at 2.8625 -2.275 90)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pinfunction "PMODE_16")
			(pintype "input")
		)
		(pad "17" thru_hole circle
			(at -1 -1.8 90)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "EP_17")
			(pintype "power_in")
		)
		(pad "17" thru_hole circle
			(at -1 -0.6 90)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "EP_17")
			(pintype "power_in")
		)
		(pad "17" thru_hole circle
			(at -1 0.6 90)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "EP_17")
			(pintype "power_in")
		)
		(pad "17" thru_hole circle
			(at -1 1.8 90)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "EP_17")
			(pintype "power_in")
		)
		(pad "17" thru_hole circle
			(at 0 -1.8 90)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "EP_17")
			(pintype "power_in")
		)
		(pad "17" thru_hole circle
			(at 0 -0.6 90)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "EP_17")
			(pintype "power_in")
		)
		(pad "17" smd rect
			(at 0 0 90)
			(size 2.5 4.1)
			(property pad_prop_heatsink)
			(layers "B.Cu")
			(net "GND")
			(pinfunction "EP_17")
			(pintype "power_in")
			(zone_connect 2)
		)
		(pad "17" smd rect
			(at 0 0 90)
			(size 3.4 5)
			(property pad_prop_heatsink)
			(layers "F.Cu")
			(net "GND")
			(pinfunction "EP_17")
			(pintype "power_in")
			(zone_connect 2)
		)
		(pad "17" thru_hole circle
			(at 0 0.6 90)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "EP_17")
			(pintype "power_in")
		)
		(pad "17" thru_hole circle
			(at 0 1.8 90)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "EP_17")
			(pintype "power_in")
		)
		(pad "17" thru_hole circle
			(at 1 -1.8 90)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "EP_17")
			(pintype "power_in")
		)
		(pad "17" thru_hole circle
			(at 1 -0.6 90)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "EP_17")
			(pintype "power_in")
		)
		(pad "17" thru_hole circle
			(at 1 0.6 90)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "EP_17")
			(pintype "power_in")
		)
		(pad "17" thru_hole circle
			(at 1 1.8 90)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "EP_17")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_SO.3dshapes/HTSSOP-16-1EP_4.4x5mm_P0.65mm_EP3.4x5mm_Mask2.46x2.31mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 194.2167 101.1333 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C24"
			(at 0 -1.43 270)
			(layer "F.SilkS")
		)
		(property "Value" "100 nF"
			(at 0 1.43 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(U4-VCP)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+12V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0805_2012Metric"
		(layer "F.Cu")
		(at 203.3617 94.2633)
		(descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "inductor")
		(property "Reference" "FB1"
			(at 0 -1.55 0)
			(layer "F.SilkS")
		)
		(property "Value" "FerriteBead"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ferrite bead"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "Inductor_* L_* *Ferrite*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0625 0)
			(size 0.875 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(U2-VO+)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0625 0)
			(size 0.875 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(J3-Pin_2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 198.2792 114.5708 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C23"
			(at 0 -1.43 270)
			(layer "F.SilkS")
		)
		(property "Value" "100 nF"
			(at 0 1.43 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(U4-VREF)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 189.2292 112.9133 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R33"
			(at 0 -1.65 180)
			(layer "F.SilkS")
		)
		(property "Value" "1kΩ"
			(at 0 1.65 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(U4-nFAULT)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "/RIGHT_FAULT")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 173.1867 109.9958 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R15"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "75 kΩ"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(C10-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(U2-IN+)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 193.4042 75.9458)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R18"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "100 kΩ"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(U3-VREF)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 151.4367 97.5708 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing)")
		(tags "capacitor")
		(property "Reference" "C5"
			(at 0 -1.68 180)
			(layer "F.SilkS")
		)
		(property "Value" "1.0µF  X7R"
			(at 0 1.68 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(D2-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 201.8417 117.8208)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R20"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "100 kΩ"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(U4-VREF)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 188.6942 87.2458)
		(descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x05 2.54mm single row")
		(property "Reference" "J2"
			(at 0 -2.38 0)
			(layer "F.SilkS")
		)
		(property "Value" "SWD"
			(at 0 12.54 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "connector/pin_header_socket"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2" "3" "4" "5")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 5.08 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+3V3")
			(pinfunction "Pin_1_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/SWDIO")
			(pinfunction "Pin_2_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/NRST")
			(pinfunction "Pin_3_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/SWCLK")
			(pinfunction "Pin_4_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "Pin_5_5")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 138.9167 103.8508)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R6"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "10 kΩ"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(C3-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 191.5292 78.7583)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R27"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "3,3 kΩ"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(U3-IPROPI)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 170.7167 83.7258 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing)")
		(tags "capacitor")
		(property "Reference" "C19"
			(at 0 -1.68 270)
			(layer "F.SilkS")
		)
		(property "Value" "22nF"
			(at 0 1.68 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(U3-CPH)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(U3-CPL)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 138.2167 107.7883 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing)")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 0 -1.68 90)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(C3-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 174.5292 81.4458 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C17"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "22 nF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(U3-CPL)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 193.8117 91.2458 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R22"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "1kΩ"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "/LEFT_DIR")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(U3-PH{slash}IN2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 175.0917 94.6633 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing)")
		(tags "capacitor")
		(property "Reference" "C15"
			(at -0.3133 -1.7083 90)
			(layer "F.SilkS")
		)
		(property "Value" "4,7 µF"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 183.6042 109.7883 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R34"
			(at 0 -1.65 180)
			(layer "F.SilkS")
		)
		(property "Value" "1kΩ"
			(at 0 1.65 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(U4-IPROPI)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "/CURRENT_RIGHT")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 179.4367 81.8708 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R32"
			(at 0 -1.65 270)
			(layer "F.SilkS")
		)
		(property "Value" "1kΩ"
			(at 0 1.65 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(U3-IPROPI)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "/CURRENT_LEFT")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 203.4042 105.0083)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C26"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "100 nF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+12V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_Tantalum_SMD:CP_EIA-6032-28_Kemet-C"
		(layer "F.Cu")
		(at 155.743122 108.5758)
		(descr "Tantalum Capacitor SMD Kemet-C (6032-28 Metric), IPC-7352 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf)")
		(tags "capacitor tantalum")
		(property "Reference" "C7"
			(at 0 -2.55 0)
			(layer "F.SilkS")
		)
		(property "Value" "22µF 16V"
			(at 0 2.55 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.47 0)
			(size 2.07 2.39)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.120773)
			(net "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.47 0)
			(size 2.07 2.39)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.120773)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-6032-28_Kemet-C.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.00mm"
		(layer "F.Cu")
		(at 199.028889 100.750705 90)
		(descr "CP, Radial series, Radial, pin pitch=2.00mm, diameter=5mm, height=7mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 2.00mm diameter 5mm height 7mm Electrolytic Capacitor")
		(property "Reference" "C29"
			(at 1 -3.75 270)
			(layer "F.SilkS")
		)
		(property "Value" "47µF, 35V"
			(at 1 3.75 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "capacitor/THT/other"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 1 0 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15625)
			(net "+12V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 183.7167 72.5083)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C28"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "10 nF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(U3-IPROPI)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 165.4992 96.0083)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing)")
		(tags "capacitor")
		(property "Reference" "C8"
			(at 0 -1.68 0)
			(layer "F.SilkS")
		)
		(property "Value" "1.0µF  X7R"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 203.4042 110.6333)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C30"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "10 nF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(U4-IPROPI)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "VITO:SOT230P700X180-4N"
		(layer "F.Cu")
		(at 158.9617 93.0258 90)
		(descr "3-Lead Plastic Small Outline Transistor (DB) [SOT-223]")
		(tags "Integrated Circuit")
		(property "Reference" "IC2"
			(at 0 0 270)
			(layer "F.SilkS")
		)
		(property "Value" "MCP1792-3302H/DB"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22075b.pdf"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "MCP1790-3302E/DB, Low Dropout Voltage Regulator, 0.07A, 3.3 V +/-2.5%, 6  30 Vin, 4-Pin SOT-223"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "1.8"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Microchip"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "MCP1790-3302E/DB"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "579-MCP1790-3302E/DB"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Microchip-Technology-Atmel/MCP1790-3302E-DB?qs=gsqZ4L1luKoGoO0qj299JQ%3D%3D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Part Number" "MCP1790-3302E/DB"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Price/Stock" "https://www.arrow.com/en/products/mcp1790-3302edb/microchip-technology?region=nac"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2" "3" "4")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.15 -2.3 180)
			(size 0.95 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(D2-K)")
			(pinfunction "VIN_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -3.15 0 180)
			(size 0.95 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pinfunction "GND_1_2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -3.15 2.3 180)
			(size 0.95 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "+3V3")
			(pinfunction "VOUT_3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 3.15 0 90)
			(size 1.75 3.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pinfunction "GND_2_4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "MCP1790-3302E_DB.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:HTSSOP-16-1EP_4.4x5mm_P0.65mm_EP3.4x5mm_Mask2.46x2.31mm_ThermalVias"
		(layer "F.Cu")
		(at 177.0742 75.820923 180)
		(descr "HTSSOP, 16 Pin (Texas Instruments PWP0016C, based on JEDEC MO-153 variation ABT, 1.00mm body thickness, https://www.ti.com/lit/ml/pptd023ac/pptd023ac.pdf, https://www.ti.com/lit/ds/symlink/drv8833.pdf#page=27, https://www.jedec.org/document_search?search_api_views_fulltext=MO-153)")
		(tags "HTSSOP SO Texas_PWP0016C Texas_PowerPAD-TSSOP")
		(property "Reference" "U3"
			(at 0 -3.45 180)
			(layer "F.SilkS")
		)
		(property "Value" "DRV8874QPWPRQ1"
			(at 0 3.45 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "package/gullwing"
			(at 0 0 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "12" "13" "14" "1" "2" "3" "5" "16" "7" "15" "11" "9" "17" "8"
					"10" "4" "6"
				)
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.615 0 180)
			(size 0.99 1.86)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd rect
			(at 0 0 180)
			(size 2.46 2.31)
			(layers "F.Mask")
		)
		(pad "" smd roundrect
			(at 0.615 0 180)
			(size 0.99 1.86)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -2.8625 -2.275 180)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(U3-EN{slash}IN1)")
			(pinfunction "EN/IN1_1")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2.8625 -1.625 180)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(U3-PH{slash}IN2)")
			(pinfunction "PH/IN2_2")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -2.8625 -0.975 180)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(U3-nSLEEP)")
			(pinfunction "nSLEEP_3")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -2.8625 -0.325 180)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(U3-nFAULT)")
			(pinfunction "nFAULT_4")
			(pintype "open_collector")
		)
		(pad "5" smd roundrect
			(at -2.8625 0.325 180)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(U3-VREF)")
			(pinfunction "VREF_5")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -2.8625 0.975 180)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(U3-IPROPI)")
			(pinfunction "IPROPI_6")
			(pintype "output")
		)
		(pad "7" smd roundrect
			(at -2.8625 1.625 180)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pinfunction "IMODE_7")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at -2.8625 2.275 180)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/MOTOR_L+")
			(pinfunction "OUT1_8")
			(pintype "power_out")
		)
		(pad "9" smd roundrect
			(at 2.8625 2.275 180)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pinfunction "PGND_9")
			(pintype "power_in")
		)
		(pad "10" smd roundrect
			(at 2.8625 1.625 180)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/MOTOR_L-")
			(pinfunction "OUT2_10")
			(pintype "power_out")
		)
		(pad "11" smd roundrect
			(at 2.8625 0.975 180)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+12V")
			(pinfunction "VM_11")
			(pintype "power_in")
		)
		(pad "12" smd roundrect
			(at 2.8625 0.325 180)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(U3-VCP)")
			(pinfunction "VCP_12")
			(pintype "passive")
		)
		(pad "13" smd roundrect
			(at 2.8625 -0.325 180)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(U3-CPH)")
			(pinfunction "CPH_13")
			(pintype "passive")
		)
		(pad "14" smd roundrect
			(at 2.8625 -0.975 180)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(U3-CPL)")
			(pinfunction "CPL_14")
			(pintype "passive")
		)
		(pad "15" smd roundrect
			(at 2.8625 -1.625 180)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pinfunction "GND_15")
			(pintype "power_in")
		)
		(pad "16" smd roundrect
			(at 2.8625 -2.275 180)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pinfunction "PMODE_16")
			(pintype "input")
		)
		(pad "17" thru_hole circle
			(at -1 -1.8 180)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "EP_17")
			(pintype "power_in")
		)
		(pad "17" thru_hole circle
			(at -1 -0.6 180)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "EP_17")
			(pintype "power_in")
		)
		(pad "17" thru_hole circle
			(at -1 0.6 180)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "EP_17")
			(pintype "power_in")
		)
		(pad "17" thru_hole circle
			(at -1 1.8 180)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "EP_17")
			(pintype "power_in")
		)
		(pad "17" thru_hole circle
			(at 0 -1.8 180)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "EP_17")
			(pintype "power_in")
		)
		(pad "17" thru_hole circle
			(at 0 -0.6 180)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "EP_17")
			(pintype "power_in")
		)
		(pad "17" smd rect
			(at 0 0 180)
			(size 2.5 4.1)
			(property pad_prop_heatsink)
			(layers "B.Cu")
			(net "GND")
			(pinfunction "EP_17")
			(pintype "power_in")
			(zone_connect 2)
		)
		(pad "17" smd rect
			(at 0 0 180)
			(size 3.4 5)
			(property pad_prop_heatsink)
			(layers "F.Cu")
			(net "GND")
			(pinfunction "EP_17")
			(pintype "power_in")
			(zone_connect 2)
		)
		(pad "17" thru_hole circle
			(at 0 0.6 180)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "EP_17")
			(pintype "power_in")
		)
		(pad "17" thru_hole circle
			(at 0 1.8 180)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "EP_17")
			(pintype "power_in")
		)
		(pad "17" thru_hole circle
			(at 1 -1.8 180)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "EP_17")
			(pintype "power_in")
		)
		(pad "17" thru_hole circle
			(at 1 -0.6 180)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "EP_17")
			(pintype "power_in")
		)
		(pad "17" thru_hole circle
			(at 1 0.6 180)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "EP_17")
			(pintype "power_in")
		)
		(pad "17" thru_hole circle
			(at 1 1.8 180)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "EP_17")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_SO.3dshapes/HTSSOP-16-1EP_4.4x5mm_P0.65mm_EP3.4x5mm_Mask2.46x2.31mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 130.3742 68.1208 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R1"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "33kΩ"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "/LOCK_12V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(C1-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 182.6667 87.9133 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R12"
			(at 0 -1.65 180)
			(layer "F.SilkS")
		)
		(property "Value" "10 kΩ"
			(at 0 1.65 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "/NRST")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "VITO:QFP80P900X900X160-32N"
		(layer "F.Cu")
		(at 179.468977 102.568523 -90)
		(descr "LQFP - 32-pin, 7 x 7 mm")
		(tags "Integrated Circuit")
		(property "Reference" "U1"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "STM32G081KBT6"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "6" "10" "13" "9" "27" "7" "14" "8" "15" "24" "25" "4" "5" "11"
					"16" "18" "21" "17" "19" "22" "20" "1" "2" "3" "12" "23" "26" "28" "29"
					"30" "31" "32"
				)
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" smd rect
			(at -4.238 -2.8)
			(size 0.6 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(U1-PB9-Pad1)")
			(pinfunction "PB9_1")
			(pintype "bidirectional+no_connect")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd rect
			(at -4.238 -2)
			(size 0.6 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(U1-PC14-Pad2)")
			(pinfunction "PC14_2")
			(pintype "bidirectional+no_connect")
			(thermal_bridge_angle 45)
		)
		(pad "3" smd rect
			(at -4.238 -1.2)
			(size 0.6 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(U1-PC15-Pad3)")
			(pinfunction "PC15_3")
			(pintype "bidirectional+no_connect")
			(thermal_bridge_angle 45)
		)
		(pad "4" smd rect
			(at -4.238 -0.4)
			(size 0.6 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "+3V3")
			(pinfunction "VDD/VDDA_4")
			(pintype "power_in")
			(thermal_bridge_angle 45)
		)
		(pad "5" smd rect
			(at -4.238 0.4)
			(size 0.6 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pinfunction "VSS/VSSA_5")
			(pintype "power_in")
			(thermal_bridge_angle 45)
		)
		(pad "6" smd rect
			(at -4.238 1.2)
			(size 0.6 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/NRST")
			(pinfunction "PF2/NRST_6")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "7" smd rect
			(at -4.238 2)
			(size 0.6 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/CURRENT_LEFT")
			(pinfunction "PA0_/_ADC_IN0_7")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "8" smd rect
			(at -4.238 2.8)
			(size 0.6 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/CURRENT_RIGHT")
			(pinfunction "PA1_/_ADC_IN1_8")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "9" smd rect
			(at -2.8 4.238 270)
			(size 0.6 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/E_IGN_12V")
			(pinfunction "PA2_/_USART2_TX_9")
			(pintype "output")
			(thermal_bridge_angle 45)
		)
		(pad "10" smd rect
			(at -2 4.238 270)
			(size 0.6 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/E_LOCK_12V")
			(pinfunction "PA3_USART2_RX_10")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "11" smd rect
			(at -1.2 4.238 270)
			(size 0.6 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/AUDIO")
			(pinfunction "PA4_/_ADC_IN4_11")
			(pintype "output")
			(thermal_bridge_angle 45)
		)
		(pad "12" smd rect
			(at -0.4 4.238 270)
			(size 0.6 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(U1-PA5_{slash}_ADC_IN5-Pad12)")
			(pinfunction "PA5_/_ADC_IN5_12")
			(pintype "input+no_connect")
			(thermal_bridge_angle 45)
		)
		(pad "13" smd rect
			(at 0.4 4.238 270)
			(size 0.6 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/E_UNLOCK_12V")
			(pinfunction "PA6_/_ADC_IN6_13")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "14" smd rect
			(at 1.2 4.238 270)
			(size 0.6 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/LEFT_FAULT")
			(pinfunction "PA7_14")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "15" smd rect
			(at 2 4.238 270)
			(size 0.6 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/RIGHT_FAULT")
			(pinfunction "PB0_15")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "16" smd rect
			(at 2.8 4.238 270)
			(size 0.6 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/SHUTDOWN")
			(pinfunction "PB1_/_ADC_IN9_16")
			(pintype "output")
			(thermal_bridge_angle 45)
		)
		(pad "17" smd rect
			(at 4.238 2.8)
			(size 0.6 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/LEFT_SLEEP")
			(pinfunction "PB2_17")
			(pintype "output")
			(thermal_bridge_angle 45)
		)
		(pad "18" smd rect
			(at 4.238 2)
			(size 0.6 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/LEFT_EN")
			(pinfunction "PA8_TIM1_CH1_18")
			(pintype "output")
			(thermal_bridge_angle 45)
		)
		(pad "19" smd rect
			(at 4.238 1.2)
			(size 0.6 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/RIGHT_EN")
			(pinfunction "PA9_/_TIM1_CH2_19")
			(pintype "output")
			(thermal_bridge_angle 45)
		)
		(pad "20" smd rect
			(at 4.238 0.4)
			(size 0.6 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/RIGHT_SLEEP")
			(pinfunction "PC6_20")
			(pintype "output")
			(thermal_bridge_angle 45)
		)
		(pad "21" smd rect
			(at 4.238 -0.4)
			(size 0.6 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/LEFT_DIR")
			(pinfunction "PA10_21")
			(pintype "output")
			(thermal_bridge_angle 45)
		)
		(pad "22" smd rect
			(at 4.238 -1.2)
			(size 0.6 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/RIGHT_DIR")
			(pinfunction "PA11_22")
			(pintype "output")
			(thermal_bridge_angle 45)
		)
		(pad "23" smd rect
			(at 4.238 -2)
			(size 0.6 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(U1-PA12-Pad23)")
			(pinfunction "PA12_23")
			(pintype "output+no_connect")
			(thermal_bridge_angle 45)
		)
		(pad "24" smd rect
			(at 4.238 -2.8)
			(size 0.6 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/SWDIO")
			(pinfunction "PA13_/_SWDIO_24")
			(pintype "bidirectional")
			(thermal_bridge_angle 45)
		)
		(pad "25" smd rect
			(at 2.8 -4.238 270)
			(size 0.6 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/SWCLK")
			(pinfunction "PA14_/_SWCLK/BOOT0_25")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "26" smd rect
			(at 2 -4.238 270)
			(size 0.6 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(U1-PA15-Pad26)")
			(pinfunction "PA15_26")
			(pintype "output+no_connect")
			(thermal_bridge_angle 45)
		)
		(pad "27" smd rect
			(at 1.2 -4.238 270)
			(size 0.6 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/FOLD_IN")
			(pinfunction "PB3_27")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "28" smd rect
			(at 0.4 -4.238 270)
			(size 0.6 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(U1-PB4-Pad28)")
			(pinfunction "PB4_28")
			(pintype "bidirectional+no_connect")
			(thermal_bridge_angle 45)
		)
		(pad "29" smd rect
			(at -0.4 -4.238 270)
			(size 0.6 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(U1-PB5-Pad29)")
			(pinfunction "PB5_29")
			(pintype "bidirectional+no_connect")
			(thermal_bridge_angle 45)
		)
		(pad "30" smd rect
			(at -1.2 -4.238 270)
			(size 0.6 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(U1-PB6-Pad30)")
			(pinfunction "PB6_30")
			(pintype "bidirectional+no_connect")
			(thermal_bridge_angle 45)
		)
		(pad "31" smd rect
			(at -2 -4.238 270)
			(size 0.6 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(U1-PB7-Pad31)")
			(pinfunction "PB7_31")
			(pintype "bidirectional+no_connect")
			(thermal_bridge_angle 45)
		)
		(pad "32" smd rect
			(at -2.8 -4.238 270)
			(size 0.6 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(U1-PB8-Pad32)")
			(pinfunction "PB8_32")
			(pintype "bidirectional+no_connect")
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "Diode_SMD:D_SMA"
		(layer "F.Cu")
		(at 155.8617 82.174383 90)
		(descr "Diode SMA (DO-214AC)")
		(tags "Diode SMA (DO-214AC)")
		(property "Reference" "D2"
			(at 0 -2.5 270)
			(layer "F.SilkS")
		)
		(property "Value" "MRA4003T3G"
			(at 0 2.6 270)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/MRA4003T3-D.PDF"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "300V, 1A, General Purpose Rectifier Diode, SMA(DO-214AC)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*SMA*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2 0 90)
			(size 2.5 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1388888889)
			(net "Net-(D2-K)")
			(pinfunction "K_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2 0 90)
			(size 2.5 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1388888889)
			(net "+12V")
			(pinfunction "A_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 155.3742 73.4333 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R8"
			(at 0 -1.65 270)
			(layer "F.SilkS")
		)
		(property "Value" "100KΩ"
			(at 0 1.65 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(C1-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "/E_LOCK_12V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 177.0417 89.4758)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R31"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "1kΩ"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(U3-nFAULT)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "/LEFT_FAULT")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0805_2012Metric"
		(layer "F.Cu")
		(at 201.4867 85.5133 180)
		(descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "inductor")
		(property "Reference" "FB2"
			(at 0 -1.55 180)
			(layer "F.SilkS")
		)
		(property "Value" "FerriteBead"
			(at 0 1.55 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ferrite bead"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "Inductor_* L_* *Ferrite*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0625 0 180)
			(size 0.875 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(J3-Pin_1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0625 0 180)
			(size 0.875 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(U2-VO-)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 174.5292 70.1958 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C25"
			(at 0 -1.43 270)
			(layer "F.SilkS")
		)
		(property "Value" "100 nF"
			(at 0 1.43 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+12V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_XH_B2B-XH-AM_1x02_P2.50mm_Vertical"
		(layer "F.Cu")
		(at 200.4992 79.3383)
		(descr "JST XH series connector, B2B-XH-AM, with boss (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf)")
		(tags "connector JST XH vertical boss")
		(property "Reference" "J3"
			(at 1.25 -3.55 0)
			(layer "F.SilkS")
		)
		(property "Value" "Speaker_out"
			(at 1.25 4.6 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "connector/JST"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 1.25 2.7 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -1.6 2)
			(size 1.2 1.2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net "Net-(J3-Pin_1)")
			(pinfunction "Pin_1_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.5 0)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J3-Pin_2)")
			(pinfunction "Pin_2_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_JST.3dshapes/JST_XH_B2B-XH-AM_1x02_P2.50mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 140.0617 68.1208 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R4"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "10 kΩ"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(C1-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 171.1042 94.7883)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R14"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100 kΩ"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(U2-*SHUTDOWN)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "VITO:NCV4274CDT50RKG"
		(layer "F.Cu")
		(at 146.4867 112.4708 90)
		(descr "DPAK (SINGLE GAUGE) TO-252 (369C) ISSUE F_1")
		(tags "Integrated Circuit")
		(property "Reference" "IC1"
			(at 4.943 0 270)
			(layer "F.SilkS")
		)
		(property "Value" "NCV4274CDT50RKG"
			(at 4.943 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NCV4274C-D.PDF"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "3.3 V and 5.0 V, 2.0% Output Options; Very Low Dropout Voltage; Protections: +60 V Peak Transient Voltage -42V Reverse Voltage Short Circuit Thermal Overload; AECQ100 Grade 1 Qualified and PPAP Capable"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "2.38"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "863-NCV4274CDT50RKG"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/onsemi/NCV4274CDT50RKG?qs=tCMd4XlZ%2FiBk5MdmOBr7cw%3D%3D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "onsemi"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "NCV4274CDT50RKG"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "2" "3" "1")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 4.943 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 8.95 2.285 180)
			(size 1.6 3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(D2-K)")
			(pinfunction "INPUT_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.77 0 180)
			(size 5.8 6.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pinfunction "GND_2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 8.95 -2.285 180)
			(size 1.6 3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "+5V")
			(pinfunction "OUTPUT_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "NCV4274CDT50RKG.stp"
			(offset
				(xyz 4.199999746 0 0.4999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 -90)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 143.2917 97.9133)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R10"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100KΩ"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(C3-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "/E_IGN_12V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 183.7167 75.3208 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C20"
			(at 0 -1.43 180)
			(layer "F.SilkS")
		)
		(property "Value" "100 nF"
			(at 0 1.43 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(U3-VREF)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 171.1042 91.6633)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R5"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "10 kΩ"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(C2-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 201.3417 89.6633 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing)")
		(tags "capacitor")
		(property "Reference" "C16"
			(at 0 -1.68 270)
			(layer "F.SilkS")
		)
		(property "Value" "1nF"
			(at 0 1.68 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(J3-Pin_2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(J3-Pin_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 192.9667 110.5083 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R30"
			(at 0 -1.43 270)
			(layer "F.SilkS")
		)
		(property "Value" "10 kΩ"
			(at 0 1.43 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(U4-nFAULT)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 171.4042 69.2583 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C21"
			(at 0 -1.43 270)
			(layer "F.SilkS")
		)
		(property "Value" "100 nF"
			(at 0 1.43 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(U3-VCP)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+12V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 165.0617 102.8083 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R9"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "100KΩ"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(C2-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "/E_UNLOCK_12V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 178.5292 94.6633 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing)")
		(tags "capacitor")
		(property "Reference" "C9"
			(at 0.0033 1.9208 270)
			(layer "F.SilkS")
		)
		(property "Value" "100 nF"
			(at 0 1.68 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/NRST")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 136.1242 67.2583 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing)")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 0 -1.68 180)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.68 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(C1-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 187.3542 106.6633 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R11"
			(at 0 -1.65 180)
			(layer "F.SilkS")
		)
		(property "Value" "10 kΩ"
			(at 0 1.65 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "/FOLD_IN")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 192.9042 96.5383 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing)")
		(tags "capacitor")
		(property "Reference" "C22"
			(at 0 -1.68 270)
			(layer "F.SilkS")
		)
		(property "Value" "22nF"
			(at 0 1.68 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(U4-CPH)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(U4-CPL)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 169.1242 110.3083 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R7"
			(at 0 -1.65 270)
			(layer "F.SilkS")
		)
		(property "Value" "1 kΩ"
			(at 0 1.65 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "/FOLD_BUTTON")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "/FOLD_IN")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 177.0417 110.7258)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R24"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "1kΩ"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "/RIGHT_EN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(U4-EN{slash}IN1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 166.4367 91.6333 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing)")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 0 -1.68 180)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.68 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(C2-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 183.4042 82.1958 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R29"
			(at 0 -1.43 180)
			(layer "F.SilkS")
		)
		(property "Value" "10 kΩ"
			(at 0 1.43 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(U3-nFAULT)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 200.1867 74.1333 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing)")
		(tags "capacitor")
		(property "Reference" "C11"
			(at 0 -1.68 180)
			(layer "F.SilkS")
		)
		(property "Value" "100nF 25V XR7"
			(at 0 1.68 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(C11-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 204.1242 73.4333 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R16"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "75 kΩ"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(U2-IN-)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(C11-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:CP_Radial_D6.3mm_P2.50mm"
		(layer "F.Cu")
		(at 156.884916 103.117306 90)
		(descr "CP, Radial series, Radial, pin pitch=2.50mm, diameter=6.3mm, height=7mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 2.50mm diameter 6.3mm height 7mm Electrolytic Capacitor")
		(property "Reference" "C4"
			(at 1.25 -4.4 270)
			(layer "F.SilkS")
		)
		(property "Value" "220µF, 50V"
			(at 1.25 4.4 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "capacitor/THT/other"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15625)
			(net "Net-(D2-K)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "VITO:SM8S24CAH"
		(layer "F.Cu")
		(at 145.7367 86.8633)
		(descr "SM8S24CAH-1")
		(tags "TVS Diode (Bi-directional)")
		(property "Reference" "D1"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "SM8S24CA"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Bidirectional transient-voltage-suppression diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 6.3 90)
			(size 1.9 2.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pinfunction "A1_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 -2.85 90)
			(size 8.8 10)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "+12V")
			(pinfunction "A2_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "SM8S24CAH.stp"
			(offset
				(xyz 0 -5.419999995 2.099999873)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 165.4792 88.2258 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R2"
			(at 0 -1.65 180)
			(layer "F.SilkS")
		)
		(property "Value" "33kΩ"
			(at 0 1.65 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "/UNLOCK_12V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(C2-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 181.9667 94.6633 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing)")
		(tags "capacitor")
		(property "Reference" "C13"
			(at 0 -1.68 90)
			(layer "F.SilkS")
		)
		(property "Value" "100 nF"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 161.8242 108.1258 90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C14"
			(at 0 -1.85 270)
			(layer "F.SilkS")
		)
		(property "Value" "10µF"
			(at 0 1.85 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 184.5417 112.9133)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R26"
			(at 0.2183 1.9267 0)
			(layer "F.SilkS")
		)
		(property "Value" "1kΩ"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "/RIGHT_SLEEP")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(U4-nSLEEP)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "VITO:01530007Z"
		(layer "B.Cu")
		(at 144.9 68.85)
		(descr "01530007Z")
		(tags "Undefined or Miscellaneous")
		(property "Reference" "F1"
			(at 0 0.121 0)
			(layer "F.SilkS")
		)
		(property "Value" "3A External"
			(at 0 0.121 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" "http://m.littelfuse.com/~/media/commercial-vehicle/datasheets/automotive-fuse-holders/mini/littelfuse_fuse-holders-mini-153-pc-datasheet.pdf"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "LITTELFUSE - 01530007Z - FUSE HOLDER, MINI BLADE, HORIZONTAL, PCB"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Height" "7"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "576-01530007Z"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Littelfuse/01530007Z?qs=gu7KAQ731URFnx4B9aYM4g%3D%3D"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "LITTELFUSE"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "01530007Z"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "V3.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0.121 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 -1.88)
			(size 2.0828 2.0828)
			(drill 2.0828)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole circle
			(at -3.81 5.74)
			(size 1.905 1.905)
			(drill 1.27)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/VBAT")
			(pinfunction "1_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 3.81 5.74)
			(size 1.905 1.905)
			(drill 1.27)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+12V")
			(pinfunction "2_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "01530007Z.stp"
			(offset
				(xyz 0 0.1199999955 0.6999999776)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 -180)
			)
		)
	)
	(gr_rect
		(start 127.59 64.76)
		(end 207.59 119.76)
		(fill no)
		(layer "Edge.Cuts")
	)
	(zone
		(net "+12V")
		(layer "F.Cu")
		(hatch none 0.508)
		(connect_pads
			(clearance 0.2)
		)
		(min_thickness 0.0254)
		(fill yes
			(thermal_gap 0.0254)
			(thermal_bridge_width 0.2)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 158.747405 87.981502) (xy 157.934564 88.792239) (xy 157.154292 88.794096) (xy 157.153139 90.004642)
				(xy 156.258511 90.89927) (xy 142.819943 90.89927) (xy 142.616109 90.875751) (xy 140.987819 90.494928)
				(xy 140.558773 90.256302) (xy 138.975795 88.673324) (xy 138.713666 88.04049) (xy 138.713666 79.98611)
				(xy 138.975795 79.353276) (xy 140.419251 77.909819) (xy 141.052086 77.64769) (xy 154.279793 77.647593)
				(xy 155.923468 76.005129) (xy 156.556302 75.743) (xy 162.587971 75.742614) (xy 166.228863 72.102268)
				(xy 166.69103 71.856556) (xy 167.276138 71.742875) (xy 167.446847 71.726445) (xy 168.874708 71.726445)
				(xy 169.049351 71.743648) (xy 170.938571 72.119494) (xy 171.102452 72.659013) (xy 171.109899 72.660118)
				(xy 171.186305 72.583746) (xy 171.565431 72.962872) (xy 171.82756 73.595706) (xy 171.827584 74.495359)
				(xy 171.95027 74.619675) (xy 171.95027 75.90901) (xy 171.851901 76.009483) (xy 171.851901 77.698755)
				(xy 171.534901 78.016966) (xy 171.534901 79.616861) (xy 171.722216 79.62095) (xy 172.355051 79.883079)
				(xy 173.012874 80.540903) (xy 172.380771 82.066936) (xy 169.12377 82.066936) (xy 168.968696 82.220215)
				(xy 168.968483 83.407688) (xy 169.782836 84.222589) (xy 169.782836 86.272108) (xy 169.44831 86.277188)
				(xy 169.7103 86.910697) (xy 168.639097 87.9819) (xy 167.113064 87.349796) (xy 167.109459 87.317155)
				(xy 166.40978 87.316936) (xy 165.581877 86.489882) (xy 164.419939 86.490263) (xy 163.845434 87.06567)
				(xy 163.845336 89.825202) (xy 163.583207 90.458037) (xy 163.404103 90.637141) (xy 162.771268 90.89927)
				(xy 161.664889 90.89927) (xy 160.770261 90.004642) (xy 160.769875 88.795375) (xy 160.751387 88.792239)
				(xy 159.941369 87.982358)
			)
		)
	)
	(zone
		(net "+5V")
		(layer "F.Cu")
		(hatch none 0.508)
		(connect_pads
			(clearance 0.2)
		)
		(min_thickness 0.0254)
		(fill yes
			(thermal_gap 0.0254)
			(thermal_bridge_width 0.2)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 156.136893 109.084204) (xy 156.969259 109.089284) (xy 156.972864 109.979445) (xy 159.453381 109.979445)
				(xy 159.456986 108.071876) (xy 160.117618 108.071876) (xy 160.724093 108.67714) (xy 163.108704 108.677238)
				(xy 163.457789 109.026322) (xy 163.457789 110.175278) (xy 162.722681 110.910385) (xy 161.318691 111.70204)
				(xy 160.601295 111.702896) (xy 160.599038 112.107823) (xy 160.14696 112.362732) (xy 160.14696 111.888937)
				(xy 160.389269 111.884848) (xy 160.38751 110.862523) (xy 159.36688 110.86137) (xy 159.3618 110.870839)
				(xy 158.463704 110.871439) (xy 158.461019 113.313367) (xy 156.636948 114.341889) (xy 155.636723 114.341889)
				(xy 154.945564 113.856626) (xy 154.943306 111.950292) (xy 152.229156 111.949436) (xy 149.595261 110.100179)
				(xy 149.593004 107.393095) (xy 145.738346 107.392239) (xy 143.40498 105.753983) (xy 142.669693 105.018696)
				(xy 142.669693 102.022904) (xy 143.403804 101.288793) (xy 145.000733 101.288793) (xy 147.763139 102.380319)
				(xy 147.766744 105.229143) (xy 154.973428 105.229361) (xy 155.173011 105.308224) (xy 155.89743 106.032608)
				(xy 156.136893 106.033761)
			)
		)
	)
	(zone
		(net "+12V")
		(layer "F.Cu")
		(hatch none 0.508)
		(connect_pads
			(clearance 0.2)
		)
		(min_thickness 0.0254)
		(fill yes
			(thermal_gap 0.0254)
			(thermal_bridge_width 0.2)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 203.520494 105.553617) (xy 201.321914 105.553617) (xy 201.32189 104.540791) (xy 201.208557 104.536209)
				(xy 201.208338 103.897388) (xy 200.473243 103.162293) (xy 199.459257 103.163227) (xy 199.257556 103.365043)
				(xy 199.135163 103.673636) (xy 199.0315 103.777845) (xy 199.031113 103.889739) (xy 198.995734 103.893344)
				(xy 198.995515 104.02606) (xy 198.984102 104.055458) (xy 198.995515 104.063859) (xy 198.995515 104.337935)
				(xy 197.721778 103.067688) (xy 197.72029 103.033875) (xy 196.260466 101.574051) (xy 196.226653 101.572563)
				(xy 196.204273 101.550183) (xy 196.204273 99.951227) (xy 196.392451 99.763049) (xy 201.665326 99.763049)
				(xy 201.854689 99.952412) (xy 203.520494 102.301216)
			)
		)
	)
	(zone
		(net "GND")
		(layer "In1.Cu")
		(hatch none 0.508)
		(connect_pads
			(clearance 0.2)
		)
		(min_thickness 0.0254)
		(fill yes
			(thermal_gap 0.0254)
			(thermal_bridge_width 0.2)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 128.098083 65.268083) (xy 207.081918 65.268083) (xy 207.081918 119.251917) (xy 128.098083 119.251917)
			)
		)
	)
	(zone
		(net "+3V3")
		(layer "In2.Cu")
		(hatch none 0.508)
		(connect_pads
			(clearance 0.2)
		)
		(min_thickness 0.0254)
		(fill yes
			(thermal_gap 0.0254)
			(thermal_bridge_width 0.2)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 128.098083 65.268083) (xy 207.081918 65.268083) (xy 207.081918 119.251917) (xy 128.098083 119.251917)
			)
		)
	)
	(embedded_fonts no)
)
