(footprint "XIAO-ESP32-S3-DIP"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0.025 -10.35 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "XIAO-ESP32-S3-DIP"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(duplicate_pad_numbers_are_jumpers no)
	(pad "1" smd roundrect
		(at 7.62 -8.455 90)
		(size 2.432 1.524)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1)
		(thermal_bridge_angle 45)
	)
	(pad "1" thru_hole circle
		(at 7.62 -7.62 90)
		(size 1.524 1.524)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" smd roundrect
		(at 5.08 -8.455 90)
		(size 2.432 1.524)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1)
		(thermal_bridge_angle 45)
	)
	(pad "2" thru_hole circle
		(at 5.08 -7.62 90)
		(size 1.524 1.524)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" smd roundrect
		(at 2.54 -8.455 90)
		(size 2.432 1.524)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1)
		(thermal_bridge_angle 45)
	)
	(pad "3" thru_hole circle
		(at 2.54 -7.62 90)
		(size 1.524 1.524)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" smd roundrect
		(at 0 -8.455 90)
		(size 2.432 1.524)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1)
		(thermal_bridge_angle 45)
	)
	(pad "4" thru_hole circle
		(at 0 -7.62 90)
		(size 1.524 1.524)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" smd roundrect
		(at -2.54 -8.455 90)
		(size 2.432 1.524)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1)
		(thermal_bridge_angle 45)
	)
	(pad "5" thru_hole circle
		(at -2.54 -7.62 90)
		(size 1.524 1.524)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" smd roundrect
		(at -5.08 -8.455 90)
		(size 2.432 1.524)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1)
		(thermal_bridge_angle 45)
	)
	(pad "6" thru_hole circle
		(at -5.08 -7.62 90)
		(size 1.524 1.524)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" smd roundrect
		(at -7.62 -8.455 90)
		(size 2.432 1.524)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1)
		(thermal_bridge_angle 45)
	)
	(pad "7" thru_hole circle
		(at -7.62 -7.62 90)
		(size 1.524 1.524)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at -7.62 7.62 270)
		(size 1.524 1.524)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" smd roundrect
		(at -7.62 8.455 270)
		(size 2.432 1.524)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1)
		(thermal_bridge_angle 45)
	)
	(pad "9" thru_hole circle
		(at -5.08 7.62 270)
		(size 1.524 1.524)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" smd roundrect
		(at -5.08 8.455 270)
		(size 2.432 1.524)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1)
		(thermal_bridge_angle 45)
	)
	(pad "10" thru_hole circle
		(at -2.54 7.62 270)
		(size 1.524 1.524)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" smd roundrect
		(at -2.54 8.455 270)
		(size 2.432 1.524)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1)
		(thermal_bridge_angle 45)
	)
	(pad "11" thru_hole circle
		(at 0 7.62 270)
		(size 1.524 1.524)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" smd roundrect
		(at 0 8.455 270)
		(size 2.432 1.524)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1)
		(thermal_bridge_angle 45)
	)
	(pad "12" thru_hole circle
		(at 2.54 7.62 270)
		(size 1.524 1.524)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" smd roundrect
		(at 2.54 8.455 270)
		(size 2.432 1.524)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1)
		(thermal_bridge_angle 45)
	)
	(pad "13" thru_hole circle
		(at 5.08 7.62 270)
		(size 1.524 1.524)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "13" smd roundrect
		(at 5.08 8.455 270)
		(size 2.432 1.524)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1)
		(thermal_bridge_angle 45)
	)
	(pad "14" thru_hole circle
		(at 7.62 7.62 270)
		(size 1.524 1.524)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" smd roundrect
		(at 7.62 8.455 270)
		(size 2.432 1.524)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1)
		(thermal_bridge_angle 45)
	)
	(embedded_fonts no)
	(model "${AMZPATH}/3dmodels/AMz3D.3dshapes/XIAO-nRF52840 v15.step"
		(hide yes)
		(offset
			(xyz -1.778 -6.096 0.381)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
	(model "${AMZPATH}/3dmodels/AMz3D.3dshapes/Seeeduino XIAO SAMD21 v4.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	(model "${AMZPATH}/3dmodels/AMz3D.3dshapes/Seeed Studio XIAO RP2040 v26.step"
		(hide yes)
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 90)
		)
	)
	(model "${AMZPATH}/3dmodels/AMz3D.3dshapes/Seeed Studio XIAO-ESP32-C3.step"
		(hide yes)
		(offset
			(xyz -1.7018 -6.096 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
	(model "${AMZPATH}/3dmodels/AMz3D.3dshapes/XIAO-ESP32S3 v2.step"
		(hide yes)
		(offset
			(xyz -1.778 -6.1722 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
