<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.1">
<drawing>
<library>
<packages>
<package name="ST3215SB_32X15">
</package>
</packages>
<symbols>
<symbol name="ST3215SB">
<description>ST3215SB32768C0HPWBB
TUNING FORK CRYSTAL
32.768KHZ, 7PF, 3215</description>
<pin name="1"/>
<pin name="2"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="KYOCERAST3215SB">
<description>Kyocersa ST3215SB

AVX - ST3215SB32768C0HPWBB - TUNING FORK CRYSTAL, 32.768KHZ, 7PF, 3215 

TUNING FORK CRYSTAL, 32.768KHZ, 7PF, 3215
Frequency: 32.768kHz
Frequency Tolerance: ± 20ppm
Load Capacitance: 7pF
Operating Temperature Range: -40°C to +85°C
Crystal Mounting Type: SMD
No. of Pins: 2
Frequency Stability: 20ppm 

Datasheet: http://global.kyocera.com/prdct/electro/pdf/xtal/st3215sb_e.pdf</description>
<gates>
<gate name="G$1" symbol="ST3215SB"/>
</gates>
<devices>
<device name="" package="ST3215SB_32X15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
