<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.0">
<drawing>
<library>
<packages>
<package name="SO20W">
<description>&lt;b&gt;Wide Small Outline package&lt;/b&gt; 300 mil</description>
</package>
</packages>
<symbols>
<symbol name="ADM3053">
<pin name="R_S" direction="pas"/>
<pin name="GND2@0" direction="pwr"/>
<pin name="NC" direction="nc"/>
<pin name="GND1@0" direction="pwr"/>
<pin name="GND2@3" direction="pwr"/>
<pin name="CAN_H"/>
<pin name="CAN_L"/>
<pin name="V_ISOIN" direction="in"/>
<pin name="TXD" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="V_IO" direction="pwr"/>
<pin name="RXD" direction="out"/>
<pin name="GND1@1" direction="pwr"/>
<pin name="GND1@2" direction="pwr"/>
<pin name="GND1@3" direction="pwr"/>
<pin name="GND1@4" direction="pwr"/>
<pin name="GND2@1" direction="pwr"/>
<pin name="GND2@2" direction="pwr"/>
<pin name="V_REF" direction="out"/>
<pin name="V_ISOOUT" direction="out"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ADM3053" prefix="IC" uservalue="yes">
<description>&lt;b&gt;Signal and Power Isolated CAN Transceiver&lt;/b&gt;&lt;p&gt;

Analog Devices - Signal and Power Isolated CAN Transceiver
with Integrated Isolated DC-to-DC Converter</description>
<gates>
<gate name="G$1" symbol="ADM3053"/>
</gates>
<devices>
<device name="M" package="SO20W">
<connects>
<connect gate="G$1" pin="CAN_H" pad="17"/>
<connect gate="G$1" pin="CAN_L" pad="15"/>
<connect gate="G$1" pin="GND1@0" pad="1"/>
<connect gate="G$1" pin="GND1@1" pad="3"/>
<connect gate="G$1" pin="GND1@2" pad="7"/>
<connect gate="G$1" pin="GND1@3" pad="9"/>
<connect gate="G$1" pin="GND1@4" pad="10"/>
<connect gate="G$1" pin="GND2@0" pad="11"/>
<connect gate="G$1" pin="GND2@1" pad="13"/>
<connect gate="G$1" pin="GND2@2" pad="16"/>
<connect gate="G$1" pin="GND2@3" pad="20"/>
<connect gate="G$1" pin="NC" pad="2"/>
<connect gate="G$1" pin="RXD" pad="4"/>
<connect gate="G$1" pin="R_S" pad="18"/>
<connect gate="G$1" pin="TXD" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="V_IO" pad="6"/>
<connect gate="G$1" pin="V_ISOIN" pad="19"/>
<connect gate="G$1" pin="V_ISOOUT" pad="12"/>
<connect gate="G$1" pin="V_REF" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
