<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.1">
<drawing>
<library>
<description>Generated from &lt;b&gt;receiver.sch&lt;/b&gt;&lt;p&gt;
by exp-project-lbr.ulp</description>
<packages>
<package name="RECEIVER_MODUL_RECEIVER_MODUL">
<description>5.8 GHz Receiver from China. Version 1.0 . Sensity -90 dBm</description>
</package>
<package name="MAX4587">
</package>
<package name="TSH81">
</package>
<package name="GPS">
</package>
<package name="ADS7843">
</package>
<package name="LM1085">
</package>
<package name="S12B-ZR-SM4A-TF">
</package>
</packages>
<symbols>
<symbol name="RECEIVER_MODUL_5.8GHZ_RECEIVER">
<pin name="ANT" direction="in"/>
<pin name="AUDIO" direction="out"/>
<pin name="CH1" direction="in"/>
<pin name="CH2" direction="in"/>
<pin name="CH3" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND_A1" direction="pwr"/>
<pin name="GND_A2" direction="pwr"/>
<pin name="RSSI" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="VIDEO" direction="out"/>
</symbol>
<symbol name="MAX4587">
<pin name="NO4"/>
<pin name="NO3"/>
<pin name="GND"/>
<pin name="NO2"/>
<pin name="NO1"/>
<pin name="SCL"/>
<pin name="COM"/>
<pin name="A/CS"/>
<pin name="SDA"/>
<pin name="V+"/>
</symbol>
<symbol name="TSH81">
<pin name="+UB"/>
<pin name="/STBY"/>
<pin name="-"/>
<pin name="+"/>
<pin name="GND"/>
<pin name="OUT"/>
</symbol>
<symbol name="GPS">
<pin name="3D-FIX" direction="out"/>
<pin name="1PPS" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="RXD" direction="in"/>
<pin name="TXD" direction="out"/>
<pin name="VBACKUP" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="ADS7843">
<pin name="VCC"/>
<pin name="X+"/>
<pin name="Y+"/>
<pin name="X-"/>
<pin name="Y-"/>
<pin name="GND"/>
<pin name="IN3"/>
<pin name="IN4"/>
<pin name="DCLK"/>
<pin name="/CS"/>
<pin name="DIN"/>
<pin name="BUSY"/>
<pin name="DOUT"/>
<pin name="/PENIRQ"/>
<pin name="VCC(2)"/>
<pin name="VREF"/>
</symbol>
<symbol name="LM1085">
<pin name="VI"/>
<pin name="GND"/>
<pin name="VO"/>
</symbol>
<symbol name="JSTZH12">
<pin name="12"/>
<pin name="11"/>
<pin name="10"/>
<pin name="9"/>
<pin name="8"/>
<pin name="7"/>
<pin name="6"/>
<pin name="5"/>
<pin name="4"/>
<pin name="3"/>
<pin name="2"/>
<pin name="1"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="RECEIVER_MODUL_RX5808">
<description>RX5808 Receiver modul from China. -90dBm sensity. Power 5V.</description>
<gates>
<gate name="G$1" symbol="RECEIVER_MODUL_5.8GHZ_RECEIVER"/>
</gates>
<devices>
<device name="" package="RECEIVER_MODUL_RECEIVER_MODUL">
<connects>
<connect gate="G$1" pin="ANT" pad="ANT"/>
<connect gate="G$1" pin="AUDIO" pad="AUDIO"/>
<connect gate="G$1" pin="CH1" pad="CH1"/>
<connect gate="G$1" pin="CH2" pad="CH2"/>
<connect gate="G$1" pin="CH3" pad="CH3"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND1" pad="GND1"/>
<connect gate="G$1" pin="GND_A1" pad="GND_A1"/>
<connect gate="G$1" pin="GND_A2" pad="GND_A2"/>
<connect gate="G$1" pin="RSSI" pad="RSSI"/>
<connect gate="G$1" pin="VCC" pad="+5V"/>
<connect gate="G$1" pin="VIDEO" pad="VIDEO"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX4587">
<gates>
<gate name="G$1" symbol="MAX4587"/>
</gates>
<devices>
<device name="" package="MAX4587">
<connects>
<connect gate="G$1" pin="A/CS" pad="2"/>
<connect gate="G$1" pin="COM" pad="1"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="NO1" pad="6"/>
<connect gate="G$1" pin="NO2" pad="7"/>
<connect gate="G$1" pin="NO3" pad="9"/>
<connect gate="G$1" pin="NO4" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="V+" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TSH81">
<gates>
<gate name="G$1" symbol="TSH81"/>
</gates>
<devices>
<device name="" package="TSH81">
<connects>
<connect gate="G$1" pin="+" pad="3"/>
<connect gate="G$1" pin="+UB" pad="7"/>
<connect gate="G$1" pin="-" pad="2"/>
<connect gate="G$1" pin="/STBY" pad="8"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="OUT" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GPS">
<gates>
<gate name="G$1" symbol="GPS"/>
</gates>
<devices>
<device name="" package="GPS">
<connects>
<connect gate="G$1" pin="1PPS" pad="6"/>
<connect gate="G$1" pin="3D-FIX" pad="5"/>
<connect gate="G$1" pin="GND" pad="3 8 11 12 13"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="TXD" pad="9"/>
<connect gate="G$1" pin="VBACKUP" pad="4"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADS7843">
<gates>
<gate name="G$1" symbol="ADS7843"/>
</gates>
<devices>
<device name="" package="ADS7843">
<connects>
<connect gate="G$1" pin="/CS" pad="15"/>
<connect gate="G$1" pin="/PENIRQ" pad="11"/>
<connect gate="G$1" pin="BUSY" pad="13"/>
<connect gate="G$1" pin="DCLK" pad="16"/>
<connect gate="G$1" pin="DIN" pad="14"/>
<connect gate="G$1" pin="DOUT" pad="12"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="IN3" pad="7"/>
<connect gate="G$1" pin="IN4" pad="8"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="VCC(2)" pad="10"/>
<connect gate="G$1" pin="VREF" pad="9"/>
<connect gate="G$1" pin="X+" pad="2"/>
<connect gate="G$1" pin="X-" pad="4"/>
<connect gate="G$1" pin="Y+" pad="3"/>
<connect gate="G$1" pin="Y-" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1085">
<gates>
<gate name="G$1" symbol="LM1085"/>
</gates>
<devices>
<device name="" package="LM1085">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VI" pad="3"/>
<connect gate="G$1" pin="VO" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JSTZH12">
<gates>
<gate name="G$1" symbol="JSTZH12"/>
</gates>
<devices>
<device name="" package="S12B-ZR-SM4A-TF">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
