<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="100" y2="0" width="0" layer="20"/>
<wire x1="100" y1="0" x2="100" y2="80" width="0" layer="20"/>
<wire x1="100" y1="80" x2="0" y2="80" width="0" layer="20"/>
<wire x1="0" y1="80" x2="0" y2="0" width="0" layer="20"/>
<text>GBM32ST V1.0</text>
<text>AWA</text>
<text>AWA</text>
<text>2012</text>
<text>1</text>
<text>1</text>
</plain>
<libraries>
<library name="stm32">
<description>ST Cortex-M3 STM32F101/103 processor family  in LQFP100, 64, 48, BGA100, 64 and QFN36 pin versions</description>
<packages>
<package name="TQFP64">
</package>
</packages>
</library>
<library name="optocoupler">
<description>&lt;b&gt;Opto Couplers&lt;/b&gt;&lt;p&gt;
Siemens, Hewlett-Packard, Texas Instuments, Sharp, Motorola&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL04">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DO41-10">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2.54 mm, horizontal, grid 10.16 mm</description>
</package>
</packages>
</library>
<library name="resistor">
<description>&lt;b&gt;Resistors, Capacitors, Inductors&lt;/b&gt;&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;r.lbr
&lt;li&gt;cap.lbr 
&lt;li&gt;cap-fe.lbr
&lt;li&gt;captant.lbr
&lt;li&gt;polcap.lbr
&lt;li&gt;ipc-smd.lbr
&lt;/ul&gt;
All SMD packages are defined according to the IPC specifications and  CECC&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
for Electrolyt Capacitors see also :&lt;p&gt;
www.bccomponents.com &lt;p&gt;
www.panasonic.com&lt;p&gt;
www.kemet.com&lt;p&gt;
&lt;p&gt;
for trimmer refence see : &lt;u&gt;www.electrospec-inc.com/cross_references/trimpotcrossref.asp&lt;/u&gt;&lt;p&gt;

&lt;map name="nav_main"&gt;
&lt;area shape="rect" coords="0,1,140,23" href="../military_specs.asp" title=""&gt;
&lt;area shape="rect" coords="0,24,140,51" href="../about.asp" title=""&gt;
&lt;area shape="rect" coords="1,52,140,77" href="../rfq.asp" title=""&gt;
&lt;area shape="rect" coords="0,78,139,103" href="../products.asp" title=""&gt;
&lt;area shape="rect" coords="1,102,138,128" href="../excess_inventory.asp" title=""&gt;
&lt;area shape="rect" coords="1,129,138,150" href="../edge.asp" title=""&gt;
&lt;area shape="rect" coords="1,151,139,178" href="../industry_links.asp" title=""&gt;
&lt;area shape="rect" coords="0,179,139,201" href="../comments.asp" title=""&gt;
&lt;area shape="rect" coords="1,203,138,231" href="../directory.asp" title=""&gt;
&lt;area shape="default" nohref&gt;
&lt;/map&gt;

&lt;html&gt;

&lt;title&gt;&lt;/title&gt;

 &lt;LINK REL="StyleSheet" TYPE="text/css" HREF="style-sheet.css"&gt;

&lt;body bgcolor="#ffffff" text="#000000" marginwidth="0" marginheight="0" topmargin="0" leftmargin="0"&gt;
&lt;table border=0 cellspacing=0 cellpadding=0 width="100%" cellpaddding=0 height="55%"&gt;
&lt;tr valign="top"&gt;

&lt;/td&gt;
&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;TRIM-POT CROSS REFERENCE&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;RECTANGULAR MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BOURNS&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BI&amp;nbsp;TECH&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;DALE-VISHAY&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PHILIPS/MEPCO&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MURATA&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PANASONIC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;SPECTROL&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MILSPEC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;&lt;TD&gt;&amp;nbsp;&lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3 &gt;
      3005P&lt;BR&gt;
      3006P&lt;BR&gt;
      3006W&lt;BR&gt;
      3006Y&lt;BR&gt;
      3009P&lt;BR&gt;
      3009W&lt;BR&gt;
      3009Y&lt;BR&gt;
      3057J&lt;BR&gt;
      3057L&lt;BR&gt;
      3057P&lt;BR&gt;
      3057Y&lt;BR&gt;
      3059J&lt;BR&gt;
      3059L&lt;BR&gt;
      3059P&lt;BR&gt;
      3059Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      89P&lt;BR&gt;
      89W&lt;BR&gt;
      89X&lt;BR&gt;
      89PH&lt;BR&gt;
      76P&lt;BR&gt;
      89XH&lt;BR&gt;
      78SLT&lt;BR&gt;
      78L&amp;nbsp;ALT&lt;BR&gt;
      56P&amp;nbsp;ALT&lt;BR&gt;
      78P&amp;nbsp;ALT&lt;BR&gt;
      T8S&lt;BR&gt;
      78L&lt;BR&gt;
      56P&lt;BR&gt;
      78P&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      T18/784&lt;BR&gt;
      783&lt;BR&gt;
      781&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2199&lt;BR&gt;
      1697/1897&lt;BR&gt;
      1680/1880&lt;BR&gt;
      2187&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      8035EKP/CT20/RJ-20P&lt;BR&gt;
      -&lt;BR&gt;
      RJ-20X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      1211L&lt;BR&gt;
      8012EKQ&amp;nbsp;ALT&lt;BR&gt;
      8012EKR&amp;nbsp;ALT&lt;BR&gt;
      1211P&lt;BR&gt;
      8012EKJ&lt;BR&gt;
      8012EKL&lt;BR&gt;
      8012EKQ&lt;BR&gt;
      8012EKR&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      2101P&lt;BR&gt;
      2101W&lt;BR&gt;
      2101Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2102L&lt;BR&gt;
      2102S&lt;BR&gt;
      2102Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVMCOG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      43P&lt;BR&gt;
      43W&lt;BR&gt;
      43Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      40L&lt;BR&gt;
      40P&lt;BR&gt;
      40Y&lt;BR&gt;
      70Y-T602&lt;BR&gt;
      70L&lt;BR&gt;
      70P&lt;BR&gt;
      70Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SQUARE MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
   &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3250L&lt;BR&gt;
      3250P&lt;BR&gt;
      3250W&lt;BR&gt;
      3250X&lt;BR&gt;
      3252P&lt;BR&gt;
      3252W&lt;BR&gt;
      3252X&lt;BR&gt;
      3260P&lt;BR&gt;
      3260W&lt;BR&gt;
      3260X&lt;BR&gt;
      3262P&lt;BR&gt;
      3262W&lt;BR&gt;
      3262X&lt;BR&gt;
      3266P&lt;BR&gt;
      3266W&lt;BR&gt;
      3266X&lt;BR&gt;
      3290H&lt;BR&gt;
      3290P&lt;BR&gt;
      3290W&lt;BR&gt;
      3292P&lt;BR&gt;
      3292W&lt;BR&gt;
      3292X&lt;BR&gt;
      3296P&lt;BR&gt;
      3296W&lt;BR&gt;
      3296X&lt;BR&gt;
      3296Y&lt;BR&gt;
      3296Z&lt;BR&gt;
      3299P&lt;BR&gt;
      3299W&lt;BR&gt;
      3299X&lt;BR&gt;
      3299Y&lt;BR&gt;
      3299Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64P&amp;nbsp;ALT&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      64X&amp;nbsp;ALT&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66P&lt;BR&gt;
      66W&lt;BR&gt;
      66X&lt;BR&gt;
      67P&lt;BR&gt;
      67W&lt;BR&gt;
      67X&lt;BR&gt;
      67Y&lt;BR&gt;
      67Z&lt;BR&gt;
      68P&lt;BR&gt;
      68W&lt;BR&gt;
      68X&lt;BR&gt;
      67Y&amp;nbsp;ALT&lt;BR&gt;
      67Z&amp;nbsp;ALT&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      5050&lt;BR&gt;
      5091&lt;BR&gt;
      5080&lt;BR&gt;
      5087&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T63YB&lt;BR&gt;
      T63XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      5887&lt;BR&gt;
      5891&lt;BR&gt;
      5880&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T93Z&lt;BR&gt;
      T93YA&lt;BR&gt;
      T93XA&lt;BR&gt;
      T93YB&lt;BR&gt;
      T93XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKW&lt;BR&gt;
      8026EKM&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKB&lt;BR&gt;
      8026EKM&lt;BR&gt;
      1309X&lt;BR&gt;
      1309P&lt;BR&gt;
      1309W&lt;BR&gt;
      8024EKP&lt;BR&gt;
      8024EKW&lt;BR&gt;
      8024EKN&lt;BR&gt;
      RJ-9P/CT9P&lt;BR&gt;
      RJ-9W&lt;BR&gt;
      RJ-9X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3105P/3106P&lt;BR&gt;
      3105W/3106W&lt;BR&gt;
      3105X/3106X&lt;BR&gt;
      3105Y/3106Y&lt;BR&gt;
      3105Z/3105Z&lt;BR&gt;
      3102P&lt;BR&gt;
      3102W&lt;BR&gt;
      3102X&lt;BR&gt;
      3102Y&lt;BR&gt;
      3102Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMCBG&lt;BR&gt;
      EVMCCG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      55-1-X&lt;BR&gt;
      55-4-X&lt;BR&gt;
      55-3-X&lt;BR&gt;
      55-2-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      50-2-X&lt;BR&gt;
      50-4-X&lt;BR&gt;
      50-3-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      64Y&lt;BR&gt;
      64Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3323P&lt;BR&gt;
      3323S&lt;BR&gt;
      3323W&lt;BR&gt;
      3329H&lt;BR&gt;
      3329P&lt;BR&gt;
      3329W&lt;BR&gt;
      3339H&lt;BR&gt;
      3339P&lt;BR&gt;
      3339W&lt;BR&gt;
      3352E&lt;BR&gt;
      3352H&lt;BR&gt;
      3352K&lt;BR&gt;
      3352P&lt;BR&gt;
      3352T&lt;BR&gt;
      3352V&lt;BR&gt;
      3352W&lt;BR&gt;
      3362H&lt;BR&gt;
      3362M&lt;BR&gt;
      3362P&lt;BR&gt;
      3362R&lt;BR&gt;
      3362S&lt;BR&gt;
      3362U&lt;BR&gt;
      3362W&lt;BR&gt;
      3362X&lt;BR&gt;
      3386B&lt;BR&gt;
      3386C&lt;BR&gt;
      3386F&lt;BR&gt;
      3386H&lt;BR&gt;
      3386K&lt;BR&gt;
      3386M&lt;BR&gt;
      3386P&lt;BR&gt;
      3386S&lt;BR&gt;
      3386W&lt;BR&gt;
      3386X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      25P&lt;BR&gt;
      25S&lt;BR&gt;
      25RX&lt;BR&gt;
      82P&lt;BR&gt;
      82M&lt;BR&gt;
      82PA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      91E&lt;BR&gt;
      91X&lt;BR&gt;
      91T&lt;BR&gt;
      91B&lt;BR&gt;
      91A&lt;BR&gt;
      91V&lt;BR&gt;
      91W&lt;BR&gt;
      25W&lt;BR&gt;
      25V&lt;BR&gt;
      25P&lt;BR&gt;
      -&lt;BR&gt;
      25S&lt;BR&gt;
      25U&lt;BR&gt;
      25RX&lt;BR&gt;
      25X&lt;BR&gt;
      72XW&lt;BR&gt;
      72XL&lt;BR&gt;
      72PM&lt;BR&gt;
      72RX&lt;BR&gt;
      -&lt;BR&gt;
      72PX&lt;BR&gt;
      72P&lt;BR&gt;
      72RXW&lt;BR&gt;
      72RXL&lt;BR&gt;
      72X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T7YB&lt;BR&gt;
      T7YA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      TXD&lt;BR&gt;
      TYA&lt;BR&gt;
      TYP&lt;BR&gt;
      -&lt;BR&gt;
      TYD&lt;BR&gt;
      TX&lt;BR&gt;
      -&lt;BR&gt;
      150SX&lt;BR&gt;
      100SX&lt;BR&gt;
      102T&lt;BR&gt;
      101S&lt;BR&gt;
      190T&lt;BR&gt;
      150TX&lt;BR&gt;
      101&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      101SX&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ET6P&lt;BR&gt;
      ET6S&lt;BR&gt;
      ET6X&lt;BR&gt;
      RJ-6W/8014EMW&lt;BR&gt;
      RJ-6P/8014EMP&lt;BR&gt;
      RJ-6X/8014EMX&lt;BR&gt;
      TM7W&lt;BR&gt;
      TM7P&lt;BR&gt;
      TM7X&lt;BR&gt;
      -&lt;BR&gt;
      8017SMS&lt;BR&gt;
      -&lt;BR&gt;
      8017SMB&lt;BR&gt;
      8017SMA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      CT-6W&lt;BR&gt;
      CT-6H&lt;BR&gt;
      CT-6P&lt;BR&gt;
      CT-6R&lt;BR&gt;
      -&lt;BR&gt;
      CT-6V&lt;BR&gt;
      CT-6X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKV&lt;BR&gt;
      -&lt;BR&gt;
      8038EKX&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKP&lt;BR&gt;
      8038EKZ&lt;BR&gt;
      8038EKW&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3321H&lt;BR&gt;
      3321P&lt;BR&gt;
      3321N&lt;BR&gt;
      1102H&lt;BR&gt;
      1102P&lt;BR&gt;
      1102T&lt;BR&gt;
      RVA0911V304A&lt;BR&gt;
      -&lt;BR&gt;
      RVA0911H413A&lt;BR&gt;
      RVG0707V100A&lt;BR&gt;
      RVA0607V(H)306A&lt;BR&gt;
      RVA1214H213A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3104B&lt;BR&gt;
      3104C&lt;BR&gt;
      3104F&lt;BR&gt;
      3104H&lt;BR&gt;
      -&lt;BR&gt;
      3104M&lt;BR&gt;
      3104P&lt;BR&gt;
      3104S&lt;BR&gt;
      3104W&lt;BR&gt;
      3104X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      EVMQ0G&lt;BR&gt;
      EVMQIG&lt;BR&gt;
      EVMQ3G&lt;BR&gt;
      EVMS0G&lt;BR&gt;
      EVMQ0G&lt;BR&gt;
      EVMG0G&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMK4GA00B&lt;BR&gt;
      EVM30GA00B&lt;BR&gt;
      EVMK0GA00B&lt;BR&gt;
      EVM38GA00B&lt;BR&gt;
      EVMB6&lt;BR&gt;
      EVLQ0&lt;BR&gt;
      -&lt;BR&gt;
      EVMMSG&lt;BR&gt;
      EVMMBG&lt;BR&gt;
      EVMMAG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMMCS&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM0&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM3&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      62-3-1&lt;BR&gt;
      62-1-2&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67R&lt;BR&gt;
      -&lt;BR&gt;
      67P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67X&lt;BR&gt;
      63V&lt;BR&gt;
      63S&lt;BR&gt;
      63M&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63H&lt;BR&gt;
      63P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;&amp;nbsp;&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=3&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT color="#0000FF" SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SMD TRIM-POT CROSS REFERENCE&lt;/B&gt;&lt;/FONT&gt;
      &lt;P&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3224G&lt;BR&gt;
      3224J&lt;BR&gt;
      3224W&lt;BR&gt;
      3269P&lt;BR&gt;
      3269W&lt;BR&gt;
      3269X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      44G&lt;BR&gt;
      44J&lt;BR&gt;
      44W&lt;BR&gt;
      84P&lt;BR&gt;
      84W&lt;BR&gt;
      84X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST63Z&lt;BR&gt;
      ST63Y&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST5P&lt;BR&gt;
      ST5W&lt;BR&gt;
      ST5X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3314G&lt;BR&gt;
      3314J&lt;BR&gt;
      3364A/B&lt;BR&gt;
      3364C/D&lt;BR&gt;
      3364W/X&lt;BR&gt;
      3313G&lt;BR&gt;
      3313J&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      23B&lt;BR&gt;
      23A&lt;BR&gt;
      21X&lt;BR&gt;
      21W&lt;BR&gt;
      -&lt;BR&gt;
      22B&lt;BR&gt;
      22A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST5YL/ST53YL&lt;BR&gt;
      ST5YJ/5T53YJ&lt;BR&gt;
      ST-23A&lt;BR&gt;
      ST-22B&lt;BR&gt;
      ST-22&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST-4B&lt;BR&gt;
      ST-4A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST-3B&lt;BR&gt;
      ST-3A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVM-6YS&lt;BR&gt;
      EVM-1E&lt;BR&gt;
      EVM-1G&lt;BR&gt;
      EVM-1D&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      G4B&lt;BR&gt;
      G4A&lt;BR&gt;
      TR04-3S1&lt;BR&gt;
      TRG04-2S1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      DVR-43A&lt;BR&gt;
      CVR-42C&lt;BR&gt;
      CVR-42A/C&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;
&lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;ALT =&amp;nbsp;ALTERNATE&lt;/B&gt;&lt;/FONT&gt;
&lt;P&gt;

&amp;nbsp;
&lt;P&gt;
&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;
&lt;/BODY&gt;&lt;/HTML&gt;</description>
<packages>
<package name="M0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.10 W</description>
</package>
<package name="CT6032">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip
tantalum</description>
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="JP1">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
</package>
<package name="JP5Q">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
</package>
<package name="JP4">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
</package>
<package name="SJ">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
<package name="SJ_2">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2,8">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 2.8 mm with drill center</description>
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="SML0603">
<description>&lt;b&gt;SML0603-XXX (HIGH INTENSITY) LED&lt;/b&gt;&lt;p&gt;
&lt;table&gt;
&lt;tr&gt;&lt;td&gt;AG3K&lt;/td&gt;&lt;td&gt;AQUA GREEN&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;B1K&lt;/td&gt;&lt;td&gt;SUPER BLUE&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;R1K&lt;/td&gt;&lt;td&gt;SUPER RED&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;R3K&lt;/td&gt;&lt;td&gt;ULTRA RED&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;O3K&lt;/td&gt;&lt;td&gt;SUPER ORANGE&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;O3KH&lt;/td&gt;&lt;td&gt;SOFT ORANGE&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;Y3KH&lt;/td&gt;&lt;td&gt;SUPER YELLOW&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;Y3K&lt;/td&gt;&lt;td&gt;SUPER YELLOW&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;2CW&lt;/td&gt;&lt;td&gt;WHITE&lt;/td&gt;&lt;/tr&gt;
&lt;/table&gt;
Source: http://www.ledtronics.com/ds/smd-0603/Dstr0092.pdf</description>
</package>
</packages>
</library>
<library name="burr-brown">
<description>&lt;b&gt;Burr-Brown Components&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT223">
<description>&lt;b&gt;Smal Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="rcl">
<description>&lt;b&gt;Resistors, Capacitors, Inductors&lt;/b&gt;&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;r.lbr
&lt;li&gt;cap.lbr 
&lt;li&gt;cap-fe.lbr
&lt;li&gt;captant.lbr
&lt;li&gt;polcap.lbr
&lt;li&gt;ipc-smd.lbr
&lt;/ul&gt;
All SMD packages are defined according to the IPC specifications and  CECC&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
for Electrolyt Capacitors see also :&lt;p&gt;
www.bccomponents.com &lt;p&gt;
www.panasonic.com&lt;p&gt;
www.kemet.com&lt;p&gt;
http://www.secc.co.jp/pdf/os_e/2004/e_os_all.pdf &lt;b&gt;(SANYO)&lt;/b&gt;
&lt;p&gt;
for trimmer refence see : &lt;u&gt;www.electrospec-inc.com/cross_references/trimpotcrossref.asp&lt;/u&gt;&lt;p&gt;

&lt;table border=0 cellspacing=0 cellpadding=0 width="100%" cellpaddding=0&gt;
&lt;tr valign="top"&gt;

&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;TRIM-POT CROSS REFERENCE&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;RECTANGULAR MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BOURNS&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BI&amp;nbsp;TECH&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;DALE-VISHAY&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PHILIPS/MEPCO&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MURATA&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PANASONIC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;SPECTROL&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MILSPEC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;&lt;TD&gt;&amp;nbsp;&lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3 &gt;
      3005P&lt;BR&gt;
      3006P&lt;BR&gt;
      3006W&lt;BR&gt;
      3006Y&lt;BR&gt;
      3009P&lt;BR&gt;
      3009W&lt;BR&gt;
      3009Y&lt;BR&gt;
      3057J&lt;BR&gt;
      3057L&lt;BR&gt;
      3057P&lt;BR&gt;
      3057Y&lt;BR&gt;
      3059J&lt;BR&gt;
      3059L&lt;BR&gt;
      3059P&lt;BR&gt;
      3059Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      89P&lt;BR&gt;
      89W&lt;BR&gt;
      89X&lt;BR&gt;
      89PH&lt;BR&gt;
      76P&lt;BR&gt;
      89XH&lt;BR&gt;
      78SLT&lt;BR&gt;
      78L&amp;nbsp;ALT&lt;BR&gt;
      56P&amp;nbsp;ALT&lt;BR&gt;
      78P&amp;nbsp;ALT&lt;BR&gt;
      T8S&lt;BR&gt;
      78L&lt;BR&gt;
      56P&lt;BR&gt;
      78P&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      T18/784&lt;BR&gt;
      783&lt;BR&gt;
      781&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2199&lt;BR&gt;
      1697/1897&lt;BR&gt;
      1680/1880&lt;BR&gt;
      2187&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      8035EKP/CT20/RJ-20P&lt;BR&gt;
      -&lt;BR&gt;
      RJ-20X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      1211L&lt;BR&gt;
      8012EKQ&amp;nbsp;ALT&lt;BR&gt;
      8012EKR&amp;nbsp;ALT&lt;BR&gt;
      1211P&lt;BR&gt;
      8012EKJ&lt;BR&gt;
      8012EKL&lt;BR&gt;
      8012EKQ&lt;BR&gt;
      8012EKR&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      2101P&lt;BR&gt;
      2101W&lt;BR&gt;
      2101Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2102L&lt;BR&gt;
      2102S&lt;BR&gt;
      2102Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVMCOG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      43P&lt;BR&gt;
      43W&lt;BR&gt;
      43Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      40L&lt;BR&gt;
      40P&lt;BR&gt;
      40Y&lt;BR&gt;
      70Y-T602&lt;BR&gt;
      70L&lt;BR&gt;
      70P&lt;BR&gt;
      70Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SQUARE MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
   &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3250L&lt;BR&gt;
      3250P&lt;BR&gt;
      3250W&lt;BR&gt;
      3250X&lt;BR&gt;
      3252P&lt;BR&gt;
      3252W&lt;BR&gt;
      3252X&lt;BR&gt;
      3260P&lt;BR&gt;
      3260W&lt;BR&gt;
      3260X&lt;BR&gt;
      3262P&lt;BR&gt;
      3262W&lt;BR&gt;
      3262X&lt;BR&gt;
      3266P&lt;BR&gt;
      3266W&lt;BR&gt;
      3266X&lt;BR&gt;
      3290H&lt;BR&gt;
      3290P&lt;BR&gt;
      3290W&lt;BR&gt;
      3292P&lt;BR&gt;
      3292W&lt;BR&gt;
      3292X&lt;BR&gt;
      3296P&lt;BR&gt;
      3296W&lt;BR&gt;
      3296X&lt;BR&gt;
      3296Y&lt;BR&gt;
      3296Z&lt;BR&gt;
      3299P&lt;BR&gt;
      3299W&lt;BR&gt;
      3299X&lt;BR&gt;
      3299Y&lt;BR&gt;
      3299Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64P&amp;nbsp;ALT&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      64X&amp;nbsp;ALT&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66P&lt;BR&gt;
      66W&lt;BR&gt;
      66X&lt;BR&gt;
      67P&lt;BR&gt;
      67W&lt;BR&gt;
      67X&lt;BR&gt;
      67Y&lt;BR&gt;
      67Z&lt;BR&gt;
      68P&lt;BR&gt;
      68W&lt;BR&gt;
      68X&lt;BR&gt;
      67Y&amp;nbsp;ALT&lt;BR&gt;
      67Z&amp;nbsp;ALT&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      5050&lt;BR&gt;
      5091&lt;BR&gt;
      5080&lt;BR&gt;
      5087&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T63YB&lt;BR&gt;
      T63XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      5887&lt;BR&gt;
      5891&lt;BR&gt;
      5880&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T93Z&lt;BR&gt;
      T93YA&lt;BR&gt;
      T93XA&lt;BR&gt;
      T93YB&lt;BR&gt;
      T93XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKW&lt;BR&gt;
      8026EKM&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKB&lt;BR&gt;
      8026EKM&lt;BR&gt;
      1309X&lt;BR&gt;
      1309P&lt;BR&gt;
      1309W&lt;BR&gt;
      8024EKP&lt;BR&gt;
      8024EKW&lt;BR&gt;
      8024EKN&lt;BR&gt;
      RJ-9P/CT9P&lt;BR&gt;
      RJ-9W&lt;BR&gt;
      RJ-9X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3105P/3106P&lt;BR&gt;
      3105W/3106W&lt;BR&gt;
      3105X/3106X&lt;BR&gt;
      3105Y/3106Y&lt;BR&gt;
      3105Z/3105Z&lt;BR&gt;
      3102P&lt;BR&gt;
      3102W&lt;BR&gt;
      3102X&lt;BR&gt;
      3102Y&lt;BR&gt;
      3102Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMCBG&lt;BR&gt;
      EVMCCG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      55-1-X&lt;BR&gt;
      55-4-X&lt;BR&gt;
      55-3-X&lt;BR&gt;
      55-2-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      50-2-X&lt;BR&gt;
      50-4-X&lt;BR&gt;
      50-3-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      64Y&lt;BR&gt;
      64Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3323P&lt;BR&gt;
      3323S&lt;BR&gt;
      3323W&lt;BR&gt;
      3329H&lt;BR&gt;
      3329P&lt;BR&gt;
      3329W&lt;BR&gt;
      3339H&lt;BR&gt;
      3339P&lt;BR&gt;
      3339W&lt;BR&gt;
      3352E&lt;BR&gt;
      3352H&lt;BR&gt;
      3352K&lt;BR&gt;
      3352P&lt;BR&gt;
      3352T&lt;BR&gt;
      3352V&lt;BR&gt;
      3352W&lt;BR&gt;
      3362H&lt;BR&gt;
      3362M&lt;BR&gt;
      3362P&lt;BR&gt;
      3362R&lt;BR&gt;
      3362S&lt;BR&gt;
      3362U&lt;BR&gt;
      3362W&lt;BR&gt;
      3362X&lt;BR&gt;
      3386B&lt;BR&gt;
      3386C&lt;BR&gt;
      3386F&lt;BR&gt;
      3386H&lt;BR&gt;
      3386K&lt;BR&gt;
      3386M&lt;BR&gt;
      3386P&lt;BR&gt;
      3386S&lt;BR&gt;
      3386W&lt;BR&gt;
      3386X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      25P&lt;BR&gt;
      25S&lt;BR&gt;
      25RX&lt;BR&gt;
      82P&lt;BR&gt;
      82M&lt;BR&gt;
      82PA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      91E&lt;BR&gt;
      91X&lt;BR&gt;
      91T&lt;BR&gt;
      91B&lt;BR&gt;
      91A&lt;BR&gt;
      91V&lt;BR&gt;
      91W&lt;BR&gt;
      25W&lt;BR&gt;
      25V&lt;BR&gt;
      25P&lt;BR&gt;
      -&lt;BR&gt;
      25S&lt;BR&gt;
      25U&lt;BR&gt;
      25RX&lt;BR&gt;
      25X&lt;BR&gt;
      72XW&lt;BR&gt;
      72XL&lt;BR&gt;
      72PM&lt;BR&gt;
      72RX&lt;BR&gt;
      -&lt;BR&gt;
      72PX&lt;BR&gt;
      72P&lt;BR&gt;
      72RXW&lt;BR&gt;
      72RXL&lt;BR&gt;
      72X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T7YB&lt;BR&gt;
      T7YA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      TXD&lt;BR&gt;
      TYA&lt;BR&gt;
      TYP&lt;BR&gt;
      -&lt;BR&gt;
      TYD&lt;BR&gt;
      TX&lt;BR&gt;
      -&lt;BR&gt;
      150SX&lt;BR&gt;
      100SX&lt;BR&gt;
      102T&lt;BR&gt;
      101S&lt;BR&gt;
      190T&lt;BR&gt;
      150TX&lt;BR&gt;
      101&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      101SX&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ET6P&lt;BR&gt;
      ET6S&lt;BR&gt;
      ET6X&lt;BR&gt;
      RJ-6W/8014EMW&lt;BR&gt;
      RJ-6P/8014EMP&lt;BR&gt;
      RJ-6X/8014EMX&lt;BR&gt;
      TM7W&lt;BR&gt;
      TM7P&lt;BR&gt;
      TM7X&lt;BR&gt;
      -&lt;BR&gt;
      8017SMS&lt;BR&gt;
      -&lt;BR&gt;
      8017SMB&lt;BR&gt;
      8017SMA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      CT-6W&lt;BR&gt;
      CT-6H&lt;BR&gt;
      CT-6P&lt;BR&gt;
      CT-6R&lt;BR&gt;
      -&lt;BR&gt;
      CT-6V&lt;BR&gt;
      CT-6X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKV&lt;BR&gt;
      -&lt;BR&gt;
      8038EKX&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKP&lt;BR&gt;
      8038EKZ&lt;BR&gt;
      8038EKW&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3321H&lt;BR&gt;
      3321P&lt;BR&gt;
      3321N&lt;BR&gt;
      1102H&lt;BR&gt;
      1102P&lt;BR&gt;
      1102T&lt;BR&gt;
      RVA0911V304A&lt;BR&gt;
      -&lt;BR&gt;
      RVA0911H413A&lt;BR&gt;
      RVG0707V100A&lt;BR&gt;
      RVA0607V(H)306A&lt;BR&gt;
      RVA1214H213A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3104B&lt;BR&gt;
      3104C&lt;BR&gt;
      3104F&lt;BR&gt;
      3104H&lt;BR&gt;
      -&lt;BR&gt;
      3104M&lt;BR&gt;
      3104P&lt;BR&gt;
      3104S&lt;BR&gt;
      3104W&lt;BR&gt;
      3104X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      EVMQ0G&lt;BR&gt;
      EVMQIG&lt;BR&gt;
      EVMQ3G&lt;BR&gt;
      EVMS0G&lt;BR&gt;
      EVMQ0G&lt;BR&gt;
      EVMG0G&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMK4GA00B&lt;BR&gt;
      EVM30GA00B&lt;BR&gt;
      EVMK0GA00B&lt;BR&gt;
      EVM38GA00B&lt;BR&gt;
      EVMB6&lt;BR&gt;
      EVLQ0&lt;BR&gt;
      -&lt;BR&gt;
      EVMMSG&lt;BR&gt;
      EVMMBG&lt;BR&gt;
      EVMMAG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMMCS&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM0&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM3&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      62-3-1&lt;BR&gt;
      62-1-2&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67R&lt;BR&gt;
      -&lt;BR&gt;
      67P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67X&lt;BR&gt;
      63V&lt;BR&gt;
      63S&lt;BR&gt;
      63M&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63H&lt;BR&gt;
      63P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;&amp;nbsp;&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=3&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT color="#0000FF" SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SMD TRIM-POT CROSS REFERENCE&lt;/B&gt;&lt;/FONT&gt;
      &lt;P&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3224G&lt;BR&gt;
      3224J&lt;BR&gt;
      3224W&lt;BR&gt;
      3269P&lt;BR&gt;
      3269W&lt;BR&gt;
      3269X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      44G&lt;BR&gt;
      44J&lt;BR&gt;
      44W&lt;BR&gt;
      84P&lt;BR&gt;
      84W&lt;BR&gt;
      84X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST63Z&lt;BR&gt;
      ST63Y&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST5P&lt;BR&gt;
      ST5W&lt;BR&gt;
      ST5X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3314G&lt;BR&gt;
      3314J&lt;BR&gt;
      3364A/B&lt;BR&gt;
      3364C/D&lt;BR&gt;
      3364W/X&lt;BR&gt;
      3313G&lt;BR&gt;
      3313J&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      23B&lt;BR&gt;
      23A&lt;BR&gt;
      21X&lt;BR&gt;
      21W&lt;BR&gt;
      -&lt;BR&gt;
      22B&lt;BR&gt;
      22A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST5YL/ST53YL&lt;BR&gt;
      ST5YJ/5T53YJ&lt;BR&gt;
      ST-23A&lt;BR&gt;
      ST-22B&lt;BR&gt;
      ST-22&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST-4B&lt;BR&gt;
      ST-4A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST-3B&lt;BR&gt;
      ST-3A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVM-6YS&lt;BR&gt;
      EVM-1E&lt;BR&gt;
      EVM-1G&lt;BR&gt;
      EVM-1D&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      G4B&lt;BR&gt;
      G4A&lt;BR&gt;
      TR04-3S1&lt;BR&gt;
      TRG04-2S1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      DVR-43A&lt;BR&gt;
      CVR-42C&lt;BR&gt;
      CVR-42A/C&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;
&lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;ALT =&amp;nbsp;ALTERNATE&lt;/B&gt;&lt;/FONT&gt;
&lt;P&gt;

&amp;nbsp;
&lt;P&gt;
&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;</description>
<packages>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
</packages>
</library>
<library name="switch-omron">
<description>&lt;b&gt;Omron Switches&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="B3F-10XX">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-tycoelectronics">
<description>&lt;b&gt;Tyco Electronics Connector&lt;/b&gt;&lt;p&gt;
http://catalog.tycoelectronics.com&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="RJ45-NO-SHIELD">
<description>&lt;b&gt;RJ45 Low Profile&lt;/b&gt; No Shield&lt;p&gt;
For all RJ45 N and Z Series Models&lt;br&gt;
Source: www.tycoelectronics.com .. ENG_DS_1654001_1099_RJ_L_0507.pdf</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="stm32" package="TQFP64" value="STM32F10XRXT6"/>
<element name="OK1" library="optocoupler" package="DIL04" value="PC817">
<attribute name="OC_NEWARK" value="97K7059"/>
<attribute name="MPN" value="PC817X4J000F"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="9707727"/>
</element>
<element name="OK2" library="optocoupler" package="DIL04" value="PC817">
<attribute name="OC_NEWARK" value="97K7059"/>
<attribute name="MPN" value="PC817X4J000F"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="9707727"/>
</element>
<element name="OK3" library="optocoupler" package="DIL04" value="PC817">
<attribute name="OC_NEWARK" value="97K7059"/>
<attribute name="MPN" value="PC817X4J000F"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="9707727"/>
</element>
<element name="OK4" library="optocoupler" package="DIL04" value="PC817">
<attribute name="OC_NEWARK" value="97K7059"/>
<attribute name="MPN" value="PC817X4J000F"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="9707727"/>
</element>
<element name="OK5" library="optocoupler" package="DIL04" value="PC817">
<attribute name="OC_NEWARK" value="97K7059"/>
<attribute name="MPN" value="PC817X4J000F"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="9707727"/>
</element>
<element name="OK6" library="optocoupler" package="DIL04" value="PC817">
<attribute name="OC_NEWARK" value="97K7059"/>
<attribute name="MPN" value="PC817X4J000F"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="9707727"/>
</element>
<element name="OK7" library="optocoupler" package="DIL04" value="PC817">
<attribute name="OC_NEWARK" value="97K7059"/>
<attribute name="MPN" value="PC817X4J000F"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="9707727"/>
</element>
<element name="OK8" library="optocoupler" package="DIL04" value="PC817">
<attribute name="OC_NEWARK" value="97K7059"/>
<attribute name="MPN" value="PC817X4J000F"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="9707727"/>
</element>
<element name="OK9" library="optocoupler" package="DIL04" value="PC817">
<attribute name="OC_NEWARK" value="97K7059"/>
<attribute name="MPN" value="PC817X4J000F"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="9707727"/>
</element>
<element name="OK10" library="optocoupler" package="DIL04" value="PC817">
<attribute name="OC_NEWARK" value="97K7059"/>
<attribute name="MPN" value="PC817X4J000F"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="9707727"/>
</element>
<element name="OK11" library="optocoupler" package="DIL04" value="PC817">
<attribute name="OC_NEWARK" value="97K7059"/>
<attribute name="MPN" value="PC817X4J000F"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="9707727"/>
</element>
<element name="OK12" library="optocoupler" package="DIL04" value="PC817">
<attribute name="OC_NEWARK" value="97K7059"/>
<attribute name="MPN" value="PC817X4J000F"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="9707727"/>
</element>
<element name="OK13" library="optocoupler" package="DIL04" value="PC817">
<attribute name="OC_NEWARK" value="97K7059"/>
<attribute name="MPN" value="PC817X4J000F"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="9707727"/>
</element>
<element name="OK14" library="optocoupler" package="DIL04" value="PC817">
<attribute name="OC_NEWARK" value="97K7059"/>
<attribute name="MPN" value="PC817X4J000F"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="9707727"/>
</element>
<element name="OK15" library="optocoupler" package="DIL04" value="PC817">
<attribute name="OC_NEWARK" value="97K7059"/>
<attribute name="MPN" value="PC817X4J000F"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="9707727"/>
</element>
<element name="OK16" library="optocoupler" package="DIL04" value="PC817">
<attribute name="OC_NEWARK" value="97K7059"/>
<attribute name="MPN" value="PC817X4J000F"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="9707727"/>
</element>
<element name="OK17" library="optocoupler" package="DIL04" value="PC817">
<attribute name="OC_NEWARK" value="97K7059"/>
<attribute name="MPN" value="PC817X4J000F"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="9707727"/>
</element>
<element name="OK18" library="optocoupler" package="DIL04" value="PC817">
<attribute name="OC_NEWARK" value="97K7059"/>
<attribute name="MPN" value="PC817X4J000F"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="9707727"/>
</element>
<element name="OK19" library="optocoupler" package="DIL04" value="PC817">
<attribute name="OC_NEWARK" value="97K7059"/>
<attribute name="MPN" value="PC817X4J000F"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="9707727"/>
</element>
<element name="OK20" library="optocoupler" package="DIL04" value="PC817">
<attribute name="OC_NEWARK" value="97K7059"/>
<attribute name="MPN" value="PC817X4J000F"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="9707727"/>
</element>
<element name="OK21" library="optocoupler" package="DIL04" value="PC817">
<attribute name="OC_NEWARK" value="97K7059"/>
<attribute name="MPN" value="PC817X4J000F"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="9707727"/>
</element>
<element name="OK22" library="optocoupler" package="DIL04" value="PC817">
<attribute name="OC_NEWARK" value="97K7059"/>
<attribute name="MPN" value="PC817X4J000F"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="9707727"/>
</element>
<element name="OK23" library="optocoupler" package="DIL04" value="PC817">
<attribute name="OC_NEWARK" value="97K7059"/>
<attribute name="MPN" value="PC817X4J000F"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="9707727"/>
</element>
<element name="OK24" library="optocoupler" package="DIL04" value="PC817">
<attribute name="OC_NEWARK" value="97K7059"/>
<attribute name="MPN" value="PC817X4J000F"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="9707727"/>
</element>
<element name="OK25" library="optocoupler" package="DIL04" value="PC817">
<attribute name="OC_NEWARK" value="97K7059"/>
<attribute name="MPN" value="PC817X4J000F"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="9707727"/>
</element>
<element name="OK26" library="optocoupler" package="DIL04" value="PC817">
<attribute name="OC_NEWARK" value="97K7059"/>
<attribute name="MPN" value="PC817X4J000F"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="9707727"/>
</element>
<element name="OK27" library="optocoupler" package="DIL04" value="PC817">
<attribute name="OC_NEWARK" value="97K7059"/>
<attribute name="MPN" value="PC817X4J000F"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="9707727"/>
</element>
<element name="OK28" library="optocoupler" package="DIL04" value="PC817">
<attribute name="OC_NEWARK" value="97K7059"/>
<attribute name="MPN" value="PC817X4J000F"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="9707727"/>
</element>
<element name="OK29" library="optocoupler" package="DIL04" value="PC817">
<attribute name="OC_NEWARK" value="97K7059"/>
<attribute name="MPN" value="PC817X4J000F"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="9707727"/>
</element>
<element name="OK30" library="optocoupler" package="DIL04" value="PC817">
<attribute name="OC_NEWARK" value="97K7059"/>
<attribute name="MPN" value="PC817X4J000F"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="9707727"/>
</element>
<element name="OK31" library="optocoupler" package="DIL04" value="PC817">
<attribute name="OC_NEWARK" value="97K7059"/>
<attribute name="MPN" value="PC817X4J000F"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="9707727"/>
</element>
<element name="OK32" library="optocoupler" package="DIL04" value="PC817">
<attribute name="OC_NEWARK" value="97K7059"/>
<attribute name="MPN" value="PC817X4J000F"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="9707727"/>
</element>
<element name="D1" library="diode" package="DO41-10" value="1N4004"/>
<element name="D2" library="diode" package="DO41-10" value="1N4004"/>
<element name="D3" library="diode" package="DO41-10" value="1N4004"/>
<element name="D4" library="diode" package="DO41-10" value="1N4004"/>
<element name="R1" library="resistor" package="M0805" value="680R"/>
<element name="JP1" library="jumper" package="JP1" value=""/>
<element name="D5" library="diode" package="DO41-10" value="1N4004"/>
<element name="D6" library="diode" package="DO41-10" value="1N4004"/>
<element name="D7" library="diode" package="DO41-10" value="1N4004"/>
<element name="D8" library="diode" package="DO41-10" value="1N4004"/>
<element name="R2" library="resistor" package="M0805" value="680R"/>
<element name="JP2" library="jumper" package="JP1" value=""/>
<element name="H1" library="holes" package="2,8" value="MOUNT-HOLE2.8"/>
<element name="H2" library="holes" package="2,8" value="MOUNT-HOLE2.8"/>
<element name="H3" library="holes" package="2,8" value="MOUNT-HOLE2.8"/>
<element name="H4" library="holes" package="2,8" value="MOUNT-HOLE2.8"/>
<element name="JP3" library="jumper" package="JP5Q" value=""/>
<element name="JP4" library="jumper" package="JP1" value=""/>
<element name="LED1" library="led" package="SML0603" value=""/>
<element name="R3" library="resistor" package="M0805" value=""/>
<element name="LED2" library="led" package="SML0603" value=""/>
<element name="R4" library="resistor" package="M0805" value=""/>
<element name="D9" library="diode" package="DO41-10" value="1N4004"/>
<element name="D10" library="diode" package="DO41-10" value="1N4004"/>
<element name="D11" library="diode" package="DO41-10" value="1N4004"/>
<element name="D12" library="diode" package="DO41-10" value="1N4004"/>
<element name="R5" library="resistor" package="M0805" value="680R"/>
<element name="JP5" library="jumper" package="JP1" value=""/>
<element name="D13" library="diode" package="DO41-10" value="1N4004"/>
<element name="D14" library="diode" package="DO41-10" value="1N4004"/>
<element name="D15" library="diode" package="DO41-10" value="1N4004"/>
<element name="D16" library="diode" package="DO41-10" value="1N4004"/>
<element name="R6" library="resistor" package="M0805" value="680R"/>
<element name="JP6" library="jumper" package="JP1" value=""/>
<element name="D17" library="diode" package="DO41-10" value="1N4004"/>
<element name="D18" library="diode" package="DO41-10" value="1N4004"/>
<element name="D19" library="diode" package="DO41-10" value="1N4004"/>
<element name="D20" library="diode" package="DO41-10" value="1N4004"/>
<element name="R7" library="resistor" package="M0805" value="680R"/>
<element name="JP7" library="jumper" package="JP1" value=""/>
<element name="D21" library="diode" package="DO41-10" value="1N4004"/>
<element name="D22" library="diode" package="DO41-10" value="1N4004"/>
<element name="D23" library="diode" package="DO41-10" value="1N4004"/>
<element name="D24" library="diode" package="DO41-10" value="1N4004"/>
<element name="R8" library="resistor" package="M0805" value="680R"/>
<element name="JP8" library="jumper" package="JP1" value=""/>
<element name="D25" library="diode" package="DO41-10" value="1N4004"/>
<element name="D26" library="diode" package="DO41-10" value="1N4004"/>
<element name="D27" library="diode" package="DO41-10" value="1N4004"/>
<element name="D28" library="diode" package="DO41-10" value="1N4004"/>
<element name="R9" library="resistor" package="M0805" value="680R"/>
<element name="JP9" library="jumper" package="JP1" value=""/>
<element name="D29" library="diode" package="DO41-10" value="1N4004"/>
<element name="D30" library="diode" package="DO41-10" value="1N4004"/>
<element name="D31" library="diode" package="DO41-10" value="1N4004"/>
<element name="D32" library="diode" package="DO41-10" value="1N4004"/>
<element name="R10" library="resistor" package="M0805" value="680R"/>
<element name="JP10" library="jumper" package="JP1" value=""/>
<element name="D33" library="diode" package="DO41-10" value="1N4004"/>
<element name="D34" library="diode" package="DO41-10" value="1N4004"/>
<element name="D35" library="diode" package="DO41-10" value="1N4004"/>
<element name="D36" library="diode" package="DO41-10" value="1N4004"/>
<element name="R11" library="resistor" package="M0805" value="680R"/>
<element name="JP11" library="jumper" package="JP1" value=""/>
<element name="D37" library="diode" package="DO41-10" value="1N4004"/>
<element name="D38" library="diode" package="DO41-10" value="1N4004"/>
<element name="D39" library="diode" package="DO41-10" value="1N4004"/>
<element name="D40" library="diode" package="DO41-10" value="1N4004"/>
<element name="R12" library="resistor" package="M0805" value="680R"/>
<element name="JP12" library="jumper" package="JP1" value=""/>
<element name="D41" library="diode" package="DO41-10" value="1N4004"/>
<element name="D42" library="diode" package="DO41-10" value="1N4004"/>
<element name="D43" library="diode" package="DO41-10" value="1N4004"/>
<element name="D44" library="diode" package="DO41-10" value="1N4004"/>
<element name="R13" library="resistor" package="M0805" value="680R"/>
<element name="JP13" library="jumper" package="JP1" value=""/>
<element name="D45" library="diode" package="DO41-10" value="1N4004"/>
<element name="D46" library="diode" package="DO41-10" value="1N4004"/>
<element name="D47" library="diode" package="DO41-10" value="1N4004"/>
<element name="D48" library="diode" package="DO41-10" value="1N4004"/>
<element name="R14" library="resistor" package="M0805" value="680R"/>
<element name="JP14" library="jumper" package="JP1" value=""/>
<element name="D49" library="diode" package="DO41-10" value="1N4004"/>
<element name="D50" library="diode" package="DO41-10" value="1N4004"/>
<element name="D51" library="diode" package="DO41-10" value="1N4004"/>
<element name="D52" library="diode" package="DO41-10" value="1N4004"/>
<element name="R15" library="resistor" package="M0805" value="680R"/>
<element name="JP15" library="jumper" package="JP1" value=""/>
<element name="D53" library="diode" package="DO41-10" value="1N4004"/>
<element name="D54" library="diode" package="DO41-10" value="1N4004"/>
<element name="D55" library="diode" package="DO41-10" value="1N4004"/>
<element name="D56" library="diode" package="DO41-10" value="1N4004"/>
<element name="R16" library="resistor" package="M0805" value="680R"/>
<element name="JP16" library="jumper" package="JP1" value=""/>
<element name="D57" library="diode" package="DO41-10" value="1N4004"/>
<element name="D58" library="diode" package="DO41-10" value="1N4004"/>
<element name="D59" library="diode" package="DO41-10" value="1N4004"/>
<element name="D60" library="diode" package="DO41-10" value="1N4004"/>
<element name="R17" library="resistor" package="M0805" value="680R"/>
<element name="JP17" library="jumper" package="JP1" value=""/>
<element name="D61" library="diode" package="DO41-10" value="1N4004"/>
<element name="D62" library="diode" package="DO41-10" value="1N4004"/>
<element name="D63" library="diode" package="DO41-10" value="1N4004"/>
<element name="D64" library="diode" package="DO41-10" value="1N4004"/>
<element name="R18" library="resistor" package="M0805" value="680R"/>
<element name="JP18" library="jumper" package="JP1" value=""/>
<element name="D65" library="diode" package="DO41-10" value="1N4004"/>
<element name="D66" library="diode" package="DO41-10" value="1N4004"/>
<element name="D67" library="diode" package="DO41-10" value="1N4004"/>
<element name="D68" library="diode" package="DO41-10" value="1N4004"/>
<element name="R19" library="resistor" package="M0805" value="680R"/>
<element name="JP19" library="jumper" package="JP1" value=""/>
<element name="D69" library="diode" package="DO41-10" value="1N4004"/>
<element name="D70" library="diode" package="DO41-10" value="1N4004"/>
<element name="D71" library="diode" package="DO41-10" value="1N4004"/>
<element name="D72" library="diode" package="DO41-10" value="1N4004"/>
<element name="R20" library="resistor" package="M0805" value="680R"/>
<element name="JP20" library="jumper" package="JP1" value=""/>
<element name="JP21" library="jumper" package="JP1" value=""/>
<element name="D73" library="diode" package="DO41-10" value="1N4004"/>
<element name="D74" library="diode" package="DO41-10" value="1N4004"/>
<element name="D75" library="diode" package="DO41-10" value="1N4004"/>
<element name="D76" library="diode" package="DO41-10" value="1N4004"/>
<element name="R21" library="resistor" package="M0805" value="680R"/>
<element name="JP22" library="jumper" package="JP1" value=""/>
<element name="D77" library="diode" package="DO41-10" value="1N4004"/>
<element name="D78" library="diode" package="DO41-10" value="1N4004"/>
<element name="D79" library="diode" package="DO41-10" value="1N4004"/>
<element name="D80" library="diode" package="DO41-10" value="1N4004"/>
<element name="R22" library="resistor" package="M0805" value="680R"/>
<element name="JP23" library="jumper" package="JP1" value=""/>
<element name="D81" library="diode" package="DO41-10" value="1N4004"/>
<element name="D82" library="diode" package="DO41-10" value="1N4004"/>
<element name="D83" library="diode" package="DO41-10" value="1N4004"/>
<element name="D84" library="diode" package="DO41-10" value="1N4004"/>
<element name="R23" library="resistor" package="M0805" value="680R"/>
<element name="JP24" library="jumper" package="JP1" value=""/>
<element name="D85" library="diode" package="DO41-10" value="1N4004"/>
<element name="D86" library="diode" package="DO41-10" value="1N4004"/>
<element name="D87" library="diode" package="DO41-10" value="1N4004"/>
<element name="D88" library="diode" package="DO41-10" value="1N4004"/>
<element name="R24" library="resistor" package="M0805" value="680R"/>
<element name="JP25" library="jumper" package="JP1" value=""/>
<element name="D89" library="diode" package="DO41-10" value="1N4004"/>
<element name="D90" library="diode" package="DO41-10" value="1N4004"/>
<element name="D91" library="diode" package="DO41-10" value="1N4004"/>
<element name="D92" library="diode" package="DO41-10" value="1N4004"/>
<element name="R25" library="resistor" package="M0805" value="680R"/>
<element name="JP26" library="jumper" package="JP1" value=""/>
<element name="D93" library="diode" package="DO41-10" value="1N4004"/>
<element name="D94" library="diode" package="DO41-10" value="1N4004"/>
<element name="D95" library="diode" package="DO41-10" value="1N4004"/>
<element name="D96" library="diode" package="DO41-10" value="1N4004"/>
<element name="R26" library="resistor" package="M0805" value="680R"/>
<element name="JP27" library="jumper" package="JP1" value=""/>
<element name="D97" library="diode" package="DO41-10" value="1N4004"/>
<element name="D98" library="diode" package="DO41-10" value="1N4004"/>
<element name="D99" library="diode" package="DO41-10" value="1N4004"/>
<element name="D100" library="diode" package="DO41-10" value="1N4004"/>
<element name="R27" library="resistor" package="M0805" value="680R"/>
<element name="JP28" library="jumper" package="JP1" value=""/>
<element name="D101" library="diode" package="DO41-10" value="1N4004"/>
<element name="D102" library="diode" package="DO41-10" value="1N4004"/>
<element name="D103" library="diode" package="DO41-10" value="1N4004"/>
<element name="D104" library="diode" package="DO41-10" value="1N4004"/>
<element name="R28" library="resistor" package="M0805" value="680R"/>
<element name="JP29" library="jumper" package="JP1" value=""/>
<element name="D105" library="diode" package="DO41-10" value="1N4004"/>
<element name="D106" library="diode" package="DO41-10" value="1N4004"/>
<element name="D107" library="diode" package="DO41-10" value="1N4004"/>
<element name="D108" library="diode" package="DO41-10" value="1N4004"/>
<element name="R29" library="resistor" package="M0805" value="680R"/>
<element name="JP30" library="jumper" package="JP1" value=""/>
<element name="D109" library="diode" package="DO41-10" value="1N4004"/>
<element name="D110" library="diode" package="DO41-10" value="1N4004"/>
<element name="D111" library="diode" package="DO41-10" value="1N4004"/>
<element name="D112" library="diode" package="DO41-10" value="1N4004"/>
<element name="R30" library="resistor" package="M0805" value="680R"/>
<element name="JP31" library="jumper" package="JP1" value=""/>
<element name="D113" library="diode" package="DO41-10" value="1N4004"/>
<element name="D114" library="diode" package="DO41-10" value="1N4004"/>
<element name="D115" library="diode" package="DO41-10" value="1N4004"/>
<element name="D116" library="diode" package="DO41-10" value="1N4004"/>
<element name="R31" library="resistor" package="M0805" value="680R"/>
<element name="JP32" library="jumper" package="JP1" value=""/>
<element name="D117" library="diode" package="DO41-10" value="1N4004"/>
<element name="D118" library="diode" package="DO41-10" value="1N4004"/>
<element name="D119" library="diode" package="DO41-10" value="1N4004"/>
<element name="D120" library="diode" package="DO41-10" value="1N4004"/>
<element name="R32" library="resistor" package="M0805" value="680R"/>
<element name="JP33" library="jumper" package="JP1" value=""/>
<element name="D121" library="diode" package="DO41-10" value="1N4004"/>
<element name="D122" library="diode" package="DO41-10" value="1N4004"/>
<element name="D123" library="diode" package="DO41-10" value="1N4004"/>
<element name="D124" library="diode" package="DO41-10" value="1N4004"/>
<element name="R33" library="resistor" package="M0805" value="680R"/>
<element name="JP34" library="jumper" package="JP1" value=""/>
<element name="D125" library="diode" package="DO41-10" value="1N4004"/>
<element name="D126" library="diode" package="DO41-10" value="1N4004"/>
<element name="D127" library="diode" package="DO41-10" value="1N4004"/>
<element name="D128" library="diode" package="DO41-10" value="1N4004"/>
<element name="R34" library="resistor" package="M0805" value="680R"/>
<element name="JP35" library="jumper" package="JP1" value=""/>
<element name="LED3" library="led" package="SML0603" value=""/>
<element name="R35" library="resistor" package="M0805" value=""/>
<element name="LED4" library="led" package="SML0603" value=""/>
<element name="R36" library="resistor" package="M0805" value=""/>
<element name="LED5" library="led" package="SML0603" value=""/>
<element name="R37" library="resistor" package="M0805" value=""/>
<element name="LED6" library="led" package="SML0603" value=""/>
<element name="R38" library="resistor" package="M0805" value=""/>
<element name="LED7" library="led" package="SML0603" value=""/>
<element name="R39" library="resistor" package="M0805" value=""/>
<element name="LED8" library="led" package="SML0603" value=""/>
<element name="R40" library="resistor" package="M0805" value=""/>
<element name="LED9" library="led" package="SML0603" value=""/>
<element name="R41" library="resistor" package="M0805" value=""/>
<element name="LED10" library="led" package="SML0603" value=""/>
<element name="R42" library="resistor" package="M0805" value=""/>
<element name="LED11" library="led" package="SML0603" value=""/>
<element name="R43" library="resistor" package="M0805" value=""/>
<element name="LED12" library="led" package="SML0603" value=""/>
<element name="R44" library="resistor" package="M0805" value=""/>
<element name="LED13" library="led" package="SML0603" value=""/>
<element name="R45" library="resistor" package="M0805" value=""/>
<element name="LED14" library="led" package="SML0603" value=""/>
<element name="R46" library="resistor" package="M0805" value=""/>
<element name="LED15" library="led" package="SML0603" value=""/>
<element name="R47" library="resistor" package="M0805" value=""/>
<element name="LED16" library="led" package="SML0603" value=""/>
<element name="R48" library="resistor" package="M0805" value=""/>
<element name="LED17" library="led" package="SML0603" value=""/>
<element name="R49" library="resistor" package="M0805" value=""/>
<element name="LED18" library="led" package="SML0603" value=""/>
<element name="R50" library="resistor" package="M0805" value=""/>
<element name="LED19" library="led" package="SML0603" value=""/>
<element name="R51" library="resistor" package="M0805" value=""/>
<element name="LED20" library="led" package="SML0603" value=""/>
<element name="R52" library="resistor" package="M0805" value=""/>
<element name="LED21" library="led" package="SML0603" value=""/>
<element name="R53" library="resistor" package="M0805" value=""/>
<element name="LED22" library="led" package="SML0603" value=""/>
<element name="R54" library="resistor" package="M0805" value=""/>
<element name="LED23" library="led" package="SML0603" value=""/>
<element name="R55" library="resistor" package="M0805" value=""/>
<element name="LED24" library="led" package="SML0603" value=""/>
<element name="R56" library="resistor" package="M0805" value=""/>
<element name="LED25" library="led" package="SML0603" value=""/>
<element name="R57" library="resistor" package="M0805" value=""/>
<element name="LED26" library="led" package="SML0603" value=""/>
<element name="R58" library="resistor" package="M0805" value=""/>
<element name="LED27" library="led" package="SML0603" value=""/>
<element name="R59" library="resistor" package="M0805" value=""/>
<element name="LED28" library="led" package="SML0603" value=""/>
<element name="R60" library="resistor" package="M0805" value=""/>
<element name="LED29" library="led" package="SML0603" value=""/>
<element name="R61" library="resistor" package="M0805" value=""/>
<element name="LED30" library="led" package="SML0603" value=""/>
<element name="R62" library="resistor" package="M0805" value=""/>
<element name="LED31" library="led" package="SML0603" value=""/>
<element name="R63" library="resistor" package="M0805" value=""/>
<element name="LED32" library="led" package="SML0603" value=""/>
<element name="R64" library="resistor" package="M0805" value=""/>
<element name="IC1" library="burr-brown" package="SOT223" value="REG1117">
<attribute name="OC_NEWARK" value="14P6981"/>
<attribute name="MPN" value="REG1117"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1097566"/>
</element>
<element name="C1" library="resistor" package="CT6032" value=""/>
<element name="C2" library="resistor" package="CT6032" value=""/>
<element name="C3" library="rcl" package="C0805" value=""/>
<element name="C4" library="rcl" package="C0805" value=""/>
<element name="C5" library="rcl" package="C0805" value=""/>
<element name="C6" library="rcl" package="C0805" value=""/>
<element name="C9" library="rcl" package="C0805" value=""/>
<element name="JP36" library="jumper" package="JP4" value=""/>
<element name="R65" library="resistor" package="M0805" value="10k"/>
<element name="R66" library="resistor" package="M0805" value="10k"/>
<element name="C10" library="rcl" package="C0805" value=""/>
<element name="R67" library="resistor" package="M0805" value="10k"/>
<element name="R68" library="resistor" package="M0805" value="10k"/>
<element name="SJ1" library="jumper" package="SJ" value=""/>
<element name="SJ3" library="jumper" package="SJ_2" value=""/>
<element name="SJ4" library="jumper" package="SJ" value=""/>
<element name="S1" library="switch-omron" package="B3F-10XX" value="">
<attribute name="OC_NEWARK" value="36M3542"/>
<attribute name="MPN" value="B3F-1000"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="176432"/>
</element>
<element name="X1" library="con-tycoelectronics" package="RJ45-NO-SHIELD" value="RJ45-6L-B">
<attribute name="OC_NEWARK" value="16R6090"/>
<attribute name="MPN" value="RJ45-6L-B"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="X2" library="con-tycoelectronics" package="RJ45-NO-SHIELD" value="RJ45-6L-B">
<attribute name="OC_NEWARK" value="16R6090"/>
<attribute name="MPN" value="RJ45-6L-B"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
</elements>
<signals>
<signal name="N$2">
<contactref element="D3" pad="A"/>
<contactref element="D4" pad="C"/>
</signal>
<signal name="N$3">
<contactref element="D1" pad="C"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="N$4">
<contactref element="D2" pad="C"/>
<contactref element="D4" pad="A"/>
<contactref element="OK1" pad="2"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="OK1" pad="1"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="GLCP">
<contactref element="D1" pad="A"/>
<contactref element="D3" pad="C"/>
<contactref element="R1" pad="1"/>
<contactref element="D5" pad="A"/>
<contactref element="D7" pad="C"/>
<contactref element="R2" pad="1"/>
<contactref element="D9" pad="A"/>
<contactref element="D11" pad="C"/>
<contactref element="R5" pad="1"/>
<contactref element="D13" pad="A"/>
<contactref element="D15" pad="C"/>
<contactref element="R6" pad="1"/>
<contactref element="D17" pad="A"/>
<contactref element="D19" pad="C"/>
<contactref element="R7" pad="1"/>
<contactref element="D23" pad="C"/>
<contactref element="R8" pad="1"/>
<contactref element="D21" pad="A"/>
<contactref element="R9" pad="1"/>
<contactref element="D27" pad="C"/>
<contactref element="D25" pad="A"/>
<contactref element="D29" pad="A"/>
<contactref element="D31" pad="C"/>
<contactref element="R10" pad="1"/>
<contactref element="D33" pad="A"/>
<contactref element="D35" pad="C"/>
<contactref element="R11" pad="1"/>
<contactref element="D39" pad="C"/>
<contactref element="R12" pad="1"/>
<contactref element="D37" pad="A"/>
<contactref element="R13" pad="1"/>
<contactref element="D43" pad="C"/>
<contactref element="D41" pad="A"/>
<contactref element="D45" pad="A"/>
<contactref element="D47" pad="C"/>
<contactref element="R14" pad="1"/>
<contactref element="D49" pad="A"/>
<contactref element="D51" pad="C"/>
<contactref element="R15" pad="1"/>
<contactref element="D55" pad="C"/>
<contactref element="R16" pad="1"/>
<contactref element="D53" pad="A"/>
<contactref element="R17" pad="1"/>
<contactref element="D59" pad="C"/>
<contactref element="D57" pad="A"/>
<contactref element="D61" pad="A"/>
<contactref element="D63" pad="C"/>
<contactref element="R18" pad="1"/>
<contactref element="JP4" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="D7" pad="A"/>
<contactref element="D8" pad="C"/>
</signal>
<signal name="N$8">
<contactref element="D5" pad="C"/>
<contactref element="D6" pad="A"/>
</signal>
<signal name="N$9">
<contactref element="D6" pad="C"/>
<contactref element="D8" pad="A"/>
<contactref element="JP2" pad="2"/>
<contactref element="OK2" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="R2" pad="2"/>
<contactref element="OK2" pad="1"/>
</signal>
<signal name="GND">
<contactref element="OK1" pad="3"/>
<contactref element="OK2" pad="3"/>
<contactref element="OK3" pad="3"/>
<contactref element="OK4" pad="3"/>
<contactref element="OK5" pad="3"/>
<contactref element="OK6" pad="3"/>
<contactref element="OK7" pad="3"/>
<contactref element="OK8" pad="3"/>
<contactref element="OK9" pad="3"/>
<contactref element="OK10" pad="3"/>
<contactref element="OK11" pad="3"/>
<contactref element="OK12" pad="3"/>
<contactref element="OK13" pad="3"/>
<contactref element="OK14" pad="3"/>
<contactref element="OK15" pad="3"/>
<contactref element="OK16" pad="3"/>
<contactref element="OK32" pad="3"/>
<contactref element="OK31" pad="3"/>
<contactref element="OK17" pad="3"/>
<contactref element="OK18" pad="3"/>
<contactref element="OK19" pad="3"/>
<contactref element="OK20" pad="3"/>
<contactref element="OK21" pad="3"/>
<contactref element="OK22" pad="3"/>
<contactref element="OK23" pad="3"/>
<contactref element="OK24" pad="3"/>
<contactref element="OK25" pad="3"/>
<contactref element="OK26" pad="3"/>
<contactref element="OK27" pad="3"/>
<contactref element="OK28" pad="3"/>
<contactref element="OK29" pad="3"/>
<contactref element="OK30" pad="3"/>
<contactref element="JP36" pad="3"/>
<contactref element="C1" pad="-"/>
<contactref element="C3" pad="2"/>
<contactref element="IC1" pad="1"/>
<contactref element="C4" pad="2"/>
<contactref element="C2" pad="-"/>
<contactref element="C5" pad="2"/>
<contactref element="U1" pad="18"/>
<contactref element="U1" pad="63"/>
<contactref element="U1" pad="47"/>
<contactref element="U1" pad="31"/>
<contactref element="C6" pad="2"/>
<contactref element="U1" pad="12"/>
<contactref element="C9" pad="2"/>
<contactref element="JP3" pad="5"/>
<contactref element="C10" pad="2"/>
<contactref element="SJ1" pad="1"/>
<contactref element="SJ4" pad="1"/>
<contactref element="S1" pad="3"/>
<contactref element="S1" pad="4"/>
<contactref element="X1" pad="3"/>
<contactref element="X1" pad="5"/>
<contactref element="X2" pad="3"/>
<contactref element="X2" pad="5"/>
</signal>
<signal name="GBM0">
<contactref element="OK1" pad="4"/>
<contactref element="LED1" pad="C"/>
<contactref element="U1" pad="14"/>
</signal>
<signal name="N$14">
<contactref element="LED1" pad="A"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="GBM1">
<contactref element="LED2" pad="C"/>
<contactref element="OK2" pad="4"/>
<contactref element="U1" pad="15"/>
</signal>
<signal name="N$16">
<contactref element="LED2" pad="A"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="D11" pad="A"/>
<contactref element="D12" pad="C"/>
</signal>
<signal name="N$17">
<contactref element="D9" pad="C"/>
<contactref element="D10" pad="A"/>
</signal>
<signal name="N$18">
<contactref element="D10" pad="C"/>
<contactref element="D12" pad="A"/>
<contactref element="JP5" pad="2"/>
<contactref element="OK3" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="R5" pad="2"/>
<contactref element="OK3" pad="1"/>
</signal>
<signal name="N$21">
<contactref element="D15" pad="A"/>
<contactref element="D16" pad="C"/>
</signal>
<signal name="N$22">
<contactref element="D13" pad="C"/>
<contactref element="D14" pad="A"/>
</signal>
<signal name="N$23">
<contactref element="D14" pad="C"/>
<contactref element="D16" pad="A"/>
<contactref element="JP6" pad="2"/>
<contactref element="OK4" pad="2"/>
</signal>
<signal name="N$24">
<contactref element="R6" pad="2"/>
<contactref element="OK4" pad="1"/>
</signal>
<signal name="GLCN">
<contactref element="JP4" pad="1"/>
<contactref element="JP1" pad="1"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP5" pad="1"/>
<contactref element="JP6" pad="1"/>
<contactref element="JP7" pad="1"/>
<contactref element="JP8" pad="1"/>
<contactref element="JP9" pad="1"/>
<contactref element="JP10" pad="1"/>
<contactref element="JP11" pad="1"/>
<contactref element="JP12" pad="1"/>
<contactref element="JP13" pad="1"/>
<contactref element="JP14" pad="1"/>
<contactref element="JP15" pad="1"/>
<contactref element="JP16" pad="1"/>
<contactref element="JP17" pad="1"/>
<contactref element="JP18" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="D19" pad="A"/>
<contactref element="D20" pad="C"/>
</signal>
<signal name="N$20">
<contactref element="D17" pad="C"/>
<contactref element="D18" pad="A"/>
</signal>
<signal name="N$25">
<contactref element="D18" pad="C"/>
<contactref element="D20" pad="A"/>
<contactref element="JP7" pad="2"/>
<contactref element="OK5" pad="2"/>
</signal>
<signal name="N$26">
<contactref element="R7" pad="2"/>
<contactref element="OK5" pad="1"/>
</signal>
<signal name="N$27">
<contactref element="D23" pad="A"/>
<contactref element="D24" pad="C"/>
</signal>
<signal name="N$28">
<contactref element="D21" pad="C"/>
<contactref element="D22" pad="A"/>
</signal>
<signal name="N$29">
<contactref element="D22" pad="C"/>
<contactref element="D24" pad="A"/>
<contactref element="JP8" pad="2"/>
<contactref element="OK6" pad="2"/>
</signal>
<signal name="N$30">
<contactref element="R8" pad="2"/>
<contactref element="OK6" pad="1"/>
</signal>
<signal name="N$31">
<contactref element="D27" pad="A"/>
<contactref element="D28" pad="C"/>
</signal>
<signal name="N$32">
<contactref element="D25" pad="C"/>
<contactref element="D26" pad="A"/>
</signal>
<signal name="N$33">
<contactref element="D26" pad="C"/>
<contactref element="D28" pad="A"/>
<contactref element="JP9" pad="2"/>
<contactref element="OK7" pad="2"/>
</signal>
<signal name="N$34">
<contactref element="R9" pad="2"/>
<contactref element="OK7" pad="1"/>
</signal>
<signal name="N$35">
<contactref element="D31" pad="A"/>
<contactref element="D32" pad="C"/>
</signal>
<signal name="N$36">
<contactref element="D29" pad="C"/>
<contactref element="D30" pad="A"/>
</signal>
<signal name="N$37">
<contactref element="D30" pad="C"/>
<contactref element="D32" pad="A"/>
<contactref element="JP10" pad="2"/>
<contactref element="OK8" pad="2"/>
</signal>
<signal name="N$38">
<contactref element="R10" pad="2"/>
<contactref element="OK8" pad="1"/>
</signal>
<signal name="N$39">
<contactref element="D35" pad="A"/>
<contactref element="D36" pad="C"/>
</signal>
<signal name="N$40">
<contactref element="D33" pad="C"/>
<contactref element="D34" pad="A"/>
</signal>
<signal name="N$41">
<contactref element="D34" pad="C"/>
<contactref element="D36" pad="A"/>
<contactref element="JP11" pad="2"/>
<contactref element="OK9" pad="2"/>
</signal>
<signal name="N$42">
<contactref element="R11" pad="2"/>
<contactref element="OK9" pad="1"/>
</signal>
<signal name="N$43">
<contactref element="D39" pad="A"/>
<contactref element="D40" pad="C"/>
</signal>
<signal name="N$44">
<contactref element="D37" pad="C"/>
<contactref element="D38" pad="A"/>
</signal>
<signal name="N$45">
<contactref element="D38" pad="C"/>
<contactref element="D40" pad="A"/>
<contactref element="JP12" pad="2"/>
<contactref element="OK10" pad="2"/>
</signal>
<signal name="N$46">
<contactref element="R12" pad="2"/>
<contactref element="OK10" pad="1"/>
</signal>
<signal name="N$47">
<contactref element="D43" pad="A"/>
<contactref element="D44" pad="C"/>
</signal>
<signal name="N$48">
<contactref element="D41" pad="C"/>
<contactref element="D42" pad="A"/>
</signal>
<signal name="N$49">
<contactref element="D42" pad="C"/>
<contactref element="D44" pad="A"/>
<contactref element="JP13" pad="2"/>
<contactref element="OK11" pad="2"/>
</signal>
<signal name="N$50">
<contactref element="R13" pad="2"/>
<contactref element="OK11" pad="1"/>
</signal>
<signal name="N$51">
<contactref element="D47" pad="A"/>
<contactref element="D48" pad="C"/>
</signal>
<signal name="N$52">
<contactref element="D45" pad="C"/>
<contactref element="D46" pad="A"/>
</signal>
<signal name="N$53">
<contactref element="D46" pad="C"/>
<contactref element="D48" pad="A"/>
<contactref element="JP14" pad="2"/>
<contactref element="OK12" pad="2"/>
</signal>
<signal name="N$54">
<contactref element="R14" pad="2"/>
<contactref element="OK12" pad="1"/>
</signal>
<signal name="N$55">
<contactref element="D51" pad="A"/>
<contactref element="D52" pad="C"/>
</signal>
<signal name="N$56">
<contactref element="D49" pad="C"/>
<contactref element="D50" pad="A"/>
</signal>
<signal name="N$57">
<contactref element="D50" pad="C"/>
<contactref element="D52" pad="A"/>
<contactref element="JP15" pad="2"/>
<contactref element="OK13" pad="2"/>
</signal>
<signal name="N$58">
<contactref element="R15" pad="2"/>
<contactref element="OK13" pad="1"/>
</signal>
<signal name="N$59">
<contactref element="D55" pad="A"/>
<contactref element="D56" pad="C"/>
</signal>
<signal name="N$60">
<contactref element="D53" pad="C"/>
<contactref element="D54" pad="A"/>
</signal>
<signal name="N$61">
<contactref element="D54" pad="C"/>
<contactref element="D56" pad="A"/>
<contactref element="JP16" pad="2"/>
<contactref element="OK14" pad="2"/>
</signal>
<signal name="N$62">
<contactref element="R16" pad="2"/>
<contactref element="OK14" pad="1"/>
</signal>
<signal name="N$63">
<contactref element="D59" pad="A"/>
<contactref element="D60" pad="C"/>
</signal>
<signal name="N$64">
<contactref element="D57" pad="C"/>
<contactref element="D58" pad="A"/>
</signal>
<signal name="N$65">
<contactref element="D58" pad="C"/>
<contactref element="D60" pad="A"/>
<contactref element="JP17" pad="2"/>
<contactref element="OK15" pad="2"/>
</signal>
<signal name="N$66">
<contactref element="R17" pad="2"/>
<contactref element="OK15" pad="1"/>
</signal>
<signal name="N$67">
<contactref element="D63" pad="A"/>
<contactref element="D64" pad="C"/>
</signal>
<signal name="N$68">
<contactref element="D61" pad="C"/>
<contactref element="D62" pad="A"/>
</signal>
<signal name="N$69">
<contactref element="D62" pad="C"/>
<contactref element="D64" pad="A"/>
<contactref element="JP18" pad="2"/>
<contactref element="OK16" pad="2"/>
</signal>
<signal name="N$70">
<contactref element="R18" pad="2"/>
<contactref element="OK16" pad="1"/>
</signal>
<signal name="N$71">
<contactref element="D67" pad="A"/>
<contactref element="D68" pad="C"/>
</signal>
<signal name="N$72">
<contactref element="D65" pad="C"/>
<contactref element="D66" pad="A"/>
</signal>
<signal name="N$73">
<contactref element="D66" pad="C"/>
<contactref element="D68" pad="A"/>
<contactref element="JP19" pad="2"/>
<contactref element="OK17" pad="2"/>
</signal>
<signal name="N$74">
<contactref element="R19" pad="2"/>
<contactref element="OK17" pad="1"/>
</signal>
<signal name="N$75">
<contactref element="D71" pad="A"/>
<contactref element="D72" pad="C"/>
</signal>
<signal name="N$76">
<contactref element="D69" pad="C"/>
<contactref element="D70" pad="A"/>
</signal>
<signal name="N$77">
<contactref element="D70" pad="C"/>
<contactref element="D72" pad="A"/>
<contactref element="JP20" pad="2"/>
<contactref element="OK18" pad="2"/>
</signal>
<signal name="N$78">
<contactref element="R20" pad="2"/>
<contactref element="OK18" pad="1"/>
</signal>
<signal name="N$79">
<contactref element="D75" pad="A"/>
<contactref element="D76" pad="C"/>
</signal>
<signal name="N$80">
<contactref element="D73" pad="C"/>
<contactref element="D74" pad="A"/>
</signal>
<signal name="N$81">
<contactref element="D74" pad="C"/>
<contactref element="D76" pad="A"/>
<contactref element="JP22" pad="2"/>
<contactref element="OK19" pad="2"/>
</signal>
<signal name="N$82">
<contactref element="R21" pad="2"/>
<contactref element="OK19" pad="1"/>
</signal>
<signal name="N$83">
<contactref element="D79" pad="A"/>
<contactref element="D80" pad="C"/>
</signal>
<signal name="N$84">
<contactref element="D77" pad="C"/>
<contactref element="D78" pad="A"/>
</signal>
<signal name="N$85">
<contactref element="D78" pad="C"/>
<contactref element="D80" pad="A"/>
<contactref element="JP23" pad="2"/>
<contactref element="OK20" pad="2"/>
</signal>
<signal name="N$86">
<contactref element="R22" pad="2"/>
<contactref element="OK20" pad="1"/>
</signal>
<signal name="GLC1P">
<contactref element="JP21" pad="2"/>
<contactref element="D65" pad="A"/>
<contactref element="D67" pad="C"/>
<contactref element="R19" pad="1"/>
<contactref element="D71" pad="C"/>
<contactref element="R20" pad="1"/>
<contactref element="D69" pad="A"/>
<contactref element="R21" pad="1"/>
<contactref element="D75" pad="C"/>
<contactref element="D73" pad="A"/>
<contactref element="D77" pad="A"/>
<contactref element="D79" pad="C"/>
<contactref element="R22" pad="1"/>
<contactref element="D81" pad="A"/>
<contactref element="D83" pad="C"/>
<contactref element="R23" pad="1"/>
<contactref element="D87" pad="C"/>
<contactref element="R24" pad="1"/>
<contactref element="D85" pad="A"/>
<contactref element="R25" pad="1"/>
<contactref element="D91" pad="C"/>
<contactref element="D89" pad="A"/>
<contactref element="D93" pad="A"/>
<contactref element="D95" pad="C"/>
<contactref element="R26" pad="1"/>
<contactref element="D97" pad="A"/>
<contactref element="D99" pad="C"/>
<contactref element="R27" pad="1"/>
<contactref element="D103" pad="C"/>
<contactref element="R28" pad="1"/>
<contactref element="D101" pad="A"/>
<contactref element="R29" pad="1"/>
<contactref element="D107" pad="C"/>
<contactref element="D105" pad="A"/>
<contactref element="D109" pad="A"/>
<contactref element="D111" pad="C"/>
<contactref element="R30" pad="1"/>
<contactref element="D113" pad="A"/>
<contactref element="D115" pad="C"/>
<contactref element="R31" pad="1"/>
<contactref element="D119" pad="C"/>
<contactref element="R32" pad="1"/>
<contactref element="D117" pad="A"/>
<contactref element="R33" pad="1"/>
<contactref element="D123" pad="C"/>
<contactref element="D121" pad="A"/>
<contactref element="D125" pad="A"/>
<contactref element="D127" pad="C"/>
<contactref element="R34" pad="1"/>
</signal>
<signal name="N$88">
<contactref element="D83" pad="A"/>
<contactref element="D84" pad="C"/>
</signal>
<signal name="N$89">
<contactref element="D81" pad="C"/>
<contactref element="D82" pad="A"/>
</signal>
<signal name="N$90">
<contactref element="D82" pad="C"/>
<contactref element="D84" pad="A"/>
<contactref element="JP24" pad="2"/>
<contactref element="OK21" pad="2"/>
</signal>
<signal name="N$91">
<contactref element="R23" pad="2"/>
<contactref element="OK21" pad="1"/>
</signal>
<signal name="N$92">
<contactref element="D87" pad="A"/>
<contactref element="D88" pad="C"/>
</signal>
<signal name="N$93">
<contactref element="D85" pad="C"/>
<contactref element="D86" pad="A"/>
</signal>
<signal name="N$94">
<contactref element="D86" pad="C"/>
<contactref element="D88" pad="A"/>
<contactref element="JP25" pad="2"/>
<contactref element="OK22" pad="2"/>
</signal>
<signal name="N$95">
<contactref element="R24" pad="2"/>
<contactref element="OK22" pad="1"/>
</signal>
<signal name="N$96">
<contactref element="D91" pad="A"/>
<contactref element="D92" pad="C"/>
</signal>
<signal name="N$97">
<contactref element="D89" pad="C"/>
<contactref element="D90" pad="A"/>
</signal>
<signal name="N$98">
<contactref element="D90" pad="C"/>
<contactref element="D92" pad="A"/>
<contactref element="JP26" pad="2"/>
<contactref element="OK23" pad="2"/>
</signal>
<signal name="N$99">
<contactref element="R25" pad="2"/>
<contactref element="OK23" pad="1"/>
</signal>
<signal name="N$100">
<contactref element="D95" pad="A"/>
<contactref element="D96" pad="C"/>
</signal>
<signal name="N$101">
<contactref element="D93" pad="C"/>
<contactref element="D94" pad="A"/>
</signal>
<signal name="N$102">
<contactref element="D94" pad="C"/>
<contactref element="D96" pad="A"/>
<contactref element="JP27" pad="2"/>
<contactref element="OK24" pad="2"/>
</signal>
<signal name="N$103">
<contactref element="R26" pad="2"/>
<contactref element="OK24" pad="1"/>
</signal>
<signal name="N$104">
<contactref element="D99" pad="A"/>
<contactref element="D100" pad="C"/>
</signal>
<signal name="N$105">
<contactref element="D97" pad="C"/>
<contactref element="D98" pad="A"/>
</signal>
<signal name="N$106">
<contactref element="D98" pad="C"/>
<contactref element="D100" pad="A"/>
<contactref element="JP28" pad="2"/>
<contactref element="OK25" pad="2"/>
</signal>
<signal name="N$107">
<contactref element="R27" pad="2"/>
<contactref element="OK25" pad="1"/>
</signal>
<signal name="N$108">
<contactref element="D103" pad="A"/>
<contactref element="D104" pad="C"/>
</signal>
<signal name="N$109">
<contactref element="D101" pad="C"/>
<contactref element="D102" pad="A"/>
</signal>
<signal name="N$110">
<contactref element="D102" pad="C"/>
<contactref element="D104" pad="A"/>
<contactref element="JP29" pad="2"/>
<contactref element="OK26" pad="2"/>
</signal>
<signal name="N$111">
<contactref element="R28" pad="2"/>
<contactref element="OK26" pad="1"/>
</signal>
<signal name="N$112">
<contactref element="D107" pad="A"/>
<contactref element="D108" pad="C"/>
</signal>
<signal name="N$113">
<contactref element="D105" pad="C"/>
<contactref element="D106" pad="A"/>
</signal>
<signal name="N$114">
<contactref element="D106" pad="C"/>
<contactref element="D108" pad="A"/>
<contactref element="JP30" pad="2"/>
<contactref element="OK27" pad="2"/>
</signal>
<signal name="N$115">
<contactref element="R29" pad="2"/>
<contactref element="OK27" pad="1"/>
</signal>
<signal name="N$116">
<contactref element="D111" pad="A"/>
<contactref element="D112" pad="C"/>
</signal>
<signal name="N$117">
<contactref element="D109" pad="C"/>
<contactref element="D110" pad="A"/>
</signal>
<signal name="N$118">
<contactref element="D110" pad="C"/>
<contactref element="D112" pad="A"/>
<contactref element="JP31" pad="2"/>
<contactref element="OK28" pad="2"/>
</signal>
<signal name="N$119">
<contactref element="R30" pad="2"/>
<contactref element="OK28" pad="1"/>
</signal>
<signal name="N$120">
<contactref element="D115" pad="A"/>
<contactref element="D116" pad="C"/>
</signal>
<signal name="N$121">
<contactref element="D113" pad="C"/>
<contactref element="D114" pad="A"/>
</signal>
<signal name="N$122">
<contactref element="D114" pad="C"/>
<contactref element="D116" pad="A"/>
<contactref element="JP32" pad="2"/>
<contactref element="OK29" pad="2"/>
</signal>
<signal name="N$123">
<contactref element="R31" pad="2"/>
<contactref element="OK29" pad="1"/>
</signal>
<signal name="N$124">
<contactref element="D119" pad="A"/>
<contactref element="D120" pad="C"/>
</signal>
<signal name="N$125">
<contactref element="D117" pad="C"/>
<contactref element="D118" pad="A"/>
</signal>
<signal name="N$126">
<contactref element="D118" pad="C"/>
<contactref element="D120" pad="A"/>
<contactref element="JP33" pad="2"/>
<contactref element="OK30" pad="2"/>
</signal>
<signal name="N$127">
<contactref element="R32" pad="2"/>
<contactref element="OK30" pad="1"/>
</signal>
<signal name="N$128">
<contactref element="D123" pad="A"/>
<contactref element="D124" pad="C"/>
</signal>
<signal name="N$129">
<contactref element="D121" pad="C"/>
<contactref element="D122" pad="A"/>
</signal>
<signal name="N$130">
<contactref element="D122" pad="C"/>
<contactref element="D124" pad="A"/>
<contactref element="JP34" pad="2"/>
<contactref element="OK31" pad="2"/>
</signal>
<signal name="N$131">
<contactref element="R33" pad="2"/>
<contactref element="OK31" pad="1"/>
</signal>
<signal name="N$132">
<contactref element="D127" pad="A"/>
<contactref element="D128" pad="C"/>
</signal>
<signal name="N$133">
<contactref element="D125" pad="C"/>
<contactref element="D126" pad="A"/>
</signal>
<signal name="N$134">
<contactref element="D126" pad="C"/>
<contactref element="D128" pad="A"/>
<contactref element="JP35" pad="2"/>
<contactref element="OK32" pad="2"/>
</signal>
<signal name="N$135">
<contactref element="R34" pad="2"/>
<contactref element="OK32" pad="1"/>
</signal>
<signal name="GBM2">
<contactref element="LED3" pad="C"/>
<contactref element="OK3" pad="4"/>
<contactref element="U1" pad="16"/>
</signal>
<signal name="N$137">
<contactref element="LED3" pad="A"/>
<contactref element="R35" pad="1"/>
</signal>
<signal name="GBM3">
<contactref element="LED4" pad="C"/>
<contactref element="OK4" pad="4"/>
<contactref element="U1" pad="17"/>
</signal>
<signal name="N$139">
<contactref element="LED4" pad="A"/>
<contactref element="R36" pad="1"/>
</signal>
<signal name="GBM4">
<contactref element="LED5" pad="C"/>
<contactref element="OK5" pad="4"/>
<contactref element="U1" pad="20"/>
</signal>
<signal name="N$141">
<contactref element="LED5" pad="A"/>
<contactref element="R37" pad="1"/>
</signal>
<signal name="GBM5">
<contactref element="LED6" pad="C"/>
<contactref element="OK6" pad="4"/>
<contactref element="U1" pad="21"/>
</signal>
<signal name="N$143">
<contactref element="LED6" pad="A"/>
<contactref element="R38" pad="1"/>
</signal>
<signal name="GBM6">
<contactref element="LED7" pad="C"/>
<contactref element="OK7" pad="4"/>
<contactref element="U1" pad="22"/>
</signal>
<signal name="N$145">
<contactref element="LED7" pad="A"/>
<contactref element="R39" pad="1"/>
</signal>
<signal name="GBM7">
<contactref element="LED8" pad="C"/>
<contactref element="OK8" pad="4"/>
<contactref element="U1" pad="23"/>
</signal>
<signal name="N$147">
<contactref element="LED8" pad="A"/>
<contactref element="R40" pad="1"/>
</signal>
<signal name="GBM8">
<contactref element="LED9" pad="C"/>
<contactref element="OK9" pad="4"/>
<contactref element="U1" pad="39"/>
</signal>
<signal name="N$149">
<contactref element="LED9" pad="A"/>
<contactref element="R41" pad="1"/>
</signal>
<signal name="GBM9">
<contactref element="LED10" pad="C"/>
<contactref element="OK10" pad="4"/>
<contactref element="U1" pad="40"/>
</signal>
<signal name="N$151">
<contactref element="LED10" pad="A"/>
<contactref element="R42" pad="1"/>
</signal>
<signal name="GBM10">
<contactref element="LED11" pad="C"/>
<contactref element="OK11" pad="4"/>
<contactref element="U1" pad="51"/>
</signal>
<signal name="N$153">
<contactref element="LED11" pad="A"/>
<contactref element="R43" pad="1"/>
</signal>
<signal name="GBM11">
<contactref element="LED12" pad="C"/>
<contactref element="OK12" pad="4"/>
<contactref element="U1" pad="52"/>
</signal>
<signal name="N$155">
<contactref element="LED12" pad="A"/>
<contactref element="R44" pad="1"/>
</signal>
<signal name="GBM12">
<contactref element="LED13" pad="C"/>
<contactref element="OK13" pad="4"/>
<contactref element="U1" pad="53"/>
</signal>
<signal name="N$157">
<contactref element="LED13" pad="A"/>
<contactref element="R45" pad="1"/>
</signal>
<signal name="GBM13">
<contactref element="LED14" pad="C"/>
<contactref element="OK14" pad="4"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="N$159">
<contactref element="LED14" pad="A"/>
<contactref element="R46" pad="1"/>
</signal>
<signal name="GBM14">
<contactref element="LED15" pad="C"/>
<contactref element="OK15" pad="4"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="N$161">
<contactref element="LED15" pad="A"/>
<contactref element="R47" pad="1"/>
</signal>
<signal name="GBM15">
<contactref element="LED16" pad="C"/>
<contactref element="OK16" pad="4"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="N$163">
<contactref element="LED16" pad="A"/>
<contactref element="R48" pad="1"/>
</signal>
<signal name="V3_3">
<contactref element="R3" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="R35" pad="2"/>
<contactref element="R36" pad="2"/>
<contactref element="R37" pad="2"/>
<contactref element="R38" pad="2"/>
<contactref element="R39" pad="2"/>
<contactref element="R40" pad="2"/>
<contactref element="R41" pad="2"/>
<contactref element="R42" pad="2"/>
<contactref element="R43" pad="2"/>
<contactref element="R44" pad="2"/>
<contactref element="R45" pad="2"/>
<contactref element="R46" pad="2"/>
<contactref element="R47" pad="2"/>
<contactref element="R48" pad="2"/>
<contactref element="R49" pad="2"/>
<contactref element="R50" pad="2"/>
<contactref element="R51" pad="2"/>
<contactref element="R52" pad="2"/>
<contactref element="R53" pad="2"/>
<contactref element="R54" pad="2"/>
<contactref element="R55" pad="2"/>
<contactref element="R56" pad="2"/>
<contactref element="R57" pad="2"/>
<contactref element="R58" pad="2"/>
<contactref element="R59" pad="2"/>
<contactref element="R60" pad="2"/>
<contactref element="R61" pad="2"/>
<contactref element="R62" pad="2"/>
<contactref element="R63" pad="2"/>
<contactref element="R64" pad="2"/>
<contactref element="JP36" pad="1"/>
<contactref element="U1" pad="32"/>
<contactref element="U1" pad="48"/>
<contactref element="U1" pad="64"/>
<contactref element="U1" pad="19"/>
<contactref element="C6" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="U1" pad="13"/>
<contactref element="C4" pad="1"/>
<contactref element="IC1" pad="2"/>
<contactref element="C2" pad="+"/>
<contactref element="JP3" pad="6"/>
<contactref element="R65" pad="2"/>
<contactref element="R66" pad="2"/>
<contactref element="R68" pad="2"/>
<contactref element="R67" pad="2"/>
<contactref element="SJ3" pad="1"/>
<contactref element="SJ4" pad="2"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="LED17" pad="A"/>
<contactref element="R49" pad="1"/>
</signal>
<signal name="N$164">
<contactref element="LED18" pad="A"/>
<contactref element="R50" pad="1"/>
</signal>
<signal name="N$165">
<contactref element="LED19" pad="A"/>
<contactref element="R51" pad="1"/>
</signal>
<signal name="N$166">
<contactref element="LED20" pad="A"/>
<contactref element="R52" pad="1"/>
</signal>
<signal name="N$167">
<contactref element="LED21" pad="A"/>
<contactref element="R53" pad="1"/>
</signal>
<signal name="N$168">
<contactref element="LED22" pad="A"/>
<contactref element="R54" pad="1"/>
</signal>
<signal name="N$169">
<contactref element="LED23" pad="A"/>
<contactref element="R55" pad="1"/>
</signal>
<signal name="N$170">
<contactref element="LED24" pad="A"/>
<contactref element="R56" pad="1"/>
</signal>
<signal name="N$171">
<contactref element="LED25" pad="A"/>
<contactref element="R57" pad="1"/>
</signal>
<signal name="N$172">
<contactref element="LED26" pad="A"/>
<contactref element="R58" pad="1"/>
</signal>
<signal name="N$173">
<contactref element="LED27" pad="A"/>
<contactref element="R59" pad="1"/>
</signal>
<signal name="N$174">
<contactref element="LED28" pad="A"/>
<contactref element="R60" pad="1"/>
</signal>
<signal name="N$175">
<contactref element="LED29" pad="A"/>
<contactref element="R61" pad="1"/>
</signal>
<signal name="N$176">
<contactref element="LED30" pad="A"/>
<contactref element="R62" pad="1"/>
</signal>
<signal name="N$177">
<contactref element="LED31" pad="A"/>
<contactref element="R63" pad="1"/>
</signal>
<signal name="N$178">
<contactref element="LED32" pad="A"/>
<contactref element="R64" pad="1"/>
</signal>
<signal name="GBM16">
<contactref element="LED17" pad="C"/>
<contactref element="OK17" pad="4"/>
<contactref element="U1" pad="8"/>
</signal>
<signal name="GBM17">
<contactref element="LED18" pad="C"/>
<contactref element="OK18" pad="4"/>
<contactref element="U1" pad="9"/>
</signal>
<signal name="GBM18">
<contactref element="LED19" pad="C"/>
<contactref element="OK19" pad="4"/>
<contactref element="U1" pad="10"/>
</signal>
<signal name="GBM19">
<contactref element="LED20" pad="C"/>
<contactref element="OK20" pad="4"/>
<contactref element="U1" pad="11"/>
</signal>
<signal name="GBM20">
<contactref element="LED21" pad="C"/>
<contactref element="OK21" pad="4"/>
<contactref element="U1" pad="24"/>
</signal>
<signal name="GBM21">
<contactref element="LED22" pad="C"/>
<contactref element="OK22" pad="4"/>
<contactref element="U1" pad="25"/>
</signal>
<signal name="GBM22">
<contactref element="LED23" pad="C"/>
<contactref element="OK23" pad="4"/>
<contactref element="U1" pad="37"/>
</signal>
<signal name="GBM23">
<contactref element="LED24" pad="C"/>
<contactref element="OK24" pad="4"/>
<contactref element="U1" pad="38"/>
</signal>
<signal name="GBM24">
<contactref element="LED25" pad="C"/>
<contactref element="OK25" pad="4"/>
<contactref element="U1" pad="26"/>
</signal>
<signal name="GBM25">
<contactref element="LED26" pad="C"/>
<contactref element="OK26" pad="4"/>
<contactref element="U1" pad="27"/>
</signal>
<signal name="GBM26">
<contactref element="LED27" pad="C"/>
<contactref element="OK27" pad="4"/>
<contactref element="U1" pad="28"/>
</signal>
<signal name="GBM27">
<contactref element="LED28" pad="C"/>
<contactref element="OK28" pad="4"/>
<contactref element="U1" pad="55"/>
</signal>
<signal name="GBM28">
<contactref element="LED29" pad="C"/>
<contactref element="OK29" pad="4"/>
<contactref element="U1" pad="56"/>
</signal>
<signal name="GBM29">
<contactref element="LED30" pad="C"/>
<contactref element="OK30" pad="4"/>
<contactref element="U1" pad="57"/>
</signal>
<signal name="GBM30">
<contactref element="LED31" pad="C"/>
<contactref element="OK31" pad="4"/>
<contactref element="U1" pad="58"/>
</signal>
<signal name="GBM31">
<contactref element="LED32" pad="C"/>
<contactref element="OK32" pad="4"/>
<contactref element="U1" pad="59"/>
</signal>
<signal name="GLC1N">
<contactref element="JP35" pad="1"/>
<contactref element="JP34" pad="1"/>
<contactref element="JP33" pad="1"/>
<contactref element="JP32" pad="1"/>
<contactref element="JP31" pad="1"/>
<contactref element="JP30" pad="1"/>
<contactref element="JP29" pad="1"/>
<contactref element="JP28" pad="1"/>
<contactref element="JP27" pad="1"/>
<contactref element="JP26" pad="1"/>
<contactref element="JP25" pad="1"/>
<contactref element="JP24" pad="1"/>
<contactref element="JP23" pad="1"/>
<contactref element="JP22" pad="1"/>
<contactref element="JP20" pad="1"/>
<contactref element="JP21" pad="1"/>
<contactref element="JP19" pad="1"/>
</signal>
<signal name="SWDIO">
<contactref element="U1" pad="46"/>
<contactref element="JP36" pad="4"/>
</signal>
<signal name="SWCLK">
<contactref element="U1" pad="49"/>
<contactref element="JP36" pad="2"/>
</signal>
<signal name="V5_0">
<contactref element="IC1" pad="3"/>
<contactref element="C3" pad="1"/>
<contactref element="C1" pad="+"/>
<contactref element="SJ3" pad="3"/>
</signal>
<signal name="S88N_RX">
<contactref element="U1" pad="42"/>
<contactref element="X1" pad="2"/>
</signal>
<signal name="S88N_CLK">
<contactref element="U1" pad="43"/>
<contactref element="X1" pad="4"/>
<contactref element="X2" pad="4"/>
</signal>
<signal name="S88N_PS">
<contactref element="U1" pad="44"/>
<contactref element="X1" pad="6"/>
<contactref element="X2" pad="6"/>
</signal>
<signal name="S88N_RST">
<contactref element="U1" pad="45"/>
<contactref element="X1" pad="7"/>
<contactref element="X2" pad="7"/>
</signal>
<signal name="S88N_RAILDATA">
<contactref element="U1" pad="50"/>
<contactref element="X1" pad="8"/>
<contactref element="X2" pad="8"/>
</signal>
<signal name="S88N_TX">
<contactref element="U1" pad="41"/>
<contactref element="X2" pad="2"/>
</signal>
<signal name="S88N_VCC">
<contactref element="SJ3" pad="2"/>
<contactref element="X1" pad="1"/>
<contactref element="X2" pad="1"/>
</signal>
<signal name="I2C_SCL">
<contactref element="JP3" pad="1"/>
<contactref element="U1" pad="61"/>
<contactref element="R67" pad="1"/>
</signal>
<signal name="RS232_TX">
<contactref element="JP3" pad="3"/>
<contactref element="U1" pad="29"/>
</signal>
<signal name="SPI_CLK">
<contactref element="JP3" pad="7"/>
<contactref element="U1" pad="34"/>
</signal>
<signal name="SPI_MOSI">
<contactref element="JP3" pad="9"/>
<contactref element="U1" pad="36"/>
</signal>
<signal name="I2C_SDA">
<contactref element="JP3" pad="2"/>
<contactref element="U1" pad="62"/>
<contactref element="R68" pad="1"/>
</signal>
<signal name="RS232_RX">
<contactref element="JP3" pad="4"/>
<contactref element="U1" pad="30"/>
</signal>
<signal name="SPI_CS">
<contactref element="JP3" pad="8"/>
<contactref element="U1" pad="33"/>
</signal>
<signal name="SPI_MISO">
<contactref element="JP3" pad="10"/>
<contactref element="U1" pad="35"/>
</signal>
<signal name="N$1">
<contactref element="U1" pad="60"/>
<contactref element="R65" pad="1"/>
<contactref element="SJ1" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="R66" pad="1"/>
<contactref element="U1" pad="7"/>
<contactref element="C10" pad="1"/>
<contactref element="S1" pad="1"/>
<contactref element="S1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
