<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<library>
<packages>
<package name="PLCC6">
</package>
</packages>
<symbols>
<symbol name="WS2812">
<pin name="DO" direction="out"/>
<pin name="DI" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="N/C"/>
<pin name="VDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WS2812" prefix="U">
<description>WS2812 Intelligent RGB LED</description>
<gates>
<gate name="G$1" symbol="WS2812"/>
</gates>
<devices>
<device name="" package="PLCC6">
<connects>
<connect gate="G$1" pin="DI" pad="2"/>
<connect gate="G$1" pin="DO" pad="1"/>
<connect gate="G$1" pin="N/C" pad="4"/>
<connect gate="G$1" pin="VCC" pad="3"/>
<connect gate="G$1" pin="VDD" pad="5"/>
<connect gate="G$1" pin="VSS" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
