<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.1">
<drawing>
<board>
<plain>
<wire x1="8.89" y1="22.86" x2="187.94" y2="22.86" width="0" layer="20"/>
<wire x1="187.94" y1="22.86" x2="190.48" y2="162.23" width="0" layer="20"/>
<wire x1="190.48" y1="162.23" x2="11.43" y2="162.23" width="0" layer="20"/>
<wire x1="11.43" y1="162.23" x2="8.89" y2="22.86" width="0" layer="20"/>
</plain>
<libraries>
<library name="atmel">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Configurable logic, microcontrollers, nonvolatile memories&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt;CD-ROM : Configurable Logic Microcontroller Nonvolatile Memory
&lt;li&gt;CadSoft download site, www.cadsoft.de or www.cadsoftusa.com , file at90smcu_v400.zip
&lt;li&gt;avr.lbr
&lt;/ul&gt;
&lt;author&gt;Revised by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL40">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="74xx-eu">
<description>&lt;b&gt;TTL Devices, 74xx Series with European Symbols&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Texas Instruments &lt;i&gt;TTL Data Book&lt;/i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;Volume 1, 1996.
&lt;li&gt;TTL Data Book, Volume 2 , 1993
&lt;li&gt;National Seminconductor Databook 1990, ALS/LS Logic
&lt;li&gt;ttl 74er digital data dictionary, ECA Electronic + Acustic GmbH, ISBN 3-88109-032-0
&lt;li&gt;http://icmaster.com/ViewCompare.asp
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SO20W">
<description>&lt;b&gt;Wide Small Outline package&lt;/b&gt; 300 mil</description>
</package>
</packages>
</library>
<library name="resistor">
<description>&lt;b&gt;Resistors, Capacitors, Inductors&lt;/b&gt;&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;r.lbr
&lt;li&gt;cap.lbr 
&lt;li&gt;cap-fe.lbr
&lt;li&gt;captant.lbr
&lt;li&gt;polcap.lbr
&lt;li&gt;ipc-smd.lbr
&lt;/ul&gt;
All SMD packages are defined according to the IPC specifications and  CECC&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
for Electrolyt Capacitors see also :&lt;p&gt;
www.bccomponents.com &lt;p&gt;
www.panasonic.com&lt;p&gt;
www.kemet.com&lt;p&gt;
&lt;p&gt;
for trimmer refence see : &lt;u&gt;www.electrospec-inc.com/cross_references/trimpotcrossref.asp&lt;/u&gt;&lt;p&gt;

&lt;map name="nav_main"&gt;
&lt;area shape="rect" coords="0,1,140,23" href="../military_specs.asp" title=""&gt;
&lt;area shape="rect" coords="0,24,140,51" href="../about.asp" title=""&gt;
&lt;area shape="rect" coords="1,52,140,77" href="../rfq.asp" title=""&gt;
&lt;area shape="rect" coords="0,78,139,103" href="../products.asp" title=""&gt;
&lt;area shape="rect" coords="1,102,138,128" href="../excess_inventory.asp" title=""&gt;
&lt;area shape="rect" coords="1,129,138,150" href="../edge.asp" title=""&gt;
&lt;area shape="rect" coords="1,151,139,178" href="../industry_links.asp" title=""&gt;
&lt;area shape="rect" coords="0,179,139,201" href="../comments.asp" title=""&gt;
&lt;area shape="rect" coords="1,203,138,231" href="../directory.asp" title=""&gt;
&lt;area shape="default" nohref&gt;
&lt;/map&gt;

&lt;html&gt;

&lt;title&gt;&lt;/title&gt;

 &lt;LINK REL="StyleSheet" TYPE="text/css" HREF="style-sheet.css"&gt;

&lt;body bgcolor="#ffffff" text="#000000" marginwidth="0" marginheight="0" topmargin="0" leftmargin="0"&gt;
&lt;table border=0 cellspacing=0 cellpadding=0 width="100%" cellpaddding=0 height="55%"&gt;
&lt;tr valign="top"&gt;

&lt;/td&gt;
&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;TRIM-POT CROSS REFERENCE&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;RECTANGULAR MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BOURNS&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BI&amp;nbsp;TECH&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;DALE-VISHAY&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PHILIPS/MEPCO&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MURATA&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PANASONIC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;SPECTROL&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MILSPEC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;&lt;TD&gt;&amp;nbsp;&lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3 &gt;
      3005P&lt;BR&gt;
      3006P&lt;BR&gt;
      3006W&lt;BR&gt;
      3006Y&lt;BR&gt;
      3009P&lt;BR&gt;
      3009W&lt;BR&gt;
      3009Y&lt;BR&gt;
      3057J&lt;BR&gt;
      3057L&lt;BR&gt;
      3057P&lt;BR&gt;
      3057Y&lt;BR&gt;
      3059J&lt;BR&gt;
      3059L&lt;BR&gt;
      3059P&lt;BR&gt;
      3059Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      89P&lt;BR&gt;
      89W&lt;BR&gt;
      89X&lt;BR&gt;
      89PH&lt;BR&gt;
      76P&lt;BR&gt;
      89XH&lt;BR&gt;
      78SLT&lt;BR&gt;
      78L&amp;nbsp;ALT&lt;BR&gt;
      56P&amp;nbsp;ALT&lt;BR&gt;
      78P&amp;nbsp;ALT&lt;BR&gt;
      T8S&lt;BR&gt;
      78L&lt;BR&gt;
      56P&lt;BR&gt;
      78P&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      T18/784&lt;BR&gt;
      783&lt;BR&gt;
      781&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2199&lt;BR&gt;
      1697/1897&lt;BR&gt;
      1680/1880&lt;BR&gt;
      2187&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      8035EKP/CT20/RJ-20P&lt;BR&gt;
      -&lt;BR&gt;
      RJ-20X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      1211L&lt;BR&gt;
      8012EKQ&amp;nbsp;ALT&lt;BR&gt;
      8012EKR&amp;nbsp;ALT&lt;BR&gt;
      1211P&lt;BR&gt;
      8012EKJ&lt;BR&gt;
      8012EKL&lt;BR&gt;
      8012EKQ&lt;BR&gt;
      8012EKR&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      2101P&lt;BR&gt;
      2101W&lt;BR&gt;
      2101Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2102L&lt;BR&gt;
      2102S&lt;BR&gt;
      2102Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVMCOG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      43P&lt;BR&gt;
      43W&lt;BR&gt;
      43Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      40L&lt;BR&gt;
      40P&lt;BR&gt;
      40Y&lt;BR&gt;
      70Y-T602&lt;BR&gt;
      70L&lt;BR&gt;
      70P&lt;BR&gt;
      70Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SQUARE MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
   &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3250L&lt;BR&gt;
      3250P&lt;BR&gt;
      3250W&lt;BR&gt;
      3250X&lt;BR&gt;
      3252P&lt;BR&gt;
      3252W&lt;BR&gt;
      3252X&lt;BR&gt;
      3260P&lt;BR&gt;
      3260W&lt;BR&gt;
      3260X&lt;BR&gt;
      3262P&lt;BR&gt;
      3262W&lt;BR&gt;
      3262X&lt;BR&gt;
      3266P&lt;BR&gt;
      3266W&lt;BR&gt;
      3266X&lt;BR&gt;
      3290H&lt;BR&gt;
      3290P&lt;BR&gt;
      3290W&lt;BR&gt;
      3292P&lt;BR&gt;
      3292W&lt;BR&gt;
      3292X&lt;BR&gt;
      3296P&lt;BR&gt;
      3296W&lt;BR&gt;
      3296X&lt;BR&gt;
      3296Y&lt;BR&gt;
      3296Z&lt;BR&gt;
      3299P&lt;BR&gt;
      3299W&lt;BR&gt;
      3299X&lt;BR&gt;
      3299Y&lt;BR&gt;
      3299Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64P&amp;nbsp;ALT&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      64X&amp;nbsp;ALT&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66P&lt;BR&gt;
      66W&lt;BR&gt;
      66X&lt;BR&gt;
      67P&lt;BR&gt;
      67W&lt;BR&gt;
      67X&lt;BR&gt;
      67Y&lt;BR&gt;
      67Z&lt;BR&gt;
      68P&lt;BR&gt;
      68W&lt;BR&gt;
      68X&lt;BR&gt;
      67Y&amp;nbsp;ALT&lt;BR&gt;
      67Z&amp;nbsp;ALT&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      5050&lt;BR&gt;
      5091&lt;BR&gt;
      5080&lt;BR&gt;
      5087&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T63YB&lt;BR&gt;
      T63XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      5887&lt;BR&gt;
      5891&lt;BR&gt;
      5880&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T93Z&lt;BR&gt;
      T93YA&lt;BR&gt;
      T93XA&lt;BR&gt;
      T93YB&lt;BR&gt;
      T93XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKW&lt;BR&gt;
      8026EKM&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKB&lt;BR&gt;
      8026EKM&lt;BR&gt;
      1309X&lt;BR&gt;
      1309P&lt;BR&gt;
      1309W&lt;BR&gt;
      8024EKP&lt;BR&gt;
      8024EKW&lt;BR&gt;
      8024EKN&lt;BR&gt;
      RJ-9P/CT9P&lt;BR&gt;
      RJ-9W&lt;BR&gt;
      RJ-9X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3105P/3106P&lt;BR&gt;
      3105W/3106W&lt;BR&gt;
      3105X/3106X&lt;BR&gt;
      3105Y/3106Y&lt;BR&gt;
      3105Z/3105Z&lt;BR&gt;
      3102P&lt;BR&gt;
      3102W&lt;BR&gt;
      3102X&lt;BR&gt;
      3102Y&lt;BR&gt;
      3102Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMCBG&lt;BR&gt;
      EVMCCG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      55-1-X&lt;BR&gt;
      55-4-X&lt;BR&gt;
      55-3-X&lt;BR&gt;
      55-2-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      50-2-X&lt;BR&gt;
      50-4-X&lt;BR&gt;
      50-3-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      64Y&lt;BR&gt;
      64Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3323P&lt;BR&gt;
      3323S&lt;BR&gt;
      3323W&lt;BR&gt;
      3329H&lt;BR&gt;
      3329P&lt;BR&gt;
      3329W&lt;BR&gt;
      3339H&lt;BR&gt;
      3339P&lt;BR&gt;
      3339W&lt;BR&gt;
      3352E&lt;BR&gt;
      3352H&lt;BR&gt;
      3352K&lt;BR&gt;
      3352P&lt;BR&gt;
      3352T&lt;BR&gt;
      3352V&lt;BR&gt;
      3352W&lt;BR&gt;
      3362H&lt;BR&gt;
      3362M&lt;BR&gt;
      3362P&lt;BR&gt;
      3362R&lt;BR&gt;
      3362S&lt;BR&gt;
      3362U&lt;BR&gt;
      3362W&lt;BR&gt;
      3362X&lt;BR&gt;
      3386B&lt;BR&gt;
      3386C&lt;BR&gt;
      3386F&lt;BR&gt;
      3386H&lt;BR&gt;
      3386K&lt;BR&gt;
      3386M&lt;BR&gt;
      3386P&lt;BR&gt;
      3386S&lt;BR&gt;
      3386W&lt;BR&gt;
      3386X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      25P&lt;BR&gt;
      25S&lt;BR&gt;
      25RX&lt;BR&gt;
      82P&lt;BR&gt;
      82M&lt;BR&gt;
      82PA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      91E&lt;BR&gt;
      91X&lt;BR&gt;
      91T&lt;BR&gt;
      91B&lt;BR&gt;
      91A&lt;BR&gt;
      91V&lt;BR&gt;
      91W&lt;BR&gt;
      25W&lt;BR&gt;
      25V&lt;BR&gt;
      25P&lt;BR&gt;
      -&lt;BR&gt;
      25S&lt;BR&gt;
      25U&lt;BR&gt;
      25RX&lt;BR&gt;
      25X&lt;BR&gt;
      72XW&lt;BR&gt;
      72XL&lt;BR&gt;
      72PM&lt;BR&gt;
      72RX&lt;BR&gt;
      -&lt;BR&gt;
      72PX&lt;BR&gt;
      72P&lt;BR&gt;
      72RXW&lt;BR&gt;
      72RXL&lt;BR&gt;
      72X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T7YB&lt;BR&gt;
      T7YA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      TXD&lt;BR&gt;
      TYA&lt;BR&gt;
      TYP&lt;BR&gt;
      -&lt;BR&gt;
      TYD&lt;BR&gt;
      TX&lt;BR&gt;
      -&lt;BR&gt;
      150SX&lt;BR&gt;
      100SX&lt;BR&gt;
      102T&lt;BR&gt;
      101S&lt;BR&gt;
      190T&lt;BR&gt;
      150TX&lt;BR&gt;
      101&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      101SX&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ET6P&lt;BR&gt;
      ET6S&lt;BR&gt;
      ET6X&lt;BR&gt;
      RJ-6W/8014EMW&lt;BR&gt;
      RJ-6P/8014EMP&lt;BR&gt;
      RJ-6X/8014EMX&lt;BR&gt;
      TM7W&lt;BR&gt;
      TM7P&lt;BR&gt;
      TM7X&lt;BR&gt;
      -&lt;BR&gt;
      8017SMS&lt;BR&gt;
      -&lt;BR&gt;
      8017SMB&lt;BR&gt;
      8017SMA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      CT-6W&lt;BR&gt;
      CT-6H&lt;BR&gt;
      CT-6P&lt;BR&gt;
      CT-6R&lt;BR&gt;
      -&lt;BR&gt;
      CT-6V&lt;BR&gt;
      CT-6X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKV&lt;BR&gt;
      -&lt;BR&gt;
      8038EKX&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKP&lt;BR&gt;
      8038EKZ&lt;BR&gt;
      8038EKW&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3321H&lt;BR&gt;
      3321P&lt;BR&gt;
      3321N&lt;BR&gt;
      1102H&lt;BR&gt;
      1102P&lt;BR&gt;
      1102T&lt;BR&gt;
      RVA0911V304A&lt;BR&gt;
      -&lt;BR&gt;
      RVA0911H413A&lt;BR&gt;
      RVG0707V100A&lt;BR&gt;
      RVA0607V(H)306A&lt;BR&gt;
      RVA1214H213A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3104B&lt;BR&gt;
      3104C&lt;BR&gt;
      3104F&lt;BR&gt;
      3104H&lt;BR&gt;
      -&lt;BR&gt;
      3104M&lt;BR&gt;
      3104P&lt;BR&gt;
      3104S&lt;BR&gt;
      3104W&lt;BR&gt;
      3104X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      EVMQ0G&lt;BR&gt;
      EVMQIG&lt;BR&gt;
      EVMQ3G&lt;BR&gt;
      EVMS0G&lt;BR&gt;
      EVMQ0G&lt;BR&gt;
      EVMG0G&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMK4GA00B&lt;BR&gt;
      EVM30GA00B&lt;BR&gt;
      EVMK0GA00B&lt;BR&gt;
      EVM38GA00B&lt;BR&gt;
      EVMB6&lt;BR&gt;
      EVLQ0&lt;BR&gt;
      -&lt;BR&gt;
      EVMMSG&lt;BR&gt;
      EVMMBG&lt;BR&gt;
      EVMMAG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMMCS&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM0&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM3&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      62-3-1&lt;BR&gt;
      62-1-2&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67R&lt;BR&gt;
      -&lt;BR&gt;
      67P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67X&lt;BR&gt;
      63V&lt;BR&gt;
      63S&lt;BR&gt;
      63M&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63H&lt;BR&gt;
      63P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;&amp;nbsp;&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=3&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT color="#0000FF" SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SMD TRIM-POT CROSS REFERENCE&lt;/B&gt;&lt;/FONT&gt;
      &lt;P&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3224G&lt;BR&gt;
      3224J&lt;BR&gt;
      3224W&lt;BR&gt;
      3269P&lt;BR&gt;
      3269W&lt;BR&gt;
      3269X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      44G&lt;BR&gt;
      44J&lt;BR&gt;
      44W&lt;BR&gt;
      84P&lt;BR&gt;
      84W&lt;BR&gt;
      84X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST63Z&lt;BR&gt;
      ST63Y&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST5P&lt;BR&gt;
      ST5W&lt;BR&gt;
      ST5X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3314G&lt;BR&gt;
      3314J&lt;BR&gt;
      3364A/B&lt;BR&gt;
      3364C/D&lt;BR&gt;
      3364W/X&lt;BR&gt;
      3313G&lt;BR&gt;
      3313J&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      23B&lt;BR&gt;
      23A&lt;BR&gt;
      21X&lt;BR&gt;
      21W&lt;BR&gt;
      -&lt;BR&gt;
      22B&lt;BR&gt;
      22A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST5YL/ST53YL&lt;BR&gt;
      ST5YJ/5T53YJ&lt;BR&gt;
      ST-23A&lt;BR&gt;
      ST-22B&lt;BR&gt;
      ST-22&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST-4B&lt;BR&gt;
      ST-4A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST-3B&lt;BR&gt;
      ST-3A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVM-6YS&lt;BR&gt;
      EVM-1E&lt;BR&gt;
      EVM-1G&lt;BR&gt;
      EVM-1D&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      G4B&lt;BR&gt;
      G4A&lt;BR&gt;
      TR04-3S1&lt;BR&gt;
      TRG04-2S1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      DVR-43A&lt;BR&gt;
      CVR-42C&lt;BR&gt;
      CVR-42A/C&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;
&lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;ALT =&amp;nbsp;ALTERNATE&lt;/B&gt;&lt;/FONT&gt;
&lt;P&gt;

&amp;nbsp;
&lt;P&gt;
&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;
&lt;/BODY&gt;&lt;/HTML&gt;</description>
<packages>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="M1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.25 W</description>
</package>
<package name="140CLH-1010">
<description>&lt;b&gt;Aluminum electrolytic capacitors SMD (Chip)&lt;/b&gt;&lt;p&gt;
Long life base plate, High temperature 140 CLH&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
</packages>
</library>
<library name="con-ml">
<description>&lt;b&gt;Harting  Connectors&lt;/b&gt;&lt;p&gt;
Low profile connectors, straight&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="ML16">
<description>&lt;b&gt;HARTING&lt;/b&gt;</description>
</package>
<package name="ML10">
<description>&lt;b&gt;HARTING&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="crystal">
<description>&lt;b&gt;Crystals and Crystal Resonators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="CSM-7X-DU">
<description>&lt;b&gt;SMD CRYSTAL&lt;/b&gt;&lt;p&gt;
Source: www.ecsxtal.com .. Crystal 3.6864MHz CSM_7X_DU.PDF</description>
</package>
</packages>
</library>
<library name="con-harting-ml">
<description>&lt;b&gt;Harting  &amp; 3M Connectors&lt;/b&gt;&lt;p&gt;
Low profile connectors, straight&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="ML6">
<description>&lt;b&gt;HARTING&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT223">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SMC">
<description>&lt;b&gt;DIODE&lt;/b&gt;</description>
</package>
<package name="SMB">
<description>&lt;B&gt;DIODE&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="con-amp-quick">
<description>&lt;b&gt;AMP Connectors, Type QUICK&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="02P">
<description>&lt;b&gt;AMP QUICK CONNECTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="transistor-fet">
<description>&lt;b&gt;Field Effect Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
Symbols changed according to IEC617&lt;p&gt; 
All types, packages and assignment to symbols and pins checked&lt;p&gt;
Package outlines partly checked&lt;p&gt;
&lt;p&gt;
JFET = junction FET&lt;p&gt;
IGBT-x = insulated gate bipolar transistor&lt;p&gt;
x=N: NPN; x=P: PNP&lt;p&gt;
IGFET-mc-nnn; (IGFET=insulated gate field effect transistor)&lt;P&gt;
m=D: depletion mode (Verdr&amp;auml;ngungstyp)&lt;p&gt;
m=E: enhancement mode (Anreicherungstyp)&lt;p&gt;
c: N=N-channel; P=P-Channel&lt;p&gt;
GDSB: gate, drain, source, bulk&lt;p&gt;
&lt;p&gt;
by R. Vogg  15.March.2002</description>
<packages>
<package name="SO-8">
<description>&lt;b&gt;SO 8 small outline&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="atmel" package="DIL40" value="MEGA32-P">
<attribute name="OC_NEWARK" value="51P1794"/>
<attribute name="MPN" value="ATMEGA32-16PU"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1661729"/>
</element>
<element name="IC2" library="74xx-eu" package="SO20W" value="74ACT573D"/>
<element name="R1" library="resistor" package="R1206" value="100"/>
<element name="R2" library="resistor" package="R1206" value="100"/>
<element name="R3" library="resistor" package="R1206" value="100"/>
<element name="R4" library="resistor" package="R1206" value="100"/>
<element name="R5" library="resistor" package="R1206" value="100"/>
<element name="R6" library="resistor" package="R1206" value="100"/>
<element name="R7" library="resistor" package="R1206" value="100"/>
<element name="R8" library="resistor" package="R1206" value="100"/>
<element name="IC3" library="74xx-eu" package="SO20W" value="74ACT573D"/>
<element name="R9" library="resistor" package="R1206" value="100"/>
<element name="R10" library="resistor" package="R1206" value="100"/>
<element name="R11" library="resistor" package="R1206" value="100"/>
<element name="R12" library="resistor" package="R1206" value="100"/>
<element name="R13" library="resistor" package="R1206" value="100"/>
<element name="R14" library="resistor" package="R1206" value="100"/>
<element name="R15" library="resistor" package="R1206" value="100"/>
<element name="R16" library="resistor" package="R1206" value="100"/>
<element name="SV1" library="con-ml" package="ML16" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="IC4" library="74xx-eu" package="SO20W" value="74ACT573D"/>
<element name="R17" library="resistor" package="R1206" value="100"/>
<element name="R18" library="resistor" package="R1206" value="100"/>
<element name="R19" library="resistor" package="R1206" value="100"/>
<element name="R20" library="resistor" package="R1206" value="100"/>
<element name="R21" library="resistor" package="R1206" value="100"/>
<element name="R22" library="resistor" package="R1206" value="100"/>
<element name="R23" library="resistor" package="R1206" value="100"/>
<element name="R24" library="resistor" package="R1206" value="100"/>
<element name="IC5" library="74xx-eu" package="SO20W" value="74ACT573D"/>
<element name="R25" library="resistor" package="R1206" value="100"/>
<element name="R26" library="resistor" package="R1206" value="100"/>
<element name="R27" library="resistor" package="R1206" value="100"/>
<element name="R28" library="resistor" package="R1206" value="100"/>
<element name="R29" library="resistor" package="R1206" value="100"/>
<element name="R30" library="resistor" package="R1206" value="100"/>
<element name="R31" library="resistor" package="R1206" value="100"/>
<element name="R32" library="resistor" package="R1206" value="100"/>
<element name="SV2" library="con-ml" package="ML16" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="IC6" library="74xx-eu" package="SO20W" value="74ACT573D"/>
<element name="R33" library="resistor" package="R1206" value="100"/>
<element name="R34" library="resistor" package="R1206" value="100"/>
<element name="R35" library="resistor" package="R1206" value="100"/>
<element name="R36" library="resistor" package="R1206" value="100"/>
<element name="R37" library="resistor" package="R1206" value="100"/>
<element name="R38" library="resistor" package="R1206" value="100"/>
<element name="R39" library="resistor" package="R1206" value="100"/>
<element name="R40" library="resistor" package="R1206" value="100"/>
<element name="IC7" library="74xx-eu" package="SO20W" value="74ACT573D"/>
<element name="R41" library="resistor" package="R1206" value="100"/>
<element name="R42" library="resistor" package="R1206" value="100"/>
<element name="R43" library="resistor" package="R1206" value="100"/>
<element name="R44" library="resistor" package="R1206" value="100"/>
<element name="R45" library="resistor" package="R1206" value="100"/>
<element name="R46" library="resistor" package="R1206" value="100"/>
<element name="R47" library="resistor" package="R1206" value="100"/>
<element name="R48" library="resistor" package="R1206" value="100"/>
<element name="SV3" library="con-ml" package="ML16" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="IC8" library="74xx-eu" package="SO20W" value="74ACT573D"/>
<element name="R49" library="resistor" package="R1206" value="100"/>
<element name="R50" library="resistor" package="R1206" value="100"/>
<element name="R51" library="resistor" package="R1206" value="100"/>
<element name="R52" library="resistor" package="R1206" value="100"/>
<element name="R53" library="resistor" package="R1206" value="100"/>
<element name="R54" library="resistor" package="R1206" value="100"/>
<element name="R55" library="resistor" package="R1206" value="100"/>
<element name="R56" library="resistor" package="R1206" value="100"/>
<element name="IC9" library="74xx-eu" package="SO20W" value="74ACT573D"/>
<element name="R57" library="resistor" package="R1206" value="100"/>
<element name="R58" library="resistor" package="R1206" value="100"/>
<element name="R59" library="resistor" package="R1206" value="100"/>
<element name="R60" library="resistor" package="R1206" value="100"/>
<element name="R61" library="resistor" package="R1206" value="100"/>
<element name="R62" library="resistor" package="R1206" value="100"/>
<element name="R63" library="resistor" package="R1206" value="100"/>
<element name="R64" library="resistor" package="R1206" value="100"/>
<element name="SV4" library="con-ml" package="ML16" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="IC10" library="74xx-eu" package="SO20W" value="74HCT273DW"/>
<element name="SV5" library="con-ml" package="ML10" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="Q9" library="crystal" package="CSM-7X-DU" value="CSM-7X-DU">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="C1" library="resistor" package="C1206" value="22p"/>
<element name="C2" library="resistor" package="C1206" value="22p"/>
<element name="C3" library="resistor" package="C1206" value="100n"/>
<element name="C4" library="resistor" package="C1206" value="100n"/>
<element name="C5" library="resistor" package="C1206" value="100n"/>
<element name="C6" library="resistor" package="C1206" value="100n"/>
<element name="C7" library="resistor" package="C1206" value="100n"/>
<element name="C8" library="resistor" package="C1206" value="100n"/>
<element name="C9" library="resistor" package="C1206" value="100n"/>
<element name="C10" library="resistor" package="C1206" value="100n"/>
<element name="C11" library="resistor" package="C1206" value="100n"/>
<element name="C12" library="resistor" package="C1206" value="100n"/>
<element name="C13" library="resistor" package="C1206" value="100n"/>
<element name="C14" library="resistor" package="C1206" value="100n"/>
<element name="SV6" library="con-harting-ml" package="ML6" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="LED1" library="led" package="LED5MM" value=""/>
<element name="LED2" library="led" package="LED5MM" value=""/>
<element name="R65" library="resistor" package="M1206" value="330"/>
<element name="R66" library="resistor" package="M1206" value="330"/>
<element name="IC11" library="linear" package="SOT223" value="TS 2940 CW-5.0"/>
<element name="C15" library="resistor" package="C1206" value="100n"/>
<element name="C16" library="resistor" package="C1206" value="100n"/>
<element name="C17" library="resistor" package="140CLH-1010" value="470uF - 25V"/>
<element name="C18" library="resistor" package="140CLH-1010" value="470uF - 25V"/>
<element name="D1" library="diode" package="SMC" value="STPS 340 S"/>
<element name="D2" library="diode" package="SMB" value=""/>
<element name="SL1" library="con-amp-quick" package="02P" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="Q1" library="transistor-fet" package="SO-8" value="IRF 7220"/>
<element name="Q2" library="transistor-fet" package="SO-8" value="IRF 7220"/>
<element name="Q3" library="transistor-fet" package="SO-8" value="IRF 7220"/>
<element name="Q4" library="transistor-fet" package="SO-8" value="IRF 7220"/>
<element name="Q5" library="transistor-fet" package="SO-8" value="IRF 7220"/>
<element name="Q6" library="transistor-fet" package="SO-8" value="IRF 7220"/>
<element name="Q7" library="transistor-fet" package="SO-8" value="IRF 7220"/>
<element name="Q8" library="transistor-fet" package="SO-8" value="IRF 7220"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="IC2" pad="19"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="IC2" pad="18"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="IC2" pad="17"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="IC2" pad="16"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="IC2" pad="15"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="IC2" pad="14"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="IC2" pad="13"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="IC2" pad="12"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="IC3" pad="19"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="IC3" pad="18"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="IC3" pad="17"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="IC3" pad="16"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="IC3" pad="15"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="IC3" pad="14"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="IC3" pad="13"/>
<contactref element="R15" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="IC3" pad="12"/>
<contactref element="R16" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="R8" pad="2"/>
<contactref element="SV1" pad="15"/>
</signal>
<signal name="N$18">
<contactref element="R7" pad="2"/>
<contactref element="SV1" pad="13"/>
</signal>
<signal name="N$19">
<contactref element="R6" pad="2"/>
<contactref element="SV1" pad="11"/>
</signal>
<signal name="N$20">
<contactref element="R5" pad="2"/>
<contactref element="SV1" pad="9"/>
</signal>
<signal name="N$21">
<contactref element="R4" pad="2"/>
<contactref element="SV1" pad="7"/>
</signal>
<signal name="N$22">
<contactref element="R3" pad="2"/>
<contactref element="SV1" pad="5"/>
</signal>
<signal name="N$23">
<contactref element="R2" pad="2"/>
<contactref element="SV1" pad="3"/>
</signal>
<signal name="N$24">
<contactref element="R1" pad="2"/>
<contactref element="SV1" pad="1"/>
</signal>
<signal name="N$25">
<contactref element="R9" pad="2"/>
<contactref element="SV1" pad="16"/>
</signal>
<signal name="N$26">
<contactref element="R10" pad="2"/>
<contactref element="SV1" pad="14"/>
</signal>
<signal name="N$27">
<contactref element="SV1" pad="12"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="N$28">
<contactref element="R12" pad="2"/>
<contactref element="SV1" pad="10"/>
</signal>
<signal name="N$29">
<contactref element="R13" pad="2"/>
<contactref element="SV1" pad="8"/>
</signal>
<signal name="N$30">
<contactref element="R16" pad="2"/>
<contactref element="SV1" pad="2"/>
</signal>
<signal name="N$31">
<contactref element="R15" pad="2"/>
<contactref element="SV1" pad="4"/>
</signal>
<signal name="N$32">
<contactref element="R14" pad="2"/>
<contactref element="SV1" pad="6"/>
</signal>
<signal name="N$33">
<contactref element="IC4" pad="19"/>
<contactref element="R17" pad="1"/>
</signal>
<signal name="N$34">
<contactref element="IC4" pad="18"/>
<contactref element="R18" pad="1"/>
</signal>
<signal name="N$35">
<contactref element="IC4" pad="17"/>
<contactref element="R19" pad="1"/>
</signal>
<signal name="N$36">
<contactref element="IC4" pad="16"/>
<contactref element="R20" pad="1"/>
</signal>
<signal name="N$37">
<contactref element="IC4" pad="15"/>
<contactref element="R21" pad="1"/>
</signal>
<signal name="N$38">
<contactref element="IC4" pad="14"/>
<contactref element="R22" pad="1"/>
</signal>
<signal name="N$39">
<contactref element="IC4" pad="13"/>
<contactref element="R23" pad="1"/>
</signal>
<signal name="N$40">
<contactref element="IC4" pad="12"/>
<contactref element="R24" pad="1"/>
</signal>
<signal name="N$41">
<contactref element="IC5" pad="19"/>
<contactref element="R25" pad="1"/>
</signal>
<signal name="N$42">
<contactref element="IC5" pad="18"/>
<contactref element="R26" pad="1"/>
</signal>
<signal name="N$43">
<contactref element="IC5" pad="17"/>
<contactref element="R27" pad="1"/>
</signal>
<signal name="N$44">
<contactref element="IC5" pad="16"/>
<contactref element="R28" pad="1"/>
</signal>
<signal name="N$45">
<contactref element="IC5" pad="15"/>
<contactref element="R29" pad="1"/>
</signal>
<signal name="N$46">
<contactref element="IC5" pad="14"/>
<contactref element="R30" pad="1"/>
</signal>
<signal name="N$47">
<contactref element="IC5" pad="13"/>
<contactref element="R31" pad="1"/>
</signal>
<signal name="N$48">
<contactref element="IC5" pad="12"/>
<contactref element="R32" pad="1"/>
</signal>
<signal name="N$49">
<contactref element="R24" pad="2"/>
<contactref element="SV2" pad="15"/>
</signal>
<signal name="N$50">
<contactref element="R23" pad="2"/>
<contactref element="SV2" pad="13"/>
</signal>
<signal name="N$51">
<contactref element="R22" pad="2"/>
<contactref element="SV2" pad="11"/>
</signal>
<signal name="N$52">
<contactref element="R21" pad="2"/>
<contactref element="SV2" pad="9"/>
</signal>
<signal name="N$53">
<contactref element="R20" pad="2"/>
<contactref element="SV2" pad="7"/>
</signal>
<signal name="N$54">
<contactref element="R19" pad="2"/>
<contactref element="SV2" pad="5"/>
</signal>
<signal name="N$55">
<contactref element="R18" pad="2"/>
<contactref element="SV2" pad="3"/>
</signal>
<signal name="N$56">
<contactref element="R17" pad="2"/>
<contactref element="SV2" pad="1"/>
</signal>
<signal name="N$57">
<contactref element="R25" pad="2"/>
<contactref element="SV2" pad="16"/>
</signal>
<signal name="N$58">
<contactref element="R26" pad="2"/>
<contactref element="SV2" pad="14"/>
</signal>
<signal name="N$59">
<contactref element="SV2" pad="12"/>
<contactref element="R27" pad="2"/>
</signal>
<signal name="N$60">
<contactref element="R28" pad="2"/>
<contactref element="SV2" pad="10"/>
</signal>
<signal name="N$61">
<contactref element="R29" pad="2"/>
<contactref element="SV2" pad="8"/>
</signal>
<signal name="N$62">
<contactref element="R32" pad="2"/>
<contactref element="SV2" pad="2"/>
</signal>
<signal name="N$63">
<contactref element="R31" pad="2"/>
<contactref element="SV2" pad="4"/>
</signal>
<signal name="N$64">
<contactref element="R30" pad="2"/>
<contactref element="SV2" pad="6"/>
</signal>
<signal name="N$65">
<contactref element="IC6" pad="19"/>
<contactref element="R33" pad="1"/>
</signal>
<signal name="N$66">
<contactref element="IC6" pad="18"/>
<contactref element="R34" pad="1"/>
</signal>
<signal name="N$67">
<contactref element="IC6" pad="17"/>
<contactref element="R35" pad="1"/>
</signal>
<signal name="N$68">
<contactref element="IC6" pad="16"/>
<contactref element="R36" pad="1"/>
</signal>
<signal name="N$69">
<contactref element="IC6" pad="15"/>
<contactref element="R37" pad="1"/>
</signal>
<signal name="N$70">
<contactref element="IC6" pad="14"/>
<contactref element="R38" pad="1"/>
</signal>
<signal name="N$71">
<contactref element="IC6" pad="13"/>
<contactref element="R39" pad="1"/>
</signal>
<signal name="N$72">
<contactref element="IC6" pad="12"/>
<contactref element="R40" pad="1"/>
</signal>
<signal name="N$73">
<contactref element="IC7" pad="19"/>
<contactref element="R41" pad="1"/>
</signal>
<signal name="N$74">
<contactref element="IC7" pad="18"/>
<contactref element="R42" pad="1"/>
</signal>
<signal name="N$75">
<contactref element="IC7" pad="17"/>
<contactref element="R43" pad="1"/>
</signal>
<signal name="N$76">
<contactref element="IC7" pad="16"/>
<contactref element="R44" pad="1"/>
</signal>
<signal name="N$77">
<contactref element="IC7" pad="15"/>
<contactref element="R45" pad="1"/>
</signal>
<signal name="N$78">
<contactref element="IC7" pad="14"/>
<contactref element="R46" pad="1"/>
</signal>
<signal name="N$79">
<contactref element="IC7" pad="13"/>
<contactref element="R47" pad="1"/>
</signal>
<signal name="N$80">
<contactref element="IC7" pad="12"/>
<contactref element="R48" pad="1"/>
</signal>
<signal name="N$81">
<contactref element="R40" pad="2"/>
<contactref element="SV3" pad="15"/>
</signal>
<signal name="N$82">
<contactref element="R39" pad="2"/>
<contactref element="SV3" pad="13"/>
</signal>
<signal name="N$83">
<contactref element="R38" pad="2"/>
<contactref element="SV3" pad="11"/>
</signal>
<signal name="N$84">
<contactref element="R37" pad="2"/>
<contactref element="SV3" pad="9"/>
</signal>
<signal name="N$85">
<contactref element="R36" pad="2"/>
<contactref element="SV3" pad="7"/>
</signal>
<signal name="N$86">
<contactref element="R35" pad="2"/>
<contactref element="SV3" pad="5"/>
</signal>
<signal name="N$87">
<contactref element="R34" pad="2"/>
<contactref element="SV3" pad="3"/>
</signal>
<signal name="N$88">
<contactref element="R33" pad="2"/>
<contactref element="SV3" pad="1"/>
</signal>
<signal name="N$89">
<contactref element="R41" pad="2"/>
<contactref element="SV3" pad="16"/>
</signal>
<signal name="N$90">
<contactref element="R42" pad="2"/>
<contactref element="SV3" pad="14"/>
</signal>
<signal name="N$91">
<contactref element="SV3" pad="12"/>
<contactref element="R43" pad="2"/>
</signal>
<signal name="N$92">
<contactref element="R44" pad="2"/>
<contactref element="SV3" pad="10"/>
</signal>
<signal name="N$93">
<contactref element="R45" pad="2"/>
<contactref element="SV3" pad="8"/>
</signal>
<signal name="N$94">
<contactref element="R48" pad="2"/>
<contactref element="SV3" pad="2"/>
</signal>
<signal name="N$95">
<contactref element="R47" pad="2"/>
<contactref element="SV3" pad="4"/>
</signal>
<signal name="N$96">
<contactref element="R46" pad="2"/>
<contactref element="SV3" pad="6"/>
</signal>
<signal name="N$97">
<contactref element="IC8" pad="19"/>
<contactref element="R49" pad="1"/>
</signal>
<signal name="N$98">
<contactref element="IC8" pad="18"/>
<contactref element="R50" pad="1"/>
</signal>
<signal name="N$99">
<contactref element="IC8" pad="17"/>
<contactref element="R51" pad="1"/>
</signal>
<signal name="N$100">
<contactref element="IC8" pad="16"/>
<contactref element="R52" pad="1"/>
</signal>
<signal name="N$101">
<contactref element="IC8" pad="15"/>
<contactref element="R53" pad="1"/>
</signal>
<signal name="N$102">
<contactref element="IC8" pad="14"/>
<contactref element="R54" pad="1"/>
</signal>
<signal name="N$103">
<contactref element="IC8" pad="13"/>
<contactref element="R55" pad="1"/>
</signal>
<signal name="N$104">
<contactref element="IC8" pad="12"/>
<contactref element="R56" pad="1"/>
</signal>
<signal name="N$105">
<contactref element="IC9" pad="19"/>
<contactref element="R57" pad="1"/>
</signal>
<signal name="N$106">
<contactref element="IC9" pad="18"/>
<contactref element="R58" pad="1"/>
</signal>
<signal name="N$107">
<contactref element="IC9" pad="17"/>
<contactref element="R59" pad="1"/>
</signal>
<signal name="N$108">
<contactref element="IC9" pad="16"/>
<contactref element="R60" pad="1"/>
</signal>
<signal name="N$109">
<contactref element="IC9" pad="15"/>
<contactref element="R61" pad="1"/>
</signal>
<signal name="N$110">
<contactref element="IC9" pad="14"/>
<contactref element="R62" pad="1"/>
</signal>
<signal name="N$111">
<contactref element="IC9" pad="13"/>
<contactref element="R63" pad="1"/>
</signal>
<signal name="N$112">
<contactref element="IC9" pad="12"/>
<contactref element="R64" pad="1"/>
</signal>
<signal name="N$113">
<contactref element="R56" pad="2"/>
<contactref element="SV4" pad="15"/>
</signal>
<signal name="N$114">
<contactref element="R55" pad="2"/>
<contactref element="SV4" pad="13"/>
</signal>
<signal name="N$115">
<contactref element="R54" pad="2"/>
<contactref element="SV4" pad="11"/>
</signal>
<signal name="N$116">
<contactref element="R53" pad="2"/>
<contactref element="SV4" pad="9"/>
</signal>
<signal name="N$117">
<contactref element="R52" pad="2"/>
<contactref element="SV4" pad="7"/>
</signal>
<signal name="N$118">
<contactref element="R51" pad="2"/>
<contactref element="SV4" pad="5"/>
</signal>
<signal name="N$119">
<contactref element="R50" pad="2"/>
<contactref element="SV4" pad="3"/>
</signal>
<signal name="N$120">
<contactref element="R49" pad="2"/>
<contactref element="SV4" pad="1"/>
</signal>
<signal name="N$121">
<contactref element="R57" pad="2"/>
<contactref element="SV4" pad="16"/>
</signal>
<signal name="N$122">
<contactref element="R58" pad="2"/>
<contactref element="SV4" pad="14"/>
</signal>
<signal name="N$123">
<contactref element="SV4" pad="12"/>
<contactref element="R59" pad="2"/>
</signal>
<signal name="N$124">
<contactref element="R60" pad="2"/>
<contactref element="SV4" pad="10"/>
</signal>
<signal name="N$125">
<contactref element="R61" pad="2"/>
<contactref element="SV4" pad="8"/>
</signal>
<signal name="N$126">
<contactref element="R64" pad="2"/>
<contactref element="SV4" pad="2"/>
</signal>
<signal name="N$127">
<contactref element="R63" pad="2"/>
<contactref element="SV4" pad="4"/>
</signal>
<signal name="N$128">
<contactref element="R62" pad="2"/>
<contactref element="SV4" pad="6"/>
</signal>
<signal name="N$129">
<contactref element="IC2" pad="9"/>
<contactref element="IC3" pad="9"/>
<contactref element="IC4" pad="9"/>
<contactref element="IC5" pad="9"/>
<contactref element="IC7" pad="9"/>
<contactref element="IC8" pad="9"/>
<contactref element="IC9" pad="9"/>
<contactref element="IC6" pad="9"/>
<contactref element="IC1" pad="33"/>
</signal>
<signal name="N$130">
<contactref element="IC9" pad="8"/>
<contactref element="IC8" pad="8"/>
<contactref element="IC7" pad="8"/>
<contactref element="IC6" pad="8"/>
<contactref element="IC5" pad="8"/>
<contactref element="IC4" pad="8"/>
<contactref element="IC3" pad="8"/>
<contactref element="IC2" pad="8"/>
<contactref element="IC1" pad="34"/>
</signal>
<signal name="N$131">
<contactref element="IC9" pad="7"/>
<contactref element="IC8" pad="7"/>
<contactref element="IC7" pad="7"/>
<contactref element="IC6" pad="7"/>
<contactref element="IC5" pad="7"/>
<contactref element="IC4" pad="7"/>
<contactref element="IC3" pad="7"/>
<contactref element="IC2" pad="7"/>
<contactref element="IC1" pad="35"/>
</signal>
<signal name="N$132">
<contactref element="IC9" pad="6"/>
<contactref element="IC8" pad="6"/>
<contactref element="IC7" pad="6"/>
<contactref element="IC6" pad="6"/>
<contactref element="IC5" pad="6"/>
<contactref element="IC4" pad="6"/>
<contactref element="IC3" pad="6"/>
<contactref element="IC2" pad="6"/>
<contactref element="IC1" pad="36"/>
</signal>
<signal name="N$133">
<contactref element="IC9" pad="5"/>
<contactref element="IC8" pad="5"/>
<contactref element="IC7" pad="5"/>
<contactref element="IC6" pad="5"/>
<contactref element="IC5" pad="5"/>
<contactref element="IC4" pad="5"/>
<contactref element="IC3" pad="5"/>
<contactref element="IC2" pad="5"/>
<contactref element="IC1" pad="37"/>
</signal>
<signal name="N$134">
<contactref element="IC9" pad="4"/>
<contactref element="IC8" pad="4"/>
<contactref element="IC7" pad="4"/>
<contactref element="IC6" pad="4"/>
<contactref element="IC5" pad="4"/>
<contactref element="IC4" pad="4"/>
<contactref element="IC3" pad="4"/>
<contactref element="IC2" pad="4"/>
<contactref element="IC1" pad="38"/>
</signal>
<signal name="N$135">
<contactref element="IC9" pad="3"/>
<contactref element="IC8" pad="3"/>
<contactref element="IC7" pad="3"/>
<contactref element="IC6" pad="3"/>
<contactref element="IC5" pad="3"/>
<contactref element="IC4" pad="3"/>
<contactref element="IC3" pad="3"/>
<contactref element="IC2" pad="3"/>
<contactref element="IC1" pad="39"/>
</signal>
<signal name="N$136">
<contactref element="IC9" pad="2"/>
<contactref element="IC8" pad="2"/>
<contactref element="IC7" pad="2"/>
<contactref element="IC6" pad="2"/>
<contactref element="IC5" pad="2"/>
<contactref element="IC4" pad="2"/>
<contactref element="IC3" pad="2"/>
<contactref element="IC2" pad="2"/>
<contactref element="IC1" pad="40"/>
</signal>
<signal name="N$137">
<contactref element="IC9" pad="11"/>
<contactref element="IC1" pad="22"/>
</signal>
<signal name="N$138">
<contactref element="IC2" pad="11"/>
<contactref element="IC1" pad="29"/>
</signal>
<signal name="N$139">
<contactref element="IC3" pad="11"/>
<contactref element="IC1" pad="28"/>
</signal>
<signal name="N$140">
<contactref element="IC4" pad="11"/>
<contactref element="IC1" pad="27"/>
</signal>
<signal name="N$141">
<contactref element="IC5" pad="11"/>
<contactref element="IC1" pad="26"/>
</signal>
<signal name="N$142">
<contactref element="IC6" pad="11"/>
<contactref element="IC1" pad="25"/>
</signal>
<signal name="N$143">
<contactref element="IC7" pad="11"/>
<contactref element="IC1" pad="24"/>
</signal>
<signal name="N$144">
<contactref element="IC8" pad="11"/>
<contactref element="IC1" pad="23"/>
</signal>
<signal name="N$145">
<contactref element="IC1" pad="14"/>
<contactref element="IC10" pad="3"/>
</signal>
<signal name="N$146">
<contactref element="IC1" pad="15"/>
<contactref element="IC10" pad="4"/>
</signal>
<signal name="N$147">
<contactref element="IC1" pad="16"/>
<contactref element="IC10" pad="7"/>
</signal>
<signal name="N$148">
<contactref element="IC1" pad="17"/>
<contactref element="IC10" pad="8"/>
</signal>
<signal name="N$149">
<contactref element="IC1" pad="18"/>
<contactref element="IC10" pad="13"/>
</signal>
<signal name="N$150">
<contactref element="IC1" pad="19"/>
<contactref element="IC10" pad="14"/>
</signal>
<signal name="N$151">
<contactref element="IC1" pad="20"/>
<contactref element="IC10" pad="17"/>
</signal>
<signal name="N$152">
<contactref element="IC1" pad="21"/>
<contactref element="IC10" pad="18"/>
</signal>
<signal name="VCC">
<contactref element="Q1" pad="1"/>
<contactref element="Q1" pad="2"/>
<contactref element="Q1" pad="3"/>
<contactref element="Q5" pad="1"/>
<contactref element="Q5" pad="2"/>
<contactref element="Q5" pad="3"/>
<contactref element="Q7" pad="1"/>
<contactref element="Q7" pad="2"/>
<contactref element="Q7" pad="3"/>
<contactref element="Q8" pad="1"/>
<contactref element="Q8" pad="2"/>
<contactref element="Q8" pad="3"/>
<contactref element="Q4" pad="1"/>
<contactref element="Q4" pad="2"/>
<contactref element="Q4" pad="3"/>
<contactref element="Q3" pad="1"/>
<contactref element="Q3" pad="2"/>
<contactref element="Q3" pad="3"/>
<contactref element="Q2" pad="1"/>
<contactref element="Q2" pad="2"/>
<contactref element="Q2" pad="3"/>
<contactref element="Q6" pad="1"/>
<contactref element="Q6" pad="2"/>
<contactref element="Q6" pad="3"/>
<contactref element="SV6" pad="2"/>
<contactref element="R65" pad="2"/>
<contactref element="R66" pad="2"/>
<contactref element="IC11" pad="3"/>
<contactref element="C15" pad="1"/>
<contactref element="C17" pad="+"/>
<contactref element="IC10" pad="1"/>
<contactref element="IC1" pad="30"/>
<contactref element="C3" pad="2"/>
<contactref element="IC1" pad="10"/>
<contactref element="C4" pad="2"/>
<contactref element="IC10" pad="20"/>
<contactref element="C6" pad="2"/>
<contactref element="IC9" pad="20"/>
<contactref element="C14" pad="2"/>
<contactref element="IC9" pad="20"/>
<contactref element="IC8" pad="20"/>
<contactref element="C9" pad="2"/>
<contactref element="IC8" pad="20"/>
<contactref element="IC7" pad="20"/>
<contactref element="C8" pad="2"/>
<contactref element="IC7" pad="20"/>
<contactref element="IC6" pad="20"/>
<contactref element="IC6" pad="20"/>
<contactref element="C7" pad="2"/>
<contactref element="IC5" pad="20"/>
<contactref element="IC5" pad="20"/>
<contactref element="C13" pad="2"/>
<contactref element="IC4" pad="20"/>
<contactref element="IC4" pad="20"/>
<contactref element="C12" pad="2"/>
<contactref element="IC3" pad="20"/>
<contactref element="IC3" pad="20"/>
<contactref element="C11" pad="2"/>
<contactref element="IC2" pad="20"/>
<contactref element="C10" pad="2"/>
<contactref element="IC2" pad="20"/>
</signal>
<signal name="N$153">
<contactref element="SV5" pad="10"/>
<contactref element="Q4" pad="5"/>
<contactref element="Q4" pad="6"/>
<contactref element="Q4" pad="7"/>
<contactref element="Q4" pad="8"/>
</signal>
<signal name="N$154">
<contactref element="SV5" pad="8"/>
<contactref element="Q3" pad="5"/>
<contactref element="Q3" pad="6"/>
<contactref element="Q3" pad="7"/>
<contactref element="Q3" pad="8"/>
</signal>
<signal name="N$155">
<contactref element="SV5" pad="6"/>
<contactref element="Q2" pad="5"/>
<contactref element="Q2" pad="6"/>
<contactref element="Q2" pad="7"/>
<contactref element="Q2" pad="8"/>
</signal>
<signal name="N$156">
<contactref element="SV5" pad="4"/>
<contactref element="Q1" pad="5"/>
<contactref element="Q1" pad="6"/>
<contactref element="Q1" pad="7"/>
<contactref element="Q1" pad="8"/>
</signal>
<signal name="N$157">
<contactref element="SV5" pad="9"/>
<contactref element="Q5" pad="5"/>
<contactref element="Q5" pad="6"/>
<contactref element="Q5" pad="7"/>
<contactref element="Q5" pad="8"/>
</signal>
<signal name="N$158">
<contactref element="SV5" pad="7"/>
<contactref element="Q6" pad="5"/>
<contactref element="Q6" pad="6"/>
<contactref element="Q6" pad="7"/>
<contactref element="Q6" pad="8"/>
</signal>
<signal name="N$159">
<contactref element="SV5" pad="5"/>
<contactref element="Q7" pad="5"/>
<contactref element="Q7" pad="6"/>
<contactref element="Q7" pad="7"/>
<contactref element="Q7" pad="8"/>
</signal>
<signal name="N$160">
<contactref element="SV5" pad="3"/>
<contactref element="Q8" pad="5"/>
<contactref element="Q8" pad="6"/>
<contactref element="Q8" pad="7"/>
<contactref element="Q8" pad="8"/>
</signal>
<signal name="N$161">
<contactref element="IC10" pad="2"/>
<contactref element="Q8" pad="4"/>
</signal>
<signal name="N$162">
<contactref element="IC10" pad="5"/>
<contactref element="Q7" pad="4"/>
</signal>
<signal name="N$163">
<contactref element="IC10" pad="6"/>
<contactref element="Q6" pad="4"/>
</signal>
<signal name="N$164">
<contactref element="IC10" pad="9"/>
<contactref element="Q5" pad="4"/>
</signal>
<signal name="N$165">
<contactref element="IC10" pad="12"/>
<contactref element="Q4" pad="4"/>
</signal>
<signal name="N$166">
<contactref element="IC10" pad="15"/>
<contactref element="Q3" pad="4"/>
</signal>
<signal name="N$167">
<contactref element="IC10" pad="16"/>
<contactref element="Q2" pad="4"/>
</signal>
<signal name="N$168">
<contactref element="IC10" pad="19"/>
<contactref element="Q1" pad="4"/>
</signal>
<signal name="N$169">
<contactref element="IC1" pad="12"/>
<contactref element="C1" pad="2"/>
<contactref element="Q9" pad="2"/>
</signal>
<signal name="N$170">
<contactref element="IC1" pad="13"/>
<contactref element="C2" pad="2"/>
<contactref element="Q9" pad="1"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="SV6" pad="6"/>
<contactref element="C15" pad="2"/>
<contactref element="C17" pad="-"/>
<contactref element="IC11" pad="2"/>
<contactref element="D2" pad="A"/>
<contactref element="C18" pad="-"/>
<contactref element="C16" pad="2"/>
<contactref element="IC2" pad="1"/>
<contactref element="IC3" pad="1"/>
<contactref element="IC4" pad="1"/>
<contactref element="IC5" pad="1"/>
<contactref element="IC6" pad="1"/>
<contactref element="IC7" pad="1"/>
<contactref element="IC8" pad="1"/>
<contactref element="IC9" pad="1"/>
<contactref element="SL1" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="IC1" pad="31"/>
<contactref element="IC1" pad="11"/>
<contactref element="C4" pad="1"/>
<contactref element="IC10" pad="10"/>
<contactref element="C6" pad="1"/>
<contactref element="IC10" pad="10"/>
<contactref element="IC9" pad="10"/>
<contactref element="C14" pad="1"/>
<contactref element="IC9" pad="10"/>
<contactref element="IC8" pad="10"/>
<contactref element="C9" pad="1"/>
<contactref element="IC8" pad="10"/>
<contactref element="IC7" pad="10"/>
<contactref element="IC7" pad="10"/>
<contactref element="C8" pad="1"/>
<contactref element="IC6" pad="10"/>
<contactref element="C7" pad="1"/>
<contactref element="IC6" pad="10"/>
<contactref element="IC5" pad="10"/>
<contactref element="C13" pad="1"/>
<contactref element="IC5" pad="10"/>
<contactref element="IC4" pad="10"/>
<contactref element="C12" pad="1"/>
<contactref element="IC4" pad="10"/>
<contactref element="IC3" pad="10"/>
<contactref element="C11" pad="1"/>
<contactref element="IC3" pad="10"/>
<contactref element="IC2" pad="10"/>
<contactref element="IC2" pad="10"/>
<contactref element="C10" pad="1"/>
</signal>
<signal name="N$171">
<contactref element="IC1" pad="32"/>
<contactref element="C5" pad="2"/>
</signal>
<signal name="N$194">
<contactref element="IC1" pad="8"/>
<contactref element="SV6" pad="3"/>
</signal>
<signal name="N$195">
<contactref element="IC1" pad="7"/>
<contactref element="SV6" pad="1"/>
</signal>
<signal name="N$196">
<contactref element="IC1" pad="6"/>
<contactref element="SV6" pad="4"/>
</signal>
<signal name="N$197">
<contactref element="IC1" pad="9"/>
<contactref element="SV6" pad="5"/>
</signal>
<signal name="N$198">
<contactref element="R65" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$199">
<contactref element="R66" pad="1"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="N$200">
<contactref element="IC1" pad="5"/>
<contactref element="LED1" pad="K"/>
</signal>
<signal name="N$201">
<contactref element="IC1" pad="4"/>
<contactref element="LED2" pad="K"/>
</signal>
<signal name="N$202">
<contactref element="SL1" pad="2"/>
<contactref element="D1" pad="A"/>
<contactref element="D2" pad="C"/>
</signal>
<signal name="N$203">
<contactref element="D1" pad="C"/>
<contactref element="IC11" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="C18" pad="+"/>
</signal>
<signal name="N$205">
<contactref element="IC1" pad="1"/>
<contactref element="IC10" pad="11"/>
</signal>
<signal name="N$216">
</signal>
<signal name="N$227">
</signal>
<signal name="N$228">
</signal>
<signal name="N$231">
</signal>
<signal name="N$232">
</signal>
<signal name="N$233">
</signal>
<signal name="N$234">
</signal>
<signal name="N$235">
</signal>
<signal name="N$239">
</signal>
<signal name="N$240">
</signal>
<signal name="N$241">
</signal>
<signal name="N$242">
</signal>
<signal name="N$243">
</signal>
<signal name="N$244">
</signal>
<signal name="N$245">
</signal>
<signal name="N$246">
</signal>
<signal name="N$247">
</signal>
<signal name="N$248">
</signal>
<signal name="N$249">
</signal>
<signal name="N$250">
</signal>
<signal name="N$251">
</signal>
<signal name="N$252">
</signal>
<signal name="N$253">
</signal>
<signal name="N$254">
</signal>
<signal name="N$255">
</signal>
<signal name="N$256">
</signal>
<signal name="N$258">
</signal>
<signal name="N$259">
</signal>
<signal name="N$260">
</signal>
<signal name="N$261">
</signal>
<signal name="N$262">
</signal>
<signal name="N$263">
</signal>
<signal name="N$264">
</signal>
<signal name="N$174">
</signal>
<signal name="N$175">
</signal>
<signal name="N$172">
</signal>
<signal name="N$173">
</signal>
<signal name="N$176">
</signal>
</signals>
</board>
</drawing>
</eagle>
