<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<library>
<packages>
<package name="STM32F407_LQFP176">
<description>LQFP176 Package for STM32F407IGT6
by Ersan Günes v0.1</description>
</package>
</packages>
<symbols>
<symbol name="STM32F407_LQFP176_RL">
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PE4"/>
<pin name="PE5"/>
<pin name="PE6"/>
<pin name="VBAT" direction="pwr"/>
<pin name="PI8"/>
<pin name="PC13"/>
<pin name="PC14/OSC32_IN"/>
<pin name="PC15/OSC32_OUT"/>
<pin name="PI9"/>
<pin name="PI10"/>
<pin name="PI11"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="PF0"/>
<pin name="PF1"/>
<pin name="PF2"/>
<pin name="PF3"/>
<pin name="PF4"/>
<pin name="PF5"/>
<pin name="VSS_1" direction="pwr"/>
<pin name="VDD_1" direction="pwr"/>
<pin name="PF6"/>
<pin name="PF7"/>
<pin name="PF8"/>
<pin name="PF9"/>
<pin name="PF10"/>
<pin name="PH0/OSC_IN"/>
<pin name="PH1/OSC_OUT"/>
<pin name="NRST"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="VDD_2" direction="pwr"/>
<pin name="VSSA" direction="pwr"/>
<pin name="VREF+" direction="pwr"/>
<pin name="VDDA" direction="pwr"/>
<pin name="PA0/WKUP"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PH2"/>
<pin name="PH3"/>
<pin name="PH4"/>
<pin name="PH5"/>
<pin name="PA3"/>
<pin name="VSS_4" direction="pwr"/>
<pin name="VDD_3" direction="pwr"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2/BOOT_1"/>
<pin name="PF11"/>
<pin name="PF12"/>
<pin name="VSS_5" direction="pwr"/>
<pin name="VDD_4" direction="pwr"/>
<pin name="PF13"/>
<pin name="PF14"/>
<pin name="PF15"/>
<pin name="PG0"/>
<pin name="PG1"/>
<pin name="PE7"/>
<pin name="PE8"/>
<pin name="PE9"/>
<pin name="VSS_6" direction="pwr"/>
<pin name="VDD_5" direction="pwr"/>
<pin name="PE10"/>
<pin name="PE11"/>
<pin name="PE12"/>
<pin name="PE13"/>
<pin name="PE14"/>
<pin name="PE15"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="VCAP_1" direction="pwr"/>
<pin name="VDD_6" direction="pwr"/>
<pin name="PH6"/>
<pin name="PH7"/>
<pin name="PH8"/>
<pin name="PH9"/>
<pin name="PH10"/>
<pin name="PH11"/>
<pin name="PH12"/>
<pin name="VSS_7" direction="pwr"/>
<pin name="VDD_7" direction="pwr"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PD8"/>
<pin name="PD9"/>
<pin name="PD10"/>
<pin name="PD11"/>
<pin name="PD12"/>
<pin name="PD13"/>
<pin name="VSS_8" direction="pwr"/>
<pin name="VDD_8" direction="pwr"/>
<pin name="PD14"/>
<pin name="PD15"/>
<pin name="PG2"/>
<pin name="PG3"/>
<pin name="PG4"/>
<pin name="PG5"/>
<pin name="PG6"/>
<pin name="PG7"/>
<pin name="PG8"/>
<pin name="VSS_9" direction="pwr"/>
<pin name="VDD_9" direction="pwr"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PA8"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PA13"/>
<pin name="VCAP_2" direction="pwr"/>
<pin name="VSS_10" direction="pwr"/>
<pin name="VDD_10" direction="pwr"/>
<pin name="PH13"/>
<pin name="PH14"/>
<pin name="PH15"/>
<pin name="PI0"/>
<pin name="PI1"/>
<pin name="PI2"/>
<pin name="PI3"/>
<pin name="VSS_11" direction="pwr"/>
<pin name="VDD_11" direction="pwr"/>
<pin name="PA14"/>
<pin name="PA15"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD2"/>
<pin name="PD3"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="VSS_12" direction="pwr"/>
<pin name="VDD_12" direction="pwr"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PG9"/>
<pin name="PG10"/>
<pin name="PG11"/>
<pin name="PG12"/>
<pin name="PG13"/>
<pin name="PG14"/>
<pin name="VSS_13" direction="pwr"/>
<pin name="VDD_13" direction="pwr"/>
<pin name="PG15"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="BOOT_0"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PE0"/>
<pin name="PE1"/>
<pin name="PDR_ON"/>
<pin name="VDD_14" direction="pwr"/>
<pin name="PI4"/>
<pin name="PI5"/>
<pin name="PI6"/>
<pin name="PI7"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="STM32F407_LQFP176" prefix="IC_">
<description>STM32F407 in LQFP176 Package, 176 Pin
Microcontroller (MCU) ARM Cortex M4 1024kB FLASH 168 Mhz 192kB SRAM</description>
<gates>
<gate name="G$1" symbol="STM32F407_LQFP176_RL"/>
</gates>
<devices>
<device name="" package="STM32F407_LQFP176">
<connects>
<connect gate="G$1" pin="BOOT_0" pad="P$166"/>
<connect gate="G$1" pin="NRST" pad="P$31"/>
<connect gate="G$1" pin="PA0/WKUP" pad="P$40"/>
<connect gate="G$1" pin="PA1" pad="P$41"/>
<connect gate="G$1" pin="PA10" pad="P$121"/>
<connect gate="G$1" pin="PA11" pad="P$122"/>
<connect gate="G$1" pin="PA12" pad="P$123"/>
<connect gate="G$1" pin="PA13" pad="P$124"/>
<connect gate="G$1" pin="PA14" pad="P$137"/>
<connect gate="G$1" pin="PA15" pad="P$138"/>
<connect gate="G$1" pin="PA2" pad="P$42"/>
<connect gate="G$1" pin="PA3" pad="P$47"/>
<connect gate="G$1" pin="PA4" pad="P$50"/>
<connect gate="G$1" pin="PA5" pad="P$51"/>
<connect gate="G$1" pin="PA6" pad="P$52"/>
<connect gate="G$1" pin="PA7" pad="P$53"/>
<connect gate="G$1" pin="PA8" pad="P$119"/>
<connect gate="G$1" pin="PA9" pad="P$120"/>
<connect gate="G$1" pin="PB0" pad="P$56"/>
<connect gate="G$1" pin="PB1" pad="P$57"/>
<connect gate="G$1" pin="PB10" pad="P$79"/>
<connect gate="G$1" pin="PB11" pad="P$80"/>
<connect gate="G$1" pin="PB12" pad="P$92"/>
<connect gate="G$1" pin="PB13" pad="P$93"/>
<connect gate="G$1" pin="PB14" pad="P$94"/>
<connect gate="G$1" pin="PB15" pad="P$95"/>
<connect gate="G$1" pin="PB2/BOOT_1" pad="P$58"/>
<connect gate="G$1" pin="PB3" pad="P$161"/>
<connect gate="G$1" pin="PB4" pad="P$162"/>
<connect gate="G$1" pin="PB5" pad="P$163"/>
<connect gate="G$1" pin="PB6" pad="P$164"/>
<connect gate="G$1" pin="PB7" pad="P$165"/>
<connect gate="G$1" pin="PB8" pad="P$167"/>
<connect gate="G$1" pin="PB9" pad="P$168"/>
<connect gate="G$1" pin="PC0" pad="P$32"/>
<connect gate="G$1" pin="PC1" pad="P$33"/>
<connect gate="G$1" pin="PC10" pad="P$139"/>
<connect gate="G$1" pin="PC11" pad="P$140"/>
<connect gate="G$1" pin="PC12" pad="P$141"/>
<connect gate="G$1" pin="PC13" pad="P$8"/>
<connect gate="G$1" pin="PC14/OSC32_IN" pad="P$9"/>
<connect gate="G$1" pin="PC15/OSC32_OUT" pad="P$10"/>
<connect gate="G$1" pin="PC2" pad="P$34"/>
<connect gate="G$1" pin="PC3" pad="P$35"/>
<connect gate="G$1" pin="PC4" pad="P$54"/>
<connect gate="G$1" pin="PC5" pad="P$55"/>
<connect gate="G$1" pin="PC6" pad="P$115"/>
<connect gate="G$1" pin="PC7" pad="P$116"/>
<connect gate="G$1" pin="PC8" pad="P$117"/>
<connect gate="G$1" pin="PC9" pad="P$118"/>
<connect gate="G$1" pin="PD0" pad="P$142"/>
<connect gate="G$1" pin="PD1" pad="P$143"/>
<connect gate="G$1" pin="PD10" pad="P$98"/>
<connect gate="G$1" pin="PD11" pad="P$99"/>
<connect gate="G$1" pin="PD12" pad="P$100"/>
<connect gate="G$1" pin="PD13" pad="P$101"/>
<connect gate="G$1" pin="PD14" pad="P$104"/>
<connect gate="G$1" pin="PD15" pad="P$105"/>
<connect gate="G$1" pin="PD2" pad="P$144"/>
<connect gate="G$1" pin="PD3" pad="P$145"/>
<connect gate="G$1" pin="PD4" pad="P$146"/>
<connect gate="G$1" pin="PD5" pad="P$147"/>
<connect gate="G$1" pin="PD6" pad="P$150"/>
<connect gate="G$1" pin="PD7" pad="P$151"/>
<connect gate="G$1" pin="PD8" pad="P$96"/>
<connect gate="G$1" pin="PD9" pad="P$97"/>
<connect gate="G$1" pin="PDR_ON" pad="P$171"/>
<connect gate="G$1" pin="PE0" pad="P$169"/>
<connect gate="G$1" pin="PE1" pad="P$170"/>
<connect gate="G$1" pin="PE10" pad="P$73"/>
<connect gate="G$1" pin="PE11" pad="P$74"/>
<connect gate="G$1" pin="PE12" pad="P$75"/>
<connect gate="G$1" pin="PE13" pad="P$76"/>
<connect gate="G$1" pin="PE14" pad="P$77"/>
<connect gate="G$1" pin="PE15" pad="P$78"/>
<connect gate="G$1" pin="PE2" pad="P$1"/>
<connect gate="G$1" pin="PE3" pad="P$2"/>
<connect gate="G$1" pin="PE4" pad="P$3"/>
<connect gate="G$1" pin="PE5" pad="P$4"/>
<connect gate="G$1" pin="PE6" pad="P$5"/>
<connect gate="G$1" pin="PE7" pad="P$68"/>
<connect gate="G$1" pin="PE8" pad="P$69"/>
<connect gate="G$1" pin="PE9" pad="P$70"/>
<connect gate="G$1" pin="PF0" pad="P$16"/>
<connect gate="G$1" pin="PF1" pad="P$17"/>
<connect gate="G$1" pin="PF10" pad="P$28"/>
<connect gate="G$1" pin="PF11" pad="P$59"/>
<connect gate="G$1" pin="PF12" pad="P$60"/>
<connect gate="G$1" pin="PF13" pad="P$63"/>
<connect gate="G$1" pin="PF14" pad="P$64"/>
<connect gate="G$1" pin="PF15" pad="P$65"/>
<connect gate="G$1" pin="PF2" pad="P$18"/>
<connect gate="G$1" pin="PF3" pad="P$19"/>
<connect gate="G$1" pin="PF4" pad="P$20"/>
<connect gate="G$1" pin="PF5" pad="P$21"/>
<connect gate="G$1" pin="PF6" pad="P$24"/>
<connect gate="G$1" pin="PF7" pad="P$25"/>
<connect gate="G$1" pin="PF8" pad="P$26"/>
<connect gate="G$1" pin="PF9" pad="P$27"/>
<connect gate="G$1" pin="PG0" pad="P$66"/>
<connect gate="G$1" pin="PG1" pad="P$67"/>
<connect gate="G$1" pin="PG10" pad="P$153"/>
<connect gate="G$1" pin="PG11" pad="P$154"/>
<connect gate="G$1" pin="PG12" pad="P$155"/>
<connect gate="G$1" pin="PG13" pad="P$156"/>
<connect gate="G$1" pin="PG14" pad="P$157"/>
<connect gate="G$1" pin="PG15" pad="P$160"/>
<connect gate="G$1" pin="PG2" pad="P$106"/>
<connect gate="G$1" pin="PG3" pad="P$107"/>
<connect gate="G$1" pin="PG4" pad="P$108"/>
<connect gate="G$1" pin="PG5" pad="P$109"/>
<connect gate="G$1" pin="PG6" pad="P$110"/>
<connect gate="G$1" pin="PG7" pad="P$111"/>
<connect gate="G$1" pin="PG8" pad="P$112"/>
<connect gate="G$1" pin="PG9" pad="P$152"/>
<connect gate="G$1" pin="PH0/OSC_IN" pad="P$29"/>
<connect gate="G$1" pin="PH1/OSC_OUT" pad="P$30"/>
<connect gate="G$1" pin="PH10" pad="P$87"/>
<connect gate="G$1" pin="PH11" pad="P$88"/>
<connect gate="G$1" pin="PH12" pad="P$89"/>
<connect gate="G$1" pin="PH13" pad="P$128"/>
<connect gate="G$1" pin="PH14" pad="P$129"/>
<connect gate="G$1" pin="PH15" pad="P$130"/>
<connect gate="G$1" pin="PH2" pad="P$43"/>
<connect gate="G$1" pin="PH3" pad="P$44"/>
<connect gate="G$1" pin="PH4" pad="P$45"/>
<connect gate="G$1" pin="PH5" pad="P$46"/>
<connect gate="G$1" pin="PH6" pad="P$83"/>
<connect gate="G$1" pin="PH7" pad="P$84"/>
<connect gate="G$1" pin="PH8" pad="P$85"/>
<connect gate="G$1" pin="PH9" pad="P$86"/>
<connect gate="G$1" pin="PI0" pad="P$131"/>
<connect gate="G$1" pin="PI1" pad="P$132"/>
<connect gate="G$1" pin="PI10" pad="P$12"/>
<connect gate="G$1" pin="PI11" pad="P$13"/>
<connect gate="G$1" pin="PI2" pad="P$133"/>
<connect gate="G$1" pin="PI3" pad="P$134"/>
<connect gate="G$1" pin="PI4" pad="P$173"/>
<connect gate="G$1" pin="PI5" pad="P$174"/>
<connect gate="G$1" pin="PI6" pad="P$175"/>
<connect gate="G$1" pin="PI7" pad="P$176"/>
<connect gate="G$1" pin="PI8" pad="P$7"/>
<connect gate="G$1" pin="PI9" pad="P$11"/>
<connect gate="G$1" pin="VBAT" pad="P$6"/>
<connect gate="G$1" pin="VCAP_1" pad="P$81"/>
<connect gate="G$1" pin="VCAP_2" pad="P$125"/>
<connect gate="G$1" pin="VDD" pad="P$15"/>
<connect gate="G$1" pin="VDDA" pad="P$39"/>
<connect gate="G$1" pin="VDD_1" pad="P$23"/>
<connect gate="G$1" pin="VDD_10" pad="P$127"/>
<connect gate="G$1" pin="VDD_11" pad="P$136"/>
<connect gate="G$1" pin="VDD_12" pad="P$149"/>
<connect gate="G$1" pin="VDD_13" pad="P$159"/>
<connect gate="G$1" pin="VDD_14" pad="P$172"/>
<connect gate="G$1" pin="VDD_2" pad="P$36"/>
<connect gate="G$1" pin="VDD_3" pad="P$49"/>
<connect gate="G$1" pin="VDD_4" pad="P$62"/>
<connect gate="G$1" pin="VDD_5" pad="P$72"/>
<connect gate="G$1" pin="VDD_6" pad="P$82"/>
<connect gate="G$1" pin="VDD_7" pad="P$91"/>
<connect gate="G$1" pin="VDD_8" pad="P$103"/>
<connect gate="G$1" pin="VDD_9" pad="P$114"/>
<connect gate="G$1" pin="VREF+" pad="P$38"/>
<connect gate="G$1" pin="VSS" pad="P$14"/>
<connect gate="G$1" pin="VSSA" pad="P$37"/>
<connect gate="G$1" pin="VSS_1" pad="P$22"/>
<connect gate="G$1" pin="VSS_10" pad="P$126"/>
<connect gate="G$1" pin="VSS_11" pad="P$135"/>
<connect gate="G$1" pin="VSS_12" pad="P$148"/>
<connect gate="G$1" pin="VSS_13" pad="P$158"/>
<connect gate="G$1" pin="VSS_4" pad="P$48"/>
<connect gate="G$1" pin="VSS_5" pad="P$61"/>
<connect gate="G$1" pin="VSS_6" pad="P$71"/>
<connect gate="G$1" pin="VSS_7" pad="P$90"/>
<connect gate="G$1" pin="VSS_8" pad="P$102"/>
<connect gate="G$1" pin="VSS_9" pad="P$113"/>
</connects>
<technologies>
<technology name="LQFP"/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
