| Kinetis SDK Demo Applications User Guide 1.0.0-beta Freescale Semiconductor, Inc.

- Main Page
- Related Pages
- Demos

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Flextimer PWM Introduction
Flextimer PWM Demo

Introduction and the function/configuration of Flextimer PWM. More...

### FTM PWM Introduction

# Overview

This application demonstrates the FTM edge-aligned PWM function.This application uses one TWR-K64F120M board.For TWR-K64F120M board: Output PWM from FTM3 Channel 1, which is connected to PTE6 (LED D5 on board). The LED D5 on TWR-K64F120M board increases/decreases lightness according to PWM pulse width changes.For FRDM-K64F120M board: Output PWM from FTM0 Channel 0 on PTC1, PTC1 (J1 Pin5) is connected by external wire with PTE26 (J2 Pin1 LED Green). The LED Green on FRDM-K64F120M board increases/decreases lightness according to PWM pulse width changes.

# Supported platforms

Currently, the ftm_pwm project is supported on the following platforms:

- TWR-K64F120M
- FRDM-K64F120M