| Kinetis SDK Demo Applications User Guide 1.0.0-beta Freescale Semiconductor, Inc.

- Main Page
- Related Pages
- Demos

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Watchdog Timer Demo Introduction
Watchdog Timer Demo

Introduction of the Watchdog Timer demo application. More...

### Watchdog Timer Demo Introduction

# Overview

The watchdog demo application demonstrates how the watchdog signals interrupt and reset. The overflow time for a watchdog timer is approximately 2 seconds.

# Supported platforms

Currently, the watchdog demo is supported on the following platforms:

- TWR-K64F120M
- FRDM-K64F120M

# Serial terminal configuration

The serial terminal is configured for the following settings:

- 115200
- 8 data bits
- No parity
- 1 stop bit