| Kinetis SDK Demo Applications User Guide 1.0.0-beta Freescale Semiconductor, Inc.

- Main Page
- Related Pages
- Demos

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
low_power_adc.h
Go to the documentation of this file.
1 /*******************************************************************************
2 * Copyright (c) 2013 - 2014, Freescale Semiconductor, Inc. *
3 * All rights reserved. *
4 * *
5 * Redistribution and use in source and binary forms, with or without modifi- *
6 * cation, are permitted provided that the following conditions are met: *
7 * *
8 * o Redistributions of source code must retain the above copyright notice, *
9 * this list of conditions and the following disclaimer. *
10 * *
11 * o Redistributions in binary form must reproduce the above copyright notice, *
12 * this list of conditions and the following disclaimer in the documentation *
13 * and/or other materials provided with the distribution. *
14 * *
15 * o Neither the name of Freescale Semiconductor, Inc. nor the names of its *
16 * contributors may be used to endorse or promote products derived from this *
17 * software without specific prior written permission. *
18 * *
19 * THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS" *
20 * AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE *
21 * IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE *
22 * ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT HOLDER OR CONTRIBUTORS BE *
23 * LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR *
24 * CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF *
25 * SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS *
26 * INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN *
27 * CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) *
28 * ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE *
29 * POSSIBILITY OF SUCH DAMAGE. *
30 * *
31 *******************************************************************************/
32
33
34 #ifndef __LOWPOWER_ADC_H__
35 #define __LOWPOWER_ADC_H__
36
37 #include <stdint.h>
38
39
43 typedef struct lowPowerAdcBoundaries
44 {
45 uint32_t upperBoundary;
46 uint32_t lowerBoundary;
47 } lowPowerAdcBoundaries_t;
48
49
53 void init_hardware(void);
54
58 void LowPowerTimerIRQHandler(void);
59
63 void ADC1IRQHandler(void);
64
68 void InitLowPowerTmr(void);
69
75 uint32_t GetCurrentTempValue(void);
76
86 lowPowerAdcBoundaries_t TempSensorCalibration(uint32_t updateBoundariesCounter,
87 uint32_t *tempArray);
88
89 #endif /* __LOWPOWER_ADC_H__ */
90
91 /*******************************************************************************
92 * EOF
93 *******************************************************************************/
LowPowerTimerIRQHandler
void LowPowerTimerIRQHandler(void)
Low Power Timer Interrupt handler. Clear LPT Compare flag.
Definition: low_power_adc.c:102
lowPowerAdcBoundaries_t::lowerBoundary
uint32_t lowerBoundary
Definition: low_power_adc.h:46
init_hardware
static void init_hardware(void)
Init hardware for TWR-K70F120M.
Definition: flexcan_demo/src/main.c:95
lowPowerAdcBoundaries_t::upperBoundary
uint32_t upperBoundary
Definition: low_power_adc.h:45
ADC1IRQHandler
void ADC1IRQHandler(void)
ADC Interrupt handler. Get current ADC value and set conversionCompleted flag.
Definition: low_power_adc.c:133
InitLowPowerTmr
void InitLowPowerTmr(void)
Initialize Low Power Timer. Use 1 kHz LPO with no preescaler and enable LPT interrupt.
Definition: low_power_adc.c:108
lowPowerAdcBoundaries_t
Boundaries struct.
Definition: low_power_adc.h:43
GetCurrentTempValue
uint32_t GetCurrentTempValue(void)
Calculate current temperature.
Definition: low_power_adc.c:142
TempSensorCalibration
lowPowerAdcBoundaries_t TempSensorCalibration(uint32_t updateBoundariesCounter, uint32_t *tempArray)
Calculate current temperature.
Definition: low_power_adc.c:150