| Kinetis SDK Demo Applications User Guide 1.0.0-beta Freescale Semiconductor, Inc.

- Main Page
- Related Pages
- Demos

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
gpio_uart.h
Go to the documentation of this file.
1 /*
2 * Copyright (c) 2013 - 2014, Freescale Semiconductor, Inc.
3 * All rights reserved.
4 *
5 * Redistribution and use in source and binary forms, with or without modification,
6 * are permitted provided that the following conditions are met:
7 *
8 * o Redistributions of source code must retain the above copyright notice, this list
9 * of conditions and the following disclaimer.
10 *
11 * o Redistributions in binary form must reproduce the above copyright notice, this
12 * list of conditions and the following disclaimer in the documentation and/or
13 * other materials provided with the distribution.
14 *
15 * o Neither the name of Freescale Semiconductor, Inc. nor the names of its
16 * contributors may be used to endorse or promote products derived from this
17 * software without specific prior written permission.
18 *
19 * THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS" AND
20 * ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED
21 * WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE
22 * DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT HOLDER OR CONTRIBUTORS BE LIABLE FOR
23 * ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES
24 * (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES;
25 * LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON
26 * ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT
27 * (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS
28 * SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
29 */
30
31 #ifndef _GPIO_UART_H_
32 #define _GPIO_UART_H_
33
34 /*******************************************************************************
35 * Definitions
36 ******************************************************************************/
37
38 #if (defined(CPU_MK70FN1M0VMJ12))
39
40 #define UART_RX_INSTANCE HW_PORTE
41 #define UART_RX_PIN_NUM 17
42 #define UART_TX_INSTANCE HW_PORTE
43 #define UART_TX_PIN_NUM 16
44
45 #elif ((defined(twrk22f120m)) || (defined(frdmk22f120m)))
46
47 #define UART_RX_INSTANCE HW_PORTE
48 #define UART_RX_PIN_NUM 1
49 #define UART_TX_INSTANCE HW_PORTE
50 #define UART_TX_PIN_NUM 0
51
52 #elif (defined(twrk64f120m))
53
54 #define UART_RX_INSTANCE HW_PORTC
55 #define UART_RX_PIN_NUM 3
56 #define UART_TX_INSTANCE HW_PORTC
57 #define UART_TX_PIN_NUM 4
58
59 #elif (defined(frdmk64f120m))
60
61 #define UART_RX_INSTANCE HW_PORTB
62 #define UART_RX_PIN_NUM 16
63 #define UART_TX_INSTANCE HW_PORTB
64 #define UART_TX_PIN_NUM 17
65
66 #else
67 #error No valid platform defined.
68 #endif
69
70 #endif /* END _GPIO_UART_H_ */