<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.0.0">
<drawing>
<library>
<packages>
<package name="TSSOP28">
<description>&lt;b&gt;Thin Shrink Small Outline Plastic 28&lt;/b&gt;&lt;p&gt;
MAX3223-MAX3243.pdf</description>
</package>
</packages>
<symbols>
<symbol name="PCF8885">
<pin name="VDD" direction="pwr"/>
<pin name="IN0"/>
<pin name="!INT_IN" direction="in"/>
<pin name="CLK_IN" direction="in"/>
<pin name="IN5"/>
<pin name="IN3"/>
<pin name="CPC0"/>
<pin name="CPC1"/>
<pin name="CPC2"/>
<pin name="CPC3"/>
<pin name="CPC4"/>
<pin name="CPC5"/>
<pin name="CPC6"/>
<pin name="CPC7"/>
<pin name="CLK_OUT" direction="out"/>
<pin name="!INT" direction="out"/>
<pin name="A0" direction="in"/>
<pin name="IN1"/>
<pin name="VSS" direction="pwr"/>
<pin name="SCL" direction="in"/>
<pin name="SLEEP" direction="in"/>
<pin name="SDA"/>
<pin name="IN2"/>
<pin name="VDD_INTREGD" direction="pwr"/>
<pin name="IN6"/>
<pin name="IN7"/>
<pin name="IN4"/>
<pin name="TEST" direction="in"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="PCF8885" prefix="IC">
<description>&lt;b&gt;Capacitive 8-channel touch
and proximity sensor&lt;/b&gt;&lt;p&gt;
Capacitive 8-channel touch
and proximity sensor with
auto-calibration and very
low power consumption</description>
<gates>
<gate name="G$1" symbol="PCF8885"/>
</gates>
<devices>
<device name="TS" package="TSSOP28">
<connects>
<connect gate="G$1" pin="!INT" pad="25"/>
<connect gate="G$1" pin="!INT_IN" pad="27"/>
<connect gate="G$1" pin="A0" pad="23"/>
<connect gate="G$1" pin="CLK_IN" pad="28"/>
<connect gate="G$1" pin="CLK_OUT" pad="1"/>
<connect gate="G$1" pin="CPC0" pad="18"/>
<connect gate="G$1" pin="CPC1" pad="17"/>
<connect gate="G$1" pin="CPC2" pad="16"/>
<connect gate="G$1" pin="CPC3" pad="15"/>
<connect gate="G$1" pin="CPC4" pad="14"/>
<connect gate="G$1" pin="CPC5" pad="13"/>
<connect gate="G$1" pin="CPC6" pad="12"/>
<connect gate="G$1" pin="CPC7" pad="11"/>
<connect gate="G$1" pin="IN0" pad="10"/>
<connect gate="G$1" pin="IN1" pad="9"/>
<connect gate="G$1" pin="IN2" pad="8"/>
<connect gate="G$1" pin="IN3" pad="7"/>
<connect gate="G$1" pin="IN4" pad="6"/>
<connect gate="G$1" pin="IN5" pad="5"/>
<connect gate="G$1" pin="IN6" pad="4"/>
<connect gate="G$1" pin="IN7" pad="3"/>
<connect gate="G$1" pin="SCL" pad="20"/>
<connect gate="G$1" pin="SDA" pad="21"/>
<connect gate="G$1" pin="SLEEP" pad="24"/>
<connect gate="G$1" pin="TEST" pad="22"/>
<connect gate="G$1" pin="VDD" pad="26"/>
<connect gate="G$1" pin="VDD_INTREGD" pad="2"/>
<connect gate="G$1" pin="VSS" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
