{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Kalkulation"],"not_rendered":{"charts":0,"images":7,"macros":1,"external_links":0,"defined_names":16,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Kalkulation","index":0,"n_rows":20,"n_cols":12,"rows_kept":20,"cut":false,"hidden":false,"merged":[[14,3,15,3],[14,4,15,4],[15,6,16,6],[3,10,4,10],[3,11,4,11],[5,10,6,10],[5,11,6,11]]}
[]
[null,null,null,"CPU Freq.  (in MHz)",8,null,"CTC  Wert",249,null,"Gewünschte Zeit      ( in us)","Prescaler (8 bit)","CTC Wert"]
[null,null,null,null,null,null,null,null,null,9999999]
[null,"Prescaler",null,"Zeit in us","Zeit in ms",null,"Zeit in us","Zeit in ms",null,null,"Prescaler (16 bit)","CTC Wert"]
[null,1,1,{"$f":"1/(E$2/$B5)","v":0.125},{"$f":"IF(D5>0,D5/1000,\"\")","v":1.25E-4},null,{"$f":"IF(D5>0,D5*($H$2+1),\"\")","v":31.25},{"$f":"IFERROR(IF(G5>0,G5/1000),\"\")","v":3.125E-2}]
[null,8,1,{"$f":"1/(E$2/$B6)","v":1},{"$f":"IF(D6>0,D6/1000,\"\")","v":1E-3},null,{"$f":"IF(D6>0,D6*($H$2+1),\"\")","v":250},0.25]
[null,32,0,null,"",null,"",""]
[null,64,1,{"$f":"1/(E$2/$B8)","v":8},8.0000000000000002E-3,null,2000,2]
[null,128,0,null,"",null,"",""]
[null,256,1,{"$f":"1/(E$2/$B10)","v":32},3.2000000000000001E-2,null,8000,8]
[null,1024,1,{"$f":"1/(E$2/$B11)","v":128},0.128,null,32000,32]
[]
[]
[]
[null,null,null,"Gewünschte Baudrate",10400]
[null,null,null,null,null,null,"Synchronous Master Mode"]
[null,null,null,"Register","U2Xn=0","U2Xn=1"]
[null,null,null,"UBRRH",0,0,1]
[null,null,null,"UBRRL",47,95,128]
[null,null,null,"Fehler",1.6339869281046804E-3,1.6168148746968924E-3,-1.0025501251220703E-3]