<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="15" x2="0" y2="35" width="0" layer="20"/>
<wire x1="0" y1="35" x2="15" y2="49.5" width="0" layer="20"/>
<wire x1="15" y1="49.5" x2="20" y2="49.5" width="0" layer="20"/>
<wire x1="20" y1="49.5" x2="25" y2="46" width="0" layer="20" curve="90"/>
<wire x1="25" y1="46" x2="30" y2="49.5" width="0" layer="20" curve="90"/>
<wire x1="30" y1="49.5" x2="35" y2="49.5" width="0" layer="20"/>
<wire x1="35" y1="49.5" x2="50" y2="35" width="0" layer="20"/>
<wire x1="50" y1="35" x2="50" y2="15" width="0" layer="20"/>
<wire x1="50" y1="15" x2="35" y2="0.5" width="0" layer="20"/>
<wire x1="35" y1="0.5" x2="15" y2="0.5" width="0" layer="20"/>
<wire x1="15" y1="0.5" x2="0" y2="15" width="0" layer="20"/>
<hole x="14.51" y="10.8" drill="3.2"/>
<hole x="40.15" y="40.15" drill="3.2"/>
<text>PB6</text>
<text>PB7</text>
<text>PB8</text>
<text>PB0</text>
<text>PB1</text>
<text>PB2</text>
<text>PB3</text>
<text>PB4</text>
<text>PB5</text>
<text>PB14</text>
<text>PB15</text>
<text>PB13</text>
<text>PB12</text>
<text>PB11</text>
<text>PB10</text>
<text>PB9</text>
<text>PC14</text>
<text>PC15</text>
<text>SCL2</text>
<text>SDA2</text>
<text>SCL1</text>
<text>-</text>
<text>+</text>
<text>+</text>
<text>-</text>
<text>+</text>
<text>+</text>
<text>SDA1</text>
<text>-</text>
<text>+</text>
<text>+</text>
<text>GND</text>
<text>RSense</text>
<text>RSense</text>
<text>RSense</text>
<text>RSENSE
0.1=1A
0.13=0.76A
0.15=.667A
.3=.333A</text>
<text>Hausbus
HighPowerLED</text>
<text>rev20150622</text>
<text>-</text>
<text>+</text>
<text>+</text>
<text>GND</text>
<text>LED1 - PB3
LED2 - PB0
LED3 - PB1
LED4 - PB4</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X09_LOCK">
</package>
<package name="1X02_LOCK">
</package>
</packages>
</library>
<library name="hausbus">
<packages>
<package name="TSOT23-5">
<description>&lt;b&gt;TSOT23-5&lt;/b&gt; Thin SOT23 (0.9mm)</description>
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TO-92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="INDUCTOR-1206">
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SMB">
<description>&lt;B&gt;DIODE&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="SparkFun-Connectors" package="1X09_LOCK" value="M09LOCK"/>
<element name="JP2" library="SparkFun-Connectors" package="1X09_LOCK" value="M09LOCK"/>
<element name="JP3" library="SparkFun-Connectors" package="1X09_LOCK" value="M09LOCK"/>
<element name="JP4" library="SparkFun-Connectors" package="1X09_LOCK" value="M09LOCK"/>
<element name="IC2" library="hausbus" package="TSOT23-5" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="SparkFun-Connectors" package="1X02_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="SparkFun-DiscreteSemi" package="TO-92" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0805" value="2.2k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="SparkFun-Passives" package="INDUCTOR-1206" value="47uH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RSENSE1" library="SparkFun-Resistors" package="0805" value="0.3"/>
<element name="D1" library="diode" package="SMB" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0805" value="4.7uF X5R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="hausbus" package="TSOT23-5" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="SparkFun-Connectors" package="1X02_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="SparkFun-DiscreteSemi" package="TO-92" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0805" value="2.2k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L2" library="SparkFun-Passives" package="INDUCTOR-1206" value="47uH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RSENSE2" library="SparkFun-Resistors" package="0805" value="0.3"/>
<element name="D2" library="diode" package="SMB" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0805" value="4.7uF X5R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC3" library="hausbus" package="TSOT23-5" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED3" library="SparkFun-Connectors" package="1X02_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q3" library="SparkFun-DiscreteSemi" package="TO-92" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0805" value="2.2k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L3" library="SparkFun-Passives" package="INDUCTOR-1206" value="47uH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RSENSE3" library="SparkFun-Resistors" package="0805" value="0.3"/>
<element name="D3" library="diode" package="SMB" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="0805" value="4.7uF X5R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="7-30V" library="SparkFun-Connectors" package="1X02_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC4" library="hausbus" package="TSOT23-5" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED4" library="SparkFun-Connectors" package="1X02_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q4" library="SparkFun-DiscreteSemi" package="TO-92" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0805" value="2.2k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L4" library="SparkFun-Passives" package="INDUCTOR-1206" value="47uH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RSENSE4" library="SparkFun-Resistors" package="0805" value="0.3"/>
<element name="D4" library="diode" package="SMB" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0805" value="4.7uF X5R">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="JP2" pad="8"/>
<contactref element="JP2" pad="3"/>
<contactref element="JP3" pad="8"/>
<contactref element="JP3" pad="5"/>
<contactref element="JP3" pad="1"/>
<contactref element="JP2" pad="9"/>
<contactref element="JP2" pad="6"/>
<contactref element="JP3" pad="6"/>
<contactref element="JP3" pad="2"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP2" pad="2"/>
<contactref element="JP2" pad="5"/>
<contactref element="JP3" pad="7"/>
<contactref element="JP3" pad="3"/>
<contactref element="JP3" pad="4"/>
<contactref element="JP3" pad="9"/>
<contactref element="JP2" pad="4"/>
<contactref element="JP2" pad="7"/>
<contactref element="C1" pad="2"/>
<contactref element="Q1" pad="1"/>
<contactref element="IC2" pad="GND"/>
<contactref element="C2" pad="2"/>
<contactref element="Q2" pad="1"/>
<contactref element="IC1" pad="GND"/>
<contactref element="C3" pad="2"/>
<contactref element="Q3" pad="1"/>
<contactref element="IC3" pad="GND"/>
<contactref element="7-30V" pad="1"/>
<contactref element="C4" pad="2"/>
<contactref element="Q4" pad="1"/>
<contactref element="IC4" pad="GND"/>
</signal>
<signal name="N$1">
<contactref element="L1" pad="P$2"/>
<contactref element="L1" pad="P$2"/>
<contactref element="IC2" pad="LX"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="PB0">
<contactref element="R3" pad="2"/>
<contactref element="JP1" pad="8"/>
</signal>
<signal name="PB1">
<contactref element="R2" pad="2"/>
<contactref element="JP1" pad="9"/>
</signal>
<signal name="PB3">
<contactref element="JP1" pad="1"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="Q1" pad="2"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="RSENSE1" pad="1"/>
<contactref element="D1" pad="C"/>
<contactref element="IC2" pad="VIN"/>
<contactref element="C1" pad="1"/>
<contactref element="RSENSE2" pad="1"/>
<contactref element="D2" pad="C"/>
<contactref element="IC1" pad="VIN"/>
<contactref element="C2" pad="1"/>
<contactref element="RSENSE3" pad="1"/>
<contactref element="D3" pad="C"/>
<contactref element="IC3" pad="VIN"/>
<contactref element="C3" pad="1"/>
<contactref element="7-30V" pad="2"/>
<contactref element="RSENSE4" pad="1"/>
<contactref element="D4" pad="C"/>
<contactref element="IC4" pad="VIN"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="RSENSE1" pad="2"/>
<contactref element="LED1" pad="1"/>
<contactref element="IC2" pad="VSENSE"/>
</signal>
<signal name="N$6">
<contactref element="LED1" pad="2"/>
<contactref element="L1" pad="P$1"/>
</signal>
<signal name="N$7">
<contactref element="IC2" pad="ADJ"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="L2" pad="P$2"/>
<contactref element="L2" pad="P$2"/>
<contactref element="IC1" pad="LX"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="N$5">
<contactref element="Q2" pad="2"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="RSENSE2" pad="2"/>
<contactref element="LED2" pad="1"/>
<contactref element="IC1" pad="VSENSE"/>
</signal>
<signal name="N$11">
<contactref element="LED2" pad="2"/>
<contactref element="L2" pad="P$1"/>
</signal>
<signal name="N$12">
<contactref element="IC1" pad="ADJ"/>
<contactref element="Q2" pad="3"/>
</signal>
<signal name="N$13">
<contactref element="L3" pad="P$2"/>
<contactref element="L3" pad="P$2"/>
<contactref element="IC3" pad="LX"/>
<contactref element="D3" pad="A"/>
</signal>
<signal name="N$14">
<contactref element="Q3" pad="2"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="RSENSE3" pad="2"/>
<contactref element="LED3" pad="1"/>
<contactref element="IC3" pad="VSENSE"/>
</signal>
<signal name="N$16">
<contactref element="LED3" pad="2"/>
<contactref element="L3" pad="P$1"/>
</signal>
<signal name="ADJ2">
<contactref element="IC3" pad="ADJ"/>
<contactref element="Q3" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="L4" pad="P$2"/>
<contactref element="L4" pad="P$2"/>
<contactref element="IC4" pad="LX"/>
<contactref element="D4" pad="A"/>
</signal>
<signal name="N$9">
<contactref element="Q4" pad="2"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="RSENSE4" pad="2"/>
<contactref element="LED4" pad="1"/>
<contactref element="IC4" pad="VSENSE"/>
</signal>
<signal name="N$19">
<contactref element="LED4" pad="2"/>
<contactref element="L4" pad="P$1"/>
</signal>
<signal name="N$20">
<contactref element="IC4" pad="ADJ"/>
<contactref element="Q4" pad="3"/>
</signal>
<signal name="PB4">
<contactref element="JP1" pad="2"/>
<contactref element="R4" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
