<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="160" y2="0" width="0" layer="20"/>
<wire x1="160" y1="0" x2="160" y2="100" width="0" layer="20"/>
<wire x1="160" y1="100" x2="0" y2="100" width="0" layer="20"/>
<wire x1="0" y1="100" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="eagle-ltspice">
<description>Default symbols for import LTspice schematics&lt;p&gt;
2012-10-29 alf@cadsoft.de&lt;br&gt;</description>
<packages>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;</description>
</package>
</packages>
</library>
<library name="micro-stm_v3">
<description>&lt;b&gt;ARM 32-bit Cortex™ MCUs&lt;/b&gt;&lt;p&gt;

&lt;author&gt;Created by jb@jenszuhause.de&lt;/author&gt;&lt;p&gt;
&lt;b&gt;You are using this libary by your own risk.&lt;/b&gt;&lt;br&gt;
&lt;b&gt;Make sure to check everything well due to this libary before using it.&lt;/b&gt;</description>
<packages>
<package name="LQFP176">
<description>&lt;b&gt;LQFP176&lt;/b&gt;&lt;p&gt;
24 x 24 mm, 176-pin low-profile quad flat package</description>
</package>
<package name="LQFP100">
<description>&lt;b&gt;LQFP100&lt;/b&gt;&lt;p&gt;
14 x 14 mm, 100-pin low-profile quad flat package</description>
</package>
</packages>
</library>
<library name="switch-omron">
<description>&lt;b&gt;Omron Switches&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="B3F-10XX">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="IS42S16320D">
<packages>
<package name="TSOP54-II">
<description>&lt;b&gt;TSOP 54&lt;/b&gt; Type II&lt;p&gt;</description>
</package>
</packages>
</library>
<library name="con-hirose">
<description>&lt;b&gt;Hirose Connectors&lt;/b&gt;&lt;p&gt;
www.hirose.co.jp&lt;p&gt;
Include : &lt;br&gt;
con-hirose-df12d(3.0)60dp0.5v80.lbr from Bob Starr &amp;lt;rtzaudio@mindspring.com&amp;gt;&lt;br&gt;
con-hirose.lbr from Bob Starr &amp;lt;rtzaudio@mindspring.com&amp;gt;&lt;br&gt;</description>
<packages>
<package name="FH12-40S-0.5SH">
<description>&lt;b&gt;0.5mm Pitch Connectors For FPC/FFC&lt;/b&gt;&lt;p&gt;
Source: &lt;a href= "http://www.hirose.co.jp/cataloge_hp/e58605370.pdf"&gt;Data sheet&lt;/a&gt;&lt;p&gt;</description>
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="JP2">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-FreqCtrl">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find crystals and oscillators and other things that go "tick".&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="HC49UP">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="IQD-Frequency-Products">
<description>&lt;b&gt;Crystals and Oscillators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by IQD Frequency Products&lt;/author&gt;</description>
<packages>
<package name="85SMX">
<description>&lt;b&gt;IQD Frequency Products SMD Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="AD7606">
<packages>
<package name="QFP50P1200X1200X160-64N">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C_C1" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C10" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C11" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C12" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C13" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C14" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C15" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C16" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C17" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C18" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C19" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C2" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C20" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C21" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C22" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C23" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C24" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C25" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C26" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C3" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C4" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C5" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C6" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C7" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C8" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C9" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_T1" library="eagle-ltspice" package="C1206" value="10µF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_T2" library="eagle-ltspice" package="C1206" value="1µF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_T3" library="eagle-ltspice" package="C1206" value="1µF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_T4" library="eagle-ltspice" package="C1206" value="2.2µF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_T5" library="eagle-ltspice" package="C1206" value="2.2µF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="IC1" library="micro-stm_v3" package="LQFP176" value="STM32F429IGT"/>
<element name="R1" library="eagle-ltspice" package="R0805" value="10k">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="R"/>
</element>
<element name="RESET_SW" library="switch-omron" package="B3F-10XX" value="">
<attribute name="OC_NEWARK" value="36M3542"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="176432"/>
<attribute name="MPN" value="B3F-1000"/>
</element>
<element name="U$1" library="IS42S16320D" package="TSOP54-II" value="IS42S16320"/>
<element name="X1" library="con-hirose" package="FH12-40S-0.5SH" value="FH12-40S-0.5SH">
<attribute name="OC_NEWARK" value="34M6178"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1324556"/>
<attribute name="MPN" value="FH12-40S-0.5SH(55)"/>
</element>
<element name="BOOT_JMP" library="jumper" package="JP2" value=""/>
<element name="Y1" library="SparkFun-FreqCtrl" package="HC49UP" value="8MHz"/>
<element name="C_C27" library="eagle-ltspice" package="C0805" value="18pF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C28" library="eagle-ltspice" package="C0805" value="18pF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="R2" library="eagle-ltspice" package="R0805" value="220">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="R"/>
</element>
<element name="X2" library="IQD-Frequency-Products" package="85SMX" value="32.768kHz"/>
<element name="C_C29" library="eagle-ltspice" package="C0805" value="12pF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C30" library="eagle-ltspice" package="C0805" value="12pF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="IC2" library="micro-stm_v3" package="LQFP100" value="STM32F407VGT"/>
<element name="Y2" library="SparkFun-FreqCtrl" package="HC49UP" value="8MHz"/>
<element name="C_C31" library="eagle-ltspice" package="C0805" value="18pF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C32" library="eagle-ltspice" package="C0805" value="18pF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="R3" library="eagle-ltspice" package="R0805" value="220">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="R"/>
</element>
<element name="C_C33" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C34" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C35" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C36" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C37" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_T6" library="eagle-ltspice" package="C1206" value="10µF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="X3" library="IQD-Frequency-Products" package="85SMX" value="32.768kHz"/>
<element name="C_C38" library="eagle-ltspice" package="C0805" value="12pF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C39" library="eagle-ltspice" package="C0805" value="12pF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_T7" library="eagle-ltspice" package="C1206" value="2.2µF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_T8" library="eagle-ltspice" package="C1206" value="2.2µF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="U1" library="AD7606" package="QFP50P1200X1200X160-64N" value="AD7606BSTZ">
<attribute name="SUPPLIER" value="Analog Devices"/>
<attribute name="OC_FARNELL" value="1864685"/>
<attribute name="PACKAGE" value="LQFP-64"/>
<attribute name="MPN" value="AD7606BSTZ"/>
<attribute name="OC_NEWARK" value="76R7614"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="C_T2" pad="2"/>
<contactref element="C_C17" pad="2"/>
<contactref element="C_T3" pad="2"/>
<contactref element="C_C18" pad="2"/>
<contactref element="C_C16" pad="2"/>
<contactref element="IC1" pad="37"/>
<contactref element="IC1" pad="48"/>
<contactref element="RESET_SW" pad="4"/>
<contactref element="C_C19" pad="2"/>
<contactref element="RESET_SW" pad="3"/>
<contactref element="C_T5" pad="2"/>
<contactref element="C_T4" pad="2"/>
<contactref element="C_C15" pad="2"/>
<contactref element="C_C14" pad="2"/>
<contactref element="C_C13" pad="2"/>
<contactref element="C_C12" pad="2"/>
<contactref element="C_C11" pad="2"/>
<contactref element="C_C10" pad="2"/>
<contactref element="C_C9" pad="2"/>
<contactref element="C_C8" pad="2"/>
<contactref element="C_C7" pad="2"/>
<contactref element="C_C6" pad="2"/>
<contactref element="C_C5" pad="2"/>
<contactref element="C_C4" pad="2"/>
<contactref element="C_C3" pad="2"/>
<contactref element="C_C2" pad="2"/>
<contactref element="C_C1" pad="2"/>
<contactref element="C_T1" pad="2"/>
<contactref element="IC1" pad="14"/>
<contactref element="IC1" pad="22"/>
<contactref element="IC1" pad="61"/>
<contactref element="IC1" pad="71"/>
<contactref element="IC1" pad="90"/>
<contactref element="IC1" pad="102"/>
<contactref element="IC1" pad="113"/>
<contactref element="IC1" pad="126"/>
<contactref element="IC1" pad="135"/>
<contactref element="IC1" pad="148"/>
<contactref element="IC1" pad="158"/>
<contactref element="U$1" pad="54"/>
<contactref element="U$1" pad="28"/>
<contactref element="U$1" pad="41"/>
<contactref element="U$1" pad="52"/>
<contactref element="U$1" pad="6"/>
<contactref element="U$1" pad="12"/>
<contactref element="U$1" pad="46"/>
<contactref element="C_C26" pad="2"/>
<contactref element="C_C25" pad="2"/>
<contactref element="C_C24" pad="2"/>
<contactref element="C_C23" pad="2"/>
<contactref element="C_C22" pad="2"/>
<contactref element="C_C21" pad="2"/>
<contactref element="C_C20" pad="2"/>
<contactref element="BOOT_JMP" pad="1"/>
<contactref element="X1" pad="3"/>
<contactref element="X1" pad="29"/>
<contactref element="X1" pad="36"/>
<contactref element="C_C28" pad="1"/>
<contactref element="C_C27" pad="1"/>
<contactref element="C_C30" pad="2"/>
<contactref element="C_C29" pad="2"/>
<contactref element="C_C32" pad="1"/>
<contactref element="C_C31" pad="1"/>
<contactref element="C_C37" pad="2"/>
<contactref element="C_C36" pad="2"/>
<contactref element="C_C35" pad="2"/>
<contactref element="C_C34" pad="2"/>
<contactref element="C_C33" pad="2"/>
<contactref element="C_T6" pad="2"/>
<contactref element="IC2" pad="10"/>
<contactref element="IC2" pad="74"/>
<contactref element="IC2" pad="99"/>
<contactref element="IC2" pad="27"/>
<contactref element="C_C39" pad="2"/>
<contactref element="C_C38" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="C_T5" pad="1"/>
<contactref element="IC1" pad="125"/>
</signal>
<signal name="N$3">
<contactref element="C_T4" pad="1"/>
<contactref element="IC1" pad="81"/>
</signal>
<signal name="N$1">
<contactref element="IC1" pad="166"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="R1" pad="1"/>
<contactref element="BOOT_JMP" pad="2"/>
</signal>
<signal name="+3V3">
<contactref element="C_C16" pad="1"/>
<contactref element="IC1" pad="6"/>
<contactref element="C_C17" pad="1"/>
<contactref element="C_T2" pad="1"/>
<contactref element="IC1" pad="39"/>
<contactref element="IC1" pad="38"/>
<contactref element="C_T3" pad="1"/>
<contactref element="C_C18" pad="1"/>
<contactref element="IC1" pad="171"/>
<contactref element="C_C15" pad="1"/>
<contactref element="C_C14" pad="1"/>
<contactref element="C_C13" pad="1"/>
<contactref element="C_C12" pad="1"/>
<contactref element="C_C11" pad="1"/>
<contactref element="C_C10" pad="1"/>
<contactref element="C_C9" pad="1"/>
<contactref element="C_C8" pad="1"/>
<contactref element="C_C7" pad="1"/>
<contactref element="C_C6" pad="1"/>
<contactref element="C_C5" pad="1"/>
<contactref element="C_C4" pad="1"/>
<contactref element="C_C3" pad="1"/>
<contactref element="C_C2" pad="1"/>
<contactref element="C_C1" pad="1"/>
<contactref element="C_T1" pad="1"/>
<contactref element="IC1" pad="36"/>
<contactref element="IC1" pad="49"/>
<contactref element="IC1" pad="82"/>
<contactref element="IC1" pad="172"/>
<contactref element="IC1" pad="15"/>
<contactref element="IC1" pad="23"/>
<contactref element="IC1" pad="62"/>
<contactref element="IC1" pad="72"/>
<contactref element="IC1" pad="91"/>
<contactref element="IC1" pad="103"/>
<contactref element="IC1" pad="114"/>
<contactref element="IC1" pad="127"/>
<contactref element="IC1" pad="136"/>
<contactref element="IC1" pad="149"/>
<contactref element="IC1" pad="159"/>
<contactref element="U$1" pad="27"/>
<contactref element="U$1" pad="1"/>
<contactref element="U$1" pad="14"/>
<contactref element="U$1" pad="3"/>
<contactref element="U$1" pad="49"/>
<contactref element="U$1" pad="43"/>
<contactref element="U$1" pad="9"/>
<contactref element="C_C23" pad="1"/>
<contactref element="C_C24" pad="1"/>
<contactref element="C_C20" pad="1"/>
<contactref element="C_C21" pad="1"/>
<contactref element="C_C22" pad="1"/>
<contactref element="C_C25" pad="1"/>
<contactref element="C_C26" pad="1"/>
<contactref element="BOOT_JMP" pad="3"/>
<contactref element="X1" pad="4"/>
<contactref element="X1" pad="31"/>
<contactref element="C_C37" pad="1"/>
<contactref element="C_C36" pad="1"/>
<contactref element="C_C35" pad="1"/>
<contactref element="C_C34" pad="1"/>
<contactref element="C_C33" pad="1"/>
<contactref element="C_T6" pad="1"/>
<contactref element="IC2" pad="28"/>
<contactref element="IC2" pad="50"/>
<contactref element="IC2" pad="19"/>
<contactref element="IC2" pad="75"/>
<contactref element="IC2" pad="100"/>
<contactref element="IC2" pad="11"/>
</signal>
<signal name="NRST_F429">
<contactref element="IC1" pad="31"/>
</signal>
<signal name="N$7">
<contactref element="RESET_SW" pad="1"/>
<contactref element="RESET_SW" pad="2"/>
<contactref element="C_C19" pad="1"/>
</signal>
<signal name="RAM1_A0">
<contactref element="IC1" pad="16"/>
<contactref element="U$1" pad="23"/>
</signal>
<signal name="RAM1_A2">
<contactref element="IC1" pad="18"/>
<contactref element="U$1" pad="25"/>
</signal>
<signal name="RAM1_A3">
<contactref element="IC1" pad="19"/>
<contactref element="U$1" pad="26"/>
</signal>
<signal name="RAM1_A4">
<contactref element="IC1" pad="20"/>
<contactref element="U$1" pad="29"/>
</signal>
<signal name="RAM1_A5">
<contactref element="IC1" pad="21"/>
<contactref element="U$1" pad="30"/>
</signal>
<signal name="RAM1_A6">
<contactref element="IC1" pad="60"/>
<contactref element="U$1" pad="31"/>
</signal>
<signal name="RAM1_A7">
<contactref element="IC1" pad="63"/>
<contactref element="U$1" pad="32"/>
</signal>
<signal name="RAM1_A8">
<contactref element="IC1" pad="64"/>
<contactref element="U$1" pad="33"/>
</signal>
<signal name="RAM1_A9">
<contactref element="IC1" pad="65"/>
<contactref element="U$1" pad="34"/>
</signal>
<signal name="RAM1_A10">
<contactref element="IC1" pad="66"/>
<contactref element="U$1" pad="22"/>
</signal>
<signal name="RAM1_A11">
<contactref element="IC1" pad="67"/>
<contactref element="U$1" pad="35"/>
</signal>
<signal name="RAM1_A12">
<contactref element="IC1" pad="106"/>
<contactref element="U$1" pad="36"/>
</signal>
<signal name="RAM1_D1">
<contactref element="IC1" pad="105"/>
<contactref element="U$1" pad="4"/>
</signal>
<signal name="RAM1_D0">
<contactref element="IC1" pad="104"/>
<contactref element="U$1" pad="2"/>
</signal>
<signal name="RAM1_D2">
<contactref element="IC1" pad="142"/>
<contactref element="U$1" pad="5"/>
</signal>
<signal name="RAM1_D3">
<contactref element="IC1" pad="143"/>
<contactref element="U$1" pad="7"/>
</signal>
<signal name="RAM1_D4">
<contactref element="IC1" pad="68"/>
<contactref element="U$1" pad="8"/>
</signal>
<signal name="RAM1_D5">
<contactref element="IC1" pad="69"/>
<contactref element="U$1" pad="10"/>
</signal>
<signal name="RAM1_D6">
<contactref element="IC1" pad="70"/>
<contactref element="U$1" pad="11"/>
</signal>
<signal name="RAM1_D7">
<contactref element="IC1" pad="73"/>
<contactref element="U$1" pad="13"/>
</signal>
<signal name="RAM1_D8">
<contactref element="IC1" pad="74"/>
<contactref element="U$1" pad="42"/>
</signal>
<signal name="RAM1_D9">
<contactref element="IC1" pad="75"/>
<contactref element="U$1" pad="44"/>
</signal>
<signal name="RAM1_D10">
<contactref element="IC1" pad="76"/>
<contactref element="U$1" pad="45"/>
</signal>
<signal name="RAM1_D11">
<contactref element="IC1" pad="77"/>
<contactref element="U$1" pad="47"/>
</signal>
<signal name="RAM1_D12">
<contactref element="IC1" pad="78"/>
<contactref element="U$1" pad="48"/>
</signal>
<signal name="RAM1_D13">
<contactref element="IC1" pad="96"/>
<contactref element="U$1" pad="50"/>
</signal>
<signal name="RAM1_D14">
<contactref element="IC1" pad="97"/>
<contactref element="U$1" pad="51"/>
</signal>
<signal name="RAM1_D15">
<contactref element="IC1" pad="98"/>
<contactref element="U$1" pad="53"/>
</signal>
<signal name="RAM1_A1">
<contactref element="IC1" pad="17"/>
<contactref element="U$1" pad="24"/>
</signal>
<signal name="RAM1_BA0">
<contactref element="IC1" pad="108"/>
<contactref element="U$1" pad="20"/>
</signal>
<signal name="RAM1_BA1">
<contactref element="IC1" pad="109"/>
<contactref element="U$1" pad="21"/>
</signal>
<signal name="RAM1_DQML">
<contactref element="IC1" pad="169"/>
<contactref element="U$1" pad="15"/>
</signal>
<signal name="RAM1_DQMH">
<contactref element="IC1" pad="170"/>
<contactref element="U$1" pad="39"/>
</signal>
<signal name="RAM1_CLK">
<contactref element="U$1" pad="38"/>
<contactref element="IC1" pad="112"/>
</signal>
<signal name="RAM1_CKE">
<contactref element="IC1" pad="84"/>
<contactref element="U$1" pad="37"/>
</signal>
<signal name="RAM1_WE">
<contactref element="IC1" pad="32"/>
<contactref element="U$1" pad="16"/>
</signal>
<signal name="RAM1_CS">
<contactref element="IC1" pad="83"/>
<contactref element="U$1" pad="19"/>
</signal>
<signal name="RAM1_RAS">
<contactref element="IC1" pad="59"/>
<contactref element="U$1" pad="18"/>
</signal>
<signal name="RAM1_CAS">
<contactref element="IC1" pad="160"/>
<contactref element="U$1" pad="17" route="any" routetag="G$1.!CAS"/>
</signal>
<signal name="TFT_LEDPWM">
<contactref element="X1" pad="1"/>
</signal>
<signal name="+5V">
<contactref element="X1" pad="2"/>
</signal>
<signal name="TFT_VSYNC">
<contactref element="X1" pad="33"/>
<contactref element="IC1" pad="11"/>
</signal>
<signal name="TFT_DE">
<contactref element="X1" pad="34"/>
<contactref element="IC1" pad="28"/>
</signal>
<signal name="TFT_R0">
<contactref element="IC1" pad="43"/>
<contactref element="X1" pad="5"/>
</signal>
<signal name="TFT_R1">
<contactref element="IC1" pad="44"/>
<contactref element="X1" pad="6"/>
</signal>
<signal name="TFT_R2">
<contactref element="X1" pad="7"/>
<contactref element="IC1" pad="139"/>
</signal>
<signal name="TFT_R3">
<contactref element="IC1" pad="86"/>
<contactref element="X1" pad="8"/>
</signal>
<signal name="TFT_R4">
<contactref element="X1" pad="9"/>
<contactref element="IC1" pad="122"/>
</signal>
<signal name="TFT_R5">
<contactref element="X1" pad="10"/>
<contactref element="IC1" pad="123"/>
</signal>
<signal name="TFT_R6">
<contactref element="IC1" pad="89"/>
<contactref element="X1" pad="11"/>
</signal>
<signal name="TFT_R7">
<contactref element="IC1" pad="110"/>
<contactref element="X1" pad="12"/>
</signal>
<signal name="TFT_G0">
<contactref element="IC1" pad="4"/>
<contactref element="X1" pad="13"/>
</signal>
<signal name="TFT_G1">
<contactref element="IC1" pad="5"/>
<contactref element="X1" pad="14"/>
</signal>
<signal name="TFT_G2">
<contactref element="IC1" pad="128"/>
<contactref element="X1" pad="15"/>
</signal>
<signal name="TFT_G3">
<contactref element="IC1" pad="129"/>
<contactref element="X1" pad="16"/>
</signal>
<signal name="TFT_G4">
<contactref element="IC1" pad="130"/>
<contactref element="X1" pad="17"/>
</signal>
<signal name="TFT_G5">
<contactref element="IC1" pad="131"/>
<contactref element="X1" pad="18"/>
</signal>
<signal name="TFT_G6">
<contactref element="IC1" pad="132"/>
<contactref element="X1" pad="19"/>
</signal>
<signal name="TFT_G7">
<contactref element="IC1" pad="133"/>
<contactref element="X1" pad="20"/>
</signal>
<signal name="TFT_B0">
<contactref element="IC1" pad="3"/>
<contactref element="X1" pad="21"/>
</signal>
<signal name="TFT_B1">
<contactref element="IC1" pad="155"/>
<contactref element="X1" pad="22"/>
</signal>
<signal name="TFT_B3">
<contactref element="IC1" pad="154"/>
<contactref element="X1" pad="24"/>
</signal>
<signal name="TFT_B2">
<contactref element="IC1" pad="150"/>
<contactref element="X1" pad="23"/>
</signal>
<signal name="TFT_B4">
<contactref element="IC1" pad="173"/>
<contactref element="X1" pad="25"/>
</signal>
<signal name="TFT_B5">
<contactref element="IC1" pad="174"/>
<contactref element="X1" pad="26"/>
</signal>
<signal name="TFT_B6">
<contactref element="IC1" pad="167"/>
<contactref element="X1" pad="27"/>
</signal>
<signal name="TFT_B7">
<contactref element="IC1" pad="168"/>
<contactref element="X1" pad="28"/>
</signal>
<signal name="TFT_CLK">
<contactref element="IC1" pad="111"/>
<contactref element="X1" pad="30"/>
</signal>
<signal name="TFT_HSYNC">
<contactref element="IC1" pad="12"/>
<contactref element="X1" pad="32"/>
</signal>
<signal name="N$5">
<contactref element="IC1" pad="30"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="IC1" pad="29"/>
<contactref element="Y1" pad="2"/>
<contactref element="C_C28" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="Y1" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="C_C27" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="IC1" pad="10"/>
<contactref element="C_C30" pad="1"/>
<contactref element="X2" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="IC1" pad="9"/>
<contactref element="C_C29" pad="1"/>
<contactref element="X2" pad="4"/>
</signal>
<signal name="VDDA">
<contactref element="IC2" pad="22"/>
</signal>
<signal name="VSSA">
<contactref element="IC2" pad="20"/>
</signal>
<signal name="VBAT">
<contactref element="IC2" pad="6"/>
</signal>
<signal name="VREF+">
<contactref element="IC2" pad="21"/>
</signal>
<signal name="VCAP1">
<contactref element="IC2" pad="49"/>
</signal>
<signal name="VCAP2">
<contactref element="IC2" pad="73"/>
</signal>
<signal name="N$11">
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="Y2" pad="2"/>
<contactref element="C_C32" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="Y2" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="C_C31" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="C_C39" pad="1"/>
<contactref element="X3" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="C_C38" pad="1"/>
<contactref element="X3" pad="4"/>
</signal>
<signal name="GND1">
<contactref element="C_T8" pad="2"/>
<contactref element="C_T7" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="C_T8" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="C_T7" pad="1"/>
</signal>
<signal name="AVCC_2">
<contactref element="U1" pad="1"/>
</signal>
<signal name="AVCC_3">
<contactref element="U1" pad="38"/>
</signal>
<signal name="AVCC_4">
<contactref element="U1" pad="37"/>
</signal>
<signal name="AVCC">
<contactref element="U1" pad="48"/>
</signal>
<signal name="VDRIVE">
<contactref element="U1" pad="23"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
