<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="156.3624" y1="67.6656" x2="156.3624" y2="99.9744" width="0" layer="20"/>
<wire x1="156.3624" y1="99.9744" x2="38.7096" y2="99.9744" width="0" layer="20"/>
<wire x1="38.7096" y1="99.9744" x2="24.384" y2="85.6488" width="0" layer="20"/>
<wire x1="24.384" y1="85.6488" x2="24.384" y2="41.148" width="0" layer="20"/>
<text>COUTX</text>
<text>COUTX</text>
<text>TOP</text>
<text>INT1</text>
<text>INT2</text>
<text>BOTTOM</text>
<text>INPUT 10-30V 10A</text>
<text>OUTPUT 20V, 5A</text>
<text>Vin</text>
<text>Vout ERROR</text>
<text>Vout</text>
<wire x1="156.3624" y1="67.6656" x2="129.8448" y2="41.148" width="0" layer="20"/>
<wire x1="129.8448" y1="41.148" x2="24.384" y2="41.148" width="0" layer="20"/>
<text>_</text>
<text>+</text>
<text>+</text>
<text>_</text>
<text>_</text>
<text>+</text>
<text>_</text>
<text>+</text>
<text>PLACEHOLDER text, source + license info</text>
</plain>
<libraries>
<library name="AcceleratedDesigns_Lib">
<packages>
<package name="SM_RADIAL_6.3BMM">
</package>
<package name="1206">
</package>
<package name="1210">
</package>
<package name="SMA">
</package>
<package name="SRP1270">
</package>
<package name="TRANS_NEXFET_Q5A">
</package>
<package name="DNH0008A">
</package>
<package name="2512">
</package>
<package name="PWP0028F_N">
</package>
</packages>
</library>
<library name="Seeed-OPL-Resistor">
<packages>
<package name="R2512">
<description>2512</description>
</package>
<package name="R0402">
</package>
<package name="R0805">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
<package name="0805">
</package>
<package name="0603-CAP">
</package>
</packages>
</library>
<library name="phoenix_spt">
<packages>
<package name="1990973">
</package>
</packages>
</library>
<library name="Littelfuse_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 25/07/2012 10:23:27</description>
<packages>
<package name="451_453">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="SML0805">
<description>&lt;b&gt;SML0805-2CW-TR (0805 PROFILE)&lt;/b&gt; COOL WHITE&lt;p&gt;
Source: http://www.ledtronics.com/ds/smd-0603/Dstr0093.pdf</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="CBULK" library="AcceleratedDesigns_Lib" package="SM_RADIAL_6.3BMM" value="68uF">
<attribute name="MANUFACTURER_PART_NUMBER" value="UUD1V680MCL1GS"/>
<attribute name="CAP" value="6.8E-5"/>
<attribute name="ESR" value="0.34"/>
<attribute name="MANUFACTURER_NAME" value="Nichicon"/>
<attribute name="IRMS" value="0.28"/>
<attribute name="VDC" value="35.0"/>
<attribute name="VENDOR" value="Nichicon"/>
<attribute name="NAME"/>
</element>
<element name="CIN" library="AcceleratedDesigns_Lib" package="1206" value="4.7uF">
<attribute name="MANUFACTURER_PART_NUMBER" value="GRM31CR71H475KA12L"/>
<attribute name="CAP" value="4.7E-6"/>
<attribute name="ESR" value="0.0"/>
<attribute name="MANUFACTURER_NAME" value="MuRata"/>
<attribute name="IRMS" value="0.0"/>
<attribute name="VDC" value="50.0"/>
<attribute name="VENDOR" value="MuRata"/>
<attribute name="NAME"/>
</element>
<element name="CIN_2" library="AcceleratedDesigns_Lib" package="1206" value="4.7uF">
<attribute name="MANUFACTURER_PART_NUMBER" value="GRM31CR71H475KA12L"/>
<attribute name="MANUFACTURER_NAME" value="MuRata"/>
<attribute name="VENDOR" value="MuRata"/>
<attribute name="VDC" value="50.0"/>
<attribute name="CAP" value="4.7E-6"/>
<attribute name="ESR" value="0.0"/>
<attribute name="IRMS" value="0.0"/>
</element>
<element name="CIN_3" library="AcceleratedDesigns_Lib" package="1206" value="4.7uF">
<attribute name="MANUFACTURER_PART_NUMBER" value="GRM31CR71H475KA12L"/>
<attribute name="CAP" value="4.7E-6"/>
<attribute name="ESR" value="0.0"/>
<attribute name="MANUFACTURER_NAME" value="MuRata"/>
<attribute name="IRMS" value="0.0"/>
<attribute name="VDC" value="50.0"/>
<attribute name="VENDOR" value="MuRata"/>
</element>
<element name="COUTX" library="AcceleratedDesigns_Lib" package="1210" value="4.7uF">
<attribute name="MANUFACTURER_PART_NUMBER" value="C3225X6S1H475K"/>
<attribute name="CAP" value="4.7E-6"/>
<attribute name="ESR" value="0.003329"/>
<attribute name="MANUFACTURER_NAME" value="TDK"/>
<attribute name="IRMS" value="0.0"/>
<attribute name="VDC" value="50.0"/>
<attribute name="VENDOR" value="TDK"/>
<attribute name="DATASHEETURL" value="http://www.tdk.co.jp/tefe02/e4573%5Fc.pdf"/>
</element>
<element name="COUTX2" library="AcceleratedDesigns_Lib" package="1210" value="4.7uF">
<attribute name="MANUFACTURER_PART_NUMBER" value="C3225X6S1H475K"/>
<attribute name="CAP" value="4.7E-6"/>
<attribute name="ESR" value="0.003329"/>
<attribute name="MANUFACTURER_NAME" value="TDK"/>
<attribute name="IRMS" value="0.0"/>
<attribute name="VDC" value="50.0"/>
<attribute name="VENDOR" value="TDK"/>
<attribute name="DATASHEETURL" value="http://www.tdk.co.jp/tefe02/e4573%5Fc.pdf"/>
</element>
<element name="COUTX2_2" library="AcceleratedDesigns_Lib" package="1210" value="4.7uF">
<attribute name="MANUFACTURER_PART_NUMBER" value="C3225X6S1H475K"/>
<attribute name="CAP" value="4.7E-6"/>
<attribute name="ESR" value="0.003329"/>
<attribute name="MANUFACTURER_NAME" value="TDK"/>
<attribute name="IRMS" value="0.0"/>
<attribute name="VDC" value="50.0"/>
<attribute name="VENDOR" value="TDK"/>
<attribute name="DATASHEETURL" value="http://www.tdk.co.jp/tefe02/e4573%5Fc.pdf"/>
</element>
<element name="COUTX2_3" library="AcceleratedDesigns_Lib" package="1210" value="4.7uF">
<attribute name="MANUFACTURER_PART_NUMBER" value="C3225X6S1H475K"/>
<attribute name="CAP" value="4.7E-6"/>
<attribute name="ESR" value="0.003329"/>
<attribute name="MANUFACTURER_NAME" value="TDK"/>
<attribute name="IRMS" value="0.0"/>
<attribute name="VDC" value="50.0"/>
<attribute name="VENDOR" value="TDK"/>
<attribute name="DATASHEETURL" value="http://www.tdk.co.jp/tefe02/e4573%5Fc.pdf"/>
</element>
<element name="COUTX2_4" library="AcceleratedDesigns_Lib" package="1210" value="4.7uF">
<attribute name="MANUFACTURER_PART_NUMBER" value="C3225X6S1H475K"/>
<attribute name="CAP" value="4.7E-6"/>
<attribute name="ESR" value="0.003329"/>
<attribute name="MANUFACTURER_NAME" value="TDK"/>
<attribute name="IRMS" value="0.0"/>
<attribute name="VDC" value="50.0"/>
<attribute name="VENDOR" value="TDK"/>
<attribute name="DATASHEETURL" value="http://www.tdk.co.jp/tefe02/e4573%5Fc.pdf"/>
</element>
<element name="COUTX2_5" library="AcceleratedDesigns_Lib" package="1210" value="4.7uF">
<attribute name="MANUFACTURER_PART_NUMBER" value="C3225X6S1H475K"/>
<attribute name="CAP" value="4.7E-6"/>
<attribute name="ESR" value="0.003329"/>
<attribute name="MANUFACTURER_NAME" value="TDK"/>
<attribute name="IRMS" value="0.0"/>
<attribute name="VDC" value="50.0"/>
<attribute name="VENDOR" value="TDK"/>
<attribute name="DATASHEETURL" value="http://www.tdk.co.jp/tefe02/e4573%5Fc.pdf"/>
</element>
<element name="COUTX3" library="AcceleratedDesigns_Lib" package="1210" value="4.7uF">
<attribute name="MANUFACTURER_PART_NUMBER" value="C3225X6S1H475K"/>
<attribute name="CAP" value="4.7E-6"/>
<attribute name="ESR" value="0.003329"/>
<attribute name="MANUFACTURER_NAME" value="TDK"/>
<attribute name="IRMS" value="0.0"/>
<attribute name="VDC" value="50.0"/>
<attribute name="VENDOR" value="TDK"/>
<attribute name="DATASHEETURL" value="http://www.tdk.co.jp/tefe02/e4573%5Fc.pdf"/>
</element>
<element name="COUTX3_2" library="AcceleratedDesigns_Lib" package="1210" value="4.7uF">
<attribute name="MANUFACTURER_PART_NUMBER" value="C3225X6S1H475K"/>
<attribute name="CAP" value="4.7E-6"/>
<attribute name="ESR" value="0.003329"/>
<attribute name="MANUFACTURER_NAME" value="TDK"/>
<attribute name="IRMS" value="0.0"/>
<attribute name="VDC" value="50.0"/>
<attribute name="VENDOR" value="TDK"/>
<attribute name="DATASHEETURL" value="http://www.tdk.co.jp/tefe02/e4573%5Fc.pdf"/>
</element>
<element name="COUTX3_3" library="AcceleratedDesigns_Lib" package="1210" value="4.7uF">
<attribute name="MANUFACTURER_PART_NUMBER" value="C3225X6S1H475K"/>
<attribute name="CAP" value="4.7E-6"/>
<attribute name="ESR" value="0.003329"/>
<attribute name="MANUFACTURER_NAME" value="TDK"/>
<attribute name="IRMS" value="0.0"/>
<attribute name="VDC" value="50.0"/>
<attribute name="VENDOR" value="TDK"/>
<attribute name="DATASHEETURL" value="http://www.tdk.co.jp/tefe02/e4573%5Fc.pdf"/>
</element>
<element name="COUTX3_4" library="AcceleratedDesigns_Lib" package="1210" value="4.7uF">
<attribute name="MANUFACTURER_PART_NUMBER" value="C3225X6S1H475K"/>
<attribute name="CAP" value="4.7E-6"/>
<attribute name="ESR" value="0.003329"/>
<attribute name="MANUFACTURER_NAME" value="TDK"/>
<attribute name="IRMS" value="0.0"/>
<attribute name="VDC" value="50.0"/>
<attribute name="VENDOR" value="TDK"/>
<attribute name="DATASHEETURL" value="http://www.tdk.co.jp/tefe02/e4573%5Fc.pdf"/>
</element>
<element name="COUTX3_5" library="AcceleratedDesigns_Lib" package="1210" value="4.7uF">
<attribute name="MANUFACTURER_PART_NUMBER" value="C3225X6S1H475K"/>
<attribute name="CAP" value="4.7E-6"/>
<attribute name="ESR" value="0.003329"/>
<attribute name="MANUFACTURER_NAME" value="TDK"/>
<attribute name="IRMS" value="0.0"/>
<attribute name="VDC" value="50.0"/>
<attribute name="VENDOR" value="TDK"/>
<attribute name="DATASHEETURL" value="http://www.tdk.co.jp/tefe02/e4573%5Fc.pdf"/>
</element>
<element name="COUTX_2" library="AcceleratedDesigns_Lib" package="1210" value="4.7uF">
<attribute name="MANUFACTURER_PART_NUMBER" value="C3225X6S1H475K"/>
<attribute name="CAP" value="4.7E-6"/>
<attribute name="ESR" value="0.003329"/>
<attribute name="MANUFACTURER_NAME" value="TDK"/>
<attribute name="IRMS" value="0.0"/>
<attribute name="VDC" value="50.0"/>
<attribute name="VENDOR" value="TDK"/>
<attribute name="DATASHEETURL" value="http://www.tdk.co.jp/tefe02/e4573%5Fc.pdf"/>
</element>
<element name="COUTX_3" library="AcceleratedDesigns_Lib" package="1210" value="4.7uF">
<attribute name="MANUFACTURER_PART_NUMBER" value="C3225X6S1H475K"/>
<attribute name="CAP" value="4.7E-6"/>
<attribute name="ESR" value="0.003329"/>
<attribute name="MANUFACTURER_NAME" value="TDK"/>
<attribute name="IRMS" value="0.0"/>
<attribute name="VDC" value="50.0"/>
<attribute name="VENDOR" value="TDK"/>
<attribute name="DATASHEETURL" value="http://www.tdk.co.jp/tefe02/e4573%5Fc.pdf"/>
</element>
<element name="COUTX_4" library="AcceleratedDesigns_Lib" package="1210" value="4.7uF">
<attribute name="MANUFACTURER_PART_NUMBER" value="C3225X6S1H475K"/>
<attribute name="CAP" value="4.7E-6"/>
<attribute name="ESR" value="0.003329"/>
<attribute name="MANUFACTURER_NAME" value="TDK"/>
<attribute name="IRMS" value="0.0"/>
<attribute name="VDC" value="50.0"/>
<attribute name="VENDOR" value="TDK"/>
<attribute name="DATASHEETURL" value="http://www.tdk.co.jp/tefe02/e4573%5Fc.pdf"/>
</element>
<element name="COUTX_5" library="AcceleratedDesigns_Lib" package="1210" value="4.7uF">
<attribute name="MANUFACTURER_PART_NUMBER" value="C3225X6S1H475K"/>
<attribute name="CAP" value="4.7E-6"/>
<attribute name="ESR" value="0.003329"/>
<attribute name="MANUFACTURER_NAME" value="TDK"/>
<attribute name="IRMS" value="0.0"/>
<attribute name="VDC" value="50.0"/>
<attribute name="VENDOR" value="TDK"/>
<attribute name="DATASHEETURL" value="http://www.tdk.co.jp/tefe02/e4573%5Fc.pdf"/>
</element>
<element name="D2" library="AcceleratedDesigns_Lib" package="SMA" value="500mV">
<attribute name="MANUFACTURER_PART_NUMBER" value="SS14-E3/61T"/>
<attribute name="MANUFACTURER_NAME" value="Vishay-Semiconductor"/>
<attribute name="IO" value="1.0"/>
<attribute name="VFATIO" value="0.5"/>
<attribute name="VRRM" value="40.0"/>
<attribute name="VENDOR" value="Vishay-Semiconductor"/>
<attribute name="DATASHEETURL" value="http://www.vishay.com/docs/88746/88746.pdf"/>
<attribute name="NAME"/>
</element>
<element name="D3" library="AcceleratedDesigns_Lib" package="SMA" value="500mV">
<attribute name="MANUFACTURER_PART_NUMBER" value="B230A-13-F"/>
<attribute name="MANUFACTURER_NAME" value="Diodes Inc."/>
<attribute name="IO" value="2.0"/>
<attribute name="VFATIO" value="0.5"/>
<attribute name="VRRM" value="30.0"/>
<attribute name="VENDOR" value="Diodes Inc."/>
<attribute name="DATASHEETURL" value="http://www.diodes.com/datasheets/ds13004.pdf"/>
<attribute name="NAME"/>
</element>
<element name="DBOOT1" library="AcceleratedDesigns_Lib" package="SMA" value="500mV">
<attribute name="MANUFACTURER_PART_NUMBER" value="SS14-E3/61T"/>
<attribute name="MANUFACTURER_NAME" value="Vishay-Semiconductor"/>
<attribute name="IO" value="1.0"/>
<attribute name="VFATIO" value="0.5"/>
<attribute name="VRRM" value="40.0"/>
<attribute name="VENDOR" value="Vishay-Semiconductor"/>
<attribute name="DATASHEETURL" value="http://www.vishay.com/docs/88746/88746.pdf"/>
<attribute name="NAME"/>
</element>
<element name="DBOOT2" library="AcceleratedDesigns_Lib" package="SMA" value="500mV">
<attribute name="MANUFACTURER_PART_NUMBER" value="SS14-E3/61T"/>
<attribute name="MANUFACTURER_NAME" value="Vishay-Semiconductor"/>
<attribute name="IO" value="1.0"/>
<attribute name="VFATIO" value="0.5"/>
<attribute name="VRRM" value="40.0"/>
<attribute name="VENDOR" value="Vishay-Semiconductor"/>
<attribute name="DATASHEETURL" value="http://www.vishay.com/docs/88746/88746.pdf"/>
<attribute name="NAME"/>
</element>
<element name="DF" library="AcceleratedDesigns_Lib" package="SMA" value="500mV">
<attribute name="MANUFACTURER_PART_NUMBER" value="SS14-E3/61T"/>
<attribute name="MANUFACTURER_NAME" value="Vishay-Semiconductor"/>
<attribute name="IO" value="1.0"/>
<attribute name="VFATIO" value="0.5"/>
<attribute name="VRRM" value="40.0"/>
<attribute name="VENDOR" value="Vishay-Semiconductor"/>
<attribute name="DATASHEETURL" value="http://www.vishay.com/docs/88746/88746.pdf"/>
<attribute name="NAME"/>
</element>
<element name="L1" library="AcceleratedDesigns_Lib" package="SRP1270" value="4.7uH">
<attribute name="IDC" value="15.0"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="SRP1270-4R7M"/>
<attribute name="MANUFACTURER_NAME" value="Bourns"/>
<attribute name="DCR" value="0.0112"/>
<attribute name="L" value="4.7E-6"/>
<attribute name="VENDOR" value="Bourns"/>
<attribute name="NAME"/>
</element>
<element name="M1" library="AcceleratedDesigns_Lib" package="TRANS_NEXFET_Q5A" value="40V">
<attribute name="MANUFACTURER_PART_NUMBER" value="CSD18504Q5A"/>
<attribute name="MANUFACTURER_NAME" value="Texas Instruments"/>
<attribute name="RDSON45" value="0.0098"/>
<attribute name="IDSMAX" value="50.0"/>
<attribute name="VDSMAX" value="40.0"/>
<attribute name="QUANTITY" value="1"/>
<attribute name="QGTYP" value="7.7"/>
<attribute name="VENDOR" value="Texas Instruments"/>
<attribute name="DATASHEETURL" value="http://www.ti.com/lit/ds/symlink/csd18504q5a.pdf"/>
<attribute name="NAME"/>
</element>
<element name="M2" library="AcceleratedDesigns_Lib" package="TRANS_NEXFET_Q5A" value="60V">
<attribute name="MANUFACTURER_PART_NUMBER" value="CSD18537NQ5A"/>
<attribute name="MANUFACTURER_NAME" value="Texas Instruments"/>
<attribute name="RDSON45" value="0.014559"/>
<attribute name="IDSMAX" value="50.0"/>
<attribute name="VDSMAX" value="60.0"/>
<attribute name="QUANTITY" value="1"/>
<attribute name="QGTYP" value="14.0"/>
<attribute name="VENDOR" value="Texas Instruments"/>
<attribute name="DATASHEETURL" value="http://www.ti.com/lit/ds/symlink/csd18537nq5a.pdf"/>
<attribute name="NAME"/>
</element>
<element name="M3" library="AcceleratedDesigns_Lib" package="DNH0008A" value="30V">
<attribute name="MANUFACTURER_PART_NUMBER" value="CSD17551Q3A"/>
<attribute name="MANUFACTURER_NAME" value="Texas Instruments"/>
<attribute name="RDSON45" value="0.0118"/>
<attribute name="IDSMAX" value="48.0"/>
<attribute name="VDSMAX" value="30.0"/>
<attribute name="QUANTITY" value="1"/>
<attribute name="QGTYP" value="6.0"/>
<attribute name="VENDOR" value="Texas Instruments"/>
<attribute name="DATASHEETURL" value="http://www.ti.com/lit/ds/symlink/csd17551q3a.pdf"/>
<attribute name="NAME"/>
</element>
<element name="M4" library="AcceleratedDesigns_Lib" package="TRANS_NEXFET_Q5A" value="CSD18504Q5A">
<attribute name="MANUFACTURER_PART_NUMBER" value="CSD18504Q5A"/>
<attribute name="MANUFACTURER_NAME" value="Texas Instruments"/>
<attribute name="RDSON45" value="0.0098"/>
<attribute name="IDSMAX" value="50.0"/>
<attribute name="VDSMAX" value="40.0"/>
<attribute name="QUANTITY" value="1"/>
<attribute name="QGTYP" value="7.7"/>
<attribute name="VENDOR" value="Texas Instruments"/>
<attribute name="DATASHEETURL" value="http://www.ti.com/lit/ds/symlink/csd18504q5a.pdf"/>
<attribute name="NAME"/>
</element>
<element name="RCOMP" library="SparkFun-Resistors" package="0603-RES" value="7.32k">
<attribute name="NAME"/>
</element>
<element name="RCSG" library="SparkFun-Resistors" package="0603-RES" value="100">
<attribute name="NAME"/>
</element>
<element name="RCSP" library="SparkFun-Resistors" package="0603-RES" value="100">
<attribute name="NAME"/>
</element>
<element name="RF" library="SparkFun-Resistors" package="0603-RES" value="10">
<attribute name="NAME"/>
</element>
<element name="RFBB" library="SparkFun-Resistors" package="0603-RES" value="20k">
<attribute name="NAME"/>
</element>
<element name="RFBT" library="SparkFun-Resistors" package="0603-RES" value="475k">
<attribute name="NAME"/>
</element>
<element name="RMODE" library="SparkFun-Resistors" package="0603-RES" value="93.1k">
<attribute name="NAME"/>
</element>
<element name="RSENSE" library="AcceleratedDesigns_Lib" package="2512" value="8m">
<attribute name="TOLERANCE" value="1.0"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="PMR100HZPFU8L00"/>
<attribute name="MANUFACTURER_NAME" value="Rohm"/>
<attribute name="RESISTANCE" value="0.0080"/>
<attribute name="POWER" value="2.0"/>
<attribute name="VENDOR" value="Rohm"/>
<attribute name="NAME"/>
</element>
<element name="RT" library="SparkFun-Resistors" package="0603-RES" value="73.2k">
<attribute name="NAME"/>
</element>
<element name="RUV1" library="SparkFun-Resistors" package="0603-RES" value="35.7k">
<attribute name="NAME"/>
</element>
<element name="RUV2" library="SparkFun-Resistors" package="0603-RES" value="249k">
<attribute name="NAME"/>
</element>
<element name="U1" library="AcceleratedDesigns_Lib" package="PWP0028F_N" value="Value">
<attribute name="COMPTYPE" value="IC"/>
<attribute name="MANUFACTURER" value="Texas Instruments"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="LM5175PWPR"/>
<attribute name="PIN_COUNT" value="29"/>
<attribute name="MANUFACTURER_NAME" value="Texas Instruments"/>
<attribute name="MOUNTTYPE" value="SMT"/>
<attribute name="PACKAGEREFERENCE" value="PWP0028F"/>
<attribute name="TYPE" value="TYPE"/>
<attribute name="REFDES" value="RefDes"/>
<attribute name="ROHS" value="Y"/>
<attribute name="PARTNUMBER" value="LM5175PWP"/>
<attribute name="NAME"/>
</element>
<element name="RISNS_N" library="SparkFun-Resistors" package="0603-RES" value="158k">
<attribute name="NAME"/>
</element>
<element name="RISNS_P" library="SparkFun-Resistors" package="0603-RES" value="158k">
<attribute name="NAME"/>
</element>
<element name="RSNS" library="Seeed-OPL-Resistor" package="R2512" value="0,005R">
<attribute name="POWER" value="3w"/>
<attribute name="TOL" value="+-1%"/>
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="1206" value="10uF">
<attribute name="PROD_ID" value="CAP-10057"/>
<attribute name="NAME"/>
</element>
<element name="R1" library="Seeed-OPL-Resistor" package="R0402" value="0R">
<attribute name="VALUE"/>
</element>
<element name="R2" library="Seeed-OPL-Resistor" package="R0402" value="0R">
<attribute name="VALUE"/>
</element>
<element name="U$3" library="phoenix_spt" package="1990973" value="1990973">
<attribute name="MANUFACTURER" value="phoenix contact"/>
</element>
<element name="U$4" library="phoenix_spt" package="1990973" value="1990973">
<attribute name="MANUFACTURER" value="phoenix contact"/>
</element>
<element name="M5" library="AcceleratedDesigns_Lib" package="TRANS_NEXFET_Q5A" value="40V">
<attribute name="IDSMAX" value="50.0"/>
<attribute name="MANUFACTURER_NAME" value="Texas Instruments"/>
<attribute name="RDSON45" value="0.0098"/>
<attribute name="QUANTITY" value="1"/>
<attribute name="VDSMAX" value="40.0"/>
<attribute name="QGTYP" value="7.7"/>
<attribute name="VENDOR" value="Texas Instruments"/>
<attribute name="DATASHEETURL" value="http://www.ti.com/lit/ds/symlink/csd18504q5a.pdf"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="CSD18504Q5A"/>
<attribute name="NAME"/>
</element>
<element name="CCS" library="SparkFun-Capacitors" package="0805" value="2.2uF">
<attribute name="NAME"/>
</element>
<element name="CSLOPE" library="SparkFun-Capacitors" package="0805" value="2.2uF">
<attribute name="NAME"/>
</element>
<element name="CCOMP2" library="SparkFun-Capacitors" package="0805" value="2.2uF">
<attribute name="NAME"/>
</element>
<element name="CCOMP" library="SparkFun-Capacitors" package="0805" value="2.2uF">
<attribute name="NAME"/>
</element>
<element name="CSS" library="SparkFun-Capacitors" package="0805" value="22nF">
<attribute name="NAME"/>
</element>
<element name="CVCC" library="SparkFun-Capacitors" package="0805" value="2.2uF">
<attribute name="NAME"/>
</element>
<element name="CF" library="SparkFun-Capacitors" package="0805" value="2.2uF">
<attribute name="NAME"/>
</element>
<element name="CBOOT1" library="SparkFun-Capacitors" package="0603-CAP" value="100nF">
<attribute name="NAME"/>
</element>
<element name="F1" library="Littelfuse_By_element14_Batch_1" package="451_453" value="10A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ISNS" library="SparkFun-Capacitors" package="0805" value="2.2uF">
<attribute name="NAME"/>
</element>
<element name="F2" library="Littelfuse_By_element14_Batch_1" package="451_453" value="10A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CISNS1" library="SparkFun-Capacitors" package="0603-CAP" value="2.2pF">
<attribute name="NAME"/>
</element>
<element name="CISNS2" library="SparkFun-Capacitors" package="0603-CAP" value="2.2pF">
<attribute name="NAME"/>
</element>
<element name="RINEN" library="Seeed-OPL-Resistor" package="R0805" value="0R">
<attribute name="NAME"/>
</element>
<element name="RINEN1" library="Seeed-OPL-Resistor" package="R0805" value="NP">
<attribute name="NAME"/>
</element>
<element name="R4" library="Seeed-OPL-Resistor" package="R0402" value="0R">
<attribute name="VALUE"/>
</element>
<element name="R3" library="Seeed-OPL-Resistor" package="R0402" value="0R">
<attribute name="VALUE"/>
</element>
<element name="CBIAS" library="SparkFun-Capacitors" package="0805" value="1µF">
<attribute name="NAME"/>
</element>
<element name="CBOOT2" library="SparkFun-Capacitors" package="0603-CAP" value="100nF">
<attribute name="NAME"/>
</element>
<element name="LED1" library="led" package="SML0805" value="green">
<attribute name="NAME"/>
</element>
<element name="LED2" library="led" package="SML0805" value="red">
<attribute name="NAME"/>
</element>
<element name="LED3" library="led" package="SML0805" value="green">
<attribute name="NAME"/>
</element>
<element name="RLED1" library="SparkFun-Resistors" package="0603-RES" value="15k">
<attribute name="NAME"/>
</element>
<element name="RLED3" library="SparkFun-Resistors" package="0603-RES" value="10k">
<attribute name="NAME"/>
</element>
<element name="RLED2_L" library="SparkFun-Resistors" package="0603-RES" value="2k">
<attribute name="NAME"/>
</element>
<element name="RLED2_H" library="SparkFun-Resistors" package="0603-RES" value="6k">
<attribute name="NAME"/>
</element>
<element name="CCS1" library="SparkFun-Capacitors" package="0603-CAP" value="2.2pF">
<attribute name="NAME"/>
</element>
<element name="CCS2" library="SparkFun-Capacitors" package="0603-CAP" value="2.2pF">
<attribute name="NAME"/>
</element>
<element name="R5" library="Seeed-OPL-Resistor" package="R0402" value="0R">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="FILTER">
<contactref element="COUTX3_5" pad="1"/>
<contactref element="COUTX3_4" pad="1"/>
<contactref element="COUTX3_3" pad="1"/>
<contactref element="COUTX3_2" pad="1"/>
<contactref element="COUTX3" pad="1"/>
<contactref element="COUTX2_5" pad="1"/>
<contactref element="COUTX2_4" pad="1"/>
<contactref element="COUTX2_3" pad="1"/>
<contactref element="COUTX2_2" pad="1"/>
<contactref element="COUTX2" pad="1"/>
<contactref element="COUTX_5" pad="1"/>
<contactref element="COUTX_4" pad="1"/>
<contactref element="COUTX_3" pad="1"/>
<contactref element="COUTX_2" pad="1"/>
<contactref element="COUTX" pad="1"/>
<contactref element="RFBT" pad="1"/>
<contactref element="RSNS" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="M3" pad="5"/>
<contactref element="M3" pad="5"/>
<contactref element="M3" pad="5"/>
<contactref element="M3" pad="5"/>
<contactref element="M3" pad="5"/>
<contactref element="M3" pad="6"/>
<contactref element="M3" pad="7"/>
<contactref element="M3" pad="8"/>
<contactref element="M3" pad="9"/>
<contactref element="D3" pad="1"/>
</signal>
<signal name="19">
<contactref element="CBOOT1" pad="2"/>
<contactref element="U1" pad="26"/>
<contactref element="DBOOT1" pad="1"/>
</signal>
<signal name="_SW1_1">
<contactref element="U1" pad="28"/>
<contactref element="CBOOT1" pad="1"/>
<contactref element="M2" pad="5"/>
<contactref element="M2" pad="5"/>
<contactref element="M2" pad="5"/>
<contactref element="M2" pad="5"/>
<contactref element="M2" pad="5"/>
<contactref element="M2" pad="6"/>
<contactref element="M2" pad="7"/>
<contactref element="M2" pad="8"/>
<contactref element="M2" pad="9"/>
<contactref element="D2" pad="1"/>
<contactref element="L1" pad="1"/>
<contactref element="M1" pad="1"/>
<contactref element="M1" pad="1"/>
<contactref element="M1" pad="1"/>
<contactref element="M1" pad="2"/>
<contactref element="M1" pad="3"/>
</signal>
<signal name="_SW2_2">
<contactref element="CBOOT2" pad="1"/>
<contactref element="U1" pad="18"/>
<contactref element="L1" pad="2"/>
<contactref element="M4" pad="5"/>
<contactref element="M4" pad="5"/>
<contactref element="M4" pad="5"/>
<contactref element="M4" pad="5"/>
<contactref element="M4" pad="5"/>
<contactref element="M4" pad="6"/>
<contactref element="M4" pad="7"/>
<contactref element="M4" pad="8"/>
<contactref element="M4" pad="9"/>
<contactref element="M3" pad="1"/>
<contactref element="M3" pad="1"/>
<contactref element="M3" pad="1"/>
<contactref element="M3" pad="2"/>
<contactref element="M3" pad="3"/>
<contactref element="D3" pad="2"/>
</signal>
<signal name="IN">
<contactref element="U1" pad="3"/>
<contactref element="F1" pad="P$2"/>
<contactref element="RINEN" pad="1"/>
<contactref element="RLED1" pad="1"/>
<contactref element="CIN" pad="1"/>
<contactref element="CBULK" pad="1"/>
<contactref element="CIN_2" pad="1"/>
<contactref element="CIN_3" pad="1"/>
<contactref element="M1" pad="5"/>
<contactref element="M1" pad="5"/>
<contactref element="M1" pad="5"/>
<contactref element="M1" pad="5"/>
<contactref element="M1" pad="5"/>
<contactref element="M1" pad="6"/>
<contactref element="M1" pad="7"/>
<contactref element="M1" pad="8"/>
<contactref element="M1" pad="9"/>
<contactref element="DF" pad="2"/>
<contactref element="RUV2" pad="1"/>
</signal>
<signal name="22">
<contactref element="U1" pad="23"/>
<contactref element="DBOOT2" pad="2"/>
<contactref element="DBOOT1" pad="2"/>
<contactref element="CVCC" pad="1"/>
</signal>
<signal name="6">
<contactref element="RSENSE" pad="1"/>
<contactref element="M4" pad="1"/>
<contactref element="M4" pad="1"/>
<contactref element="M4" pad="1"/>
<contactref element="M4" pad="2"/>
<contactref element="M4" pad="3"/>
<contactref element="M2" pad="1"/>
<contactref element="M2" pad="1"/>
<contactref element="M2" pad="1"/>
<contactref element="M2" pad="2"/>
<contactref element="M2" pad="3"/>
<contactref element="D2" pad="2"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="FB">
<contactref element="RFBT" pad="2"/>
<contactref element="RFBB" pad="1"/>
<contactref element="U1" pad="11"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="22"/>
<contactref element="U1" pad="29"/>
<contactref element="U1" pad="5"/>
<contactref element="RSENSE" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="COUTX_5" pad="2"/>
<contactref element="COUTX_4" pad="2"/>
<contactref element="COUTX_3" pad="2"/>
<contactref element="COUTX_2" pad="2"/>
<contactref element="COUTX" pad="2"/>
<contactref element="COUTX3_5" pad="2"/>
<contactref element="COUTX3_4" pad="2"/>
<contactref element="COUTX3_3" pad="2"/>
<contactref element="COUTX3_2" pad="2"/>
<contactref element="COUTX3" pad="2"/>
<contactref element="COUTX2_5" pad="2"/>
<contactref element="COUTX2_4" pad="2"/>
<contactref element="COUTX2_3" pad="2"/>
<contactref element="COUTX2_2" pad="2"/>
<contactref element="CIN_2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="CIN_3" pad="2"/>
<contactref element="CIN" pad="2"/>
<contactref element="CBULK" pad="2"/>
<contactref element="U$4" pad="P$1"/>
<contactref element="U$4" pad="P$2"/>
<contactref element="M5" pad="1"/>
<contactref element="M5" pad="2"/>
<contactref element="M5" pad="3"/>
<contactref element="COUTX2" pad="2"/>
<contactref element="RINEN1" pad="2"/>
<contactref element="CBIAS" pad="1"/>
<contactref element="LED1" pad="C"/>
<contactref element="LED3" pad="C"/>
<contactref element="RLED2_L" pad="2"/>
<contactref element="RFBB" pad="2"/>
<contactref element="U1" pad="10"/>
<contactref element="R5" pad="2"/>
<contactref element="RUV1" pad="2"/>
<contactref element="CF" pad="2"/>
<contactref element="CVCC" pad="2"/>
</signal>
<signal name="ISNS-">
<contactref element="CISNS1" pad="1"/>
<contactref element="U1" pad="13"/>
<contactref element="ISNS" pad="1"/>
<contactref element="RISNS_N" pad="1"/>
</signal>
<signal name="ISNS+">
<contactref element="CISNS2" pad="1"/>
<contactref element="U1" pad="14"/>
<contactref element="RISNS_P" pad="1"/>
<contactref element="ISNS" pad="2"/>
</signal>
<signal name="OUT">
<contactref element="C3" pad="1"/>
<contactref element="F2" pad="P$1"/>
<contactref element="RSNS" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="CBIAS" pad="2"/>
<contactref element="RLED3" pad="1"/>
<contactref element="RLED2_H" pad="1"/>
<contactref element="U1" pad="12"/>
<contactref element="U1" pad="24"/>
</signal>
<signal name="IN_PREFUSE">
<contactref element="U$3" pad="P$1"/>
<contactref element="U$3" pad="P$2"/>
<contactref element="F1" pad="P$1"/>
</signal>
<signal name="GND_IN">
<contactref element="U$3" pad="P$3"/>
<contactref element="U$3" pad="P$4"/>
<contactref element="M5" pad="9"/>
<contactref element="M5" pad="5"/>
<contactref element="M5" pad="7"/>
<contactref element="M5" pad="6"/>
<contactref element="M5" pad="8"/>
</signal>
<signal name="N$4">
<contactref element="U$4" pad="P$3"/>
<contactref element="U$4" pad="P$4"/>
<contactref element="F2" pad="P$2"/>
</signal>
<signal name="_LDRV1">
<contactref element="M2" pad="4"/>
<contactref element="U1" pad="25"/>
</signal>
<signal name="_HDRV1">
<contactref element="M1" pad="4"/>
<contactref element="U1" pad="27"/>
</signal>
<signal name="_LDRV2">
<contactref element="M4" pad="4"/>
<contactref element="U1" pad="21"/>
</signal>
<signal name="_HDRV2">
<contactref element="M3" pad="4"/>
<contactref element="U1" pad="19"/>
</signal>
<signal name="N$7">
</signal>
<signal name="N$8">
</signal>
<signal name="N$9">
</signal>
<signal name="N$10">
</signal>
<signal name="N$12">
</signal>
<signal name="N$13">
</signal>
<signal name="N$14">
</signal>
<signal name="N$5">
</signal>
<signal name="N$1">
<contactref element="RINEN1" pad="1"/>
<contactref element="RINEN" pad="2"/>
<contactref element="M5" pad="4"/>
</signal>
<signal name="PGOOD">
<contactref element="LED2" pad="C"/>
<contactref element="U1" pad="17"/>
</signal>
<signal name="N$6">
<contactref element="LED1" pad="A"/>
<contactref element="RLED1" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="RLED3" pad="2"/>
<contactref element="LED3" pad="A"/>
</signal>
<signal name="N$18">
<contactref element="RLED2_L" pad="1"/>
<contactref element="RLED2_H" pad="2"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="RCS_N">
<contactref element="RCSG" pad="2"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="RCS_P">
<contactref element="RCSP" pad="2"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="CS">
<contactref element="RCSP" pad="1"/>
<contactref element="CCS" pad="1"/>
<contactref element="CCS1" pad="1"/>
<contactref element="U1" pad="16"/>
</signal>
<signal name="CSG">
<contactref element="CCS2" pad="1"/>
<contactref element="U1" pad="15"/>
<contactref element="RCSG" pad="1"/>
<contactref element="CCS" pad="2"/>
</signal>
<signal name="N$2">
</signal>
<signal name="N$3">
</signal>
<signal name="AGND">
<contactref element="CSS" pad="2"/>
<contactref element="CCOMP" pad="2"/>
<contactref element="CCOMP2" pad="2"/>
<contactref element="RT" pad="2"/>
<contactref element="RMODE" pad="2"/>
<contactref element="CCS1" pad="2"/>
<contactref element="CCS2" pad="2"/>
<contactref element="CISNS1" pad="2"/>
<contactref element="CISNS2" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="CSLOPE" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="U1" pad="20"/>
<contactref element="CBOOT2" pad="2"/>
<contactref element="DBOOT2" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="CSLOPE" pad="1"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="N$21">
<contactref element="U1" pad="6"/>
<contactref element="RT" pad="1"/>
</signal>
<signal name="N$22">
<contactref element="U1" pad="4"/>
<contactref element="RMODE" pad="1"/>
</signal>
<signal name="N$23">
<contactref element="RCOMP" pad="1"/>
<contactref element="CCOMP2" pad="1"/>
</signal>
<signal name="N$24">
<contactref element="RCOMP" pad="2"/>
<contactref element="CCOMP" pad="1"/>
</signal>
<signal name="N$25">
<contactref element="CSS" pad="1"/>
<contactref element="U1" pad="8"/>
</signal>
<signal name="RSNS_P">
<contactref element="R4" pad="2"/>
<contactref element="RISNS_P" pad="2"/>
</signal>
<signal name="RSNS_N">
<contactref element="R3" pad="2"/>
<contactref element="RISNS_N" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="RF" pad="2"/>
<contactref element="U1" pad="2"/>
<contactref element="CF" pad="1"/>
</signal>
<signal name="N$30">
<contactref element="RF" pad="1"/>
<contactref element="DF" pad="1"/>
</signal>
<signal name="N$28">
<contactref element="RUV2" pad="2"/>
<contactref element="RUV1" pad="1"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="N$11">
</signal>
</signals>
</board>
</drawing>
</eagle>
